{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":1330,"n_cols":2,"rows_kept":1330,"cut":false,"hidden":false,"merged":[]}
["item_alias","item_name"]
["UF1通量","UF1_FluxF"]
["UF2通量","UF2_FluxF"]
["UF1渗透率","UF1Per"]
["UF2渗透率","UF2Per"]
["RO1二三段产水比","RO1_SPK"]
["RO2二三段产水比","RO2_SPK"]
["进水量","water_in"]
["外供水流量","water_out"]
["总进水水温","AR.ZJS_SW（废）"]
["UF1步序与时长","UF1_DB"]
["UF2步序与时长","UF2_DB"]
["RO1步序与时长","RO1_DB"]
["RO2步序与时长","RO2_DB"]
["温湿度：一楼温度1","WSD_1L_WD_1"]
["温湿度：一楼温度2","WSD_1L_WD_2"]
["温湿度：一楼温度3","WSD_1L_WD_3"]
["温湿度：二楼温度1","WSD_2L_WD_1"]
["温湿度：二楼温度2","WSD_2L_WD_2"]
["1#RO产水流量","1#RO_CSFLOW"]
["2#RO产水流量","2#RO_CSFLOW"]
["反渗透进水ORP超高（组态弹窗用）","ORP_CX"]
["1#次钠加药泵故障","DR.P_1#CNB_FAULT"]
["1#次钠加药泵运行","DR.P_1#CNB_RFB"]
["1#出水碱加药泵故障","DR.P_1#CSJB_FAULT"]
["1#出水碱加药泵运行","DR.P_1#CSJB_RFB"]
["1#回用水泵故障","DR.P_1#HYSB_FAULT"]
["1#回用水泵运行","DR.P_1#HYSB_RFB"]
["1#PAC加药泵故障","DR.P_1#PACB_FAULT"]
["1#PAC加药泵运行","DR.P_1#PACB_RFB"]
["1#RO段间泵故障","DR.P_1#RODJB_FAULT"]
["1#RO段间泵运行","DR.P_1#RODJB_RFB"]
["1#RO高压泵故障","DR.P_1#ROGYB_FAULT"]
["1#RO高压泵运行","DR.P_1#ROGYB_RFB"]
["1#RO还原剂加药泵故障","DR.P_1#HYJB_FAULT"]
["1#RO还原剂加药泵运行","DR.P_1#HYJB_RFB"]
["1#酸加药泵故障","DR.P_1#SB_FAULT"]
["1#酸加药泵运行","DR.P_1#SB_RFB"]
["1#杀菌剂加药泵故障","DR.P_1#SJB_FAULT"]
["1#杀菌剂加药泵运行","DR.P_1#SJB_RFB"]
["1#超滤碱加药泵故障","DR.P_1#UF_JB_FAULT"]
["1#超滤碱加药泵运行","DR.P_1#UF_JB_RFB"]
["1#超滤反洗泵故障","DR.P_1#UFBWB_FAULT"]
["1#超滤反洗泵运行","DR.P_1#UFBWB_RFB"]
["1#阻垢剂加药泵故障","DR.P_1#ZGJB_FAULT"]
["1#阻垢剂加药泵运行","DR.P_1#ZGJB_RFB"]
["1#中和还原剂加药泵故障","DR.P_1#ZH_HYJ_FAULT"]
["1#中和还原剂加药泵运行","DR.P_1#ZH_HYJ_RFB"]
["2#次钠加药泵故障","DR.P_2#CNB_FAULT"]
["2#次钠加药泵运行","DR.P_2#CNB_RFB"]
["2#出水碱加药泵故障","DR.P_2#CSJB_FAULT"]
["2#出水碱加药泵运行","DR.P_2#CSJB_RFB"]
["2#回用水泵故障","DR.P_2#HYSB_FAULT"]
["2#回用水泵运行","DR.P_2#HYSB_RFB"]
["2#PAC加药泵故障","DR.P_2#PACB_FAULT"]
["2#PAC加药泵运行","DR.P_2#PACB_RFB"]
["2#RO段间泵故障","DR.P_2#RODJB_FAULT"]
["2#RO段间泵运行","DR.P_2#RODJB_RFB"]
["2#RO高压泵故障","DR.P_2#ROGYB_FAULT"]
["2#RO高压泵运行","DR.P_2#ROGYB_RFB"]
["2#RO还原剂加药泵故障","DR.P_2#HYJB_FAULT"]
["2#RO还原剂加药泵运行","DR.P_2#HYJB_RFB"]
["2#酸加药泵故障","DR.P_2#SB_FAULT"]
["2#酸加药泵运行","DR.P_2#SB_RFB"]
["2#杀菌剂加药泵故障","DR.P_2#SJB_FAULT"]
["2#杀菌剂加药泵运行","DR.P_2#SJB_RFB"]
["2#超滤碱加药泵故障","DR.P_2#UF_JB_FAULT"]
["2#超滤碱加药泵运行","DR.P_2#UF_JB_RFB"]
["2#超滤反洗泵故障","DR.P_2#UFBWB_FAULT"]
["2#超滤反洗泵运行","DR.P_2#UFBWB_RFB"]
["2#阻垢剂加药泵故障","DR.P_2#ZGJB_FAULT"]
["2#阻垢剂加药泵运行","DR.P_2#ZGJB_RFB"]
["2#中和还原剂加药泵故障","DR.P_2#ZH_HYJ_FAULT"]
["2#中和还原剂加药泵运行","DR.P_2#ZH_HYJ_RFB"]
["3#阻垢剂加药泵故障","DR.P_3#ZGJB_FAULT"]
["3#阻垢剂加药泵运行","DR.P_3#ZGJB_RFB"]
["废水泵故障","DR.P_FSB_FAULT"]
["废水泵运行","DR.P_FSB_RFB"]
["加热器故障","DR.P_JRQ_FAULT"]
["加热器启动","DR.P_JRQ_OUTPUT"]
["加热器运行","DR.P_JRQ_RFB"]
["潜污泵故障","DR.P_QWB_FAULT"]
["潜污泵运行","DR.P_QWB_RFB"]
["清洗水泵故障","DR.P_QXSB_FAULT"]
["清洗水泵运行","DR.P_QXSB_RFB"]
["反渗透供水泵故障","DR.P_ROGSB_FAULT"]
["反渗透供水泵运行","DR.P_ROGSB_RFB"]
["超滤供水泵故障","DR.P_UFGSB_FAULT"]
["超滤供水泵运行","DR.P_UFGSB_RFB"]
["中和泵故障","DR.P_ZH_FAULT"]
["中和泵运行","DR.P_ZH_RFB"]
["RO1一段压差高","DR.RO1_1D_YC_HIGH"]
["RO1二段压差高","DR.RO1_2D_YC_HIGH"]
["RO1执行一段碱维护","DR.RO1_ACT_1DJWH"]
["RO1执行一段杀菌","DR.RO1_ACT_1DSJ"]
["RO1执行一段酸维护","DR.RO1_ACT_1DSWH"]
["RO1执行二三段碱维护","DR.RO1_ACT_2/3DJWH"]
["RO1执行二三段杀菌维护","DR.RO1_ACT_2/3DSJWH"]
["RO1执行二三段酸维护","DR.RO1_ACT_2/3DSWH"]
["RO1执行冲洗","DR.RO1_ACT_CX"]
["RO1执行超越过滤","DR.RO1_ACT_CYGL"]
["RO1执行超越停机冲洗","DR.RO1_ACT_CYTJCX"]
["RO1执行超越停机加药冲洗","DR.RO1_ACT_CYTJJYCX"]
["RO1执行非正常停机冲洗","DR.RO1_ACT_FZCTJCX"]
["RO1执行过滤","DR.RO1_ACT_GL"]
["RO1执行长时间停机加药冲洗","DR.RO1_ACT_LONGTIME_CEB"]
["RO1启用反洗泵","DR.RO1_APPLY_RO_FXB"]
["RO1启用供水泵","DR.RO1_APPLY_RO_GSB"]
["RO1启用还原剂泵","DR.RO1_APPLY_RO_HYJB"]
["RO1启用还原剂阀","DR.RO1_APPLY_RO_HYJF"]
["RO1启用气洗阀","DR.RO1_APPLY_RO_QXF"]
["RO1启用阻垢剂泵","DR.RO1_APPLY_RO_ZGJB"]
["RO1启用杀菌泵","DR.RO1_APPLY_SJB"]
["RO1启用杀菌阀","DR.RO1_APPLY_SJF"]
["RO1启用维护碱泵","DR.RO1_APPLY_WHJB"]
["RO1启用维护碱阀","DR.RO1_APPLY_WHJF"]
["RO1启用维护酸泵","DR.RO1_APPLY_WHSB"]
["RO1启用维护酸阀","DR.RO1_APPLY_WHSF"]
["RO1二三段碱维护","DR.RO1_BT_2/3DJWH"]
["RO1电导率高","DR.RO1_DDL_HIGH"]
["RO1正在过滤标记","DR.RO1_FLAG_GLING"]
["RO1系统报错","DR.RO1_SYSTEM_ERROR"]
["RO1该杀菌了","DR.RO1_TIME_FOR_SJ"]
["RO2一段压差高","DR.RO2_1D_YC_HIGH"]
["RO2二段压差高","DR.RO2_2D_YC_HIGH"]
["RO2执行一段碱维护","DR.RO2_ACT_1DJWH"]
["RO2执行一段杀菌","DR.RO2_ACT_1DSJ"]
["RO2执行一段酸维护","DR.RO2_ACT_1DSWH"]
["RO2执行二三段碱维护","DR.RO2_ACT_2/3DJWH"]
["RO2执行二三段杀菌维护","DR.RO2_ACT_2/3DSJWH"]
["RO2执行二三段酸维护","DR.RO2_ACT_2/3DSWH"]
["RO2执行冲洗","DR.RO2_ACT_CX"]
["RO2执行超越过滤","DR.RO2_ACT_CYGL"]
["RO2执行超越停机冲洗","DR.RO2_ACT_CYTJCX"]
["RO2执行超越停机加药冲洗","DR.RO2_ACT_CYTJJYCX"]
["RO2执行非正常停机冲洗","DR.RO2_ACT_FZCTJCX"]
["RO2执行过滤","DR.RO2_ACT_GL"]
["RO2执行长时间停机加药冲洗","DR.RO2_ACT_LONGTIME_CEB"]
["RO2启用反洗泵","DR.RO2_APPLY_RO_FXB"]
["RO2启用供水泵","DR.RO2_APPLY_RO_GSB"]
["RO2启用还原剂泵","DR.RO2_APPLY_RO_HYJB"]
["RO2启用还原剂阀","DR.RO2_APPLY_RO_HYJF"]
["RO2启用气洗阀","DR.RO2_APPLY_RO_QXF"]
["RO2启用阻垢剂泵","DR.RO2_APPLY_RO_ZGJB"]
["RO2启用杀菌泵","DR.RO2_APPLY_SJB"]
["RO2启用杀菌阀","DR.RO2_APPLY_SJF"]
["RO2启用维护碱泵","DR.RO2_APPLY_WHJB"]
["RO2启用维护碱阀","DR.RO2_APPLY_WHJF"]
["RO2启用维护酸泵","DR.RO2_APPLY_WHSB"]
["RO2启用维护酸阀","DR.RO2_APPLY_WHSF"]
["RO2二三段碱维护","DR.RO2_BT_2/3DJWH"]
["RO2电导率高","DR.RO2_DDL_HIGH"]
["RO2正在过滤标记","DR.RO2_FLAG_GLING"]
["RO2系统报错","DR.RO2_SYSTEM_ERROR"]
["RO2该杀菌了","DR.RO2_TIME_FOR_SJ"]
["UF1启用供水泵","DR.UF1_APPLY_GSB"]
["UF1启用PAC泵","DR.UF1_APPLY_PAC_B"]
["UF1启用PAC阀","DR.UF1_APPLY_PAC-V"]
["UF1启用调节阀","DR.UF1_APPLY_TJV"]
["UF1自动过滤启动","DR.UF1_AUTOSTART_GL"]
["UF1手动反洗操作","DR.UF1_BT_BW"]
["UF1手动CEB操作","DR.UF1_BT_CEB"]
["UF1手动CIP操作","DR.UF1_BT_CIP"]
["UF1手动冲水操作","DR.UF1_BT_CS"]
["UF1手动清除过滤流量","DR.UF1_BT_ERASE_GLFLOW"]
["UF1手动过滤操作","DR.UF1_BT_GL"]
["UF1手动初始化操作","DR.UF1_BT_INAI"]
["UF1压差高限值报错","DR.UF1_ERR_YC_H"]
["UF1压差高高值报错","DR.UF1_ERR_YC_HH"]
["UF1药剂残留报错","DR.UF1_ERR_YJCL"]
["UF1膜内有药标志","DR.UF1_FLAG_MNYY"]
["UF1无它CEB标志","DR.UF1_FLAG_NOOTHERCEB"]
["UF1系统报错","DR.UF1_SYS_ERR"]
["UF2启用PAC泵","DR.UF2_APPLY_PAC_B"]
["UF2启用PAC阀","DR.UF2_APPLY_PAC_V"]
["UF2自动过滤启动","DR.UF2_AUTOSTART_GL"]
["UF2手动反洗操作","DR.UF2_BT_BW"]
["UF2手动CEB操作","DR.UF2_BT_CEB"]
["UF2手动CIP操作","DR.UF2_BT_CIP"]
["UF2手动冲水操作","DR.UF2_BT_CS"]
["UF2手动清除过滤流量","DR.UF2_BT_ERASE_GLFLOW"]
["UF2手动过滤操作","DR.UF2_BT_GL"]
["UF2手动初始化操作","DR.UF2_BT_INAI"]
["UF2压差高限值报错","DR.UF2_ERR_YC_H"]
["UF2压差高高值报错","DR.UF2_ERR_YC_HH"]
["UF2药剂残留报错","DR.UF2_ERR_YJCL"]
["UF2膜内有药标志","DR.UF2_FLAG_MNYY"]
["UF2无它CEB标志","DR.UF2_FLAG_NOOTHERCEB"]
["UF2系统报错","DR.UF2_SYS_ERR"]
["UF1反洗进水阀故障","DR.V_1#UF_BWJS_ERR"]
["UF1反洗进水阀总故障","DR.V_1#UF_BWJS_ERRT"]
["UF1反洗排水阀故障","DR.V_1#UF_BWPS_ERR"]
["UF1反洗排水阀总故障","DR.V_1#UF_BWPS_ERRT"]
["UF1产水阀故障","DR.V_1#UF_CS_ERR"]
["UF1产水阀总故障","DR.V_1#UF_CS_ERRT"]
["UF1排气阀1故障","DR.V_1#UF_PQ1_ERR"]
["UF1排气阀1总故障","DR.V_1#UF_PQ1_ERRT"]
["UF1排气阀2故障","DR.V_1#UF_PQ2_ERR"]
["UF1排气阀2总故障","DR.V_1#UF_PQ2_ERRT"]
["UF1排气阀3故障","DR.V_1#UF_PQ3_ERR"]
["UF1排气阀3总故障","DR.V_1#UF_PQ3_ERRT"]
["UF1排气阀4故障","DR.V_1#UF_PQ4_ERR"]
["UF1排气阀4总故障","DR.V_1#UF_PQ4_ERRT"]
["UF1隔断阀故障","DR.V_1#UFCIPGL_EER"]
["UF1隔断阀总故障","DR.V_1#UFCIPGL_ERRT"]
["RO1不合格阀故障","DR.V_1RO_BHG_ERR"]
["RO1不合格阀总故障","DR.V_1RO_BHG_ERRT"]
["RO1产水阀故障","DR.V_1RO_CS_ERR"]
["RO1产水阀总故障","DR.V_1RO_CS_ERRT"]
["RO1进水阀故障","DR.V_1RO_JS_ERR"]
["RO1进水阀总故障","DR.V_1RO_JS_ERRT"]
["RO1二段产水排气阀故障","DR.V_1ROEDCSPQ_ERR"]
["RO1二段产水排气阀总故障","DR.V_1ROEDCSPQ_ERRT"]
["RO1二段进水排气阀故障","DR.V_1ROEDJSPQ_ERR"]
["RO1二段进水排气阀总故障","DR.V_1ROEDJSPQ_ERRT"]
["RO1二段浓水排气阀故障","DR.V_1ROEDNSPQ_ERR"]
["RO1二段浓水排气阀总故障","DR.V_1ROEDNSPQ_ERRT"]
["RO1三段产水排气阀故障","DR.V_1ROSDCSPQ_ERR"]
["RO1三段产水排气阀总故障","DR.V_1ROSDCSPQ_ERRT"]
["RO1三段冲洗排水阀故障","DR.V_1ROSDCXPS_ERR"]
["RO1三段冲洗排水阀总故障","DR.V_1ROSDCXPS_ERRT"]
["RO1三段进水排气阀故障","DR.V_1ROSDJSPQ_ERR"]
["RO1三段进水排气阀总故障","DR.V_1ROSDJSPQ_ERRT"]
["RO1三段浓水排气阀故障","DR.V_1ROSDNSPQ_ERR"]
["RO1三段浓水排气阀总故障","DR.V_1ROSDNSPQ_ERRT"]
["RO1一段冲洗进水阀故障","DR.V_1ROYDBWJS_ERR"]
["RO1一段冲洗进水阀总故障","DR.V_1ROYDBWJS_ERRT"]
["RO1一段冲洗排水阀故障","DR.V_1ROYDBWPS_ERR"]
["RO1一段冲洗排水阀总故障","DR.V_1ROYDBWPS_ERRT"]
["RO1一段产水排气阀1故障","DR.V_1ROYDCSP1_ERR"]
["RO1一段产水排气阀1总故障","DR.V_1ROYDCSP1_ERRT"]
["RO1一段产水排气阀2故障","DR.V_1ROYDCSP2_ERR"]
["RO1一段产水排气阀2总故障","DR.V_1ROYDCSP2_ERRT"]
["RO1一段超越旁路阀故障","DR.V_1ROYDCYPL_ERR"]
["RO1一段超越旁路阀总故障","DR.V_1ROYDCYPL_ERRT"]
["RO1一段进水排气阀1故障","DR.V_1ROYDJSP1_ERR"]
["RO1一段进水排气阀1总故障","DR.V_1ROYDJSP1_ERRT"]
["RO1一段进水排气阀2故障","DR.V_1ROYDJSP2_ERR"]
["RO1一段进水排气阀2总故障","DR.V_1ROYDJSP2_ERRT"]
["RO1一段浓水排气阀1故障","DR.V_1ROYDNSP1_ERR"]
["RO1一段浓水排气阀1总故障","DR.V_1ROYDNSP1_ERRT"]
["RO1一段浓水排气阀2故障","DR.V_1ROYDNSP2_ERR"]
["RO1一段浓水排气阀2总故障","DR.V_1ROYDNSP2_ERRT"]
["RO1一段隔离阀故障","DR.V_1ROYDQXGL_ERR"]
["RO1一段隔离阀总故障","DR.V_1ROYDQXGL_ERRT"]
["UF2反洗进水阀故障","DR.V_2#UF_BWJS_ERR"]
["UF2反洗进水阀总故障","DR.V_2#UF_BWJS_ERRT"]
["UF2反洗排水阀故障","DR.V_2#UF_BWPS_ERR"]
["UF2反洗排水阀总故障","DR.V_2#UF_BWPS_ERRT"]
["UF2产水阀故障","DR.V_2#UF_CS_ERR"]
["UF2产水阀总故障","DR.V_2#UF_CS_ERRT"]
["UF2排气阀1故障","DR.V_2#UF_PQ1_ERR"]
["UF2排气阀1总故障","DR.V_2#UF_PQ1_ERRT"]
["UF2排气阀2故障","DR.V_2#UF_PQ2_ERR"]
["UF2排气阀2总故障","DR.V_2#UF_PQ2_ERRT"]
["UF2排气阀3故障","DR.V_2#UF_PQ3_ERR"]
["UF2排气阀3总故障","DR.V_2#UF_PQ3_ERRT"]
["UF2排气阀4故障","DR.V_2#UF_PQ4_ERR"]
["UF2排气阀4总故障","DR.V_2#UF_PQ4_ERRT"]
["UF2隔断阀故障","DR.V_2#UFCIPGL_ERR"]
["UF2隔断阀总故障","DR.V_2#UFCIPGL_ERRT"]
["RO2不合格阀故障","DR.V_2RO_BHG_ERR"]
["RO2不合格阀总故障","DR.V_2RO_BHG_ERRT"]
["RO2产水阀故障","DR.V_2RO_CS_ERR"]
["RO2产水阀总故障","DR.V_2RO_CS_ERRT"]
["RO2进水阀故障","DR.V_2RO_JS_ERR"]
["RO2进水阀总故障","DR.V_2RO_JS_ERRT"]
["RO2二段产水排气阀故障","DR.V_2ROEDCSPQ_ERR"]
["RO2二段产水排气阀总故障","DR.V_2ROEDCSPQ_ERRT"]
["RO2二段进水排气阀故障","DR.V_2ROEDJSPQ_ERR"]
["RO2二段进水排气阀总故障","DR.V_2ROEDJSPQ_ERRT"]
["RO2二段浓水排气阀故障","DR.V_2ROEDNSPQ_ERR"]
["RO2二段浓水排气阀总故障","DR.V_2ROEDNSPQ_ERRT"]
["RO2三段产水排气阀故障","DR.V_2ROSDCSPQ_ERR"]
["RO2三段产水排气阀总故障","DR.V_2ROSDCSPQ_ERRT"]
["RO2三段冲洗排水阀故障","DR.V_2ROSDCXPS_ERR"]
["RO2三段冲洗排水阀总故障","DR.V_2ROSDCXPS_ERRT"]
["RO2三段进水排气阀故障","DR.V_2ROSDJSPQ_ERR"]
["RO2三段进水排气阀总故障","DR.V_2ROSDJSPQ_ERRT"]
["RO2三段浓水排气阀故障","DR.V_2ROSDNSPQ_ERR"]
["RO2三段浓水排气阀总故障","DR.V_2ROSDNSPQ_ERRT"]
["RO2一段冲洗进水阀故障","DR.V_2ROYDBWJS_ERR"]
["RO2一段冲洗进水阀总故障","DR.V_2ROYDBWJS_ERRT"]
["RO2一段冲洗排水阀故障","DR.V_2ROYDBWPS_ERR"]
["RO2一段冲洗排水阀总故障","DR.V_2ROYDBWPS_ERRT"]
["RO2一段产水排气阀1故障","DR.V_2ROYDCSP1_ERR"]
["RO2一段产水排气阀1总故障","DR.V_2ROYDCSP1_ERRT"]
["RO2一段产水排气阀2故障","DR.V_2ROYDCSP2_ERR"]
["RO2一段产水排气阀2总故障","DR.V_2ROYDCSP2_ERRT"]
["RO2一段超越旁路阀故障","DR.V_2ROYDCYPL_ERR"]
["RO2一段超越旁路阀总故障","DR.V_2ROYDCYPL_ERRT"]
["RO2一段进水排气阀1故障","DR.V_2ROYDJSP1_ERR"]
["RO2一段进水排气阀1总故障","DR.V_2ROYDJSP1_ERRT"]
["RO2一段进水排气阀2故障","DR.V_2ROYDJSP2_ERR"]
["RO2一段进水排气阀2总故障","DR.V_2ROYDJSP2_ERRT"]
["RO2一段浓水排气阀1故障","DR.V_2ROYDNSP1_ERR"]
["RO2一段浓水排气阀1总故障","DR.V_2ROYDNSP1_ERRT"]
["RO2一段浓水排气阀2故障","DR.V_2ROYDNSP2_ERR"]
["RO2一段浓水排气阀2总故障","DR.V_2ROYDNSP2_ERRT"]
["RO2一段隔离阀故障","DR.V_2ROYDQXGL_ERR"]
["RO2一段隔离阀总故障","DR.V_2ROYDQXGL_ERRT"]
["反洗废水外排阀故障","DR.V_BW_WP_ERR"]
["反洗废水外排阀总故障","DR.V_BW_WP_ERRT"]
["CEB排放阀故障","DR.V_CEB_WP_ERR"]
["CEB排放阀总故障","DR.V_CEB_WP_ERRT"]
["RO气洗阀故障","DR.V_RO_QX_ERR"]
["RO气洗阀总故障","DR.V_RO_QX_ERRT"]
["UF1进水调节阀关状态","DR.V_UF1_TJV_CFB"]
["UF1进水调节阀开状态","DR.V_UF1_TJV_OFB"]
["UF2进水调节阀关状态","DR.V_UF2_TJV_CFB"]
["UF2进水调节阀开状态","DR.V_UF2_TJV_OFB"]
["中和外排阀故障","DR.V_ZH_WP_ERR"]
["中和外排阀总故障","DR.V_ZH_WP_ERRT"]
["1#出水碱加药泵频率反馈","AR.1#CSJB_FRE_FB_O"]
["1#回用水泵电流反馈","AR.1#HYSB_CUR_FB_O"]
["1#回用水泵频率反馈","AR.1#HYSB_FRE_FB_O"]
["1#回用水泵后轴温度","AR.1#HYSB_HZ_TEMP_O"]
["1#回用水泵前轴温度","AR.1#HYSB_QZ_TEMP_O"]
["1#PAC加药泵频率反馈","AR.1#PAC_FRE_FB_O"]
["1#RO产水电导","AR.1#RO_CSDD_O"]
["1#RO产水压力","AR.1#RO_CSPRESS_O"]
["1#RO二段产水流量","AR.1#RO_EDCSFLOW_O"]
["1#RO二段进水压力","AR.1#RO_EDJSPRESS_O"]
["1#RO二段浓水压力","AR.1#RO_EDNSPRESS_O"]
["1#RO进水流量","AR.1#RO_JSFLOW_O"]
["1#RO进水压力","AR.1#RO_JSPRESS_O"]
["1#RO浓水流量","AR.1#RO_NSFLOW_O"]
["1#RO三段产水流量","AR.1#RO_SDCSFLOW_O"]
["1#RO三段进水压力","AR.1#RO_SDJSPRESS_O"]
["1#RO三段浓水压力","AR.1#RO_SDNSPRESS_O"]
["1#RO段间泵电流反馈","AR.1#RODJB_CUR_FB_O"]
["1#RO段间泵测振反馈","AR.1#RODJB_CZ_O"]
["1#RO段间泵频率反馈","AR.1#RODJB_FRE_FB_O"]
["1#RO段间泵后轴温度","AR.1#RODJB_HZ_TEMP_O"]
["1#RO段间泵前轴温度","AR.1#RODJB_QZ_TEMP_O"]
["1#RO高压泵电流反馈","AR.1#ROGYB_CUR_FB_O"]
["1#RO高压泵测振反馈","AR.1#ROGYB_CZ_O"]
["1#RO高压泵频率反馈","AR.1#ROGYB_FRE_FB_O"]
["1#RO高压泵后轴温度反馈","AR.1#ROGYB_HZ_TEMP_O"]
["1#RO高压泵前轴温度反馈","AR.1#ROGYB_QZ_TEMP_O"]
["1#RO还原剂加药泵频率反馈","AR.1#ROHYJ_FRE_FB_O"]
["1#杀菌剂加药泵频率反馈","AR.1#SJB_FRE_FB_O"]
["1#UF产水压力","AR.1#UF_CSPRESS_O"]
["1#UF进水流量","AR.1#UF_JSFLOW_O"]
["1#UF进水压力","AR.1#UF_JSPRESS_O"]
["1#UF调节阀开度反馈","AR.1#UF_V_FB_O"]
["1#UF反洗泵电流反馈","AR.1#UFBWB_CUR_FB_O"]
["1#UF反洗泵频率反馈","AR.1#UFBWB_FRE_FB_O"]
["1#UF反洗泵后轴温度反馈","AR.1#UFBWB_HZ_TEMP_O"]
["1#UF反洗泵前轴温度反馈","AR.1#UFBWB_QZ_TEMP_O"]
["1#阻垢剂流量","AR.1#ZGJ_FLOW_O"]
["1#阻垢剂加药泵频率反馈","AR.1#ZGJ_FRE_FB_O"]
["2#出水碱加药泵频率反馈","AR.2#CSJB_FRE_FB_O"]
["2#回用水泵电流反馈","AR.2#HYSB_CUR_FB_O"]
["2#回用水泵频率反馈","AR.2#HYSB_FRE_FB_O"]
["2#回用水泵后轴温度","AR.2#HYSB_HZ_TEMP_O"]
["2#回用水泵前轴温度","AR.2#HYSB_QZ_TEMP_O"]
["2#PAC加药泵频率反馈","AR.2#PAC_FRE_FB_O"]
["2#RO产水电导","AR.2#RO_CSDD_O"]
["2#RO产水压力","AR.2#RO_CSPRESS_O"]
["2#RO二段产水流量","AR.2#RO_EDCSFLOW_O"]
["2#RO二段进水压力","AR.2#RO_EDJSPRESS_O"]
["2#RO二段浓水压力","AR.2#RO_EDNSPRESS_O"]
["2#RO进水流量","AR.2#RO_JSFLOW_O"]
["2#RO进水压力","AR.2#RO_JSPRESS_O"]
["2#RO浓水流量","AR.2#RO_NSFLOW_O"]
["2#RO三段产水流量","AR.2#RO_SDCSFLOW_O"]
["2#RO三段进水压力","AR.2#RO_SDJSPRESS_O"]
["2#RO三段浓水压力","AR.2#RO_SDNSPRESS_O"]
["2#RO段间泵电流反馈","AR.2#RODJB_CUR_FB_O"]
["2#RO段间泵测振反馈","AR.2#RODJB_CZ_O"]
["2#RO段间泵频率反馈","AR.2#RODJB_FRE_FB_O"]
["2#RO段间泵后轴温度","AR.2#RODJB_HZ_TEMP_O"]
["2#RO段间泵前轴温度","AR.2#RODJB_QZ_TEMP_O"]
["2#RO高压泵电流反馈","AR.2#ROGYB_CUR_FB_O"]
["2#RO高压泵测振反馈","AR.2#ROGYB_CZ_O"]
["2#RO高压泵频率反馈","AR.2#ROGYB_FRE_FB_O"]
["2#RO高压泵后轴温度反馈","AR.2#ROGYB_HZ_TEMP_O"]
["2#RO高压泵前轴温度反馈","AR.2#ROGYB_QZ_TEMP_O"]
["2#RO还原剂加药泵频率反馈","AR.2#ROHYJ_FRE_FB_O"]
["2#杀菌剂加药泵频率反馈","AR.2#SJB_FRE_FB_O"]
["2#UF产水压力","AR.2#UF_CSPRESS_O"]
["2#UF进水流量","AR.2#UF_JSFLOW_O"]
["2#UF进水压力","AR.2#UF_JSPRESS_O"]
["2#UF调节阀开度反馈","AR.2#UF_V_FB_O"]
["2#UF反洗泵电流反馈","AR.2#UFBWB_CUR_FB_O"]
["2#UF反洗泵频率反馈","AR.2#UFBWB_FRE_FB_O"]
["2#UF反洗泵后轴温度反馈","AR.2#UFBWB_HZ_TEMP_O"]
["2#UF反洗泵前轴温度反馈","AR.2#UFBWB_QZ_TEMP_O"]
["2#阻垢剂流量","AR.2#ZGJ_FLOW_O"]
["2#阻垢剂加药泵频率反馈","AR.2#ZGJ_FRE_FB_O"]
["3#阻垢剂加药泵频率反馈","AR.3#ZGJ_FRE_FB_O"]
["空气压力","AR.AIR_PRESS_O"]
["次钠液位高高限值","AR.ALARM_CN_HHR"]
["次钠液位高限值","AR.ALARM_CN_HR"]
["次钠液位","AR.ALARM_CN_IN"]
["次钠液位低低限值","AR.ALARM_CN_LLR"]
["次钠液位低限值","AR.ALARM_CN_LR"]
["废水箱液位高高限值","AR.ALARM_FSX_HHR"]
["废水箱液位高限值","AR.ALARM_FSX_HR"]
["废水箱液位","AR.ALARM_FSX_IN"]
["废水箱液位低低限值","AR.ALARM_FSX_LLR"]
["废水箱液位低限值","AR.ALARM_FSX_LR"]
["还原剂液位高高限值","AR.ALARM_HYJ_HHR"]
["还原剂液位高限值","AR.ALARM_HYJ_HR"]
["还原剂液位","AR.ALARM_HYJ_IN"]
["还原剂液位低低限值","AR.ALARM_HYJ_LLR"]
["还原剂液位低限值","AR.ALARM_HYJ_LR"]
["碱液位高高限值","AR.ALARM_J_HHR"]
["碱液位高限值","AR.ALARM_J_HR"]
["碱液位","AR.ALARM_J_IN"]
["碱液位低低限值","AR.ALARM_J_LLR"]
["碱液位低限值","AR.ALARM_J_LR"]
["进水箱1液位高高限值","AR.ALARM_JSX1_HHR"]
["进水箱1液位高限值","AR.ALARM_JSX1_HR"]
["进水箱1液位","AR.ALARM_JSX1_IN"]
["进水箱1液位低低限值","AR.ALARM_JSX1_LLR"]
["进水箱1液位低限值","AR.ALARM_JSX1_LR"]
["进水箱2液位高高限值","AR.ALARM_JSX2_HHR"]
["进水箱2液位高限值","AR.ALARM_JSX2_HR"]
["进水箱2液位","AR.ALARM_JSX2_IN"]
["进水箱2液位低低限值","AR.ALARM_JSX2_LLR"]
["进水箱2液位低限值","AR.ALARM_JSX2_LR"]
["絮凝剂液位高高限值","AR.ALARM_PAC_HHR"]
["絮凝剂液位高限值","AR.ALARM_PAC_HR"]
["絮凝剂液位","AR.ALARM_PAC_IN"]
["絮凝剂液位低低限值","AR.ALARM_PAC_LLR"]
["絮凝剂液位低限值","AR.ALARM_PAC_LR"]
["CIP水箱液位高高限值","AR.ALARM_QXSX_HHR"]
["CIP水箱液位高限值","AR.ALARM_QXSX_HR"]
["CIP水箱液位","AR.ALARM_QXSX_IN"]
["CIP水箱液位低低限值","AR.ALARM_QXSX_LLR"]
["CIP水箱液位低限值","AR.ALARM_QXSX_LR"]
["RO产水箱液位高高限值","AR.ALARM_RO_CSX_HHR"]
["RO产水箱液位高限值","AR.ALARM_RO_CSX_HR"]
["RO产水箱液位","AR.ALARM_RO_CSX_IN"]
["RO产水箱液位低低限值","AR.ALARM_RO_CSX_LLR"]
["RO产水箱液位低限值","AR.ALARM_RO_CSX_LR"]
["酸液位高高限值","AR.ALARM_S_HHR"]
["酸液位高限值","AR.ALARM_S_HR"]
["酸液位","AR.ALARM_S_IN"]
["酸液位低低限值","AR.ALARM_S_LLR"]
["酸液位低限值","AR.ALARM_S_LR"]
["杀菌剂液位高高限值","AR.ALARM_SJJ_HHR"]
["杀菌剂液位高限值","AR.ALARM_SJJ_HR"]
["杀菌剂液位","AR.ALARM_SJJ_IN"]
["杀菌剂液位低低限值","AR.ALARM_SJJ_LLR"]
["杀菌剂液位低限值","AR.ALARM_SJJ_LR"]
["UF产水箱液位高高限值","AR.ALARM_UF_CSX_HHR"]
["UF产水箱液位高限值","AR.ALARM_UF_CSX_HR"]
["UF产水箱液位","AR.ALARM_UF_CSX_IN"]
["UF产水箱液位低低限值","AR.ALARM_UF_CSX_LLR"]
["UF产水箱液位低限值","AR.ALARM_UF_CSX_LR"]
["阻垢剂液位高高限值","AR.ALARM_ZGJ_HHR"]
["阻垢剂液位高限值","AR.ALARM_ZGJ_HR"]
["阻垢剂液位","AR.ALARM_ZGJ_IN"]
["阻垢剂液位低低限值","AR.ALARM_ZGJ_LLR"]
["阻垢剂液位低限值","AR.ALARM_ZGJ_LR"]
["中和水箱液位高高限值","AR.ALARM_ZHSX_HHR"]
["中和水箱液位高限值","AR.ALARM_ZHSX_HR"]
["中和水箱液位","AR.ALARM_ZHSX_IN"]
["中和水箱液位低低限值","AR.ALARM_ZHSX_LLR"]
["中和水箱液位低限值","AR.ALARM_ZHSX_LR"]
["反洗流量","AR.BW_FLOW_O"]
["反洗压力","AR.BW_PRESS_O"]
["次钠液位","AR.CN_LEVEL_O"]
["RO产水箱液位","AR.CS_LEVEL_O"]
["废水箱液位","AR.FS_LEVEL_O"]
["废水泵后轴温度","AR.FSB_HZ_TEMP_O"]
["废水泵前轴温度","AR.FSB_QZ_TEMP_O"]
["还原剂液位","AR.HYJ_LEVEL_O"]
["回用水A流量","AR.HYS_A_FLOW_O"]
["回用水B流量","AR.HYS_B_FLOW_O"]
["回用水PH","AR.HYS_PH_O"]
["碱液位","AR.J_LEVEL_O"]
["进水箱1液位","AR.JSX1_LEVEL_O"]
["进水箱2液位","AR.JSX2_LEVEL_O"]
["1#次钠加药泵频率反馈","AR.P_1#CNB_FRE_FB"]
["1#次钠加药泵运行时间","AR.P_1#CNB_RUNTIME"]
["1#出水碱加药泵频率反馈","AR.P_1#CSJB_FRE_FB"]
["1#出水碱加药泵运行时间","AR.P_1#CSJB_RUNTIME"]
["1#回用水泵频率反馈","AR.P_1#HYSB_FRE_FB"]
["1#回用水泵运行时间","AR.P_1#HYSB_RUNTIME"]
["1#PAC加药泵频率反馈","AR.P_1#PACB_FRE_FB"]
["1#PAC加药泵运行时间","AR.P_1#PACB_RUNTIME"]
["1#RO段间泵频率反馈","AR.P_1#RODJB_FRE_FB"]
["1#RO段间泵运行时间","AR.P_1#RODJB_RUNTIME"]
["1#RO高压泵频率反馈","AR.P_1#ROGYB_FRE_FB"]
["1#RO高压泵运行时间","AR.P_1#ROGYB_RUNTIME"]
["1#RO还原剂加药泵频率反馈","AR.P_1#HYJB_FRE_FB"]
["1#RO还原剂加药泵运行时间","AR.P_1#HYJB_RUNTIME"]
["1#酸加药泵频率反馈","AR.P_1#SB_FRE_FB"]
["1#酸加药泵运行时间","AR.P_1#SB_RUNTIME"]
["1#杀菌剂加药泵频率反馈","AR.P_1#SJB_FRE_FB"]
["1#杀菌剂加药泵运行时间","AR.P_1#SJB_RUNTIME"]
["1#超滤碱加药泵频率反馈","AR.P_1#UF_JB_FRE_FB"]
["1#超滤碱加药泵运行时间","AR.P_1#UF_JB_RUNTIME"]
["1#UF反洗泵频率反馈","AR.P_1#UFBWB_FRE_FB"]
["1#UF反洗泵运行时间","AR.P_1#UFBWB_RUNTIME"]
["1#阻垢剂加药泵频率反馈","AR.P_1#ZGJB_FRE_FB"]
["1#阻垢剂加药泵运行时间","AR.P_1#ZGJB_RUNTIME"]
["1#中和还原剂加药泵频率反馈","AR.P_1#ZH_HYJ_FRE_FB"]
["1#中和还原剂加药泵运行时间","AR.P_1#ZH_HYJ_RUNTIME"]
["2#次钠加药泵频率反馈","AR.P_2#CNB_FRE_FB"]
["2#次钠加药泵运行时间","AR.P_2#CNB_RUNTIME"]
["2#出水碱加药泵频率反馈","AR.P_2#CSJB_FRE_FB"]
["2#出水碱加药泵运行时间","AR.P_2#CSJB_RUNTIME"]
["2#回用水泵频率反馈","AR.P_2#HYSB_FRE_FB"]
["2#回用水泵运行时间","AR.P_2#HYSB_RUNTIME"]
["2#PAC加药泵频率反馈","AR.P_2#PACB_FRE_FB"]
["2#PAC加药泵运行时间","AR.P_2#PACB_RUNTIME"]
["2#RO段间泵频率反馈","AR.P_2#RODJB_FRE_FB"]
["2#RO段间泵运行时间","AR.P_2#RODJB_RUNTIME"]
["2#RO高压泵频率反馈","AR.P_2#ROGYB_FRE_FB"]
["2#RO高压泵运行时间","AR.P_2#ROGYB_RUNTIME"]
["2#RO还原剂加药泵频率反馈","AR.P_2#HYJB_FRE_FB"]
["2#RO还原剂加药泵运行时间","AR.P_2#HYJB_RUNTIME"]
["2#酸加药泵频率反馈","AR.P_2#SB_FRE_FB"]
["2#酸加药泵运行时间","AR.P_2#SB_RUNTIME"]
["2#杀菌剂加药泵频率反馈","AR.P_2#SJB_FRE_FB"]
["2#杀菌剂加药泵运行时间","AR.P_2#SJB_RUNTIME"]
["2#超滤碱加药泵频率反馈","AR.P_2#UF_JB_FRE_FB"]
["2#超滤碱加药泵运行时间","AR.P_2#UF_JB_RUNTIME"]
["2#UF反洗泵频率反馈","AR.P_2#UFBWB_FRE_FB"]
["2#UF反洗泵运行时间","AR.P_2#UFBWB_RUNTIME"]
["2#阻垢剂加药泵频率反馈","AR.P_2#ZGJB_FRE_FB"]
["2#阻垢剂加药泵运行时间","AR.P_2#ZGJB_RUNTIME"]
["2#中和还原剂加药泵频率反馈","AR.P_2#ZH_HYJ_FRE_FB"]
["2#中和还原剂加药泵运行时间","AR.P_2#ZH_HYJ_RUNTIME"]
["3#阻垢剂加药泵频率反馈","AR.P_3#ZGJB_FRE_FB"]
["3#阻垢剂加药泵运行时间","AR.P_3#ZGJB_RUNTIME"]
["废水泵频率反馈","AR.P_FSB_FRE_FB"]
["废水泵运行时间","AR.P_FSB_RUNTIME"]
["加热器频率反馈","AR.P_JRQ_FRE_FB"]
["加热器运行时间","AR.P_JRQ_RUNTIME"]
["潜污泵频率反馈","AR.P_QWB_FRE_FB"]
["潜污泵运行时间","AR.P_QWB_RUNTIME"]
["清洗水泵频率反馈","AR.P_QXSB_FRE_FB"]
["清洗水泵运行时间","AR.P_QXSB_RUNTIME"]
["RO供水泵频率反馈","AR.P_ROGSB_FRE_FB"]
["RO供水泵运行时间","AR.P_ROGSB_RUNTIME"]
["UF供水泵频率反馈","AR.P_UFGSB_FRE_FB"]
["UF供水泵运行时间","AR.P_UFGSB_RUNTIME"]
["中和泵频率反馈","AR.P_ZH_FRE_FB"]
["中和泵运行时间","AR.P_ZH_RUNTIME"]
["絮凝剂液位","AR.PAC_LEVEL_O"]
["CIP水箱液位","AR.QXS_LEVEL_O"]
["CIP水PH","AR.QXS_PH_O"]
["CIP水温度","AR.QXS_TEMP_O"]
["清洗水泵电流","AR.QXSB_CUR_FB_O"]
["清洗水泵频率反馈","AR.QXSB_FRE_FB_O"]
["清洗水泵后轴温度反馈","AR.QXSB_HZ_TEMP_O"]
["清洗水泵前轴温度反馈","AR.QXSB_QZ_TEMP_O"]
["RO供水泵后轴温度反馈","AR.RO_GSB_HZ_TEMP_O"]
["RO供水泵前轴温度反馈","AR.RO_GSB_QZ_TEMP_0"]
["RO进水电导","AR.RO_JSDD_O"]
["RO进水ORP","AR.RO_JSORP_O"]
["RO进水PH","AR.RO_JSPH_O"]
["RO外供水电导","AR.RO_WSDD_O"]
["RO1一段压差","AR.RO1_1D_YC"]
["RO1一段产水流量","AR.RO1_1DUAN_CS_FLOW"]
["RO1一段已碱维护天数","AR.RO1_1DYJWH_DAYS"]
["RO1一段已杀菌天数","AR.RO1_1DYSJ_DAYS"]
["RO1一段已酸维护天数","AR.RO1_1DYSWH_DAYS"]
["RO1二三段已碱维护天数","AR.RO1_23DYJWH_DAYS"]
["RO1二三段已杀菌天数","AR.RO1_23DYSJ_DAYS"]
["RO1二三段已酸维护天数","AR.RO1_23DYSWH_DAYS"]
["RO1二段压差","AR.RO1_2D_YC"]
["RO1CODE_一段碱维护","AR.RO1_CODE_1DJWH"]
["RO1CODE_一段杀菌","AR.RO1_CODE_1DSJ"]
["RO1CODE_一段酸维护","AR.RO1_CODE_1DSWH"]
["RO1CODE_二三段碱维护","AR.RO1_CODE_23DJWH"]
["RO1CODE_二三段杀菌","AR.RO1_CODE_23DSJ"]
["RO1CODE_二三段酸维护","AR.RO1_CODE_23DSWH"]
["RO1CODE_冲洗","AR.RO1_CODE_CX"]
["1#RO高压泵频率输出","AR.RO1_GYB_FR_OUT"]
["RO1系统定时","AR.RO1_HMI_SET_TIME"]
["RO1系统计时","AR.RO1_HMI_SYSTEM_TIME"]
["RO1产水率","AR.RO1_RATE_CS"]
["RO1SET_一段碱维护天数","AR.RO1_SET_1DJWH_DAYS"]
["RO1SET_一段碱维后气水混洗时间","AR.RO1_SET_1DJWHHX_TIME"]
["RO1SET_一段碱维后水洗时间","AR.RO1_SET_1DJWHSX_TIME"]
["RO1SET_一段碱维加碱时间","AR.RO1_SET_1DJWJJ_TIME"]
["RO1SET_一段碱维浸泡时间","AR.RO1_SET_1DJWJP_TIME"]
["RO1SET_一段杀菌天数","AR.RO1_SET_1DSJ_DAYS"]
["RO1Set一段杀菌时间","AR.RO1_SET_1DSJ_TIME"]
["RO1Set_一段杀菌浸泡时间","AR.RO1_SET_1DSJJP_TIME"]
["RO1Set一段杀菌结束反冲排气时间","AR.RO1_SET_1DSJJS_TIME"]
["RO1Set一段杀菌结束气水冲时间","AR.RO1_SET_1DSJJSQ_TIME"]
["RO1SET_一段酸维护天数","AR.RO1_SET_1DSWH_DAYS"]
["RO1SET_一段酸维后气水混洗时间","AR.RO1_SET_1DSWHHX_TIME"]
["RO1SET_一段酸维后水洗时间","AR.RO1_SET_1DSWHSX_TIME"]
["RO1SET_一段酸维浸泡时间","AR.RO1_SET_1DSWJP_TIME"]
["RO1SET_一段酸维加酸时间","AR.RO1_SET_1DSWJS_TIME"]
["RO1Set_二三段正冲时间","AR.RO1_SET_2/3DZC_TIME"]
["RO1SET_二三段碱维护天数","AR.RO1_SET_23DJWH_DAYS"]
["RO1SET_二三段碱维护时间","AR.RO1_SET_23DJWH_TIME"]
["RO1SET_二三段碱维护后冲洗时间","AR.RO1_SET_23DJWHHCX_T"]
["RO1SET_二三段碱维护浸泡时间","AR.RO1_SET_23DJWHJ_TIME"]
["RO1SET_二三段杀菌天数","AR.RO1_SET_23DSJ_DAYS"]
["RO1SET_二三段杀菌后冲洗时间","AR.RO1_SET_23DSJCX_TIME"]
["RO1SET_二三段杀菌浸泡时间","AR.RO1_SET_23DSJJP_TIME"]
["RO1SET_二三段杀菌维护时间","AR.RO1_SET_23DSJWH_TIME"]
["RO1SET_二三段酸维护天数","AR.RO1_SET_23DSWH_DAYS"]
["RO1SET_二三段酸维护时间","AR.RO1_SET_23DSWH_TIME"]
["RO1SET_二三段酸维护后冲洗时间","AR.RO1_SET_23SWHHC_TIME"]
["RO1SET_二三段酸维护浸泡时间","AR.RO1_SET_23SWHJP_TIME"]
["RO1SET_超越过滤冲水排气时间","AR.RO1_SET_CYSGLCSPQ_T"]
["RO1SET_超越停机冲洗时间","AR.RO1_SET_CYTJCX_T"]
["RO1SET_超越停机加药冲洗时间","AR.RO1_SET_CYTJJYCX_T"]
["RO1SET_电导率","AR.RO1_SET_DDL"]
["RO1Set反冲时间","AR.RO1_SET_FC_TIME"]
["RO1Set过滤产水时间","AR.RO1_SET_GLCS_TIME"]
["RO1SET_GSPump_频率_L","AR.RO1_SET_GSPUMP_FR_L"]
["RO1SET_GYPump_频率","AR.RO1_SET_GYPUMP_FR"]
["RO1SET_GYPump_频率_H","AR.RO1_SET_GYPUMP_FR_H"]
["RO1SET_GYPump_频率_L","AR.RO1_SET_GYPUMP_FR_L"]
["RO1SET_加药冲洗反冲洗时间","AR.RO1_SET_JYCXFC_T"]
["RO1SET_加药冲洗正冲洗时间","AR.RO1_SET_JYCXZC_TIME"]
["RO1Set开机冲洗时间","AR.RO1_SET_KJCX_TIME"]
["RO1SET_ORP","AR.RO1_SET_ORP"]
["RO1SET_气水混洗时间","AR.RO1_SET_QSHX_TIEM"]
["RO1Set_水反洗排气时间","AR.RO1_SET_SFXPQ_TIME"]
["RO1SET_杀菌后反冲时间","AR.RO1_SET_SJHFC_TIME"]
["RO1SET_杀菌后正冲时间","AR.RO1_SET_SJHZC_TIME"]
["RO1SET杀菌流量","AR.RO1_SET_SJLL"]
["RO1Set停机加药冲洗时间","AR.RO1_SET_TJJYCX_TIME"]
["RO1SET_预杀菌天数","AR.RO1_SET_YSJ_DAYS"]
["RO1Set正冲时间","AR.RO1_SET_ZC_TIME"]
["RO1SET正冲流量","AR.RO1_SET_ZCLL"]
["RO1步序","AR.RO1_STEP"]
["RO1总产水流量","AR.RO1_TOTAL_CSLL"]
["RO1总过滤次数","AR.RO1_TOTAL_GL_CS"]
["RO1总进水流量","AR.RO1_TOTAL_JSLL"]
["RO1总浓水流量","AR.RO1_TOTAL_NSLL"]
["RO2一段压差","AR.RO2_1D_YC"]
["RO2一段产水流量","AR.RO2_1DUAN_CS_FLOW"]
["RO2一段已碱维护天数","AR.RO2_1DYJWH_DAYS"]
["RO2一段已杀菌天数","AR.RO2_1DYSJ_DAYS"]
["RO2一段已酸维护天数","AR.RO2_1DYSWH_DAYS"]
["RO2二三段已碱维护天数","AR.RO2_23DYJWH_DAYS"]
["RO2二三段已杀菌天数","AR.RO2_23DYSJ_DAYS"]
["RO2二三段已酸维护天数","AR.RO2_23DYSWH_DAYS"]
["RO2二段压差","AR.RO2_2D_YC"]
["RO2CODE_一段碱维护","AR.RO2_CODE_1DJWH"]
["RO2CODE_一段杀菌","AR.RO2_CODE_1DSJ"]
["RO2CODE_一段酸维护","AR.RO2_CODE_1DSWH"]
["RO2CODE_二三段碱维护","AR.RO2_CODE_23DJWH"]
["RO2CODE_二三段杀菌","AR.RO2_CODE_23DSJ"]
["RO2CODE_二三段酸维护","AR.RO2_CODE_23DSWH"]
["RO2CODE_冲洗","AR.RO2_CODE_CX"]
["2#RO供水泵频率输出","AR.RO2_GSB_FR_OUT"]
["2#RO高压泵频率输出","AR.RO2_GYB_FR_OUT"]
["RO2系统定时","AR.RO2_HMI_SET_TIME"]
["RO2系统计时","AR.RO2_HMI_SYSTEM_TIME"]
["RO2产水率","AR.RO2_RATE_CS"]
["RO2SET_一段碱维护天数","AR.RO2_SET_1DJWH_DAYS"]
["RO2SET_一段碱维后气水混洗时间","AR.RO2_SET_1DJWHHX_TIME"]
["RO2SET_一段碱维后水洗时间","AR.RO2_SET_1DJWHSX_TIME"]
["RO2SET_一段碱维加碱时间","AR.RO2_SET_1DJWJJ_TIME"]
["RO2SET_一段碱维浸泡时间","AR.RO2_SET_1DJWJP_TIME"]
["RO2SET_一段杀菌天数","AR.RO2_SET_1DSJ_DAYS"]
["RO2Set一段杀菌时间","AR.RO2_SET_1DSJ_TIME"]
["RO2Set_一段杀菌浸泡时间","AR.RO2_SET_1DSJJP_TIME"]
["RO2Set一段杀菌结束反冲排气时间","AR.RO2_SET_1DSJJS_TIME"]
["RO2Set一段杀菌结束气水冲时间","AR.RO2_SET_1DSJJSQ_TIME"]
["RO2SET_一段酸维护天数","AR.RO2_SET_1DSWH_DAYS"]
["RO2SET_一段酸维后气水混洗时间","AR.RO2_SET_1DSWHHX_TIME"]
["RO2SET_一段酸维后水洗时间","AR.RO2_SET_1DSWHSX_TIME"]
["RO2SET_一段酸维浸泡时间","AR.RO2_SET_1DSWJP_TIME"]
["RO2SET_一段酸维加酸时间","AR.RO2_SET_1DSWJS_TIME"]
["RO2Set_二三段正冲时间","AR.RO2_SET_2/3DZC_TIME"]
["RO2SET_二三段碱维护天数","AR.RO2_SET_23DJWH_DAYS"]
["RO2SET_二三段碱维护时间","AR.RO2_SET_23DJWH_TIME"]
["RO2SET_二三段碱维护后冲洗时间","AR.RO2_SET_23DJWHHCX_T"]
["RO2SET_二三段碱维护浸泡时间","AR.RO2_SET_23DJWHJ_TIME"]
["RO2SET_二三段杀菌天数","AR.RO2_SET_23DSJ_DAYS"]
["RO2SET_二三段杀菌后冲洗时间","AR.RO2_SET_23DSJCX_TIME"]
["RO2SET_二三段杀菌浸泡时间","AR.RO2_SET_23DSJJP_TIME"]
["RO2SET_二三段杀菌维护时间","AR.RO2_SET_23DSJWH_TIME"]
["RO2SET_二三段酸维护天数","AR.RO2_SET_23DSWH_DAYS"]
["RO2SET_二三段酸维护时间","AR.RO2_SET_23DSWH_TIME"]
["RO2SET_二三段酸维护后冲洗时间","AR.RO2_SET_23SWHHC_TIME"]
["RO2SET_二三段酸维护浸泡时间","AR.RO2_SET_23SWHJP_TIME"]
["RO2SET_超越过滤冲水排气时间","AR.RO2_SET_CYSGLCSPQ_T"]
["RO2SET_超越停机冲洗时间","AR.RO2_SET_CYTJCX_T"]
["RO2SET_超越停机加药冲洗时间","AR.RO2_SET_CYTJJYCX_T"]
["RO2SET_电导率","AR.RO2_SET_DDL"]
["RO2Set反冲时间","AR.RO2_SET_FC_TIME"]
["RO2Set过滤产水时间","AR.RO2_SET_GLCS_TIME"]
["RO2SET_GSPump_频率_L","AR.RO2_SET_GSPUMP_FR_L"]
["RO2SET_GYPump_频率","AR.RO2_SET_GYPUMP_FR"]
["RO2SET_GYPump_频率_H","AR.RO2_SET_GYPUMP_FR_H"]
["RO2SET_GYPump_频率_L","AR.RO2_SET_GYPUMP_FR_L"]
["RO2SET_加药冲洗反冲洗时间","AR.RO2_SET_JYCXFC_T"]
["RO2SET_加药冲洗正冲洗时间","AR.RO2_SET_JYCXZC_TIME"]
["RO2Set开机冲洗时间","AR.RO2_SET_KJCX_TIME"]
["RO2SET_ORP","AR.RO2_SET_ORP"]
["RO2SET_气水混洗时间","AR.RO2_SET_QSHX_TIEM"]
["RO2Set_水反洗排气时间","AR.RO2_SET_SFXPQ_TIME"]
["RO2SET_杀菌后反冲时间","AR.RO2_SET_SJHFC_TIME"]
["RO2SET_杀菌后正冲时间","AR.RO2_SET_SJHZC_TIME"]
["RO2SET杀菌流量","AR.RO2_SET_SJLL"]
["RO2Set停机加药冲洗时间","AR.RO2_SET_TJJYCX_TIME"]
["RO2SET_预杀菌天数","AR.RO2_SET_YSJ_DAYS"]
["RO2Set正冲时间","AR.RO2_SET_ZC_TIME"]
["RO2SET正冲流量","AR.RO2_SET_ZCLL"]
["RO2步序","AR.RO2_STEP"]
["RO2总产水流量","AR.RO2_TOTAL_CSLL"]
["RO2总过滤次数","AR.RO2_TOTAL_GL_CS"]
["RO2总进水流量","AR.RO2_TOTAL_JSLL"]
["RO2总浓水流量","AR.RO2_TOTAL_NSLL"]
["RO供水泵电流","AR.ROGSB_CUR_FB_O"]
["RO供水泵频率反馈","AR.ROGSB_FRE_FB_O"]
["酸液位","AR.S_LEVEL_O"]
["杀菌剂液位","AR.SJJ_LEVEL_O"]
["UF产水浊度","AR.UF_CS_ZD_O"]
["UF产水箱液位","AR.UF_CSLEVEL_O"]
["UF1反洗次数显示","AR.UF1_OUT_BW_CS"]
["UF1反洗流量累计","AR.UF1_OUT_BW_FLOW_ADD"]
["UF1反洗总次数累计","AR.UF1_OUT_BW_ZCS"]
["UF1过滤流量累计","AR.UF1_OUT_GL_FLOW_ADD"]
["UF1系统显示时间","AR.UF1_OUT_SYS_TIME"]
["UF1跨膜压差","AR.UF1_SSD_KMYC"]
["UF1步序","AR.UF1_STEP"]
["UF2反洗次数显示","AR.UF2_OUT_BW_CS"]
["UF2反洗流量累计","AR.UF2_OUT_BW_FLOW_ADD"]
["UF2反洗总次数累计","AR.UF2_OUT_BW_ZCS"]
["UF2过滤流量累计","AR.UF2_OUT_GL_FLOW_ADD"]
["UF2系统显示时间","AR.UF2_OUT_SYS_TIME"]
["UF2跨膜压差","AR.UF2_SSD_KMYC"]
["UF2步序","AR.UF2_STEP"]
["UF供水泵电流","AR.UFGSB_CUR_FB_O"]
["UF供水泵频率反馈","AR.UFGSB_FRE_FB_O"]
["UF供水泵后轴温度反馈","AR.UFGSB_HZ_TEMP_O"]
["UF供水泵前轴温度反馈","AR.UFGSB_QZ_TEMP_O"]
["UF1调节阀开度反馈","AR.V_UF1_TJV_KD_FB"]
["UF2调节阀开度反馈","AR.V_UF2_TJV_KD_FB"]
["阻垢剂液位","AR.ZGJ_LEVEL_O"]
["中和水箱液位","AR.ZH_LEVEL_O"]
["中和水箱ORP","AR.ZH_ORP_O"]
["中和水箱PH","AR.ZH_PH_O"]
["中和泵后轴温度","AR.ZHB_HZ_TEMP_O"]
["中和泵前轴温度","AR.ZHB_QZ_TEMP_O"]
["进水压力","AR.ZJS_PRESS_O"]
["进水温度","AR.ZJS_TEMP_O"]
["UF进水浊度","AR.ZJS_ZD_O"]
["2号阻垢剂泵给RO1用","DR.PUBLIC_BYZGJB4_1"]
["2号阻垢剂泵给RO2用","DR.PUBLIC_BYZGJB4_2"]
["UF其它设备CEB中","DR.PUBLIC_OTHER_CEBING"]
["UF其它设备反洗中","DR.PUBLIC_OTHER_BWING"]
["其它RO在过滤中","DR.PUBLIC_OTHERRO_GLING"]
["RO其他设备杀菌中","DR.PUBLIC_RO_OTHER_SJ"]
["RO其他设备冲洗中","DR.PUBLIC_RO_OTHER_CX"]
["RO_系统自动","DR.PUBLIC_RO_SYS_AUOTO"]
["RO_系统手动","DR.PUBLIC_RO_SYS_MAN"]
["UF系统自动","DR.PUBLIC_UF_SYS_AUTO"]
["UF系统手动","DR.PUBLIC_UF_SYS_MAN"]
["UF1_TJF_PID模式","DR.PUBLIC_UF1_TJF_PID"]
["UF2_TJF_PID模式","DR.PUBLIC_UF2_TJF_PID"]
["RO1系统报错","DR.PUBLIC_BY_B00L_1"]
["RO2系统报错","DR.PUBLIC_BY_BOOL_2"]
["UF2 PID频率输出","AR.PUBLIC_2#UF_FXB_PID"]
["2号垢剂泵切换","AR.PUBLIC_BYZGJB_QH"]
["RO_回用水泵频率PID输出","AR.PUBLIC_RO_HYSB_PID_S"]
["RO_手动输入运行数量","AR.PUBLIC_RO_MAN_SETNUM"]
["RO1_段间泵频率PID输出","AR.PUBLIC_RO1_DJB_PID_S"]
["RO1_高压泵频率PID输出","AR.PUBLIC_RO1_GYB_PID_S"]
["RO1膜通量","AR.PUBLIC_RO1_MTL"]
["RO2_段间泵频率PID输出","AR.PUBLIC_RO2_DJB_PID_S"]
["RO2_高压泵频率PID输出","AR.PUBLIC_RO2_GYB_PID_S"]
["RO2膜通量","AR.PUBLIC_RO2_MTL"]
["RO反洗泵定频OUT","AR.PUBLIC_RO_FXB_FRE_S"]
["RO供水泵定频OUT","AR.PUBLIC_RO_GSB_FRE_S"]
["RO回用水泵恒压值SP","AR.PUBLIC_RO_HYSB_SP"]
["UF1 PID频率输出","AR.PUBLIC_1#UF_FXB_PID"]
["UF手动输入运行数量","AR.PUBLIC_UF_MAN_SETNUM"]
["UF1调节阀PID开度","AR.PUBLIC_UF1_TJV_PID_O"]
["UF1冲水排气调节阀开度set","AR.PUBLIC_UF1TJFCSPQSET"]
["UF1过滤起始调节阀PID开度set","AR.PUBLIC_UF1TJFGLSET"]
["UF2调节阀PID开度","AR.PUBLIC_UF2_TJV_PID_O"]
["UF2冲水排气调节阀开度set","AR.PUBLIC_UF2TJFCSPQSET"]
["UF2过滤起始调节阀PID开度set","AR.PUBLIC_UF2TJFGLSET"]
["UF反洗泵流量SP","AR.PUBLIC_UF_FXB_LL_S"]
["UF反洗泵频率OUT","AR.PUBLIC_UF_FXB_FRE_S"]
["UF供水泵频率OUT","AR.PUBLIC_UF_GSB_FRE_S"]
["RO1三段压差","AR.PUBLIC_BY_REAL_1"]
["RO2三段压差","AR.PUBLIC_BY_REAL_2"]
["回用水泵正向有功电能","AR.ZZ_1#HYSB_EP"]
["1#RO段间泵正向有功电能","AR.ZZ_1#RODJB_EP"]
["1#RO高压泵正向有功电能","AR.ZZ_1#ROGYB_EP"]
["1#UF反洗泵正向有功电能","AR.ZZ_1#UFBWB_EP"]
["2#回用水泵正向有功电能","AR.ZZ_2#HYSB_EP"]
["2#空压机正向有功电能","AR.ZZ_2#KYJ_EP"]
["2#RO段间泵正向有功电能","AR.ZZ_2#RODJB_EP"]
["2#RO高压泵正向有功电能","AR.ZZ_2#ROGYB_EP"]
["2#UF反洗泵正向有功电能","AR.ZZ_2#UFBWB_EP"]
["1#电源进线正向有功电能","AR.ZZ_DYJX1_EP"]
["2#电源进线正向有功电能","AR.ZZ_DYJX2_EP"]
["1楼暖通正向有功电能","AR.ZZ_F1NT_EP"]
["2楼暖通正向有功电能","AR.ZZ_F2NT_EP"]
["废水排放泵正向有功电能","AR.ZZ_FSPFB_EP"]
["电源加热正向有功电能","AR.ZZ_JR_EP"]
["加药间正向有功电能","AR.ZZ_JYJ_EP"]
["1#空压机正向有功电能","AR.ZZ_KYJ_EP"]
["1#照明模块第一路","AR.ZZ_MB_1#ZM1"]
["1#照明模块第二路","AR.ZZ_MB_1#ZM2"]
["1#照明模块第三路","AR.ZZ_MB_1#ZM3"]
["1#照明模块第四路","AR.ZZ_MB_1#ZM4"]
["1#照明模块第五路","AR.ZZ_MB_1#ZM5"]
["1#照明模块第六路","AR.ZZ_MB_1#ZM6"]
["2#照明模块第一路","AR.ZZ_MB_2#ZM1"]
["2#照明模块第二路","AR.ZZ_MB_2#ZM2"]
["2#照明模块第三路","AR.ZZ_MB_2#ZM3"]
["2#照明模块第四路","AR.ZZ_MB_2#ZM4"]
["2#照明模块第五路","AR.ZZ_MB_2#ZM5"]
["2#照明模块第六路","AR.ZZ_MB_2#ZM6"]
["3#照明模块第一路","AR.ZZ_MB_3#ZM1"]
["3#照明模块第二路","AR.ZZ_MB_3#ZM2"]
["3#照明模块第三路","AR.ZZ_MB_3#ZM3"]
["3#照明模块第四路","AR.ZZ_MB_3#ZM4"]
["3#照明模块第五路","AR.ZZ_MB_3#ZM5"]
["3#照明模块第六路","AR.ZZ_MB_3#ZM6"]
["4#照明模块第一路","AR.ZZ_MB_4#ZM1"]
["4#照明模块第二路","AR.ZZ_MB_4#ZM2"]
["4#照明模块第三路","AR.ZZ_MB_4#ZM3"]
["4#照明模块第四路","AR.ZZ_MB_4#ZM4"]
["4#照明模块第五路","AR.ZZ_MB_4#ZM5"]
["4#照明模块第六路","AR.ZZ_MB_4#ZM6"]
["一楼温湿度1湿度","AR.ZZ_MB_F1WSD1_SD"]
["一楼温湿度1温度","AR.ZZ_MB_F1WSD1_WD"]
["一楼温湿度2湿度","AR.ZZ_MB_F1WSD2_SD"]
["一楼温湿度2温度","AR.ZZ_MB_F1WSD2_WD"]
["一楼温湿度3湿度","AR.ZZ_MB_F1WSD3_SD"]
["一楼温湿度3温度","AR.ZZ_MB_F1WSD3_WD"]
["一楼烟感1","AR.ZZ_MB_F1YG1"]
["一楼烟感2","AR.ZZ_MB_F1YG2"]
["一楼烟感3","AR.ZZ_MB_F1YG3"]
["二楼温湿度1湿度","AR.ZZ_MB_F2WSD1_SD"]
["二楼温湿度1温度","AR.ZZ_MB_F2WSD1_WD"]
["二楼温湿度2湿度","AR.ZZ_MB_F2WSD2_SD"]
["二楼温湿度2温度","AR.ZZ_MB_F2WSD2_WD"]
["二楼烟感1","AR.ZZ_MB_F2YG1"]
["二楼烟感2","AR.ZZ_MB_F2YG2"]
["前端泵房正向有功电能","AR.ZZ_QDBF_EP"]
["清洗水泵正向有功电能","AR.ZZ_QXSB_EP"]
["RO供水泵正向有功电能","AR.ZZ_ROGSB_EP"]
["溶药正向有功电能","AR.ZZ_RY_EP"]
["UF供水泵正向有功电能","AR.ZZ_UFGSB_EP"]
["UPS正向有功电能","AR.ZZ_UPS_EP"]
["中和废水泵正向有功电能","AR.ZZ_ZHFSB_EP"]
["RO1三段压差读取","AR.RO1_EX_3DYCREAD"]
["RO2三段压差读取","AR.RO2_EX_3DYCREAD"]
["RO产水池启动RO数量0","AR.YWLD_RO_CSC_LDUPNUM0"]
["RO产水池启动RO数量1","AR.YWLD_RO_CSC_LDUPNUM1"]
["RO产水池启动RO数量2","AR.YWLD_RO_CSC_LDUPNUM2"]
["RO产水池启动二套RO液位","AR.YWLD_RO_CSC_LDYWR[0]"]
["RO产水池启动一套RO液位","AR.YWLD_RO_CSC_LDYWR[1]"]
["RO产水池停止RO液位","AR.YWLD_RO_CSC_LDYWR[2]"]
["RO进水池启动数量0","AR.YWLD_RO_JSC_LDUPNUM0"]
["RO进水池启动RO数量1","AR.YWLD_RO_JSC_LDUPNUM1"]
["RO进水池启动RO数量2","AR.YWLD_RO_JSC_LDUPNUM2"]
["RO进水箱停RO液位","AR.YWLD_RO_JSC_LDYWR[0]"]
["RO进水箱启动一套RO液位","AR.YWLD_RO_JSC_LDYWR[1]"]
["RO进水箱启动二套RO液位","AR.YWLD_RO_JSC_LDYWR[2]"]
["RO产水池启动RO数量","AR.YWLD_SSDROCSCNEEDNUM"]
["RO进水池启动RO数量","AR.YWLD_SSDROJSCNEEDNUM"]
["UF产水池启动UF数量","AR.YWLD_SSDUFCSCNEEDNUM"]
["UF进水池启动UF数量","AR.YWLD_SSDUFJSCNEEDNUM"]
["UF自动液位启动数量","AR.YWLD_SSDUFNEEDNUM_YW"]
["UF产水池启动UF数量0","AR.YWLD_UF_CSC_LDUPNUM0"]
["UF产水池启动UF数量1","AR.YWLD_UF_CSC_LDUPNUM1"]
["UF产水池启动UF数量2","AR.YWLD_UF_CSC_LDUPNUM2"]
["UF产水箱启两套UF液位","AR.YWLD_UF_CSC_LDYWR[0]"]
["UF产水箱启一套UF液位","AR.YWLD_UF_CSC_LDYWR[1]"]
["UF产水箱启零套UF液位","AR.YWLD_UF_CSC_LDYWR[2]"]
["UF进水池启动数量0","AR.YWLD_UF_JSC_LDUPNUM0"]
["UF进水池启动数量1","AR.YWLD_UF_JSC_LDUPNUM1"]
["UF进水池启动数量2","AR.YWLD_UF_JSC_LDUPNUM2"]
["UF进水池停UF液位","AR.YWLD_UF_JSC_LDYWR[0]"]
["UF进水池启动一套UF液位","AR.YWLD_UF_JSC_LDYWR[1]"]
["UF进水池启动二套UF液位","AR.YWLD_UF_JSC_LDYWR[2]"]
["反洗水泵A震动温度","AR.ZZ_FXSB_A_ZD_WD"]
["反洗水泵A震动X轴速度","AR.ZZ_FXSB_A_ZD_XZSD"]
["反洗水泵A震动X轴位移","AR.ZZ_FXSB_A_ZD_XZWY"]
["反洗水泵A震动Y轴速度","AR.ZZ_FXSB_A_ZD_YZSD"]
["反洗水泵A震动Y轴位移","AR.ZZ_FXSB_A_ZD_YZWY"]
["反洗水泵A震动Z轴速度","AR.ZZ_FXSB_A_ZD_ZZSD"]
["反洗水泵A震动Z轴位移","AR.ZZ_FXSB_A_ZD_ZZWY"]
["反洗水泵B震动温度","AR.ZZ_FXSB_B_ZD_WD"]
["反洗水泵B震动X轴速度","AR.ZZ_FXSB_B_ZD_XZSD"]
["反洗水泵B震动X轴位移","AR.ZZ_FXSB_B_ZD_XZWY"]
["反洗水泵B震动Y轴速度","AR.ZZ_FXSB_B_ZD_YZSD"]
["反洗水泵B震动Y轴位移","AR.ZZ_FXSB_B_ZD_YZWY"]
["反洗水泵B震动Z轴速度","AR.ZZ_FXSB_B_ZD_ZZSD"]
["反洗水泵B震动Z轴位移","AR.ZZ_FXSB_B_ZD_ZZWY"]
["回用水泵A震动温度","AR.ZZ_HYSB_A_ZD_WD"]
["回用水泵A震动X轴速度","AR.ZZ_HYSB_A_ZD_XZSD"]
["回用水泵A震动X轴位移","AR.ZZ_HYSB_A_ZD_XZWY"]
["回用水泵A震动Y轴速度","AR.ZZ_HYSB_A_ZD_YZSD"]
["回用水泵A震动Y轴位移","AR.ZZ_HYSB_A_ZD_YZWY"]
["回用水泵A震动Z轴速度","AR.ZZ_HYSB_A_ZD_ZZSD"]
["回用水泵A震动Z轴位移","AR.ZZ_HYSB_A_ZD_ZZWY"]
["回用水泵B震动温度","AR.ZZ_HYSB_B_ZD_WD"]
["回用水泵B震动X轴速度","AR.ZZ_HYSB_B_ZD_XZSD"]
["回用水泵B震动X轴位移","AR.ZZ_HYSB_B_ZD_XZWY"]
["回用水泵B震动Y轴速度","AR.ZZ_HYSB_B_ZD_YZSD"]
["回用水泵B震动Y轴位移","AR.ZZ_HYSB_B_ZD_YZWY"]
["回用水泵B震动Z轴速度","AR.ZZ_HYSB_B_ZD_ZZSD"]
["回用水泵B震动Z轴位移","AR.ZZ_HYSB_B_ZD_ZZWY"]
["RO供水泵震动温度","AR.ZZ_ROGSB_ZD_WD"]
["RO供水泵震动X轴速度","AR.ZZ_ROGSB_ZD_XZSD"]
["RO供水泵震动X轴位移","AR.ZZ_ROGSB_ZD_XZWY"]
["RO供水泵震动Y轴速度","AR.ZZ_ROGSB_ZD_YZSD"]
["RO供水泵震动Y轴位移","AR.ZZ_ROGSB_ZD_YZWY"]
["RO供水泵震动Z轴速度","AR.ZZ_ROGSB_ZD_ZZSD"]
["RO供水泵震动Z轴位移","AR.ZZ_ROGSB_ZD_ZZWY"]
["外供水泵震动温度","AR.ZZ_WGSB_ZD_WD"]
["外供水泵震动X轴速度","AR.ZZ_WGSB_ZD_XZSD"]
["外供水泵震动X轴位移","AR.ZZ_WGSB_ZD_XZWY"]
["外供水泵震动Y轴速度","AR.ZZ_WGSB_ZD_YZSD"]
["外供水泵震动Y轴位移","AR.ZZ_WGSB_ZD_YZWY"]
["外供水泵震动Z轴速度","AR.ZZ_WGSB_ZD_ZZSD"]
["外供水泵震动Z轴位移","AR.ZZ_WGSB_ZD_ZZWY"]
["RO1三段压差高","DR.RO1_EX_3DYCG"]
["RO1一段进水压力高","DR.RO1_EX_PRESSHH_11"]
["RO1一段浓水压力高","DR.RO1_EX_PRESSHH_12"]
["RO1二段压力高","DR.RO1_EX_PRESSHH_22"]
["RO1三段进水压力高","DR.RO1_EX_PRESSHH_31"]
["RO1三段浓水压力高","DR.RO1_EX_PRESSHH_32"]
["RO1_FLG_段间泵出口压力大","DR.RO1_EX2_DJBCKYLD"]
["RO1_FLG_高压泵出口压力大","DR.RO1_EX2_FLG_GYBCKYLD"]
["RO1_FLG_过滤停机不冲洗","DR.RO1_EX2_FLG_TJBCX"]
["RO1_FLG_过滤停机整体冲洗","DR.RO1_EX2_FLG_TJZTCX"]
["RO1_FLG_膜里有药","DR.RO1_EX2_MLYY"]
["RO1_FLG_过滤停机冲二三段","DR.RO1_EX2_TJC23D"]
["RO2三段压差高","DR.RO2_EX_3DYCG"]
["RO2一段进水压力高","DR.RO2_EX_PRESSHH_11"]
["RO2一段浓水压力高","DR.RO2_EX_PRESSHH_12"]
["RO2二段压力高","DR.RO2_EX_PRESSHH_22"]
["RO2三段进水压力高","DR.RO2_EX_PRESSHH_31"]
["RO2三段浓水压力高","DR.RO2_EX_PRESSHH_32"]
["RO2_FLG_段间泵出口压力大","DR.RO2_EX2_DJBCKYLD"]
["RO2_FLG_高压泵出口压力大","DR.RO2_EX2_FLG_GYBCKYLD"]
["RO2_FLG_过滤停机不冲洗","DR.RO2_EX2_FLG_TJBCX"]
["RO2_FLG_过滤停机整体冲洗","DR.RO2_EX2_FLG_TJZTCX"]
["RO2_FLG_膜里有药","DR.RO2_EX2_MLYY"]
["RO2_FLG_过滤停机冲二三段","DR.RO2_EX2_TJC23D"]
["加药间1噪音频率1","AR.ZZ_ZY_FR1"]
["加药间1噪音频率10","AR.ZZ_ZY_FR10"]
["加药间1噪音频率100","AR.ZZ_ZY_FR100"]
["加药间1噪音频率101","AR.ZZ_ZY_FR101"]
["加药间1噪音频率102","AR.ZZ_ZY_FR102"]
["加药间1噪音频率103","AR.ZZ_ZY_FR103"]
["加药间1噪音频率104","AR.ZZ_ZY_FR104"]
["加药间1噪音频率105","AR.ZZ_ZY_FR105"]
["加药间1噪音频率106","AR.ZZ_ZY_FR106"]
["加药间1噪音频率107","AR.ZZ_ZY_FR107"]
["加药间1噪音频率108","AR.ZZ_ZY_FR108"]
["加药间1噪音频率109","AR.ZZ_ZY_FR109"]
["加药间1噪音频率11","AR.ZZ_ZY_FR11"]
["加药间1噪音频率110","AR.ZZ_ZY_FR110"]
["加药间1噪音频率111","AR.ZZ_ZY_FR111"]
["加药间1噪音频率112","AR.ZZ_ZY_FR112"]
["加药间1噪音频率113","AR.ZZ_ZY_FR113"]
["加药间1噪音频率114","AR.ZZ_ZY_FR114"]
["加药间1噪音频率115","AR.ZZ_ZY_FR115"]
["加药间1噪音频率116","AR.ZZ_ZY_FR116"]
["加药间1噪音频率117","AR.ZZ_ZY_FR117"]
["加药间1噪音频率118","AR.ZZ_ZY_FR118"]
["加药间1噪音频率119","AR.ZZ_ZY_FR119"]
["加药间1噪音频率12","AR.ZZ_ZY_FR12"]
["加药间1噪音频率120","AR.ZZ_ZY_FR120"]
["加药间1噪音频率121","AR.ZZ_ZY_FR121"]
["加药间1噪音频率122","AR.ZZ_ZY_FR122"]
["加药间1噪音频率123","AR.ZZ_ZY_FR123"]
["加药间1噪音频率124","AR.ZZ_ZY_FR124"]
["加药间1噪音频率125","AR.ZZ_ZY_FR125"]
["加药间1噪音频率126","AR.ZZ_ZY_FR126"]
["加药间1噪音频率127","AR.ZZ_ZY_FR127"]
["加药间1噪音频率13","AR.ZZ_ZY_FR13"]
["加药间1噪音频率14","AR.ZZ_ZY_FR14"]
["加药间1噪音频率15","AR.ZZ_ZY_FR15"]
["加药间1噪音频率16","AR.ZZ_ZY_FR16"]
["加药间1噪音频率17","AR.ZZ_ZY_FR17"]
["加药间1噪音频率18","AR.ZZ_ZY_FR18"]
["加药间1噪音频率19","AR.ZZ_ZY_FR19"]
["加药间1噪音频率2","AR.ZZ_ZY_FR2"]
["加药间1噪音频率20","AR.ZZ_ZY_FR20"]
["加药间1噪音频率21","AR.ZZ_ZY_FR21"]
["加药间1噪音频率22","AR.ZZ_ZY_FR22"]
["加药间1噪音频率23","AR.ZZ_ZY_FR23"]
["加药间1噪音频率24","AR.ZZ_ZY_FR24"]
["加药间1噪音频率25","AR.ZZ_ZY_FR25"]
["加药间1噪音频率26","AR.ZZ_ZY_FR26"]
["加药间1噪音频率27","AR.ZZ_ZY_FR27"]
["加药间1噪音频率28","AR.ZZ_ZY_FR28"]
["加药间1噪音频率29","AR.ZZ_ZY_FR29"]
["加药间1噪音频率3","AR.ZZ_ZY_FR3"]
["加药间1噪音频率30","AR.ZZ_ZY_FR30"]
["加药间1噪音频率31","AR.ZZ_ZY_FR31"]
["加药间1噪音频率32","AR.ZZ_ZY_FR32"]
["加药间1噪音频率33","AR.ZZ_ZY_FR33"]
["加药间1噪音频率34","AR.ZZ_ZY_FR34"]
["加药间1噪音频率35","AR.ZZ_ZY_FR35"]
["加药间1噪音频率36","AR.ZZ_ZY_FR36"]
["加药间1噪音频率37","AR.ZZ_ZY_FR37"]
["加药间1噪音频率38","AR.ZZ_ZY_FR38"]
["加药间1噪音频率39","AR.ZZ_ZY_FR39"]
["加药间1噪音频率4","AR.ZZ_ZY_FR4"]
["加药间1噪音频率40","AR.ZZ_ZY_FR40"]
["加药间1噪音频率41","AR.ZZ_ZY_FR41"]
["加药间1噪音频率42","AR.ZZ_ZY_FR42"]
["加药间1噪音频率43","AR.ZZ_ZY_FR43"]
["加药间1噪音频率44","AR.ZZ_ZY_FR44"]
["加药间1噪音频率45","AR.ZZ_ZY_FR45"]
["加药间1噪音频率46","AR.ZZ_ZY_FR46"]
["加药间1噪音频率47","AR.ZZ_ZY_FR47"]
["加药间1噪音频率48","AR.ZZ_ZY_FR48"]
["加药间1噪音频率49","AR.ZZ_ZY_FR49"]
["加药间1噪音频率5","AR.ZZ_ZY_FR5"]
["加药间1噪音频率50","AR.ZZ_ZY_FR50"]
["加药间1噪音频率51","AR.ZZ_ZY_FR51"]
["加药间1噪音频率52","AR.ZZ_ZY_FR52"]
["加药间1噪音频率53","AR.ZZ_ZY_FR53"]
["加药间1噪音频率54","AR.ZZ_ZY_FR54"]
["加药间1噪音频率55","AR.ZZ_ZY_FR55"]
["加药间1噪音频率56","AR.ZZ_ZY_FR56"]
["加药间1噪音频率57","AR.ZZ_ZY_FR57"]
["加药间1噪音频率58","AR.ZZ_ZY_FR58"]
["加药间1噪音频率59","AR.ZZ_ZY_FR59"]
["加药间1噪音频率6","AR.ZZ_ZY_FR6"]
["加药间1噪音频率60","AR.ZZ_ZY_FR60"]
["加药间1噪音频率61","AR.ZZ_ZY_FR61"]
["加药间1噪音频率62","AR.ZZ_ZY_FR62"]
["加药间1噪音频率63","AR.ZZ_ZY_FR63"]
["加药间1噪音频率64","AR.ZZ_ZY_FR64"]
["加药间1噪音频率65","AR.ZZ_ZY_FR65"]
["加药间1噪音频率66","AR.ZZ_ZY_FR66"]
["加药间1噪音频率67","AR.ZZ_ZY_FR67"]
["加药间1噪音频率68","AR.ZZ_ZY_FR68"]
["加药间1噪音频率69","AR.ZZ_ZY_FR69"]
["加药间1噪音频率7","AR.ZZ_ZY_FR7"]
["加药间1噪音频率70","AR.ZZ_ZY_FR70"]
["加药间1噪音频率71","AR.ZZ_ZY_FR71"]
["加药间1噪音频率72","AR.ZZ_ZY_FR72"]
["加药间1噪音频率73","AR.ZZ_ZY_FR73"]
["加药间1噪音频率74","AR.ZZ_ZY_FR74"]
["加药间1噪音频率75","AR.ZZ_ZY_FR75"]
["加药间1噪音频率76","AR.ZZ_ZY_FR76"]
["加药间1噪音频率77","AR.ZZ_ZY_FR77"]
["加药间1噪音频率78","AR.ZZ_ZY_FR78"]
["加药间1噪音频率79","AR.ZZ_ZY_FR79"]
["加药间1噪音频率8","AR.ZZ_ZY_FR8"]
["加药间1噪音频率80","AR.ZZ_ZY_FR80"]
["加药间1噪音频率81","AR.ZZ_ZY_FR81"]
["加药间1噪音频率82","AR.ZZ_ZY_FR82"]
["加药间1噪音频率83","AR.ZZ_ZY_FR83"]
["加药间1噪音频率84","AR.ZZ_ZY_FR84"]
["加药间1噪音频率85","AR.ZZ_ZY_FR85"]
["加药间1噪音频率86","AR.ZZ_ZY_FR86"]
["加药间1噪音频率87","AR.ZZ_ZY_FR87"]
["加药间1噪音频率88","AR.ZZ_ZY_FR88"]
["加药间1噪音频率89","AR.ZZ_ZY_FR89"]
["加药间1噪音频率9","AR.ZZ_ZY_FR9"]
["加药间1噪音频率90","AR.ZZ_ZY_FR90"]
["加药间1噪音频率91","AR.ZZ_ZY_FR91"]
["加药间1噪音频率92","AR.ZZ_ZY_FR92"]
["加药间1噪音频率93","AR.ZZ_ZY_FR93"]
["加药间1噪音频率94","AR.ZZ_ZY_FR94"]
["加药间1噪音频率95","AR.ZZ_ZY_FR95"]
["加药间1噪音频率96","AR.ZZ_ZY_FR96"]
["加药间1噪音频率97","AR.ZZ_ZY_FR97"]
["加药间1噪音频率98","AR.ZZ_ZY_FR98"]
["加药间1噪音频率99","AR.ZZ_ZY_FR99"]
["加药间2噪音频率1","AR.ZZ_ZY2_FR1"]
["加药间2噪音频率10","AR.ZZ_ZY2_FR10"]
["加药间2噪音频率100","AR.ZZ_ZY2_FR100"]
["加药间2噪音频率101","AR.ZZ_ZY2_FR101"]
["加药间2噪音频率102","AR.ZZ_ZY2_FR102"]
["加药间2噪音频率103","AR.ZZ_ZY2_FR103"]
["加药间2噪音频率104","AR.ZZ_ZY2_FR104"]
["加药间2噪音频率105","AR.ZZ_ZY2_FR105"]
["加药间2噪音频率106","AR.ZZ_ZY2_FR106"]
["加药间2噪音频率107","AR.ZZ_ZY2_FR107"]
["加药间2噪音频率108","AR.ZZ_ZY2_FR108"]
["加药间2噪音频率109","AR.ZZ_ZY2_FR109"]
["加药间2噪音频率11","AR.ZZ_ZY2_FR11"]
["加药间2噪音频率110","AR.ZZ_ZY2_FR110"]
["加药间2噪音频率111","AR.ZZ_ZY2_FR111"]
["加药间2噪音频率112","AR.ZZ_ZY2_FR112"]
["加药间2噪音频率113","AR.ZZ_ZY2_FR113"]
["加药间2噪音频率114","AR.ZZ_ZY2_FR114"]
["加药间2噪音频率115","AR.ZZ_ZY2_FR115"]
["加药间2噪音频率116","AR.ZZ_ZY2_FR116"]
["加药间2噪音频率117","AR.ZZ_ZY2_FR117"]
["加药间2噪音频率118","AR.ZZ_ZY2_FR118"]
["加药间2噪音频率119","AR.ZZ_ZY2_FR119"]
["加药间2噪音频率12","AR.ZZ_ZY2_FR12"]
["加药间2噪音频率120","AR.ZZ_ZY2_FR120"]
["加药间2噪音频率121","AR.ZZ_ZY2_FR121"]
["加药间2噪音频率122","AR.ZZ_ZY2_FR122"]
["加药间2噪音频率123","AR.ZZ_ZY2_FR123"]
["加药间2噪音频率124","AR.ZZ_ZY2_FR124"]
["加药间2噪音频率125","AR.ZZ_ZY2_FR125"]
["加药间2噪音频率126","AR.ZZ_ZY2_FR126"]
["加药间2噪音频率127","AR.ZZ_ZY2_FR127"]
["加药间2噪音频率13","AR.ZZ_ZY2_FR13"]
["加药间2噪音频率14","AR.ZZ_ZY2_FR14"]
["加药间2噪音频率15","AR.ZZ_ZY2_FR15"]
["加药间2噪音频率16","AR.ZZ_ZY2_FR16"]
["加药间2噪音频率17","AR.ZZ_ZY2_FR17"]
["加药间2噪音频率18","AR.ZZ_ZY2_FR18"]
["加药间2噪音频率19","AR.ZZ_ZY2_FR19"]
["加药间2噪音频率2","AR.ZZ_ZY2_FR2"]
["加药间2噪音频率20","AR.ZZ_ZY2_FR20"]
["加药间2噪音频率21","AR.ZZ_ZY2_FR21"]
["加药间2噪音频率22","AR.ZZ_ZY2_FR22"]
["加药间2噪音频率23","AR.ZZ_ZY2_FR23"]
["加药间2噪音频率24","AR.ZZ_ZY2_FR24"]
["加药间2噪音频率25","AR.ZZ_ZY2_FR25"]
["加药间2噪音频率26","AR.ZZ_ZY2_FR26"]
["加药间2噪音频率27","AR.ZZ_ZY2_FR27"]
["加药间2噪音频率28","AR.ZZ_ZY2_FR28"]
["加药间2噪音频率29","AR.ZZ_ZY2_FR29"]
["加药间2噪音频率3","AR.ZZ_ZY2_FR3"]
["加药间2噪音频率30","AR.ZZ_ZY2_FR30"]
["加药间2噪音频率31","AR.ZZ_ZY2_FR31"]
["加药间2噪音频率32","AR.ZZ_ZY2_FR32"]
["加药间2噪音频率33","AR.ZZ_ZY2_FR33"]
["加药间2噪音频率34","AR.ZZ_ZY2_FR34"]
["加药间2噪音频率35","AR.ZZ_ZY2_FR35"]
["加药间2噪音频率36","AR.ZZ_ZY2_FR36"]
["加药间2噪音频率37","AR.ZZ_ZY2_FR37"]
["加药间2噪音频率38","AR.ZZ_ZY2_FR38"]
["加药间2噪音频率39","AR.ZZ_ZY2_FR39"]
["加药间2噪音频率4","AR.ZZ_ZY2_FR4"]
["加药间2噪音频率40","AR.ZZ_ZY2_FR40"]
["加药间2噪音频率41","AR.ZZ_ZY2_FR41"]
["加药间2噪音频率42","AR.ZZ_ZY2_FR42"]
["加药间2噪音频率43","AR.ZZ_ZY2_FR43"]
["加药间2噪音频率44","AR.ZZ_ZY2_FR44"]
["加药间2噪音频率45","AR.ZZ_ZY2_FR45"]
["加药间2噪音频率46","AR.ZZ_ZY2_FR46"]
["加药间2噪音频率47","AR.ZZ_ZY2_FR47"]
["加药间2噪音频率48","AR.ZZ_ZY2_FR48"]
["加药间2噪音频率49","AR.ZZ_ZY2_FR49"]
["加药间2噪音频率5","AR.ZZ_ZY2_FR5"]
["加药间2噪音频率50","AR.ZZ_ZY2_FR50"]
["加药间2噪音频率51","AR.ZZ_ZY2_FR51"]
["加药间2噪音频率52","AR.ZZ_ZY2_FR52"]
["加药间2噪音频率53","AR.ZZ_ZY2_FR53"]
["加药间2噪音频率54","AR.ZZ_ZY2_FR54"]
["加药间2噪音频率55","AR.ZZ_ZY2_FR55"]
["加药间2噪音频率56","AR.ZZ_ZY2_FR56"]
["加药间2噪音频率57","AR.ZZ_ZY2_FR57"]
["加药间2噪音频率58","AR.ZZ_ZY2_FR58"]
["加药间2噪音频率59","AR.ZZ_ZY2_FR59"]
["加药间2噪音频率6","AR.ZZ_ZY2_FR6"]
["加药间2噪音频率60","AR.ZZ_ZY2_FR60"]
["加药间2噪音频率61","AR.ZZ_ZY2_FR61"]
["加药间2噪音频率62","AR.ZZ_ZY2_FR62"]
["加药间2噪音频率63","AR.ZZ_ZY2_FR63"]
["加药间2噪音频率64","AR.ZZ_ZY2_FR64"]
["加药间2噪音频率65","AR.ZZ_ZY2_FR65"]
["加药间2噪音频率66","AR.ZZ_ZY2_FR66"]
["加药间2噪音频率67","AR.ZZ_ZY2_FR67"]
["加药间2噪音频率68","AR.ZZ_ZY2_FR68"]
["加药间2噪音频率69","AR.ZZ_ZY2_FR69"]
["加药间2噪音频率7","AR.ZZ_ZY2_FR7"]
["加药间2噪音频率70","AR.ZZ_ZY2_FR70"]
["加药间2噪音频率71","AR.ZZ_ZY2_FR71"]
["加药间2噪音频率72","AR.ZZ_ZY2_FR72"]
["加药间2噪音频率73","AR.ZZ_ZY2_FR73"]
["加药间2噪音频率74","AR.ZZ_ZY2_FR74"]
["加药间2噪音频率75","AR.ZZ_ZY2_FR75"]
["加药间2噪音频率76","AR.ZZ_ZY2_FR76"]
["加药间2噪音频率77","AR.ZZ_ZY2_FR77"]
["加药间2噪音频率78","AR.ZZ_ZY2_FR78"]
["加药间2噪音频率79","AR.ZZ_ZY2_FR79"]
["加药间2噪音频率8","AR.ZZ_ZY2_FR8"]
["加药间2噪音频率80","AR.ZZ_ZY2_FR80"]
["加药间2噪音频率81","AR.ZZ_ZY2_FR81"]
["加药间2噪音频率82","AR.ZZ_ZY2_FR82"]
["加药间2噪音频率83","AR.ZZ_ZY2_FR83"]
["加药间2噪音频率84","AR.ZZ_ZY2_FR84"]
["加药间2噪音频率85","AR.ZZ_ZY2_FR85"]
["加药间2噪音频率86","AR.ZZ_ZY2_FR86"]
["加药间2噪音频率87","AR.ZZ_ZY2_FR87"]
["加药间2噪音频率88","AR.ZZ_ZY2_FR88"]
["加药间2噪音频率89","AR.ZZ_ZY2_FR89"]
["加药间2噪音频率9","AR.ZZ_ZY2_FR9"]
["加药间2噪音频率90","AR.ZZ_ZY2_FR90"]
["加药间2噪音频率91","AR.ZZ_ZY2_FR91"]
["加药间2噪音频率92","AR.ZZ_ZY2_FR92"]
["加药间2噪音频率93","AR.ZZ_ZY2_FR93"]
["加药间2噪音频率94","AR.ZZ_ZY2_FR94"]
["加药间2噪音频率95","AR.ZZ_ZY2_FR95"]
["加药间2噪音频率96","AR.ZZ_ZY2_FR96"]
["加药间2噪音频率97","AR.ZZ_ZY2_FR97"]
["加药间2噪音频率98","AR.ZZ_ZY2_FR98"]
["加药间2噪音频率99","AR.ZZ_ZY2_FR99"]
["前端补水泵—自动","DR.QD_BSB_BT_AUTO"]
["前端补水泵——启动","DR.QD_BSB_BT_START"]
["前端补水泵——停止","DR.QD_BSB_BT_STOP"]
["前端补水泵——故障","DR.QD_BSB_FAULT"]
["前端补水泵——输出","DR.QD_BSB_OUTPUT"]
["前端补水泵——ready","DR.QD_BSB_READY"]
["前端补水泵——运行反馈","DR.QD_BSB_RFB"]
["前端补水阀——自动","DR.QD_BSF_BT_AUTO"]
["前端补水阀——开阀","DR.QD_BSF_BT_CLOSE"]
["前端补水阀——关阀","DR.QD_BSF_BT_OPEN"]
["前端补水阀——关ing","DR.QD_BSF_CING"]
["前端补水阀——自动关","DR.QD_BSF_CLOSEAUTO"]
["前端补水阀——故障 ","DR.QD_BSF_ERR"]
["前端补水阀——总故障 ","DR.QD_BSF_ERRT"]
["前端排气阀故障","DR.QD_PQF_ERR"]
["前端排气阀总故障","DR.QD_PQF_ERRT"]
["前端破真空阀故障","DR.QD_PZKF_ERR"]
["前端破真空阀总故障","DR.QD_PZKF_ERRT"]
["故障_引水装置补水超时","DR.QD_QT_44_3"]
["用户华晟-流量计温度","AI.WG_FLOW_HS2_00"]
["用户华晟-流量计压力","AI.WG_FLOW_HS2_01"]
["用户华晟-补偿前流量","AI.WG_FLOW_HS2_02"]
["用户华晟-补偿后流量","AI.WG_FLOW_HS2_03"]
["用户华晟-累计流量","AI.WG_FLOW_HS2_04"]
["用户芯动-流量计温度","AI.WG_FLOW_XD_00"]
["用户芯动-流量计压力","AI.WG_FLOW_XD_01"]
["用户芯动-补偿前流量","AI.WG_FLOW_XD_02"]
["用户芯动-补偿后流量","AI.WG_FLOW_XD_03"]
["用户芯动-累计流量","AI.WG_FLOW_XD_04"]
["前端补水泵","AR.QD_BSB_FRE_FB"]
["前端补水泵","AR.QD_BSB_FRESET"]
["前端补水泵","AR.QD_BSB_RUNTIME"]
["RO产水加碱频率1套","AR.QD_LD_R164"]
["RO产水加碱频率2套","AR.QD_LD_R168"]
["RO产水加碱频率备1","AR.QD_LD_R172"]
["RO产水加碱频率备2","AR.QD_LD_R176"]
["前端补水参照时间","AR.QD_QT_BSTIMESET"]
["前端补水计时","AR.QD_QT_TIMEADD"]
["前端液位触发后延时补水计时","AR.QD_QT_TIMEDELAYADD"]
["备","AR.UF_LD_R152"]
["备","AR.UF_LD_R156"]
["备","AR.UF_LD_R182"]
["极点总供水流量计","AI.WG_FLOW_JD_04"]
["F1空调地址","AI.ZZ_AC1S_ADR"]
["F1空调波特率","AI.ZZ_AC1S_BD"]
["F1空调红外状态","AI.ZZ_AC1S_IR"]
["F1空调湿度","AI.ZZ_AC1S_RH"]
["F1空调温度","AI.ZZ_AC1S_T"]
["F1空调运行状态检测信号值","AI.ZZ_AC1S_VALUE"]
["F2电控柜侧空调地址","AI.ZZ_AC2S_ADR"]
["F2电控柜侧空调波特率","AI.ZZ_AC2S_BD"]
["F2电控柜侧空调红外状态","AI.ZZ_AC2S_IR"]
["F2电控柜侧空调湿度","AI.ZZ_AC2S_RH"]
["F2电控柜侧空调温度","AI.ZZ_AC2S_T"]
["F2电控柜侧空调运行状态检测信号值","AI.ZZ_AC2S_VALUE"]
["F2空调地址","AI.ZZ_AC3S_ADR"]
["F2空调波特率","AI.ZZ_AC3S_BD"]
["F2空调红外状态","AI.ZZ_AC3S_IR"]
["F2空调湿度","AI.ZZ_AC3S_RH"]
["F2空调温度","AI.ZZ_AC3S_T"]
["F2空调运行状态检测信号值","AI.ZZ_AC3S_VALUE"]
["ORP-X0","AR.ROHYJ_ARR_X_ORP0"]
["ORP-X1","AR.ROHYJ_ARR_X_ORP1"]
["ORP-X10","AR.ROHYJ_ARR_X_ORP10"]
["ORP-X11","AR.ROHYJ_ARR_X_ORP11"]
["ORP-X12","AR.ROHYJ_ARR_X_ORP12"]
["ORP-X13","AR.ROHYJ_ARR_X_ORP13"]
["ORP-X14","AR.ROHYJ_ARR_X_ORP14"]
["ORP-X15","AR.ROHYJ_ARR_X_ORP15"]
["ORP-X2","AR.ROHYJ_ARR_X_ORP2"]
["ORP-X3","AR.ROHYJ_ARR_X_ORP3"]
["ORP-X4","AR.ROHYJ_ARR_X_ORP4"]
["ORP-X5","AR.ROHYJ_ARR_X_ORP5"]
["ORP-X6","AR.ROHYJ_ARR_X_ORP6"]
["ORP-X7","AR.ROHYJ_ARR_X_ORP7"]
["ORP-X8","AR.ROHYJ_ARR_X_ORP8"]
["ORP-X9","AR.ROHYJ_ARR_X_ORP9"]
["HYJ—Y——0","AR.ROHYJ_ARR_Y1_HYJ0"]
["HYJ—Y——1","AR.ROHYJ_ARR_Y1_HYJ1"]
["HYJ—Y——10","AR.ROHYJ_ARR_Y1_HYJ10"]
["HYJ—Y——11","AR.ROHYJ_ARR_Y1_HYJ11"]
["HYJ—Y——12","AR.ROHYJ_ARR_Y1_HYJ12"]
["HYJ—Y——13","AR.ROHYJ_ARR_Y1_HYJ13"]
["HYJ—Y——14","AR.ROHYJ_ARR_Y1_HYJ14"]
["HYJ—Y——15","AR.ROHYJ_ARR_Y1_HYJ15"]
["HYJ—Y——2","AR.ROHYJ_ARR_Y1_HYJ2"]
["HYJ—Y——3","AR.ROHYJ_ARR_Y1_HYJ3"]
["HYJ—Y——4","AR.ROHYJ_ARR_Y1_HYJ4"]
["HYJ—Y——5","AR.ROHYJ_ARR_Y1_HYJ5"]
["HYJ—Y——6","AR.ROHYJ_ARR_Y1_HYJ6"]
["HYJ—Y——7","AR.ROHYJ_ARR_Y1_HYJ7"]
["HYJ—Y——8","AR.ROHYJ_ARR_Y1_HYJ8"]
["HYJ—Y——9","AR.ROHYJ_ARR_Y1_HYJ9"]
["还原剂额定加药量","AR.ROHYJ_HYJJYBRATEDDO"]
["还原剂药液流量","AR.ROHYJ_JS_HYJFLOWNEED"]
["进水流量修正系数","AR.ROHYJ_K_FLOWWATER"]
["ORP中间值","AR.ROHYJ_ORP_MID"]
["ORP实验值","AR.ROHYJ_ORP_SYZ"]
["还原剂泵数量","AR.ROHYJ_SET_BASICHYJ_N"]
["进水流量修正后值","AR.ROHYJ_SSD_FLOWW_XZ"]
["进水流量","AR.ROHYJ_SSD_FLOWWATER"]
["还原剂浓度","AR.ROHYJ_SSD_HYJ_ND"]
["还原剂流量计（如有）","AR.ROHYJ_SSD_HYJND_FLOW"]
["还原剂Y1","AR.ROHYJ_Y1_OUT"]
["加药量标定指标—0","DR.ROHYJ_ARR_FLAG_X0"]
["加药量标定指标—1","DR.ROHYJ_ARR_FLAG_X1"]
["加药量标定指标—10","DR.ROHYJ_ARR_FLAG_X10"]
["加药量标定指标—11","DR.ROHYJ_ARR_FLAG_X11"]
["加药量标定指标—12","DR.ROHYJ_ARR_FLAG_X12"]
["加药量标定指标—13","DR.ROHYJ_ARR_FLAG_X13"]
["加药量标定指标—14","DR.ROHYJ_ARR_FLAG_X14"]
["加药量标定指标—15","DR.ROHYJ_ARR_FLAG_X15"]
["加药量标定指标—2","DR.ROHYJ_ARR_FLAG_X2"]
["加药量标定指标—3","DR.ROHYJ_ARR_FLAG_X3"]
["加药量标定指标—4","DR.ROHYJ_ARR_FLAG_X4"]
["加药量标定指标—5","DR.ROHYJ_ARR_FLAG_X5"]
["加药量标定指标—6","DR.ROHYJ_ARR_FLAG_X6"]
["加药量标定指标—7","DR.ROHYJ_ARR_FLAG_X7"]
["加药量标定指标—8","DR.ROHYJ_ARR_FLAG_X8"]
["加药量标定指标—9","DR.ROHYJ_ARR_FLAG_X9"]
["华盛瞬时流量","AR.WGLL_HS_SSLL"]
["华盛流体速度","AR.WGLL_HS_LTSD"]
["华盛累计流量","AR.WGLL_HS_LJLL"]
["芯动补偿前流量","AR.WGLL_XD_BCQLL"]
["芯动补偿后流量","AR.WGLL_XD_BCHLL"]
["芯动累计流量","AR.WGLL_XD_LJLL"]
["极光累计流量","AR.WGLL_JG_LJLL"]
["反渗透回收率","ROHSL"]