{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":842,"n_cols":2,"rows_kept":842,"cut":false,"hidden":false,"merged":[]}
["item_alias","item_name"]
["UF步序和产水时长","UF_DB"]
["RO步序和产水时长","RO_DB"]
["进水量","water_in"]
["外供水流量","water_out"]
["UF反洗前压差","UF_BW_Before_TMP"]
["UF反洗后压差","UF_BW_After_TMP"]
["加药进线电流1A","JY_JXDL_1A"]
["加药进线电流1B","JY_JXDL_1B"]
["加药进线电流1C","JY_JXDL_1C"]
["RO进线电流1A","RO_JXDL_1A"]
["RO进线电流1B","RO_JXDL_1B"]
["RO进线电流1C","RO_JXDL_1C"]
["UF进线电流1A","UF_JXDL_1A"]
["UF进线电流1B","UF_JXDL_1B"]
["UF进线电流1C","UF_JXDL_1C"]
["UF运行过滤压差","UF_FF_TMP"]
["APPLY_13","ns=6;s=APPLY_13"]
["APPLY_14","ns=6;s=APPLY_14"]
["APPLY_15","ns=6;s=APPLY_15"]
["Apply_9","ns=6;s=APPLY_9"]
["Apply_次钠加药","ns=6;s=APPLY_CNJY"]
["Apply反洗泵BW","ns=6;s=APPLY_FXB_BW"]
["Apply反洗泵CEB","ns=6;s=APPLY_FXB_CEB"]
["Apply公共阀BW阀","ns=6;s=APPLY_GGF_BWV"]
["Apply公共阀CEB阀","ns=6;s=APPLY_GGF_CEBV"]
["Apply供水泵FW","ns=6;s=APPLY_GSB_FW"]
["Apply_碱加药","ns=6;s=APPLY_JJY"]
["Apply_PAC加药","ns=6;s=APPLY_PACJY"]
["Apply_酸加药","ns=6;s=APPLY_SJY"]
["Apply提升泵1","ns=6;s=APPLY_TSB1"]
["Apply提升泵2","ns=6;s=APPLY_TSB2"]
["药剂残留","ns=6;s=DRUG_ERR"]
["ERR_5","ns=6;s=ERR_5"]
["ERR_6","ns=6;s=ERR_6"]
["ERR_7","ns=6;s=ERR_7"]
["产水池A连锁","ns=6;s=FLAG_LS_CSCA"]
["产水池B连锁","ns=6;s=FLAG_LS_CSCB"]
["进水池A连锁","ns=6;s=FLAG_LS_JSCA"]
["进水池B连锁","ns=6;s=FLAG_LS_JSCB"]
["加热器1故障","ns=6;s=JBQ_JY_JRQ1_FAULT"]
["加热器1启动","ns=6;s=JBQ_JY_JRQ1_OUTPUT"]
["加热器1运行","ns=6;s=JBQ_JY_JRQ1_RFB"]
["加热器2故障","ns=6;s=JBQ_JY_JRQ2_FAULT"]
["加热器2启动","ns=6;s=JBQ_JY_JRQ2_OUTPUT"]
["加热器2运行","ns=6;s=JBQ_JY_JRQ2_RFB"]
["CEB还原剂加药泵1故障","ns=6;s=P_CEB_HYJ1_FAULT"]
["CEB还原剂加药泵1启动","ns=6;s=P_CEB_HYJ1_OUTPUT"]
["CEB还原剂加药泵1运行","ns=6;s=P_CEB_HYJ1_RFB"]
["CEB还原剂加药泵2故障","ns=6;s=P_CEB_HYJ2_FAULT"]
["CEB还原剂加药泵2启动","ns=6;s=P_CEB_HYJ2_OUTPUT"]
["CEB还原剂加药泵2运行","ns=6;s=P_CEB_HYJ2_RFB"]
["CIP泵故障","ns=6;s=P_JY_CIPB_FAULT"]
["CIP泵运行","ns=6;s=P_JY_CIPB_RFB"]
["次钠加药泵1故障","ns=6;s=P_JY_CN1_FAULT"]
["次钠加药泵1启动","ns=6;s=P_JY_CN1_OUTPUT"]
["次钠加药泵1运行","ns=6;s=P_JY_CN1_RFB"]
["次钠加药泵2故障","ns=6;s=P_JY_CN2_FAULT"]
["次钠加药泵2启动","ns=6;s=P_JY_CN2_OUTPUT"]
["次钠加药泵2运行","ns=6;s=P_JY_CN2_RFB"]
["反洗风机故障","ns=6;s=P_JY_FX_FJ_FAULT"]
["反洗风机启动","ns=6;s=P_JY_FX_FJ_OUTPUT"]
["反洗风机运行","ns=6;s=P_JY_FX_FJ_RFB"]
["还原剂加药泵故障","ns=6;s=P_JY_HYJ_FAULT"]
["还原剂加药泵运行","ns=6;s=P_JY_HYJ_RFB"]
["碱加药泵1故障","ns=6;s=P_JY_JJ1_FAULT"]
["碱加药泵1启动","ns=6;s=P_JY_JJ1_OUTPUT"]
["碱加药泵1运行","ns=6;s=P_JY_JJ1_RFB"]
["碱加药泵2故障","ns=6;s=P_JY_JJ2_FAULT"]
["碱加药泵2启动","ns=6;s=P_JY_JJ2_OUTPUT"]
["碱加药泵2运行","ns=6;s=P_JY_JJ2_RFB"]
["酸加药泵1故障","ns=6;s=P_JY_JS1_FAULT"]
["酸加药泵1启动","ns=6;s=P_JY_JS1_OUTPUT"]
["酸加药泵1运行","ns=6;s=P_JY_JS1_RFB"]
["酸加药泵2故障","ns=6;s=P_JY_JS2_FAULT"]
["酸加药泵2启动","ns=6;s=P_JY_JS2_OUTPUT"]
["酸加药泵2运行","ns=6;s=P_JY_JS2_RFB"]
["泵坑潜污泵1故障","ns=6;s=P_JY_QWB1_FAULT"]
["泵坑潜污泵1启动","ns=6;s=P_JY_QWB1_OUTPUT"]
["泵坑潜污泵1运行","ns=6;s=P_JY_QWB1_RFB"]
["泵坑潜污泵2故障","ns=6;s=P_JY_QWB2_FAULT"]
["泵坑潜污泵2启动","ns=6;s=P_JY_QWB2_OUTPUT"]
["泵坑潜污泵2运行","ns=6;s=P_JY_QWB2_RFB"]
["杀菌剂加药泵故障","ns=6;s=P_JY_SJJ_FAULT"]
["杀菌剂加药泵运行","ns=6;s=P_JY_SJJ_RFB"]
["塑料泵故障","ns=6;s=P_JY_SLB_FAULT"]
["塑料泵运行","ns=6;s=P_JY_SLB_RFB"]
["外供水碱加药泵1故障","ns=6;s=P_JY_WGSJ1_FAULT"]
["外供水碱加药泵1启动","ns=6;s=P_JY_WGSJ1_OUTPUT"]
["外供水碱加药泵1运行","ns=6;s=P_JY_WGSJ1_RFB"]
["外供水碱加药泵2故障","ns=6;s=P_JY_WGSJ2_FAULT"]
["外供水碱加药泵2启动","ns=6;s=P_JY_WGSJ2_OUTPUT"]
["外供水碱加药泵2运行","ns=6;s=P_JY_WGSJ2_RFB"]
["阻垢剂加药泵故障","ns=6;s=P_JY_ZGJ_FAULT"]
["阻垢剂加药泵运行","ns=6;s=P_JY_ZGJ_RFB"]
["反渗透段间泵故障","ns=6;s=P_RO_DJB_FAULT"]
["反渗透段间泵运行","ns=6;s=P_RO_DJB_RFB"]
["反渗透供水泵故障","ns=6;s=P_RO_GSB_FAULT"]
["反渗透供水泵运行","ns=6;s=P_RO_GSB_RFB"]
["反渗透高压泵故障","ns=6;s=P_RO_GYB_FAULT"]
["反渗透高压泵运行","ns=6;s=P_RO_GYB_RFB"]
["超滤产水泵故障","ns=6;s=P_UF_CSB_FAULT"]
["超滤产水泵运行","ns=6;s=P_UF_CSB_RFB"]
["超滤反洗泵故障","ns=6;s=P_UF_FXB_FAULT"]
["超滤反洗泵运行","ns=6;s=P_UF_FXB_RFB"]
["UF供水泵1故障","ns=6;s=P_UF_GSB1_FAULT"]
["UF供水泵1启动","ns=6;s=P_UF_GSB1_OUTPUT"]
["UF供水泵1运行","ns=6;s=P_UF_GSB1_RFB"]
["UF供水泵2故障","ns=6;s=P_UF_GSB2_FAULT"]
["UF供水泵2启动","ns=6;s=P_UF_GSB2_OUTPUT"]
["UF供水泵2运行","ns=6;s=P_UF_GSB2_RFB"]
["超滤排空泵故障","ns=6;s=P_UF_PKB_FAULT"]
["超滤排空泵运行","ns=6;s=P_UF_PKB_RFB"]
["超滤提升泵1故障","ns=6;s=P_UF_TSB1_FAULT"]
["超滤提升泵1启动","ns=6;s=P_UF_TSB1_OUTPUT"]
["超滤提升泵1运行","ns=6;s=P_UF_TSB1_RFB"]
["超滤提升泵2故障","ns=6;s=P_UF_TSB2_FAULT"]
["超滤提升泵2启动","ns=6;s=P_UF_TSB2_OUTPUT"]
["超滤提升泵2运行","ns=6;s=P_UF_TSB2_RFB"]
["RO_19_ERR","ns=6;s=RO_19_ERR"]
["RO_20_ERR","ns=6;s=RO_20_ERR"]
["RO_21_ERR","ns=6;s=RO_21_ERR"]
["RO_22_ERR","ns=6;s=RO_22_ERR"]
["RO_23_ERR","ns=6;s=RO_23_ERR"]
["RO_24_ERR","ns=6;s=RO_24_ERR"]
["RO_25_ERR","ns=6;s=RO_25_ERR"]
["RO_26_ERR","ns=6;s=RO_26_ERR"]
["RO_27_ERR","ns=6;s=RO_27_ERR"]
["RO_28_ERR","ns=6;s=RO_28_ERR"]
["RO_29_ERR","ns=6;s=RO_29_ERR"]
["RO_30_ERR","ns=6;s=RO_30_ERR"]
["RO_31_ERR","ns=6;s=RO_31_ERR"]
["RO_32_ERR","ns=6;s=RO_32_ERR"]
["启动冲洗泵","ns=6;s=RO_APPLY_CXB_ON"]
["启动段间泵","ns=6;s=RO_APPLY_DJB_ON"]
["启用供水泵","ns=6;s=RO_APPLY_GSB_ON"]
["启动还原剂","ns=6;s=RO_APPLY_HYJ_ON"]
["启动杀菌剂","ns=6;s=RO_APPLY_SJJ_ON"]
["启动出水排气阀","ns=6;s=RO_APPLY_V_CSPQ"]
["启动进水排气阀","ns=6;s=RO_APPLY_V_JSPQ"]
["启动浓水排气阀","ns=6;s=RO_APPLY_V_NSPQ"]
["启动阻垢剂","ns=6;s=RO_APPLY_ZGJ_ON"]
["启用增压泵","ns=6;s=RO_APPLY_ZYB_ON"]
["RO_APPLY1","ns=6;s=RO_APPLY1"]
["RO_APPLY2","ns=6;s=RO_APPLY2"]
["RO_APPLY20","ns=6;s=RO_APPLY20"]
["RO_APPLY24","ns=6;s=RO_APPLY24"]
["RO_APPLY25","ns=6;s=RO_APPLY25"]
["RO_APPLY26","ns=6;s=RO_APPLY26"]
["RO_APPLY27","ns=6;s=RO_APPLY27"]
["RO_APPLY28","ns=6;s=RO_APPLY28"]
["RO_APPLY29","ns=6;s=RO_APPLY29"]
["RO_APPLY3","ns=6;s=RO_APPLY3"]
["RO_APPLY30","ns=6;s=RO_APPLY30"]
["RO_APPLY31","ns=6;s=RO_APPLY31"]
["RO_APPLY4","ns=6;s=RO_APPLY4"]
["RO_APPLY5","ns=6;s=RO_APPLY5"]
["RO_APPLY6","ns=6;s=RO_APPLY6"]
["RO_APPLY7","ns=6;s=RO_APPLY7"]
["RO_APPLY8","ns=6;s=RO_APPLY8"]
["RO_BTN_10","ns=6;s=RO_BTN_10"]
["RO_BTN_11","ns=6;s=RO_BTN_11"]
["RO_BTN_20","ns=6;s=RO_BTN_20"]
["RO_BTN_22","ns=6;s=RO_BTN_22"]
["RO_BTN_23","ns=6;s=RO_BTN_23"]
["RO_BTN_24","ns=6;s=RO_BTN_24"]
["RO_BTN_25","ns=6;s=RO_BTN_25"]
["RO_BTN_26","ns=6;s=RO_BTN_26"]
["RO_BTN_27","ns=6;s=RO_BTN_27"]
["RO_BTN_28","ns=6;s=RO_BTN_28"]
["RO_BTN_29","ns=6;s=RO_BTN_29"]
["RO_BTN_30","ns=6;s=RO_BTN_30"]
["RO_BTN_31","ns=6;s=RO_BTN_31"]
["RO_BTN_5","ns=6;s=RO_BTN_5"]
["RO_BTN_6","ns=6;s=RO_BTN_6"]
["RO_BTN_7","ns=6;s=RO_BTN_7"]
["半自动：反洗（脉冲）","ns=6;s=RO_BTN_CX"]
["急停","ns=6;s=RO_BTN_EMG"]
["初始化","ns=6;s=RO_BTN_INITIAL"]
["累计流量清零","ns=6;s=RO_BTN_LJLL_CLEAR"]
["半自动：CEB（脉冲）","ns=6;s=RO_BTN_SJX"]
["半自动：开机 (置位)","ns=6;s=RO_BTN_START"]
["全自动：投运/停机","ns=6;s=RO_BTN_TY"]
["仪表屏蔽","ns=6;s=RO_BTN_YBDIS"]
["阀门自动","ns=6;s=RO_BTN_YVS_AUTO"]
["ERR_电导率H","ns=6;s=RO_DDL_H_ERR"]
["ERR_电导率HH","ns=6;s=RO_DDL_HH_ERR"]
["ERR_膜内有药","ns=6;s=RO_MNYY_ERR"]
["段间泵出口压力高","ns=6;s=RO_PDJB_CK_H"]
["段间泵进口压力低","ns=6;s=RO_PDJB_JK_L"]
["ERR_水泵故障","ns=6;s=RO_PUMP_ERR"]
["增压泵出口压力高","ns=6;s=RO_PZYB_CK_H"]
["增压泵进口压力低","ns=6;s=RO_PZYB_JK_L"]
["ERR_系统故障","ns=6;s=RO_SYSTEM_ERR"]
["ERR_压差I_H","ns=6;s=RO_TMP1_H_ERR"]
["ERR_压差I_HH","ns=6;s=RO_TMP1_HH_ERR"]
["ERR_压差II_H","ns=6;s=RO_TMP2_H_ERR"]
["ERR_压差II_HH","ns=6;s=RO_TMP2_HH_ERR"]
["ERR_压差III_H","ns=6;s=RO_TMP3_H_ERR"]
["ERR_压差III_HH","ns=6;s=RO_TMP3_HH_ERR"]
["ERR_压差高故障","ns=6;s=RO_TMPHH_ERR"]
["ERR_仪表故障","ns=6;s=RO_YB_ERR"]
["ERR_阀门故障","ns=6;s=RO_YV_ERR"]
["系统故障","ns=6;s=SYSTEM_ERR"]
["压差H","ns=6;s=TMP_H_ERR"]
["压差HH","ns=6;s=TMP_HH_ERR"]
["APPLY_13","ns=6;s=UF_APPLY_13"]
["APPLY_14","ns=6;s=UF_APPLY_14"]
["APPLY_15","ns=6;s=UF_APPLY_15"]
["Apply_9","ns=6;s=UF_APPLY_9"]
["Apply_次钠加药","ns=6;s=UF_APPLY_CNJY"]
["Apply反洗泵BW","ns=6;s=UF_APPLY_FXB_BW"]
["Apply反洗泵CEB","ns=6;s=UF_APPLY_FXB_CEB"]
["Apply公共阀BW阀","ns=6;s=UF_APPLY_GGF_BWV"]
["Apply公共阀CEB阀","ns=6;s=UF_APPLY_GGF_CEBV"]
["Apply供水泵FW","ns=6;s=UF_APPLY_GSB_FW"]
["Apply_碱加药","ns=6;s=UF_APPLY_JJY"]
["Apply_PAC加药","ns=6;s=UF_APPLY_PACJY"]
["Apply_酸加药","ns=6;s=UF_APPLY_SJY"]
["Apply提升泵1","ns=6;s=UF_APPLY_TSB1"]
["Apply提升泵2","ns=6;s=UF_APPLY_TSB2"]
["UF_BTN_12","ns=6;s=UF_BTN_12"]
["UF_BTN_13","ns=6;s=UF_BTN_13"]
["UF_BTN_14","ns=6;s=UF_BTN_14"]
["UF_BTN_15","ns=6;s=UF_BTN_15"]
["UF_BTN_16","ns=6;s=UF_BTN_16"]
["UF_BTN_20","ns=6;s=UF_BTN_20"]
["UF_BTN_21","ns=6;s=UF_BTN_21"]
["UF_BTN_22","ns=6;s=UF_BTN_22"]
["UF_BTN_23","ns=6;s=UF_BTN_23"]
["半自动：反洗（脉冲）","ns=6;s=UF_BTN_CX"]
["急停","ns=6;s=UF_BTN_EMG"]
["初始化","ns=6;s=UF_BTN_INITIAL"]
["累计流量清零","ns=6;s=UF_BTN_LL_CLEAR"]
["气擦洗屏蔽","ns=6;s=UF_BTN_QCXDIS"]
["半自动：CEB（脉冲）","ns=6;s=UF_BTN_SJX"]
["半自动：开机 (置位)","ns=6;s=UF_BTN_START"]
["全自动：投运/停机","ns=6;s=UF_BTN_TY"]
["药剂残留","ns=6;s=UF_DRUG_ERR"]
["ERR_5","ns=6;s=UF_ERR_5"]
["ERR_6","ns=6;s=UF_ERR_6"]
["ERR_7","ns=6;s=UF_ERR_7"]
["产水池A连锁","ns=6;s=UF_FLAG_LS_CSCA"]
["产水池B连锁","ns=6;s=UF_FLAG_LS_CSCB"]
["进水池A连锁","ns=6;s=UF_FLAG_LS_JSCA"]
["进水池B连锁","ns=6;s=UF_FLAG_LS_JSCB"]
["系统故障","ns=6;s=UF_SYSTEM_ERR"]
["压差H","ns=6;s=UF_TMP_H_ERR"]
["压差HH","ns=6;s=UF_TMP_HH_ERR"]
["膜组阀门故障","ns=6;s=UF_VALVE_ERR"]
["加药间CIP补水阀故障","ns=6;s=V_JY_CIPBS_ERR"]
["加药间CIP补水阀总故障","ns=6;s=V_JY_CIPBS_ERRT"]
["加药间CIP排放阀故障","ns=6;s=V_JY_CIPPF_ERR"]
["加药间CIP排放阀总故障","ns=6;s=V_JY_CIPPF_ERRT"]
["RO产水箱补水阀故障","ns=6;s=V_JY_CSBS_ERR"]
["RO产水箱补水阀总故障","ns=6;s=V_JY_CSBS_ERRT"]
["加药间冲洗阀故障","ns=6;s=V_JY_CX_ERR"]
["加药间冲洗阀总故障","ns=6;s=V_JY_CX_ERRT"]
["UF废水外排阀故障","ns=6;s=V_JY_UFFS_ERR"]
["UF废水外排阀总故障","ns=6;s=V_JY_UFFS_ERRT"]
["RO外供水阀故障","ns=6;s=V_JY_WG_ERR"]
["RO外供水阀总故障","ns=6;s=V_JY_WG_ERRT"]
["加药间外供碱阀故障","ns=6;s=V_JY_WGJ_ERR"]
["加药间外供碱阀总故障","ns=6;s=V_JY_WGJ_ERRT"]
["RO不合格水阀故障","ns=6;s=V_RO_BHGF_ERR"]
["RO不合格水阀总故障","ns=6;s=V_RO_BHGF_ERRT"]
["RO生化进水阀故障","ns=6;s=V_RO_BYF1_ERR"]
["RO生化进水阀总故障","ns=6;s=V_RO_BYF1_ERRT"]
["RO产水阀故障","ns=6;s=V_RO_CSF_ERR"]
["RO产水阀总故障","ns=6;s=V_RO_CSF_ERRT"]
["RO冲洗进水阀故障","ns=6;s=V_RO_CXJSF_ERR"]
["RO冲洗进水阀总故障","ns=6;s=V_RO_CXJSF_ERRT"]
["RO冲洗排水阀故障","ns=6;s=V_RO_CXPSF_ERR"]
["RO冲洗排水阀总故障","ns=6;s=V_RO_CXPSF_ERRT"]
["RO一段反洗进水阀故障","ns=6;s=V_RO_FJSF_ERR"]
["RO一段反洗进水阀总故障","ns=6;s=V_RO_FJSF_ERRT"]
["RO一段反洗排水阀故障","ns=6;s=V_RO_FPSF_ERR"]
["RO一段反洗排水阀总故障","ns=6;s=V_RO_FPSF_ERRT"]
["RO还原剂阀故障","ns=6;s=V_RO_HYJF_ERR"]
["RO还原剂阀总故障","ns=6;s=V_RO_HYJF_ERRT"]
["RO进水阀故障","ns=6;s=V_RO_JSF_ERR"]
["RO进水阀总故障","ns=6;s=V_RO_JSF_ERRT"]
["RO排气阀1故障","ns=6;s=V_RO_PQF1_ERR"]
["RO排气阀1总故障","ns=6;s=V_RO_PQF1_ERRT"]
["RO排气阀2故障","ns=6;s=V_RO_PQF2_ERR"]
["RO排气阀2总故障","ns=6;s=V_RO_PQF2_ERRT"]
["RO排气阀3故障","ns=6;s=V_RO_PQF3_ERR"]
["RO排气阀3总故障","ns=6;s=V_RO_PQF3_ERRT"]
["RO排气阀4故障","ns=6;s=V_RO_PQF4_ERR"]
["RO排气阀4总故障","ns=6;s=V_RO_PQF4_ERRT"]
["RO排气阀5故障","ns=6;s=V_RO_PQF5_ERR"]
["RO排气阀5总故障","ns=6;s=V_RO_PQF5_ERRT"]
["RO排气阀6故障","ns=6;s=V_RO_PQF6_ERR"]
["RO排气阀6总故障","ns=6;s=V_RO_PQF6_ERRT"]
["RO排气阀7故障","ns=6;s=V_RO_PQF7_ERR"]
["RO排气阀7总故障","ns=6;s=V_RO_PQF7_ERRT"]
["RO排气阀8故障","ns=6;s=V_RO_PQF8_ERR"]
["RO排气阀8总故障","ns=6;s=V_RO_PQF8_ERRT"]
["RO排气阀9故障","ns=6;s=V_RO_PQF9_ERR"]
["RO排气阀9总故障","ns=6;s=V_RO_PQF9_ERRT"]
["RO杀菌剂阀故障","ns=6;s=V_RO_SJJF_ERR"]
["RO杀菌剂阀总故障","ns=6;s=V_RO_SJJF_ERRT"]
["RO阻垢剂阀故障","ns=6;s=V_RO_ZGJF_ERR"]
["RO阻垢剂阀总故障","ns=6;s=V_RO_ZGJF_ERRT"]
["UF曝气阀故障","ns=6;s=V_UF_BQF_ERR"]
["UF曝气阀总故障","ns=6;s=V_UF_BQF_ERRT"]
["UF产水阀故障","ns=6;s=V_UF_CSF_ERR"]
["UF产水阀总故障","ns=6;s=V_UF_CSF_ERRT"]
["UF反洗阀故障","ns=6;s=V_UF_FXF_ERR"]
["UF反洗阀总故障","ns=6;s=V_UF_FXF_ERRT"]
["UF还原阀故障","ns=6;s=V_UF_HYF_ERR"]
["UF还原阀总故障","ns=6;s=V_UF_HYF_ERRT"]
["UF进水阀故障","ns=6;s=V_UF_JSF_ERR"]
["UF进水阀总故障","ns=6;s=V_UF_JSF_ERRT"]
["UF排空阀故障","ns=6;s=V_UF_PKF_ERR"]
["UF排空阀总故障","ns=6;s=V_UF_PKF_ERRT"]
["UF水射器电磁阀故障","ns=6;s=V_UF_SSQF_ERR"]
["UF水射器电磁阀总故障","ns=6;s=V_UF_SSQF_ERRT"]
["UF中和外排阀故障","ns=6;s=V_UF_ZHWPF_ERR"]
["UF中和外排阀总故障","ns=6;s=V_UF_ZHWPF_ERRT"]
["膜组阀门故障","ns=6;s=VALVE_ERR"]
["空气流量计反馈","ns=3;s=AI_JYAIR_OUT"]
["空压机压变1反馈","ns=3;s=AI_JYAIRYL1_OUT"]
["空压机压变2反馈","ns=3;s=AI_JYAIRYL2_OUT"]
["反馈","ns=3;s=AI_JYBY1_OUT"]
["反馈","ns=3;s=AI_JYBY2_OUT"]
["CIP泵频率反馈","ns=3;s=AI_JYCIPB_FR_OUT"]
["CIPph反馈","ns=3;s=AI_JYCIPPH_OUT"]
["cip清洗流量计反馈","ns=3;s=AI_JYCIPQXLL_OUT"]
["次钠液位反馈","ns=3;s=AI_JYCNYW_OUT"]
["外供水电导反馈","ns=3;s=AI_JYCSDD_OUT"]
["产水流量计1反馈","ns=3;s=AI_JYCSLL1_OUT"]
["产水流量计2反馈","ns=3;s=AI_JYCSLL2_OUT"]
["外供水PH反馈","ns=3;s=AI_JYCSPH_OUT"]
["产水温度反馈","ns=3;s=AI_JYCSWD_OUT"]
["产水压力变送器反馈","ns=3;s=AI_JYCSYL_OUT"]
["反洗风机频率反馈","ns=3;s=AI_JYFJ_FR_OUT"]
["还原剂液位反馈","ns=3;s=AI_JYHYJYW_OUT"]
["高级生物进水流量计反馈","ns=3;s=AI_JYJSLL1_OUT"]
["Y2B进水流量计反馈","ns=3;s=AI_JYJSLL2_OUT"]
["碱液位反馈","ns=3;s=AI_JYJYW_OUT"]
["清洗水箱液位计反馈","ns=3;s=AI_JYQXSXYW_OUT"]
["反渗透产水液位计反馈","ns=3;s=AI_JYROCSYW_OUT"]
["杀菌剂液位反馈","ns=3;s=AI_JYSJJYW_OUT"]
["酸液位反馈","ns=3;s=AI_JYSYW_OUT"]
["超滤产水液位计反馈","ns=3;s=AI_JYUFCSYW_OUT"]
["超滤提升泵液位计反馈","ns=3;s=AI_JYUFTSBYW_OUT"]
["尾水排放流量计反馈","ns=3;s=AI_JYWSLL_OUT"]
["阻垢剂液位反馈","ns=3;s=AI_JYZGJYW_OUT"]
["二段产水流量反馈","ns=3;s=AI_RO2DCSLL_OUT"]
["产水电导反馈","ns=3;s=AI_ROCSDD_OUT"]
["产水压力反馈","ns=3;s=AI_ROCSYL_OUT"]
["RO段间泵频率反馈","ns=3;s=AI_RODJB_FR_OUT"]
["段间泵进口压力反馈","ns=3;s=AI_RODJJKYL_OUT"]
["段间压力反馈","ns=3;s=AI_RODJYL_OUT"]
["RO供水泵频率反馈","ns=3;s=AI_ROGSB_FR_OUT"]
["RO高压泵频率反馈","ns=3;s=AI_ROGYB_FR_OUT"]
["进水电导反馈","ns=3;s=AI_ROJSDD_OUT"]
["进水流量反馈","ns=3;s=AI_ROJSLL_OUT"]
["进水ORP反馈","ns=3;s=AI_ROJSORP_OUT"]
["进水PH反馈","ns=3;s=AI_ROJSPH_OUT"]
["进水压力反馈","ns=3;s=AI_ROJSYL_OUT"]
["浓水流量反馈","ns=3;s=AI_RONSLL_OUT"]
["浓水压力反馈","ns=3;s=AI_RONSYL_OUT"]
["空压机流量反馈","ns=3;s=AI_UFAIR_OUT"]
["UF产水泵频率反馈","ns=3;s=AI_UFCSB_FR_OUT"]
["UF产水流量反馈","ns=3;s=AI_UFCSLL_OUT"]
["UF产水压力反馈","ns=3;s=AI_UFCSYL_OUT"]
["UF产水浊度反馈","ns=3;s=AI_UFCSZD_OUT"]
["UF反洗泵频率反馈","ns=3;s=AI_UFFXB_FR_OUT"]
["UF反洗流量反馈","ns=3;s=AI_UFFXLL_OUT"]
["UF进水ORP反馈","ns=3;s=AI_UFJSORP_OUT"]
["UF进水ph反馈","ns=3;s=AI_UFJSPH_OUT"]
["UF进水温度反馈","ns=3;s=AI_UFJSYW_OUT"]
["UF进水浊度反馈","ns=3;s=AI_UFJSZD_OUT"]
["UF膜堆液位反馈","ns=3;s=AI_UFMDYW_OUT"]
["UF排空泵频率反馈","ns=3;s=AI_UFPKB_FR_OUT"]
["UF提升泵1频率反馈","ns=3;s=AI_UFTSB1_FR_OUT"]
["UF提升泵2频率反馈","ns=3;s=AI_UFTSB2_FR_OUT"]
["真空管液位反馈","ns=3;s=AI_UFZKGYW_OUT"]
["中和水箱液位高高限值","ns=3;s=ALARM_ZHSX_HHR"]
["中和水箱液位高限值","ns=3;s=ALARM_ZHSX_HR"]
["中和水箱液位","ns=3;s=ALARM_ZHSX_IN"]
["中和水箱液位低低限值","ns=3;s=ALARM_ZHSX_LLR"]
["中和水箱液位低限值","ns=3;s=ALARM_ZHSX_LR"]
["加热器1频率反馈","ns=3;s=JBQ_JY_JRQ1_FRE_FB"]
["加热器1运行时间","ns=3;s=JBQ_JY_JRQ1_RUNTIME"]
["加热器2频率反馈","ns=3;s=JBQ_JY_JRQ2_FRE_FB"]
["加热器2运行时间","ns=3;s=JBQ_JY_JRQ2_RUNTIME"]
["CEB还原剂加药泵1频率反馈","ns=3;s=P_CEB_HYJ1_FRE_FB"]
["CEB还原剂加药泵1运行时间","ns=3;s=P_CEB_HYJ1_RUNTIME"]
["CEB还原剂加药泵2频率反馈","ns=3;s=P_CEB_HYJ2_FRE_FB"]
["CEB还原剂加药泵2运行时间","ns=3;s=P_CEB_HYJ2_RUNTIME"]
["CIP泵频率反馈","ns=3;s=P_JY_CIPB_FRE_FB"]
["CIP泵运行时间","ns=3;s=P_JY_CIPB_RUNTIME"]
["次钠加药泵1频率反馈","ns=3;s=P_JY_CN1_FRE_FB"]
["次钠加药泵1运行时间","ns=3;s=P_JY_CN1_RUNTIME"]
["次钠加药泵2频率反馈","ns=3;s=P_JY_CN2_FRE_FB"]
["次钠加药泵2运行时间","ns=3;s=P_JY_CN2_RUNTIME"]
["反洗风机频率反馈","ns=3;s=P_JY_FX_FJ_FRE_FB"]
["反洗风机运行时间","ns=3;s=P_JY_FX_FJ_RUNTIME"]
["还原剂加药泵频率反馈","ns=3;s=P_JY_HYJ_FRE_FB"]
["还原剂加药泵运行时间","ns=3;s=P_JY_HYJ_RUNTIME"]
["碱加药泵1频率反馈","ns=3;s=P_JY_JJ1_FRE_FB"]
["碱加药泵1运行时间","ns=3;s=P_JY_JJ1_RUNTIME"]
["碱加药泵2频率反馈","ns=3;s=P_JY_JJ2_FRE_FB"]
["碱加药泵2运行时间","ns=3;s=P_JY_JJ2_RUNTIME"]
["酸加药泵1频率反馈","ns=3;s=P_JY_JS1_FRE_FB"]
["酸加药泵1运行时间","ns=3;s=P_JY_JS1_RUNTIME"]
["酸加药泵2频率反馈","ns=3;s=P_JY_JS2_FRE_FB"]
["酸加药泵2运行时间","ns=3;s=P_JY_JS2_RUNTIME"]
["潜污泵1频率反馈","ns=3;s=P_JY_QWB1_FRE_FB"]
["潜污泵1运行时间","ns=3;s=P_JY_QWB1_RUNTIME"]
["潜污泵2频率反馈","ns=3;s=P_JY_QWB2_FRE_FB"]
["潜污泵2运行时间","ns=3;s=P_JY_QWB2_RUNTIME"]
["杀菌剂加药泵频率反馈","ns=3;s=P_JY_SJJ_FRE_FB"]
["杀菌剂加药泵运行时间","ns=3;s=P_JY_SJJ_RUNTIME"]
["塑料泵频率反馈","ns=3;s=P_JY_SLB_FRE_FB"]
["塑料泵运行时间","ns=3;s=P_JY_SLB_RUNTIME"]
["外供水碱加药泵1频率反馈","ns=3;s=P_JY_WGSJ1_FRE_FB"]
["外供水碱加药泵1运行时间","ns=3;s=P_JY_WGSJ1_RUNTIME"]
["外供水碱加药泵2频率反馈","ns=3;s=P_JY_WGSJ2_FRE_FB"]
["外供水碱加药泵2运行时间","ns=3;s=P_JY_WGSJ2_RUNTIME"]
["阻垢剂加药泵频率反馈","ns=3;s=P_JY_ZGJ_FRE_FB"]
["阻垢剂加药泵运行时间","ns=3;s=P_JY_ZGJ_RUNTIME"]
["RO段间泵频率反馈","ns=3;s=P_RO_DJB_FRE_FB"]
["RO段间泵运行时间","ns=3;s=P_RO_DJB_RUNTIME"]
["RO供水泵频率反馈","ns=3;s=P_RO_GSB_FRE_FB"]
["RO供水泵运行时间","ns=3;s=P_RO_GSB_RUNTIME"]
["RO高压泵频率反馈","ns=3;s=P_RO_GYB_FRE_FB"]
["RO高压泵运行时间","ns=3;s=P_RO_GYB_RUNTIME"]
["UF产水泵频率反馈","ns=3;s=P_UF_CSB_FRE_FB"]
["UF产水泵运行时间","ns=3;s=P_UF_CSB_RUNTIME"]
["UF反洗泵频率反馈","ns=3;s=P_UF_FXB_FRE_FB"]
["UF反洗泵运行时间","ns=3;s=P_UF_FXB_RUNTIME"]
["UF供水泵1频率反馈","ns=3;s=P_UF_GSB1_FRE_FB"]
["UF供水泵1运行时间","ns=3;s=P_UF_GSB1_RUNTIME"]
["UF供水泵2频率反馈","ns=3;s=P_UF_GSB2_FRE_FB"]
["UF供水泵2运行时间","ns=3;s=P_UF_GSB2_RUNTIME"]
["UF排空泵频率反馈","ns=3;s=P_UF_PKB_FRE_FB"]
["UF排空泵运行时间","ns=3;s=P_UF_PKB_RUNTIME"]
["UF提升泵1频率反馈","ns=3;s=P_UF_TSB1_FRE_FB"]
["UF提升泵1运行时间","ns=3;s=P_UF_TSB1_RUNTIME"]
["UF提升泵2频率反馈","ns=3;s=P_UF_TSB2_FRE_FB"]
["UF提升泵2运行时间","ns=3;s=P_UF_TSB2_RUNTIME"]
["SSD_Press_12dj","ns=3;s=RO_12DJYL_SSD"]
["SSD_Flow_1dcs","ns=3;s=RO_1DCSLL_SSD"]
["SSD_Flow_1djs","ns=3;s=RO_1DJSLL_SSD"]
["SSD_Press_23dj","ns=3;s=RO_23DJYL_SSD"]
["SSD_Flow_2dcs","ns=3;s=RO_2DCSLL_SSD"]
["SSD_Flow_2djs","ns=3;s=RO_2DJSLL_SSD"]
["SSD_Flow_3dcs","ns=3;s=RO_3DCSLL_SSD"]
["SSD_Flow_3djs","ns=3;s=RO_3DJSLL_SSD"]
["反洗码","ns=3;s=RO_BW_CODE"]
["SSD_Press_by","ns=3;s=RO_BYYL_SSD"]
["CEB码","ns=3;s=RO_CEB_CODE"]
["SSD_PressCha1","ns=3;s=RO_CHA1YL_SSD"]
["SSD_PressCha2","ns=3;s=RO_CHA2YL_SSD"]
["SSD_PressCha3","ns=3;s=RO_CHA3YL_SSD"]
["SSD_产水率","ns=3;s=RO_CS_RATE_SSD"]
["Set充水时间","ns=3;s=RO_CS_TIME_SET"]
["SSD_csddl","ns=3;s=RO_CSDDL_SSD"]
["SSD_产水量累计Dint","ns=3;s=RO_CSLJ_OUT"]
["SSD_产水量累计","ns=3;s=RO_CSLJ_SSD"]
["Set充水时排气时间","ns=3;s=RO_CSPQ_TIME_SET"]
["SSD_Press_cs","ns=3;s=RO_CSYL_SSD"]
["提示","ns=3;s=RO_CUE"]
["Set冲洗时间","ns=3;s=RO_CX_TIME_SET"]
["SSD_冲洗量累计","ns=3;s=RO_CXLJ_SSD"]
["SSD_冲洗流量","ns=3;s=RO_CXLL_SSD"]
["Set_ddl_HR","ns=3;s=RO_DDL_H_SET"]
["Set_ddl_HHR","ns=3;s=RO_DDL_HH_SET"]
["HZ_Pdjb_HH","ns=3;s=RO_DJB_FRE_HH_SET"]
["HZ_Pdjb_LL","ns=3;s=RO_DJB_FRE_LL_SET"]
["HZ_Pdjb_PIDOut","ns=3;s=RO_DJB_FRE_PID_OUT"]
["OUT_段间泵流量Need","ns=3;s=RO_DJBLL_NEED_OUT"]
["Set_段间泵过滤流量","ns=3;s=RO_DJGLLL_SET"]
["报错","ns=3;s=RO_FAULT"]
["Set反洗时间I","ns=3;s=RO_FX1_TIME_SET"]
["Set反洗时间II","ns=3;s=RO_FX2_TIME_SET"]
["Set反洗时间III","ns=3;s=RO_FX3_TIME_SET"]
["OUT_过滤时间","ns=3;s=RO_GL_TIME_OUT"]
["Set过滤时间","ns=3;s=RO_GL_TIME_SET"]
["Out_过滤次数","ns=3;s=RO_GL_TIMES_OUT"]
["HZ_Pgyb_HH","ns=3;s=RO_GYB_FRE_HH_SET"]
["HZ_Pgyb_LL","ns=3;s=RO_GYB_FRE_LL_SET"]
["HZ_Pdjb_ManSet","ns=3;s=RO_GYB_FRE_MANSET"]
["HZ_Pgyb_PIDOut","ns=3;s=RO_GYB_FRE_PID_OUT"]
["Out_故障时间","ns=3;s=RO_GZ_TIME_OUT"]
["SSD_jsddl","ns=3;s=RO_JSDDL_SSD"]
["OUT_进水流量need","ns=3;s=RO_JSLL_NEED_OUT"]
["SSD_Press_js","ns=3;s=RO_JSYL_SSD"]
["Set_开机冲洗流量","ns=3;s=RO_KJCXLL_SET"]
["模式","ns=3;s=RO_MODE"]
["SSD_Flow_ns","ns=3;s=RO_NS_SSD"]
["SSD_Flow_nshl","ns=3;s=RO_NSH1_SSD"]
["SSD_Press_ns","ns=3;s=RO_NSYL_SSD"]
["Out_12","ns=3;s=RO_OUT_12"]
["Out_13","ns=3;s=RO_OUT_13"]
["Out_14","ns=3;s=RO_OUT_14"]
["Out_15","ns=3;s=RO_OUT_15"]
["Out_16","ns=3;s=RO_OUT_16"]
["Out_17","ns=3;s=RO_OUT_17"]
["Out_20","ns=3;s=RO_OUT_20"]
["Set_PressPump_ck_H","ns=3;s=RO_P_CK_H_SET"]
["Set_PressPump_jk_L","ns=3;s=RO_P_JK_L_SET"]
["Set_排气时间1","ns=3;s=RO_PQ1_TIME_SET"]
["Set_排气时间2","ns=3;s=RO_PQ2_TIME_SET"]
["Set_排气时间3","ns=3;s=RO_PQ3_TIME_SET"]
["Set_排气时间4","ns=3;s=RO_PQ4_TIME_SET"]
["Set_排气时间5","ns=3;s=RO_PQ5_TIME_SET"]
["Set_排气时间6","ns=3;s=RO_PQ6_TIME_SET"]
["Set_R16","ns=3;s=RO_SET16"]
["Set杀菌冲洗时间","ns=3;s=RO_SJCX_TIME_SET"]
["Set_杀菌冲洗流量","ns=3;s=RO_SJCXLL_SET"]
["Set杀菌浸泡时间","ns=3;s=RO_SJJP_TIME_SET"]
["Set杀菌加药时间","ns=3;s=RO_SJJY_TIME_SET"]
["Set_杀菌加药流量","ns=3;s=RO_SJJYLL_SET"]
["步序","ns=3;s=RO_STEP"]
["Out_系统时间","ns=3;s=RO_SYSTEM_TIME_OUT"]
["Set_压差I_H","ns=3;s=RO_TMP1H_SET"]
["Set_压差I_HH","ns=3;s=RO_TMP1HH_SET"]
["Set_压差II_H","ns=3;s=RO_TMP2H_SET"]
["Set_压差II_HH","ns=3;s=RO_TMP2HH_SET"]
["Set_压差III_H","ns=3;s=RO_TMP3H_SET"]
["Set_压差III_HH","ns=3;s=RO_TMP3HH_SET"]
["SSD_脱盐率","ns=3;s=RO_TYL_SSD"]
["ZBY_R10","ns=3;s=RO_ZBY_R10"]
["ZBY_R11","ns=3;s=RO_ZBY_R11"]
["ZBY_R12","ns=3;s=RO_ZBY_R12"]
["ZBY_R14","ns=3;s=RO_ZBY_R14"]
["ZBY_R15","ns=3;s=RO_ZBY_R15"]
["ZBY_R16","ns=3;s=RO_ZBY_R16"]
["ZBY_R17","ns=3;s=RO_ZBY_R17"]
["ZBY_R5","ns=3;s=RO_ZBY_R5"]
["ZBY_R6","ns=3;s=RO_ZBY_R6"]
["ZBY_R7","ns=3;s=RO_ZBY_R7"]
["ZBY_R8","ns=3;s=RO_ZBY_R8"]
["SSD_Flow_zcs","ns=3;s=RO_ZCS_SSD"]
["OUT_增压泵流量Need","ns=3;s=RO_ZYBLL_NEED_OUT"]
["Set_增压泵过滤流量","ns=3;s=RO_ZYGLLL_SET"]
["0ut_动作时间","ns=3;s=UF_ACTION_TIME_OUT"]
["UF_BWCODE","ns=3;s=UF_BWCODE"]
["Out_反洗用水累计","ns=3;s=UF_BWLJ_FLOW"]
["Set反洗流量","ns=3;s=UF_BWLL_SET"]
["UF_CEBCODE","ns=3;s=UF_CEBCODE"]
["CEB碱洗冲洗时间1","ns=3;s=UF_CEBJCX1_TIME_SET"]
["CEB碱洗冲洗时间2","ns=3;s=UF_CEBJCX2_TIME_SET"]
["CEB碱洗浸泡时间","ns=3;s=UF_CEBJJP_TIME_SET"]
["CEB碱加药时间","ns=3;s=UF_CEBJJY_TIME_SET"]
["CEB碱气洗时间","ns=3;s=UF_CEBJX_TIME_SET"]
["SetCEB流量","ns=3;s=UF_CEBLL_SET"]
["CEB酸洗冲洗时间1","ns=3;s=UF_CEBSCX1_TIME_SET"]
["CEB酸洗冲洗时间2","ns=3;s=UF_CEBSCX2_TIME_SET"]
["CEB酸洗浸泡时间","ns=3;s=UF_CEBSJP_TIME_SET"]
["CEB酸加药时间","ns=3;s=UF_CEBSJY_TIME_SET"]
["CEB酸气洗时间","ns=3;s=UF_CEBSQX_TIME_SET"]
["SSDCIP清洗流量计","ns=3;s=UF_CIPQX_FLOW"]
["SSD产水浊度","ns=3;s=UF_CS_NTU"]
["SSD产水压力","ns=3;s=UF_CS_PRESS"]
["提示关键字","ns=3;s=UF_CUE"]
["DInt_10","ns=3;s=UF_DINT10"]
["DInt_3","ns=3;s=UF_DINT3"]
["DInt_4","ns=3;s=UF_DINT4"]
["DInt_5","ns=3;s=UF_DINT5"]
["DInt_6","ns=3;s=UF_DINT6"]
["DInt_7","ns=3;s=UF_DINT7"]
["DInt_8","ns=3;s=UF_DINT8"]
["DInt_9","ns=3;s=UF_DINT9"]
["故障关键字","ns=3;s=UF_FAULT"]
["SSD反洗流量计","ns=3;s=UF_FX_FLOW"]
["Out_过滤时间","ns=3;s=UF_GL_TIME_OUT"]
["Set过滤时间","ns=3;s=UF_GL_TIME_SET"]
["Out_过滤次数","ns=3;s=UF_GL_TIMES_OUT"]
["Out_过滤总次数","ns=3;s=UF_GL_TTS_OUT"]
["Out_过滤产水累计","ns=3;s=UF_GLLJ_FLOW"]
["Set过滤流量","ns=3;s=UF_GLLL_SET"]
["Oot延时过滤次数","ns=3;s=UF_GLYS_TIMES_OUT"]
["Set延时过滤次数","ns=3;s=UF_GLYS_TIMES_SET"]
["Set后冲CEB时间1","ns=3;s=UF_HC1_TIME_SET"]
["Set后冲CEB时间2","ns=3;s=UF_HC2_TIME_SET"]
["Set后冲CEB气洗时间","ns=3;s=UF_HCQX_TIME_SET"]
["SSD进水流量计","ns=3;s=UF_JS_FLOW"]
["SSD进水压力","ns=3;s=UF_JS_PRESS"]
["SSD进水累计流量","ns=3;s=UF_JSLJ_FLOW"]
["膜组模式","ns=3;s=UF_MODE"]
["SSD气擦洗流量","ns=3;s=UF_QCX_FLOW"]
["Set气擦洗时间","ns=3;s=UF_QCX_TIME_SET"]
["UF_REAL1","ns=3;s=UF_REAL1"]
["UF_REAL10","ns=3;s=UF_REAL10"]
["UF_REAL11","ns=3;s=UF_REAL11"]
["UF_REAL12","ns=3;s=UF_REAL12"]
["UF_REAL2","ns=3;s=UF_REAL2"]
["UF_REAL3","ns=3;s=UF_REAL3"]
["UF_REAL4","ns=3;s=UF_REAL4"]
["UF_REAL5","ns=3;s=UF_REAL5"]
["UF_REAL6","ns=3;s=UF_REAL6"]
["UF_REAL7","ns=3;s=UF_REAL7"]
["UF_REAL8","ns=3;s=UF_REAL8"]
["UF_REAL9","ns=3;s=UF_REAL9"]
["UF_SET1","ns=3;s=UF_SET1"]
["UF_SET2","ns=3;s=UF_SET2"]
["UF_SET3","ns=3;s=UF_SET3"]
["步序关键字","ns=3;s=UF_STEP"]
["Out_系统时间","ns=3;s=UF_SYSTEM_TIME_OUT"]
["SSD调节阀开度","ns=3;s=UF_TJV_KD"]
["SSD跨膜压差","ns=3;s=UF_TMP"]
["Set压差HR","ns=3;s=UF_TMP_H_SET"]
["Set压差HHR","ns=3;s=UF_TMP_HH_SET"]
["Set水反洗时间1","ns=3;s=UF_WBW1_TIME_SET"]
["Set水反洗时间2","ns=3;s=UF_WBW2_TIME_SET"]
["Set正冲流量","ns=3;s=UF_ZCLL_SET"]
["废水收集槽高液位","ns=6;s=DI_JY_FQ_FS_H"]
["废水收集槽低液位","ns=6;s=DI_JY_FQ_FS_L"]
["T2B水池高液位","ns=6;s=DI_JY_FQ_T2B_H"]
["T2B水池低液位","ns=6;s=DI_JY_FQ_T2B_L"]
["1#空压机故障","ns=6;s=DI_JY_KYJ_1_ERR"]
["1#空压机运行","ns=6;s=DI_JY_KYJ_1_RUN"]
["1#空压机故障","ns=6;s=DI_JY_KYJ_2_ERR"]
["2#空压机运行","ns=6;s=DI_JY_KYJ_2_RUN"]
["膜池浮球_高液位","ns=6;s=DI_UF_YW_H"]
["膜池浮球_低液位","ns=6;s=DI_UF_YW_L"]
["RO产水流量累计1","ns=3;s=LJ_FLOW_ROCS1"]
["RO产水流量累计2","ns=3;s=LJ_FLOW_ROCS2"]
["RO冲洗流量累计","ns=3;s=LJ_FLOW_ROCX"]
["RO浓水水流量累计1","ns=3;s=LJ_FLOW_RONS1"]
["RO浓水水流量累计2","ns=3;s=LJ_FLOW_RONS2"]
["杀菌剂加药箱液位H","ns=6;s=DI_JY_SJJ_H"]
["杀菌剂加药箱液位L","ns=6;s=DI_JY_SJJ_L"]
["还原剂加药箱液位H","ns=6;s=DI_JY_HYJ_H"]
["还原剂加药箱液位L","ns=6;s=DI_JY_HYJ_L"]
["阻垢剂加药箱液位H","ns=6;s=DI_JY_ZGJ_H"]
["阻垢剂加药箱液位L","ns=6;s=DI_JY_ZGJ_L"]
["中和池高液位","ns=6;s=DI_JY_ZHCYW_H"]
["中和池低液位","ns=6;s=DI_JY_ZHCYW_L"]
["次钠加药箱液位H","ns=6;s=DI_JY_CN_H"]
["次钠加药箱液位L","ns=6;s=DI_JY_CN_L"]
["氢氧化钠加药箱液位H","ns=6;s=DI_JY_NAOH_H"]
["氢氧化钠加药箱液位L","ns=6;s=DI_JY_NAOH_L"]
["柠檬酸加药箱液位H","ns=6;s=DI_JY_NMS_H"]
["柠檬酸加药箱液位L","ns=6;s=DI_JY_NMS_L"]
["RO外供水池高液位","ns=6;s=DI_JY_ROWGSCYW_H"]
["RO外供水池低液位","ns=6;s=DI_JY_ROWGSCYW_L"]
["RO供水泵温度","ns=3;s=VB1_TEM"]
["RO供水泵X轴速度","ns=3;s=VB1_X_Z_SD"]
["RO供水泵X轴位移","ns=3;s=VB1_X_Z_WY"]
["RO供水泵Y轴速度","ns=3;s=VB1_Y_Z_SD"]
["RO供水泵Y轴位移","ns=3;s=VB1_Y_Z_WY"]
["RO供水泵Z轴速度","ns=3;s=VB1_Z_Z_SD"]
["RO供水泵Z轴位移","ns=3;s=VB1_Z_Z_WY"]
["RO段间泵温度","ns=3;s=VB2_TEM"]
["RO段间泵X轴速度","ns=3;s=VB2_X_Z_SD"]
["RO段间泵X轴位移","ns=3;s=VB2_X_Z_WY"]
["RO段间泵Y轴速度","ns=3;s=VB2_Y_Z_SD"]
["RO段间泵Y轴位移","ns=3;s=VB2_Y_Z_WY"]
["RO段间泵Z轴速度","ns=3;s=VB2_Z_Z_SD"]
["RO段间泵Z轴位移","ns=3;s=VB2_Z_Z_WY"]
["UF反洗泵温度","ns=3;s=VB3_TEM"]
["UF反洗泵X轴速度","ns=3;s=VB3_X_Z_SD"]
["UF反洗泵X轴位移","ns=3;s=VB3_X_Z_WY"]
["UF反洗泵Y轴速度","ns=3;s=VB3_Y_Z_SD"]
["UF反洗泵Y轴位移","ns=3;s=VB3_Y_Z_WY"]
["UF反洗泵Z轴速度","ns=3;s=VB3_Z_Z_SD"]
["UF反洗泵Z轴位移","ns=3;s=VB3_Z_Z_WY"]
["UF排空泵温度","ns=3;s=VB4_TEM"]
["UF排空泵X轴速度","ns=3;s=VB4_X_Z_SD"]
["UF排空泵X轴位移","ns=3;s=VB4_X_Z_WY"]
["UF排空泵Y轴速度","ns=3;s=VB4_Y_Z_SD"]
["UF排空泵Y轴位移","ns=3;s=VB4_Y_Z_WY"]
["UF排空泵Z轴速度","ns=3;s=VB4_Z_Z_SD"]
["UF排空泵Z轴位移","ns=3;s=VB4_Z_Z_WY"]
["UF产水泵温度","ns=3;s=VB5_TEM"]
["UF产水泵X轴速度","ns=3;s=VB5_X_Z_SD"]
["UF产水泵X轴位移","ns=3;s=VB5_X_Z_WY"]
["UF产水泵Y轴速度","ns=3;s=VB5_Y_Z_SD"]
["UF产水泵Y轴位移","ns=3;s=VB5_Y_Z_WY"]
["UF产水泵Z轴速度","ns=3;s=VB5_Z_Z_SD"]
["UF产水泵Z轴位移","ns=3;s=VB5_Z_Z_WY"]
["CIP清洗水泵温度","ns=3;s=VB6_TEM"]
["CIP清洗水泵X轴速度","ns=3;s=VB6_X_Z_SD"]
["CIP清洗水泵X轴位移","ns=3;s=VB6_X_Z_WY"]
["CIP清洗水泵Y轴速度","ns=3;s=VB6_Y_Z_SD"]
["CIP清洗水泵Y轴位移","ns=3;s=VB6_Y_Z_WY"]
["CIP清洗水泵Z轴速度","ns=3;s=VB6_Z_Z_SD"]
["CIP清洗水泵Z轴位移","ns=3;s=VB6_Z_Z_WY"]
["反洗风机温度","ns=3;s=VB7_TEM"]
["反洗风机X轴速度","ns=3;s=VB7_X_Z_SD"]
["反洗风机X轴位移","ns=3;s=VB7_X_Z_WY"]
["反洗风机Y轴速度","ns=3;s=VB7_Y_Z_SD"]
["反洗风机Y轴位移","ns=3;s=VB7_Y_Z_WY"]
["反洗风机Z轴速度","ns=3;s=VB7_Z_Z_SD"]
["反洗风机Z轴位移","ns=3;s=VB7_Z_Z_WY"]
["RO高压泵温度","ns=3;s=VB8_TEM"]
["RO高压泵X轴速度","ns=3;s=VB8_X_Z_SD"]
["RO高压泵X轴位移","ns=3;s=VB8_X_Z_WY"]
["RO高压泵Y轴速度","ns=3;s=VB8_Y_Z_SD"]
["RO高压泵Y轴位移","ns=3;s=VB8_Y_Z_WY"]
["RO高压泵Z轴速度","ns=3;s=VB8_Z_Z_SD"]
["RO高压泵Z轴位移","ns=3;s=VB8_Z_Z_WY"]
["超滤进水上方烟感","ns=3;s=YG1_ALARM"]
["RO模架上方烟感","ns=3;s=YG2_ALARM"]
["RO控制柜上方烟感","ns=3;s=YG3_ALARM"]
["加药间上方烟感","ns=3;s=YG4_ALARM"]
["通道","ns=3;s=YG4_ID"]
["加药间控制柜总进线电能","ns=3;s=Z1_EP"]
["加药间控制柜总进线IA","ns=3;s=Z1_IA"]
["加药间控制柜总进线IB","ns=3;s=Z1_IB"]
["加药间控制柜总进线IC","ns=3;s=Z1_IC"]
["加药间控制柜总进线总功率","ns=3;s=Z1_POWER"]
["加药间控制柜总进线UA","ns=3;s=Z1_UA"]
["加药间控制柜总进线UB","ns=3;s=Z1_UB"]
["加药间控制柜总进线UC","ns=3;s=Z1_UC"]
["反洗风机电能","ns=3;s=Z2_EP"]
["反洗风机IA","ns=3;s=Z2_IA"]
["反洗风机IB","ns=3;s=Z2_IB"]
["反洗风机IC","ns=3;s=Z2_IC"]
["反洗风机总功率","ns=3;s=Z2_POWER"]
["反洗风机UA","ns=3;s=Z2_UA"]
["反洗风机UB","ns=3;s=Z2_UB"]
["反洗风机UC","ns=3;s=Z2_UC"]
["CIP泵电能","ns=3;s=Z3_EP"]
["CIP泵IA","ns=3;s=Z3_IA"]
["CIP泵IB","ns=3;s=Z3_IB"]
["CIP泵IC","ns=3;s=Z3_IC"]
["CIP泵总功率","ns=3;s=Z3_POWER"]
["CIP泵UA","ns=3;s=Z3_UA"]
["CIP泵UB","ns=3;s=Z3_UB"]
["CIP泵UC","ns=3;s=Z3_UC"]
["1#电加热器电能","ns=3;s=Z4_EP"]
["1#电加热器IA","ns=3;s=Z4_IA"]
["1#电加热器IB","ns=3;s=Z4_IB"]
["1#电加热器IC","ns=3;s=Z4_IC"]
["1#电加热器总功率","ns=3;s=Z4_POWER"]
["1#电加热器UA","ns=3;s=Z4_UA"]
["1#电加热器UB","ns=3;s=Z4_UB"]
["1#电加热器UC","ns=3;s=Z4_UC"]
["2#电加热器电能","ns=3;s=Z5_EP"]
["2#电加热器IA","ns=3;s=Z5_IA"]
["2#电加热器IB","ns=3;s=Z5_IB"]
["2#电加热器IC","ns=3;s=Z5_IC"]
["2#电加热器总功率","ns=3;s=Z5_POWER"]
["2#电加热器UA","ns=3;s=Z5_UA"]
["2#电加热器UB","ns=3;s=Z5_UB"]
["2#电加热器UC","ns=3;s=Z5_UC"]
["RO控制柜总进线电能","ns=3;s=Z6_EP"]
["RO控制柜总进线IA","ns=3;s=Z6_IA"]
["RO控制柜总进线IB","ns=3;s=Z6_IB"]
["RO控制柜总进线IC","ns=3;s=Z6_IC"]
["RO控制柜总进线总功率","ns=3;s=Z6_POWER"]
["RO控制柜总进线UA","ns=3;s=Z6_UA"]
["RO控制柜总进线UB","ns=3;s=Z6_UB"]
["RO控制柜总进线UC","ns=3;s=Z6_UC"]
["RO高压泵电能","ns=3;s=Z7_EP"]
["RO高压泵IA","ns=3;s=Z7_IA"]
["RO高压泵IB","ns=3;s=Z7_IB"]
["RO高压泵IC","ns=3;s=Z7_IC"]
["RO高压泵总功率","ns=3;s=Z7_POWER"]
["RO高压泵UA","ns=3;s=Z7_UA"]
["RO高压泵UB","ns=3;s=Z7_UB"]
["RO高压泵UC","ns=3;s=Z7_UC"]
["RO供水泵电能","ns=3;s=Z8_EP"]
["RO供水泵IA","ns=3;s=Z8_IA"]
["RO供水泵IB","ns=3;s=Z8_IB"]
["RO供水泵IC","ns=3;s=Z8_IC"]
["RO供水泵总功率","ns=3;s=Z8_POWER"]
["RO供水泵UA","ns=3;s=Z8_UA"]
["RO供水泵UB","ns=3;s=Z8_UB"]
["RO供水泵UC","ns=3;s=Z8_UC"]
["RO供段间泵电能","ns=3;s=Z9_EP"]
["RO供段间泵IA","ns=3;s=Z9_IA"]
["RO供段间泵IB","ns=3;s=Z9_IB"]
["RO供段间泵IC","ns=3;s=Z9_IC"]
["RO供段间泵总功率","ns=3;s=Z9_POWER"]
["RO供段间泵UA","ns=3;s=Z9_UA"]
["RO供段间泵UB","ns=3;s=Z9_UB"]
["RO供段间泵UC","ns=3;s=Z9_UC"]
["UF控制柜总进线电能","ns=3;s=Z10_EP"]
["UF控制柜总进线IA","ns=3;s=Z10_IA"]
["UF控制柜总进线IB","ns=3;s=Z10_IB"]
["UF控制柜总进线IC","ns=3;s=Z10_IC"]
["UF控制柜总进线总功率","ns=3;s=Z10_POWER"]
["UF控制柜总进线UA","ns=3;s=Z10_UA"]
["UF控制柜总进线UB","ns=3;s=Z10_UB"]
["UF控制柜总进线UC","ns=3;s=Z10_UC"]
["UF产水泵电能","ns=3;s=Z11_EP"]
["UF产水泵IA","ns=3;s=Z11_IA"]
["UF产水泵IB","ns=3;s=Z11_IB"]
["UF产水泵IC","ns=3;s=Z11_IC"]
["UF产水泵总功率","ns=3;s=Z11_POWER"]
["UF产水泵UA","ns=3;s=Z11_UA"]
["UF产水泵UB","ns=3;s=Z11_UB"]
["UF产水泵UC","ns=3;s=Z11_UC"]
["UF排空泵电能","ns=3;s=Z12_EP"]
["UF排空泵IA","ns=3;s=Z12_IA"]
["UF排空泵IB","ns=3;s=Z12_IB"]
["UF排空泵IC","ns=3;s=Z12_IC"]
["UF排空泵总功率","ns=3;s=Z12_POWER"]
["UF排空泵UA","ns=3;s=Z12_UA"]
["UF排空泵UB","ns=3;s=Z12_UB"]
["UF排空泵UC","ns=3;s=Z12_UC"]
["UF反洗泵电能","ns=3;s=Z13_EP"]
["UF反洗泵IA","ns=3;s=Z13_IA"]
["UF反洗泵IB","ns=3;s=Z13_IB"]
["UF反洗泵IC","ns=3;s=Z13_IC"]
["UF反洗泵总功率","ns=3;s=Z13_POWER"]
["UF反洗泵UA","ns=3;s=Z13_UA"]
["UF反洗泵UB","ns=3;s=Z13_UB"]
["UF反洗泵UC","ns=3;s=Z13_UC"]
["UF 1#提升泵电能","ns=3;s=Z14_EP"]
["UF 1#提升泵IA","ns=3;s=Z14_IA"]
["UF 1#提升泵IB","ns=3;s=Z14_IB"]
["UF 1#提升泵IC","ns=3;s=Z14_IC"]
["UF 1#提升泵总功率","ns=3;s=Z14_POWER"]
["UF 1#提升泵UA","ns=3;s=Z14_UA"]
["UF 1#提升泵UB","ns=3;s=Z14_UB"]
["UF 1#提升泵UC","ns=3;s=Z14_UC"]
["UF 2#提升泵电能","ns=3;s=Z15_EP"]
["UF 2#提升泵IA","ns=3;s=Z15_IA"]
["UF 2#提升泵IB","ns=3;s=Z15_IB"]
["UF 2#提升泵IC","ns=3;s=Z15_IC"]
["UF 2#提升泵总功率","ns=3;s=Z15_POWER"]
["UF 2#提升泵UA","ns=3;s=Z15_UA"]
["UF 2#提升泵UB","ns=3;s=Z15_UB"]
["UF 2#提升泵UC","ns=3;s=Z15_UC"]
["RO外供水碱泵HZ0","ns=3;s=RO_WGS_JB_A0"]
["RO外供水碱泵HZ1","ns=3;s=RO_WGS_JB_A1"]
["RO外供水碱泵HZ10","ns=3;s=RO_WGS_JB_A10"]
["RO外供水碱泵HZ11","ns=3;s=RO_WGS_JB_A11"]
["RO外供水碱泵HZ12","ns=3;s=RO_WGS_JB_A12"]
["RO外供水碱泵HZ13","ns=3;s=RO_WGS_JB_A13"]
["RO外供水碱泵HZ14","ns=3;s=RO_WGS_JB_A14"]
["RO外供水碱泵HZ15","ns=3;s=RO_WGS_JB_A15"]
["RO外供水碱泵HZ2","ns=3;s=RO_WGS_JB_A2"]
["RO外供水碱泵HZ3","ns=3;s=RO_WGS_JB_A3"]
["RO外供水碱泵HZ4","ns=3;s=RO_WGS_JB_A4"]
["RO外供水碱泵HZ5","ns=3;s=RO_WGS_JB_A5"]
["RO外供水碱泵HZ6","ns=3;s=RO_WGS_JB_A6"]
["RO外供水碱泵HZ7","ns=3;s=RO_WGS_JB_A7"]
["RO外供水碱泵HZ8","ns=3;s=RO_WGS_JB_A8"]
["RO外供水碱泵HZ9","ns=3;s=RO_WGS_JB_A9"]
["反渗透进水ORP超高（组态弹窗用）","ORP_CX"]
["反渗透回收率","ROHSL"]