{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":1318,"n_cols":2,"rows_kept":1318,"cut":false,"hidden":false,"merged":[]}
["item_alias","item_name"]
["进水量","water_in"]
["外供水流量","water_out"]
["RO1脱盐率","RO1_TYL"]
["RO2脱盐率","RO2_TYL"]
["UF1渗透率","UF1Per"]
["UF2渗透率","UF2Per"]
["1#次钠加药泵故障","ns=6;s=P_1#CNB_FAULT"]
["1#次钠加药泵运行","ns=6;s=P_1#CNB_RFB"]
["1#出水碱加药泵故障","ns=6;s=P_1#CSJB_FAULT"]
["1#出水碱加药泵运行","ns=6;s=P_1#CSJB_RFB"]
["1#回用水泵故障","ns=6;s=P_1#HYSB_FAULT"]
["1#回用水泵运行","ns=6;s=P_1#HYSB_RFB"]
["1#PAC加药泵故障","ns=6;s=P_1#PACB_FAULT"]
["1#PAC加药泵运行","ns=6;s=P_1#PACB_RFB"]
["1#RO段间泵故障","ns=6;s=P_1#RODJB_FAULT"]
["1#RO段间泵运行","ns=6;s=P_1#RODJB_RFB"]
["1#RO高压泵故障","ns=6;s=P_1#ROGYB_FAULT"]
["1#RO高压泵运行","ns=6;s=P_1#ROGYB_RFB"]
["1#RO还原剂加药泵故障","ns=6;s=P_1#HYJB_FAULT"]
["1#RO还原剂加药泵运行","ns=6;s=P_1#HYJB_RFB"]
["1#酸加药泵故障","ns=6;s=P_1#SB_FAULT"]
["1#酸加药泵运行","ns=6;s=P_1#SB_RFB"]
["1#杀菌剂加药泵故障","ns=6;s=P_1#SJB_FAULT"]
["1#杀菌剂加药泵运行","ns=6;s=P_1#SJB_RFB"]
["1#超滤碱加药泵故障","ns=6;s=P_1#UF_JB_FAULT"]
["1#超滤碱加药泵运行","ns=6;s=P_1#UF_JB_RFB"]
["1#超滤反洗泵故障","ns=6;s=P_1#UFBWB_FAULT"]
["1#超滤反洗泵运行","ns=6;s=P_1#UFBWB_RFB"]
["1#阻垢剂加药泵故障","ns=6;s=P_1#ZGJB_FAULT"]
["1#阻垢剂加药泵运行","ns=6;s=P_1#ZGJB_RFB"]
["1#中和还原剂加药泵故障","ns=6;s=P_1#ZH_HYJ_FAULT"]
["1#中和还原剂加药泵运行","ns=6;s=P_1#ZH_HYJ_RFB"]
["2#次钠加药泵故障","ns=6;s=P_2#CNB_FAULT"]
["2#次钠加药泵运行","ns=6;s=P_2#CNB_RFB"]
["2#出水碱加药泵故障","ns=6;s=P_2#CSJB_FAULT"]
["2#出水碱加药泵运行","ns=6;s=P_2#CSJB_RFB"]
["2#回用水泵故障","ns=6;s=P_2#HYSB_FAULT"]
["2#回用水泵运行","ns=6;s=P_2#HYSB_RFB"]
["2#PAC加药泵故障","ns=6;s=P_2#PACB_FAULT"]
["2#PAC加药泵运行","ns=6;s=P_2#PACB_RFB"]
["2#RO段间泵故障","ns=6;s=P_2#RODJB_FAULT"]
["2#RO段间泵运行","ns=6;s=P_2#RODJB_RFB"]
["2#RO高压泵故障","ns=6;s=P_2#ROGYB_FAULT"]
["2#RO高压泵运行","ns=6;s=P_2#ROGYB_RFB"]
["2#RO还原剂加药泵故障","ns=6;s=P_2#HYJB_FAULT"]
["2#RO还原剂加药泵运行","ns=6;s=P_2#HYJB_RFB"]
["2#酸加药泵故障","ns=6;s=P_2#SB_FAULT"]
["2#酸加药泵运行","ns=6;s=P_2#SB_RFB"]
["2#杀菌剂加药泵故障","ns=6;s=P_2#SJB_FAULT"]
["2#杀菌剂加药泵运行","ns=6;s=P_2#SJB_RFB"]
["2#超滤碱加药泵故障","ns=6;s=P_2#UF_JB_FAULT"]
["2#超滤碱加药泵运行","ns=6;s=P_2#UF_JB_RFB"]
["2#超滤反洗泵故障","ns=6;s=P_2#UFBWB_FAULT"]
["2#超滤反洗泵运行","ns=6;s=P_2#UFBWB_RFB"]
["2#阻垢剂加药泵故障","ns=6;s=P_2#ZGJB_FAULT"]
["2#阻垢剂加药泵运行","ns=6;s=P_2#ZGJB_RFB"]
["2#中和还原剂加药泵故障","ns=6;s=P_2#ZH_HYJ_FAULT"]
["2#中和还原剂加药泵运行","ns=6;s=P_2#ZH_HYJ_RFB"]
["3#阻垢剂加药泵故障","ns=6;s=P_3#ZGJB_FAULT"]
["3#阻垢剂加药泵运行","ns=6;s=P_3#ZGJB_RFB"]
["废水泵故障","ns=6;s=P_FSB_FAULT"]
["废水泵运行","ns=6;s=P_FSB_RFB"]
["加热器故障","ns=6;s=P_JRQ_FAULT"]
["加热器启动","ns=6;s=P_JRQ_OUTPUT"]
["加热器运行","ns=6;s=P_JRQ_RFB"]
["潜污泵故障","ns=6;s=P_QWB_FAULT"]
["潜污泵运行","ns=6;s=P_QWB_RFB"]
["清洗水泵故障","ns=6;s=P_QXSB_FAULT"]
["清洗水泵运行","ns=6;s=P_QXSB_RFB"]
["反渗透供水泵故障","ns=6;s=P_ROGSB_FAULT"]
["反渗透供水泵运行","ns=6;s=P_ROGSB_RFB"]
["超滤供水泵故障","ns=6;s=P_UFGSB_FAULT"]
["超滤供水泵运行","ns=6;s=P_UFGSB_RFB"]
["中和泵故障","ns=6;s=P_ZH_FAULT"]
["中和泵运行","ns=6;s=P_ZH_RFB"]
["RO1一段压差高","ns=6;s=RO1_1D_YC_HIGH"]
["RO1二段压差高","ns=6;s=RO1_2D_YC_HIGH"]
["RO1执行一段碱维护","ns=6;s=RO1_ACT_1DJWH"]
["RO1执行一段杀菌","ns=6;s=RO1_ACT_1DSJ"]
["RO1执行一段酸维护","ns=6;s=RO1_ACT_1DSWH"]
["RO1执行二三段碱维护","ns=6;s=RO1_ACT_2/3DJWH"]
["RO1执行二三段杀菌维护","ns=6;s=RO1_ACT_2/3DSJWH"]
["RO1执行二三段酸维护","ns=6;s=RO1_ACT_2/3DSWH"]
["RO1执行冲洗","ns=6;s=RO1_ACT_CX"]
["RO1执行超越过滤","ns=6;s=RO1_ACT_CYGL"]
["RO1执行超越停机冲洗","ns=6;s=RO1_ACT_CYTJCX"]
["RO1执行超越停机加药冲洗","ns=6;s=RO1_ACT_CYTJJYCX"]
["RO1执行非正常停机冲洗","ns=6;s=RO1_ACT_FZCTJCX"]
["RO1执行过滤","ns=6;s=RO1_ACT_GL"]
["RO1执行长时间停机加药冲洗","ns=6;s=RO1_ACT_LONGTIME_CEB"]
["RO1启用反洗泵","ns=6;s=RO1_APPLY_RO_FXB"]
["RO1启用供水泵","ns=6;s=RO1_APPLY_RO_GSB"]
["RO1启用还原剂泵","ns=6;s=RO1_APPLY_RO_HYJB"]
["RO1启用还原剂阀","ns=6;s=RO1_APPLY_RO_HYJF"]
["RO1启用气洗阀","ns=6;s=RO1_APPLY_RO_QXF"]
["RO1启用阻垢剂泵","ns=6;s=RO1_APPLY_RO_ZGJB"]
["RO1启用杀菌泵","ns=6;s=RO1_APPLY_SJB"]
["RO1启用杀菌阀","ns=6;s=RO1_APPLY_SJF"]
["RO1启用维护碱泵","ns=6;s=RO1_APPLY_WHJB"]
["RO1启用维护碱阀","ns=6;s=RO1_APPLY_WHJF"]
["RO1启用维护酸泵","ns=6;s=RO1_APPLY_WHSB"]
["RO1启用维护酸阀","ns=6;s=RO1_APPLY_WHSF"]
["RO1二三段碱维护","ns=6;s=RO1_BT_2/3DJWH"]
["RO1电导率高","ns=6;s=RO1_DDL_HIGH"]
["RO1正在过滤标记","ns=6;s=RO1_FLAG_GLING"]
["RO1系统报错","ns=6;s=RO1_SYSTEM_ERROR"]
["RO1该杀菌了","ns=6;s=RO1_TIME_FOR_SJ"]
["RO2一段压差高","ns=6;s=RO2_1D_YC_HIGH"]
["RO2二段压差高","ns=6;s=RO2_2D_YC_HIGH"]
["RO2执行一段碱维护","ns=6;s=RO2_ACT_1DJWH"]
["RO2执行一段杀菌","ns=6;s=RO2_ACT_1DSJ"]
["RO2执行一段酸维护","ns=6;s=RO2_ACT_1DSWH"]
["RO2执行二三段碱维护","ns=6;s=RO2_ACT_2/3DJWH"]
["RO2执行二三段杀菌维护","ns=6;s=RO2_ACT_2/3DSJWH"]
["RO2执行二三段酸维护","ns=6;s=RO2_ACT_2/3DSWH"]
["RO2执行冲洗","ns=6;s=RO2_ACT_CX"]
["RO2执行超越过滤","ns=6;s=RO2_ACT_CYGL"]
["RO2执行超越停机冲洗","ns=6;s=RO2_ACT_CYTJCX"]
["RO2执行超越停机加药冲洗","ns=6;s=RO2_ACT_CYTJJYCX"]
["RO2执行非正常停机冲洗","ns=6;s=RO2_ACT_FZCTJCX"]
["RO2执行过滤","ns=6;s=RO2_ACT_GL"]
["RO2执行长时间停机加药冲洗","ns=6;s=RO2_ACT_LONGTIME_CEB"]
["RO2启用反洗泵","ns=6;s=RO2_APPLY_RO_FXB"]
["RO2启用供水泵","ns=6;s=RO2_APPLY_RO_GSB"]
["RO2启用还原剂泵","ns=6;s=RO2_APPLY_RO_HYJB"]
["RO2启用还原剂阀","ns=6;s=RO2_APPLY_RO_HYJF"]
["RO2启用气洗阀","ns=6;s=RO2_APPLY_RO_QXF"]
["RO2启用阻垢剂泵","ns=6;s=RO2_APPLY_RO_ZGJB"]
["RO2启用杀菌泵","ns=6;s=RO2_APPLY_SJB"]
["RO2启用杀菌阀","ns=6;s=RO2_APPLY_SJF"]
["RO2启用维护碱泵","ns=6;s=RO2_APPLY_WHJB"]
["RO2启用维护碱阀","ns=6;s=RO2_APPLY_WHJF"]
["RO2启用维护酸泵","ns=6;s=RO2_APPLY_WHSB"]
["RO2启用维护酸阀","ns=6;s=RO2_APPLY_WHSF"]
["RO2二三段碱维护","ns=6;s=RO2_BT_2/3DJWH"]
["RO2电导率高","ns=6;s=RO2_DDL_HIGH"]
["RO2正在过滤标记","ns=6;s=RO2_FLAG_GLING"]
["RO2系统报错","ns=6;s=RO2_SYSTEM_ERROR"]
["RO2该杀菌了","ns=6;s=RO2_TIME_FOR_SJ"]
["UF1启用供水泵","ns=6;s=UF1_APPLY_GSB"]
["UF1启用PAC泵","ns=6;s=UF1_APPLY_PAC_B"]
["UF1启用PAC阀","ns=6;s=UF1_APPLY_PAC-V"]
["UF1启用调节阀","ns=6;s=UF1_APPLY_TJV"]
["UF1自动过滤启动","ns=6;s=UF1_AUTOSTART_GL"]
["UF1手动反洗操作","ns=6;s=UF1_BT_BW"]
["UF1手动CEB操作","ns=6;s=UF1_BT_CEB"]
["UF1手动CIP操作","ns=6;s=UF1_BT_CIP"]
["UF1手动冲水操作","ns=6;s=UF1_BT_CS"]
["UF1手动清除过滤流量","ns=6;s=UF1_BT_ERASE_GLFLOW"]
["UF1手动过滤操作","ns=6;s=UF1_BT_GL"]
["UF1手动初始化操作","ns=6;s=UF1_BT_INAI"]
["UF1压差高限值报错","ns=6;s=UF1_ERR_YC_H"]
["UF1压差高高值报错","ns=6;s=UF1_ERR_YC_HH"]
["UF1药剂残留报错","ns=6;s=UF1_ERR_YJCL"]
["UF1膜内有药标志","ns=6;s=UF1_FLAG_MNYY"]
["UF1无它CEB标志","ns=6;s=UF1_FLAG_NOOTHERCEB"]
["UF1系统报错","ns=6;s=UF1_SYS_ERR"]
["UF2启用PAC泵","ns=6;s=UF2_APPLY_PAC_B"]
["UF2启用PAC阀","ns=6;s=UF2_APPLY_PAC_V"]
["UF2自动过滤启动","ns=6;s=UF2_AUTOSTART_GL"]
["UF2手动反洗操作","ns=6;s=UF2_BT_BW"]
["UF2手动CEB操作","ns=6;s=UF2_BT_CEB"]
["UF2手动CIP操作","ns=6;s=UF2_BT_CIP"]
["UF2手动冲水操作","ns=6;s=UF2_BT_CS"]
["UF2手动清除过滤流量","ns=6;s=UF2_BT_ERASE_GLFLOW"]
["UF2手动过滤操作","ns=6;s=UF2_BT_GL"]
["UF2手动初始化操作","ns=6;s=UF2_BT_INAI"]
["UF2压差高限值报错","ns=6;s=UF2_ERR_YC_H"]
["UF2压差高高值报错","ns=6;s=UF2_ERR_YC_HH"]
["UF2药剂残留报错","ns=6;s=UF2_ERR_YJCL"]
["UF2膜内有药标志","ns=6;s=UF2_FLAG_MNYY"]
["UF2无它CEB标志","ns=6;s=UF2_FLAG_NOOTHERCEB"]
["UF2系统报错","ns=6;s=UF2_SYS_ERR"]
["UF1反洗进水阀故障","ns=6;s=V_1#UF_BWJS_ERR"]
["UF1反洗进水阀总故障","ns=6;s=V_1#UF_BWJS_ERRT"]
["UF1反洗排水阀故障","ns=6;s=V_1#UF_BWPS_ERR"]
["UF1反洗排水阀总故障","ns=6;s=V_1#UF_BWPS_ERRT"]
["UF1产水阀故障","ns=6;s=V_1#UF_CS_ERR"]
["UF1产水阀总故障","ns=6;s=V_1#UF_CS_ERRT"]
["UF1排气阀1故障","ns=6;s=V_1#UF_PQ1_ERR"]
["UF1排气阀1总故障","ns=6;s=V_1#UF_PQ1_ERRT"]
["UF1排气阀2故障","ns=6;s=V_1#UF_PQ2_ERR"]
["UF1排气阀2总故障","ns=6;s=V_1#UF_PQ2_ERRT"]
["UF1排气阀3故障","ns=6;s=V_1#UF_PQ3_ERR"]
["UF1排气阀3总故障","ns=6;s=V_1#UF_PQ3_ERRT"]
["UF1排气阀4故障","ns=6;s=V_1#UF_PQ4_ERR"]
["UF1排气阀4总故障","ns=6;s=V_1#UF_PQ4_ERRT"]
["UF1隔断阀故障","ns=6;s=V_1#UFCIPGL_EER"]
["UF1隔断阀总故障","ns=6;s=V_1#UFCIPGL_ERRT"]
["RO1不合格阀故障","ns=6;s=V_1RO_BHG_ERR"]
["RO1不合格阀总故障","ns=6;s=V_1RO_BHG_ERRT"]
["RO1产水阀故障","ns=6;s=V_1RO_CS_ERR"]
["RO1产水阀总故障","ns=6;s=V_1RO_CS_ERRT"]
["RO1进水阀故障","ns=6;s=V_1RO_JS_ERR"]
["RO1进水阀总故障","ns=6;s=V_1RO_JS_ERRT"]
["RO1二段产水排气阀故障","ns=6;s=V_1ROEDCSPQ_ERR"]
["RO1二段产水排气阀总故障","ns=6;s=V_1ROEDCSPQ_ERRT"]
["RO1二段进水排气阀故障","ns=6;s=V_1ROEDJSPQ_ERR"]
["RO1二段进水排气阀总故障","ns=6;s=V_1ROEDJSPQ_ERRT"]
["RO1二段浓水排气阀故障","ns=6;s=V_1ROEDNSPQ_ERR"]
["RO1二段浓水排气阀总故障","ns=6;s=V_1ROEDNSPQ_ERRT"]
["RO1三段产水排气阀故障","ns=6;s=V_1ROSDCSPQ_ERR"]
["RO1三段产水排气阀总故障","ns=6;s=V_1ROSDCSPQ_ERRT"]
["RO1三段冲洗排水阀故障","ns=6;s=V_1ROSDCXPS_ERR"]
["RO1三段冲洗排水阀总故障","ns=6;s=V_1ROSDCXPS_ERRT"]
["RO1三段进水排气阀故障","ns=6;s=V_1ROSDJSPQ_ERR"]
["RO1三段进水排气阀总故障","ns=6;s=V_1ROSDJSPQ_ERRT"]
["RO1三段浓水排气阀故障","ns=6;s=V_1ROSDNSPQ_ERR"]
["RO1三段浓水排气阀总故障","ns=6;s=V_1ROSDNSPQ_ERRT"]
["RO1一段冲洗进水阀故障","ns=6;s=V_1ROYDBWJS_ERR"]
["RO1一段冲洗进水阀总故障","ns=6;s=V_1ROYDBWJS_ERRT"]
["RO1一段冲洗排水阀故障","ns=6;s=V_1ROYDBWPS_ERR"]
["RO1一段冲洗排水阀总故障","ns=6;s=V_1ROYDBWPS_ERRT"]
["RO1一段产水排气阀1故障","ns=6;s=V_1ROYDCSP1_ERR"]
["RO1一段产水排气阀1总故障","ns=6;s=V_1ROYDCSP1_ERRT"]
["RO1一段产水排气阀2故障","ns=6;s=V_1ROYDCSP2_ERR"]
["RO1一段产水排气阀2总故障","ns=6;s=V_1ROYDCSP2_ERRT"]
["RO1一段超越旁路阀故障","ns=6;s=V_1ROYDCYPL_ERR"]
["RO1一段超越旁路阀总故障","ns=6;s=V_1ROYDCYPL_ERRT"]
["RO1一段进水排气阀1故障","ns=6;s=V_1ROYDJSP1_ERR"]
["RO1一段进水排气阀1总故障","ns=6;s=V_1ROYDJSP1_ERRT"]
["RO1一段进水排气阀2故障","ns=6;s=V_1ROYDJSP2_ERR"]
["RO1一段进水排气阀2总故障","ns=6;s=V_1ROYDJSP2_ERRT"]
["RO1一段浓水排气阀1故障","ns=6;s=V_1ROYDNSP1_ERR"]
["RO1一段浓水排气阀1总故障","ns=6;s=V_1ROYDNSP1_ERRT"]
["RO1一段浓水排气阀2故障","ns=6;s=V_1ROYDNSP2_ERR"]
["RO1一段浓水排气阀2总故障","ns=6;s=V_1ROYDNSP2_ERRT"]
["RO1一段隔离阀故障","ns=6;s=V_1ROYDQXGL_ERR"]
["RO1一段隔离阀总故障","ns=6;s=V_1ROYDQXGL_ERRT"]
["UF2反洗进水阀故障","ns=6;s=V_2#UF_BWJS_ERR"]
["UF2反洗进水阀总故障","ns=6;s=V_2#UF_BWJS_ERRT"]
["UF2反洗排水阀故障","ns=6;s=V_2#UF_BWPS_ERR"]
["UF2反洗排水阀总故障","ns=6;s=V_2#UF_BWPS_ERRT"]
["UF2产水阀故障","ns=6;s=V_2#UF_CS_ERR"]
["UF2产水阀总故障","ns=6;s=V_2#UF_CS_ERRT"]
["UF2排气阀1故障","ns=6;s=V_2#UF_PQ1_ERR"]
["UF2排气阀1总故障","ns=6;s=V_2#UF_PQ1_ERRT"]
["UF2排气阀2故障","ns=6;s=V_2#UF_PQ2_ERR"]
["UF2排气阀2总故障","ns=6;s=V_2#UF_PQ2_ERRT"]
["UF2排气阀3故障","ns=6;s=V_2#UF_PQ3_ERR"]
["UF2排气阀3总故障","ns=6;s=V_2#UF_PQ3_ERRT"]
["UF2排气阀4故障","ns=6;s=V_2#UF_PQ4_ERR"]
["UF2排气阀4总故障","ns=6;s=V_2#UF_PQ4_ERRT"]
["UF2隔断阀故障","ns=6;s=V_2#UFCIPGL_ERR"]
["UF2隔断阀总故障","ns=6;s=V_2#UFCIPGL_ERRT"]
["RO2不合格阀故障","ns=6;s=V_2RO_BHG_ERR"]
["RO2不合格阀总故障","ns=6;s=V_2RO_BHG_ERRT"]
["RO2产水阀故障","ns=6;s=V_2RO_CS_ERR"]
["RO2产水阀总故障","ns=6;s=V_2RO_CS_ERRT"]
["RO2进水阀故障","ns=6;s=V_2RO_JS_ERR"]
["RO2进水阀总故障","ns=6;s=V_2RO_JS_ERRT"]
["RO2二段产水排气阀故障","ns=6;s=V_2ROEDCSPQ_ERR"]
["RO2二段产水排气阀总故障","ns=6;s=V_2ROEDCSPQ_ERRT"]
["RO2二段进水排气阀故障","ns=6;s=V_2ROEDJSPQ_ERR"]
["RO2二段进水排气阀总故障","ns=6;s=V_2ROEDJSPQ_ERRT"]
["RO2二段浓水排气阀故障","ns=6;s=V_2ROEDNSPQ_ERR"]
["RO2二段浓水排气阀总故障","ns=6;s=V_2ROEDNSPQ_ERRT"]
["RO2三段产水排气阀故障","ns=6;s=V_2ROSDCSPQ_ERR"]
["RO2三段产水排气阀总故障","ns=6;s=V_2ROSDCSPQ_ERRT"]
["RO2三段冲洗排水阀故障","ns=6;s=V_2ROSDCXPS_ERR"]
["RO2三段冲洗排水阀总故障","ns=6;s=V_2ROSDCXPS_ERRT"]
["RO2三段进水排气阀故障","ns=6;s=V_2ROSDJSPQ_ERR"]
["RO2三段进水排气阀总故障","ns=6;s=V_2ROSDJSPQ_ERRT"]
["RO2三段浓水排气阀故障","ns=6;s=V_2ROSDNSPQ_ERR"]
["RO2三段浓水排气阀总故障","ns=6;s=V_2ROSDNSPQ_ERRT"]
["RO2一段冲洗进水阀故障","ns=6;s=V_2ROYDBWJS_ERR"]
["RO2一段冲洗进水阀总故障","ns=6;s=V_2ROYDBWJS_ERRT"]
["RO2一段冲洗排水阀故障","ns=6;s=V_2ROYDBWPS_ERR"]
["RO2一段冲洗排水阀总故障","ns=6;s=V_2ROYDBWPS_ERRT"]
["RO2一段产水排气阀1故障","ns=6;s=V_2ROYDCSP1_ERR"]
["RO2一段产水排气阀1总故障","ns=6;s=V_2ROYDCSP1_ERRT"]
["RO2一段产水排气阀2故障","ns=6;s=V_2ROYDCSP2_ERR"]
["RO2一段产水排气阀2总故障","ns=6;s=V_2ROYDCSP2_ERRT"]
["RO2一段超越旁路阀故障","ns=6;s=V_2ROYDCYPL_ERR"]
["RO2一段超越旁路阀总故障","ns=6;s=V_2ROYDCYPL_ERRT"]
["RO2一段进水排气阀1故障","ns=6;s=V_2ROYDJSP1_ERR"]
["RO2一段进水排气阀1总故障","ns=6;s=V_2ROYDJSP1_ERRT"]
["RO2一段进水排气阀2故障","ns=6;s=V_2ROYDJSP2_ERR"]
["RO2一段进水排气阀2总故障","ns=6;s=V_2ROYDJSP2_ERRT"]
["RO2一段浓水排气阀1故障","ns=6;s=V_2ROYDNSP1_ERR"]
["RO2一段浓水排气阀1总故障","ns=6;s=V_2ROYDNSP1_ERRT"]
["RO2一段浓水排气阀2故障","ns=6;s=V_2ROYDNSP2_ERR"]
["RO2一段浓水排气阀2总故障","ns=6;s=V_2ROYDNSP2_ERRT"]
["RO2一段隔离阀故障","ns=6;s=V_2ROYDQXGL_ERR"]
["RO2一段隔离阀总故障","ns=6;s=V_2ROYDQXGL_ERRT"]
["反洗废水外排阀故障","ns=6;s=V_BW_WP_ERR"]
["反洗废水外排阀总故障","ns=6;s=V_BW_WP_ERRT"]
["CEB排放阀故障","ns=6;s=V_CEB_WP_ERR"]
["CEB排放阀总故障","ns=6;s=V_CEB_WP_ERRT"]
["RO气洗阀故障","ns=6;s=V_RO_QX_ERR"]
["RO气洗阀总故障","ns=6;s=V_RO_QX_ERRT"]
["UF1进水调节阀关状态","ns=6;s=V_UF1_TJV_CFB"]
["UF1进水调节阀开状态","ns=6;s=V_UF1_TJV_OFB"]
["UF2进水调节阀关状态","ns=6;s=V_UF2_TJV_CFB"]
["UF2进水调节阀开状态","ns=6;s=V_UF2_TJV_OFB"]
["中和外排阀故障","ns=6;s=V_ZH_WP_ERR"]
["中和外排阀总故障","ns=6;s=V_ZH_WP_ERRT"]
["1#出水碱加药泵频率反馈","ns=3;s=1#CSJB_FRE_FB_O"]
["1#回用水泵电流反馈","ns=3;s=1#HYSB_CUR_FB_O"]
["1#回用水泵频率反馈","ns=3;s=1#HYSB_FRE_FB_O"]
["1#回用水泵后轴温度","ns=3;s=1#HYSB_HZ_TEMP_O"]
["1#回用水泵前轴温度","ns=3;s=1#HYSB_QZ_TEMP_O"]
["1#PAC加药泵频率反馈","ns=3;s=1#PAC_FRE_FB_O"]
["1#RO产水电导","ns=3;s=1#RO_CSDD_O"]
["1#RO产水压力","ns=3;s=1#RO_CSPRESS_O"]
["1#RO二段产水流量","ns=3;s=1#RO_EDCSFLOW_O"]
["1#RO二段进水压力","ns=3;s=1#RO_EDJSPRESS_O"]
["1#RO二段浓水压力","ns=3;s=1#RO_EDNSPRESS_O"]
["1#RO进水流量","ns=3;s=1#RO_JSFLOW_O"]
["1#RO进水压力","ns=3;s=1#RO_JSPRESS_O"]
["1#RO浓水流量","ns=3;s=1#RO_NSFLOW_O"]
["1#RO三段产水流量","ns=3;s=1#RO_SDCSFLOW_O"]
["1#RO三段进水压力","ns=3;s=1#RO_SDJSPRESS_O"]
["1#RO三段浓水压力","ns=3;s=1#RO_SDNSPRESS_O"]
["1#RO段间泵电流反馈","ns=3;s=1#RODJB_CUR_FB_O"]
["1#RO段间泵测振反馈","ns=3;s=1#RODJB_CZ_O"]
["1#RO段间泵频率反馈","ns=3;s=1#RODJB_FRE_FB_O"]
["1#RO段间泵后轴温度","ns=3;s=1#RODJB_HZ_TEMP_O"]
["1#RO段间泵前轴温度","ns=3;s=1#RODJB_QZ_TEMP_O"]
["1#RO高压泵电流反馈","ns=3;s=1#ROGYB_CUR_FB_O"]
["1#RO高压泵测振反馈","ns=3;s=1#ROGYB_CZ_O"]
["1#RO高压泵频率反馈","ns=3;s=1#ROGYB_FRE_FB_O"]
["1#RO高压泵后轴温度反馈","ns=3;s=1#ROGYB_HZ_TEMP_O"]
["1#RO高压泵前轴温度反馈","ns=3;s=1#ROGYB_QZ_TEMP_O"]
["1#RO还原剂加药泵频率反馈","ns=3;s=1#ROHYJ_FRE_FB_O"]
["1#杀菌剂加药泵频率反馈","ns=3;s=1#SJB_FRE_FB_O"]
["1#UF产水压力","ns=3;s=1#UF_CSPRESS_O"]
["1#UF进水流量","ns=3;s=1#UF_JSFLOW_O"]
["1#UF进水压力","ns=3;s=1#UF_JSPRESS_O"]
["1#UF调节阀开度反馈","ns=3;s=1#UF_V_FB_O"]
["1#UF反洗泵电流反馈","ns=3;s=1#UFBWB_CUR_FB_O"]
["1#UF反洗泵频率反馈","ns=3;s=1#UFBWB_FRE_FB_O"]
["1#UF反洗泵后轴温度反馈","ns=3;s=1#UFBWB_HZ_TEMP_O"]
["1#UF反洗泵前轴温度反馈","ns=3;s=1#UFBWB_QZ_TEMP_O"]
["1#阻垢剂流量","ns=3;s=1#ZGJ_FLOW_O"]
["1#阻垢剂加药泵频率反馈","ns=3;s=1#ZGJ_FRE_FB_O"]
["2#出水碱加药泵频率反馈","ns=3;s=2#CSJB_FRE_FB_O"]
["2#回用水泵电流反馈","ns=3;s=2#HYSB_CUR_FB_O"]
["2#回用水泵频率反馈","ns=3;s=2#HYSB_FRE_FB_O"]
["2#回用水泵后轴温度","ns=3;s=2#HYSB_HZ_TEMP_O"]
["2#回用水泵前轴温度","ns=3;s=2#HYSB_QZ_TEMP_O"]
["2#PAC加药泵频率反馈","ns=3;s=2#PAC_FRE_FB_O"]
["2#RO产水电导","ns=3;s=2#RO_CSDD_O"]
["2#RO产水压力","ns=3;s=2#RO_CSPRESS_O"]
["2#RO二段产水流量","ns=3;s=2#RO_EDCSFLOW_O"]
["2#RO二段进水压力","ns=3;s=2#RO_EDJSPRESS_O"]
["2#RO二段浓水压力","ns=3;s=2#RO_EDNSPRESS_O"]
["2#RO进水流量","ns=3;s=2#RO_JSFLOW_O"]
["2#RO进水压力","ns=3;s=2#RO_JSPRESS_O"]
["2#RO浓水流量","ns=3;s=2#RO_NSFLOW_O"]
["2#RO三段产水流量","ns=3;s=2#RO_SDCSFLOW_O"]
["2#RO三段进水压力","ns=3;s=2#RO_SDJSPRESS_O"]
["2#RO三段浓水压力","ns=3;s=2#RO_SDNSPRESS_O"]
["2#RO段间泵电流反馈","ns=3;s=2#RODJB_CUR_FB_O"]
["2#RO段间泵测振反馈","ns=3;s=2#RODJB_CZ_O"]
["2#RO段间泵频率反馈","ns=3;s=2#RODJB_FRE_FB_O"]
["2#RO段间泵后轴温度","ns=3;s=2#RODJB_HZ_TEMP_O"]
["2#RO段间泵前轴温度","ns=3;s=2#RODJB_QZ_TEMP_O"]
["2#RO高压泵电流反馈","ns=3;s=2#ROGYB_CUR_FB_O"]
["2#RO高压泵测振反馈","ns=3;s=2#ROGYB_CZ_O"]
["2#RO高压泵频率反馈","ns=3;s=2#ROGYB_FRE_FB_O"]
["2#RO高压泵后轴温度反馈","ns=3;s=2#ROGYB_HZ_TEMP_O"]
["2#RO高压泵前轴温度反馈","ns=3;s=2#ROGYB_QZ_TEMP_O"]
["2#RO还原剂加药泵频率反馈","ns=3;s=2#ROHYJ_FRE_FB_O"]
["2#杀菌剂加药泵频率反馈","ns=3;s=2#SJB_FRE_FB_O"]
["2#UF产水压力","ns=3;s=2#UF_CSPRESS_O"]
["2#UF进水流量","ns=3;s=2#UF_JSFLOW_O"]
["2#UF进水压力","ns=3;s=2#UF_JSPRESS_O"]
["2#UF调节阀开度反馈","ns=3;s=2#UF_V_FB_O"]
["2#UF反洗泵电流反馈","ns=3;s=2#UFBWB_CUR_FB_O"]
["2#UF反洗泵频率反馈","ns=3;s=2#UFBWB_FRE_FB_O"]
["2#UF反洗泵后轴温度反馈","ns=3;s=2#UFBWB_HZ_TEMP_O"]
["2#UF反洗泵前轴温度反馈","ns=3;s=2#UFBWB_QZ_TEMP_O"]
["2#阻垢剂流量","ns=3;s=2#ZGJ_FLOW_O"]
["2#阻垢剂加药泵频率反馈","ns=3;s=2#ZGJ_FRE_FB_O"]
["3#阻垢剂加药泵频率反馈","ns=3;s=3#ZGJ_FRE_FB_O"]
["空气压力","ns=3;s=AIR_PRESS_O"]
["次钠液位高高限值","ns=3;s=ALARM_CN_HHR"]
["次钠液位高限值","ns=3;s=ALARM_CN_HR"]
["次钠液位","ns=3;s=ALARM_CN_IN"]
["次钠液位低低限值","ns=3;s=ALARM_CN_LLR"]
["次钠液位低限值","ns=3;s=ALARM_CN_LR"]
["废水箱液位高高限值","ns=3;s=ALARM_FSX_HHR"]
["废水箱液位高限值","ns=3;s=ALARM_FSX_HR"]
["废水箱液位","ns=3;s=ALARM_FSX_IN"]
["废水箱液位低低限值","ns=3;s=ALARM_FSX_LLR"]
["废水箱液位低限值","ns=3;s=ALARM_FSX_LR"]
["还原剂液位高高限值","ns=3;s=ALARM_HYJ_HHR"]
["还原剂液位高限值","ns=3;s=ALARM_HYJ_HR"]
["还原剂液位","ns=3;s=ALARM_HYJ_IN"]
["还原剂液位低低限值","ns=3;s=ALARM_HYJ_LLR"]
["还原剂液位低限值","ns=3;s=ALARM_HYJ_LR"]
["碱液位高高限值","ns=3;s=ALARM_J_HHR"]
["碱液位高限值","ns=3;s=ALARM_J_HR"]
["碱液位","ns=3;s=ALARM_J_IN"]
["碱液位低低限值","ns=3;s=ALARM_J_LLR"]
["碱液位低限值","ns=3;s=ALARM_J_LR"]
["进水箱1液位高高限值","ns=3;s=ALARM_JSX1_HHR"]
["进水箱1液位高限值","ns=3;s=ALARM_JSX1_HR"]
["进水箱1液位","ns=3;s=ALARM_JSX1_IN"]
["进水箱1液位低低限值","ns=3;s=ALARM_JSX1_LLR"]
["进水箱1液位低限值","ns=3;s=ALARM_JSX1_LR"]
["进水箱2液位高高限值","ns=3;s=ALARM_JSX2_HHR"]
["进水箱2液位高限值","ns=3;s=ALARM_JSX2_HR"]
["进水箱2液位","ns=3;s=ALARM_JSX2_IN"]
["进水箱2液位低低限值","ns=3;s=ALARM_JSX2_LLR"]
["进水箱2液位低限值","ns=3;s=ALARM_JSX2_LR"]
["絮凝剂液位高高限值","ns=3;s=ALARM_PAC_HHR"]
["絮凝剂液位高限值","ns=3;s=ALARM_PAC_HR"]
["絮凝剂液位","ns=3;s=ALARM_PAC_IN"]
["絮凝剂液位低低限值","ns=3;s=ALARM_PAC_LLR"]
["絮凝剂液位低限值","ns=3;s=ALARM_PAC_LR"]
["CIP水箱液位高高限值","ns=3;s=ALARM_QXSX_HHR"]
["CIP水箱液位高限值","ns=3;s=ALARM_QXSX_HR"]
["CIP水箱液位","ns=3;s=ALARM_QXSX_IN"]
["CIP水箱液位低低限值","ns=3;s=ALARM_QXSX_LLR"]
["CIP水箱液位低限值","ns=3;s=ALARM_QXSX_LR"]
["RO产水箱液位高高限值","ns=3;s=ALARM_RO_CSX_HHR"]
["RO产水箱液位高限值","ns=3;s=ALARM_RO_CSX_HR"]
["RO产水箱液位","ns=3;s=ALARM_RO_CSX_IN"]
["RO产水箱液位低低限值","ns=3;s=ALARM_RO_CSX_LLR"]
["RO产水箱液位低限值","ns=3;s=ALARM_RO_CSX_LR"]
["酸液位高高限值","ns=3;s=ALARM_S_HHR"]
["酸液位高限值","ns=3;s=ALARM_S_HR"]
["酸液位","ns=3;s=ALARM_S_IN"]
["酸液位低低限值","ns=3;s=ALARM_S_LLR"]
["酸液位低限值","ns=3;s=ALARM_S_LR"]
["杀菌剂液位高高限值","ns=3;s=ALARM_SJJ_HHR"]
["杀菌剂液位高限值","ns=3;s=ALARM_SJJ_HR"]
["杀菌剂液位","ns=3;s=ALARM_SJJ_IN"]
["杀菌剂液位低低限值","ns=3;s=ALARM_SJJ_LLR"]
["杀菌剂液位低限值","ns=3;s=ALARM_SJJ_LR"]
["UF产水箱液位高高限值","ns=3;s=ALARM_UF_CSX_HHR"]
["UF产水箱液位高限值","ns=3;s=ALARM_UF_CSX_HR"]
["UF产水箱液位","ns=3;s=ALARM_UF_CSX_IN"]
["UF产水箱液位低低限值","ns=3;s=ALARM_UF_CSX_LLR"]
["UF产水箱液位低限值","ns=3;s=ALARM_UF_CSX_LR"]
["阻垢剂液位高高限值","ns=3;s=ALARM_ZGJ_HHR"]
["阻垢剂液位高限值","ns=3;s=ALARM_ZGJ_HR"]
["阻垢剂液位","ns=3;s=ALARM_ZGJ_IN"]
["阻垢剂液位低低限值","ns=3;s=ALARM_ZGJ_LLR"]
["阻垢剂液位低限值","ns=3;s=ALARM_ZGJ_LR"]
["中和水箱液位高高限值","ns=3;s=ALARM_ZHSX_HHR"]
["中和水箱液位高限值","ns=3;s=ALARM_ZHSX_HR"]
["中和水箱液位","ns=3;s=ALARM_ZHSX_IN"]
["中和水箱液位低低限值","ns=3;s=ALARM_ZHSX_LLR"]
["中和水箱液位低限值","ns=3;s=ALARM_ZHSX_LR"]
["反洗流量","ns=3;s=BW_FLOW_O"]
["反洗压力","ns=3;s=BW_PRESS_O"]
["次钠液位","ns=3;s=CN_LEVEL_O"]
["RO产水箱液位","ns=3;s=CS_LEVEL_O"]
["废水箱液位","ns=3;s=FS_LEVEL_O"]
["废水泵后轴温度","ns=3;s=FSB_HZ_TEMP_O"]
["废水泵前轴温度","ns=3;s=FSB_QZ_TEMP_O"]
["还原剂液位","ns=3;s=HYJ_LEVEL_O"]
["回用水A流量","ns=3;s=HYS_A_FLOW_O"]
["回用水B流量","ns=3;s=HYS_B_FLOW_O"]
["回用水PH","ns=3;s=HYS_PH_O"]
["碱液位","ns=3;s=J_LEVEL_O"]
["进水箱1液位","ns=3;s=JSX1_LEVEL_O"]
["进水箱2液位","ns=3;s=JSX2_LEVEL_O"]
["1#次钠加药泵频率反馈","ns=3;s=P_1#CNB_FRE_FB"]
["1#次钠加药泵运行时间","ns=3;s=P_1#CNB_RUNTIME"]
["1#出水碱加药泵频率反馈","ns=3;s=P_1#CSJB_FRE_FB"]
["1#出水碱加药泵运行时间","ns=3;s=P_1#CSJB_RUNTIME"]
["1#回用水泵频率反馈","ns=3;s=P_1#HYSB_FRE_FB"]
["1#回用水泵运行时间","ns=3;s=P_1#HYSB_RUNTIME"]
["1#PAC加药泵频率反馈","ns=3;s=P_1#PACB_FRE_FB"]
["1#PAC加药泵运行时间","ns=3;s=P_1#PACB_RUNTIME"]
["1#RO段间泵频率反馈","ns=3;s=P_1#RODJB_FRE_FB"]
["1#RO段间泵运行时间","ns=3;s=P_1#RODJB_RUNTIME"]
["1#RO高压泵频率反馈","ns=3;s=P_1#ROGYB_FRE_FB"]
["1#RO高压泵运行时间","ns=3;s=P_1#ROGYB_RUNTIME"]
["1#RO还原剂加药泵频率反馈","ns=3;s=P_1#HYJB_FRE_FB"]
["1#RO还原剂加药泵运行时间","ns=3;s=P_1#HYJB_RUNTIME"]
["1#酸加药泵频率反馈","ns=3;s=P_1#SB_FRE_FB"]
["1#酸加药泵运行时间","ns=3;s=P_1#SB_RUNTIME"]
["1#杀菌剂加药泵频率反馈","ns=3;s=P_1#SJB_FRE_FB"]
["1#杀菌剂加药泵运行时间","ns=3;s=P_1#SJB_RUNTIME"]
["1#超滤碱加药泵频率反馈","ns=3;s=P_1#UF_JB_FRE_FB"]
["1#超滤碱加药泵运行时间","ns=3;s=P_1#UF_JB_RUNTIME"]
["1#UF反洗泵频率反馈","ns=3;s=P_1#UFBWB_FRE_FB"]
["1#UF反洗泵运行时间","ns=3;s=P_1#UFBWB_RUNTIME"]
["1#阻垢剂加药泵频率反馈","ns=3;s=P_1#ZGJB_FRE_FB"]
["1#阻垢剂加药泵运行时间","ns=3;s=P_1#ZGJB_RUNTIME"]
["1#中和还原剂加药泵频率反馈","ns=3;s=P_1#ZH_HYJ_FRE_FB"]
["1#中和还原剂加药泵运行时间","ns=3;s=P_1#ZH_HYJ_RUNTIME"]
["2#次钠加药泵频率反馈","ns=3;s=P_2#CNB_FRE_FB"]
["2#次钠加药泵运行时间","ns=3;s=P_2#CNB_RUNTIME"]
["2#出水碱加药泵频率反馈","ns=3;s=P_2#CSJB_FRE_FB"]
["2#出水碱加药泵运行时间","ns=3;s=P_2#CSJB_RUNTIME"]
["2#回用水泵频率反馈","ns=3;s=P_2#HYSB_FRE_FB"]
["2#回用水泵运行时间","ns=3;s=P_2#HYSB_RUNTIME"]
["2#PAC加药泵频率反馈","ns=3;s=P_2#PACB_FRE_FB"]
["2#PAC加药泵运行时间","ns=3;s=P_2#PACB_RUNTIME"]
["2#RO段间泵频率反馈","ns=3;s=P_2#RODJB_FRE_FB"]
["2#RO段间泵运行时间","ns=3;s=P_2#RODJB_RUNTIME"]
["2#RO高压泵频率反馈","ns=3;s=P_2#ROGYB_FRE_FB"]
["2#RO高压泵运行时间","ns=3;s=P_2#ROGYB_RUNTIME"]
["2#RO还原剂加药泵频率反馈","ns=3;s=P_2#HYJB_FRE_FB"]
["2#RO还原剂加药泵运行时间","ns=3;s=P_2#HYJB_RUNTIME"]
["2#酸加药泵频率反馈","ns=3;s=P_2#SB_FRE_FB"]
["2#酸加药泵运行时间","ns=3;s=P_2#SB_RUNTIME"]
["2#杀菌剂加药泵频率反馈","ns=3;s=P_2#SJB_FRE_FB"]
["2#杀菌剂加药泵运行时间","ns=3;s=P_2#SJB_RUNTIME"]
["2#超滤碱加药泵频率反馈","ns=3;s=P_2#UF_JB_FRE_FB"]
["2#超滤碱加药泵运行时间","ns=3;s=P_2#UF_JB_RUNTIME"]
["2#UF反洗泵频率反馈","ns=3;s=P_2#UFBWB_FRE_FB"]
["2#UF反洗泵运行时间","ns=3;s=P_2#UFBWB_RUNTIME"]
["2#阻垢剂加药泵频率反馈","ns=3;s=P_2#ZGJB_FRE_FB"]
["2#阻垢剂加药泵运行时间","ns=3;s=P_2#ZGJB_RUNTIME"]
["2#中和还原剂加药泵频率反馈","ns=3;s=P_2#ZH_HYJ_FRE_FB"]
["2#中和还原剂加药泵运行时间","ns=3;s=P_2#ZH_HYJ_RUNTIME"]
["3#阻垢剂加药泵频率反馈","ns=3;s=P_3#ZGJB_FRE_FB"]
["3#阻垢剂加药泵运行时间","ns=3;s=P_3#ZGJB_RUNTIME"]
["废水泵频率反馈","ns=3;s=P_FSB_FRE_FB"]
["废水泵运行时间","ns=3;s=P_FSB_RUNTIME"]
["加热器频率反馈","ns=3;s=P_JRQ_FRE_FB"]
["加热器运行时间","ns=3;s=P_JRQ_RUNTIME"]
["潜污泵频率反馈","ns=3;s=P_QWB_FRE_FB"]
["潜污泵运行时间","ns=3;s=P_QWB_RUNTIME"]
["清洗水泵频率反馈","ns=3;s=P_QXSB_FRE_FB"]
["清洗水泵运行时间","ns=3;s=P_QXSB_RUNTIME"]
["RO供水泵频率反馈","ns=3;s=P_ROGSB_FRE_FB"]
["RO供水泵运行时间","ns=3;s=P_ROGSB_RUNTIME"]
["UF供水泵频率反馈","ns=3;s=P_UFGSB_FRE_FB"]
["UF供水泵运行时间","ns=3;s=P_UFGSB_RUNTIME"]
["中和泵频率反馈","ns=3;s=P_ZH_FRE_FB"]
["中和泵运行时间","ns=3;s=P_ZH_RUNTIME"]
["絮凝剂液位","ns=3;s=PAC_LEVEL_O"]
["CIP水箱液位","ns=3;s=QXS_LEVEL_O"]
["CIP水PH","ns=3;s=QXS_PH_O"]
["CIP水温度","ns=3;s=QXS_TEMP_O"]
["清洗水泵电流","ns=3;s=QXSB_CUR_FB_O"]
["清洗水泵频率反馈","ns=3;s=QXSB_FRE_FB_O"]
["清洗水泵后轴温度反馈","ns=3;s=QXSB_HZ_TEMP_O"]
["清洗水泵前轴温度反馈","ns=3;s=QXSB_QZ_TEMP_O"]
["RO供水泵后轴温度反馈","ns=3;s=RO_GSB_HZ_TEMP_O"]
["RO供水泵前轴温度反馈","ns=3;s=RO_GSB_QZ_TEMP_0"]
["RO进水电导","ns=3;s=RO_JSDD_O"]
["RO进水ORP","ns=3;s=RO_JSORP_O"]
["RO进水PH","ns=3;s=RO_JSPH_O"]
["RO外供水电导","ns=3;s=RO_WSDD_O"]
["RO1一段压差","ns=3;s=RO1_1D_YC"]
["RO1一段产水流量","ns=3;s=RO1_1DUAN_CS_FLOW"]
["RO1一段已碱维护天数","ns=3;s=RO1_1DYJWH_DAYS"]
["RO1一段已杀菌天数","ns=3;s=RO1_1DYSJ_DAYS"]
["RO1一段已酸维护天数","ns=3;s=RO1_1DYSWH_DAYS"]
["RO1二三段已碱维护天数","ns=3;s=RO1_23DYJWH_DAYS"]
["RO1二三段已杀菌天数","ns=3;s=RO1_23DYSJ_DAYS"]
["RO1二三段已酸维护天数","ns=3;s=RO1_23DYSWH_DAYS"]
["RO1二段压差","ns=3;s=RO1_2D_YC"]
["RO1CODE_一段碱维护","ns=3;s=RO1_CODE_1DJWH"]
["RO1CODE_一段杀菌","ns=3;s=RO1_CODE_1DSJ"]
["RO1CODE_一段酸维护","ns=3;s=RO1_CODE_1DSWH"]
["RO1CODE_二三段碱维护","ns=3;s=RO1_CODE_23DJWH"]
["RO1CODE_二三段杀菌","ns=3;s=RO1_CODE_23DSJ"]
["RO1CODE_二三段酸维护","ns=3;s=RO1_CODE_23DSWH"]
["RO1CODE_冲洗","ns=3;s=RO1_CODE_CX"]
["1#RO高压泵频率输出","ns=3;s=RO1_GYB_FR_OUT"]
["RO1系统定时","ns=3;s=RO1_HMI_SET_TIME"]
["RO1系统计时","ns=3;s=RO1_HMI_SYSTEM_TIME"]
["RO1产水率","ns=3;s=RO1_RATE_CS"]
["RO1SET_一段碱维护天数","ns=3;s=RO1_SET_1DJWH_DAYS"]
["RO1SET_一段碱维后气水混洗时间","ns=3;s=RO1_SET_1DJWHHX_TIME"]
["RO1SET_一段碱维后水洗时间","ns=3;s=RO1_SET_1DJWHSX_TIME"]
["RO1SET_一段碱维加碱时间","ns=3;s=RO1_SET_1DJWJJ_TIME"]
["RO1SET_一段碱维浸泡时间","ns=3;s=RO1_SET_1DJWJP_TIME"]
["RO1SET_一段杀菌天数","ns=3;s=RO1_SET_1DSJ_DAYS"]
["RO1Set一段杀菌时间","ns=3;s=RO1_SET_1DSJ_TIME"]
["RO1Set_一段杀菌浸泡时间","ns=3;s=RO1_SET_1DSJJP_TIME"]
["RO1Set一段杀菌结束反冲排气时间","ns=3;s=RO1_SET_1DSJJS_TIME"]
["RO1Set一段杀菌结束气水冲时间","ns=3;s=RO1_SET_1DSJJSQ_TIME"]
["RO1SET_一段酸维护天数","ns=3;s=RO1_SET_1DSWH_DAYS"]
["RO1SET_一段酸维后气水混洗时间","ns=3;s=RO1_SET_1DSWHHX_TIME"]
["RO1SET_一段酸维后水洗时间","ns=3;s=RO1_SET_1DSWHSX_TIME"]
["RO1SET_一段酸维浸泡时间","ns=3;s=RO1_SET_1DSWJP_TIME"]
["RO1SET_一段酸维加酸时间","ns=3;s=RO1_SET_1DSWJS_TIME"]
["RO1Set_二三段正冲时间","ns=3;s=RO1_SET_2/3DZC_TIME"]
["RO1SET_二三段碱维护天数","ns=3;s=RO1_SET_23DJWH_DAYS"]
["RO1SET_二三段碱维护时间","ns=3;s=RO1_SET_23DJWH_TIME"]
["RO1SET_二三段碱维护后冲洗时间","ns=3;s=RO1_SET_23DJWHHCX_T"]
["RO1SET_二三段碱维护浸泡时间","ns=3;s=RO1_SET_23DJWHJ_TIME"]
["RO1SET_二三段杀菌天数","ns=3;s=RO1_SET_23DSJ_DAYS"]
["RO1SET_二三段杀菌后冲洗时间","ns=3;s=RO1_SET_23DSJCX_TIME"]
["RO1SET_二三段杀菌浸泡时间","ns=3;s=RO1_SET_23DSJJP_TIME"]
["RO1SET_二三段杀菌维护时间","ns=3;s=RO1_SET_23DSJWH_TIME"]
["RO1SET_二三段酸维护天数","ns=3;s=RO1_SET_23DSWH_DAYS"]
["RO1SET_二三段酸维护时间","ns=3;s=RO1_SET_23DSWH_TIME"]
["RO1SET_二三段酸维护后冲洗时间","ns=3;s=RO1_SET_23SWHHC_TIME"]
["RO1SET_二三段酸维护浸泡时间","ns=3;s=RO1_SET_23SWHJP_TIME"]
["RO1SET_超越过滤冲水排气时间","ns=3;s=RO1_SET_CYSGLCSPQ_T"]
["RO1SET_超越停机冲洗时间","ns=3;s=RO1_SET_CYTJCX_T"]
["RO1SET_超越停机加药冲洗时间","ns=3;s=RO1_SET_CYTJJYCX_T"]
["RO1SET_电导率","ns=3;s=RO1_SET_DDL"]
["RO1Set反冲时间","ns=3;s=RO1_SET_FC_TIME"]
["RO1Set过滤产水时间","ns=3;s=RO1_SET_GLCS_TIME"]
["RO1SET_GSPump_频率_L","ns=3;s=RO1_SET_GSPUMP_FR_L"]
["RO1SET_GYPump_频率","ns=3;s=RO1_SET_GYPUMP_FR"]
["RO1SET_GYPump_频率_H","ns=3;s=RO1_SET_GYPUMP_FR_H"]
["RO1SET_GYPump_频率_L","ns=3;s=RO1_SET_GYPUMP_FR_L"]
["RO1SET_加药冲洗反冲洗时间","ns=3;s=RO1_SET_JYCXFC_T"]
["RO1SET_加药冲洗正冲洗时间","ns=3;s=RO1_SET_JYCXZC_TIME"]
["RO1Set开机冲洗时间","ns=3;s=RO1_SET_KJCX_TIME"]
["RO1SET_ORP","ns=3;s=RO1_SET_ORP"]
["RO1SET_气水混洗时间","ns=3;s=RO1_SET_QSHX_TIEM"]
["RO1Set_水反洗排气时间","ns=3;s=RO1_SET_SFXPQ_TIME"]
["RO1SET_杀菌后反冲时间","ns=3;s=RO1_SET_SJHFC_TIME"]
["RO1SET_杀菌后正冲时间","ns=3;s=RO1_SET_SJHZC_TIME"]
["RO1SET杀菌流量","ns=3;s=RO1_SET_SJLL"]
["RO1Set停机加药冲洗时间","ns=3;s=RO1_SET_TJJYCX_TIME"]
["RO1SET_预杀菌天数","ns=3;s=RO1_SET_YSJ_DAYS"]
["RO1Set正冲时间","ns=3;s=RO1_SET_ZC_TIME"]
["RO1SET正冲流量","ns=3;s=RO1_SET_ZCLL"]
["RO1步序","ns=3;s=RO1_STEP"]
["RO1总产水流量","ns=3;s=RO1_TOTAL_CSLL"]
["RO1总过滤次数","ns=3;s=RO1_TOTAL_GL_CS"]
["RO1总进水流量","ns=3;s=RO1_TOTAL_JSLL"]
["RO1总浓水流量","ns=3;s=RO1_TOTAL_NSLL"]
["RO2一段压差","ns=3;s=RO2_1D_YC"]
["RO2一段产水流量","ns=3;s=RO2_1DUAN_CS_FLOW"]
["RO2一段已碱维护天数","ns=3;s=RO2_1DYJWH_DAYS"]
["RO2一段已杀菌天数","ns=3;s=RO2_1DYSJ_DAYS"]
["RO2一段已酸维护天数","ns=3;s=RO2_1DYSWH_DAYS"]
["RO2二三段已碱维护天数","ns=3;s=RO2_23DYJWH_DAYS"]
["RO2二三段已杀菌天数","ns=3;s=RO2_23DYSJ_DAYS"]
["RO2二三段已酸维护天数","ns=3;s=RO2_23DYSWH_DAYS"]
["RO2二段压差","ns=3;s=RO2_2D_YC"]
["RO2CODE_一段碱维护","ns=3;s=RO2_CODE_1DJWH"]
["RO2CODE_一段杀菌","ns=3;s=RO2_CODE_1DSJ"]
["RO2CODE_一段酸维护","ns=3;s=RO2_CODE_1DSWH"]
["RO2CODE_二三段碱维护","ns=3;s=RO2_CODE_23DJWH"]
["RO2CODE_二三段杀菌","ns=3;s=RO2_CODE_23DSJ"]
["RO2CODE_二三段酸维护","ns=3;s=RO2_CODE_23DSWH"]
["RO2CODE_冲洗","ns=3;s=RO2_CODE_CX"]
["2#RO供水泵频率输出","ns=3;s=RO2_GSB_FR_OUT"]
["2#RO高压泵频率输出","ns=3;s=RO2_GYB_FR_OUT"]
["RO2系统定时","ns=3;s=RO2_HMI_SET_TIME"]
["RO2系统计时","ns=3;s=RO2_HMI_SYSTEM_TIME"]
["RO2产水率","ns=3;s=RO2_RATE_CS"]
["RO2SET_一段碱维护天数","ns=3;s=RO2_SET_1DJWH_DAYS"]
["RO2SET_一段碱维后气水混洗时间","ns=3;s=RO2_SET_1DJWHHX_TIME"]
["RO2SET_一段碱维后水洗时间","ns=3;s=RO2_SET_1DJWHSX_TIME"]
["RO2SET_一段碱维加碱时间","ns=3;s=RO2_SET_1DJWJJ_TIME"]
["RO2SET_一段碱维浸泡时间","ns=3;s=RO2_SET_1DJWJP_TIME"]
["RO2SET_一段杀菌天数","ns=3;s=RO2_SET_1DSJ_DAYS"]
["RO2Set一段杀菌时间","ns=3;s=RO2_SET_1DSJ_TIME"]
["RO2Set_一段杀菌浸泡时间","ns=3;s=RO2_SET_1DSJJP_TIME"]
["RO2Set一段杀菌结束反冲排气时间","ns=3;s=RO2_SET_1DSJJS_TIME"]
["RO2Set一段杀菌结束气水冲时间","ns=3;s=RO2_SET_1DSJJSQ_TIME"]
["RO2SET_一段酸维护天数","ns=3;s=RO2_SET_1DSWH_DAYS"]
["RO2SET_一段酸维后气水混洗时间","ns=3;s=RO2_SET_1DSWHHX_TIME"]
["RO2SET_一段酸维后水洗时间","ns=3;s=RO2_SET_1DSWHSX_TIME"]
["RO2SET_一段酸维浸泡时间","ns=3;s=RO2_SET_1DSWJP_TIME"]
["RO2SET_一段酸维加酸时间","ns=3;s=RO2_SET_1DSWJS_TIME"]
["RO2Set_二三段正冲时间","ns=3;s=RO2_SET_2/3DZC_TIME"]
["RO2SET_二三段碱维护天数","ns=3;s=RO2_SET_23DJWH_DAYS"]
["RO2SET_二三段碱维护时间","ns=3;s=RO2_SET_23DJWH_TIME"]
["RO2SET_二三段碱维护后冲洗时间","ns=3;s=RO2_SET_23DJWHHCX_T"]
["RO2SET_二三段碱维护浸泡时间","ns=3;s=RO2_SET_23DJWHJ_TIME"]
["RO2SET_二三段杀菌天数","ns=3;s=RO2_SET_23DSJ_DAYS"]
["RO2SET_二三段杀菌后冲洗时间","ns=3;s=RO2_SET_23DSJCX_TIME"]
["RO2SET_二三段杀菌浸泡时间","ns=3;s=RO2_SET_23DSJJP_TIME"]
["RO2SET_二三段杀菌维护时间","ns=3;s=RO2_SET_23DSJWH_TIME"]
["RO2SET_二三段酸维护天数","ns=3;s=RO2_SET_23DSWH_DAYS"]
["RO2SET_二三段酸维护时间","ns=3;s=RO2_SET_23DSWH_TIME"]
["RO2SET_二三段酸维护后冲洗时间","ns=3;s=RO2_SET_23SWHHC_TIME"]
["RO2SET_二三段酸维护浸泡时间","ns=3;s=RO2_SET_23SWHJP_TIME"]
["RO2SET_超越过滤冲水排气时间","ns=3;s=RO2_SET_CYSGLCSPQ_T"]
["RO2SET_超越停机冲洗时间","ns=3;s=RO2_SET_CYTJCX_T"]
["RO2SET_超越停机加药冲洗时间","ns=3;s=RO2_SET_CYTJJYCX_T"]
["RO2SET_电导率","ns=3;s=RO2_SET_DDL"]
["RO2Set反冲时间","ns=3;s=RO2_SET_FC_TIME"]
["RO2Set过滤产水时间","ns=3;s=RO2_SET_GLCS_TIME"]
["RO2SET_GSPump_频率_L","ns=3;s=RO2_SET_GSPUMP_FR_L"]
["RO2SET_GYPump_频率","ns=3;s=RO2_SET_GYPUMP_FR"]
["RO2SET_GYPump_频率_H","ns=3;s=RO2_SET_GYPUMP_FR_H"]
["RO2SET_GYPump_频率_L","ns=3;s=RO2_SET_GYPUMP_FR_L"]
["RO2SET_加药冲洗反冲洗时间","ns=3;s=RO2_SET_JYCXFC_T"]
["RO2SET_加药冲洗正冲洗时间","ns=3;s=RO2_SET_JYCXZC_TIME"]
["RO2Set开机冲洗时间","ns=3;s=RO2_SET_KJCX_TIME"]
["RO2SET_ORP","ns=3;s=RO2_SET_ORP"]
["RO2SET_气水混洗时间","ns=3;s=RO2_SET_QSHX_TIEM"]
["RO2Set_水反洗排气时间","ns=3;s=RO2_SET_SFXPQ_TIME"]
["RO2SET_杀菌后反冲时间","ns=3;s=RO2_SET_SJHFC_TIME"]
["RO2SET_杀菌后正冲时间","ns=3;s=RO2_SET_SJHZC_TIME"]
["RO2SET杀菌流量","ns=3;s=RO2_SET_SJLL"]
["RO2Set停机加药冲洗时间","ns=3;s=RO2_SET_TJJYCX_TIME"]
["RO2SET_预杀菌天数","ns=3;s=RO2_SET_YSJ_DAYS"]
["RO2Set正冲时间","ns=3;s=RO2_SET_ZC_TIME"]
["RO2SET正冲流量","ns=3;s=RO2_SET_ZCLL"]
["RO2步序","ns=3;s=RO2_STEP"]
["RO2总产水流量","ns=3;s=RO2_TOTAL_CSLL"]
["RO2总过滤次数","ns=3;s=RO2_TOTAL_GL_CS"]
["RO2总进水流量","ns=3;s=RO2_TOTAL_JSLL"]
["RO2总浓水流量","ns=3;s=RO2_TOTAL_NSLL"]
["RO供水泵电流","ns=3;s=ROGSB_CUR_FB_O"]
["RO供水泵频率反馈","ns=3;s=ROGSB_FRE_FB_O"]
["酸液位","ns=3;s=S_LEVEL_O"]
["杀菌剂液位","ns=3;s=SJJ_LEVEL_O"]
["UF产水浊度","ns=3;s=UF_CS_ZD_O"]
["UF产水箱液位","ns=3;s=UF_CSLEVEL_O"]
["UF1反洗次数显示","ns=3;s=UF1_OUT_BW_CS"]
["UF1反洗流量累计","ns=3;s=UF1_OUT_BW_FLOW_ADD"]
["UF1反洗总次数累计","ns=3;s=UF1_OUT_BW_ZCS"]
["UF1过滤流量累计","ns=3;s=UF1_OUT_GL_FLOW_ADD"]
["UF1系统显示时间","ns=3;s=UF1_OUT_SYS_TIME"]
["UF1跨膜压差","ns=3;s=UF1_SSD_KMYC"]
["UF1步序","ns=3;s=UF1_STEP"]
["UF2反洗次数显示","ns=3;s=UF2_OUT_BW_CS"]
["UF2反洗流量累计","ns=3;s=UF2_OUT_BW_FLOW_ADD"]
["UF2反洗总次数累计","ns=3;s=UF2_OUT_BW_ZCS"]
["UF2过滤流量累计","ns=3;s=UF2_OUT_GL_FLOW_ADD"]
["UF2系统显示时间","ns=3;s=UF2_OUT_SYS_TIME"]
["UF2跨膜压差","ns=3;s=UF2_SSD_KMYC"]
["UF2步序","ns=3;s=UF2_STEP"]
["UF供水泵电流","ns=3;s=UFGSB_CUR_FB_O"]
["UF供水泵频率反馈","ns=3;s=UFGSB_FRE_FB_O"]
["UF供水泵后轴温度反馈","ns=3;s=UFGSB_HZ_TEMP_O"]
["UF供水泵前轴温度反馈","ns=3;s=UFGSB_QZ_TEMP_O"]
["UF1调节阀开度反馈","ns=3;s=V_UF1_TJV_KD_FB"]
["UF2调节阀开度反馈","ns=3;s=V_UF2_TJV_KD_FB"]
["阻垢剂液位","ns=3;s=ZGJ_LEVEL_O"]
["中和水箱液位","ns=3;s=ZH_LEVEL_O"]
["中和水箱ORP","ns=3;s=ZH_ORP_O"]
["中和水箱PH","ns=3;s=ZH_PH_O"]
["中和泵后轴温度","ns=3;s=ZHB_HZ_TEMP_O"]
["中和泵前轴温度","ns=3;s=ZHB_QZ_TEMP_O"]
["进水压力","ns=3;s=ZJS_PRESS_O"]
["进水温度","ns=3;s=ZJS_TEMP_O"]
["UF进水浊度","ns=3;s=ZJS_ZD_O"]
["2号阻垢剂泵给RO1用","ns=6;s=PUBLIC_BYZGJB4_1"]
["2号阻垢剂泵给RO2用","ns=6;s=PUBLIC_BYZGJB4_2"]
["UF其它设备CEB中","ns=6;s=PUBLIC_OTHER_CEBING"]
["UF其它设备反洗中","ns=6;s=PUBLIC_OTHER_BWING"]
["其它RO在过滤中","ns=6;s=PUBLIC_OTHERRO_GLING"]
["RO其他设备杀菌中","ns=6;s=PUBLIC_RO_OTHER_SJ"]
["RO其他设备冲洗中","ns=6;s=PUBLIC_RO_OTHER_CX"]
["RO_系统自动","ns=6;s=PUBLIC_RO_SYS_AUOTO"]
["RO_系统手动","ns=6;s=PUBLIC_RO_SYS_MAN"]
["UF系统自动","ns=6;s=PUBLIC_UF_SYS_AUTO"]
["UF系统手动","ns=6;s=PUBLIC_UF_SYS_MAN"]
["UF1_TJF_PID模式","ns=6;s=PUBLIC_UF1_TJF_PID"]
["UF2_TJF_PID模式","ns=6;s=PUBLIC_UF2_TJF_PID"]
["RO1系统报错","ns=6;s=PUBLIC_BY_B00L_1"]
["RO2系统报错","ns=6;s=PUBLIC_BY_BOOL_2"]
["UF2 PID频率输出","ns=3;s=PUBLIC_2#UF_FXB_PID"]
["2号垢剂泵切换","ns=3;s=PUBLIC_BYZGJB_QH"]
["RO_回用水泵频率PID输出","ns=3;s=PUBLIC_RO_HYSB_PID_S"]
["RO_手动输入运行数量","ns=3;s=PUBLIC_RO_MAN_SETNUM"]
["RO1_段间泵频率PID输出","ns=3;s=PUBLIC_RO1_DJB_PID_S"]
["RO1_高压泵频率PID输出","ns=3;s=PUBLIC_RO1_GYB_PID_S"]
["RO1膜通量","ns=3;s=PUBLIC_RO1_MTL"]
["RO2_段间泵频率PID输出","ns=3;s=PUBLIC_RO2_DJB_PID_S"]
["RO2_高压泵频率PID输出","ns=3;s=PUBLIC_RO2_GYB_PID_S"]
["RO2膜通量","ns=3;s=PUBLIC_RO2_MTL"]
["RO反洗泵定频OUT","ns=3;s=PUBLIC_RO_FXB_FRE_S"]
["RO供水泵定频OUT","ns=3;s=PUBLIC_RO_GSB_FRE_S"]
["RO回用水泵恒压值SP","ns=3;s=PUBLIC_RO_HYSB_SP"]
["UF1 PID频率输出","ns=3;s=PUBLIC_1#UF_FXB_PID"]
["UF手动输入运行数量","ns=3;s=PUBLIC_UF_MAN_SETNUM"]
["UF1调节阀PID开度","ns=3;s=PUBLIC_UF1_TJV_PID_O"]
["UF1冲水排气调节阀开度set","ns=3;s=PUBLIC_UF1TJFCSPQSET"]
["UF1过滤起始调节阀PID开度set","ns=3;s=PUBLIC_UF1TJFGLSET"]
["UF2调节阀PID开度","ns=3;s=PUBLIC_UF2_TJV_PID_O"]
["UF2冲水排气调节阀开度set","ns=3;s=PUBLIC_UF2TJFCSPQSET"]
["UF2过滤起始调节阀PID开度set","ns=3;s=PUBLIC_UF2TJFGLSET"]
["UF反洗泵流量SP","ns=3;s=PUBLIC_UF_FXB_LL_S"]
["UF反洗泵频率OUT","ns=3;s=PUBLIC_UF_FXB_FRE_S"]
["UF供水泵频率OUT","ns=3;s=PUBLIC_UF_GSB_FRE_S"]
["RO1三段压差","ns=3;s=PUBLIC_BY_REAL_1"]
["RO2三段压差","ns=3;s=PUBLIC_BY_REAL_2"]
["反渗透外供泵正向有功电能","ns=3;s=ZZ_ROWGB_EP"]
["反渗透外供泵总功率","ns=3;s=ZZ_ROWGB_POWER"]
["1#RO段间泵正向有功电能","ns=3;s=ZZ_1#RODJB_EP"]
["1#RO段间泵总功率","ns=3;s=ZZ_1#RODJB_POWER"]
["1#RO高压泵正向有功电能","ns=3;s=ZZ_1#ROGYB_EP"]
["1#RO高压泵总功率","ns=3;s=ZZ_1#ROGYB_POWER"]
["1#UF反洗泵正向有功电能","ns=3;s=ZZ_1#UFBWB_EP"]
["1#UF反洗泵总功率","ns=3;s=ZZ_1#UFBWB_POWER"]
["大流量冲洗泵正向有功电能","ns=3;s=ZZ_DLLCXB_EP"]
["大流量冲洗泵总功率","ns=3;s=ZZ_DLLCXB_POWER"]
["2#RO段间泵正向有功电能","ns=3;s=ZZ_2#RODJB_EP"]
["2#RO段间泵总功率","ns=3;s=ZZ_2#RODJB_POWER"]
["2#RO高压泵正向有功电能","ns=3;s=ZZ_2#ROGYB_EP"]
["2#RO高压泵总功率","ns=3;s=ZZ_2#ROGYB_POWER"]
["2#UF反洗泵正向有功电能","ns=3;s=ZZ_2#UFBWB_EP"]
["2#UF反洗泵总功率","ns=3;s=ZZ_2#UFBWB_POWER"]
["泵房柜总进线正向有功电能","ns=3;s=ZZ_BFGZJX_EP"]
["泵房柜总进线总功率","ns=3;s=ZZ_BFGZJX_POWER"]
["超滤柜总进线正向有功电能","ns=3;s=ZZ_UFGZJX_EP"]
["超滤柜总进线总功率","ns=3;s=ZZ_UFGZJX_POWER"]
["2#反渗透柜总进线正向有功电能","ns=3;s=ZZ_2#ROGZJX_EP"]
["2#反渗透柜总进线总功率","ns=3;s=ZZ_2#ROGZJX_POWER"]
["废水排放泵正向有功电能","ns=3;s=ZZ_FSPFB_EP"]
["废水排放泵总功率","ns=3;s=ZZ_FSPFB_POWER"]
["加药柜总进线正向有功电能","ns=3;s=ZZ_JYGZJX_EP"]
["加药柜总进线总功率","ns=3;s=ZZ_JYGZJX_POWER"]
["1#反渗透柜总进线正向有功电能","ns=3;s=ZZ_1#ROGZJX_EP"]
["1#反渗透柜总进线总功率","ns=3;s=ZZ_1#ROGZJX_POWER"]
["1#照明模块第一路","ns=3;s=ZZ_MB_1#ZM1"]
["1#照明模块第二路","ns=3;s=ZZ_MB_1#ZM2"]
["1#照明模块第三路","ns=3;s=ZZ_MB_1#ZM3"]
["1#照明模块第四路","ns=3;s=ZZ_MB_1#ZM4"]
["1#照明模块第五路","ns=3;s=ZZ_MB_1#ZM5"]
["1#照明模块第六路","ns=3;s=ZZ_MB_1#ZM6"]
["2#照明模块第一路","ns=3;s=ZZ_MB_2#ZM1"]
["2#照明模块第二路","ns=3;s=ZZ_MB_2#ZM2"]
["2#照明模块第三路","ns=3;s=ZZ_MB_2#ZM3"]
["2#照明模块第四路","ns=3;s=ZZ_MB_2#ZM4"]
["2#照明模块第五路","ns=3;s=ZZ_MB_2#ZM5"]
["2#照明模块第六路","ns=3;s=ZZ_MB_2#ZM6"]
["3#照明模块第一路","ns=3;s=ZZ_MB_3#ZM1"]
["3#照明模块第二路","ns=3;s=ZZ_MB_3#ZM2"]
["3#照明模块第三路","ns=3;s=ZZ_MB_3#ZM3"]
["3#照明模块第四路","ns=3;s=ZZ_MB_3#ZM4"]
["3#照明模块第五路","ns=3;s=ZZ_MB_3#ZM5"]
["3#照明模块第六路","ns=3;s=ZZ_MB_3#ZM6"]
["4#照明模块第一路","ns=3;s=ZZ_MB_4#ZM1"]
["4#照明模块第二路","ns=3;s=ZZ_MB_4#ZM2"]
["4#照明模块第三路","ns=3;s=ZZ_MB_4#ZM3"]
["4#照明模块第四路","ns=3;s=ZZ_MB_4#ZM4"]
["4#照明模块第五路","ns=3;s=ZZ_MB_4#ZM5"]
["4#照明模块第六路","ns=3;s=ZZ_MB_4#ZM6"]
["湿度9#","ns=3;s=ZZ_MB_SD9"]
["温度9#","ns=3;s=ZZ_MB_WD9"]
["湿度4#","ns=3;s=ZZ_MB_SD4"]
["温度4#","ns=3;s=ZZ_MB_WD4"]
["湿度10#","ns=3;s=ZZ_MB_SD10"]
["温度10#","ns=3;s=ZZ_MB_WD10"]
["烟感9#","ns=3;s=ZZ_MB_YG9"]
["烟感4#","ns=3;s=ZZ_MB_YG4"]
["烟感10#","ns=3;s=ZZ_MB_YG10"]
["湿度11#","ns=3;s=ZZ_MB_SD11"]
["温度11#","ns=3;s=ZZ_MB_WD11"]
["湿度5#","ns=3;s=ZZ_MB_SD5"]
["温度5#","ns=3;s=ZZ_MB_WD5"]
["烟感11#","ns=3;s=ZZ_MB_YG11"]
["烟感5#","ns=3;s=ZZ_MB_YG5"]
["RO供水泵正向有功电能","ns=3;s=ZZ_ROGSB_EP"]
["RO供水泵总功率","ns=3;s=ZZ_ROGSB_POWER"]
["UF供水泵正向有功电能","ns=3;s=ZZ_UFGSB_EP"]
["UF供水泵总功率","ns=3;s=ZZ_UFGSB_POWER"]
["中和废水泵正向有功电能","ns=3;s=ZZ_ZHFSB_EP"]
["中和废水泵总功率","ns=3;s=ZZ_ZHFSB_POWER"]
["RO1三段压差读取","ns=3;s=RO1_EX_3DYCREAD"]
["RO2三段压差读取","ns=3;s=RO2_EX_3DYCREAD"]
["RO产水池启动RO数量0","ns=3;s=YWLD_RO_CSC_LDUPNUM0"]
["RO产水池启动RO数量1","ns=3;s=YWLD_RO_CSC_LDUPNUM1"]
["RO产水池启动RO数量2","ns=3;s=YWLD_RO_CSC_LDUPNUM2"]
["RO产水池启动二套RO液位","ns=3;s=YWLD_RO_CSC_LDYWR[0]"]
["RO产水池启动一套RO液位","ns=3;s=YWLD_RO_CSC_LDYWR[1]"]
["RO产水池停止RO液位","ns=3;s=YWLD_RO_CSC_LDYWR[2]"]
["RO进水池启动数量0","ns=3;s=YWLD_RO_JSC_LDUPNUM0"]
["RO进水池启动RO数量1","ns=3;s=YWLD_RO_JSC_LDUPNUM1"]
["RO进水池启动RO数量2","ns=3;s=YWLD_RO_JSC_LDUPNUM2"]
["RO进水箱停RO液位","ns=3;s=YWLD_RO_JSC_LDYWR[0]"]
["RO进水箱启动一套RO液位","ns=3;s=YWLD_RO_JSC_LDYWR[1]"]
["RO进水箱启动二套RO液位","ns=3;s=YWLD_RO_JSC_LDYWR[2]"]
["RO产水池启动RO数量","ns=3;s=YWLD_SSDROCSCNEEDNUM"]
["RO进水池启动RO数量","ns=3;s=YWLD_SSDROJSCNEEDNUM"]
["UF产水池启动UF数量","ns=3;s=YWLD_SSDUFCSCNEEDNUM"]
["UF进水池启动UF数量","ns=3;s=YWLD_SSDUFJSCNEEDNUM"]
["UF自动液位启动数量","ns=3;s=YWLD_SSDUFNEEDNUM_YW"]
["UF产水池启动UF数量0","ns=3;s=YWLD_UF_CSC_LDUPNUM0"]
["UF产水池启动UF数量1","ns=3;s=YWLD_UF_CSC_LDUPNUM1"]
["UF产水池启动UF数量2","ns=3;s=YWLD_UF_CSC_LDUPNUM2"]
["UF产水箱启两套UF液位","ns=3;s=YWLD_UF_CSC_LDYWR[0]"]
["UF产水箱启一套UF液位","ns=3;s=YWLD_UF_CSC_LDYWR[1]"]
["UF产水箱启零套UF液位","ns=3;s=YWLD_UF_CSC_LDYWR[2]"]
["UF进水池启动数量0","ns=3;s=YWLD_UF_JSC_LDUPNUM0"]
["UF进水池启动数量1","ns=3;s=YWLD_UF_JSC_LDUPNUM1"]
["UF进水池启动数量2","ns=3;s=YWLD_UF_JSC_LDUPNUM2"]
["UF进水池停UF液位","ns=3;s=YWLD_UF_JSC_LDYWR[0]"]
["UF进水池启动一套UF液位","ns=3;s=YWLD_UF_JSC_LDYWR[1]"]
["UF进水池启动二套UF液位","ns=3;s=YWLD_UF_JSC_LDYWR[2]"]
["反洗水泵A震动温度","ns=3;s=ZZ_FXSB_A_ZD_WD"]
["反洗水泵A震动X轴速度","ns=3;s=ZZ_FXSB_A_ZD_XZSD"]
["反洗水泵A震动X轴位移","ns=3;s=ZZ_FXSB_A_ZD_XZWY"]
["反洗水泵A震动Y轴速度","ns=3;s=ZZ_FXSB_A_ZD_YZSD"]
["反洗水泵A震动Y轴位移","ns=3;s=ZZ_FXSB_A_ZD_YZWY"]
["反洗水泵A震动Z轴速度","ns=3;s=ZZ_FXSB_A_ZD_ZZSD"]
["反洗水泵A震动Z轴位移","ns=3;s=ZZ_FXSB_A_ZD_ZZWY"]
["反洗水泵B震动温度","ns=3;s=ZZ_FXSB_B_ZD_WD"]
["反洗水泵B震动X轴速度","ns=3;s=ZZ_FXSB_B_ZD_XZSD"]
["反洗水泵B震动X轴位移","ns=3;s=ZZ_FXSB_B_ZD_XZWY"]
["反洗水泵B震动Y轴速度","ns=3;s=ZZ_FXSB_B_ZD_YZSD"]
["反洗水泵B震动Y轴位移","ns=3;s=ZZ_FXSB_B_ZD_YZWY"]
["反洗水泵B震动Z轴速度","ns=3;s=ZZ_FXSB_B_ZD_ZZSD"]
["反洗水泵B震动Z轴位移","ns=3;s=ZZ_FXSB_B_ZD_ZZWY"]
["大流量冲洗泵震动温度","ns=3;s=ZZ_DLLCXB_ZD_WD"]
["大流量冲洗泵震动X轴速度","ns=3;s=ZZ_DLLCXB_ZD_XZSD"]
["大流量冲洗泵震动X轴位移","ns=3;s=ZZ_DLLCXB_ZD_XZWY"]
["大流量冲洗泵震动Y轴速度","ns=3;s=ZZ_DLLCXB_ZD_YZSD"]
["大流量冲洗泵震动Y轴位移","ns=3;s=ZZ_DLLCXB_ZD_YZWY"]
["大流量冲洗泵震动Z轴速度","ns=3;s=ZZ_DLLCXB_ZD_ZZSD"]
["大流量冲洗泵震动Z轴位移","ns=3;s=ZZ_DLLCXB_ZD_ZZWY"]
["超滤供水泵震动温度","ns=3;s=ZZ_UFGSB_ZD_WD"]
["超滤供水泵震动X轴速度","ns=3;s=ZZ_UFGSB_ZD_XZSD"]
["超滤供水泵震动X轴位移","ns=3;s=ZZ_UFGSB_ZD_XZWY"]
["超滤供水泵震动Y轴速度","ns=3;s=ZZ_UFGSB_ZD_YZSD"]
["超滤供水泵震动Y轴位移","ns=3;s=ZZ_UFGSB_ZD_YZWY"]
["超滤供水泵震动Z轴速度","ns=3;s=ZZ_UFGSB_ZD_ZZSD"]
["超滤供水泵震动Z轴位移","ns=3;s=ZZ_UFGSB_ZD_ZZWY"]
["RO供水泵震动温度","ns=3;s=ZZ_ROGSB_ZD_WD"]
["RO供水泵震动X轴速度","ns=3;s=ZZ_ROGSB_ZD_XZSD"]
["RO供水泵震动X轴位移","ns=3;s=ZZ_ROGSB_ZD_XZWY"]
["RO供水泵震动Y轴速度","ns=3;s=ZZ_ROGSB_ZD_YZSD"]
["RO供水泵震动Y轴位移","ns=3;s=ZZ_ROGSB_ZD_YZWY"]
["RO供水泵震动Z轴速度","ns=3;s=ZZ_ROGSB_ZD_ZZSD"]
["RO供水泵震动Z轴位移","ns=3;s=ZZ_ROGSB_ZD_ZZWY"]
["外供水泵震动温度","ns=3;s=ZZ_WGSB_ZD_WD"]
["外供水泵震动X轴速度","ns=3;s=ZZ_WGSB_ZD_XZSD"]
["外供水泵震动X轴位移","ns=3;s=ZZ_WGSB_ZD_XZWY"]
["外供水泵震动Y轴速度","ns=3;s=ZZ_WGSB_ZD_YZSD"]
["外供水泵震动Y轴位移","ns=3;s=ZZ_WGSB_ZD_YZWY"]
["外供水泵震动Z轴速度","ns=3;s=ZZ_WGSB_ZD_ZZSD"]
["外供水泵震动Z轴位移","ns=3;s=ZZ_WGSB_ZD_ZZWY"]
["RO1三段压差高","ns=6;s=RO1_EX_3DYCG"]
["RO1一段进水压力高","ns=6;s=RO1_EX_PRESSHH_11"]
["RO1一段浓水压力高","ns=6;s=RO1_EX_PRESSHH_12"]
["RO1二段压力高","ns=6;s=RO1_EX_PRESSHH_22"]
["RO1三段进水压力高","ns=6;s=RO1_EX_PRESSHH_31"]
["RO1三段浓水压力高","ns=6;s=RO1_EX_PRESSHH_32"]
["RO1_FLG_段间泵出口压力大","ns=6;s=RO1_EX2_DJBCKYLD"]
["RO1_FLG_高压泵出口压力大","ns=6;s=RO1_EX2_FLG_GYBCKYLD"]
["RO1_FLG_过滤停机不冲洗","ns=6;s=RO1_EX2_FLG_TJBCX"]
["RO1_FLG_过滤停机整体冲洗","ns=6;s=RO1_EX2_FLG_TJZTCX"]
["RO1_FLG_膜里有药","ns=6;s=RO1_EX2_MLYY"]
["RO1_FLG_过滤停机冲二三段","ns=6;s=RO1_EX2_TJC23D"]
["RO2三段压差高","ns=6;s=RO2_EX_3DYCG"]
["RO2一段进水压力高","ns=6;s=RO2_EX_PRESSHH_11"]
["RO2一段浓水压力高","ns=6;s=RO2_EX_PRESSHH_12"]
["RO2二段压力高","ns=6;s=RO2_EX_PRESSHH_22"]
["RO2三段进水压力高","ns=6;s=RO2_EX_PRESSHH_31"]
["RO2三段浓水压力高","ns=6;s=RO2_EX_PRESSHH_32"]
["RO2_FLG_段间泵出口压力大","ns=6;s=RO2_EX2_DJBCKYLD"]
["RO2_FLG_高压泵出口压力大","ns=6;s=RO2_EX2_FLG_GYBCKYLD"]
["RO2_FLG_过滤停机不冲洗","ns=6;s=RO2_EX2_FLG_TJBCX"]
["RO2_FLG_过滤停机整体冲洗","ns=6;s=RO2_EX2_FLG_TJZTCX"]
["RO2_FLG_膜里有药","ns=6;s=RO2_EX2_MLYY"]
["RO2_FLG_过滤停机冲二三段","ns=6;s=RO2_EX2_TJC23D"]
["加药间1噪音频率1","ns=3;s=ZZ_ZY_FR1"]
["加药间1噪音频率10","ns=3;s=ZZ_ZY_FR10"]
["加药间1噪音频率100","ns=3;s=ZZ_ZY_FR100"]
["加药间1噪音频率101","ns=3;s=ZZ_ZY_FR101"]
["加药间1噪音频率102","ns=3;s=ZZ_ZY_FR102"]
["加药间1噪音频率103","ns=3;s=ZZ_ZY_FR103"]
["加药间1噪音频率104","ns=3;s=ZZ_ZY_FR104"]
["加药间1噪音频率105","ns=3;s=ZZ_ZY_FR105"]
["加药间1噪音频率106","ns=3;s=ZZ_ZY_FR106"]
["加药间1噪音频率107","ns=3;s=ZZ_ZY_FR107"]
["加药间1噪音频率108","ns=3;s=ZZ_ZY_FR108"]
["加药间1噪音频率109","ns=3;s=ZZ_ZY_FR109"]
["加药间1噪音频率11","ns=3;s=ZZ_ZY_FR11"]
["加药间1噪音频率110","ns=3;s=ZZ_ZY_FR110"]
["加药间1噪音频率111","ns=3;s=ZZ_ZY_FR111"]
["加药间1噪音频率112","ns=3;s=ZZ_ZY_FR112"]
["加药间1噪音频率113","ns=3;s=ZZ_ZY_FR113"]
["加药间1噪音频率114","ns=3;s=ZZ_ZY_FR114"]
["加药间1噪音频率115","ns=3;s=ZZ_ZY_FR115"]
["加药间1噪音频率116","ns=3;s=ZZ_ZY_FR116"]
["加药间1噪音频率117","ns=3;s=ZZ_ZY_FR117"]
["加药间1噪音频率118","ns=3;s=ZZ_ZY_FR118"]
["加药间1噪音频率119","ns=3;s=ZZ_ZY_FR119"]
["加药间1噪音频率12","ns=3;s=ZZ_ZY_FR12"]
["加药间1噪音频率120","ns=3;s=ZZ_ZY_FR120"]
["加药间1噪音频率121","ns=3;s=ZZ_ZY_FR121"]
["加药间1噪音频率122","ns=3;s=ZZ_ZY_FR122"]
["加药间1噪音频率123","ns=3;s=ZZ_ZY_FR123"]
["加药间1噪音频率124","ns=3;s=ZZ_ZY_FR124"]
["加药间1噪音频率125","ns=3;s=ZZ_ZY_FR125"]
["加药间1噪音频率126","ns=3;s=ZZ_ZY_FR126"]
["加药间1噪音频率127","ns=3;s=ZZ_ZY_FR127"]
["加药间1噪音频率13","ns=3;s=ZZ_ZY_FR13"]
["加药间1噪音频率14","ns=3;s=ZZ_ZY_FR14"]
["加药间1噪音频率15","ns=3;s=ZZ_ZY_FR15"]
["加药间1噪音频率16","ns=3;s=ZZ_ZY_FR16"]
["加药间1噪音频率17","ns=3;s=ZZ_ZY_FR17"]
["加药间1噪音频率18","ns=3;s=ZZ_ZY_FR18"]
["加药间1噪音频率19","ns=3;s=ZZ_ZY_FR19"]
["加药间1噪音频率2","ns=3;s=ZZ_ZY_FR2"]
["加药间1噪音频率20","ns=3;s=ZZ_ZY_FR20"]
["加药间1噪音频率21","ns=3;s=ZZ_ZY_FR21"]
["加药间1噪音频率22","ns=3;s=ZZ_ZY_FR22"]
["加药间1噪音频率23","ns=3;s=ZZ_ZY_FR23"]
["加药间1噪音频率24","ns=3;s=ZZ_ZY_FR24"]
["加药间1噪音频率25","ns=3;s=ZZ_ZY_FR25"]
["加药间1噪音频率26","ns=3;s=ZZ_ZY_FR26"]
["加药间1噪音频率27","ns=3;s=ZZ_ZY_FR27"]
["加药间1噪音频率28","ns=3;s=ZZ_ZY_FR28"]
["加药间1噪音频率29","ns=3;s=ZZ_ZY_FR29"]
["加药间1噪音频率3","ns=3;s=ZZ_ZY_FR3"]
["加药间1噪音频率30","ns=3;s=ZZ_ZY_FR30"]
["加药间1噪音频率31","ns=3;s=ZZ_ZY_FR31"]
["加药间1噪音频率32","ns=3;s=ZZ_ZY_FR32"]
["加药间1噪音频率33","ns=3;s=ZZ_ZY_FR33"]
["加药间1噪音频率34","ns=3;s=ZZ_ZY_FR34"]
["加药间1噪音频率35","ns=3;s=ZZ_ZY_FR35"]
["加药间1噪音频率36","ns=3;s=ZZ_ZY_FR36"]
["加药间1噪音频率37","ns=3;s=ZZ_ZY_FR37"]
["加药间1噪音频率38","ns=3;s=ZZ_ZY_FR38"]
["加药间1噪音频率39","ns=3;s=ZZ_ZY_FR39"]
["加药间1噪音频率4","ns=3;s=ZZ_ZY_FR4"]
["加药间1噪音频率40","ns=3;s=ZZ_ZY_FR40"]
["加药间1噪音频率41","ns=3;s=ZZ_ZY_FR41"]
["加药间1噪音频率42","ns=3;s=ZZ_ZY_FR42"]
["加药间1噪音频率43","ns=3;s=ZZ_ZY_FR43"]
["加药间1噪音频率44","ns=3;s=ZZ_ZY_FR44"]
["加药间1噪音频率45","ns=3;s=ZZ_ZY_FR45"]
["加药间1噪音频率46","ns=3;s=ZZ_ZY_FR46"]
["加药间1噪音频率47","ns=3;s=ZZ_ZY_FR47"]
["加药间1噪音频率48","ns=3;s=ZZ_ZY_FR48"]
["加药间1噪音频率49","ns=3;s=ZZ_ZY_FR49"]
["加药间1噪音频率5","ns=3;s=ZZ_ZY_FR5"]
["加药间1噪音频率50","ns=3;s=ZZ_ZY_FR50"]
["加药间1噪音频率51","ns=3;s=ZZ_ZY_FR51"]
["加药间1噪音频率52","ns=3;s=ZZ_ZY_FR52"]
["加药间1噪音频率53","ns=3;s=ZZ_ZY_FR53"]
["加药间1噪音频率54","ns=3;s=ZZ_ZY_FR54"]
["加药间1噪音频率55","ns=3;s=ZZ_ZY_FR55"]
["加药间1噪音频率56","ns=3;s=ZZ_ZY_FR56"]
["加药间1噪音频率57","ns=3;s=ZZ_ZY_FR57"]
["加药间1噪音频率58","ns=3;s=ZZ_ZY_FR58"]
["加药间1噪音频率59","ns=3;s=ZZ_ZY_FR59"]
["加药间1噪音频率6","ns=3;s=ZZ_ZY_FR6"]
["加药间1噪音频率60","ns=3;s=ZZ_ZY_FR60"]
["加药间1噪音频率61","ns=3;s=ZZ_ZY_FR61"]
["加药间1噪音频率62","ns=3;s=ZZ_ZY_FR62"]
["加药间1噪音频率63","ns=3;s=ZZ_ZY_FR63"]
["加药间1噪音频率64","ns=3;s=ZZ_ZY_FR64"]
["加药间1噪音频率65","ns=3;s=ZZ_ZY_FR65"]
["加药间1噪音频率66","ns=3;s=ZZ_ZY_FR66"]
["加药间1噪音频率67","ns=3;s=ZZ_ZY_FR67"]
["加药间1噪音频率68","ns=3;s=ZZ_ZY_FR68"]
["加药间1噪音频率69","ns=3;s=ZZ_ZY_FR69"]
["加药间1噪音频率7","ns=3;s=ZZ_ZY_FR7"]
["加药间1噪音频率70","ns=3;s=ZZ_ZY_FR70"]
["加药间1噪音频率71","ns=3;s=ZZ_ZY_FR71"]
["加药间1噪音频率72","ns=3;s=ZZ_ZY_FR72"]
["加药间1噪音频率73","ns=3;s=ZZ_ZY_FR73"]
["加药间1噪音频率74","ns=3;s=ZZ_ZY_FR74"]
["加药间1噪音频率75","ns=3;s=ZZ_ZY_FR75"]
["加药间1噪音频率76","ns=3;s=ZZ_ZY_FR76"]
["加药间1噪音频率77","ns=3;s=ZZ_ZY_FR77"]
["加药间1噪音频率78","ns=3;s=ZZ_ZY_FR78"]
["加药间1噪音频率79","ns=3;s=ZZ_ZY_FR79"]
["加药间1噪音频率8","ns=3;s=ZZ_ZY_FR8"]
["加药间1噪音频率80","ns=3;s=ZZ_ZY_FR80"]
["加药间1噪音频率81","ns=3;s=ZZ_ZY_FR81"]
["加药间1噪音频率82","ns=3;s=ZZ_ZY_FR82"]
["加药间1噪音频率83","ns=3;s=ZZ_ZY_FR83"]
["加药间1噪音频率84","ns=3;s=ZZ_ZY_FR84"]
["加药间1噪音频率85","ns=3;s=ZZ_ZY_FR85"]
["加药间1噪音频率86","ns=3;s=ZZ_ZY_FR86"]
["加药间1噪音频率87","ns=3;s=ZZ_ZY_FR87"]
["加药间1噪音频率88","ns=3;s=ZZ_ZY_FR88"]
["加药间1噪音频率89","ns=3;s=ZZ_ZY_FR89"]
["加药间1噪音频率9","ns=3;s=ZZ_ZY_FR9"]
["加药间1噪音频率90","ns=3;s=ZZ_ZY_FR90"]
["加药间1噪音频率91","ns=3;s=ZZ_ZY_FR91"]
["加药间1噪音频率92","ns=3;s=ZZ_ZY_FR92"]
["加药间1噪音频率93","ns=3;s=ZZ_ZY_FR93"]
["加药间1噪音频率94","ns=3;s=ZZ_ZY_FR94"]
["加药间1噪音频率95","ns=3;s=ZZ_ZY_FR95"]
["加药间1噪音频率96","ns=3;s=ZZ_ZY_FR96"]
["加药间1噪音频率97","ns=3;s=ZZ_ZY_FR97"]
["加药间1噪音频率98","ns=3;s=ZZ_ZY_FR98"]
["加药间1噪音频率99","ns=3;s=ZZ_ZY_FR99"]
["加药间2噪音频率1","ns=3;s=ZZ_ZY2_FR1"]
["加药间2噪音频率10","ns=3;s=ZZ_ZY2_FR10"]
["加药间2噪音频率100","ns=3;s=ZZ_ZY2_FR100"]
["加药间2噪音频率101","ns=3;s=ZZ_ZY2_FR101"]
["加药间2噪音频率102","ns=3;s=ZZ_ZY2_FR102"]
["加药间2噪音频率103","ns=3;s=ZZ_ZY2_FR103"]
["加药间2噪音频率104","ns=3;s=ZZ_ZY2_FR104"]
["加药间2噪音频率105","ns=3;s=ZZ_ZY2_FR105"]
["加药间2噪音频率106","ns=3;s=ZZ_ZY2_FR106"]
["加药间2噪音频率107","ns=3;s=ZZ_ZY2_FR107"]
["加药间2噪音频率108","ns=3;s=ZZ_ZY2_FR108"]
["加药间2噪音频率109","ns=3;s=ZZ_ZY2_FR109"]
["加药间2噪音频率11","ns=3;s=ZZ_ZY2_FR11"]
["加药间2噪音频率110","ns=3;s=ZZ_ZY2_FR110"]
["加药间2噪音频率111","ns=3;s=ZZ_ZY2_FR111"]
["加药间2噪音频率112","ns=3;s=ZZ_ZY2_FR112"]
["加药间2噪音频率113","ns=3;s=ZZ_ZY2_FR113"]
["加药间2噪音频率114","ns=3;s=ZZ_ZY2_FR114"]
["加药间2噪音频率115","ns=3;s=ZZ_ZY2_FR115"]
["加药间2噪音频率116","ns=3;s=ZZ_ZY2_FR116"]
["加药间2噪音频率117","ns=3;s=ZZ_ZY2_FR117"]
["加药间2噪音频率118","ns=3;s=ZZ_ZY2_FR118"]
["加药间2噪音频率119","ns=3;s=ZZ_ZY2_FR119"]
["加药间2噪音频率12","ns=3;s=ZZ_ZY2_FR12"]
["加药间2噪音频率120","ns=3;s=ZZ_ZY2_FR120"]
["加药间2噪音频率121","ns=3;s=ZZ_ZY2_FR121"]
["加药间2噪音频率122","ns=3;s=ZZ_ZY2_FR122"]
["加药间2噪音频率123","ns=3;s=ZZ_ZY2_FR123"]
["加药间2噪音频率124","ns=3;s=ZZ_ZY2_FR124"]
["加药间2噪音频率125","ns=3;s=ZZ_ZY2_FR125"]
["加药间2噪音频率126","ns=3;s=ZZ_ZY2_FR126"]
["加药间2噪音频率127","ns=3;s=ZZ_ZY2_FR127"]
["加药间2噪音频率13","ns=3;s=ZZ_ZY2_FR13"]
["加药间2噪音频率14","ns=3;s=ZZ_ZY2_FR14"]
["加药间2噪音频率15","ns=3;s=ZZ_ZY2_FR15"]
["加药间2噪音频率16","ns=3;s=ZZ_ZY2_FR16"]
["加药间2噪音频率17","ns=3;s=ZZ_ZY2_FR17"]
["加药间2噪音频率18","ns=3;s=ZZ_ZY2_FR18"]
["加药间2噪音频率19","ns=3;s=ZZ_ZY2_FR19"]
["加药间2噪音频率2","ns=3;s=ZZ_ZY2_FR2"]
["加药间2噪音频率20","ns=3;s=ZZ_ZY2_FR20"]
["加药间2噪音频率21","ns=3;s=ZZ_ZY2_FR21"]
["加药间2噪音频率22","ns=3;s=ZZ_ZY2_FR22"]
["加药间2噪音频率23","ns=3;s=ZZ_ZY2_FR23"]
["加药间2噪音频率24","ns=3;s=ZZ_ZY2_FR24"]
["加药间2噪音频率25","ns=3;s=ZZ_ZY2_FR25"]
["加药间2噪音频率26","ns=3;s=ZZ_ZY2_FR26"]
["加药间2噪音频率27","ns=3;s=ZZ_ZY2_FR27"]
["加药间2噪音频率28","ns=3;s=ZZ_ZY2_FR28"]
["加药间2噪音频率29","ns=3;s=ZZ_ZY2_FR29"]
["加药间2噪音频率3","ns=3;s=ZZ_ZY2_FR3"]
["加药间2噪音频率30","ns=3;s=ZZ_ZY2_FR30"]
["加药间2噪音频率31","ns=3;s=ZZ_ZY2_FR31"]
["加药间2噪音频率32","ns=3;s=ZZ_ZY2_FR32"]
["加药间2噪音频率33","ns=3;s=ZZ_ZY2_FR33"]
["加药间2噪音频率34","ns=3;s=ZZ_ZY2_FR34"]
["加药间2噪音频率35","ns=3;s=ZZ_ZY2_FR35"]
["加药间2噪音频率36","ns=3;s=ZZ_ZY2_FR36"]
["加药间2噪音频率37","ns=3;s=ZZ_ZY2_FR37"]
["加药间2噪音频率38","ns=3;s=ZZ_ZY2_FR38"]
["加药间2噪音频率39","ns=3;s=ZZ_ZY2_FR39"]
["加药间2噪音频率4","ns=3;s=ZZ_ZY2_FR4"]
["加药间2噪音频率40","ns=3;s=ZZ_ZY2_FR40"]
["加药间2噪音频率41","ns=3;s=ZZ_ZY2_FR41"]
["加药间2噪音频率42","ns=3;s=ZZ_ZY2_FR42"]
["加药间2噪音频率43","ns=3;s=ZZ_ZY2_FR43"]
["加药间2噪音频率44","ns=3;s=ZZ_ZY2_FR44"]
["加药间2噪音频率45","ns=3;s=ZZ_ZY2_FR45"]
["加药间2噪音频率46","ns=3;s=ZZ_ZY2_FR46"]
["加药间2噪音频率47","ns=3;s=ZZ_ZY2_FR47"]
["加药间2噪音频率48","ns=3;s=ZZ_ZY2_FR48"]
["加药间2噪音频率49","ns=3;s=ZZ_ZY2_FR49"]
["加药间2噪音频率5","ns=3;s=ZZ_ZY2_FR5"]
["加药间2噪音频率50","ns=3;s=ZZ_ZY2_FR50"]
["加药间2噪音频率51","ns=3;s=ZZ_ZY2_FR51"]
["加药间2噪音频率52","ns=3;s=ZZ_ZY2_FR52"]
["加药间2噪音频率53","ns=3;s=ZZ_ZY2_FR53"]
["加药间2噪音频率54","ns=3;s=ZZ_ZY2_FR54"]
["加药间2噪音频率55","ns=3;s=ZZ_ZY2_FR55"]
["加药间2噪音频率56","ns=3;s=ZZ_ZY2_FR56"]
["加药间2噪音频率57","ns=3;s=ZZ_ZY2_FR57"]
["加药间2噪音频率58","ns=3;s=ZZ_ZY2_FR58"]
["加药间2噪音频率59","ns=3;s=ZZ_ZY2_FR59"]
["加药间2噪音频率6","ns=3;s=ZZ_ZY2_FR6"]
["加药间2噪音频率60","ns=3;s=ZZ_ZY2_FR60"]
["加药间2噪音频率61","ns=3;s=ZZ_ZY2_FR61"]
["加药间2噪音频率62","ns=3;s=ZZ_ZY2_FR62"]
["加药间2噪音频率63","ns=3;s=ZZ_ZY2_FR63"]
["加药间2噪音频率64","ns=3;s=ZZ_ZY2_FR64"]
["加药间2噪音频率65","ns=3;s=ZZ_ZY2_FR65"]
["加药间2噪音频率66","ns=3;s=ZZ_ZY2_FR66"]
["加药间2噪音频率67","ns=3;s=ZZ_ZY2_FR67"]
["加药间2噪音频率68","ns=3;s=ZZ_ZY2_FR68"]
["加药间2噪音频率69","ns=3;s=ZZ_ZY2_FR69"]
["加药间2噪音频率7","ns=3;s=ZZ_ZY2_FR7"]
["加药间2噪音频率70","ns=3;s=ZZ_ZY2_FR70"]
["加药间2噪音频率71","ns=3;s=ZZ_ZY2_FR71"]
["加药间2噪音频率72","ns=3;s=ZZ_ZY2_FR72"]
["加药间2噪音频率73","ns=3;s=ZZ_ZY2_FR73"]
["加药间2噪音频率74","ns=3;s=ZZ_ZY2_FR74"]
["加药间2噪音频率75","ns=3;s=ZZ_ZY2_FR75"]
["加药间2噪音频率76","ns=3;s=ZZ_ZY2_FR76"]
["加药间2噪音频率77","ns=3;s=ZZ_ZY2_FR77"]
["加药间2噪音频率78","ns=3;s=ZZ_ZY2_FR78"]
["加药间2噪音频率79","ns=3;s=ZZ_ZY2_FR79"]
["加药间2噪音频率8","ns=3;s=ZZ_ZY2_FR8"]
["加药间2噪音频率80","ns=3;s=ZZ_ZY2_FR80"]
["加药间2噪音频率81","ns=3;s=ZZ_ZY2_FR81"]
["加药间2噪音频率82","ns=3;s=ZZ_ZY2_FR82"]
["加药间2噪音频率83","ns=3;s=ZZ_ZY2_FR83"]
["加药间2噪音频率84","ns=3;s=ZZ_ZY2_FR84"]
["加药间2噪音频率85","ns=3;s=ZZ_ZY2_FR85"]
["加药间2噪音频率86","ns=3;s=ZZ_ZY2_FR86"]
["加药间2噪音频率87","ns=3;s=ZZ_ZY2_FR87"]
["加药间2噪音频率88","ns=3;s=ZZ_ZY2_FR88"]
["加药间2噪音频率89","ns=3;s=ZZ_ZY2_FR89"]
["加药间2噪音频率9","ns=3;s=ZZ_ZY2_FR9"]
["加药间2噪音频率90","ns=3;s=ZZ_ZY2_FR90"]
["加药间2噪音频率91","ns=3;s=ZZ_ZY2_FR91"]
["加药间2噪音频率92","ns=3;s=ZZ_ZY2_FR92"]
["加药间2噪音频率93","ns=3;s=ZZ_ZY2_FR93"]
["加药间2噪音频率94","ns=3;s=ZZ_ZY2_FR94"]
["加药间2噪音频率95","ns=3;s=ZZ_ZY2_FR95"]
["加药间2噪音频率96","ns=3;s=ZZ_ZY2_FR96"]
["加药间2噪音频率97","ns=3;s=ZZ_ZY2_FR97"]
["加药间2噪音频率98","ns=3;s=ZZ_ZY2_FR98"]
["加药间2噪音频率99","ns=3;s=ZZ_ZY2_FR99"]
["前端补水泵—自动","ns=6;s=QD_BSB_BT_AUTO"]
["前端补水泵——启动","ns=6;s=QD_BSB_BT_START"]
["前端补水泵——停止","ns=6;s=QD_BSB_BT_STOP"]
["前端补水泵——故障","ns=6;s=QD_BSB_FAULT"]
["前端补水泵——输出","ns=6;s=QD_BSB_OUTPUT"]
["前端补水泵——ready","ns=6;s=QD_BSB_READY"]
["前端补水泵——运行反馈","ns=6;s=QD_BSB_RFB"]
["前端补水阀——自动","ns=6;s=QD_BSF_BT_AUTO"]
["前端补水阀——开阀","ns=6;s=QD_BSF_BT_CLOSE"]
["前端补水阀——关阀","ns=6;s=QD_BSF_BT_OPEN"]
["前端补水阀——关ing","ns=6;s=QD_BSF_CING"]
["前端补水阀——自动关","ns=6;s=QD_BSF_CLOSEAUTO"]
["前端补水阀——故障 ","ns=6;s=QD_BSF_ERR"]
["前端补水阀——总故障 ","ns=6;s=QD_BSF_ERRT"]
["前端排气阀故障","ns=6;s=QD_PQF_ERR"]
["前端排气阀总故障","ns=6;s=QD_PQF_ERRT"]
["前端破真空阀故障","ns=6;s=QD_PZKF_ERR"]
["前端破真空阀总故障","ns=6;s=QD_PZKF_ERRT"]
["故障_引水装置补水超时","ns=6;s=QD_QT_44_3"]
["用户华晟-流量计温度","ns=1;s=WG_FLOW_HS2_00"]
["用户华晟-流量计压力","ns=1;s=WG_FLOW_HS2_01"]
["用户华晟-补偿前流量","ns=1;s=WG_FLOW_HS2_02"]
["用户华晟-补偿后流量","ns=1;s=WG_FLOW_HS2_03"]
["用户华晟-累计流量","ns=1;s=WG_FLOW_HS2_04"]
["用户芯动-流量计温度","ns=1;s=WG_FLOW_XD_00"]
["用户芯动-流量计压力","ns=1;s=WG_FLOW_XD_01"]
["用户芯动-补偿前流量","ns=1;s=WG_FLOW_XD_02"]
["用户芯动-补偿后流量","ns=1;s=WG_FLOW_XD_03"]
["用户芯动-累计流量","ns=1;s=WG_FLOW_XD_04"]
["前端补水泵","ns=3;s=QD_BSB_FRE_FB"]
["前端补水泵","ns=3;s=QD_BSB_FRESET"]
["前端补水泵","ns=3;s=QD_BSB_RUNTIME"]
["RO产水加碱频率1套","ns=3;s=QD_LD_R164"]
["RO产水加碱频率2套","ns=3;s=QD_LD_R168"]
["RO产水加碱频率备1","ns=3;s=QD_LD_R172"]
["RO产水加碱频率备2","ns=3;s=QD_LD_R176"]
["前端补水参照时间","ns=3;s=QD_QT_BSTIMESET"]
["前端补水计时","ns=3;s=QD_QT_TIMEADD"]
["前端液位触发后延时补水计时","ns=3;s=QD_QT_TIMEDELAYADD"]
["备","ns=3;s=UF_LD_R152"]
["备","ns=3;s=UF_LD_R156"]
["备","ns=3;s=UF_LD_R182"]
["极点总供水流量计","ns=1;s=WG_FLOW_JD_04"]
["F1空调地址","ns=1;s=ZZ_AC1S_ADR"]
["F1空调波特率","ns=1;s=ZZ_AC1S_BD"]
["F1空调红外状态","ns=1;s=ZZ_AC1S_IR"]
["F1空调湿度","ns=1;s=ZZ_AC1S_RH"]
["F1空调温度","ns=1;s=ZZ_AC1S_T"]
["F1空调运行状态检测信号值","ns=1;s=ZZ_AC1S_VALUE"]
["F2电控柜侧空调地址","ns=1;s=ZZ_AC2S_ADR"]
["F2电控柜侧空调波特率","ns=1;s=ZZ_AC2S_BD"]
["F2电控柜侧空调红外状态","ns=1;s=ZZ_AC2S_IR"]
["F2电控柜侧空调湿度","ns=1;s=ZZ_AC2S_RH"]
["F2电控柜侧空调温度","ns=1;s=ZZ_AC2S_T"]
["F2电控柜侧空调运行状态检测信号值","ns=1;s=ZZ_AC2S_VALUE"]
["F2空调地址","ns=1;s=ZZ_AC3S_ADR"]
["F2空调波特率","ns=1;s=ZZ_AC3S_BD"]
["F2空调红外状态","ns=1;s=ZZ_AC3S_IR"]
["F2空调湿度","ns=1;s=ZZ_AC3S_RH"]
["F2空调温度","ns=1;s=ZZ_AC3S_T"]
["F2空调运行状态检测信号值","ns=1;s=ZZ_AC3S_VALUE"]
["CIP补水阀故障","ns=6;s=V_F_CIPBSF_ERR"]
["CIP补水阀总故障","ns=6;s=V_F_CIPBSF_ERRT"]
["1#超滤提升泵故障","ns=6;s=P_1#UFTSB_FAULT"]
["1#超滤提升泵运行","ns=6;s=P_1#UFTSB_RFB"]
["1#超滤提升泵频率反馈","ns=3;s=P_1#UFTSB_FRE_FB"]
["1#超滤提升泵运行时间","ns=3;s=P_1#UFTSB_RUNTIME"]
["2#超滤提升泵故障","ns=6;s=P_2#UFTSB_FAULT"]
["2#超滤提升泵运行","ns=6;s=P_2#UFTSB_RFB"]
["2#超滤提升泵频率反馈","ns=3;s=P_2#UFTSB_FRE_FB"]
["2#超滤提升泵运行时间","ns=3;s=P_2#UFTSB_RUNTIME"]
["1#湿地提升泵故障","ns=6;s=P_1#SDTSB_FAULT"]
["1#湿地提升泵运行","ns=6;s=P_1#SDTSB_RFB"]
["1#湿地提升泵频率反馈","ns=3;s=P_1#SDTSB_FRE_FB"]
["1#湿地提升泵运行时间","ns=3;s=P_1#SDTSB_RUNTIME"]
["2#湿地提升泵故障","ns=6;s=P_2#SDTSB_FAULT"]
["2#湿地提升泵运行","ns=6;s=P_2#SDTSB_RFB"]
["2#湿地提升泵频率反馈","ns=3;s=P_2#SDTSB_FRE_FB"]
["2#湿地提升泵运行时间","ns=3;s=P_2#SDTSB_RUNTIME"]
["超滤进水取样阀故障","ns=6;s=QYF_UFJS_ERR"]
["超滤进水取样阀总故障","ns=6;s=QYF_UFJS_ERRT"]
["超滤产水取样阀故障","ns=6;s=QYF_UFCS_ERR"]
["超滤产水取样阀总故障","ns=6;s=QYF_UFCS_ERRT"]
["反渗透产水取样阀故障","ns=6;s=QYF_ROCS_ERR"]
["反渗透产水取样阀总故障","ns=6;s=QYF_ROCS_ERRT"]
["反渗透外供水取样阀故障","ns=6;s=QYF_ROWG_ERR"]
["反渗透外供水取样阀总故障","ns=6;s=QYF_ROWG_ERRT"]
["3700","ns=6;s=ZH_END_HCL"]
["3701","ns=6;s=ZH_END_NAOH"]
["3702","ns=6;s=ZH_END_SBS"]
["3703","ns=6;s=ZH_END_TOTAL"]
["3704","ns=6;s=ZH_READY_HCL"]
["3705","ns=6;s=ZH_READY_NAOH"]
["3706","ns=6;s=ZH_READY_SBS"]
["3707","ns=6;s=ZH_READY_TOTAL"]
["3708","ns=6;s=ZH_READY_ZH"]
["3709","ns=3;s=ZH_LT_ZHC_H"]
["3710","ns=3;s=ZH_LT_ZHC_L"]
["3711","ns=3;s=ZH_ORP_H"]
["3712","ns=3;s=ZH_ORP_HH"]
["3713","ns=3;s=ZH_PH_H"]
["3714","ns=3;s=ZH_PH_HH"]
["3715","ns=3;s=ZH_PH_L"]
["3716","ns=3;s=ZH_PH_LL"]
["3717","ns=3;s=ZH_TIME_CYCLE"]
["3718","ns=3;s=ZH_TIME_FAULT"]
["3719","ns=3;s=ZH_TIME_ORP_H"]
["3720","ns=3;s=ZH_TIME_ORP_HH"]
["3721","ns=3;s=ZH_TIME_PH_H"]
["3722","ns=3;s=ZH_TIME_PH_HH"]
["3723","ns=3;s=ZH_TIME_PH_L"]
["3724","ns=3;s=ZH_TIME_PH_LL"]
["3725","ns=3;s=ZH_TIME_RUNING"]
["3726","ns=3;s=ZH_TIME_SET"]
["3727","ns=3;s=ZH_WORD_STEP"]
["2#RO段间泵效率","2#RODJB_Eff"]
["1#RO段间泵效率","1#RODJB_Eff"]
["反渗透外供泵效率","ROWGB_Eff"]
["2#RO高压泵效率","2#ROGYB_Eff"]
["1#RO高压泵效率","1#ROGYB_Eff"]
["反渗透回收率","ROHSL"]