{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":3535,"n_cols":2,"rows_kept":3535,"cut":false,"hidden":false,"merged":[]}
["item_alias","item_name"]
["UF1通量","UF1_FluxF"]
["UF2通量","UF2_FluxF"]
["UF1渗透率","UF1Per"]
["UF2渗透率","UF2Per"]
["RO1二三段产水比","RO1_SPK"]
["RO2二三段产水比","RO2_SPK"]
["进水量","water_in"]
["外供水流量","water_out"]
["总进水水温","AR.ZJS_SW（废）"]
["UF1步序与时长","UF1_DB"]
["UF2步序与时长","UF2_DB"]
["RO1步序与时长","RO1_DB"]
["RO2步序与时长","RO2_DB"]
["温湿度：一楼温度1","WSD_1L_WD_1"]
["温湿度：一楼温度2","WSD_1L_WD_2"]
["温湿度：一楼温度3","WSD_1L_WD_3"]
["温湿度：二楼温度1","WSD_2L_WD_1"]
["温湿度：二楼温度2","WSD_2L_WD_2"]
["1#RO产水流量","1#RO_CSFLOW"]
["2#RO产水流量","2#RO_CSFLOW"]
["进水ORP超高限值报警","AR.RO_JSORP_H"]
["RO1运行时高压泵进口低压开关，关闭","RO1_GYB_JKYLKG_CLOSE_1"]
["RO2运行时高压泵进口低压开关，关闭","RO2_GYB_JKYLKG_CLOSE_1"]
["反渗透进水ORP超高（组态弹窗用）","ORP_CX"]
["次钠加药箱高报警","DR.ALARM_CN_H"]
["次钠加药箱超高报警","DR.ALARM_CN_HH"]
["次钠加药箱低报警","DR.ALARM_CN_L"]
["次钠加药箱超低报警","DR.ALARM_CN_LL"]
["反洗废水箱高报警","DR.ALARM_FSX_H"]
["反洗废水箱超高报警","DR.ALARM_FSX_HH"]
["反洗废水箱低报警","DR.ALARM_FSX_L"]
["反洗废水箱超低报警","DR.ALARM_FSX_LL"]
["还原剂加药箱高报警","DR.ALARM_HYJ_H"]
["还原剂加药箱超高报警","DR.ALARM_HYJ_HH"]
["还原剂加药箱低报警","DR.ALARM_HYJ_L"]
["还原剂加药箱超低报警","DR.ALARM_HYJ_LL"]
["碱加药箱高报警","DR.ALARM_J_H"]
["碱加药箱超高报警","DR.ALARM_J_HH"]
["碱加药箱低报警","DR.ALARM_J_L"]
["碱加药箱超低报警","DR.ALARM_J_LL"]
["超滤原水箱1高报警","DR.ALARM_JSX1_H"]
["超滤原水箱1超高报警","DR.ALARM_JSX1_HH"]
["超滤原水箱1低报警","DR.ALARM_JSX1_L"]
["超滤原水箱1超低报警","DR.ALARM_JSX1_LL"]
["超滤原水箱2高报警","DR.ALARM_JSX2_H"]
["超滤原水箱2超高报警","DR.ALARM_JSX2_HH"]
["超滤原水箱2低报警","DR.ALARM_JSX2_L"]
["超滤原水箱2超低报警","DR.ALARM_JSX2_LL"]
["PAC加药箱高报警","DR.ALARM_PAC_H"]
["PAC加药箱超高报警","DR.ALARM_PAC_HH"]
["PAC加药箱低报警","DR.ALARM_PAC_L"]
["PAC加药箱超低报警","DR.ALARM_PAC_LL"]
["清洗水箱高报警","DR.ALARM_QXSX_H"]
["清洗水箱超高报警","DR.ALARM_QXSX_HH"]
["清洗水箱低报警","DR.ALARM_QXSX_L"]
["清洗水箱超低报警","DR.ALARM_QXSX_LL"]
["反渗透产水箱高报警","DR.ALARM_RO_CSX_H"]
["反渗透产水箱超高报警","DR.ALARM_RO_CSX_HH"]
["反渗透产水箱低报警","DR.ALARM_RO_CSX_L"]
["反渗透产水箱超低报警","DR.ALARM_RO_CSX_LL"]
["酸加药箱高报警","DR.ALARM_S_H"]
["酸加药箱超高报警","DR.ALARM_S_HH"]
["酸加药箱低报警","DR.ALARM_S_L"]
["酸加药箱超低报警","DR.ALARM_S_LL"]
["杀菌剂加药箱高报警","DR.ALARM_SJJ_H"]
["杀菌剂加药箱超高报警","DR.ALARM_SJJ_HH"]
["杀菌剂加药箱低报警","DR.ALARM_SJJ_L"]
["杀菌剂加药箱超低报警","DR.ALARM_SJJ_LL"]
["超滤产水箱高报警","DR.ALARM_UF_CSX_H"]
["超滤产水箱超高报警","DR.ALARM_UF_CSX_HH"]
["超滤产水箱低报警","DR.ALARM_UF_CSX_L"]
["超滤产水箱超低报警","DR.ALARM_UF_CSX_LL"]
["阻垢剂加药箱高报警","DR.ALARM_ZGJ_H"]
["阻垢剂加药箱超高报警","DR.ALARM_ZGJ_HH"]
["阻垢剂加药箱低报警","DR.ALARM_ZGJ_L"]
["阻垢剂加药箱超低报警","DR.ALARM_ZGJ_LL"]
["中和水箱高报警","DR.ALARM_ZHSX_H"]
["中和水箱超高报警","DR.ALARM_ZHSX_HH"]
["中和水箱低报警","DR.ALARM_ZHSX_L"]
["中和水箱超低报警","DR.ALARM_ZHSX_LL"]
["还原剂搅拌器自动启动","DR.JBQ_HYJ_AUTOSTART"]
["还原剂搅拌器手自动","DR.JBQ_HYJ_BT_AUTO"]
["还原剂搅拌器故障复位","DR.JBQ_HYJ_BT_RESET"]
["还原剂搅拌器手动启动","DR.JBQ_HYJ_BT_START"]
["还原剂搅拌器手动停止","DR.JBQ_HYJ_BT_STOP"]
["还原剂搅拌器故障","DR.JBQ_HYJ_FAULT"]
["还原剂搅拌器启动","DR.JBQ_HYJ_OUTPUT"]
["还原剂搅拌器启动准备好","DR.JBQ_HYJ_READY"]
["还原剂搅拌器远程","DR.JBQ_HYJ_REM"]
["还原剂搅拌器运行","DR.JBQ_HYJ_RFB"]
["PAC搅拌器自动启动","DR.JBQ_PAC_AUTOSTART"]
["PAC搅拌器手自动","DR.JBQ_PAC_BT_AUTO"]
["PAC搅拌器故障复位","DR.JBQ_PAC_BT_RESET"]
["PAC搅拌器手动启动","DR.JBQ_PAC_BT_START"]
["PAC搅拌器手动停止","DR.JBQ_PAC_BT_STOP"]
["PAC搅拌器故障","DR.JBQ_PAC_FAULT"]
["PAC搅拌器启动","DR.JBQ_PAC_OUTPUT"]
["PAC搅拌器启动准备好","DR.JBQ_PAC_READY"]
["PAC搅拌器远程","DR.JBQ_PAC_REM"]
["PAC搅拌器运行","DR.JBQ_PAC_RFB"]
["酸搅拌器自动启动","DR.JBQ_S_AUTOSTART"]
["酸搅拌器手自动","DR.JBQ_S_BT_AUTO"]
["酸搅拌器故障复位","DR.JBQ_S_BT_RESET"]
["酸搅拌器手动启动","DR.JBQ_S_BT_START"]
["酸搅拌器手动停止","DR.JBQ_S_BT_STOP"]
["酸搅拌器故障","DR.JBQ_S_FAULT"]
["酸搅拌器启动","DR.JBQ_S_OUTPUT"]
["酸搅拌器启动准备好","DR.JBQ_S_READY"]
["酸搅拌器远程","DR.JBQ_S_REM"]
["酸搅拌器运行","DR.JBQ_S_RFB"]
["阻垢剂搅拌器自动启动","DR.JBQ_ZGJ_AUTOSTART"]
["阻垢剂搅拌器手自动","DR.JBQ_ZGJ_BT_AUTO"]
["阻垢剂搅拌器故障复位","DR.JBQ_ZGJ_BT_RESET"]
["阻垢剂搅拌器手动启动","DR.JBQ_ZGJ_BT_START"]
["阻垢剂搅拌器手动停止","DR.JBQ_ZGJ_BT_STOP"]
["阻垢剂搅拌器故障","DR.JBQ_ZGJ_FAULT"]
["阻垢剂搅拌器启动","DR.JBQ_ZGJ_OUTPUT"]
["阻垢剂搅拌器启动准备好","DR.JBQ_ZGJ_READY"]
["阻垢剂搅拌器远程","DR.JBQ_ZGJ_REM"]
["阻垢剂搅拌器运行","DR.JBQ_ZGJ_RFB"]
["1#次钠加药泵自动启动","DR.P_1#CNB_AUTOSTART"]
["1#次钠加药泵手自动","DR.P_1#CNB_BT_AUTO"]
["1#次钠加药泵故障复位","DR.P_1#CNB_BT_RESET"]
["1#次钠加药泵手动启动","DR.P_1#CNB_BT_START"]
["1#次钠加药泵手动停止","DR.P_1#CNB_BT_STOP"]
["1#次钠加药泵故障","DR.P_1#CNB_FAULT"]
["1#次钠加药泵启动","DR.P_1#CNB_OUTPUT"]
["1#次钠加药泵启动准备好","DR.P_1#CNB_READY"]
["1#次钠加药泵远程","DR.P_1#CNB_REM"]
["1#次钠加药泵运行","DR.P_1#CNB_RFB"]
["1#出水碱加药泵自动启动","DR.P_1#CSJB_AUTOSTART"]
["1#出水碱加药泵手自动","DR.P_1#CSJB_BT_AUTO"]
["1#出水碱加药泵故障复位","DR.P_1#CSJB_BT_RESET"]
["1#出水碱加药泵手动启动","DR.P_1#CSJB_BT_START"]
["1#出水碱加药泵手动停止","DR.P_1#CSJB_BT_STOP"]
["1#出水碱加药泵故障","DR.P_1#CSJB_FAULT"]
["1#出水碱加药泵启动","DR.P_1#CSJB_OUTPUT"]
["1#出水碱加药泵启动准备好","DR.P_1#CSJB_READY"]
["1#出水碱加药泵远程","DR.P_1#CSJB_REM"]
["1#出水碱加药泵运行","DR.P_1#CSJB_RFB"]
["1#回用水泵自动启动","DR.P_1#HYSB_AUTOSTART"]
["1#回用水泵手自动","DR.P_1#HYSB_BT_AUTO"]
["1#回用水泵故障复位","DR.P_1#HYSB_BT_RESET"]
["1#回用水泵手动启动","DR.P_1#HYSB_BT_START"]
["1#回用水泵手动停止","DR.P_1#HYSB_BT_STOP"]
["1#回用水泵故障","DR.P_1#HYSB_FAULT"]
["1#回用水泵启动","DR.P_1#HYSB_OUTPUT"]
["1#回用水泵启动准备好","DR.P_1#HYSB_READY"]
["1#回用水泵远程","DR.P_1#HYSB_REM"]
["1#回用水泵运行","DR.P_1#HYSB_RFB"]
["1#PAC加药泵自动启动","DR.P_1#PACB_AUTOSTART"]
["1#PAC加药泵手自动","DR.P_1#PACB_BT_AUTO"]
["1#PAC加药泵故障复位","DR.P_1#PACB_BT_RESET"]
["1#PAC加药泵手动启动","DR.P_1#PACB_BT_START"]
["1#PAC加药泵手动停止","DR.P_1#PACB_BT_STOP"]
["1#PAC加药泵故障","DR.P_1#PACB_FAULT"]
["1#PAC加药泵启动","DR.P_1#PACB_OUTPUT"]
["1#PAC加药泵启动准备好","DR.P_1#PACB_READY"]
["1#PAC加药泵远程","DR.P_1#PACB_REM"]
["1#PAC加药泵运行","DR.P_1#PACB_RFB"]
["1#RO段间泵自动启动","DR.P_1#RODJB_AUTOSTART"]
["1#RO段间泵手自动","DR.P_1#RODJB_BT_AUTO"]
["1#RO段间泵故障复位","DR.P_1#RODJB_BT_RESET"]
["1#RO段间泵手动启动","DR.P_1#RODJB_BT_START"]
["1#RO段间泵手动停止","DR.P_1#RODJB_BT_STOP"]
["1#RO段间泵故障","DR.P_1#RODJB_FAULT"]
["1#RO段间泵启动","DR.P_1#RODJB_OUTPUT"]
["1#RO段间泵启动准备好","DR.P_1#RODJB_READY"]
["1#RO段间泵远程","DR.P_1#RODJB_REM"]
["1#RO段间泵运行","DR.P_1#RODJB_RFB"]
["1#RO高压泵自动启动","DR.P_1#ROGYB_AUTOSTART"]
["1#RO高压泵手自动","DR.P_1#ROGYB_BT_AUTO"]
["1#RO高压泵故障复位","DR.P_1#ROGYB_BT_RESET"]
["1#RO高压泵手动启动","DR.P_1#ROGYB_BT_START"]
["1#RO高压泵手动停止","DR.P_1#ROGYB_BT_STOP"]
["1#RO高压泵故障","DR.P_1#ROGYB_FAULT"]
["1#RO高压泵启动","DR.P_1#ROGYB_OUTPUT"]
["1#RO高压泵启动准备好","DR.P_1#ROGYB_READY"]
["1#RO高压泵远程","DR.P_1#ROGYB_REM"]
["1#RO高压泵运行","DR.P_1#ROGYB_RFB"]
["1#RO还原剂加药泵自动启动","DR.P_1#HYJB_AUTOSTART"]
["1#RO还原剂加药泵手自动","DR.P_1#HYJB_BT_AUTO"]
["1#RO还原剂加药泵故障复位","DR.P_1#HYJB_BT_RESET"]
["1#RO还原剂加药泵手动启动","DR.P_1#HYJB_BT_START"]
["1#RO还原剂加药泵手动停止","DR.P_1#HYJB_BT_STOP"]
["1#RO还原剂加药泵故障","DR.P_1#HYJB_FAULT"]
["1#RO还原剂加药泵启动","DR.P_1#HYJB_OUTPUT"]
["1#RO还原剂加药泵启动准备好","DR.P_1#HYJB_READY"]
["1#RO还原剂加药泵远程","DR.P_1#HYJB_REM"]
["1#RO还原剂加药泵运行","DR.P_1#HYJB_RFB"]
["1#酸加药泵自动启动","DR.P_1#SB_AUTOSTART"]
["1#酸加药泵手自动","DR.P_1#SB_BT_AUTO"]
["1#酸加药泵故障复位","DR.P_1#SB_BT_RESET"]
["1#酸加药泵手动启动","DR.P_1#SB_BT_START"]
["1#酸加药泵手动停止","DR.P_1#SB_BT_STOP"]
["1#酸加药泵故障","DR.P_1#SB_FAULT"]
["1#酸加药泵启动","DR.P_1#SB_OUTPUT"]
["1#酸加药泵启动准备好","DR.P_1#SB_READY"]
["1#酸加药泵远程","DR.P_1#SB_REM"]
["1#酸加药泵运行","DR.P_1#SB_RFB"]
["1#杀菌剂加药泵自动启动","DR.P_1#SJB_AUTOSTART"]
["1#杀菌剂加药泵手自动","DR.P_1#SJB_BT_AUTO"]
["1#杀菌剂加药泵故障复位","DR.P_1#SJB_BT_RESET"]
["1#杀菌剂加药泵手动启动","DR.P_1#SJB_BT_START"]
["1#杀菌剂加药泵手动停止","DR.P_1#SJB_BT_STOP"]
["1#杀菌剂加药泵故障","DR.P_1#SJB_FAULT"]
["1#杀菌剂加药泵启动","DR.P_1#SJB_OUTPUT"]
["1#杀菌剂加药泵启动准备好","DR.P_1#SJB_READY"]
["1#杀菌剂加药泵远程","DR.P_1#SJB_REM"]
["1#杀菌剂加药泵运行","DR.P_1#SJB_RFB"]
["1#超滤碱加药泵自动启动","DR.P_1#UF_JB_AUTOSTART"]
["1#超滤碱加药泵手自动","DR.P_1#UF_JB_BT_AUTO"]
["1#超滤碱加药泵故障复位","DR.P_1#UF_JB_BT_RESET"]
["1#超滤碱加药泵手动启动","DR.P_1#UF_JB_BT_START"]
["1#超滤碱加药泵手动停止","DR.P_1#UF_JB_BT_STOP"]
["1#超滤碱加药泵故障","DR.P_1#UF_JB_FAULT"]
["1#超滤碱加药泵启动","DR.P_1#UF_JB_OUTPUT"]
["1#超滤碱加药泵启动准备好","DR.P_1#UF_JB_READY"]
["1#超滤碱加药泵远程","DR.P_1#UF_JB_REM"]
["1#超滤碱加药泵运行","DR.P_1#UF_JB_RFB"]
["1#超滤反洗泵自动启动","DR.P_1#UFBWB_AUTOSTART"]
["1#超滤反洗泵手自动","DR.P_1#UFBWB_BT_AUTO"]
["1#超滤反洗泵故障复位","DR.P_1#UFBWB_BT_RESET"]
["1#超滤反洗泵手动启动","DR.P_1#UFBWB_BT_START"]
["1#超滤反洗泵手动停止","DR.P_1#UFBWB_BT_STOP"]
["1#超滤反洗泵故障","DR.P_1#UFBWB_FAULT"]
["1#超滤反洗泵启动","DR.P_1#UFBWB_OUTPUT"]
["1#超滤反洗泵启动准备好","DR.P_1#UFBWB_READY"]
["1#超滤反洗泵远程","DR.P_1#UFBWB_REM"]
["1#超滤反洗泵运行","DR.P_1#UFBWB_RFB"]
["1#阻垢剂加药泵自动启动","DR.P_1#ZGJB_AUTOSTART"]
["1#阻垢剂加药泵手自动","DR.P_1#ZGJB_BT_AUTO"]
["1#阻垢剂加药泵故障复位","DR.P_1#ZGJB_BT_RESET"]
["1#阻垢剂加药泵手动启动","DR.P_1#ZGJB_BT_START"]
["1#阻垢剂加药泵手动停止","DR.P_1#ZGJB_BT_STOP"]
["1#阻垢剂加药泵故障","DR.P_1#ZGJB_FAULT"]
["1#阻垢剂加药泵启动","DR.P_1#ZGJB_OUTPUT"]
["1#阻垢剂加药泵启动准备好","DR.P_1#ZGJB_READY"]
["1#阻垢剂加药泵远程","DR.P_1#ZGJB_REM"]
["1#阻垢剂加药泵运行","DR.P_1#ZGJB_RFB"]
["1#中和还原剂加药泵自动启动","DR.P_1#ZH_HYJ_AUTOSTART"]
["1#中和还原剂加药泵手自动","DR.P_1#ZH_HYJ_BT_AUTO"]
["1#中和还原剂加药泵故障复位","DR.P_1#ZH_HYJ_BT_RESET"]
["1#中和还原剂加药泵手动启动","DR.P_1#ZH_HYJ_BT_START"]
["1#中和还原剂加药泵手动停止","DR.P_1#ZH_HYJ_BT_STOP"]
["1#中和还原剂加药泵故障","DR.P_1#ZH_HYJ_FAULT"]
["1#中和还原剂加药泵启动","DR.P_1#ZH_HYJ_OUTPUT"]
["1#中和还原剂加药泵启动准备好","DR.P_1#ZH_HYJ_READY"]
["1#中和还原剂加药泵远程","DR.P_1#ZH_HYJ_REM"]
["1#中和还原剂加药泵运行","DR.P_1#ZH_HYJ_RFB"]
["2#次钠加药泵自动启动","DR.P_2#CNB_AUTOSTART"]
["2#次钠加药泵手自动","DR.P_2#CNB_BT_AUTO"]
["2#次钠加药泵故障复位","DR.P_2#CNB_BT_RESET"]
["2#次钠加药泵手动启动","DR.P_2#CNB_BT_START"]
["2#次钠加药泵手动停止","DR.P_2#CNB_BT_STOP"]
["2#次钠加药泵故障","DR.P_2#CNB_FAULT"]
["2#次钠加药泵启动","DR.P_2#CNB_OUTPUT"]
["2#次钠加药泵启动准备好","DR.P_2#CNB_READY"]
["2#次钠加药泵远程","DR.P_2#CNB_REM"]
["2#次钠加药泵运行","DR.P_2#CNB_RFB"]
["2#出水碱加药泵自动启动","DR.P_2#CSJB_AUTOSTART"]
["2#出水碱加药泵手自动","DR.P_2#CSJB_BT_AUTO"]
["2#出水碱加药泵故障复位","DR.P_2#CSJB_BT_RESET"]
["2#出水碱加药泵手动启动","DR.P_2#CSJB_BT_START"]
["2#出水碱加药泵手动停止","DR.P_2#CSJB_BT_STOP"]
["2#出水碱加药泵故障","DR.P_2#CSJB_FAULT"]
["2#出水碱加药泵启动","DR.P_2#CSJB_OUTPUT"]
["2#出水碱加药泵启动准备好","DR.P_2#CSJB_READY"]
["2#出水碱加药泵远程","DR.P_2#CSJB_REM"]
["2#出水碱加药泵运行","DR.P_2#CSJB_RFB"]
["2#回用水泵自动启动","DR.P_2#HYSB_AUTOSTART"]
["2#回用水泵手自动","DR.P_2#HYSB_BT_AUTO"]
["2#回用水泵故障复位","DR.P_2#HYSB_BT_RESET"]
["2#回用水泵手动启动","DR.P_2#HYSB_BT_START"]
["2#回用水泵手动停止","DR.P_2#HYSB_BT_STOP"]
["2#回用水泵故障","DR.P_2#HYSB_FAULT"]
["2#回用水泵启动","DR.P_2#HYSB_OUTPUT"]
["2#回用水泵启动准备好","DR.P_2#HYSB_READY"]
["2#回用水泵远程","DR.P_2#HYSB_REM"]
["2#回用水泵运行","DR.P_2#HYSB_RFB"]
["2#PAC加药泵自动启动","DR.P_2#PACB_AUTOSTART"]
["2#PAC加药泵手自动","DR.P_2#PACB_BT_AUTO"]
["2#PAC加药泵故障复位","DR.P_2#PACB_BT_RESET"]
["2#PAC加药泵手动启动","DR.P_2#PACB_BT_START"]
["2#PAC加药泵手动停止","DR.P_2#PACB_BT_STOP"]
["2#PAC加药泵故障","DR.P_2#PACB_FAULT"]
["2#PAC加药泵启动","DR.P_2#PACB_OUTPUT"]
["2#PAC加药泵启动准备好","DR.P_2#PACB_READY"]
["2#PAC加药泵远程","DR.P_2#PACB_REM"]
["2#PAC加药泵运行","DR.P_2#PACB_RFB"]
["2#RO段间泵自动启动","DR.P_2#RODJB_AUTOSTART"]
["2#RO段间泵手自动","DR.P_2#RODJB_BT_AUTO"]
["2#RO段间泵故障复位","DR.P_2#RODJB_BT_RESET"]
["2#RO段间泵手动启动","DR.P_2#RODJB_BT_START"]
["2#RO段间泵手动停止","DR.P_2#RODJB_BT_STOP"]
["2#RO段间泵故障","DR.P_2#RODJB_FAULT"]
["2#RO段间泵启动","DR.P_2#RODJB_OUTPUT"]
["2#RO段间泵启动准备好","DR.P_2#RODJB_READY"]
["2#RO段间泵远程","DR.P_2#RODJB_REM"]
["2#RO段间泵运行","DR.P_2#RODJB_RFB"]
["2#RO高压泵自动启动","DR.P_2#ROGYB_AUTOSTART"]
["2#RO高压泵手自动","DR.P_2#ROGYB_BT_AUTO"]
["2#RO高压泵故障复位","DR.P_2#ROGYB_BT_RESET"]
["2#RO高压泵手动启动","DR.P_2#ROGYB_BT_START"]
["2#RO高压泵手动停止","DR.P_2#ROGYB_BT_STOP"]
["2#RO高压泵故障","DR.P_2#ROGYB_FAULT"]
["2#RO高压泵启动","DR.P_2#ROGYB_OUTPUT"]
["2#RO高压泵启动准备好","DR.P_2#ROGYB_READY"]
["2#RO高压泵远程","DR.P_2#ROGYB_REM"]
["2#RO高压泵运行","DR.P_2#ROGYB_RFB"]
["2#RO还原剂加药泵自动启动","DR.P_2#HYJB_AUTOSTART"]
["2#RO还原剂加药泵手自动","DR.P_2#HYJB_BT_AUTO"]
["2#RO还原剂加药泵故障复位","DR.P_2#HYJB_BT_RESET"]
["2#RO还原剂加药泵手动启动","DR.P_2#HYJB_BT_START"]
["2#RO还原剂加药泵手动停止","DR.P_2#HYJB_BT_STOP"]
["2#RO还原剂加药泵故障","DR.P_2#HYJB_FAULT"]
["2#RO还原剂加药泵启动","DR.P_2#HYJB_OUTPUT"]
["2#RO还原剂加药泵启动准备好","DR.P_2#HYJB_READY"]
["2#RO还原剂加药泵远程","DR.P_2#HYJB_REM"]
["2#RO还原剂加药泵运行","DR.P_2#HYJB_RFB"]
["2#酸加药泵自动启动","DR.P_2#SB_AUTOSTART"]
["2#酸加药泵手自动","DR.P_2#SB_BT_AUTO"]
["2#酸加药泵故障复位","DR.P_2#SB_BT_RESET"]
["2#酸加药泵手动启动","DR.P_2#SB_BT_START"]
["2#酸加药泵手动停止","DR.P_2#SB_BT_STOP"]
["2#酸加药泵故障","DR.P_2#SB_FAULT"]
["2#酸加药泵启动","DR.P_2#SB_OUTPUT"]
["2#酸加药泵启动准备好","DR.P_2#SB_RE"]
["2#酸加药泵远程","DR.P_2#SB_READY"]
["2#酸加药泵运行","DR.P_2#SB_RFB"]
["2#杀菌剂加药泵自动启动","DR.P_2#SJB_AUTOSTART"]
["2#杀菌剂加药泵手自动","DR.P_2#SJB_BT_AUTO"]
["2#杀菌剂加药泵故障复位","DR.P_2#SJB_BT_RESET"]
["2#杀菌剂加药泵手动启动","DR.P_2#SJB_BT_START"]
["2#杀菌剂加药泵手动停止","DR.P_2#SJB_BT_STOP"]
["2#杀菌剂加药泵故障","DR.P_2#SJB_FAULT"]
["2#杀菌剂加药泵启动","DR.P_2#SJB_OUTPUT"]
["2#杀菌剂加药泵启动准备好","DR.P_2#SJB_READY"]
["2#杀菌剂加药泵远程","DR.P_2#SJB_REM"]
["2#杀菌剂加药泵运行","DR.P_2#SJB_RFB"]
["2#超滤碱加药泵自动启动","DR.P_2#UF_JB_AUTOSTART"]
["2#超滤碱加药泵手自动","DR.P_2#UF_JB_BT_AUTO"]
["2#超滤碱加药泵故障复位","DR.P_2#UF_JB_BT_RESET"]
["2#超滤碱加药泵手动启动","DR.P_2#UF_JB_BT_START"]
["2#超滤碱加药泵手动停止","DR.P_2#UF_JB_BT_STOP"]
["2#超滤碱加药泵故障","DR.P_2#UF_JB_FAULT"]
["2#超滤碱加药泵启动","DR.P_2#UF_JB_OUTPUT"]
["2#超滤碱加药泵启动准备好","DR.P_2#UF_JB_READY"]
["2#超滤碱加药泵远程","DR.P_2#UF_JB_REM"]
["2#超滤碱加药泵运行","DR.P_2#UF_JB_RFB"]
["2#超滤反洗泵自动启动","DR.P_2#UFBWB_AUTOSTART"]
["2#超滤反洗泵手自动","DR.P_2#UFBWB_BT_AUTO"]
["2#超滤反洗泵故障复位","DR.P_2#UFBWB_BT_RESET"]
["2#超滤反洗泵手动启动","DR.P_2#UFBWB_BT_START"]
["2#超滤反洗泵手动停止","DR.P_2#UFBWB_BT_STOP"]
["2#超滤反洗泵故障","DR.P_2#UFBWB_FAULT"]
["2#超滤反洗泵启动","DR.P_2#UFBWB_OUTPUT"]
["2#超滤反洗泵启动准备好","DR.P_2#UFBWB_READY"]
["2#超滤反洗泵远程","DR.P_2#UFBWB_REM"]
["2#超滤反洗泵运行","DR.P_2#UFBWB_RFB"]
["2#阻垢剂加药泵自动启动","DR.P_2#ZGJB_AUTOSTART"]
["2#阻垢剂加药泵手自动","DR.P_2#ZGJB_BT_AUTO"]
["2#阻垢剂加药泵故障复位","DR.P_2#ZGJB_BT_RESET"]
["2#阻垢剂加药泵手动启动","DR.P_2#ZGJB_BT_START"]
["2#阻垢剂加药泵手动停止","DR.P_2#ZGJB_BT_STOP"]
["2#阻垢剂加药泵故障","DR.P_2#ZGJB_FAULT"]
["2#阻垢剂加药泵启动","DR.P_2#ZGJB_OUTPUT"]
["2#阻垢剂加药泵启动准备好","DR.P_2#ZGJB_READY"]
["2#阻垢剂加药泵远程","DR.P_2#ZGJB_REM"]
["2#阻垢剂加药泵运行","DR.P_2#ZGJB_RFB"]
["2#中和还原剂加药泵自动启动","DR.P_2#ZH_HYJ_AUTOSTART"]
["2#中和还原剂加药泵手自动","DR.P_2#ZH_HYJ_BT_AUTO"]
["2#中和还原剂加药泵故障复位","DR.P_2#ZH_HYJ_BT_RESET"]
["2#中和还原剂加药泵手动启动","DR.P_2#ZH_HYJ_BT_START"]
["2#中和还原剂加药泵手动停止","DR.P_2#ZH_HYJ_BT_STOP"]
["2#中和还原剂加药泵故障","DR.P_2#ZH_HYJ_FAULT"]
["2#中和还原剂加药泵启动","DR.P_2#ZH_HYJ_OUTPUT"]
["2#中和还原剂加药泵启动准备好","DR.P_2#ZH_HYJ_READY"]
["2#中和还原剂加药泵远程","DR.P_2#ZH_HYJ_REM"]
["2#中和还原剂加药泵运行","DR.P_2#ZH_HYJ_RFB"]
["3#阻垢剂加药泵自动启动","DR.P_3#ZGJB_AUTOSTART"]
["3#阻垢剂加药泵手自动","DR.P_3#ZGJB_BT_AUTO"]
["3#阻垢剂加药泵故障复位","DR.P_3#ZGJB_BT_RESET"]
["3#阻垢剂加药泵手动启动","DR.P_3#ZGJB_BT_START"]
["3#阻垢剂加药泵手动停止","DR.P_3#ZGJB_BT_STOP"]
["3#阻垢剂加药泵故障","DR.P_3#ZGJB_FAULT"]
["3#阻垢剂加药泵启动","DR.P_3#ZGJB_OUTPUT"]
["3#阻垢剂加药泵启动准备好","DR.P_3#ZGJB_READY"]
["3#阻垢剂加药泵远程","DR.P_3#ZGJB_REM"]
["3#阻垢剂加药泵运行","DR.P_3#ZGJB_RFB"]
["废水泵自动启动","DR.P_FSB_AUTOSTART"]
["废水泵手自动","DR.P_FSB_BT_AUTO"]
["废水泵故障复位","DR.P_FSB_BT_RESET"]
["废水泵手动启动","DR.P_FSB_BT_START"]
["废水泵手动停止","DR.P_FSB_BT_STOP"]
["废水泵故障","DR.P_FSB_FAULT"]
["废水泵启动","DR.P_FSB_OUTPUT"]
["废水泵启动准备好","DR.P_FSB_READY"]
["废水泵远程","DR.P_FSB_REM"]
["废水泵运行","DR.P_FSB_RFB"]
["加热器自动启动","DR.P_JRQ_AUTOSTART"]
["加热器手自动","DR.P_JRQ_BT_AUTO"]
["加热器故障复位","DR.P_JRQ_BT_RESET"]
["加热器手动启动","DR.P_JRQ_BT_START"]
["加热器手动停止","DR.P_JRQ_BT_STOP"]
["加热器故障","DR.P_JRQ_FAULT"]
["加热器启动","DR.P_JRQ_OUTPUT"]
["加热器启动准备好","DR.P_JRQ_READY"]
["加热器远程","DR.P_JRQ_REM"]
["加热器运行","DR.P_JRQ_RFB"]
["潜污泵自动启动","DR.P_QWB_AUTOSTART"]
["潜污泵手自动","DR.P_QWB_BT_AUTO"]
["潜污泵故障复位","DR.P_QWB_BT_RESET"]
["潜污泵手动启动","DR.P_QWB_BT_START"]
["潜污泵手动停止","DR.P_QWB_BT_STOP"]
["潜污泵故障","DR.P_QWB_FAULT"]
["潜污泵启动","DR.P_QWB_OUTPUT"]
["潜污泵启动准备好","DR.P_QWB_READY"]
["潜污泵远程","DR.P_QWB_REM"]
["潜污泵运行","DR.P_QWB_RFB"]
["清洗水泵自动启动","DR.P_QXSB_AUTOSTART"]
["清洗水泵手自动","DR.P_QXSB_BT_AUTO"]
["清洗水泵故障复位","DR.P_QXSB_BT_RESET"]
["清洗水泵手动启动","DR.P_QXSB_BT_START"]
["清洗水泵手动停止","DR.P_QXSB_BT_STOP"]
["清洗水泵故障","DR.P_QXSB_FAULT"]
["清洗水泵启动","DR.P_QXSB_OUTPUT"]
["清洗水泵启动准备好","DR.P_QXSB_READY"]
["清洗水泵远程","DR.P_QXSB_REM"]
["清洗水泵运行","DR.P_QXSB_RFB"]
["反渗透供水泵自动启动","DR.P_ROGSB_AUTOSTART"]
["反渗透供水泵手自动","DR.P_ROGSB_BT_AUTO"]
["反渗透供水泵故障复位","DR.P_ROGSB_BT_RESET"]
["反渗透供水泵手动启动","DR.P_ROGSB_BT_START"]
["反渗透供水泵手动停止","DR.P_ROGSB_BT_STOP"]
["反渗透供水泵故障","DR.P_ROGSB_FAULT"]
["反渗透供水泵启动","DR.P_ROGSB_OUTPUT"]
["反渗透供水泵启动准备好","DR.P_ROGSB_READY"]
["反渗透供水泵远程","DR.P_ROGSB_REM"]
["反渗透供水泵运行","DR.P_ROGSB_RFB"]
["超滤供水泵自动启动","DR.P_UFGSB_AUTOSTART"]
["超滤供水泵手自动","DR.P_UFGSB_BT_AUTO"]
["超滤供水泵故障复位","DR.P_UFGSB_BT_RESET"]
["超滤供水泵手动启动","DR.P_UFGSB_BT_START"]
["超滤供水泵手动停止","DR.P_UFGSB_BT_STOP"]
["超滤供水泵故障","DR.P_UFGSB_FAULT"]
["超滤供水泵启动","DR.P_UFGSB_OUTPUT"]
["超滤供水泵启动准备好","DR.P_UFGSB_READY"]
["超滤供水泵远程","DR.P_UFGSB_REM"]
["超滤供水泵运行","DR.P_UFGSB_RFB"]
["中和泵自动启动","DR.P_ZH_AUTOSTART"]
["中和泵手自动","DR.P_ZH_BT_AUTO"]
["中和泵故障复位","DR.P_ZH_BT_RESET"]
["中和泵手动启动","DR.P_ZH_BT_START"]
["中和泵手动停止","DR.P_ZH_BT_STOP"]
["中和泵故障","DR.P_ZH_FAULT"]
["中和泵启动","DR.P_ZH_OUTPUT"]
["中和泵启动准备好","DR.P_ZH_READY"]
["中和泵远程","DR.P_ZH_REM"]
["中和泵运行","DR.P_ZH_RFB"]
["RO1一段压差高","DR.RO1_1D_YC_HIGH"]
["RO1二三段碱维护按键","DR.RO1_2/3DJWH"]
["RO1二段压差高","DR.RO1_2D_YC_HIGH"]
["RO1执行一段碱维护","DR.RO1_ACT_1DJWH"]
["RO1执行一段杀菌","DR.RO1_ACT_1DSJ"]
["RO1执行一段酸维护","DR.RO1_ACT_1DSWH"]
["RO1执行二三段碱维护","DR.RO1_ACT_2/3DJWH"]
["RO1执行二三段杀菌维护","DR.RO1_ACT_2/3DSJWH"]
["RO1执行二三段酸维护","DR.RO1_ACT_2/3DSWH"]
["RO1执行冲洗","DR.RO1_ACT_CX"]
["RO1执行超越过滤","DR.RO1_ACT_CYGL"]
["RO1执行超越停机冲洗","DR.RO1_ACT_CYTJCX"]
["RO1执行超越停机加药冲洗","DR.RO1_ACT_CYTJJYCX"]
["RO1执行非正常停机冲洗","DR.RO1_ACT_FZCTJCX"]
["RO1执行过滤","DR.RO1_ACT_GL"]
["RO1执行长时间停机加药冲洗","DR.RO1_ACT_LONGTIME_CEB"]
["RO1允许冲洗","DR.RO1_ALLOW_CX"]
["RO1允许过滤","DR.RO1_ALLOW_GL"]
["RO1允许杀菌","DR.RO1_ALLOW_SJ"]
["RO1出栈","DR.RO1_APPLY_POP"]
["RO1清零出栈代码","DR.RO1_APPLY_POP_CLEAR"]
["RO1入栈","DR.RO1_APPLY_PUSH"]
["RO1启用反洗泵","DR.RO1_APPLY_RO_FXB"]
["RO1启用供水泵","DR.RO1_APPLY_RO_GSB"]
["RO1启用还原剂泵","DR.RO1_APPLY_RO_HYJB"]
["RO1启用还原剂阀","DR.RO1_APPLY_RO_HYJF"]
["RO1启用气洗阀","DR.RO1_APPLY_RO_QXF"]
["RO1启用阻垢剂泵","DR.RO1_APPLY_RO_ZGJB"]
["RO1启用杀菌泵","DR.RO1_APPLY_SJB"]
["RO1启用杀菌阀","DR.RO1_APPLY_SJF"]
["RO1启用维护碱泵","DR.RO1_APPLY_WHJB"]
["RO1启用维护碱阀","DR.RO1_APPLY_WHJF"]
["RO1启用维护酸泵","DR.RO1_APPLY_WHSB"]
["RO1启用维护酸阀","DR.RO1_APPLY_WHSF"]
["RO1自动启动","DR.RO1_AUTO_START"]
["RO1一段碱维护按键","DR.RO1_BT_1DJWH"]
["RO1一段酸维护按键","DR.RO1_BT_1DSWH"]
["RO1一段杀菌按键","DR.RO1_BT_1DXJ"]
["RO1二三段碱维护","DR.RO1_BT_2/3DJWH"]
["RO1二三段杀菌按键","DR.RO1_BT_2/3DSJ"]
["RO1二三段酸维护按键","DR.RO1_BT_2/3DSWH"]
["RO1自动维护按键","DR.RO1_BT_AUTO_WH"]
["RO1正常冲洗按键","DR.RO1_BT_CX"]
["RO1超越过滤按键","DR.RO1_BT_CYGL"]
["RO1超越模式按键","DR.RO1_BT_CYMS"]
["RO1超越停机冲洗按键","DR.RO1_BT_CYTJCX"]
["RO1超越停机加药冲洗按键","DR.RO1_BT_CYTJJYCX"]
["RO1急停按键","DR.RO1_BT_EMERGENCY"]
["RO1非正常冲洗按键","DR.RO1_BT_FZCCX"]
["RO1过滤按键","DR.RO1_BT_GL"]
["RO1初始化按键","DR.RO1_BT_INITIAL"]
["RO1复位按键","DR.RO1_BT_RESET"]
["RO1杀菌按键","DR.RO1_BT_SJ"]
["RO1启动按键","DR.RO1_BT_START"]
["RO1停止按键","DR.RO1_BT_STOP"]
["RO1自动按键","DR.RO1_BT_SYSTEMAUTO"]
["RO1手动按键","DR.RO1_BT_SYSTEMMANU"]
["RO1停机加药冲洗按键","DR.RO1_BT_TJJYCX"]
["RO1阀自动按键","DR.RO1_BT_VALVE_AUTO"]
["RO1电导率高","DR.RO1_DDL_HIGH"]
["RO1段间泵出口压力开关","DR.RO1_DJB_CKYLKG_OPEN"]
["RO1段间泵进口压力开关","DR.RO1_DJB_JKYLKG_CLOSE"]
["RO1正在过滤标记","DR.RO1_FLAG_GLING"]
["RO1系统准备好标记","DR.RO1_FLAG_SYS_READY"]
["RO1高压泵出口压力开关","DR.RO1_GYB_CKYLKG_OPEN"]
["RO1高压泵进口压力开关","DR.RO1_GYB_JKYLKG_CLOSE"]
["RO1系统报错","DR.RO1_SYSTEM_ERROR"]
["RO1该杀菌了","DR.RO1_TIME_FOR_SJ"]
["RO1阀准备好","DR.RO1_V_READY"]
["RO2一段压差高","DR.RO2_1D_YC_HIGH"]
["RO2二三段碱维护按键","DR.RO2_2/3DJWH"]
["RO2二段压差高","DR.RO2_2D_YC_HIGH"]
["RO2执行一段碱维护","DR.RO2_ACT_1DJWH"]
["RO2执行一段杀菌","DR.RO2_ACT_1DSJ"]
["RO2执行一段酸维护","DR.RO2_ACT_1DSWH"]
["RO2执行二三段碱维护","DR.RO2_ACT_2/3DJWH"]
["RO2执行二三段杀菌维护","DR.RO2_ACT_2/3DSJWH"]
["RO2执行二三段酸维护","DR.RO2_ACT_2/3DSWH"]
["RO2执行冲洗","DR.RO2_ACT_CX"]
["RO2执行超越过滤","DR.RO2_ACT_CYGL"]
["RO2执行超越停机冲洗","DR.RO2_ACT_CYTJCX"]
["RO2执行超越停机加药冲洗","DR.RO2_ACT_CYTJJYCX"]
["RO2执行非正常停机冲洗","DR.RO2_ACT_FZCTJCX"]
["RO2执行过滤","DR.RO2_ACT_GL"]
["RO2执行长时间停机加药冲洗","DR.RO2_ACT_LONGTIME_CEB"]
["RO2允许冲洗","DR.RO2_ALLOW_CX"]
["RO2允许过滤","DR.RO2_ALLOW_GL"]
["RO2允许杀菌","DR.RO2_ALLOW_SJ"]
["RO2出栈","DR.RO2_APPLY_POP"]
["RO2清零出栈代码","DR.RO2_APPLY_POP_CLEAR"]
["RO2入栈","DR.RO2_APPLY_PUSH"]
["RO2启用反洗泵","DR.RO2_APPLY_RO_FXB"]
["RO2启用供水泵","DR.RO2_APPLY_RO_GSB"]
["RO2启用还原剂泵","DR.RO2_APPLY_RO_HYJB"]
["RO2启用还原剂阀","DR.RO2_APPLY_RO_HYJF"]
["RO2启用气洗阀","DR.RO2_APPLY_RO_QXF"]
["RO2启用阻垢剂泵","DR.RO2_APPLY_RO_ZGJB"]
["RO2启用杀菌泵","DR.RO2_APPLY_SJB"]
["RO2启用杀菌阀","DR.RO2_APPLY_SJF"]
["RO2启用维护碱泵","DR.RO2_APPLY_WHJB"]
["RO2启用维护碱阀","DR.RO2_APPLY_WHJF"]
["RO2启用维护酸泵","DR.RO2_APPLY_WHSB"]
["RO2启用维护酸阀","DR.RO2_APPLY_WHSF"]
["RO2自动启动","DR.RO2_AUTO_START"]
["RO2一段碱维护按键","DR.RO2_BT_1DJWH"]
["RO2一段酸维护按键","DR.RO2_BT_1DSWH"]
["RO2一段杀菌按键","DR.RO2_BT_1DXJ"]
["RO2二三段碱维护","DR.RO2_BT_2/3DJWH"]
["RO2二三段杀菌按键","DR.RO2_BT_2/3DSJ"]
["RO2二三段酸维护按键","DR.RO2_BT_2/3DSWH"]
["RO2自动维护按键","DR.RO2_BT_AUTO_WH"]
["RO2正常冲洗按键","DR.RO2_BT_CX"]
["RO2超越过滤按键","DR.RO2_BT_CYGL"]
["RO2超越模式按键","DR.RO2_BT_CYMS"]
["RO2超越停机冲洗按键","DR.RO2_BT_CYTJCX"]
["RO2超越停机加药冲洗按键","DR.RO2_BT_CYTJJYCX"]
["RO2急停按键","DR.RO2_BT_EMERGENCY"]
["RO2非正常冲洗按键","DR.RO2_BT_FZCCX"]
["RO2过滤按键","DR.RO2_BT_GL"]
["RO2初始化按键","DR.RO2_BT_INITIAL"]
["RO2复位按键","DR.RO2_BT_RESET"]
["RO2杀菌按键","DR.RO2_BT_SJ"]
["RO2启动按键","DR.RO2_BT_START"]
["RO2停止按键","DR.RO2_BT_STOP"]
["RO2自动按键","DR.RO2_BT_SYSTEMAUTO"]
["RO2手动按键","DR.RO2_BT_SYSTEMMANU"]
["RO2停机加药冲洗按键","DR.RO2_BT_TJJYCX"]
["RO2阀自动按键","DR.RO2_BT_VALVE_AUTO"]
["RO2电导率高","DR.RO2_DDL_HIGH"]
["RO2段间泵出口压力开关","DR.RO2_DJB_CKYLKG_OPEN"]
["RO2段间泵进口压力开关","DR.RO2_DJB_JKYLKG_CLOSE"]
["RO2正在过滤标记","DR.RO2_FLAG_GLING"]
["RO2系统准备好标记","DR.RO2_FLAG_SYS_READY"]
["RO2高压泵出口压力开关","DR.RO2_GYB_CKYLKG_OPEN"]
["RO2高压泵进口压力开关","DR.RO2_GYB_JKYLKG_CLOSE"]
["RO2系统报错","DR.RO2_SYSTEM_ERROR"]
["RO2该杀菌了","DR.RO2_TIME_FOR_SJ"]
["RO2阀准备好","DR.RO2_V_READY"]
["UF1允许反洗","DR.UF1_ALLOW_BW"]
["UF1允许反洗气冲洗","DR.UF1_ALLOW_BWQCX"]
["UF1允许备用1","DR.UF1_ALLOW_BY1"]
["UF1允许备用2","DR.UF1_ALLOW_BY2"]
["UF1允许备用3","DR.UF1_ALLOW_BY3"]
["UF1允许CEB","DR.UF1_ALLOW_CEB"]
["UF1允许过滤","DR.UF1_ALLOW_GL"]
["UF1允许PAC","DR.UF1_ALLOW_PAC"]
["UF1启用供水泵","DR.UF1_APPLY_GSB"]
["UF1启用PAC泵","DR.UF1_APPLY_PAC_B"]
["UF1启用PAC阀","DR.UF1_APPLY_PAC-V"]
["UF1启用调节阀","DR.UF1_APPLY_TJV"]
["UF1自动过滤启动","DR.UF1_AUTOSTART_GL"]
["UF1手动反洗操作","DR.UF1_BT_BW"]
["UF1手动CEB操作","DR.UF1_BT_CEB"]
["UF1手动CIP操作","DR.UF1_BT_CIP"]
["UF1手动冲水操作","DR.UF1_BT_CS"]
["UF1手动清除过滤流量","DR.UF1_BT_ERASE_GLFLOW"]
["UF1停止操作","DR.UF1_BT_ESTOP"]
["UF1手动过滤操作","DR.UF1_BT_GL"]
["UF1手动初始化操作","DR.UF1_BT_INAI"]
["UF1手动屏蔽液位开关","DR.UF1_BT_PB_YWKG"]
["UF1故障复位操作","DR.UF1_BT_RESET"]
["UF1手自动模式操作","DR.UF1_BT_SYS_AUTO"]
["UF1阀门手自动操作","DR.UF1_BT_V_AUTO"]
["UF1 CEB碱选择","DR.UF1_CEB_J"]
["UF1 CEB酸选择","DR.UF1_CEB_S"]
["UF1压差高限值报错","DR.UF1_ERR_YC_H"]
["UF1压差高高值报错","DR.UF1_ERR_YC_HH"]
["UF1药剂残留报错","DR.UF1_ERR_YJCL"]
["UF1过滤准备好标志","DR.UF1_FLAG_GL_READY"]
["UF1膜内有药标志","DR.UF1_FLAG_MNYY"]
["UF1无它CEB标志","DR.UF1_FLAG_NOOTHERCEB"]
["UF1阀准备好标志","DR.UF1_FLAG_V_RRADY"]
["UF1系统报错","DR.UF1_SYS_ERR"]
["UF2允许反洗","DR.UF2_ALLOW_BW"]
["UF2允许反洗气冲洗","DR.UF2_ALLOW_BWQCX"]
["UF2允许备用1","DR.UF2_ALLOW_BY1"]
["UF2允许备用2","DR.UF2_ALLOW_BY2"]
["UF2允许备用3","DR.UF2_ALLOW_BY3"]
["UF2允许CEB","DR.UF2_ALLOW_CEB"]
["UF2允许过滤","DR.UF2_ALLOW_GL"]
["UF2允许PAC","DR.UF2_ALLOW_PAC"]
["UF2启用PAC泵","DR.UF2_APPLY_PAC_B"]
["UF2启用PAC阀","DR.UF2_APPLY_PAC_V"]
["UF2自动过滤启动","DR.UF2_AUTOSTART_GL"]
["UF2手动反洗操作","DR.UF2_BT_BW"]
["UF2手动CEB操作","DR.UF2_BT_CEB"]
["UF2手动CIP操作","DR.UF2_BT_CIP"]
["UF2手动冲水操作","DR.UF2_BT_CS"]
["UF2手动清除过滤流量","DR.UF2_BT_ERASE_GLFLOW"]
["UF2停止操作","DR.UF2_BT_ESTOP"]
["UF2手动过滤操作","DR.UF2_BT_GL"]
["UF2手动初始化操作","DR.UF2_BT_INAI"]
["UF2故障复位操作","DR.UF2_BT_RESET"]
["UF2手动屏蔽液位开关","DR.UF2_BT_PB_YWKG"]
["UF2手自动模式操作","DR.UF2_BT_SYS_AUTO"]
["UF2阀门手自动操作","DR.UF2_BT_V_AUTO"]
["UF2 CEB碱选择","DR.UF2_CEB_J"]
["UF2 CEB酸选择","DR.UF2_CEB_S"]
["UF2压差高限值报错","DR.UF2_ERR_YC_H"]
["UF2压差高高值报错","DR.UF2_ERR_YC_HH"]
["UF2药剂残留报错","DR.UF2_ERR_YJCL"]
["UF2过滤准备好标志","DR.UF2_FLAG_GL_READY"]
["UF2膜内有药标志","DR.UF2_FLAG_MNYY"]
["UF2无它CEB标志","DR.UF2_FLAG_NOOTHERCEB"]
["UF2阀准备好标志","DR.UF2_FLAG_V_READY"]
["UF2系统报错","DR.UF2_SYS_ERR"]
["UF1反洗进水阀手自动","DR.V_1#UF_BWJS_BT_AUTO"]
["UF1反洗进水阀手动关","DR.V_1#UF_BWJS_BT_CLOSE"]
["UF1反洗进水阀手动开","DR.V_1#UF_BWJS_BT_OPEN"]
["UF1反洗进水阀故障复位","DR.V_1#UF_BWJS_BT_RESET"]
["UF1反洗进水阀关到位","DR.V_1#UF_BWJS_CFB"]
["UF1反洗进水阀关闭中","DR.V_1#UF_BWJS_CING"]
["UF1反洗进水阀自动关闭","DR.V_1#UF_BWJS_CLOSEAUT"]
["UF1反洗进水阀故障","DR.V_1#UF_BWJS_ERR"]
["UF1反洗进水阀总故障","DR.V_1#UF_BWJS_ERRT"]
["UF1反洗进水阀开到位","DR.V_1#UF_BWJS_OFB"]
["UF1反洗进水阀打开中","DR.V_1#UF_BWJS_OING"]
["UF1反洗进水阀自动打开","DR.V_1#UF_BWJS_OPENAUTO"]
["UF1反洗进水阀关闭","DR.V_1#UF_BWJS_OUT_CLOS"]
["UF1反洗进水阀打开","DR.V_1#UF_BWJS_OUT_OPEN"]
["UF1反洗进水阀准备好","DR.V_1#UF_BWJS_READY"]
["UF1反洗进水阀远程","DR.V_1#UF_BWJS_REM"]
["UF1反洗排水阀手自动","DR.V_1#UF_BWPS_BT_AUTO"]
["UF1反洗排水阀手动关","DR.V_1#UF_BWPS_BT_CLOSE"]
["UF1反洗排水阀手动开","DR.V_1#UF_BWPS_BT_OPEN"]
["UF1反洗排水阀故障复位","DR.V_1#UF_BWPS_BT_RESET"]
["UF1反洗排水阀关到位","DR.V_1#UF_BWPS_CFB"]
["UF1反洗排水阀关闭中","DR.V_1#UF_BWPS_CING"]
["UF1反洗排水阀自动关闭","DR.V_1#UF_BWPS_CLOSEAUT"]
["UF1反洗排水阀故障","DR.V_1#UF_BWPS_ERR"]
["UF1反洗排水阀总故障","DR.V_1#UF_BWPS_ERRT"]
["UF1反洗排水阀开到位","DR.V_1#UF_BWPS_OFB"]
["UF1反洗排水阀打开中","DR.V_1#UF_BWPS_OING"]
["UF1反洗排水阀自动打开","DR.V_1#UF_BWPS_OPENAUTO"]
["UF1反洗排水阀关闭","DR.V_1#UF_BWPS_OUT_CLOS"]
["UF1反洗排水阀打开","DR.V_1#UF_BWPS_OUT_OPEN"]
["UF1反洗排水阀准备好","DR.V_1#UF_BWPS_READY"]
["UF1反洗排水阀远程","DR.V_1#UF_BWPS_REM"]
["UF1产水阀手自动","DR.V_1#UF_CS_BT_AUTO"]
["UF1产水阀手动关","DR.V_1#UF_CS_BT_CLOSE"]
["UF1产水阀手动开","DR.V_1#UF_CS_BT_OPEN"]
["UF1产水阀故障复位","DR.V_1#UF_CS_BT_RESET"]
["UF1产水阀关到位","DR.V_1#UF_CS_CFB"]
["UF1产水阀关闭中","DR.V_1#UF_CS_CING"]
["UF1产水阀自动关闭","DR.V_1#UF_CS_CLOSEAUTO"]
["UF1产水阀故障","DR.V_1#UF_CS_ERR"]
["UF1产水阀总故障","DR.V_1#UF_CS_ERRT"]
["UF1产水阀开到位","DR.V_1#UF_CS_OFB"]
["UF1产水阀打开中","DR.V_1#UF_CS_OING"]
["UF1产水阀自动打开","DR.V_1#UF_CS_OPENAUTO"]
["UF1产水阀关闭","DR.V_1#UF_CS_OUT_CLOSE"]
["UF1产水阀打开","DR.V_1#UF_CS_OUT_OPEN"]
["UF1产水阀准备好","DR.V_1#UF_CS_OUT_READY"]
["UF1产水阀远程","DR.V_1#UF_CS_REM"]
["UF1排气阀1手自动","DR.V_1#UF_PQ1_BT_AUTO"]
["UF1排气阀1手动关","DR.V_1#UF_PQ1_BT_CLOSE"]
["UF1排气阀1手动开","DR.V_1#UF_PQ1_BT_OPEN"]
["UF1排气阀1故障复位","DR.V_1#UF_PQ1_BT_RESET"]
["UF1排气阀1关到位","DR.V_1#UF_PQ1_CFB"]
["UF1排气阀1关闭中","DR.V_1#UF_PQ1_CING"]
["UF1排气阀1自动关闭","DR.V_1#UF_PQ1_CLOSEAUTO"]
["UF1排气阀1故障","DR.V_1#UF_PQ1_ERR"]
["UF1排气阀1总故障","DR.V_1#UF_PQ1_ERRT"]
["UF1排气阀1开到位","DR.V_1#UF_PQ1_OFB"]
["UF1排气阀1打开中","DR.V_1#UF_PQ1_OING"]
["UF1排气阀1自动打开","DR.V_1#UF_PQ1_OPENAUTO"]
["UF1排气阀1关闭","DR.V_1#UF_PQ1_OUT_CLOSE"]
["UF1排气阀1打开","DR.V_1#UF_PQ1_OUT_OPEN"]
["UF1排气阀1准备好","DR.V_1#UF_PQ1_OUT_READY"]
["UF1排气阀1远程","DR.V_1#UF_PQ1_REM"]
["UF1排气阀2手自动","DR.V_1#UF_PQ2_BT_AUTO"]
["UF1排气阀2手动关","DR.V_1#UF_PQ2_BT_CLOSE"]
["UF1排气阀2手动开","DR.V_1#UF_PQ2_BT_OPEN"]
["UF1排气阀2故障复位","DR.V_1#UF_PQ2_BT_RESET"]
["UF1排气阀2关到位","DR.V_1#UF_PQ2_CFB"]
["UF1排气阀2关闭中","DR.V_1#UF_PQ2_CING"]
["UF1排气阀2自动关闭","DR.V_1#UF_PQ2_CLOSEAUTO"]
["UF1排气阀2故障","DR.V_1#UF_PQ2_ERR"]
["UF1排气阀2总故障","DR.V_1#UF_PQ2_ERRT"]
["UF1排气阀2开到位","DR.V_1#UF_PQ2_OFB"]
["UF1排气阀2打开中","DR.V_1#UF_PQ2_OING"]
["UF1排气阀2自动打开","DR.V_1#UF_PQ2_OPENAUTO"]
["UF1排气阀2关闭","DR.V_1#UF_PQ2_OUT_CLOSE"]
["UF1排气阀2打开","DR.V_1#UF_PQ2_OUT_OPEN"]
["UF1排气阀2准备好","DR.V_1#UF_PQ2_OUT_READY"]
["UF1排气阀2远程","DR.V_1#UF_PQ2_REM"]
["UF1排气阀3手自动","DR.V_1#UF_PQ3_BT_AUTO"]
["UF1排气阀3手动关","DR.V_1#UF_PQ3_BT_CLOSE"]
["UF1排气阀3手动开","DR.V_1#UF_PQ3_BT_OPEN"]
["UF1排气阀3故障复位","DR.V_1#UF_PQ3_BT_RESET"]
["UF1排气阀3关到位","DR.V_1#UF_PQ3_CFB"]
["UF1排气阀3关闭中","DR.V_1#UF_PQ3_CING"]
["UF1排气阀3自动关闭","DR.V_1#UF_PQ3_CLOSEAUTO"]
["UF1排气阀3故障","DR.V_1#UF_PQ3_ERR"]
["UF1排气阀3总故障","DR.V_1#UF_PQ3_ERRT"]
["UF1排气阀3开到位","DR.V_1#UF_PQ3_OFB"]
["UF1排气阀3打开中","DR.V_1#UF_PQ3_OING"]
["UF1排气阀3自动打开","DR.V_1#UF_PQ3_OPENAUTO"]
["UF1排气阀3关闭","DR.V_1#UF_PQ3_OUT_CLOSE"]
["UF1排气阀3打开","DR.V_1#UF_PQ3_OUT_OPEN"]
["UF1排气阀3准备好","DR.V_1#UF_PQ3_READY"]
["UF1排气阀3远程","DR.V_1#UF_PQ3_REM"]
["UF1排气阀4手自动","DR.V_1#UF_PQ4_BT_AUTO"]
["UF1排气阀4手动关","DR.V_1#UF_PQ4_BT_CLOSE"]
["UF1排气阀4手动开","DR.V_1#UF_PQ4_BT_OPEN"]
["UF1排气阀4故障复位","DR.V_1#UF_PQ4_BT_RESET"]
["UF1排气阀4关到位","DR.V_1#UF_PQ4_CFB"]
["UF1排气阀4关闭中","DR.V_1#UF_PQ4_CING"]
["UF1排气阀4自动关闭","DR.V_1#UF_PQ4_CLOSEAUTO"]
["UF1排气阀4故障","DR.V_1#UF_PQ4_ERR"]
["UF1排气阀4总故障","DR.V_1#UF_PQ4_ERRT"]
["UF1排气阀4开到位","DR.V_1#UF_PQ4_OFB"]
["UF1排气阀4打开中","DR.V_1#UF_PQ4_OING"]
["UF1排气阀4自动打开","DR.V_1#UF_PQ4_OPENAUTO"]
["UF1排气阀4关闭","DR.V_1#UF_PQ4_OUT_CLOSE"]
["UF1排气阀4打开","DR.V_1#UF_PQ4_OUT_OPEN"]
["UF1排气阀4准备好","DR.V_1#UF_PQ4_OUT_READY"]
["UF1排气阀4远程","DR.V_1#UF_PQ4_REM"]
["UF1隔断阀手自动","DR.V_1#UFCIPGL_BT_AUTO"]
["UF1隔断阀手动关","DR.V_1#UFCIPGL_BT_CLOSE"]
["UF1隔断阀手动开","DR.V_1#UFCIPGL_BT_OPEN"]
["UF1隔断阀故障复位","DR.V_1#UFCIPGL_BT_RESET"]
["UF1隔断阀关到位","DR.V_1#UFCIPGL_CFB"]
["UF1隔断阀关闭中","DR.V_1#UFCIPGL_CING"]
["UF1隔断阀自动关闭","DR.V_1#UFCIPGL_CLOSEA"]
["UF1隔断阀故障","DR.V_1#UFCIPGL_EER"]
["UF1隔断阀总故障","DR.V_1#UFCIPGL_ERRT"]
["UF1隔断阀开到位","DR.V_1#UFCIPGL_OFB"]
["UF1隔断阀打开中","DR.V_1#UFCIPGL_OING"]
["UF1隔断阀自动打开","DR.V_1#UFCIPGL_OPENAU"]
["UF1隔断阀关闭","DR.V_1#UFCIPGL_OUT_CL"]
["UF1隔断阀打开","DR.V_1#UFCIPGL_OUT_OP"]
["UF1隔断阀准备好","DR.V_1#UFCIPGL_READY"]
["UF1隔断阀远程","DR.V_1#UFCIPGL_REM"]
["RO1不合格阀手自动","DR.V_1RO_BHG_BT_AUTO"]
["RO1不合格阀手动关","DR.V_1RO_BHG_BT_CLOSE"]
["RO1不合格阀手动开","DR.V_1RO_BHG_BT_OPEN"]
["RO1不合格阀故障复位","DR.V_1RO_BHG_BT_RESET"]
["RO1不合格阀关到位","DR.V_1RO_BHG_CFB"]
["RO1不合格阀关闭中","DR.V_1RO_BHG_CING"]
["RO1不合格阀自动关闭","DR.V_1RO_BHG_CLOSEAUTO"]
["RO1不合格阀故障","DR.V_1RO_BHG_ERR"]
["RO1不合格阀总故障","DR.V_1RO_BHG_ERRT"]
["RO1不合格阀开到位","DR.V_1RO_BHG_OFB"]
["RO1不合格阀打开中","DR.V_1RO_BHG_OING"]
["RO1不合格阀自动打开","DR.V_1RO_BHG_OPENAUTO"]
["RO1不合格阀关闭","DR.V_1RO_BHG_OUT_CLOSE"]
["RO1不合格阀打开","DR.V_1RO_BHG_OUT_OPEN"]
["RO1不合格阀准备好","DR.V_1RO_BHG_OUT_READY"]
["RO1不合格阀远程","DR.V_1RO_BHG_REM"]
["RO1产水阀手自动","DR.V_1RO_CS_BT_AUTO"]
["RO1产水阀手动关","DR.V_1RO_CS_BT_CLOSE"]
["RO1产水阀手动开","DR.V_1RO_CS_BT_OPEN"]
["RO1产水阀故障复位","DR.V_1RO_CS_BT_RESET"]
["RO1产水阀关到位","DR.V_1RO_CS_CFB"]
["RO1产水阀关闭中","DR.V_1RO_CS_CING"]
["RO1产水阀自动关闭","DR.V_1RO_CS_CLOSEAUTO"]
["RO1产水阀故障","DR.V_1RO_CS_ERR"]
["RO1产水阀总故障","DR.V_1RO_CS_ERRT"]
["RO1产水阀开到位","DR.V_1RO_CS_OFB"]
["RO1产水阀打开中","DR.V_1RO_CS_OING"]
["RO1产水阀自动打开","DR.V_1RO_CS_OPENAUTO"]
["RO1产水阀关闭","DR.V_1RO_CS_OUT_CLOSE"]
["RO1产水阀打开","DR.V_1RO_CS_OUT_OPEN"]
["RO1产水阀准备好","DR.V_1RO_CS_OUT_READY"]
["RO1产水阀远程","DR.V_1RO_CS_REM"]
["RO1进水阀手自动","DR.V_1RO_JS_BT_AUTO"]
["RO1进水阀手动关","DR.V_1RO_JS_BT_CLOSE"]
["RO1进水阀手动开","DR.V_1RO_JS_BT_OPEN"]
["RO1进水阀故障复位","DR.V_1RO_JS_BT_RESET"]
["RO1进水阀关到位","DR.V_1RO_JS_CFB"]
["RO1进水阀关闭中","DR.V_1RO_JS_CING"]
["RO1进水阀自动关闭","DR.V_1RO_JS_CLOSEA"]
["RO1进水阀故障","DR.V_1RO_JS_ERR"]
["RO1进水阀总故障","DR.V_1RO_JS_ERRT"]
["RO1进水阀开到位","DR.V_1RO_JS_OFB"]
["RO1进水阀打开中","DR.V_1RO_JS_OING"]
["RO1进水阀自动打开","DR.V_1RO_JS_OPENA"]
["RO1进水阀关闭","DR.V_1RO_JS_OUT_CLOSE"]
["RO1进水阀打开","DR.V_1RO_JS_OUT_OPEN"]
["RO1进水阀准备好","DR.V_1RO_JS_OUT_READY"]
["RO1进水阀远程","DR.V_1RO_JS_REM"]
["RO1二段产水排气阀手自动","DR.V_1ROEDCSPQ_BT_AUTO"]
["RO1二段产水排气阀手动关","DR.V_1ROEDCSPQ_BT_CLOSE"]
["RO1二段产水排气阀手动开","DR.V_1ROEDCSPQ_BT_OPEN"]
["RO1二段产水排气阀故障复位","DR.V_1ROEDCSPQ_BT_RESET"]
["RO1二段产水排气阀关到位","DR.V_1ROEDCSPQ_CFB"]
["RO1二段产水排气阀关闭中","DR.V_1ROEDCSPQ_CING"]
["RO1二段产水排气阀自动关闭","DR.V_1ROEDCSPQ_CLOSEA"]
["RO1二段产水排气阀故障","DR.V_1ROEDCSPQ_ERR"]
["RO1二段产水排气阀总故障","DR.V_1ROEDCSPQ_ERRT"]
["RO1二段产水排气阀开到位","DR.V_1ROEDCSPQ_OFB"]
["RO1二段产水排气阀打开中","DR.V_1ROEDCSPQ_OING"]
["RO1二段产水排气阀自动打开","DR.V_1ROEDCSPQ_OPENA"]
["RO1二段产水排气阀关闭","DR.V_1ROEDCSPQ_OUT_C"]
["RO1二段产水排气阀打开","DR.V_1ROEDCSPQ_OUT_O"]
["RO1二段产水排气阀准备好","DR.V_1ROEDCSPQ_READY"]
["RO1二段产水排气阀远程","DR.V_1ROEDCSPQ_REM"]
["RO1二段进水排气阀手自动","DR.V_1ROEDJSPQ_BT_AUTO"]
["RO1二段进水排气阀手动关","DR.V_1ROEDJSPQ_BT_CLOSE"]
["RO1二段进水排气阀手动开","DR.V_1ROEDJSPQ_BT_OPEN"]
["RO1二段进水排气阀故障复位","DR.V_1ROEDJSPQ_BT_RESET"]
["RO1二段进水排气阀关到位","DR.V_1ROEDJSPQ_CFB"]
["RO1二段进水排气阀关闭中","DR.V_1ROEDJSPQ_CING"]
["RO1二段进水排气阀自动关闭","DR.V_1ROEDJSPQ_CLOSE"]
["RO1二段进水排气阀故障","DR.V_1ROEDJSPQ_ERR"]
["RO1二段进水排气阀总故障","DR.V_1ROEDJSPQ_ERRT"]
["RO1二段进水排气阀开到位","DR.V_1ROEDJSPQ_OFB"]
["RO1二段进水排气阀打开中","DR.V_1ROEDJSPQ_OING"]
["RO1二段进水排气阀自动打开","DR.V_1ROEDJSPQ_OPENA"]
["RO1二段进水排气阀关闭","DR.V_1ROEDJSPQ_OUT_C"]
["RO1二段进水排气阀打开","DR.V_1ROEDJSPQ_OUT_O"]
["RO1二段进水排气阀准备好","DR.V_1ROEDJSPQ_READY"]
["RO1二段进水排气阀远程","DR.V_1ROEDJSPQ_REM"]
["RO1二段浓水排气阀手自动","DR.V_1ROEDNSPQ_BT_AUTO"]
["RO1二段浓水排气阀手动关","DR.V_1ROEDNSPQ_BT_CLOSE"]
["RO1二段浓水排气阀手动开","DR.V_1ROEDNSPQ_BT_OPEN"]
["RO1二段浓水排气阀故障复位","DR.V_1ROEDNSPQ_BT_RESET"]
["RO1二段浓水排气阀关到位","DR.V_1ROEDNSPQ_CFB"]
["RO1二段浓水排气阀关闭中","DR.V_1ROEDNSPQ_CING"]
["RO1二段浓水排气阀自动关闭","DR.V_1ROEDNSPQ_CLOSE"]
["RO1二段浓水排气阀故障","DR.V_1ROEDNSPQ_ERR"]
["RO1二段浓水排气阀总故障","DR.V_1ROEDNSPQ_ERRT"]
["RO1二段浓水排气阀开到位","DR.V_1ROEDNSPQ_OFB"]
["RO1二段浓水排气阀打开中","DR.V_1ROEDNSPQ_OING"]
["RO1二段浓水排气阀自动打开","DR.V_1ROEDNSPQ_OPENA"]
["RO1二段浓水排气阀关闭","DR.V_1ROEDNSPQ_OUT_C"]
["RO1二段浓水排气阀打开","DR.V_1ROEDNSPQ_OUT_O"]
["RO1二段浓水排气阀准备好","DR.V_1ROEDNSPQ_READY"]
["RO1二段浓水排气阀远程","DR.V_1ROEDNSPQ_REM"]
["RO1三段产水排气阀手自动","DR.V_1ROSDCSPQ_BT_AUTO"]
["RO1三段产水排气阀手动关","DR.V_1ROSDCSPQ_BT_CLOSE"]
["RO1三段产水排气阀手动开","DR.V_1ROSDCSPQ_BT_OPEN"]
["RO1三段产水排气阀故障复位","DR.V_1ROSDCSPQ_BT_RESET"]
["RO1三段产水排气阀关到位","DR.V_1ROSDCSPQ_CFB"]
["RO1三段产水排气阀关闭中","DR.V_1ROSDCSPQ_CING"]
["RO1三段产水排气阀自动关闭","DR.V_1ROSDCSPQ_CLOSEA"]
["RO1三段产水排气阀故障","DR.V_1ROSDCSPQ_ERR"]
["RO1三段产水排气阀总故障","DR.V_1ROSDCSPQ_ERRT"]
["RO1三段产水排气阀开到位","DR.V_1ROSDCSPQ_OFB"]
["RO1三段产水排气阀打开中","DR.V_1ROSDCSPQ_OING"]
["RO1三段产水排气阀自动打开","DR.V_1ROSDCSPQ_OPENA"]
["RO1三段产水排气阀关闭","DR.V_1ROSDCSPQ_OUT_C"]
["RO1三段产水排气阀打开","DR.V_1ROSDCSPQ_OUT_O"]
["RO1三段产水排气阀准备好","DR.V_1ROSDCSPQ_READY"]
["RO1三段产水排气阀远程","DR.V_1ROSDCSPQ_REM"]
["RO1三段冲洗排水阀手自动","DR.V_1ROSDCXPS_BT_AUTO"]
["RO1三段冲洗排水阀手动关","DR.V_1ROSDCXPS_BT_CLOSE"]
["RO1三段冲洗排水阀手动开","DR.V_1ROSDCXPS_BT_OPEN"]
["RO1三段冲洗排水阀故障复位","DR.V_1ROSDCXPS_BT_RESET"]
["RO1三段冲洗排水阀关到位","DR.V_1ROSDCXPS_CFB"]
["RO1三段冲洗排水阀关闭中","DR.V_1ROSDCXPS_CING"]
["RO1三段冲洗排水阀自动关闭","DR.V_1ROSDCXPS_CLOSEA"]
["RO1三段冲洗排水阀故障","DR.V_1ROSDCXPS_ERR"]
["RO1三段冲洗排水阀总故障","DR.V_1ROSDCXPS_ERRT"]
["RO1三段冲洗排水阀开到位","DR.V_1ROSDCXPS_OFB"]
["RO1三段冲洗排水阀打开中","DR.V_1ROSDCXPS_OING"]
["RO1三段冲洗排水阀自动打开","DR.V_1ROSDCXPS_OPENA"]
["RO1三段冲洗排水阀关闭","DR.V_1ROSDCXPS_OUT_C"]
["RO1三段冲洗排水阀打开","DR.V_1ROSDCXPS_OUT_O"]
["RO1三段冲洗排水阀准备好","DR.V_1ROSDCXPS_READY"]
["RO1三段冲洗排水阀远程","DR.V_1ROSDCXPS_REM"]
["RO1三段进水排气阀手自动","DR.V_1ROSDJSPQ_BT_AUTO"]
["RO1三段进水排气阀手动关","DR.V_1ROSDJSPQ_BT_CLOSE"]
["RO1三段进水排气阀手动开","DR.V_1ROSDJSPQ_BT_OPEN"]
["RO1三段进水排气阀故障复位","DR.V_1ROSDJSPQ_BT_RESET"]
["RO1三段进水排气阀关到位","DR.V_1ROSDJSPQ_CFB"]
["RO1三段进水排气阀关闭中","DR.V_1ROSDJSPQ_CING"]
["RO1三段进水排气阀自动关闭","DR.V_1ROSDJSPQ_CLOSEA"]
["RO1三段进水排气阀故障","DR.V_1ROSDJSPQ_ERR"]
["RO1三段进水排气阀总故障","DR.V_1ROSDJSPQ_ERRT"]
["RO1三段进水排气阀开到位","DR.V_1ROSDJSPQ_OFB"]
["RO1三段进水排气阀打开中","DR.V_1ROSDJSPQ_OING"]
["RO1三段进水排气阀自动打开","DR.V_1ROSDJSPQ_OPENA"]
["RO1三段进水排气阀关闭","DR.V_1ROSDJSPQ_OUT_C"]
["RO1三段进水排气阀打开","DR.V_1ROSDJSPQ_OUT_O"]
["RO1三段进水排气阀准备好","DR.V_1ROSDJSPQ_READY"]
["RO1三段进水排气阀远程","DR.V_1ROSDJSPQ_REM"]
["RO1三段浓水排气阀手自动","DR.V_1ROSDNSPQ_BT_AUTO"]
["RO1三段浓水排气阀手动关","DR.V_1ROSDNSPQ_BT_CLOSE"]
["RO1三段浓水排气阀手动开","DR.V_1ROSDNSPQ_BT_OPEN"]
["RO1三段浓水排气阀故障复位","DR.V_1ROSDNSPQ_BT_RESET"]
["RO1三段浓水排气阀关到位","DR.V_1ROSDNSPQ_CFB"]
["RO1三段浓水排气阀关闭中","DR.V_1ROSDNSPQ_CING"]
["RO1三段浓水排气阀自动关闭","DR.V_1ROSDNSPQ_CLOSEA"]
["RO1三段浓水排气阀故障","DR.V_1ROSDNSPQ_ERR"]
["RO1三段浓水排气阀总故障","DR.V_1ROSDNSPQ_ERRT"]
["RO1三段浓水排气阀开到位","DR.V_1ROSDNSPQ_OFB"]
["RO1三段浓水排气阀打开中","DR.V_1ROSDNSPQ_OING"]
["RO1三段浓水排气阀自动打开","DR.V_1ROSDNSPQ_OPENA"]
["RO1三段浓水排气阀关闭","DR.V_1ROSDNSPQ_OUT_C"]
["RO1三段浓水排气阀打开","DR.V_1ROSDNSPQ_OUT_O"]
["RO1三段浓水排气阀准备好","DR.V_1ROSDNSPQ_READY"]
["RO1三段浓水排气阀远程","DR.V_1ROSDNSPQ_REM"]
["RO1一段冲洗进水阀手自动","DR.V_1ROYDBWJS_BT_AUTO"]
["RO1一段冲洗进水阀手动关","DR.V_1ROYDBWJS_BT_CLOSE"]
["RO1一段冲洗进水阀手动开","DR.V_1ROYDBWJS_BT_OPEN"]
["RO1一段冲洗进水阀故障复位","DR.V_1ROYDBWJS_BT_RESET"]
["RO1一段冲洗进水阀关到位","DR.V_1ROYDBWJS_CFB"]
["RO1一段冲洗进水阀关闭中","DR.V_1ROYDBWJS_CING"]
["RO1一段冲洗进水阀自动关闭","DR.V_1ROYDBWJS_CLOSEA"]
["RO1一段冲洗进水阀故障","DR.V_1ROYDBWJS_ERR"]
["RO1一段冲洗进水阀总故障","DR.V_1ROYDBWJS_ERRT"]
["RO1一段冲洗进水阀开到位","DR.V_1ROYDBWJS_OFB"]
["RO1一段冲洗进水阀打开中","DR.V_1ROYDBWJS_OING"]
["RO1一段冲洗进水阀自动打开","DR.V_1ROYDBWJS_OPENA"]
["RO1一段冲洗进水阀关闭","DR.V_1ROYDBWJS_OUT_C"]
["RO1一段冲洗进水阀打开","DR.V_1ROYDBWJS_OUT_O"]
["RO1一段冲洗进水阀准备好","DR.V_1ROYDBWJS_READY"]
["RO1一段冲洗进水阀远程","DR.V_1ROYDBWJS_REM"]
["RO1一段冲洗排水阀手自动","DR.V_1ROYDBWPS_BT_AUTO"]
["RO1一段冲洗排水阀手动关","DR.V_1ROYDBWPS_BT_CLOSE"]
["RO1一段冲洗排水阀手动开","DR.V_1ROYDBWPS_BT_OPEN"]
["RO1一段冲洗排水阀故障复位","DR.V_1ROYDBWPS_BT_RESET"]
["RO1一段冲洗排水阀关到位","DR.V_1ROYDBWPS_CFB"]
["RO1一段冲洗排水阀关闭中","DR.V_1ROYDBWPS_CING"]
["RO1一段冲洗排水阀自动关闭","DR.V_1ROYDBWPS_CLOSEA"]
["RO1一段冲洗排水阀故障","DR.V_1ROYDBWPS_ERR"]
["RO1一段冲洗排水阀总故障","DR.V_1ROYDBWPS_ERRT"]
["RO1一段冲洗排水阀开到位","DR.V_1ROYDBWPS_OFB"]
["RO1一段冲洗排水阀打开中","DR.V_1ROYDBWPS_OING"]
["RO1一段冲洗排水阀自动打开","DR.V_1ROYDBWPS_OPENA"]
["RO1一段冲洗排水阀关闭","DR.V_1ROYDBWPS_OUT_C"]
["RO1一段冲洗排水阀打开","DR.V_1ROYDBWPS_OUT_O"]
["RO1一段冲洗排水阀准备好","DR.V_1ROYDBWPS_READY"]
["RO1一段冲洗排水阀远程","DR.V_1ROYDBWPS_REM"]
["RO1一段产水排气阀1手自动","DR.V_1ROYDCSP1_BT_AUTO"]
["RO1一段产水排气阀1手动关","DR.V_1ROYDCSP1_BT_CLOSE"]
["RO1一段产水排气阀1手动开","DR.V_1ROYDCSP1_BT_OPEN"]
["RO1一段产水排气阀1故障复位","DR.V_1ROYDCSP1_BT_RESET"]
["RO1一段产水排气阀1关到位","DR.V_1ROYDCSP1_CFB"]
["RO1一段产水排气阀1关闭中","DR.V_1ROYDCSP1_CING"]
["RO1一段产水排气阀1自动关闭","DR.V_1ROYDCSP1_CLOSA"]
["RO1一段产水排气阀1故障","DR.V_1ROYDCSP1_ERR"]
["RO1一段产水排气阀1总故障","DR.V_1ROYDCSP1_ERRT"]
["RO1一段产水排气阀1开到位","DR.V_1ROYDCSP1_OFB"]
["RO1一段产水排气阀1打开中","DR.V_1ROYDCSP1_OING"]
["RO1一段产水排气阀1自动打开","DR.V_1ROYDCSP1_OPEN"]
["RO1一段产水排气阀1关闭","DR.V_1ROYDCSP1_OUT_CL"]
["RO1一段产水排气阀1打开","DR.V_1ROYDCSP1_OUT_OP"]
["RO1一段产水排气阀1准备好","DR.V_1ROYDCSP1_READ"]
["RO1一段产水排气阀1远程","DR.V_1ROYDCSP1_REM"]
["RO1一段产水排气阀2手自动","DR.V_1ROYDCSP2_BT_AUTO"]
["RO1一段产水排气阀2手动关","DR.V_1ROYDCSP2_BT_CLOSE"]
["RO1一段产水排气阀2手动开","DR.V_1ROYDCSP2_BT_OPEN"]
["RO1一段产水排气阀2故障复位","DR.V_1ROYDCSP2_BT_RESET"]
["RO1一段产水排气阀2关到位","DR.V_1ROYDCSP2_CFB"]
["RO1一段产水排气阀2关闭中","DR.V_1ROYDCSP2_CING"]
["RO1一段产水排气阀2自动关闭","DR.V_1ROYDCSP2_CLOS"]
["RO1一段产水排气阀2故障","DR.V_1ROYDCSP2_ERR"]
["RO1一段产水排气阀2总故障","DR.V_1ROYDCSP2_ERRT"]
["RO1一段产水排气阀2开到位","DR.V_1ROYDCSP2_OFB"]
["RO1一段产水排气阀2打开中","DR.V_1ROYDCSP2_OING"]
["RO1一段产水排气阀2自动打开","DR.V_1ROYDCSP2_OPEN"]
["RO1一段产水排气阀2关闭","DR.V_1ROYDCSP2_OUTC"]
["RO1一段产水排气阀2打开","DR.V_1ROYDCSP2_OUTO"]
["RO1一段产水排气阀2准备好","DR.V_1ROYDCSP2_READY"]
["RO1一段产水排气阀2远程","DR.V_1ROYDCSP2_REM"]
["RO1一段超越旁路阀手自动","DR.V_1ROYDCYPL_BT_AUTO"]
["RO1一段超越旁路阀手动关","DR.V_1ROYDCYPL_BT_CLOSE"]
["RO1一段超越旁路阀手动开","DR.V_1ROYDCYPL_BT_OPEN"]
["RO1一段超越旁路阀故障复位","DR.V_1ROYDCYPL_BT_RESET"]
["RO1一段超越旁路阀关到位","DR.V_1ROYDCYPL_CFB"]
["RO1一段超越旁路阀关闭中","DR.V_1ROYDCYPL_CING"]
["RO1一段超越旁路阀自动关闭","DR.V_1ROYDCYPL_CLOSEA"]
["RO1一段超越旁路阀故障","DR.V_1ROYDCYPL_ERR"]
["RO1一段超越旁路阀总故障","DR.V_1ROYDCYPL_ERRT"]
["RO1一段超越旁路阀开到位","DR.V_1ROYDCYPL_OFB"]
["RO1一段超越旁路阀打开中","DR.V_1ROYDCYPL_OING"]
["RO1一段超越旁路阀自动打开","DR.V_1ROYDCYPL_OPENA"]
["RO1一段超越旁路阀关闭","DR.V_1ROYDCYPL_OUTC"]
["RO1一段超越旁路阀打开","DR.V_1ROYDCYPL_OUTO"]
["RO1一段超越旁路阀准备好","DR.V_1ROYDCYPL_READY"]
["RO1一段超越旁路阀远程","DR.V_1ROYDCYPL_REM"]
["RO1一段进水排气阀1手自动","DR.V_1ROYDJSP1_BT_AUTO"]
["RO1一段进水排气阀1手动关","DR.V_1ROYDJSP1_BT_CLOSE"]
["RO1一段进水排气阀1手动开","DR.V_1ROYDJSP1_BT_OPEN"]
["RO1一段进水排气阀1故障复位","DR.V_1ROYDJSP1_BT_RESET"]
["RO1一段进水排气阀1关到位","DR.V_1ROYDJSP1_CFB"]
["RO1一段进水排气阀1关闭中","DR.V_1ROYDJSP1_CING"]
["RO1一段进水排气阀1自动关闭","DR.V_1ROYDJSP1_CLOS"]
["RO1一段进水排气阀1故障","DR.V_1ROYDJSP1_ERR"]
["RO1一段进水排气阀1总故障","DR.V_1ROYDJSP1_ERRT"]
["RO1一段进水排气阀1开到位","DR.V_1ROYDJSP1_OFB"]
["RO1一段进水排气阀1打开中","DR.V_1ROYDJSP1_OING"]
["RO1一段进水排气阀1自动打开","DR.V_1ROYDJSP1_OPEN"]
["RO1一段进水排气阀1关闭","DR.V_1ROYDJSP1_OUTC"]
["RO1一段进水排气阀1打开","DR.V_1ROYDJSP1_OUTO"]
["RO1一段进水排气阀1准备好","DR.V_1ROYDJSP1_READY"]
["RO1一段进水排气阀1远程","DR.V_1ROYDJSP1_REM"]
["RO1一段进水排气阀2手自动","DR.V_1ROYDJSP2_BT_AUTO"]
["RO1一段进水排气阀2手动关","DR.V_1ROYDJSP2_BT_CLOSE"]
["RO1一段进水排气阀2手动开","DR.V_1ROYDJSP2_BT_OPEN"]
["RO1一段进水排气阀2故障复位","DR.V_1ROYDJSP2_BT_RESET"]
["RO1一段进水排气阀2关到位","DR.V_1ROYDJSP2_CFB"]
["RO1一段进水排气阀2关闭中","DR.V_1ROYDJSP2_CING"]
["RO1一段进水排气阀2自动关闭","DR.V_1ROYDJSP2_CLOSEA"]
["RO1一段进水排气阀2故障","DR.V_1ROYDJSP2_ERR"]
["RO1一段进水排气阀2总故障","DR.V_1ROYDJSP2_ERRT"]
["RO1一段进水排气阀2开到位","DR.V_1ROYDJSP2_OFB"]
["RO1一段进水排气阀2打开中","DR.V_1ROYDJSP2_OING"]
["RO1一段进水排气阀2自动打开","DR.V_1ROYDJSP2_OPENA"]
["RO1一段进水排气阀2关闭","DR.V_1ROYDJSP2_OUTC"]
["RO1一段进水排气阀2打开","DR.V_1ROYDJSP2_OUTO"]
["RO1一段进水排气阀2准备好","DR.V_1ROYDJSP2_READY"]
["RO1一段进水排气阀2远程","DR.V_1ROYDJSP2_REM"]
["RO1一段浓水排气阀1手自动","DR.V_1ROYDNSP1_BT_AUTO"]
["RO1一段浓水排气阀1手动关","DR.V_1ROYDNSP1_BT_CLOSE"]
["RO1一段浓水排气阀1手动开","DR.V_1ROYDNSP1_BT_OPEN"]
["RO1一段浓水排气阀1故障复位","DR.V_1ROYDNSP1_BT_RESET"]
["RO1一段浓水排气阀1关到位","DR.V_1ROYDNSP1_CFB"]
["RO1一段浓水排气阀1关闭中","DR.V_1ROYDNSP1_CING"]
["RO1一段浓水排气阀1自动关闭","DR.V_1ROYDNSP1_CLOS"]
["RO1一段浓水排气阀1故障","DR.V_1ROYDNSP1_ERR"]
["RO1一段浓水排气阀1总故障","DR.V_1ROYDNSP1_ERRT"]
["RO1一段浓水排气阀1开到位","DR.V_1ROYDNSP1_OFB"]
["RO1一段浓水排气阀1打开中","DR.V_1ROYDNSP1_OING"]
["RO1一段浓水排气阀1自动打开","DR.V_1ROYDNSP1_OPEN"]
["RO1一段浓水排气阀1关闭","DR.V_1ROYDNSP1_OUTC"]
["RO1一段浓水排气阀1打开","DR.V_1ROYDNSP1_OUTO"]
["RO1一段浓水排气阀1准备好","DR.V_1ROYDNSP1_READ"]
["RO1一段浓水排气阀1远程","DR.V_1ROYDNSP1_REM"]
["RO1一段浓水排气阀2手自动","DR.V_1ROYDNSP2_BT_AUTO"]
["RO1一段浓水排气阀2手动关","DR.V_1ROYDNSP2_BT_CLOSE"]
["RO1一段浓水排气阀2手动开","DR.V_1ROYDNSP2_BT_OPEN"]
["RO1一段浓水排气阀2故障复位","DR.V_1ROYDNSP2_BT_RESET"]
["RO1一段浓水排气阀2关到位","DR.V_1ROYDNSP2_CFB"]
["RO1一段浓水排气阀2关闭中","DR.V_1ROYDNSP2_CING"]
["RO1一段浓水排气阀2自动关闭","DR.V_1ROYDNSP2_CLOSEA"]
["RO1一段浓水排气阀2故障","DR.V_1ROYDNSP2_ERR"]
["RO1一段浓水排气阀2总故障","DR.V_1ROYDNSP2_ERRT"]
["RO1一段浓水排气阀2开到位","DR.V_1ROYDNSP2_OFB"]
["RO1一段浓水排气阀2打开中","DR.V_1ROYDNSP2_OING"]
["RO1一段浓水排气阀2自动打开","DR.V_1ROYDNSP2_OPEN"]
["RO1一段浓水排气阀2关闭","DR.V_1ROYDNSP2_OUTC"]
["RO1一段浓水排气阀2打开","DR.V_1ROYDNSP2_OUTO"]
["RO1一段浓水排气阀2准备好","DR.V_1ROYDNSP2_READY"]
["RO1一段浓水排气阀2远程","DR.V_1ROYDNSP2_REM"]
["RO1一段隔离阀手自动","DR.V_1ROYDQXGL_BT_AUTO"]
["RO1一段隔离阀手动关","DR.V_1ROYDQXGL_BT_CLOSE"]
["RO1一段隔离阀手动开","DR.V_1ROYDQXGL_BT_OPEN"]
["RO1一段隔离阀故障复位","DR.V_1ROYDQXGL_BT_RESET"]
["RO1一段隔离阀关到位","DR.V_1ROYDQXGL_CFB"]
["RO1一段隔离阀关闭中","DR.V_1ROYDQXGL_CING"]
["RO1一段隔离阀自动关闭","DR.V_1ROYDQXGL_CLOSEA"]
["RO1一段隔离阀故障","DR.V_1ROYDQXGL_ERR"]
["RO1一段隔离阀总故障","DR.V_1ROYDQXGL_ERRT"]
["RO1一段隔离阀开到位","DR.V_1ROYDQXGL_OFB"]
["RO1一段隔离阀打开中","DR.V_1ROYDQXGL_OING"]
["RO1一段隔离阀自动打开","DR.V_1ROYDQXGL_OPENA"]
["RO1一段隔离阀关闭","DR.V_1ROYDQXGL_OUT_C"]
["RO1一段隔离阀打开","DR.V_1ROYDQXGL_OUT_O"]
["RO1一段隔离阀准备好","DR.V_1ROYDQXGL_READY"]
["RO1一段隔离阀远程","DR.V_1ROYDQXGL_REM"]
["UF2反洗进水阀手自动","DR.V_2#UF_BWJS_BT_AUTO"]
["UF2反洗进水阀手动关","DR.V_2#UF_BWJS_BT_CLOSE"]
["UF2反洗进水阀手动开","DR.V_2#UF_BWJS_BT_OPEN"]
["UF2反洗进水阀故障复位","DR.V_2#UF_BWJS_BT_RESET"]
["UF2反洗进水阀关到位","DR.V_2#UF_BWJS_CFB"]
["UF2反洗进水阀关闭中","DR.V_2#UF_BWJS_CING"]
["UF2反洗进水阀自动关闭","DR.V_2#UF_BWJS_CLOSEAUT"]
["UF2反洗进水阀故障","DR.V_2#UF_BWJS_ERR"]
["UF2反洗进水阀总故障","DR.V_2#UF_BWJS_ERRT"]
["UF2反洗进水阀开到位","DR.V_2#UF_BWJS_OFB"]
["UF2反洗进水阀打开中","DR.V_2#UF_BWJS_OING"]
["UF2反洗进水阀自动打开","DR.V_2#UF_BWJS_OPENAUTO"]
["UF2反洗进水阀关闭","DR.V_2#UF_BWJS_OUT_CLOS"]
["UF2反洗进水阀打开","DR.V_2#UF_BWJS_OUT_OPEN"]
["UF2反洗进水阀准备好","DR.V_2#UF_BWJS_READY"]
["UF2反洗进水阀远程","DR.V_2#UF_BWJS_REM"]
["UF2反洗排水阀手自动","DR.V_2#UF_BWPS_BT_AUTO"]
["UF2反洗排水阀手动关","DR.V_2#UF_BWPS_BT_CLOSE"]
["UF2反洗排水阀手动开","DR.V_2#UF_BWPS_BT_OPEN"]
["UF2反洗排水阀故障复位","DR.V_2#UF_BWPS_BT_RESET"]
["UF2反洗排水阀关到位","DR.V_2#UF_BWPS_CFB"]
["UF2反洗排水阀关闭中","DR.V_2#UF_BWPS_CING"]
["UF2反洗排水阀自动关闭","DR.V_2#UF_BWPS_CLOSEAUT"]
["UF2反洗排水阀故障","DR.V_2#UF_BWPS_ERR"]
["UF2反洗排水阀总故障","DR.V_2#UF_BWPS_ERRT"]
["UF2反洗排水阀开到位","DR.V_2#UF_BWPS_OFB"]
["UF2反洗排水阀打开中","DR.V_2#UF_BWPS_OING"]
["UF2反洗排水阀自动打开","DR.V_2#UF_BWPS_OPENAUTO"]
["UF2反洗排水阀关闭","DR.V_2#UF_BWPS_OUT_CLOS"]
["UF2反洗排水阀打开","DR.V_2#UF_BWPS_OUT_OPEN"]
["UF2反洗排水阀准备好","DR.V_2#UF_BWPS_READY"]
["UF2反洗排水阀远程","DR.V_2#UF_BWPS_REM"]
["UF2产水阀手自动","DR.V_2#UF_CS_BT_AUTO"]
["UF2产水阀手动关","DR.V_2#UF_CS_BT_CLOSE"]
["UF2产水阀手动开","DR.V_2#UF_CS_BT_OPEN"]
["UF2产水阀故障复位","DR.V_2#UF_CS_BT_RESET"]
["UF2产水阀关到位","DR.V_2#UF_CS_CFB"]
["UF2产水阀关闭中","DR.V_2#UF_CS_CING"]
["UF2产水阀自动关闭","DR.V_2#UF_CS_CLOSEAUTO"]
["UF2产水阀故障","DR.V_2#UF_CS_ERR"]
["UF2产水阀总故障","DR.V_2#UF_CS_ERRT"]
["UF2产水阀开到位","DR.V_2#UF_CS_OFB"]
["UF2产水阀打开中","DR.V_2#UF_CS_OING"]
["UF2产水阀自动打开","DR.V_2#UF_CS_OPENAUTO"]
["UF2产水阀关闭","DR.V_2#UF_CS_OUT_CLOSE"]
["UF2产水阀打开","DR.V_2#UF_CS_OUT_OPEN"]
["UF2产水阀准备好","DR.V_2#UF_CS_READY"]
["UF2产水阀远程","DR.V_2#UF_CS_REM"]
["UF2排气阀1手自动","DR.V_2#UF_PQ1_BT_AUTO"]
["UF2排气阀1手动关","DR.V_2#UF_PQ1_BT_CLOSE"]
["UF2排气阀1手动开","DR.V_2#UF_PQ1_BT_OPEN"]
["UF2排气阀1故障复位","DR.V_2#UF_PQ1_BT_RESET"]
["UF2排气阀1关到位","DR.V_2#UF_PQ1_CFB"]
["UF2排气阀1关闭中","DR.V_2#UF_PQ1_CING"]
["UF2排气阀1自动关闭","DR.V_2#UF_PQ1_CLOSEAUTO"]
["UF2排气阀1故障","DR.V_2#UF_PQ1_ERR"]
["UF2排气阀1总故障","DR.V_2#UF_PQ1_ERRT"]
["UF2排气阀1开到位","DR.V_2#UF_PQ1_OFB"]
["UF2排气阀1打开中","DR.V_2#UF_PQ1_OING"]
["UF2排气阀1自动打开","DR.V_2#UF_PQ1_OPENAUTO"]
["UF2排气阀1关闭","DR.V_2#UF_PQ1_OUT_CLOSE"]
["UF2排气阀1打开","DR.V_2#UF_PQ1_OUT_OPEN"]
["UF2排气阀1准备好","DR.V_2#UF_PQ1_READY"]
["UF2排气阀1远程","DR.V_2#UF_PQ1_REM"]
["UF2排气阀2手自动","DR.V_2#UF_PQ2_BT_AUTO"]
["UF2排气阀2手动关","DR.V_2#UF_PQ2_BT_CLOSE"]
["UF2排气阀2手动开","DR.V_2#UF_PQ2_BT_OPEN"]
["UF2排气阀2故障复位","DR.V_2#UF_PQ2_BT_RESET"]
["UF2排气阀2关到位","DR.V_2#UF_PQ2_CFB"]
["UF2排气阀2关闭中","DR.V_2#UF_PQ2_CING"]
["UF2排气阀2自动关闭","DR.V_2#UF_PQ2_CLOSEAUTO"]
["UF2排气阀2故障","DR.V_2#UF_PQ2_ERR"]
["UF2排气阀2总故障","DR.V_2#UF_PQ2_ERRT"]
["UF2排气阀2开到位","DR.V_2#UF_PQ2_OFB"]
["UF2排气阀2打开中","DR.V_2#UF_PQ2_OING"]
["UF2排气阀2自动打开","DR.V_2#UF_PQ2_OPENAUTO"]
["UF2排气阀2关闭","DR.V_2#UF_PQ2_OUT_CLOSE"]
["UF2排气阀2打开","DR.V_2#UF_PQ2_OUT_OPEN"]
["UF2排气阀2准备好","DR.V_2#UF_PQ2_READY"]
["UF2排气阀2远程","DR.V_2#UF_PQ2_REM"]
["UF2排气阀3手自动","DR.V_2#UF_PQ3_BT_AUTO"]
["UF2排气阀3手动关","DR.V_2#UF_PQ3_BT_CLOSE"]
["UF2排气阀3手动开","DR.V_2#UF_PQ3_BT_OPEN"]
["UF2排气阀3故障复位","DR.V_2#UF_PQ3_BT_RESET"]
["UF2排气阀3关到位","DR.V_2#UF_PQ3_CFB"]
["UF2排气阀3关闭中","DR.V_2#UF_PQ3_CING"]
["UF2排气阀3自动关闭","DR.V_2#UF_PQ3_CLOSEAUTO"]
["UF2排气阀3故障","DR.V_2#UF_PQ3_ERR"]
["UF2排气阀3总故障","DR.V_2#UF_PQ3_ERRT"]
["UF2排气阀3开到位","DR.V_2#UF_PQ3_OFB"]
["UF2排气阀3打开中","DR.V_2#UF_PQ3_OING"]
["UF2排气阀3自动打开","DR.V_2#UF_PQ3_OPENAUTO"]
["UF2排气阀3关闭","DR.V_2#UF_PQ3_OUT_CLOSE"]
["UF2排气阀3打开","DR.V_2#UF_PQ3_OUT_OPEN"]
["UF2排气阀3准备好","DR.V_2#UF_PQ3_READY"]
["UF2排气阀3远程","DR.V_2#UF_PQ3_REM"]
["UF2排气阀4手自动","DR.V_2#UF_PQ4_BT_AUTO"]
["UF2排气阀4手动关","DR.V_2#UF_PQ4_BT_CLOSE"]
["UF2排气阀4手动开","DR.V_2#UF_PQ4_BT_OPEN"]
["UF2排气阀4故障复位","DR.V_2#UF_PQ4_BT_RESET"]
["UF2排气阀4关到位","DR.V_2#UF_PQ4_CFB"]
["UF2排气阀4关闭中","DR.V_2#UF_PQ4_CING"]
["UF2排气阀4自动关闭","DR.V_2#UF_PQ4_CLOSEAUTO"]
["UF2排气阀4故障","DR.V_2#UF_PQ4_ERR"]
["UF2排气阀4总故障","DR.V_2#UF_PQ4_ERRT"]
["UF2排气阀4开到位","DR.V_2#UF_PQ4_OFB"]
["UF2排气阀4打开中","DR.V_2#UF_PQ4_OING"]
["UF2排气阀4自动打开","DR.V_2#UF_PQ4_OPENAUTO"]
["UF2排气阀4关闭","DR.V_2#UF_PQ4_OUT_CLOSE"]
["UF2排气阀4打开","DR.V_2#UF_PQ4_OUT_OPEN"]
["UF2排气阀4准备好","DR.V_2#UF_PQ4_READY"]
["UF2排气阀4远程","DR.V_2#UF_PQ4_REM"]
["UF2隔断阀手自动","DR.V_2#UFCIPGL_BT_AUTO"]
["UF2隔断阀手动关","DR.V_2#UFCIPGL_BT_CLOSE"]
["UF2隔断阀手动开","DR.V_2#UFCIPGL_BT_OPEN"]
["UF2隔断阀故障复位","DR.V_2#UFCIPGL_BT_RESET"]
["UF2隔断阀关到位","DR.V_2#UFCIPGL_CFB"]
["UF2隔断阀关闭中","DR.V_2#UFCIPGL_CING"]
["UF2隔断阀自动关闭","DR.V_2#UFCIPGL_CLOSEA"]
["UF2隔断阀故障","DR.V_2#UFCIPGL_ERR"]
["UF2隔断阀总故障","DR.V_2#UFCIPGL_ERRT"]
["UF2隔断阀开到位","DR.V_2#UFCIPGL_OFB"]
["UF2隔断阀打开中","DR.V_2#UFCIPGL_OING"]
["UF2隔断阀自动打开","DR.V_2#UFCIPGL_OPENAU"]
["UF2隔断阀关闭","DR.V_2#UFCIPGL_OUT_CL"]
["UF2隔断阀打开","DR.V_2#UFCIPGL_OUT_OP"]
["UF2隔断阀准备好","DR.V_2#UFCIPGL_READY"]
["UF2隔断阀远程","DR.V_2#UFCIPGL_REM"]
["RO2不合格阀手自动","DR.V_2RO_BHG_BT_AUTO"]
["RO2不合格阀手动关","DR.V_2RO_BHG_BT_CLOSE"]
["RO2不合格阀手动开","DR.V_2RO_BHG_BT_OPEN"]
["RO2不合格阀故障复位","DR.V_2RO_BHG_BT_RESET"]
["RO2不合格阀关到位","DR.V_2RO_BHG_CFB"]
["RO2不合格阀关闭中","DR.V_2RO_BHG_CING"]
["RO2不合格阀自动关闭","DR.V_2RO_BHG_CLOSEAUTO"]
["RO2不合格阀故障","DR.V_2RO_BHG_ERR"]
["RO2不合格阀总故障","DR.V_2RO_BHG_ERRT"]
["RO2不合格阀开到位","DR.V_2RO_BHG_OFB"]
["RO2不合格阀打开中","DR.V_2RO_BHG_OING"]
["RO2不合格阀自动打开","DR.V_2RO_BHG_OPENAUTO"]
["RO2不合格阀关闭","DR.V_2RO_BHG_OUT_CLOSE"]
["RO2不合格阀打开","DR.V_2RO_BHG_OUT_OPEN"]
["RO2不合格阀准备好","DR.V_2RO_BHG_OUT_READY"]
["RO2不合格阀远程","DR.V_2RO_BHG_REM"]
["RO2产水阀手自动","DR.V_2RO_CS_BT_AUTO"]
["RO2产水阀手动关","DR.V_2RO_CS_BT_CLOSE"]
["RO2产水阀手动开","DR.V_2RO_CS_BT_OPEN"]
["RO2产水阀故障复位","DR.V_2RO_CS_BT_RESET"]
["RO2产水阀关到位","DR.V_2RO_CS_CFB"]
["RO2产水阀关闭中","DR.V_2RO_CS_CING"]
["RO2产水阀自动关闭","DR.V_2RO_CS_CLOSEAUTO"]
["RO2产水阀故障","DR.V_2RO_CS_ERR"]
["RO2产水阀总故障","DR.V_2RO_CS_ERRT"]
["RO2产水阀开到位","DR.V_2RO_CS_OFB"]
["RO2产水阀打开中","DR.V_2RO_CS_OING"]
["RO2产水阀自动打开","DR.V_2RO_CS_OPENAUTO"]
["RO2产水阀关闭","DR.V_2RO_CS_OUT_CLOSE"]
["RO2产水阀打开","DR.V_2RO_CS_OUT_OPEN"]
["RO2产水阀准备好","DR.V_2RO_CS_OUT_READY"]
["RO2产水阀远程","DR.V_2RO_CS_REM"]
["RO2进水阀手自动","DR.V_2RO_JS_BT_AUTO"]
["RO2进水阀手动关","DR.V_2RO_JS_BT_CLOSE"]
["RO2进水阀手动开","DR.V_2RO_JS_BT_OPEN"]
["RO2进水阀故障复位","DR.V_2RO_JS_BT_RESET"]
["RO2进水阀关到位","DR.V_2RO_JS_CFB"]
["RO2进水阀关闭中","DR.V_2RO_JS_CING"]
["RO2进水阀自动关闭","DR.V_2RO_JS_CLOSEAUTO"]
["RO2进水阀故障","DR.V_2RO_JS_ERR"]
["RO2进水阀总故障","DR.V_2RO_JS_ERRT"]
["RO2进水阀开到位","DR.V_2RO_JS_OFB"]
["RO2进水阀打开中","DR.V_2RO_JS_OING"]
["RO2进水阀自动打开","DR.V_2RO_JS_OPENAUTO"]
["RO2进水阀关闭","DR.V_2RO_JS_OUT_CLOSE"]
["RO2进水阀打开","DR.V_2RO_JS_OUT_OPEN"]
["RO2进水阀准备好","DR.V_2RO_JS_OUT_READY"]
["RO2进水阀远程","DR.V_2RO_JS_REM"]
["RO2二段产水排气阀手自动","DR.V_2ROEDCSPQ_BT_AUTO"]
["RO2二段产水排气阀手动关","DR.V_2ROEDCSPQ_BT_CLOSE"]
["RO2二段产水排气阀手动开","DR.V_2ROEDCSPQ_BT_OPEN"]
["RO2二段产水排气阀故障复位","DR.V_2ROEDCSPQ_BT_RESET"]
["RO2二段产水排气阀关到位","DR.V_2ROEDCSPQ_CFB"]
["RO2二段产水排气阀关闭中","DR.V_2ROEDCSPQ_CING"]
["RO2二段产水排气阀自动关闭","DR.V_2ROEDCSPQ_CLOSEA"]
["RO2二段产水排气阀故障","DR.V_2ROEDCSPQ_ERR"]
["RO2二段产水排气阀总故障","DR.V_2ROEDCSPQ_ERRT"]
["RO2二段产水排气阀开到位","DR.V_2ROEDCSPQ_OFB"]
["RO2二段产水排气阀打开中","DR.V_2ROEDCSPQ_OING"]
["RO2二段产水排气阀自动打开","DR.V_2ROEDCSPQ_OPENA"]
["RO2二段产水排气阀关闭","DR.V_2ROEDCSPQ_OUT_C"]
["RO2二段产水排气阀打开","DR.V_2ROEDCSPQ_OUT_O"]
["RO2二段产水排气阀准备好","DR.V_2ROEDCSPQ_READY"]
["RO2二段产水排气阀远程","DR.V_2ROEDCSPQ_REM"]
["RO2二段进水排气阀手自动","DR.V_2ROEDJSPQ_BT_AUTO"]
["RO2二段进水排气阀手动关","DR.V_2ROEDJSPQ_BT_CLOSE"]
["RO2二段进水排气阀手动开","DR.V_2ROEDJSPQ_BT_OPEN"]
["RO2二段进水排气阀故障复位","DR.V_2ROEDJSPQ_BT_RESET"]
["RO2二段进水排气阀关到位","DR.V_2ROEDJSPQ_CFB"]
["RO2二段进水排气阀关闭中","DR.V_2ROEDJSPQ_CING"]
["RO2二段进水排气阀自动关闭","DR.V_2ROEDJSPQ_CLOSEA"]
["RO2二段进水排气阀故障","DR.V_2ROEDJSPQ_ERR"]
["RO2二段进水排气阀总故障","DR.V_2ROEDJSPQ_ERRT"]
["RO2二段进水排气阀开到位","DR.V_2ROEDJSPQ_OFB"]
["RO2二段进水排气阀打开中","DR.V_2ROEDJSPQ_OING"]
["RO2二段进水排气阀自动打开","DR.V_2ROEDJSPQ_OPENA"]
["RO2二段进水排气阀关闭","DR.V_2ROEDJSPQ_OUT_C"]
["RO2二段进水排气阀打开","DR.V_2ROEDJSPQ_OUT_O"]
["RO2二段进水排气阀准备好","DR.V_2ROEDJSPQ_READY"]
["RO2二段进水排气阀远程","DR.V_2ROEDJSPQ_REM"]
["RO2二段浓水排气阀手自动","DR.V_2ROEDNSPQ_BT_AUTO"]
["RO2二段浓水排气阀手动关","DR.V_2ROEDNSPQ_BT_CLOSE"]
["RO2二段浓水排气阀手动开","DR.V_2ROEDNSPQ_BT_OPEN"]
["RO2二段浓水排气阀故障复位","DR.V_2ROEDNSPQ_BT_RESET"]
["RO2二段浓水排气阀关到位","DR.V_2ROEDNSPQ_CFB"]
["RO2二段浓水排气阀关闭中","DR.V_2ROEDNSPQ_CING"]
["RO2二段浓水排气阀自动关闭","DR.V_2ROEDNSPQ_CLOSE"]
["RO2二段浓水排气阀故障","DR.V_2ROEDNSPQ_ERR"]
["RO2二段浓水排气阀总故障","DR.V_2ROEDNSPQ_ERRT"]
["RO2二段浓水排气阀开到位","DR.V_2ROEDNSPQ_OFB"]
["RO2二段浓水排气阀打开中","DR.V_2ROEDNSPQ_OING"]
["RO2二段浓水排气阀自动打开","DR.V_2ROEDNSPQ_OPENA"]
["RO2二段浓水排气阀关闭","DR.V_2ROEDNSPQ_OUT_C"]
["RO2二段浓水排气阀打开","DR.V_2ROEDNSPQ_OUT_O"]
["RO2二段浓水排气阀准备好","DR.V_2ROEDNSPQ_READY"]
["RO2二段浓水排气阀远程","DR.V_2ROEDNSPQ_REM"]
["RO2三段产水排气阀手自动","DR.V_2ROSDCSPQ_BT_AUTO"]
["RO2三段产水排气阀手动关","DR.V_2ROSDCSPQ_BT_CLOSE"]
["RO2三段产水排气阀手动开","DR.V_2ROSDCSPQ_BT_OPEN"]
["RO2三段产水排气阀故障复位","DR.V_2ROSDCSPQ_BT_RESET"]
["RO2三段产水排气阀关到位","DR.V_2ROSDCSPQ_CFB"]
["RO2三段产水排气阀关闭中","DR.V_2ROSDCSPQ_CING"]
["RO2三段产水排气阀自动关闭","DR.V_2ROSDCSPQ_CLOSE"]
["RO2三段产水排气阀故障","DR.V_2ROSDCSPQ_ERR"]
["RO2三段产水排气阀总故障","DR.V_2ROSDCSPQ_ERRT"]
["RO2三段产水排气阀开到位","DR.V_2ROSDCSPQ_OFB"]
["RO2三段产水排气阀打开中","DR.V_2ROSDCSPQ_OING"]
["RO2三段产水排气阀自动打开","DR.V_2ROSDCSPQ_OPENA"]
["RO2三段产水排气阀关闭","DR.V_2ROSDCSPQ_OUT_C"]
["RO2三段产水排气阀打开","DR.V_2ROSDCSPQ_OUT_O"]
["RO2三段产水排气阀准备好","DR.V_2ROSDCSPQ_READY"]
["RO2三段产水排气阀远程","DR.V_2ROSDCSPQ_REM"]
["RO2三段冲洗排水阀手自动","DR.V_2ROSDCXPS_BT_AUTO"]
["RO2三段冲洗排水阀手动关","DR.V_2ROSDCXPS_BT_CLOSE"]
["RO2三段冲洗排水阀手动开","DR.V_2ROSDCXPS_BT_OPEN"]
["RO2三段冲洗排水阀故障复位","DR.V_2ROSDCXPS_BT_RESET"]
["RO2三段冲洗排水阀关到位","DR.V_2ROSDCXPS_CFB"]
["RO2三段冲洗排水阀关闭中","DR.V_2ROSDCXPS_CING"]
["RO2三段冲洗排水阀自动关闭","DR.V_2ROSDCXPS_CLOSE"]
["RO2三段冲洗排水阀故障","DR.V_2ROSDCXPS_ERR"]
["RO2三段冲洗排水阀总故障","DR.V_2ROSDCXPS_ERRT"]
["RO2三段冲洗排水阀开到位","DR.V_2ROSDCXPS_OFB"]
["RO2三段冲洗排水阀打开中","DR.V_2ROSDCXPS_OING"]
["RO2三段冲洗排水阀自动打开","DR.V_2ROSDCXPS_OPENA"]
["RO2三段冲洗排水阀关闭","DR.V_2ROSDCXPS_OUT_C"]
["RO2三段冲洗排水阀打开","DR.V_2ROSDCXPS_OUT_O"]
["RO2三段冲洗排水阀准备好","DR.V_2ROSDCXPS_READY"]
["RO2三段冲洗排水阀远程","DR.V_2ROSDCXPS_REM"]
["RO2三段进水排气阀手自动","DR.V_2ROSDJSPQ_BT_AUTO"]
["RO2三段进水排气阀手动关","DR.V_2ROSDJSPQ_BT_CLOSE"]
["RO2三段进水排气阀手动开","DR.V_2ROSDJSPQ_BT_OPEN"]
["RO2三段进水排气阀故障复位","DR.V_2ROSDJSPQ_BT_RESET"]
["RO2三段进水排气阀关到位","DR.V_2ROSDJSPQ_CFB"]
["RO2三段进水排气阀关闭中","DR.V_2ROSDJSPQ_CING"]
["RO2三段进水排气阀自动关闭","DR.V_2ROSDJSPQ_CLOSE"]
["RO2三段进水排气阀故障","DR.V_2ROSDJSPQ_ERR"]
["RO2三段进水排气阀总故障","DR.V_2ROSDJSPQ_ERRT"]
["RO2三段进水排气阀开到位","DR.V_2ROSDJSPQ_OFB"]
["RO2三段进水排气阀打开中","DR.V_2ROSDJSPQ_OING"]
["RO2三段进水排气阀自动打开","DR.V_2ROSDJSPQ_OPENA"]
["RO2三段进水排气阀关闭","DR.V_2ROSDJSPQ_OUT_C"]
["RO2三段进水排气阀打开","DR.V_2ROSDJSPQ_OUT_O"]
["RO2三段进水排气阀准备好","DR.V_2ROSDJSPQ_READY"]
["RO2三段进水排气阀远程","DR.V_2ROSDJSPQ_REM"]
["RO2三段浓水排气阀手自动","DR.V_2ROSDNSPQ_BT_AUTO"]
["RO2三段浓水排气阀手动关","DR.V_2ROSDNSPQ_BT_CLOSE"]
["RO2三段浓水排气阀手动开","DR.V_2ROSDNSPQ_BT_OPEN"]
["RO2三段浓水排气阀故障复位","DR.V_2ROSDNSPQ_BT_RESET"]
["RO2三段浓水排气阀关到位","DR.V_2ROSDNSPQ_CFB"]
["RO2三段浓水排气阀关闭中","DR.V_2ROSDNSPQ_CING"]
["RO2三段浓水排气阀自动关闭","DR.V_2ROSDNSPQ_CLOSE"]
["RO2三段浓水排气阀故障","DR.V_2ROSDNSPQ_ERR"]
["RO2三段浓水排气阀总故障","DR.V_2ROSDNSPQ_ERRT"]
["RO2三段浓水排气阀开到位","DR.V_2ROSDNSPQ_OFB"]
["RO2三段浓水排气阀打开中","DR.V_2ROSDNSPQ_OING"]
["RO2三段浓水排气阀自动打开","DR.V_2ROSDNSPQ_OPENA"]
["RO2三段浓水排气阀关闭","DR.V_2ROSDNSPQ_OUT_C"]
["RO2三段浓水排气阀打开","DR.V_2ROSDNSPQ_OUT_O"]
["RO2三段浓水排气阀准备好","DR.V_2ROSDNSPQ_READY"]
["RO2三段浓水排气阀远程","DR.V_2ROSDNSPQ_REM"]
["RO2一段冲洗进水阀手自动","DR.V_2ROYDBWJS_BT_AUTO"]
["RO2一段冲洗进水阀手动关","DR.V_2ROYDBWJS_BT_CLOSE"]
["RO2一段冲洗进水阀手动开","DR.V_2ROYDBWJS_BT_OPEN"]
["RO2一段冲洗进水阀故障复位","DR.V_2ROYDBWJS_BT_RESET"]
["RO2一段冲洗进水阀关到位","DR.V_2ROYDBWJS_CFB"]
["RO2一段冲洗进水阀关闭中","DR.V_2ROYDBWJS_CING"]
["RO2一段冲洗进水阀自动关闭","DR.V_2ROYDBWJS_CLOSEA"]
["RO2一段冲洗进水阀故障","DR.V_2ROYDBWJS_ERR"]
["RO2一段冲洗进水阀总故障","DR.V_2ROYDBWJS_ERRT"]
["RO2一段冲洗进水阀开到位","DR.V_2ROYDBWJS_OFB"]
["RO2一段冲洗进水阀打开中","DR.V_2ROYDBWJS_OING"]
["RO2一段冲洗进水阀自动打开","DR.V_2ROYDBWJS_OPENA"]
["RO2一段冲洗进水阀关闭","DR.V_2ROYDBWJS_OUT_C"]
["RO2一段冲洗进水阀打开","DR.V_2ROYDBWJS_OUT_O"]
["RO2一段冲洗进水阀准备好","DR.V_2ROYDBWJS_READY"]
["RO2一段冲洗进水阀远程","DR.V_2ROYDBWJS_REM"]
["RO2一段冲洗排水阀手自动","DR.V_2ROYDBWPS_BT_AUTO"]
["RO2一段冲洗排水阀手动关","DR.V_2ROYDBWPS_BT_CLOSE"]
["RO2一段冲洗排水阀手动开","DR.V_2ROYDBWPS_BT_OPEN"]
["RO2一段冲洗排水阀故障复位","DR.V_2ROYDBWPS_BT_RESET"]
["RO2一段冲洗排水阀关到位","DR.V_2ROYDBWPS_CFB"]
["RO2一段冲洗排水阀关闭中","DR.V_2ROYDBWPS_CING"]
["RO2一段冲洗排水阀自动关闭","DR.V_2ROYDBWPS_CLOSE"]
["RO2一段冲洗排水阀故障","DR.V_2ROYDBWPS_ERR"]
["RO2一段冲洗排水阀总故障","DR.V_2ROYDBWPS_ERRT"]
["RO2一段冲洗排水阀开到位","DR.V_2ROYDBWPS_OFB"]
["RO2一段冲洗排水阀打开中","DR.V_2ROYDBWPS_OING"]
["RO2一段冲洗排水阀自动打开","DR.V_2ROYDBWPS_OPENA"]
["RO2一段冲洗排水阀关闭","DR.V_2ROYDBWPS_OUT_C"]
["RO2一段冲洗排水阀打开","DR.V_2ROYDBWPS_OUT_O"]
["RO2一段冲洗排水阀准备好","DR.V_2ROYDBWPS_READY"]
["RO2一段冲洗排水阀远程","DR.V_2ROYDBWPS_REM"]
["RO2一段产水排气阀1手自动","DR.V_2ROYDCSP1_BT_AUTO"]
["RO2一段产水排气阀1手动关","DR.V_2ROYDCSP1_BT_CLOSE"]
["RO2一段产水排气阀1手动开","DR.V_2ROYDCSP1_BT_OPEN"]
["RO2一段产水排气阀1故障复位","DR.V_2ROYDCSP1_BT_RESET"]
["RO2一段产水排气阀1关到位","DR.V_2ROYDCSP1_CFB"]
["RO2一段产水排气阀1关闭中","DR.V_2ROYDCSP1_CING"]
["RO2一段产水排气阀1自动关闭","DR.V_2ROYDCSP1_CLOS"]
["RO2一段产水排气阀1故障","DR.V_2ROYDCSP1_ERR"]
["RO2一段产水排气阀1总故障","DR.V_2ROYDCSP1_ERRT"]
["RO2一段产水排气阀1开到位","DR.V_2ROYDCSP1_OFB"]
["RO2一段产水排气阀1打开中","DR.V_2ROYDCSP1_OING"]
["RO2一段产水排气阀1自动打开","DR.V_2ROYDCSP1_OPEN"]
["RO2一段产水排气阀1关闭","DR.V_2ROYDCSP1_OUTC"]
["RO2一段产水排气阀1打开","DR.V_2ROYDCSP1_OUTO"]
["RO2一段产水排气阀1准备好","DR.V_2ROYDCSP1_READY"]
["RO2一段产水排气阀1远程","DR.V_2ROYDCSP1_REM"]
["RO2一段产水排气阀2手自动","DR.V_2ROYDCSP2_BT_AUTO"]
["RO2一段产水排气阀2手动关","DR.V_2ROYDCSP2_BT_CLOSE"]
["RO2一段产水排气阀2手动开","DR.V_2ROYDCSP2_BT_OPEN"]
["RO2一段产水排气阀2故障复位","DR.V_2ROYDCSP2_BT_RESET"]
["RO2一段产水排气阀2关到位","DR.V_2ROYDCSP2_CFB"]
["RO2一段产水排气阀2关闭中","DR.V_2ROYDCSP2_CING"]
["RO2一段产水排气阀2自动关闭","DR.V_2ROYDCSP2_CLOSEA"]
["RO2一段产水排气阀2故障","DR.V_2ROYDCSP2_ERR"]
["RO2一段产水排气阀2总故障","DR.V_2ROYDCSP2_ERRT"]
["RO2一段产水排气阀2开到位","DR.V_2ROYDCSP2_OFB"]
["RO2一段产水排气阀2打开中","DR.V_2ROYDCSP2_OING"]
["RO2一段产水排气阀2自动打开","DR.V_2ROYDCSP2_OPEN"]
["RO2一段产水排气阀2关闭","DR.V_2ROYDCSP2_OUTC"]
["RO2一段产水排气阀2打开","DR.V_2ROYDCSP2_OUTO"]
["RO2一段产水排气阀2准备好","DR.V_2ROYDCSP2_READY"]
["RO2一段产水排气阀2远程","DR.V_2ROYDCSP2_REM"]
["RO2一段超越旁路阀手自动","DR.V_2ROYDCYPL_BT_AUTO"]
["RO2一段超越旁路阀手动关","DR.V_2ROYDCYPL_BT_CLOSE"]
["RO2一段超越旁路阀手动开","DR.V_2ROYDCYPL_BT_OPEN"]
["RO2一段超越旁路阀故障复位","DR.V_2ROYDCYPL_BT_RESET"]
["RO2一段超越旁路阀关到位","DR.V_2ROYDCYPL_CFB"]
["RO2一段超越旁路阀关闭中","DR.V_2ROYDCYPL_CING"]
["RO2一段超越旁路阀自动关闭","DR.V_2ROYDCYPL_CLOSEA"]
["RO2一段超越旁路阀故障","DR.V_2ROYDCYPL_ERR"]
["RO2一段超越旁路阀总故障","DR.V_2ROYDCYPL_ERRT"]
["RO2一段超越旁路阀开到位","DR.V_2ROYDCYPL_OFB"]
["RO2一段超越旁路阀打开中","DR.V_2ROYDCYPL_OING"]
["RO2一段超越旁路阀自动打开","DR.V_2ROYDCYPL_OPENA"]
["RO2一段超越旁路阀关闭","DR.V_2ROYDCYPL_OUT_C"]
["RO2一段超越旁路阀打开","DR.V_2ROYDCYPL_OUT_O"]
["RO2一段超越旁路阀准备好","DR.V_2ROYDCYPL_READY"]
["RO2一段超越旁路阀远程","DR.V_2ROYDCYPL_REM"]
["RO2一段进水排气阀1手自动","DR.V_2ROYDJSP1_BT_AUTO"]
["RO2一段进水排气阀1手动关","DR.V_2ROYDJSP1_BT_CLOSE"]
["RO2一段进水排气阀1手动开","DR.V_2ROYDJSP1_BT_OPEN"]
["RO2一段进水排气阀1故障复位","DR.V_2ROYDJSP1_BT_RESET"]
["RO2一段进水排气阀1关到位","DR.V_2ROYDJSP1_CFB"]
["RO2一段进水排气阀1关闭中","DR.V_2ROYDJSP1_CING"]
["RO2一段进水排气阀1自动关闭","DR.V_2ROYDJSP1_CLOSEA"]
["RO2一段进水排气阀1故障","DR.V_2ROYDJSP1_ERR"]
["RO2一段进水排气阀1总故障","DR.V_2ROYDJSP1_ERRT"]
["RO2一段进水排气阀1开到位","DR.V_2ROYDJSP1_OFB"]
["RO2一段进水排气阀1打开中","DR.V_2ROYDJSP1_OING"]
["RO2一段进水排气阀1自动打开","DR.V_2ROYDJSP1_OPEN"]
["RO2一段进水排气阀1关闭","DR.V_2ROYDJSP1_OUTC"]
["RO2一段进水排气阀1打开","DR.V_2ROYDJSP1_OUTO"]
["RO2一段进水排气阀1准备好","DR.V_2ROYDJSP1_READY"]
["RO2一段进水排气阀1远程","DR.V_2ROYDJSP1_REM"]
["RO2一段进水排气阀2手自动","DR.V_2ROYDJSP2_BT_AUTO"]
["RO2一段进水排气阀2手动关","DR.V_2ROYDJSP2_BT_CLOSE"]
["RO2一段进水排气阀2手动开","DR.V_2ROYDJSP2_BT_OPEN"]
["RO2一段进水排气阀2故障复位","DR.V_2ROYDJSP2_BT_RESET"]
["RO2一段进水排气阀2关到位","DR.V_2ROYDJSP2_CFB"]
["RO2一段进水排气阀2关闭中","DR.V_2ROYDJSP2_CING"]
["RO2一段进水排气阀2自动关闭","DR.V_2ROYDJSP2_CLOS"]
["RO2一段进水排气阀2故障","DR.V_2ROYDJSP2_ERR"]
["RO2一段进水排气阀2总故障","DR.V_2ROYDJSP2_ERRT"]
["RO2一段进水排气阀2开到位","DR.V_2ROYDJSP2_OFB"]
["RO2一段进水排气阀2打开中","DR.V_2ROYDJSP2_OING"]
["RO2一段进水排气阀2自动打开","DR.V_2ROYDJSP2_OPEN"]
["RO2一段进水排气阀2关闭","DR.V_2ROYDJSP2_OUTC"]
["RO2一段进水排气阀2打开","DR.V_2ROYDJSP2_OUTO"]
["RO2一段进水排气阀2准备好","DR.V_2ROYDJSP2_READY"]
["RO2一段进水排气阀2远程","DR.V_2ROYDJSP2_REM"]
["RO2一段浓水排气阀1手自动","DR.V_2ROYDNSP1_BT_AUTO"]
["RO2一段浓水排气阀1手动关","DR.V_2ROYDNSP1_BT_CLOSE"]
["RO2一段浓水排气阀1手动开","DR.V_2ROYDNSP1_BT_OPEN"]
["RO2一段浓水排气阀1故障复位","DR.V_2ROYDNSP1_BT_RESET"]
["RO2一段浓水排气阀1关到位","DR.V_2ROYDNSP1_CFB"]
["RO2一段浓水排气阀1关闭中","DR.V_2ROYDNSP1_CING"]
["RO2一段浓水排气阀1自动关闭","DR.V_2ROYDNSP1_CLOSEA"]
["RO2一段浓水排气阀1故障","DR.V_2ROYDNSP1_ERR"]
["RO2一段浓水排气阀1总故障","DR.V_2ROYDNSP1_ERRT"]
["RO2一段浓水排气阀1开到位","DR.V_2ROYDNSP1_OFB"]
["RO2一段浓水排气阀1打开中","DR.V_2ROYDNSP1_OING"]
["RO2一段浓水排气阀1自动打开","DR.V_2ROYDNSP1_OPENA"]
["RO2一段浓水排气阀1关闭","DR.V_2ROYDNSP1_OUTC"]
["RO2一段浓水排气阀1打开","DR.V_2ROYDNSP1_OUTO"]
["RO2一段浓水排气阀1准备好","DR.V_2ROYDNSP1_READY"]
["RO2一段浓水排气阀1远程","DR.V_2ROYDNSP1_REM"]
["RO2一段浓水排气阀2手自动","DR.V_2ROYDNSP2_BT_AUTO"]
["RO2一段浓水排气阀2手动关","DR.V_2ROYDNSP2_BT_CLOSE"]
["RO2一段浓水排气阀2手动开","DR.V_2ROYDNSP2_BT_OPEN"]
["RO2一段浓水排气阀2故障复位","DR.V_2ROYDNSP2_BT_RESET"]
["RO2一段浓水排气阀2关到位","DR.V_2ROYDNSP2_CFB"]
["RO2一段浓水排气阀2关闭中","DR.V_2ROYDNSP2_CING"]
["RO2一段浓水排气阀2自动关闭","DR.V_2ROYDNSP2_CLOSEA"]
["RO2一段浓水排气阀2故障","DR.V_2ROYDNSP2_ERR"]
["RO2一段浓水排气阀2总故障","DR.V_2ROYDNSP2_ERRT"]
["RO2一段浓水排气阀2开到位","DR.V_2ROYDNSP2_OFB"]
["RO2一段浓水排气阀2打开中","DR.V_2ROYDNSP2_OING"]
["RO2一段浓水排气阀2自动打开","DR.V_2ROYDNSP2_OPEN"]
["RO2一段浓水排气阀2关闭","DR.V_2ROYDNSP2_OUTC"]
["RO2一段浓水排气阀2打开","DR.V_2ROYDNSP2_OUTO"]
["RO2一段浓水排气阀2准备好","DR.V_2ROYDNSP2_READY"]
["RO2一段浓水排气阀2远程","DR.V_2ROYDNSP2_REM"]
["RO2一段隔离阀手自动","DR.V_2ROYDQXGL_BT_AUTO"]
["RO2一段隔离阀手动关","DR.V_2ROYDQXGL_BT_CLOSE"]
["RO2一段隔离阀手动开","DR.V_2ROYDQXGL_BT_OPEN"]
["RO2一段隔离阀故障复位","DR.V_2ROYDQXGL_BT_RESET"]
["RO2一段隔离阀关到位","DR.V_2ROYDQXGL_CFB"]
["RO2一段隔离阀关闭中","DR.V_2ROYDQXGL_CING"]
["RO2一段隔离阀自动关闭","DR.V_2ROYDQXGL_CLOSEA"]
["RO2一段隔离阀故障","DR.V_2ROYDQXGL_ERR"]
["RO2一段隔离阀总故障","DR.V_2ROYDQXGL_ERRT"]
["RO2一段隔离阀开到位","DR.V_2ROYDQXGL_OFB"]
["RO2一段隔离阀打开中","DR.V_2ROYDQXGL_OING"]
["RO2一段隔离阀自动打开","DR.V_2ROYDQXGL_OPENA"]
["RO2一段隔离阀关闭","DR.V_2ROYDQXGL_OUT_C"]
["RO2一段隔离阀打开","DR.V_2ROYDQXGL_OUT_O"]
["RO2一段隔离阀准备好","DR.V_2ROYDQXGL_READY"]
["RO2一段隔离阀远程","DR.V_2ROYDQXGL_REM"]
["反洗废水外排阀手自动","DR.V_BW_WP_BT_AUTO"]
["反洗废水外排阀手动关","DR.V_BW_WP_BT_CLOSE"]
["反洗废水外排阀手动开","DR.V_BW_WP_BT_OPEN"]
["反洗废水外排阀故障复位","DR.V_BW_WP_BT_RESET"]
["反洗废水外排阀关到位","DR.V_BW_WP_CFB"]
["反洗废水外排阀关闭中","DR.V_BW_WP_CING"]
["反洗废水外排阀自动关闭","DR.V_BW_WP_CLOSEAUTO"]
["反洗废水外排阀故障","DR.V_BW_WP_ERR"]
["反洗废水外排阀总故障","DR.V_BW_WP_ERRT"]
["反洗废水外排阀开到位","DR.V_BW_WP_OFB"]
["反洗废水外排阀打开中","DR.V_BW_WP_OING"]
["反洗废水外排阀自动打开","DR.V_BW_WP_OPENAUTO"]
["反洗废水外排阀关闭","DR.V_BW_WP_OUT_CLOSE"]
["反洗废水外排阀打开","DR.V_BW_WP_OUT_OPEN"]
["反洗废水外排阀准备好","DR.V_BW_WP_READY"]
["反洗废水外排阀远程","DR.V_BW_WP_REM"]
["CEB次钠加药阀手自动","DR.V_CEB_CN_BT_AUTO"]
["CEB次钠加药阀手动关","DR.V_CEB_CN_BT_CLOSE"]
["CEB次钠加药阀手动开","DR.V_CEB_CN_BT_OPEN"]
["CEB次钠加药阀故障复位","DR.V_CEB_CN_BT_RESET"]
["CEB次钠加药阀关到位","DR.V_CEB_CN_CFB"]
["CEB次钠加药阀关闭中","DR.V_CEB_CN_CING"]
["CEB次钠加药阀自动关闭","DR.V_CEB_CN_CLOSEAUTO"]
["CEB次钠加药阀故障","DR.V_CEB_CN_ERR"]
["CEB次钠加药阀总故障","DR.V_CEB_CN_ERRT"]
["CEB次钠加药阀开到位","DR.V_CEB_CN_OFB"]
["CEB次钠加药阀打开中","DR.V_CEB_CN_OING"]
["CEB次钠加药阀自动打开","DR.V_CEB_CN_OPENAUTO"]
["CEB次钠加药阀关闭","DR.V_CEB_CN_OUT_CLOSE"]
["CEB次钠加药阀打开","DR.V_CEB_CN_OUT_OPEN"]
["CEB次钠加药阀准备好","DR.V_CEB_CN_READY"]
["CEB次钠加药阀远程","DR.V_CEB_CN_REM"]
["CEB碱加药阀手自动","DR.V_CEB_J_BT_AUTO"]
["CEB碱加药阀手动关","DR.V_CEB_J_BT_CLOSE"]
["CEB碱加药阀手动开","DR.V_CEB_J_BT_OPEN"]
["CEB碱加药阀故障复位","DR.V_CEB_J_BT_RESET"]
["CEB碱加药阀关到位","DR.V_CEB_J_CFB"]
["CEB碱加药阀关闭中","DR.V_CEB_J_CING"]
["CEB碱加药阀自动关闭","DR.V_CEB_J_CLOSEAUTO"]
["CEB碱加药阀故障","DR.V_CEB_J_ERR"]
["CEB碱加药阀总故障","DR.V_CEB_J_ERRT"]
["CEB碱加药阀开到位","DR.V_CEB_J_OFB"]
["CEB碱加药阀打开中","DR.V_CEB_J_OING"]
["CEB碱加药阀自动打开","DR.V_CEB_J_OPENAUTO"]
["CEB碱加药阀关闭","DR.V_CEB_J_OUT_CLOSE"]
["CEB碱加药阀打开","DR.V_CEB_J_OUT_OPEN"]
["CEB碱加药阀准备好","DR.V_CEB_J_READY"]
["CEB碱加药阀远程","DR.V_CEB_J_REM"]
["CEB酸加药阀手自动","DR.V_CEB_S_BT_AUTO"]
["CEB酸加药阀手动关","DR.V_CEB_S_BT_CLOSE"]
["CEB酸加药阀手动开","DR.V_CEB_S_BT_OPEN"]
["CEB酸加药阀故障复位","DR.V_CEB_S_BT_RESET"]
["CEB酸加药阀关到位","DR.V_CEB_S_CFB"]
["CEB酸加药阀关闭中","DR.V_CEB_S_CING"]
["CEB酸加药阀自动关闭","DR.V_CEB_S_CLOSEAUTO"]
["CEB酸加药阀故障","DR.V_CEB_S_ERR"]
["CEB酸加药阀总故障","DR.V_CEB_S_ERRT"]
["CEB酸加药阀开到位","DR.V_CEB_S_OFB"]
["CEB酸加药阀打开中","DR.V_CEB_S_OING"]
["CEB酸加药阀自动打开","DR.V_CEB_S_OPENAUTO"]
["CEB酸加药阀关闭","DR.V_CEB_S_OUT_CLOSE"]
["CEB酸加药阀打开","DR.V_CEB_S_OUT_OPEN"]
["CEB酸加药阀准备好","DR.V_CEB_S_READY"]
["CEB酸加药阀远程","DR.V_CEB_S_REM"]
["CEB排放阀手自动","DR.V_CEB_WP_BT_AUTO"]
["CEB排放阀手动关","DR.V_CEB_WP_BT_CLOSE"]
["CEB排放阀手动开","DR.V_CEB_WP_BT_OPEN"]
["CEB排放阀故障复位","DR.V_CEB_WP_BT_RESET"]
["CEB排放阀关到位","DR.V_CEB_WP_CFB"]
["CEB排放阀关闭中","DR.V_CEB_WP_CING"]
["CEB排放阀自动关闭","DR.V_CEB_WP_CLOSEAUTO"]
["CEB排放阀故障","DR.V_CEB_WP_ERR"]
["CEB排放阀总故障","DR.V_CEB_WP_ERRT"]
["CEB排放阀开到位","DR.V_CEB_WP_OFB"]
["CEB排放阀打开中","DR.V_CEB_WP_OING"]
["CEB排放阀自动打开","DR.V_CEB_WP_OPENAUTO"]
["CEB排放阀关闭","DR.V_CEB_WP_OUT_CLOSE"]
["CEB排放阀打开","DR.V_CEB_WP_OUT_OPEN"]
["CEB排放阀准备好","DR.V_CEB_WP_READY"]
["CEB排放阀远程","DR.V_CEB_WP_REM"]
["回用水碱加药阀手自动","DR.V_HYS_JJ_BT_AUTO"]
["回用水碱加药阀手动关","DR.V_HYS_JJ_BT_CLOSE"]
["回用水碱加药阀手动开","DR.V_HYS_JJ_BT_OPEN"]
["回用水碱加药阀故障复位","DR.V_HYS_JJ_BT_RESET"]
["回用水碱加药阀关到位","DR.V_HYS_JJ_CFB"]
["回用水碱加药阀关闭中","DR.V_HYS_JJ_CING"]
["回用水碱加药阀自动关闭","DR.V_HYS_JJ_CLOSEAUTO"]
["回用水碱加药阀故障","DR.V_HYS_JJ_ERR"]
["回用水碱加药阀总故障","DR.V_HYS_JJ_ERRT"]
["回用水碱加药阀开到位","DR.V_HYS_JJ_OFB"]
["回用水碱加药阀打开中","DR.V_HYS_JJ_OING"]
["回用水碱加药阀自动打开","DR.V_HYS_JJ_OPENAUTO"]
["回用水碱加药阀关闭","DR.V_HYS_JJ_OUT_CLOSE"]
["回用水碱加药阀打开","DR.V_HYS_JJ_OUT_OPEN"]
["回用水碱加药阀准备好","DR.V_HYS_JJ_READY"]
["回用水碱加药阀远程","DR.V_HYS_JJ_REM"]
["絮凝剂加药阀手自动","DR.V_PAC_BT_AUTO"]
["絮凝剂加药阀手动关","DR.V_PAC_BT_CLOSE"]
["絮凝剂加药阀手动开","DR.V_PAC_BT_OPEN"]
["絮凝剂加药阀故障复位","DR.V_PAC_BT_RESET"]
["絮凝剂加药阀关到位","DR.V_PAC_CFB"]
["絮凝剂加药阀关闭中","DR.V_PAC_CING"]
["絮凝剂加药阀自动关闭","DR.V_PAC_CLOSEAUTO"]
["絮凝剂加药阀故障","DR.V_PAC_ERR"]
["絮凝剂加药阀总故障","DR.V_PAC_ERRT"]
["絮凝剂加药阀开到位","DR.V_PAC_OFB"]
["絮凝剂加药阀打开中","DR.V_PAC_OING"]
["絮凝剂加药阀自动打开","DR.V_PAC_OPENAUTO"]
["絮凝剂加药阀关闭","DR.V_PAC_OUT_CLOSE"]
["絮凝剂加药阀打开","DR.V_PAC_OUT_OPEN"]
["絮凝剂加药阀准备好","DR.V_PAC_OUT_READY"]
["絮凝剂加药阀远程","DR.V_PAC_REM"]
["RO还原剂加药阀手自动","DR.V_RO_HYJ_BT_AUTO"]
["RO还原剂加药阀手动关","DR.V_RO_HYJ_BT_CLOSE"]
["RO还原剂加药阀手动开","DR.V_RO_HYJ_BT_OPEN"]
["RO还原剂加药阀故障复位","DR.V_RO_HYJ_BT_RESET"]
["RO还原剂加药阀关到位","DR.V_RO_HYJ_CFB"]
["RO还原剂加药阀关闭中","DR.V_RO_HYJ_CING"]
["RO还原剂加药阀自动关闭","DR.V_RO_HYJ_CLOSEAUTO"]
["RO还原剂加药阀故障","DR.V_RO_HYJ_ERR"]
["RO还原剂加药阀总故障","DR.V_RO_HYJ_ERRT"]
["RO还原剂加药阀开到位","DR.V_RO_HYJ_OFB"]
["RO还原剂加药阀打开中","DR.V_RO_HYJ_OING"]
["RO还原剂加药阀自动打开","DR.V_RO_HYJ_OPENAUTO"]
["RO还原剂加药阀关闭","DR.V_RO_HYJ_OUT_CLOSE"]
["RO还原剂加药阀打开","DR.V_RO_HYJ_OUT_OPEN"]
["RO还原剂加药阀准备好","DR.V_RO_HYJ_OUT_READY"]
["RO还原剂加药阀远程","DR.V_RO_HYJ_REM"]
["RO维护碱加药阀手自动","DR.V_RO_J_BT_AUTO"]
["RO维护碱加药阀手动关","DR.V_RO_J_BT_CLOSE"]
["RO维护碱加药阀手动开","DR.V_RO_J_BT_OPEN"]
["RO维护碱加药阀故障复位","DR.V_RO_J_BT_RESET"]
["RO维护碱加药阀关到位","DR.V_RO_J_CFB"]
["RO维护碱加药阀关闭中","DR.V_RO_J_CING"]
["RO维护碱加药阀自动关闭","DR.V_RO_J_CLOSEA"]
["RO维护碱加药阀故障","DR.V_RO_J_ERR"]
["RO维护碱加药阀总故障","DR.V_RO_J_ERRT"]
["RO维护碱加药阀开到位","DR.V_RO_J_OFB"]
["RO维护碱加药阀打开中","DR.V_RO_J_OING"]
["RO维护碱加药阀自动打开","DR.V_RO_J_OPENA"]
["RO维护碱加药阀关闭","DR.V_RO_J_OUTCLOSE"]
["RO维护碱加药阀打开","DR.V_RO_J_OUTOPEN"]
["RO维护碱加药阀准备好","DR.V_RO_J_READY"]
["RO维护碱加药阀远程","DR.V_RO_J_REM"]
["RO气洗阀手自动","DR.V_RO_QX_BT_AUTO"]
["RO气洗阀手动关","DR.V_RO_QX_BT_CLOSE"]
["RO气洗阀手动开","DR.V_RO_QX_BT_OPEN"]
["RO气洗阀故障复位","DR.V_RO_QX_BT_RESET"]
["RO气洗阀关到位","DR.V_RO_QX_CFB"]
["RO气洗阀关闭中","DR.V_RO_QX_CING"]
["RO气洗阀自动关闭","DR.V_RO_QX_CLOSEAUTO"]
["RO气洗阀故障","DR.V_RO_QX_ERR"]
["RO气洗阀总故障","DR.V_RO_QX_ERRT"]
["RO气洗阀开到位","DR.V_RO_QX_OFB"]
["RO气洗阀打开中","DR.V_RO_QX_OING"]
["RO气洗阀自动打开","DR.V_RO_QX_OPENAUTO"]
["RO气洗阀关闭","DR.V_RO_QX_OUT_CLOSE"]
["RO气洗阀打开","DR.V_RO_QX_OUT_OPEN"]
["RO气洗阀准备好","DR.V_RO_QX_READY"]
["RO气洗阀远程","DR.V_RO_QX_REM"]
["RO维护酸加药阀手自动","DR.V_RO_S_BT_AUTO"]
["RO维护酸加药阀手动关","DR.V_RO_S_BT_CLOSE"]
["RO维护酸加药阀手动开","DR.V_RO_S_BT_OPEN"]
["RO维护酸加药阀故障复位","DR.V_RO_S_BT_RESET"]
["RO维护酸加药阀关到位","DR.V_RO_S_CFB"]
["RO维护酸加药阀关闭中","DR.V_RO_S_CING"]
["RO维护酸加药阀自动关闭","DR.V_RO_S_CLOSEA"]
["RO维护酸加药阀故障","DR.V_RO_S_ERR"]
["RO维护酸加药阀总故障","DR.V_RO_S_ERRT"]
["RO维护酸加药阀开到位","DR.V_RO_S_OFB"]
["RO维护酸加药阀打开中","DR.V_RO_S_OING"]
["RO维护酸加药阀自动打开","DR.V_RO_S_OPENA"]
["RO维护酸加药阀关闭","DR.V_RO_S_OUTCLOSE"]
["RO维护酸加药阀打开","DR.V_RO_S_OUTOPEN"]
["RO维护酸加药阀准备好","DR.V_RO_S_READY"]
["RO维护酸加药阀远程","DR.V_RO_S_REM"]
["杀菌剂加药阀手自动","DR.V_SJJ_BT_AUTO"]
["杀菌剂加药阀手动关","DR.V_SJJ_BT_CLOSE"]
["杀菌剂加药阀手动开","DR.V_SJJ_BT_OPEN"]
["杀菌剂加药阀故障复位","DR.V_SJJ_BT_RESET"]
["杀菌剂加药阀关到位","DR.V_SJJ_CFB"]
["杀菌剂加药阀关闭中","DR.V_SJJ_CING"]
["杀菌剂加药阀自动关闭","DR.V_SJJ_CLOSEAUTO"]
["杀菌剂加药阀故障","DR.V_SJJ_ERR"]
["杀菌剂加药阀总故障","DR.V_SJJ_ERRT"]
["杀菌剂加药阀开到位","DR.V_SJJ_OFB"]
["杀菌剂加药阀打开中","DR.V_SJJ_OING"]
["杀菌剂加药阀自动打开","DR.V_SJJ_OPENAUTO"]
["杀菌剂加药阀关闭","DR.V_SJJ_OUT_CLOSE"]
["杀菌剂加药阀打开","DR.V_SJJ_OUT_OPEN"]
["杀菌剂加药阀准备好","DR.V_SJJ_READY"]
["杀菌剂加药阀远程","DR.V_SJJ_REM"]
["UF1进水调节阀备用1","DR.V_UF1_TJV_AUTO_CLOSE"]
["UF1进水调节阀备用2","DR.V_UF1_TJV_AUTO_OPEN"]
["UF1进水调节阀手自动","DR.V_UF1_TJV_BT_AUTO"]
["UF1进水调节阀备用3","DR.V_UF1_TJV_BT_CLOSE"]
["UF1进水调节阀备用4","DR.V_UF1_TJV_BT_OPEN"]
["UF1进水调节阀备用5","DR.V_UF1_TJV_BT_RESET"]
["UF1进水调节阀关状态","DR.V_UF1_TJV_CFB"]
["UF1进水调节阀备用6","DR.V_UF1_TJV_CLOSE"]
["UF1进水调节阀备用7","DR.V_UF1_TJV_FAULT"]
["UF1进水调节阀开状态","DR.V_UF1_TJV_OFB"]
["UF1进水调节阀备用8","DR.V_UF1_TJV_OPEN"]
["UF1进水调节阀备用9","DR.V_UF1_TJV_READY"]
["UF1进水调节阀备用10","DR.V_UF1_TJV_REM"]
["UF2进水调节阀备用1","DR.V_UF2_TJV_AUTO_CLOSE"]
["UF2进水调节阀备用2","DR.V_UF2_TJV_AUTO_OPEN"]
["UF2进水调节阀手自动","DR.V_UF2_TJV_BT_AUTO"]
["UF2进水调节阀备用3","DR.V_UF2_TJV_BT_CLOSE"]
["UF2进水调节阀备用4","DR.V_UF2_TJV_BT_OPEN"]
["UF2进水调节阀备用5","DR.V_UF2_TJV_BT_RESET"]
["UF2进水调节阀关状态","DR.V_UF2_TJV_CFB"]
["UF2进水调节阀备用6","DR.V_UF2_TJV_CLOSE"]
["UF2进水调节阀备用7","DR.V_UF2_TJV_FAULT"]
["UF2进水调节阀开状态","DR.V_UF2_TJV_OFB"]
["UF2进水调节阀备用8","DR.V_UF2_TJV_OPEN"]
["UF2进水调节阀备用9","DR.V_UF2_TJV_READY"]
["UF2进水调节阀备用10","DR.V_UF2_TJV_REM"]
["阻垢剂加药阀A手自动","DR.V_ZGJ_A_BT_AUTO"]
["阻垢剂加药阀A手动关","DR.V_ZGJ_A_BT_CLOSE"]
["阻垢剂加药阀A手动开","DR.V_ZGJ_A_BT_OPEN"]
["阻垢剂加药阀A故障复位","DR.V_ZGJ_A_BT_RESET"]
["阻垢剂加药阀A关到位","DR.V_ZGJ_A_CFB"]
["阻垢剂加药阀A关闭中","DR.V_ZGJ_A_CING"]
["阻垢剂加药阀A自动关闭","DR.V_ZGJ_A_CLOSEAUTO"]
["阻垢剂加药阀A故障","DR.V_ZGJ_A_ERR"]
["阻垢剂加药阀A总故障","DR.V_ZGJ_A_ERRT"]
["阻垢剂加药阀A开到位","DR.V_ZGJ_A_OFB"]
["阻垢剂加药阀A打开中","DR.V_ZGJ_A_OING"]
["阻垢剂加药阀A自动打开","DR.V_ZGJ_A_OPENAUTO"]
["阻垢剂加药阀A关闭","DR.V_ZGJ_A_OUT_CLOSE"]
["阻垢剂加药阀A打开","DR.V_ZGJ_A_OUT_OPEN"]
["阻垢剂加药阀A准备好","DR.V_ZGJ_A_OUT_READY"]
["阻垢剂加药阀A远程","DR.V_ZGJ_A_REM"]
["阻垢剂加药阀B手自动","DR.V_ZGJ_B_BT_AUTO"]
["阻垢剂加药阀B手动关","DR.V_ZGJ_B_BT_CLOSE"]
["阻垢剂加药阀B手动开","DR.V_ZGJ_B_BT_OPEN"]
["阻垢剂加药阀B故障复位","DR.V_ZGJ_B_BT_RESET"]
["阻垢剂加药阀B关到位","DR.V_ZGJ_B_CFB"]
["阻垢剂加药阀B关闭中","DR.V_ZGJ_B_CING"]
["阻垢剂加药阀B自动关闭","DR.V_ZGJ_B_CLOSEAUTO"]
["阻垢剂加药阀B故障","DR.V_ZGJ_B_ERR"]
["阻垢剂加药阀B总故障","DR.V_ZGJ_B_ERRT"]
["阻垢剂加药阀B开到位","DR.V_ZGJ_B_OFB"]
["阻垢剂加药阀B打开中","DR.V_ZGJ_B_OING"]
["阻垢剂加药阀B自动打开","DR.V_ZGJ_B_OPENAUTO"]
["阻垢剂加药阀B关闭","DR.V_ZGJ_B_OUT_CLOSE"]
["阻垢剂加药阀B打开","DR.V_ZGJ_B_OUT_OPEN"]
["阻垢剂加药阀B准备好","DR.V_ZGJ_B_OUT_READY"]
["阻垢剂加药阀B远程","DR.V_ZGJ_B_REM"]
["中和还原剂加药阀手自动","DR.V_ZH_HYJ_BT_AUTO"]
["中和还原剂加药阀手动关","DR.V_ZH_HYJ_BT_CLOSE"]
["中和还原剂加药阀手动开","DR.V_ZH_HYJ_BT_OPEN"]
["中和还原剂加药阀故障复位","DR.V_ZH_HYJ_BT_RESET"]
["中和还原剂加药阀关到位","DR.V_ZH_HYJ_CFB"]
["中和还原剂加药阀关闭中","DR.V_ZH_HYJ_CING"]
["中和还原剂加药阀自动关闭","DR.V_ZH_HYJ_CLOSEAUTO"]
["中和还原剂加药阀故障","DR.V_ZH_HYJ_ERR"]
["中和还原剂加药阀总故障","DR.V_ZH_HYJ_ERRT"]
["中和还原剂加药阀开到位","DR.V_ZH_HYJ_OFB"]
["中和还原剂加药阀打开中","DR.V_ZH_HYJ_OING"]
["中和还原剂加药阀自动打开","DR.V_ZH_HYJ_OPENAUTO"]
["中和还原剂加药阀关闭","DR.V_ZH_HYJ_OUT_CLOSE"]
["中和还原剂加药阀打开","DR.V_ZH_HYJ_OUT_OPEN"]
["中和还原剂加药阀准备好","DR.V_ZH_HYJ_OUT_READY"]
["中和还原剂加药阀远程","DR.V_ZH_HYJ_REM"]
["中和碱加药阀手自动","DR.V_ZH_J_BT_AUTO"]
["中和碱加药阀手动关","DR.V_ZH_J_BT_CLOSE"]
["中和碱加药阀手动开","DR.V_ZH_J_BT_OPEN"]
["中和碱加药阀故障复位","DR.V_ZH_J_BT_RESET"]
["中和碱加药阀关到位","DR.V_ZH_J_CFB"]
["中和碱加药阀关闭中","DR.V_ZH_J_CING"]
["中和碱加药阀自动关闭","DR.V_ZH_J_CLOSEAUTO"]
["中和碱加药阀故障","DR.V_ZH_J_ERR"]
["中和碱加药阀总故障","DR.V_ZH_J_ERRT"]
["中和碱加药阀开到位","DR.V_ZH_J_OFB"]
["中和碱加药阀打开中","DR.V_ZH_J_OING"]
["中和碱加药阀自动打开","DR.V_ZH_J_OPENAUTO"]
["中和碱加药阀关闭","DR.V_ZH_J_OUT_CLOSE"]
["中和碱加药阀打开","DR.V_ZH_J_OUT_OPEN"]
["中和碱加药阀准备好","DR.V_ZH_J_OUT_READY"]
["中和碱加药阀远程","DR.V_ZH_J_REM"]
["中和酸加药阀手自动","DR.V_ZH_S_BT_AUTO"]
["中和酸加药阀手动关","DR.V_ZH_S_BT_CLOSE"]
["中和酸加药阀手动开","DR.V_ZH_S_BT_OPEN"]
["中和酸加药阀故障复位","DR.V_ZH_S_BT_RESET"]
["中和酸加药阀关到位","DR.V_ZH_S_CFB"]
["中和酸加药阀关闭中","DR.V_ZH_S_CING"]
["中和酸加药阀自动关闭","DR.V_ZH_S_CLOSEAUTO"]
["中和酸加药阀故障","DR.V_ZH_S_ERR"]
["中和酸加药阀总故障","DR.V_ZH_S_ERRT"]
["中和酸加药阀开到位","DR.V_ZH_S_OFB"]
["中和酸加药阀打开中","DR.V_ZH_S_OING"]
["中和酸加药阀自动打开","DR.V_ZH_S_OPENAUTO"]
["中和酸加药阀关闭","DR.V_ZH_S_OUT_CLOSE"]
["中和酸加药阀打开","DR.V_ZH_S_OUT_OPEN"]
["中和酸加药阀准备好","DR.V_ZH_S_OUT_READY"]
["中和酸加药阀远程","DR.V_ZH_S_REM"]
["中和外排阀手自动","DR.V_ZH_WP_BT_AUTO"]
["中和外排阀手动关","DR.V_ZH_WP_BT_CLOSE"]
["中和外排阀手动开","DR.V_ZH_WP_BT_OPEN"]
["中和外排阀故障复位","DR.V_ZH_WP_BT_RESET"]
["中和外排阀关到位","DR.V_ZH_WP_CFB"]
["中和外排阀关闭中","DR.V_ZH_WP_CING"]
["中和外排阀自动关闭","DR.V_ZH_WP_CLOSEAUTO"]
["中和外排阀故障","DR.V_ZH_WP_ERR"]
["中和外排阀总故障","DR.V_ZH_WP_ERRT"]
["中和外排阀开到位","DR.V_ZH_WP_OFB"]
["中和外排阀打开中","DR.V_ZH_WP_OING"]
["中和外排阀自动打开","DR.V_ZH_WP_OPENAUTO"]
["中和外排阀关闭","DR.V_ZH_WP_OUT_CLOSE"]
["中和外排阀打开","DR.V_ZH_WP_OUT_OPEN"]
["中和外排阀准备好","DR.V_ZH_WP_OUT_READY"]
["中和外排阀远程","DR.V_ZH_WP_REM"]
["中和循环阀手自动","DR.V_ZHXH_BT_AUTO"]
["中和循环阀手动关","DR.V_ZHXH_BT_CLOSE"]
["中和循环阀手动开","DR.V_ZHXH_BT_OPEN"]
["中和循环阀故障复位","DR.V_ZHXH_BT_RESET"]
["中和循环阀关到位","DR.V_ZHXH_CFB"]
["中和循环阀关闭中","DR.V_ZHXH_CING"]
["中和循环阀自动关闭","DR.V_ZHXH_CLOSEAUTO"]
["中和循环阀故障","DR.V_ZHXH_ERR"]
["中和循环阀总故障","DR.V_ZHXH_ERRT"]
["中和循环阀开到位","DR.V_ZHXH_OFB"]
["中和循环阀打开中","DR.V_ZHXH_OING"]
["中和循环阀自动打开","DR.V_ZHXH_OPENAUTO"]
["中和循环阀关闭","DR.V_ZHXH_OUT_CLOSE"]
["中和循环阀打开","DR.V_ZHXH_OUT_OPEN"]
["中和循环阀准备好","DR.V_ZHXH_OUT_READY"]
["中和循环阀远程","DR.V_ZHXH_REM"]
["1#出水碱加药泵频率反馈","AR.1#CSJB_FRE_FB_O"]
["1#回用水泵电流反馈","AR.1#HYSB_CUR_FB_O"]
["1#回用水泵频率反馈","AR.1#HYSB_FRE_FB_O"]
["1#回用水泵后轴温度","AR.1#HYSB_HZ_TEMP_O"]
["1#回用水泵前轴温度","AR.1#HYSB_QZ_TEMP_O"]
["1#PAC加药泵频率反馈","AR.1#PAC_FRE_FB_O"]
["1#RO产水电导","AR.1#RO_CSDD_O"]
["1#RO产水压力","AR.1#RO_CSPRESS_O"]
["1#RO二段产水流量","AR.1#RO_EDCSFLOW_O"]
["1#RO二段进水压力","AR.1#RO_EDJSPRESS_O"]
["1#RO二段浓水压力","AR.1#RO_EDNSPRESS_O"]
["1#RO进水流量","AR.1#RO_JSFLOW_O"]
["1#RO进水压力","AR.1#RO_JSPRESS_O"]
["1#RO浓水流量","AR.1#RO_NSFLOW_O"]
["1#RO三段产水流量","AR.1#RO_SDCSFLOW_O"]
["1#RO三段进水压力","AR.1#RO_SDJSPRESS_O"]
["1#RO三段浓水压力","AR.1#RO_SDNSPRESS_O"]
["1#RO段间泵电流反馈","AR.1#RODJB_CUR_FB_O"]
["1#RO段间泵测振反馈","AR.1#RODJB_CZ_O"]
["1#RO段间泵频率反馈","AR.1#RODJB_FRE_FB_O"]
["1#RO段间泵后轴温度","AR.1#RODJB_HZ_TEMP_O"]
["1#RO段间泵前轴温度","AR.1#RODJB_QZ_TEMP_O"]
["1#RO高压泵电流反馈","AR.1#ROGYB_CUR_FB_O"]
["1#RO高压泵测振反馈","AR.1#ROGYB_CZ_O"]
["1#RO高压泵频率反馈","AR.1#ROGYB_FRE_FB_O"]
["1#RO高压泵后轴温度反馈","AR.1#ROGYB_HZ_TEMP_O"]
["1#RO高压泵前轴温度反馈","AR.1#ROGYB_QZ_TEMP_O"]
["1#RO还原剂加药泵频率反馈","AR.1#ROHYJ_FRE_FB_O"]
["1#杀菌剂加药泵频率反馈","AR.1#SJB_FRE_FB_O"]
["1#UF产水压力","AR.1#UF_CSPRESS_O"]
["1#UF进水流量","AR.1#UF_JSFLOW_O"]
["1#UF进水压力","AR.1#UF_JSPRESS_O"]
["1#UF调节阀开度反馈","AR.1#UF_V_FB_O"]
["1#UF反洗泵电流反馈","AR.1#UFBWB_CUR_FB_O"]
["1#UF反洗泵频率反馈","AR.1#UFBWB_FRE_FB_O"]
["1#UF反洗泵后轴温度反馈","AR.1#UFBWB_HZ_TEMP_O"]
["1#UF反洗泵前轴温度反馈","AR.1#UFBWB_QZ_TEMP_O"]
["1#阻垢剂流量","AR.1#ZGJ_FLOW_O"]
["1#阻垢剂加药泵频率反馈","AR.1#ZGJ_FRE_FB_O"]
["2#出水碱加药泵频率反馈","AR.2#CSJB_FRE_FB_O"]
["2#回用水泵电流反馈","AR.2#HYSB_CUR_FB_O"]
["2#回用水泵频率反馈","AR.2#HYSB_FRE_FB_O"]
["2#回用水泵后轴温度","AR.2#HYSB_HZ_TEMP_O"]
["2#回用水泵前轴温度","AR.2#HYSB_QZ_TEMP_O"]
["2#PAC加药泵频率反馈","AR.2#PAC_FRE_FB_O"]
["2#RO产水电导","AR.2#RO_CSDD_O"]
["2#RO产水压力","AR.2#RO_CSPRESS_O"]
["2#RO二段产水流量","AR.2#RO_EDCSFLOW_O"]
["2#RO二段进水压力","AR.2#RO_EDJSPRESS_O"]
["2#RO二段浓水压力","AR.2#RO_EDNSPRESS_O"]
["2#RO进水流量","AR.2#RO_JSFLOW_O"]
["2#RO进水压力","AR.2#RO_JSPRESS_O"]
["2#RO浓水流量","AR.2#RO_NSFLOW_O"]
["2#RO三段产水流量","AR.2#RO_SDCSFLOW_O"]
["2#RO三段进水压力","AR.2#RO_SDJSPRESS_O"]
["2#RO三段浓水压力","AR.2#RO_SDNSPRESS_O"]
["2#RO段间泵电流反馈","AR.2#RODJB_CUR_FB_O"]
["2#RO段间泵测振反馈","AR.2#RODJB_CZ_O"]
["2#RO段间泵频率反馈","AR.2#RODJB_FRE_FB_O"]
["2#RO段间泵后轴温度","AR.2#RODJB_HZ_TEMP_O"]
["2#RO段间泵前轴温度","AR.2#RODJB_QZ_TEMP_O"]
["2#RO高压泵电流反馈","AR.2#ROGYB_CUR_FB_O"]
["2#RO高压泵测振反馈","AR.2#ROGYB_CZ_O"]
["2#RO高压泵频率反馈","AR.2#ROGYB_FRE_FB_O"]
["2#RO高压泵后轴温度反馈","AR.2#ROGYB_HZ_TEMP_O"]
["2#RO高压泵前轴温度反馈","AR.2#ROGYB_QZ_TEMP_O"]
["2#RO还原剂加药泵频率反馈","AR.2#ROHYJ_FRE_FB_O"]
["2#杀菌剂加药泵频率反馈","AR.2#SJB_FRE_FB_O"]
["2#UF产水压力","AR.2#UF_CSPRESS_O"]
["2#UF进水流量","AR.2#UF_JSFLOW_O"]
["2#UF进水压力","AR.2#UF_JSPRESS_O"]
["2#UF调节阀开度反馈","AR.2#UF_V_FB_O"]
["2#UF反洗泵电流反馈","AR.2#UFBWB_CUR_FB_O"]
["2#UF反洗泵频率反馈","AR.2#UFBWB_FRE_FB_O"]
["2#UF反洗泵后轴温度反馈","AR.2#UFBWB_HZ_TEMP_O"]
["2#UF反洗泵前轴温度反馈","AR.2#UFBWB_QZ_TEMP_O"]
["2#阻垢剂流量","AR.2#ZGJ_FLOW_O"]
["2#阻垢剂加药泵频率反馈","AR.2#ZGJ_FRE_FB_O"]
["3#阻垢剂加药泵频率反馈","AR.3#ZGJ_FRE_FB_O"]
["空气压力","AR.AIR_PRESS_O"]
["次钠液位高高限值","AR.ALARM_CN_HHR"]
["次钠液位高限值","AR.ALARM_CN_HR"]
["次钠液位","AR.ALARM_CN_IN"]
["次钠液位低低限值","AR.ALARM_CN_LLR"]
["次钠液位低限值","AR.ALARM_CN_LR"]
["废水箱液位高高限值","AR.ALARM_FSX_HHR"]
["废水箱液位高限值","AR.ALARM_FSX_HR"]
["废水箱液位","AR.ALARM_FSX_IN"]
["废水箱液位低低限值","AR.ALARM_FSX_LLR"]
["废水箱液位低限值","AR.ALARM_FSX_LR"]
["还原剂液位高高限值","AR.ALARM_HYJ_HHR"]
["还原剂液位高限值","AR.ALARM_HYJ_HR"]
["还原剂液位","AR.ALARM_HYJ_IN"]
["还原剂液位低低限值","AR.ALARM_HYJ_LLR"]
["还原剂液位低限值","AR.ALARM_HYJ_LR"]
["碱液位高高限值","AR.ALARM_J_HHR"]
["碱液位高限值","AR.ALARM_J_HR"]
["碱液位","AR.ALARM_J_IN"]
["碱液位低低限值","AR.ALARM_J_LLR"]
["碱液位低限值","AR.ALARM_J_LR"]
["进水箱1液位高高限值","AR.ALARM_JSX1_HHR"]
["进水箱1液位高限值","AR.ALARM_JSX1_HR"]
["进水箱1液位","AR.ALARM_JSX1_IN"]
["进水箱1液位低低限值","AR.ALARM_JSX1_LLR"]
["进水箱1液位低限值","AR.ALARM_JSX1_LR"]
["进水箱2液位高高限值","AR.ALARM_JSX2_HHR"]
["进水箱2液位高限值","AR.ALARM_JSX2_HR"]
["进水箱2液位","AR.ALARM_JSX2_IN"]
["进水箱2液位低低限值","AR.ALARM_JSX2_LLR"]
["进水箱2液位低限值","AR.ALARM_JSX2_LR"]
["絮凝剂液位高高限值","AR.ALARM_PAC_HHR"]
["絮凝剂液位高限值","AR.ALARM_PAC_HR"]
["絮凝剂液位","AR.ALARM_PAC_IN"]
["絮凝剂液位低低限值","AR.ALARM_PAC_LLR"]
["絮凝剂液位低限值","AR.ALARM_PAC_LR"]
["CIP水箱液位高高限值","AR.ALARM_QXSX_HHR"]
["CIP水箱液位高限值","AR.ALARM_QXSX_HR"]
["CIP水箱液位","AR.ALARM_QXSX_IN"]
["CIP水箱液位低低限值","AR.ALARM_QXSX_LLR"]
["CIP水箱液位低限值","AR.ALARM_QXSX_LR"]
["RO产水箱液位高高限值","AR.ALARM_RO_CSX_HHR"]
["RO产水箱液位高限值","AR.ALARM_RO_CSX_HR"]
["RO产水箱液位","AR.ALARM_RO_CSX_IN"]
["RO产水箱液位低低限值","AR.ALARM_RO_CSX_LLR"]
["RO产水箱液位低限值","AR.ALARM_RO_CSX_LR"]
["酸液位高高限值","AR.ALARM_S_HHR"]
["酸液位高限值","AR.ALARM_S_HR"]
["酸液位","AR.ALARM_S_IN"]
["酸液位低低限值","AR.ALARM_S_LLR"]
["酸液位低限值","AR.ALARM_S_LR"]
["杀菌剂液位高高限值","AR.ALARM_SJJ_HHR"]
["杀菌剂液位高限值","AR.ALARM_SJJ_HR"]
["杀菌剂液位","AR.ALARM_SJJ_IN"]
["杀菌剂液位低低限值","AR.ALARM_SJJ_LLR"]
["杀菌剂液位低限值","AR.ALARM_SJJ_LR"]
["UF产水箱液位高高限值","AR.ALARM_UF_CSX_HHR"]
["UF产水箱液位高限值","AR.ALARM_UF_CSX_HR"]
["UF产水箱液位","AR.ALARM_UF_CSX_IN"]
["UF产水箱液位低低限值","AR.ALARM_UF_CSX_LLR"]
["UF产水箱液位低限值","AR.ALARM_UF_CSX_LR"]
["阻垢剂液位高高限值","AR.ALARM_ZGJ_HHR"]
["阻垢剂液位高限值","AR.ALARM_ZGJ_HR"]
["阻垢剂液位","AR.ALARM_ZGJ_IN"]
["阻垢剂液位低低限值","AR.ALARM_ZGJ_LLR"]
["阻垢剂液位低限值","AR.ALARM_ZGJ_LR"]
["中和水箱液位高高限值","AR.ALARM_ZHSX_HHR"]
["中和水箱液位高限值","AR.ALARM_ZHSX_HR"]
["中和水箱液位","AR.ALARM_ZHSX_IN"]
["中和水箱液位低低限值","AR.ALARM_ZHSX_LLR"]
["中和水箱液位低限值","AR.ALARM_ZHSX_LR"]
["反洗流量","AR.BW_FLOW_O"]
["反洗压力","AR.BW_PRESS_O"]
["次钠液位","AR.CN_LEVEL_O"]
["RO产水箱液位","AR.CS_LEVEL_O"]
["排队输出码","AR.FIFO_OUTCODE"]
["排队数量","AR.FIFO_QUE_NUMB"]
["排队1号码","AR.FIFO_QUE1"]
["排队10号码","AR.FIFO_QUE10"]
["排队11号码","AR.FIFO_QUE11"]
["排队2号码","AR.FIFO_QUE2"]
["排队3号码","AR.FIFO_QUE3"]
["排队4号码","AR.FIFO_QUE4"]
["排队5号码","AR.FIFO_QUE5"]
["排队6号码","AR.FIFO_QUE6"]
["排队7号码","AR.FIFO_QUE7"]
["排队8号码","AR.FIFO_QUE8"]
["排队9号码","AR.FIFO_QUE9"]
["排队等待码","AR.FIFO_WAITCODE"]
["废水箱液位","AR.FS_LEVEL_O"]
["废水泵后轴温度","AR.FSB_HZ_TEMP_O"]
["废水泵前轴温度","AR.FSB_QZ_TEMP_O"]
["还原剂液位","AR.HYJ_LEVEL_O"]
["回用水A流量","AR.HYS_A_FLOW_O"]
["回用水B流量","AR.HYS_B_FLOW_O"]
["回用水PH","AR.HYS_PH_O"]
["碱液位","AR.J_LEVEL_O"]
["还原剂搅拌器频率反馈","AR.JBQ_HYJ_FRE_FB"]
["还原剂搅拌器频率设定","AR.JBQ_HYJ_FRESET"]
["还原剂搅拌器运行时间","AR.JBQ_HYJ_RUNTIME"]
["PAC搅拌器频率反馈","AR.JBQ_PAC_FRE_FB"]
["PAC搅拌器频率设定","AR.JBQ_PAC_FRESET"]
["PAC搅拌器运行时间","AR.JBQ_PAC_RUNTIME"]
["酸搅拌器频率反馈","AR.JBQ_S_FRE_FB"]
["酸搅拌器频率设定","AR.JBQ_S_FRESET"]
["酸搅拌器运行时间","AR.JBQ_S_RUNTIME"]
["阻垢剂搅拌器频率反馈","AR.JBQ_ZGJ_FRE_FB"]
["阻垢剂搅拌器频率设定","AR.JBQ_ZGJ_FRESET"]
["阻垢剂搅拌器运行时间","AR.JBQ_ZGJ_RUNTIME"]
["进水箱1液位","AR.JSX1_LEVEL_O"]
["进水箱2液位","AR.JSX2_LEVEL_O"]
["1#次钠加药泵频率反馈","AR.P_1#CNB_FRE_FB"]
["1#次钠加药泵频率设定","AR.P_1#CNB_FRESET"]
["1#次钠加药泵运行时间","AR.P_1#CNB_RUNTIME"]
["1#出水碱加药泵频率反馈","AR.P_1#CSJB_FRE_FB"]
["1#出水碱加药泵频率设定","AR.P_1#CSJB_FRESET"]
["1#出水碱加药泵运行时间","AR.P_1#CSJB_RUNTIME"]
["1#回用水泵频率反馈","AR.P_1#HYSB_FRE_FB"]
["1#回用水泵频率设定","AR.P_1#HYSB_FRESET"]
["1#回用水泵运行时间","AR.P_1#HYSB_RUNTIME"]
["1#PAC加药泵频率反馈","AR.P_1#PACB_FRE_FB"]
["1#PAC加药泵频率设定","AR.P_1#PACB_FRESET"]
["1#PAC加药泵运行时间","AR.P_1#PACB_RUNTIME"]
["1#RO段间泵频率反馈","AR.P_1#RODJB_FRE_FB"]
["1#RO段间泵频率设定","AR.P_1#RODJB_FRESET"]
["1#RO段间泵运行时间","AR.P_1#RODJB_RUNTIME"]
["1#RO高压泵频率反馈","AR.P_1#ROGYB_FRE_FB"]
["1#RO高压泵频率设定","AR.P_1#ROGYB_FRESET"]
["1#RO高压泵运行时间","AR.P_1#ROGYB_RUNTIME"]
["1#RO还原剂加药泵频率反馈","AR.P_1#HYJB_FRE_FB"]
["1#RO还原剂加药泵频率设定","AR.P_1#HYJB_FRESET"]
["1#RO还原剂加药泵运行时间","AR.P_1#HYJB_RUNTIME"]
["1#酸加药泵频率反馈","AR.P_1#SB_FRE_FB"]
["1#酸加药泵频率设定","AR.P_1#SB_FRESET"]
["1#酸加药泵运行时间","AR.P_1#SB_RUNTIME"]
["1#杀菌剂加药泵频率反馈","AR.P_1#SJB_FRE_FB"]
["1#杀菌剂加药泵频率设定","AR.P_1#SJB_FRESET"]
["1#杀菌剂加药泵运行时间","AR.P_1#SJB_RUNTIME"]
["1#超滤碱加药泵频率反馈","AR.P_1#UF_JB_FRE_FB"]
["1#超滤碱加药泵频率设定","AR.P_1#UF_JB_FRESET"]
["1#超滤碱加药泵运行时间","AR.P_1#UF_JB_RUNTIME"]
["1#UF反洗泵频率反馈","AR.P_1#UFBWB_FRE_FB"]
["1#UF反洗泵频率设定","AR.P_1#UFBWB_FRESET"]
["1#UF反洗泵运行时间","AR.P_1#UFBWB_RUNTIME"]
["1#阻垢剂加药泵频率反馈","AR.P_1#ZGJB_FRE_FB"]
["1#阻垢剂加药泵频率设定","AR.P_1#ZGJB_FRESET"]
["1#阻垢剂加药泵运行时间","AR.P_1#ZGJB_RUNTIME"]
["1#中和还原剂加药泵频率反馈","AR.P_1#ZH_HYJ_FRE_FB"]
["1#中和还原剂加药泵频率设定","AR.P_1#ZH_HYJ_FRESET"]
["1#中和还原剂加药泵运行时间","AR.P_1#ZH_HYJ_RUNTIME"]
["2#次钠加药泵频率反馈","AR.P_2#CNB_FRE_FB"]
["2#次钠加药泵频率设定","AR.P_2#CNB_FRESET"]
["2#次钠加药泵运行时间","AR.P_2#CNB_RUNTIME"]
["2#出水碱加药泵频率反馈","AR.P_2#CSJB_FRE_FB"]
["2#出水碱加药泵频率设定","AR.P_2#CSJB_FRESET"]
["2#出水碱加药泵运行时间","AR.P_2#CSJB_RUNTIME"]
["2#回用水泵频率反馈","AR.P_2#HYSB_FRE_FB"]
["2#回用水泵频率设定","AR.P_2#HYSB_FRESET"]
["2#回用水泵运行时间","AR.P_2#HYSB_RUNTIME"]
["2#PAC加药泵频率反馈","AR.P_2#PACB_FRE_FB"]
["2#PAC加药泵频率设定","AR.P_2#PACB_FRESET"]
["2#PAC加药泵运行时间","AR.P_2#PACB_RUNTIME"]
["2#RO段间泵频率反馈","AR.P_2#RODJB_FRE_FB"]
["2#RO段间泵频率设定","AR.P_2#RODJB_FRESET"]
["2#RO段间泵运行时间","AR.P_2#RODJB_RUNTIME"]
["2#RO高压泵频率反馈","AR.P_2#ROGYB_FRE_FB"]
["2#RO高压泵频率设定","AR.P_2#ROGYB_FRESET"]
["2#RO高压泵运行时间","AR.P_2#ROGYB_RUNTIME"]
["2#RO还原剂加药泵频率反馈","AR.P_2#HYJB_FRE_FB"]
["2#RO还原剂加药泵频率设定","AR.P_2#HYJB_FRESET"]
["2#RO还原剂加药泵运行时间","AR.P_2#HYJB_RUNTIME"]
["2#酸加药泵频率反馈","AR.P_2#SB_FRE_FB"]
["2#酸加药泵频率设定","AR.P_2#SB_FRESET"]
["2#酸加药泵运行时间","AR.P_2#SB_RUNTIME"]
["2#杀菌剂加药泵频率反馈","AR.P_2#SJB_FRE_FB"]
["2#杀菌剂加药泵频率设定","AR.P_2#SJB_FRESET"]
["2#杀菌剂加药泵运行时间","AR.P_2#SJB_RUNTIME"]
["2#超滤碱加药泵频率反馈","AR.P_2#UF_JB_FRE_FB"]
["2#超滤碱加药泵频率设定","AR.P_2#UF_JB_FRESET"]
["2#超滤碱加药泵运行时间","AR.P_2#UF_JB_RUNTIME"]
["2#UF反洗泵频率反馈","AR.P_2#UFBWB_FRE_FB"]
["2#UF反洗泵频率设定","AR.P_2#UFBWB_FRESET"]
["2#UF反洗泵运行时间","AR.P_2#UFBWB_RUNTIME"]
["2#阻垢剂加药泵频率反馈","AR.P_2#ZGJB_FRE_FB"]
["2#阻垢剂加药泵频率设定","AR.P_2#ZGJB_FRESET"]
["2#阻垢剂加药泵运行时间","AR.P_2#ZGJB_RUNTIME"]
["2#中和还原剂加药泵频率反馈","AR.P_2#ZH_HYJ_FRE_FB"]
["2#中和还原剂加药泵频率设定","AR.P_2#ZH_HYJ_FRESET"]
["2#中和还原剂加药泵运行时间","AR.P_2#ZH_HYJ_RUNTIME"]
["3#阻垢剂加药泵频率反馈","AR.P_3#ZGJB_FRE_FB"]
["3#阻垢剂加药泵频率设定","AR.P_3#ZGJB_FRESET"]
["3#阻垢剂加药泵运行时间","AR.P_3#ZGJB_RUNTIME"]
["废水泵频率反馈","AR.P_FSB_FRE_FB"]
["废水泵频率设定","AR.P_FSB_FRESET"]
["废水泵运行时间","AR.P_FSB_RUNTIME"]
["加热器频率反馈","AR.P_JRQ_FRE_FB"]
["加热器频率设定","AR.P_JRQ_FRESET"]
["加热器运行时间","AR.P_JRQ_RUNTIME"]
["潜污泵频率反馈","AR.P_QWB_FRE_FB"]
["潜污泵频率设定","AR.P_QWB_FRESET"]
["潜污泵运行时间","AR.P_QWB_RUNTIME"]
["清洗水泵频率反馈","AR.P_QXSB_FRE_FB"]
["清洗水泵频率设定","AR.P_QXSB_FRESET"]
["清洗水泵运行时间","AR.P_QXSB_RUNTIME"]
["RO供水泵频率反馈","AR.P_ROGSB_FRE_FB"]
["RO供水泵频率设定","AR.P_ROGSB_FRESET"]
["RO供水泵运行时间","AR.P_ROGSB_RUNTIME"]
["UF供水泵频率反馈","AR.P_UFGSB_FRE_FB"]
["UF供水泵频率设定","AR.P_UFGSB_FRESET"]
["UF供水泵运行时间","AR.P_UFGSB_RUNTIME"]
["中和泵频率反馈","AR.P_ZH_FRE_FB"]
["中和泵频率设定","AR.P_ZH_FRESET"]
["中和泵运行时间","AR.P_ZH_RUNTIME"]
["絮凝剂液位","AR.PAC_LEVEL_O"]
["CIP水箱液位","AR.QXS_LEVEL_O"]
["CIP水PH","AR.QXS_PH_O"]
["CIP水温度","AR.QXS_TEMP_O"]
["清洗水泵电流","AR.QXSB_CUR_FB_O"]
["清洗水泵频率反馈","AR.QXSB_FRE_FB_O"]
["清洗水泵后轴温度反馈","AR.QXSB_HZ_TEMP_O"]
["清洗水泵前轴温度反馈","AR.QXSB_QZ_TEMP_O"]
["RO供水泵后轴温度反馈","AR.RO_GSB_HZ_TEMP_O"]
["RO供水泵前轴温度反馈","AR.RO_GSB_QZ_TEMP_0"]
["RO进水电导","AR.RO_JSDD_O"]
["RO进水ORP","AR.RO_JSORP_O"]
["RO进水PH","AR.RO_JSPH_O"]
["RO外供水电导","AR.RO_WSDD_O"]
["RO1一段压差","AR.RO1_1D_YC"]
["RO1一段压差设定","AR.RO1_1D_YC_SET"]
["RO1一段产水流量","AR.RO1_1DUAN_CS_FLOW"]
["RO1一段已碱维护天数","AR.RO1_1DYJWH_DAYS"]
["RO1一段已杀菌天数","AR.RO1_1DYSJ_DAYS"]
["RO1一段已酸维护天数","AR.RO1_1DYSWH_DAYS"]
["RO1二三段已碱维护天数","AR.RO1_23DYJWH_DAYS"]
["RO1二三段已杀菌天数","AR.RO1_23DYSJ_DAYS"]
["RO1二三段已酸维护天数","AR.RO1_23DYSWH_DAYS"]
["RO1二段压差","AR.RO1_2D_YC"]
["RO1二段压差设定","AR.RO1_2D_YC_SET"]
["RO1CODE_一段碱维护","AR.RO1_CODE_1DJWH"]
["RO1CODE_一段杀菌","AR.RO1_CODE_1DSJ"]
["RO1CODE_一段酸维护","AR.RO1_CODE_1DSWH"]
["RO1CODE_二三段碱维护","AR.RO1_CODE_23DJWH"]
["RO1CODE_二三段杀菌","AR.RO1_CODE_23DSJ"]
["RO1CODE_二三段酸维护","AR.RO1_CODE_23DSWH"]
["RO1CODE_冲洗","AR.RO1_CODE_CX"]
["RO1设定段间泵启动频率","AR.RO1_GSB_FR_OUT"]
["1#RO高压泵频率输出","AR.RO1_GYB_FR_OUT"]
["RO1系统定时","AR.RO1_HMI_SET_TIME"]
["RO1系统计时","AR.RO1_HMI_SYSTEM_TIME"]
["RO1需要冲洗流量","AR.RO1_NEED_CXLL"]
["RO1需要段间泵流量","AR.RO1_NEED_DJBLL"]
["RO1需要供水流量","AR.RO1_NEED_GSLL"]
["RO1需要高压泵流量","AR.RO1_NEED_GYBLL"]
["RO1产水率","AR.RO1_RATE_CS"]
["RO1SET_一段碱维护天数","AR.RO1_SET_1DJWH_DAYS"]
["RO1SET_一段碱维后气水混洗时间","AR.RO1_SET_1DJWHHX_TIME"]
["RO1SET_一段碱维后水洗时间","AR.RO1_SET_1DJWHSX_TIME"]
["RO1SET_一段碱维加碱时间","AR.RO1_SET_1DJWJJ_TIME"]
["RO1SET_一段碱维浸泡时间","AR.RO1_SET_1DJWJP_TIME"]
["RO1SET_一段杀菌天数","AR.RO1_SET_1DSJ_DAYS"]
["RO1Set一段杀菌时间","AR.RO1_SET_1DSJ_TIME"]
["RO1Set_一段杀菌浸泡时间","AR.RO1_SET_1DSJJP_TIME"]
["RO1Set一段杀菌结束反冲排气时间","AR.RO1_SET_1DSJJS_TIME"]
["RO1Set一段杀菌结束气水冲时间","AR.RO1_SET_1DSJJSQ_TIME"]
["RO1SET_一段酸维护天数","AR.RO1_SET_1DSWH_DAYS"]
["RO1SET_一段酸维后气水混洗时间","AR.RO1_SET_1DSWHHX_TIME"]
["RO1SET_一段酸维后水洗时间","AR.RO1_SET_1DSWHSX_TIME"]
["RO1SET_一段酸维浸泡时间","AR.RO1_SET_1DSWJP_TIME"]
["RO1SET_一段酸维加酸时间","AR.RO1_SET_1DSWJS_TIME"]
["RO1Set_二三段正冲时间","AR.RO1_SET_2/3DZC_TIME"]
["RO1SET_二三段碱维护天数","AR.RO1_SET_23DJWH_DAYS"]
["RO1SET_二三段碱维护时间","AR.RO1_SET_23DJWH_TIME"]
["RO1SET_二三段碱维护后冲洗时间","AR.RO1_SET_23DJWHHCX_T"]
["RO1SET_二三段碱维护浸泡时间","AR.RO1_SET_23DJWHJ_TIME"]
["RO1SET_二三段杀菌天数","AR.RO1_SET_23DSJ_DAYS"]
["RO1SET_二三段杀菌后冲洗时间","AR.RO1_SET_23DSJCX_TIME"]
["RO1SET_二三段杀菌浸泡时间","AR.RO1_SET_23DSJJP_TIME"]
["RO1SET_二三段杀菌维护时间","AR.RO1_SET_23DSJWH_TIME"]
["RO1SET_二三段酸维护天数","AR.RO1_SET_23DSWH_DAYS"]
["RO1SET_二三段酸维护时间","AR.RO1_SET_23DSWH_TIME"]
["RO1SET_二三段酸维护后冲洗时间","AR.RO1_SET_23SWHHC_TIME"]
["RO1SET_二三段酸维护浸泡时间","AR.RO1_SET_23SWHJP_TIME"]
["RO1SET_超越过滤冲水排气时间","AR.RO1_SET_CYSGLCSPQ_T"]
["RO1SET_超越停机冲洗时间","AR.RO1_SET_CYTJCX_T"]
["RO1SET_超越停机加药冲洗时间","AR.RO1_SET_CYTJJYCX_T"]
["RO1SET_电导率","AR.RO1_SET_DDL"]
["RO1段间泵流量设定","AR.RO1_SET_DJBLL"]
["RO1Set反冲时间","AR.RO1_SET_FC_TIME"]
["RO1Set过滤产水时间","AR.RO1_SET_GLCS_TIME"]
["RO1供水流量设定","AR.RO1_SET_GSL"]
["RO1SET_GSPump_频率_L","AR.RO1_SET_GSPUMP_FR_L"]
["RO1SET_GYPump_频率","AR.RO1_SET_GYPUMP_FR"]
["RO1SET_GYPump_频率_H","AR.RO1_SET_GYPUMP_FR_H"]
["RO1SET_GYPump_频率_L","AR.RO1_SET_GYPUMP_FR_L"]
["RO1SET_加药冲洗反冲洗时间","AR.RO1_SET_JYCXFC_T"]
["RO1SET_加药冲洗正冲洗时间","AR.RO1_SET_JYCXZC_TIME"]
["RO1Set开机冲洗时间","AR.RO1_SET_KJCX_TIME"]
["RO1SET_ORP","AR.RO1_SET_ORP"]
["RO1SET_气水混洗时间","AR.RO1_SET_QSHX_TIEM"]
["RO1Set_水反洗排气时间","AR.RO1_SET_SFXPQ_TIME"]
["RO1SET_杀菌后反冲时间","AR.RO1_SET_SJHFC_TIME"]
["RO1SET_杀菌后正冲时间","AR.RO1_SET_SJHZC_TIME"]
["RO1杀菌浸泡时间设定","AR.RO1_SET_SJJP_TIME"]
["RO1SET杀菌流量","AR.RO1_SET_SJLL"]
["RO1Set停机加药冲洗时间","AR.RO1_SET_TJJYCX_TIME"]
["RO1SET_预杀菌天数","AR.RO1_SET_YSJ_DAYS"]
["RO1Set正冲时间","AR.RO1_SET_ZC_TIME"]
["RO1SET正冲流量","AR.RO1_SET_ZCLL"]
["RO1步序","AR.RO1_STEP"]
["RO1总产水流量","AR.RO1_TOTAL_CSLL"]
["RO1总过滤次数","AR.RO1_TOTAL_GL_CS"]
["RO1总进水流量","AR.RO1_TOTAL_JSLL"]
["RO1总浓水流量","AR.RO1_TOTAL_NSLL"]
["RO2一段压差","AR.RO2_1D_YC"]
["RO2一段压差设定","AR.RO2_1D_YC_SET"]
["RO2一段产水流量","AR.RO2_1DUAN_CS_FLOW"]
["RO2一段已碱维护天数","AR.RO2_1DYJWH_DAYS"]
["RO2一段已杀菌天数","AR.RO2_1DYSJ_DAYS"]
["RO2一段已酸维护天数","AR.RO2_1DYSWH_DAYS"]
["RO2二三段已碱维护天数","AR.RO2_23DYJWH_DAYS"]
["RO2二三段已杀菌天数","AR.RO2_23DYSJ_DAYS"]
["RO2二三段已酸维护天数","AR.RO2_23DYSWH_DAYS"]
["RO2二段压差","AR.RO2_2D_YC"]
["RO2二段压差设定","AR.RO2_2D_YC_SET"]
["RO2CODE_一段碱维护","AR.RO2_CODE_1DJWH"]
["RO2CODE_一段杀菌","AR.RO2_CODE_1DSJ"]
["RO2CODE_一段酸维护","AR.RO2_CODE_1DSWH"]
["RO2CODE_二三段碱维护","AR.RO2_CODE_23DJWH"]
["RO2CODE_二三段杀菌","AR.RO2_CODE_23DSJ"]
["RO2CODE_二三段酸维护","AR.RO2_CODE_23DSWH"]
["RO2CODE_冲洗","AR.RO2_CODE_CX"]
["2#RO供水泵频率输出","AR.RO2_GSB_FR_OUT"]
["2#RO高压泵频率输出","AR.RO2_GYB_FR_OUT"]
["RO2系统定时","AR.RO2_HMI_SET_TIME"]
["RO2系统计时","AR.RO2_HMI_SYSTEM_TIME"]
["RO2需要冲洗流量","AR.RO2_NEED_CXLL"]
["RO2需要段间泵流量","AR.RO2_NEED_DJBLL"]
["RO2需要供水流量","AR.RO2_NEED_GSLL"]
["RO2需要高压泵流量","AR.RO2_NEED_GYBLL"]
["RO2产水率","AR.RO2_RATE_CS"]
["RO2SET_一段碱维护天数","AR.RO2_SET_1DJWH_DAYS"]
["RO2SET_一段碱维后气水混洗时间","AR.RO2_SET_1DJWHHX_TIME"]
["RO2SET_一段碱维后水洗时间","AR.RO2_SET_1DJWHSX_TIME"]
["RO2SET_一段碱维加碱时间","AR.RO2_SET_1DJWJJ_TIME"]
["RO2SET_一段碱维浸泡时间","AR.RO2_SET_1DJWJP_TIME"]
["RO2SET_一段杀菌天数","AR.RO2_SET_1DSJ_DAYS"]
["RO2Set一段杀菌时间","AR.RO2_SET_1DSJ_TIME"]
["RO2Set_一段杀菌浸泡时间","AR.RO2_SET_1DSJJP_TIME"]
["RO2Set一段杀菌结束反冲排气时间","AR.RO2_SET_1DSJJS_TIME"]
["RO2Set一段杀菌结束气水冲时间","AR.RO2_SET_1DSJJSQ_TIME"]
["RO2SET_一段酸维护天数","AR.RO2_SET_1DSWH_DAYS"]
["RO2SET_一段酸维后气水混洗时间","AR.RO2_SET_1DSWHHX_TIME"]
["RO2SET_一段酸维后水洗时间","AR.RO2_SET_1DSWHSX_TIME"]
["RO2SET_一段酸维浸泡时间","AR.RO2_SET_1DSWJP_TIME"]
["RO2SET_一段酸维加酸时间","AR.RO2_SET_1DSWJS_TIME"]
["RO2Set_二三段正冲时间","AR.RO2_SET_2/3DZC_TIME"]
["RO2SET_二三段碱维护天数","AR.RO2_SET_23DJWH_DAYS"]
["RO2SET_二三段碱维护时间","AR.RO2_SET_23DJWH_TIME"]
["RO2SET_二三段碱维护后冲洗时间","AR.RO2_SET_23DJWHHCX_T"]
["RO2SET_二三段碱维护浸泡时间","AR.RO2_SET_23DJWHJ_TIME"]
["RO2SET_二三段杀菌天数","AR.RO2_SET_23DSJ_DAYS"]
["RO2SET_二三段杀菌后冲洗时间","AR.RO2_SET_23DSJCX_TIME"]
["RO2SET_二三段杀菌浸泡时间","AR.RO2_SET_23DSJJP_TIME"]
["RO2SET_二三段杀菌维护时间","AR.RO2_SET_23DSJWH_TIME"]
["RO2SET_二三段酸维护天数","AR.RO2_SET_23DSWH_DAYS"]
["RO2SET_二三段酸维护时间","AR.RO2_SET_23DSWH_TIME"]
["RO2SET_二三段酸维护后冲洗时间","AR.RO2_SET_23SWHHC_TIME"]
["RO2SET_二三段酸维护浸泡时间","AR.RO2_SET_23SWHJP_TIME"]
["RO2SET_超越过滤冲水排气时间","AR.RO2_SET_CYSGLCSPQ_T"]
["RO2SET_超越停机冲洗时间","AR.RO2_SET_CYTJCX_T"]
["RO2SET_超越停机加药冲洗时间","AR.RO2_SET_CYTJJYCX_T"]
["RO2SET_电导率","AR.RO2_SET_DDL"]
["RO2段间泵流量设定","AR.RO2_SET_DJBLL"]
["RO2Set反冲时间","AR.RO2_SET_FC_TIME"]
["RO2Set过滤产水时间","AR.RO2_SET_GLCS_TIME"]
["RO2供水流量设定","AR.RO2_SET_GSL"]
["RO2SET_GSPump_频率_L","AR.RO2_SET_GSPUMP_FR_L"]
["RO2SET_GYPump_频率","AR.RO2_SET_GYPUMP_FR"]
["RO2SET_GYPump_频率_H","AR.RO2_SET_GYPUMP_FR_H"]
["RO2SET_GYPump_频率_L","AR.RO2_SET_GYPUMP_FR_L"]
["RO2SET_加药冲洗反冲洗时间","AR.RO2_SET_JYCXFC_T"]
["RO2SET_加药冲洗正冲洗时间","AR.RO2_SET_JYCXZC_TIME"]
["RO2Set开机冲洗时间","AR.RO2_SET_KJCX_TIME"]
["RO2SET_ORP","AR.RO2_SET_ORP"]
["RO2SET_气水混洗时间","AR.RO2_SET_QSHX_TIEM"]
["RO2Set_水反洗排气时间","AR.RO2_SET_SFXPQ_TIME"]
["RO2SET_杀菌后反冲时间","AR.RO2_SET_SJHFC_TIME"]
["RO2SET_杀菌后正冲时间","AR.RO2_SET_SJHZC_TIME"]
["RO2杀菌浸泡时间设定","AR.RO2_SET_SJJP_TIME"]
["RO2SET杀菌流量","AR.RO2_SET_SJLL"]
["RO2Set停机加药冲洗时间","AR.RO2_SET_TJJYCX_TIME"]
["RO2SET_预杀菌天数","AR.RO2_SET_YSJ_DAYS"]
["RO2Set正冲时间","AR.RO2_SET_ZC_TIME"]
["RO2SET正冲流量","AR.RO2_SET_ZCLL"]
["RO2步序","AR.RO2_STEP"]
["RO2总产水流量","AR.RO2_TOTAL_CSLL"]
["RO2总过滤次数","AR.RO2_TOTAL_GL_CS"]
["RO2总进水流量","AR.RO2_TOTAL_JSLL"]
["RO2总浓水流量","AR.RO2_TOTAL_NSLL"]
["RO供水泵电流","AR.ROGSB_CUR_FB_O"]
["RO供水泵频率反馈","AR.ROGSB_FRE_FB_O"]
["酸液位","AR.S_LEVEL_O"]
["杀菌剂液位","AR.SJJ_LEVEL_O"]
["UF产水浊度","AR.UF_CS_ZD_O"]
["UF产水箱液位","AR.UF_CSLEVEL_O"]
["UF1反洗次数显示","AR.UF1_OUT_BW_CS"]
["UF1反洗流量累计","AR.UF1_OUT_BW_FLOW_ADD"]
["UF1反洗总次数累计","AR.UF1_OUT_BW_ZCS"]
["UF1过滤流量累计","AR.UF1_OUT_GL_FLOW_ADD"]
["UF1系统设置时间","AR.UF1_OUT_SET_TIME"]
["UF1系统显示时间","AR.UF1_OUT_SYS_TIME"]
["UF1设置反洗次数","AR.UF1_SET_BW_CS"]
["UF1设置反洗流量","AR.UF1_SET_BW_FLOW"]
["UF1设置冲水排气流量","AR.UF1_SET_CS_FLOW"]
["UF1设置冲水排气时间","AR.UF1_SET_CSPQ_TIME"]
["UF1设置过滤流量","AR.UF1_SET_GL_FLOW"]
["UF1设置过滤时间","AR.UF1_SET_GL_TIME"]
["UF1设置加药流量","AR.UF1_SET_JY_FLOW"]
["UF1设置跨膜压差高高值","AR.UF1_SET_KMYC_HHR"]
["UF1设置跨膜压差高值","AR.UF1_SET_KMYC_HR"]
["UF1设置酸反洗时间","AR.UF1_SET_S_BW_TIME"]
["UF1设置CEB后冲时间","AR.UF1_SETCEB_HC_TIME"]
["UF1设置CEB浸泡时间","AR.UF1_SETCEB_JP_TIME"]
["UF1设置CEB加药时间","AR.UF1_SETCEB_JY_TIME"]
["UF1设置CEB前冲时间","AR.UF1_SETCEB_QC_TIME"]
["UF1跨膜压差","AR.UF1_SSD_KMYC"]
["UF1步序","AR.UF1_STEP"]
["UF2反洗次数显示","AR.UF2_OUT_BW_CS"]
["UF2反洗流量累计","AR.UF2_OUT_BW_FLOW_ADD"]
["UF2反洗总次数累计","AR.UF2_OUT_BW_ZCS"]
["UF2过滤流量累计","AR.UF2_OUT_GL_FLOW_ADD"]
["UF2系统设置时间","AR.UF2_OUT_SET_TIME"]
["UF2系统显示时间","AR.UF2_OUT_SYS_TIME"]
["UF2设置反洗次数","AR.UF2_SET_BW_CS"]
["UF2设置反洗流量","AR.UF2_SET_BW_FLOW"]
["UF2设置冲水排气流量","AR.UF2_SET_CS_FLOW"]
["UF2设置冲水排气时间","AR.UF2_SET_CSPQ_TIME"]
["UF2设置过滤流量","AR.UF2_SET_GL_FLOW"]
["UF2设置过滤时间","AR.UF2_SET_GL_TIME"]
["UF2设置加药流量","AR.UF2_SET_JY_FLOW"]
["UF2设置跨膜压差高高值","AR.UF2_SET_KMYC_HHR"]
["UF2设置跨膜压差高值","AR.UF2_SET_KMYC_HR"]
["UF2设置酸反洗时间","AR.UF2_SET_S_BW_TIME"]
["UF2设置CEB后冲时间","AR.UF2_SETCEB_HC_TIME"]
["UF2设置CEB浸泡时间","AR.UF2_SETCEB_JP_TIME"]
["UF2设置CEB加药时间","AR.UF2_SETCEB_JY_TIME"]
["UF2设置CEB前冲时间","AR.UF2_SETCEB_QC_TIME"]
["UF2跨膜压差","AR.UF2_SSD_KMYC"]
["UF2步序","AR.UF2_STEP"]
["UF供水泵电流","AR.UFGSB_CUR_FB_O"]
["UF供水泵频率反馈","AR.UFGSB_FRE_FB_O"]
["UF供水泵后轴温度反馈","AR.UFGSB_HZ_TEMP_O"]
["UF供水泵前轴温度反馈","AR.UFGSB_QZ_TEMP_O"]
["UF1调节阀开度反馈","AR.V_UF1_TJV_KD_FB"]
["UF1调节阀开度设定","AR.V_UF1_TJV_KD_SET"]
["UF2调节阀开度反馈","AR.V_UF2_TJV_KD_FB"]
["UF2调节阀开度设定","AR.V_UF2_TJV_KD_SET"]
["阻垢剂液位","AR.ZGJ_LEVEL_O"]
["中和水箱液位","AR.ZH_LEVEL_O"]
["中和水箱ORP","AR.ZH_ORP_O"]
["中和水箱PH","AR.ZH_PH_O"]
["中和泵后轴温度","AR.ZHB_HZ_TEMP_O"]
["中和泵前轴温度","AR.ZHB_QZ_TEMP_O"]
["进水压力","AR.ZJS_PRESS_O"]
["进水温度","AR.ZJS_TEMP_O"]
["UF进水浊度","AR.ZJS_ZD_O"]
["2号阻垢剂泵给RO1用","DR.PUBLIC_BYZGJB4_1"]
["2号阻垢剂泵给RO2用","DR.PUBLIC_BYZGJB4_2"]
["UF其它设备CEB中","DR.PUBLIC_OTHER_CEBING"]
["UF其它设备反洗中","DR.PUBLIC_OTHER_BWING"]
["其它RO在过滤中","DR.PUBLIC_OTHERRO_GLING"]
["RO_回用水泵PID选择","DR.PUBLIC_RO_HYSB_PID"]
["RO其他设备杀菌中","DR.PUBLIC_RO_OTHER_SJ"]
["RO其他设备冲洗中","DR.PUBLIC_RO_OTHER_CX"]
["RO_系统自动","DR.PUBLIC_RO_SYS_AUOTO"]
["RO_系统手动","DR.PUBLIC_RO_SYS_MAN"]
["RO1_允许冲洗","DR.PUBLIC_RO1_ALLOW_CX"]
["RO1_允许过滤","DR.PUBLIC_RO1_ALLOW_GL"]
["RO1_允许杀菌","DR.PUBLIC_RO1_ALLOW_SJ"]
["RO1_段间泵PID选择","DR.PUBLIC_RO1_DJB_PID"]
["RO1_高压泵PID选择","DR.PUBLIC_RO1_GYB_PID"]
["RO2_允许冲洗","DR.PUBLIC_RO2_ALLOW_CX"]
["RO2_允许过滤","DR.PUBLIC_RO2_ALLOW_GL"]
["RO2_允许杀菌","DR.PUBLIC_RO2_ALLOW_SJ"]
["RO2_段间泵PID选择","DR.PUBLIC_RO2_DJB_PID"]
["RO2_高压泵PID选择","DR.PUBLIC_RO2_GYB_PID"]
["UF_反洗泵PID模式选择","DR.PUBLIC_UF_FXB_PID"]
["UF系统自动","DR.PUBLIC_UF_SYS_AUTO"]
["UF系统手动","DR.PUBLIC_UF_SYS_MAN"]
["UF允许反洗","DR.PUBLIC_UF1_ALLOW_BW"]
["UF1允许CEB","DR.PUBLIC_UF1_ALLOW_CEB"]
["UF允许过滤","DR.PUBLIC_UF1_ALLOW_GL"]
["UF1_TJF_PID模式","DR.PUBLIC_UF1_TJF_PID"]
["UF2允许反洗","DR.PUBLIC_UF2_ALLOW_BW"]
["UF2允许CEB","DR.PUBLIC_UF2_ALLOW_CEB"]
["UF2允许过滤","DR.PUBLIC_UF2_ALLOW_GL"]
["UF2_TJF_PID模式","DR.PUBLIC_UF2_TJF_PID"]
["RO1系统报错","DR.PUBLIC_BY_B00L_1"]
["RO2系统报错","DR.PUBLIC_BY_BOOL_2"]
["离散变量备用3","DR.PUBLIC_BY_BOOL_3"]
["离散变量备用4","DR.PUBLIC_BY_BOOL_4"]
["离散变量备用5","DR.PUBLIC_BY_BOOL_5"]
["离散变量备用6","DR.PUBLIC_BY_BOOL_6"]
["离散变量备用7","DR.PUBLIC_BY_BOOL_7"]
["离散变量备用8","DR.PUBLIC_BY_BOOL_8"]
["离散变量备用9","DR.PUBLIC_BY_BOOL_9"]
["离散变量备用10","DR.PUBLIC_BY_BOOL_10"]
["离散变量备用11","DR.PUBLIC_BY_BOOL_11"]
["离散变量备用12","DR.PUBLIC_BY_BOOL_12"]
["离散变量备用13","DR.PUBLIC_BY_BOOL_13"]
["离散变量备用14","DR.PUBLIC_BY_BOOL_14"]
["离散变量备用15","DR.PUBLIC_BY_BOOL_15"]
["离散变量备用16","DR.PUBLIC_BY_BOOL_16"]
["离散变量备用17","DR.PUBLIC_BY_BOOL_17"]
["离散变量备用18","DR.PUBLIC_BY_BOOL_18"]
["离散变量备用19","DR.PUBLIC_BY_BOOL_19"]
["离散变量备用20","DR.PUBLIC_BY_BOOL_20"]
["离散变量备用21","DR.PUBLIC_BY_BOOL_21"]
["离散变量备用22","DR.PUBLIC_BY_BOOL_22"]
["离散变量备用23","DR.PUBLIC_BY_BOOL_23"]
["离散变量备用24","DR.PUBLIC_BY_BOOL_24"]
["离散变量备用25","DR.PUBLIC_BY_BOOL_25"]
["离散变量备用26","DR.PUBLIC_BY_BOOL_26"]
["离散变量备用27","DR.PUBLIC_BY_BOOL_27"]
["离散变量备用28","DR.PUBLIC_BY_BOOL_28"]
["离散变量备用29","DR.PUBLIC_BY_BOOL_29"]
["离散变量备用30","DR.PUBLIC_BY_BOOL_30"]
["离散变量备用31","DR.PUBLIC_BY_BOOL_31"]
["离散变量备用32","DR.PUBLIC_BY_BOOL_32"]
["UF2 PID频率输出","AR.PUBLIC_2#UF_FXB_PID"]
["2号垢剂泵切换","AR.PUBLIC_BYZGJB_QH"]
["RO_回用水泵频率PID输出","AR.PUBLIC_RO_HYSB_PID_S"]
["RO_手动输入运行数量","AR.PUBLIC_RO_MAN_SETNUM"]
["RO1_段间泵频率PID输出","AR.PUBLIC_RO1_DJB_PID_S"]
["RO1_高压泵频率PID输出","AR.PUBLIC_RO1_GYB_PID_S"]
["RO1膜通量","AR.PUBLIC_RO1_MTL"]
["RO2_段间泵频率PID输出","AR.PUBLIC_RO2_DJB_PID_S"]
["RO2_高压泵频率PID输出","AR.PUBLIC_RO2_GYB_PID_S"]
["RO2膜通量","AR.PUBLIC_RO2_MTL"]
["RO反洗泵定频OUT","AR.PUBLIC_RO_FXB_FRE_S"]
["RO反洗泵频率设定[0]","AR.PUBLIC_RO_FXB_FRE_0"]
["RO反洗泵频率设定[1]","AR.PUBLIC_RO_FXB_FRE_1"]
["RO反洗泵频率设定[2]","AR.PUBLIC_RO_FXB_FRE_2"]
["RO反洗泵频率设定[3]","AR.PUBLIC_RO_FXB_FRE_3"]
["RO反洗泵频率设定[4]","AR.PUBLIC_RO_FXB_FRE_4"]
["RO反洗泵频率设定[5]","AR.PUBLIC_RO_FXB_FRE_5"]
["RO反洗泵频率设定[6]","AR.PUBLIC_RO_FXB_FRE_6"]
["RO反洗泵频率设定[7]","AR.PUBLIC_RO_FXB_FRE_7"]
["RO反洗泵频率设定[8]","AR.PUBLIC_RO_FXB_FRE_8"]
["RO反洗泵频率设定[9]","AR.PUBLIC_RO_FXB_FRE_9"]
["RO供水泵定频OUT","AR.PUBLIC_RO_GSB_FRE_S"]
["RO供水泵频率设定[0]","AR.PUBLIC_RO_GSB_FRE_0"]
["RO供水泵频率设定[1]","AR.PUBLIC_RO_GSB_FRE_1"]
["RO供水泵频率设定[2]","AR.PUBLIC_RO_GSB_FRE_2"]
["RO供水泵频率设定[3]","AR.PUBLIC_RO_GSB_FRE_3"]
["RO供水泵频率设定[4]","AR.PUBLIC_RO_GSB_FRE_4"]
["RO供水泵频率设定[5]","AR.PUBLIC_RO_GSB_FRE_5"]
["RO供水泵频率设定[6]","AR.PUBLIC_RO_GSB_FRE_6"]
["RO供水泵频率设定[7]","AR.PUBLIC_RO_GSB_FRE_7"]
["RO供水泵频率设定[8]","AR.PUBLIC_RO_GSB_FRE_8"]
["RO供水泵频率设定[9]","AR.PUBLIC_RO_GSB_FRE_9"]
["RO回用水泵恒压值SP","AR.PUBLIC_RO_HYSB_SP"]
["RO回用水泵频率设定[0]","AR.PUBLIC_RO_HYSB_FRE_0"]
["RO回用水泵频率设定[1]","AR.PUBLIC_RO_HYSB_FRE_1"]
["RO回用水泵频率设定[2]","AR.PUBLIC_RO_HYSB_FRE_2"]
["RO回用水泵频率设定[3]","AR.PUBLIC_RO_HYSB_FRE_3"]
["UF1 PID频率输出","AR.PUBLIC_1#UF_FXB_PID"]
["UF手动输入运行数量","AR.PUBLIC_UF_MAN_SETNUM"]
["UF1调节阀PID开度","AR.PUBLIC_UF1_TJV_PID_O"]
["UF1冲水排气调节阀开度set","AR.PUBLIC_UF1TJFCSPQSET"]
["UF1过滤起始调节阀PID开度set","AR.PUBLIC_UF1TJFGLSET"]
["UF2调节阀PID开度","AR.PUBLIC_UF2_TJV_PID_O"]
["UF2冲水排气调节阀开度set","AR.PUBLIC_UF2TJFCSPQSET"]
["UF2过滤起始调节阀PID开度set","AR.PUBLIC_UF2TJFGLSET"]
["UF反洗泵流量SP","AR.PUBLIC_UF_FXB_LL_S"]
["UF反洗泵频率设定[0]","AR.PUBLIC_UF_FXB_FRE_0"]
["UF反洗泵频率设定[1]","AR.PUBLIC_UF_FXB_FRE_1"]
["UF反洗泵频率设定[2]","AR.PUBLIC_UF_FXB_FRE_2"]
["UF反洗泵频率设定[3]","AR.PUBLIC_UF_FXB_FRE_3"]
["UF反洗泵频率设定[4]","AR.PUBLIC_UF_FXB_FRE_4"]
["UF反洗泵频率设定[5]","AR.PUBLIC_UF_FXB_FRE_5"]
["UF反洗泵频率设定[6]","AR.PUBLIC_UF_FXB_FRE_6"]
["UF反洗泵频率设定[7]","AR.PUBLIC_UF_FXB_FRE_7"]
["UF反洗泵频率设定[8]","AR.PUBLIC_UF_FXB_FRE_8"]
["UF反洗泵频率设定[9]","AR.PUBLIC_UF_FXB_FRE_9"]
["UF反洗泵频率OUT","AR.PUBLIC_UF_FXB_FRE_S"]
["UF供水泵频率设定[0]","AR.PUBLIC_UF_GSB_FRE_0"]
["UF供水泵频率设定[1]","AR.PUBLIC_UF_GSB_FRE_1"]
["UF供水泵频率设定[2]","AR.PUBLIC_UF_GSB_FRE_2"]
["UF供水泵频率设定[3]","AR.PUBLIC_UF_GSB_FRE_3"]
["UF供水泵频率设定[4]","AR.PUBLIC_UF_GSB_FRE_4"]
["UF供水泵频率设定[5]","AR.PUBLIC_UF_GSB_FRE_5"]
["UF供水泵频率设定[6]","AR.PUBLIC_UF_GSB_FRE_6"]
["UF供水泵频率设定[7]","AR.PUBLIC_UF_GSB_FRE_7"]
["UF供水泵频率设定[8]","AR.PUBLIC_UF_GSB_FRE_8"]
["UF供水泵频率设定[9]","AR.PUBLIC_UF_GSB_FRE_9"]
["UF供水泵频率OUT","AR.PUBLIC_UF_GSB_FRE_S"]
["RO1三段压差","AR.PUBLIC_BY_REAL_1"]
["RO2三段压差","AR.PUBLIC_BY_REAL_2"]
["实数变量备用3","AR.PUBLIC_BY_REAL_3"]
["实数变量备用4","AR.PUBLIC_BY_REAL_4"]
["实数变量备用5","AR.PUBLIC_BY_REAL_5"]
["实数变量备用6","AR.PUBLIC_BY_REAL_6"]
["实数变量备用7","AR.PUBLIC_BY_REAL_7"]
["实数变量备用8","AR.PUBLIC_BY_REAL_8"]
["实数变量备用9","AR.PUBLIC_BY_REAL_9"]
["实数变量备用10","AR.PUBLIC_BY_REAL_10"]
["实数变量备用11","AR.PUBLIC_BY_REAL_11"]
["实数变量备用12","AR.PUBLIC_BY_REAL_12"]
["实数变量备用13","AR.PUBLIC_BY_REAL_13"]
["实数变量备用14","AR.PUBLIC_BY_REAL_14"]
["实数变量备用15","AR.PUBLIC_BY_REAL_15"]
["实数变量备用16","AR.PUBLIC_BY_REAL_16"]
["实数变量备用17","AR.PUBLIC_BY_REAL_17"]
["实数变量备用18","AR.PUBLIC_BY_REAL_18"]
["实数变量备用19","AR.PUBLIC_BY_REAL_19"]
["实数变量备用20","AR.PUBLIC_BY_REAL_20"]
["实数变量备用21","AR.PUBLIC_BY_REAL_21"]
["实数变量备用22","AR.PUBLIC_BY_REAL_22"]
["实数变量备用23","AR.PUBLIC_BY_REAL_23"]
["实数变量备用24","AR.PUBLIC_BY_REAL_24"]
["实数变量备用25","AR.PUBLIC_BY_REAL_25"]
["实数变量备用26","AR.PUBLIC_BY_REAL_26"]
["实数变量备用27","AR.PUBLIC_BY_REAL_27"]
["实数变量备用28","AR.PUBLIC_BY_REAL_28"]
["实数变量备用29","AR.PUBLIC_BY_REAL_29"]
["实数变量备用30","AR.PUBLIC_BY_REAL_30"]
["实数变量备用31","AR.PUBLIC_BY_REAL_31"]
["实数变量备用32","AR.PUBLIC_BY_REAL_32"]
["回用水泵功率因数","AR.ZZ_1#HYSB_COSΘ"]
["回用水泵正向有功电能","AR.ZZ_1#HYSB_EP"]
["回用水泵相电压Ia","AR.ZZ_1#HYSB_IA"]
["回用水泵相电压Ib","AR.ZZ_1#HYSB_IB"]
["回用水泵相电压Ic","AR.ZZ_1#HYSB_IC"]
["回用水泵相电压总功率","AR.ZZ_1#HYSB_POWER"]
["回用水泵相电压Ua","AR.ZZ_1#HYSB_UA"]
["回用水泵相电压Ub","AR.ZZ_1#HYSB_UB"]
["回用水泵相电压Uc","AR.ZZ_1#HYSB_UC"]
["1#RO段间泵功率因数","AR.ZZ_1#RODJB_COSΘ"]
["1#RO段间泵正向有功电能","AR.ZZ_1#RODJB_EP"]
["1#RO段间泵相电压Ia","AR.ZZ_1#RODJB_IA"]
["1#RO段间泵相电压Ib","AR.ZZ_1#RODJB_IB"]
["1#RO段间泵相电压Ic","AR.ZZ_1#RODJB_IC"]
["1#RO段间泵相电压总功率","AR.ZZ_1#RODJB_POWER"]
["1#RO段间泵相电压Ua","AR.ZZ_1#RODJB_UA"]
["1#RO段间泵相电压Ub","AR.ZZ_1#RODJB_UB"]
["1#RO段间泵相电压Uc","AR.ZZ_1#RODJB_UC"]
["1#RO高压泵功率因数","AR.ZZ_1#ROGYB_COSΘ"]
["1#RO高压泵正向有功电能","AR.ZZ_1#ROGYB_EP"]
["1#RO高压泵相电压Ia","AR.ZZ_1#ROGYB_IA"]
["1#RO高压泵相电压Ib","AR.ZZ_1#ROGYB_IB"]
["1#RO高压泵相电压Ic","AR.ZZ_1#ROGYB_IC"]
["1#RO高压泵相电压总功率","AR.ZZ_1#ROGYB_POWER"]
["1#RO高压泵相电压Ua","AR.ZZ_1#ROGYB_UA"]
["1#RO高压泵相电压Ub","AR.ZZ_1#ROGYB_UB"]
["1#RO高压泵相电压Uc","AR.ZZ_1#ROGYB_UC"]
["1#UF反洗泵功率因数","AR.ZZ_1#UFBWB_COSΘ"]
["1#UF反洗泵正向有功电能","AR.ZZ_1#UFBWB_EP"]
["1#UF反洗泵相电压Ia","AR.ZZ_1#UFBWB_IA"]
["1#UF反洗泵相电压Ib","AR.ZZ_1#UFBWB_IB"]
["1#UF反洗泵相电压Ic","AR.ZZ_1#UFBWB_IC"]
["1#UF反洗泵相电压总功率","AR.ZZ_1#UFBWB_POWER"]
["1#UF反洗泵相电压Ua","AR.ZZ_1#UFBWB_UA"]
["1#UF反洗泵相电压Ub","AR.ZZ_1#UFBWB_UB"]
["1#UF反洗泵相电压Uc","AR.ZZ_1#UFBWB_UC"]
["2#回用水泵功率因数","AR.ZZ_2#HYSB_COSΘ"]
["2#回用水泵正向有功电能","AR.ZZ_2#HYSB_EP"]
["2#回用水泵相电压Ia","AR.ZZ_2#HYSB_IA"]
["2#回用水泵相电压Ib","AR.ZZ_2#HYSB_IB"]
["2#回用水泵相电压Ic","AR.ZZ_2#HYSB_IC"]
["2#回用水泵相电压总功率","AR.ZZ_2#HYSB_POWER"]
["2#回用水泵相电压Ua","AR.ZZ_2#HYSB_UA"]
["2#回用水泵相电压Ub","AR.ZZ_2#HYSB_UB"]
["2#回用水泵相电压Uc","AR.ZZ_2#HYSB_UC"]
["2#空压机功率因数","AR.ZZ_2#KYJ_COSΘ"]
["2#空压机正向有功电能","AR.ZZ_2#KYJ_EP"]
["2#空压机相电压Ia","AR.ZZ_2#KYJ_IA"]
["2#空压机相电压Ib","AR.ZZ_2#KYJ_IB"]
["2#空压机相电压Ic","AR.ZZ_2#KYJ_IC"]
["2#空压机相电压总功率","AR.ZZ_2#KYJ_POWER"]
["2#空压机相电压Ua","AR.ZZ_2#KYJ_UA"]
["2#空压机相电压Ub","AR.ZZ_2#KYJ_UB"]
["2#空压机相电压Uc","AR.ZZ_2#KYJ_UC"]
["2#RO段间泵功率因数","AR.ZZ_2#RODJB_COSΘ"]
["2#RO段间泵正向有功电能","AR.ZZ_2#RODJB_EP"]
["2#RO段间泵相电压Ia","AR.ZZ_2#RODJB_IA"]
["2#RO段间泵相电压Ib","AR.ZZ_2#RODJB_IB"]
["2#RO段间泵相电压Ic","AR.ZZ_2#RODJB_IC"]
["2#RO段间泵相电压总功率","AR.ZZ_2#RODJB_POWER"]
["2#RO段间泵相电压Ua","AR.ZZ_2#RODJB_UA"]
["2#RO段间泵相电压Ub","AR.ZZ_2#RODJB_UB"]
["2#RO段间泵相电压Uc","AR.ZZ_2#RODJB_UC"]
["2#RO高压泵功率因数","AR.ZZ_2#ROGYB_COSΘ"]
["2#RO高压泵正向有功电能","AR.ZZ_2#ROGYB_EP"]
["2#RO高压泵相电压Ia","AR.ZZ_2#ROGYB_IA"]
["2#RO高压泵相电压Ib","AR.ZZ_2#ROGYB_IB"]
["2#RO高压泵相电压Ic","AR.ZZ_2#ROGYB_IC"]
["2#RO高压泵相电压总功率","AR.ZZ_2#ROGYB_POWER"]
["2#RO高压泵相电压Ua","AR.ZZ_2#ROGYB_UA"]
["2#RO高压泵相电压Ub","AR.ZZ_2#ROGYB_UB"]
["2#RO高压泵相电压Uc","AR.ZZ_2#ROGYB_UC"]
["2#UF反洗泵功率因数","AR.ZZ_2#UFBWB_COSΘ"]
["2#UF反洗泵正向有功电能","AR.ZZ_2#UFBWB_EP"]
["2#UF反洗泵相电压Ia","AR.ZZ_2#UFBWB_IA"]
["2#UF反洗泵相电压Ib","AR.ZZ_2#UFBWB_IB"]
["2#UF反洗泵相电压Ic","AR.ZZ_2#UFBWB_IC"]
["2#UF反洗泵相电压总功率","AR.ZZ_2#UFBWB_POWER"]
["2#UF反洗泵相电压Ua","AR.ZZ_2#UFBWB_UA"]
["2#UF反洗泵相电压Ub","AR.ZZ_2#UFBWB_UB"]
["2#UF反洗泵相电压Uc","AR.ZZ_2#UFBWB_UC"]
["1#电源进线功率因数","AR.ZZ_DYJX1_COSΘ"]
["1#电源进线正向有功电能","AR.ZZ_DYJX1_EP"]
["1#电源进线相电压Ia","AR.ZZ_DYJX1_IA"]
["1#电源进线相电压Ib","AR.ZZ_DYJX1_IB"]
["1#电源进线相电压Ic","AR.ZZ_DYJX1_IC"]
["1#电源进线相电压总功率","AR.ZZ_DYJX1_POWER"]
["1#电源进线相电压Ua","AR.ZZ_DYJX1_UA"]
["1#电源进线相电压Ub","AR.ZZ_DYJX1_UB"]
["1#电源进线相电压Uc","AR.ZZ_DYJX1_UC"]
["2#电源进线功率因数","AR.ZZ_DYJX2_COSΘ"]
["2#电源进线正向有功电能","AR.ZZ_DYJX2_EP"]
["2#电源进线相电压Ia","AR.ZZ_DYJX2_IA"]
["2#电源进线相电压Ib","AR.ZZ_DYJX2_IB"]
["2#电源进线相电压Ic","AR.ZZ_DYJX2_IC"]
["2#电源进线相电压总功率","AR.ZZ_DYJX2_POWER"]
["2#电源进线相电压Ua","AR.ZZ_DYJX2_UA"]
["2#电源进线相电压Ub","AR.ZZ_DYJX2_UB"]
["2#电源进线相电压Uc","AR.ZZ_DYJX2_UC"]
["1楼暖通功率因数","AR.ZZ_F1NT_COSΘ"]
["1楼暖通正向有功电能","AR.ZZ_F1NT_EP"]
["1楼暖通相电压Ia","AR.ZZ_F1NT_IA"]
["1楼暖通相电压Ib","AR.ZZ_F1NT_IB"]
["1楼暖通相电压Ic","AR.ZZ_F1NT_IC"]
["1楼暖通相电压总功率","AR.ZZ_F1NT_POWER"]
["1楼暖通相电压Ua","AR.ZZ_F1NT_UA"]
["1楼暖通相电压Ub","AR.ZZ_F1NT_UB"]
["1楼暖通相电压Uc","AR.ZZ_F1NT_UC"]
["2楼暖通功率因数","AR.ZZ_F2NT_COSΘ"]
["2楼暖通正向有功电能","AR.ZZ_F2NT_EP"]
["2楼暖通相电压Ia","AR.ZZ_F2NT_IA"]
["2楼暖通相电压Ib","AR.ZZ_F2NT_IB"]
["2楼暖通相电压Ic","AR.ZZ_F2NT_IC"]
["2楼暖通相电压总功率","AR.ZZ_F2NT_POWER"]
["2楼暖通相电压Ua","AR.ZZ_F2NT_UA"]
["2楼暖通相电压Ub","AR.ZZ_F2NT_UB"]
["2楼暖通相电压Uc","AR.ZZ_F2NT_UC"]
["废水排放泵功率因数","AR.ZZ_FSPFB_COSΘ"]
["废水排放泵正向有功电能","AR.ZZ_FSPFB_EP"]
["废水排放泵相电压Ia","AR.ZZ_FSPFB_IA"]
["废水排放泵相电压Ib","AR.ZZ_FSPFB_IB"]
["废水排放泵相电压Ic","AR.ZZ_FSPFB_IC"]
["废水排放泵相电压总功率","AR.ZZ_FSPFB_POWER"]
["废水排放泵相电压Ua","AR.ZZ_FSPFB_UA"]
["废水排放泵相电压Ub","AR.ZZ_FSPFB_UB"]
["废水排放泵相电压Uc","AR.ZZ_FSPFB_UC"]
["电源加热功率因数","AR.ZZ_JR_COSΘ"]
["电源加热正向有功电能","AR.ZZ_JR_EP"]
["电源加热相电压Ia","AR.ZZ_JR_IA"]
["电源加热相电压Ib","AR.ZZ_JR_IB"]
["电源加热相电压Ic","AR.ZZ_JR_IC"]
["电源加热相电压总功率","AR.ZZ_JR_POWER"]
["电源加热相电压Ua","AR.ZZ_JR_UA"]
["电源加热相电压Ub","AR.ZZ_JR_UB"]
["电源加热相电压Uc","AR.ZZ_JR_UC"]
["加药间功率因数","AR.ZZ_JYJ_COSΘ"]
["加药间正向有功电能","AR.ZZ_JYJ_EP"]
["加药间相电压Ia","AR.ZZ_JYJ_IA"]
["加药间相电压Ib","AR.ZZ_JYJ_IB"]
["加药间相电压Ic","AR.ZZ_JYJ_IC"]
["加药间相电压总功率","AR.ZZ_JYJ_POWER"]
["加药间相电压Ua","AR.ZZ_JYJ_UA"]
["加药间相电压Ub","AR.ZZ_JYJ_UB"]
["加药间相电压Uc","AR.ZZ_JYJ_UC"]
["1#空压机功率因数","AR.ZZ_KYJ_COSΘ"]
["1#空压机正向有功电能","AR.ZZ_KYJ_EP"]
["1#空压机相电压Ia","AR.ZZ_KYJ_IA"]
["1#空压机相电压Ib","AR.ZZ_KYJ_IB"]
["1#空压机相电压Ic","AR.ZZ_KYJ_IC"]
["1#空压机相电压总功率","AR.ZZ_KYJ_POWER"]
["1#空压机相电压Ua","AR.ZZ_KYJ_UA"]
["1#空压机相电压Ub","AR.ZZ_KYJ_UB"]
["1#空压机相电压Uc","AR.ZZ_KYJ_UC"]
["1#照明模块第一路","AR.ZZ_MB_1#ZM1"]
["1#照明模块第二路","AR.ZZ_MB_1#ZM2"]
["1#照明模块第三路","AR.ZZ_MB_1#ZM3"]
["1#照明模块第四路","AR.ZZ_MB_1#ZM4"]
["1#照明模块第五路","AR.ZZ_MB_1#ZM5"]
["1#照明模块第六路","AR.ZZ_MB_1#ZM6"]
["2#照明模块第一路","AR.ZZ_MB_2#ZM1"]
["2#照明模块第二路","AR.ZZ_MB_2#ZM2"]
["2#照明模块第三路","AR.ZZ_MB_2#ZM3"]
["2#照明模块第四路","AR.ZZ_MB_2#ZM4"]
["2#照明模块第五路","AR.ZZ_MB_2#ZM5"]
["2#照明模块第六路","AR.ZZ_MB_2#ZM6"]
["3#照明模块第一路","AR.ZZ_MB_3#ZM1"]
["3#照明模块第二路","AR.ZZ_MB_3#ZM2"]
["3#照明模块第三路","AR.ZZ_MB_3#ZM3"]
["3#照明模块第四路","AR.ZZ_MB_3#ZM4"]
["3#照明模块第五路","AR.ZZ_MB_3#ZM5"]
["3#照明模块第六路","AR.ZZ_MB_3#ZM6"]
["4#照明模块第一路","AR.ZZ_MB_4#ZM1"]
["4#照明模块第二路","AR.ZZ_MB_4#ZM2"]
["4#照明模块第三路","AR.ZZ_MB_4#ZM3"]
["4#照明模块第四路","AR.ZZ_MB_4#ZM4"]
["4#照明模块第五路","AR.ZZ_MB_4#ZM5"]
["4#照明模块第六路","AR.ZZ_MB_4#ZM6"]
["一楼温湿度1湿度","AR.ZZ_MB_F1WSD1_SD"]
["一楼温湿度1温度","AR.ZZ_MB_F1WSD1_WD"]
["一楼温湿度2湿度","AR.ZZ_MB_F1WSD2_SD"]
["一楼温湿度2温度","AR.ZZ_MB_F1WSD2_WD"]
["一楼温湿度3湿度","AR.ZZ_MB_F1WSD3_SD"]
["一楼温湿度3温度","AR.ZZ_MB_F1WSD3_WD"]
["一楼烟感1","AR.ZZ_MB_F1YG1"]
["一楼烟感2","AR.ZZ_MB_F1YG2"]
["一楼烟感3","AR.ZZ_MB_F1YG3"]
["二楼温湿度1湿度","AR.ZZ_MB_F2WSD1_SD"]
["二楼温湿度1温度","AR.ZZ_MB_F2WSD1_WD"]
["二楼温湿度2湿度","AR.ZZ_MB_F2WSD2_SD"]
["二楼温湿度2温度","AR.ZZ_MB_F2WSD2_WD"]
["二楼烟感1","AR.ZZ_MB_F2YG1"]
["二楼烟感2","AR.ZZ_MB_F2YG2"]
["前端泵房功率因数","AR.ZZ_QDBF_COSΘ"]
["前端泵房正向有功电能","AR.ZZ_QDBF_EP"]
["前端泵房相电压Ia","AR.ZZ_QDBF_IA"]
["前端泵房相电压Ib","AR.ZZ_QDBF_IB"]
["前端泵房相电压Ic","AR.ZZ_QDBF_IC"]
["前端泵房相电压总功率","AR.ZZ_QDBF_POWER"]
["前端泵房相电压Ua","AR.ZZ_QDBF_UA"]
["前端泵房相电压Ub","AR.ZZ_QDBF_UB"]
["前端泵房相电压Uc","AR.ZZ_QDBF_UC"]
["清洗水泵功率因数","AR.ZZ_QXSB_COSΘ"]
["清洗水泵正向有功电能","AR.ZZ_QXSB_EP"]
["清洗水泵相电压Ia","AR.ZZ_QXSB_IA"]
["清洗水泵相电压Ib","AR.ZZ_QXSB_IB"]
["清洗水泵相电压Ic","AR.ZZ_QXSB_IC"]
["清洗水泵相电压总功率","AR.ZZ_QXSB_POWER"]
["清洗水泵相电压Ua","AR.ZZ_QXSB_UA"]
["清洗水泵相电压Ub","AR.ZZ_QXSB_UB"]
["清洗水泵相电压Uc","AR.ZZ_QXSB_UC"]
["RO供水泵功率因数","AR.ZZ_ROGSB_COSΘ"]
["RO供水泵正向有功电能","AR.ZZ_ROGSB_EP"]
["RO供水泵相电压Ia","AR.ZZ_ROGSB_IA"]
["RO供水泵相电压Ib","AR.ZZ_ROGSB_IB"]
["RO供水泵相电压Ic","AR.ZZ_ROGSB_IC"]
["RO供水泵相电压总功率","AR.ZZ_ROGSB_POWER"]
["RO供水泵相电压Ua","AR.ZZ_ROGSB_UA"]
["RO供水泵相电压Ub","AR.ZZ_ROGSB_UB"]
["RO供水泵相电压Uc","AR.ZZ_ROGSB_UC"]
["溶药功率因数","AR.ZZ_RY_COSΘ"]
["溶药正向有功电能","AR.ZZ_RY_EP"]
["溶药相电压Ia","AR.ZZ_RY_IA"]
["溶药相电压Ib","AR.ZZ_RY_IB"]
["溶药相电压Ic","AR.ZZ_RY_IC"]
["溶药相电压总功率","AR.ZZ_RY_POWER"]
["溶药相电压Ua","AR.ZZ_RY_UA"]
["溶药相电压Ub","AR.ZZ_RY_UB"]
["溶药相电压Uc","AR.ZZ_RY_UC"]
["UF供水泵功率因数","AR.ZZ_UFGSB_COSΘ"]
["UF供水泵正向有功电能","AR.ZZ_UFGSB_EP"]
["UF供水泵相电压Ia","AR.ZZ_UFGSB_IA"]
["UF供水泵相电压Ib","AR.ZZ_UFGSB_IB"]
["UF供水泵相电压Ic","AR.ZZ_UFGSB_IC"]
["UF供水泵相电压总功率","AR.ZZ_UFGSB_POWER"]
["UF供水泵相电压Ua","AR.ZZ_UFGSB_UA"]
["UF供水泵相电压Ub","AR.ZZ_UFGSB_UB"]
["UF供水泵相电压Uc","AR.ZZ_UFGSB_UC"]
["UPS功率因数","AR.ZZ_UPS_COSΘ"]
["UPS正向有功电能","AR.ZZ_UPS_EP"]
["UPS相电压Ia","AR.ZZ_UPS_IA"]
["UPS相电压Ib","AR.ZZ_UPS_IB"]
["UPS相电压Ic","AR.ZZ_UPS_IC"]
["UPS相电压总功率","AR.ZZ_UPS_POWER"]
["UPS相电压Ua","AR.ZZ_UPS_UA"]
["UPS相电压Ub","AR.ZZ_UPS_UB"]
["UPS相电压Uc","AR.ZZ_UPS_UC"]
["中和废水泵功率因数","AR.ZZ_ZHFSB_COSΘ"]
["中和废水泵正向有功电能","AR.ZZ_ZHFSB_EP"]
["中和废水泵相电压Ia","AR.ZZ_ZHFSB_IA"]
["中和废水泵相电压Ib","AR.ZZ_ZHFSB_IB"]
["中和废水泵相电压Ic","AR.ZZ_ZHFSB_IC"]
["中和废水泵相电压总功率","AR.ZZ_ZHFSB_POWER"]
["中和废水泵相电压Ua","AR.ZZ_ZHFSB_UA"]
["中和废水泵相电压Ub","AR.ZZ_ZHFSB_UB"]
["中和废水泵相电压Uc","AR.ZZ_ZHFSB_UC"]
["RO1三段压差设定","AR.RO1_EX_3DYACHASET"]
["RO1三段压差读取","AR.RO1_EX_3DYCREAD"]
["RO1压力设置HH1","AR.RO1_EX_DPT1_HHR"]
["RO1压力设置HH2","AR.RO1_EX_DPT2_HHR"]
["RO1压力设置HH3","AR.RO1_EX_DPT3_HHR"]
["RO1一段进水压力设置","AR.RO1_EX_PRESSHHR_11"]
["RO1一段浓水压力设置","AR.RO1_EX_PRESSHHR_12"]
["RO1二段压力设定","AR.RO1_EX_PRESSHHR_22"]
["RO1三段进水压力设定","AR.RO1_EX_PRESSHHR_31"]
["RO1三段浓水压力设定","AR.RO1_EX_PRESSHHR_32"]
["RO1产水压力设定","AR.RO1_EX_PRESSHHR_CS"]
["RO1实数备用1","AR.RO1_EX_ZBY_R8"]
["RO1实数备用2","AR.RO1_EX_ZBY_R9"]
["RO1过滤停机不冲洗时间设定","AR.RO1_EX2_TJBCX_TIME"]
["RO1过滤停机冲23段洗时间设定","AR.RO1_EX2_TJC23D_TIME"]
["RO1停机整体冲洗时间设定","AR.RO1_EX2_TJZTCS_TIME"]
["RO1双整备用7","AR.RO1_EX2_ZBY_DINT10"]
["RO1双整备用1","AR.RO1_EX2_ZBY_DINT4"]
["RO1双整备用2","AR.RO1_EX2_ZBY_DINT5"]
["RO1双整备用3","AR.RO1_EX2_ZBY_DINT6"]
["RO1双整备用4","AR.RO1_EX2_ZBY_DINT7"]
["RO1双整备用5","AR.RO1_EX2_ZBY_DINT8"]
["RO1双整备用6","AR.RO1_EX2_ZBY_DINT9"]
["RO1实数备用EX21","AR.RO1_EX2_ZBY_R1"]
["RO1实数备用10","AR.RO1_EX2_ZBY_R10"]
["RO1实数备用EX22","AR.RO1_EX2_ZBY_R2"]
["RO1实数备用3","AR.RO1_EX2_ZBY_R3"]
["RO1实数备用4","AR.RO1_EX2_ZBY_R4"]
["RO1实数备用5","AR.RO1_EX2_ZBY_R5"]
["RO1实数备用6","AR.RO1_EX2_ZBY_R6"]
["RO1实数备用7","AR.RO1_EX2_ZBY_R7"]
["RO1实数备用8","AR.RO1_EX2_ZBY_R8"]
["RO1实数备用9","AR.RO1_EX2_ZBY_R9"]
["RO2三段压差设定","AR.RO2_EX_3DYACHASET"]
["RO2三段压差读取","AR.RO2_EX_3DYCREAD"]
["RO2压力设置HH1","AR.RO2_EX_DPT1_HHR"]
["RO2压力设置HH2","AR.RO2_EX_DPT2_HHR"]
["RO2压力设置HH3","AR.RO2_EX_DPT3_HHR"]
["RO2一段进水压力设置","AR.RO2_EX_PRESSHHR_11"]
["RO2一段浓水压力设置","AR.RO2_EX_PRESSHHR_12"]
["RO2二段压力设定","AR.RO2_EX_PRESSHHR_22"]
["RO2三段进水压力设定","AR.RO2_EX_PRESSHHR_31"]
["RO2三段浓水压力设定","AR.RO2_EX_PRESSHHR_32"]
["RO2产水压力设定","AR.RO2_EX_PRESSHHR_CS"]
["RO2实数备用1","AR.RO2_EX_ZBY_R8"]
["RO2实数备用2","AR.RO2_EX_ZBY_R9"]
["RO2过滤停机不冲洗时间设定","AR.RO2_EX2_TJBCX_TIME"]
["RO2过滤停机冲23段洗时间设定","AR.RO2_EX2_TJC23D_TIME"]
["RO2停机整体冲洗时间设定","AR.RO2_EX2_TJZTCS_TIME"]
["RO2双整备用7","AR.RO2_EX2_ZBY_DINT10"]
["RO2双整备用1","AR.RO2_EX2_ZBY_DINT4"]
["RO2双整备用2","AR.RO2_EX2_ZBY_DINT5"]
["RO2双整备用3","AR.RO2_EX2_ZBY_DINT6"]
["RO2双整备用4","AR.RO2_EX2_ZBY_DINT7"]
["RO2双整备用5","AR.RO2_EX2_ZBY_DINT8"]
["RO2双整备用6","AR.RO2_EX2_ZBY_DINT9"]
["RO2实数备用EX21","AR.RO2_EX2_ZBY_R1"]
["RO2实数备用10","AR.RO2_EX2_ZBY_R10"]
["RO2实数备用EX22","AR.RO2_EX2_ZBY_R2"]
["RO2实数备用3","AR.RO2_EX2_ZBY_R3"]
["RO2实数备用4","AR.RO2_EX2_ZBY_R4"]
["RO2实数备用5","AR.RO2_EX2_ZBY_R5"]
["RO2实数备用6","AR.RO2_EX2_ZBY_R6"]
["RO2实数备用7","AR.RO2_EX2_ZBY_R7"]
["RO2实数备用8","AR.RO2_EX2_ZBY_R8"]
["RO2实数备用9","AR.RO2_EX2_ZBY_R9"]
["RO产水池启动RO数量0","AR.YWLD_RO_CSC_LDUPNUM0"]
["RO产水池启动RO数量1","AR.YWLD_RO_CSC_LDUPNUM1"]
["RO产水池启动RO数量2","AR.YWLD_RO_CSC_LDUPNUM2"]
["RO产水池启动二套RO液位","AR.YWLD_RO_CSC_LDYWR[0]"]
["RO产水池启动一套RO液位","AR.YWLD_RO_CSC_LDYWR[1]"]
["RO产水池停止RO液位","AR.YWLD_RO_CSC_LDYWR[2]"]
["RO进水池启动数量0","AR.YWLD_RO_JSC_LDUPNUM0"]
["RO进水池启动RO数量1","AR.YWLD_RO_JSC_LDUPNUM1"]
["RO进水池启动RO数量2","AR.YWLD_RO_JSC_LDUPNUM2"]
["RO进水箱停RO液位","AR.YWLD_RO_JSC_LDYWR[0]"]
["RO进水箱启动一套RO液位","AR.YWLD_RO_JSC_LDYWR[1]"]
["RO进水箱启动二套RO液位","AR.YWLD_RO_JSC_LDYWR[2]"]
["RO冲洗不允许液位","AR.YWLD_ROCSC_BW_LLR"]
["RO冲洗允许液位","AR.YWLD_ROCSC_BW_LR"]
["RO产水池启动RO数量","AR.YWLD_SSDROCSCNEEDNUM"]
["RO进水池启动RO数量","AR.YWLD_SSDROJSCNEEDNUM"]
["RO联动液位自动启动数量","AR.YWLD_SSDRONEEDNUM_YW"]
["UF产水池启动UF数量","AR.YWLD_SSDUFCSCNEEDNUM"]
["UF进水池启动UF数量","AR.YWLD_SSDUFJSCNEEDNUM"]
["UF自动液位启动数量","AR.YWLD_SSDUFNEEDNUM_YW"]
["UF产水池启动UF数量0","AR.YWLD_UF_CSC_LDUPNUM0"]
["UF产水池启动UF数量1","AR.YWLD_UF_CSC_LDUPNUM1"]
["UF产水池启动UF数量2","AR.YWLD_UF_CSC_LDUPNUM2"]
["UF产水箱启两套UF液位","AR.YWLD_UF_CSC_LDYWR[0]"]
["UF产水箱启一套UF液位","AR.YWLD_UF_CSC_LDYWR[1]"]
["UF产水箱启零套UF液位","AR.YWLD_UF_CSC_LDYWR[2]"]
["UF进水池启动数量0","AR.YWLD_UF_JSC_LDUPNUM0"]
["UF进水池启动数量1","AR.YWLD_UF_JSC_LDUPNUM1"]
["UF进水池启动数量2","AR.YWLD_UF_JSC_LDUPNUM2"]
["UF进水池停UF液位","AR.YWLD_UF_JSC_LDYWR[0]"]
["UF进水池启动一套UF液位","AR.YWLD_UF_JSC_LDYWR[1]"]
["UF进水池启动二套UF液位","AR.YWLD_UF_JSC_LDYWR[2]"]
["BW不允许液位","AR.YWLD_UFCSC_BW_LLR"]
["BW允许液位","AR.YWLD_UFCSC_BW_LR"]
["CEB允许液位","AR.YWLD_UFCSC_CEB_ALLOW"]
["YWLD实数备用1","AR.YWLD_ZBYR1"]
["YWLD实数备用2","AR.YWLD_ZBYR2"]
["YWLD实数备用3","AR.YWLD_ZBYR3"]
["YWLD实数备用4","AR.YWLD_ZBYR4"]
["YWLD实数备用5","AR.YWLD_ZBYR5"]
["YWLD实数备用6","AR.YWLD_ZBYR6"]
["YWLD实数备用7","AR.YWLD_ZBYR7"]
["反洗水泵A震动温度","AR.ZZ_FXSB_A_ZD_WD"]
["反洗水泵A震动X轴速度","AR.ZZ_FXSB_A_ZD_XZSD"]
["反洗水泵A震动X轴位移","AR.ZZ_FXSB_A_ZD_XZWY"]
["反洗水泵A震动Y轴速度","AR.ZZ_FXSB_A_ZD_YZSD"]
["反洗水泵A震动Y轴位移","AR.ZZ_FXSB_A_ZD_YZWY"]
["反洗水泵A震动Z轴速度","AR.ZZ_FXSB_A_ZD_ZZSD"]
["反洗水泵A震动Z轴位移","AR.ZZ_FXSB_A_ZD_ZZWY"]
["反洗水泵B震动温度","AR.ZZ_FXSB_B_ZD_WD"]
["反洗水泵B震动X轴速度","AR.ZZ_FXSB_B_ZD_XZSD"]
["反洗水泵B震动X轴位移","AR.ZZ_FXSB_B_ZD_XZWY"]
["反洗水泵B震动Y轴速度","AR.ZZ_FXSB_B_ZD_YZSD"]
["反洗水泵B震动Y轴位移","AR.ZZ_FXSB_B_ZD_YZWY"]
["反洗水泵B震动Z轴速度","AR.ZZ_FXSB_B_ZD_ZZSD"]
["反洗水泵B震动Z轴位移","AR.ZZ_FXSB_B_ZD_ZZWY"]
["回用水泵A震动温度","AR.ZZ_HYSB_A_ZD_WD"]
["回用水泵A震动X轴速度","AR.ZZ_HYSB_A_ZD_XZSD"]
["回用水泵A震动X轴位移","AR.ZZ_HYSB_A_ZD_XZWY"]
["回用水泵A震动Y轴速度","AR.ZZ_HYSB_A_ZD_YZSD"]
["回用水泵A震动Y轴位移","AR.ZZ_HYSB_A_ZD_YZWY"]
["回用水泵A震动Z轴速度","AR.ZZ_HYSB_A_ZD_ZZSD"]
["回用水泵A震动Z轴位移","AR.ZZ_HYSB_A_ZD_ZZWY"]
["回用水泵B震动温度","AR.ZZ_HYSB_B_ZD_WD"]
["回用水泵B震动X轴速度","AR.ZZ_HYSB_B_ZD_XZSD"]
["回用水泵B震动X轴位移","AR.ZZ_HYSB_B_ZD_XZWY"]
["回用水泵B震动Y轴速度","AR.ZZ_HYSB_B_ZD_YZSD"]
["回用水泵B震动Y轴位移","AR.ZZ_HYSB_B_ZD_YZWY"]
["回用水泵B震动Z轴速度","AR.ZZ_HYSB_B_ZD_ZZSD"]
["回用水泵B震动Z轴位移","AR.ZZ_HYSB_B_ZD_ZZWY"]
["RO供水泵震动温度","AR.ZZ_ROGSB_ZD_WD"]
["RO供水泵震动X轴速度","AR.ZZ_ROGSB_ZD_XZSD"]
["RO供水泵震动X轴位移","AR.ZZ_ROGSB_ZD_XZWY"]
["RO供水泵震动Y轴速度","AR.ZZ_ROGSB_ZD_YZSD"]
["RO供水泵震动Y轴位移","AR.ZZ_ROGSB_ZD_YZWY"]
["RO供水泵震动Z轴速度","AR.ZZ_ROGSB_ZD_ZZSD"]
["RO供水泵震动Z轴位移","AR.ZZ_ROGSB_ZD_ZZWY"]
["外供水泵震动温度","AR.ZZ_WGSB_ZD_WD"]
["外供水泵震动X轴速度","AR.ZZ_WGSB_ZD_XZSD"]
["外供水泵震动X轴位移","AR.ZZ_WGSB_ZD_XZWY"]
["外供水泵震动Y轴速度","AR.ZZ_WGSB_ZD_YZSD"]
["外供水泵震动Y轴位移","AR.ZZ_WGSB_ZD_YZWY"]
["外供水泵震动Z轴速度","AR.ZZ_WGSB_ZD_ZZSD"]
["外供水泵震动Z轴位移","AR.ZZ_WGSB_ZD_ZZWY"]
["RO1三段压差高","DR.RO1_EX_3DYCG"]
["RO1压差HH报警1","DR.RO1_EX_DPT1_HH"]
["RO1压差HH报警2","DR.RO1_EX_DPT2_HH"]
["RO1压差HH报警3","DR.RO1_EX_DPT3_HH"]
["RO1一段进水压力高","DR.RO1_EX_PRESSHH_11"]
["RO1一段浓水压力高","DR.RO1_EX_PRESSHH_12"]
["RO1二段压力高","DR.RO1_EX_PRESSHH_22"]
["RO1三段进水压力高","DR.RO1_EX_PRESSHH_31"]
["RO1三段浓水压力高","DR.RO1_EX_PRESSHH_32"]
["RO1产水压力高报警","DR.RO1_EX_PRESSHH_CS"]
["RO1备用1压力高报警","DR.RO1_EX_ZFLAG_BY11"]
["RO1备用2压力高报警","DR.RO1_EX_ZFLAG_BY12"]
["RO1备用3压力高报警","DR.RO1_EX_ZFLAG_BY13"]
["RO1备用4压力高报警","DR.RO1_EX_ZFLAG_BY14"]
["RO1备用5压力高报警","DR.RO1_EX_ZFLAG_BY15"]
["RO1_BT_半自动时停机按钮","DR.RO1_EX2_BT_BZDTJ"]
["RO1_备用4按钮","DR.RO1_EX2_BT_ZZBY12"]
["RO1_备用按钮5","DR.RO1_EX2_BT_ZZBY13"]
["RO1_备用按钮6","DR.RO1_EX2_BT_ZZBY14"]
["RO1_备用按钮7","DR.RO1_EX2_BT_ZZBY15"]
["RO1_备用按钮8","DR.RO1_EX2_BT_ZZBY16"]
["RO1_备用1按钮","DR.RO1_EX2_BT_ZZBY5"]
["RO1_备用2按钮","DR.RO1_EX2_BT_ZZBY6"]
["RO1_备用3按钮","DR.RO1_EX2_BT_ZZBY7"]
["RO1_冲洗申请","DR.RO1_EX2_CXSQ"]
["RO1_FLG_段间泵出口压力大","DR.RO1_EX2_DJBCKYLD"]
["RO1_FLG_高压泵出口压力大","DR.RO1_EX2_FLG_GYBCKYLD"]
["RO1_FLG_过滤停机不冲洗","DR.RO1_EX2_FLG_TJBCX"]
["RO1_FLG_过滤停机整体冲洗","DR.RO1_EX2_FLG_TJZTCX"]
["RO1_FLG_膜里有药","DR.RO1_EX2_MLYY"]
["RO1_FLG_过滤停机冲二三段","DR.RO1_EX2_TJC23D"]
["RO2三段压差高","DR.RO2_EX_3DYCG"]
["RO2压差HH报警1","DR.RO2_EX_DPT1_HH"]
["RO2压差HH报警2","DR.RO2_EX_DPT2_HH"]
["RO2压差HH报警3","DR.RO2_EX_DPT3_HH"]
["RO2一段进水压力高","DR.RO2_EX_PRESSHH_11"]
["RO2一段浓水压力高","DR.RO2_EX_PRESSHH_12"]
["RO2二段压力高","DR.RO2_EX_PRESSHH_22"]
["RO2三段进水压力高","DR.RO2_EX_PRESSHH_31"]
["RO2三段浓水压力高","DR.RO2_EX_PRESSHH_32"]
["RO2产水压力高报警","DR.RO2_EX_PRESSHH_CS"]
["RO2备用1压力高报警","DR.RO2_EX_ZFLAG_BY11"]
["RO2备用2压力高报警","DR.RO2_EX_ZFLAG_BY12"]
["RO2备用3压力高报警","DR.RO2_EX_ZFLAG_BY13"]
["RO2备用4压力高报警","DR.RO2_EX_ZFLAG_BY14"]
["RO2备用5压力高报警","DR.RO2_EX_ZFLAG_BY15"]
["RO2_BT_半自动时停机按钮","DR.RO2_EX2_BT_BZDTJ"]
["RO2_备用4按钮","DR.RO2_EX2_BT_ZZBY12"]
["RO2_备用按钮5","DR.RO2_EX2_BT_ZZBY13"]
["RO2_备用按钮6","DR.RO2_EX2_BT_ZZBY14"]
["RO2_备用按钮7","DR.RO2_EX2_BT_ZZBY15"]
["RO2_备用按钮8","DR.RO2_EX2_BT_ZZBY16"]
["RO2_备用1按钮","DR.RO2_EX2_BT_ZZBY5"]
["RO2_备用2按钮","DR.RO2_EX2_BT_ZZBY6"]
["RO2_备用3按钮","DR.RO2_EX2_BT_ZZBY7"]
["RO2_冲洗申请","DR.RO2_EX2_CXSQ"]
["RO2_FLG_段间泵出口压力大","DR.RO2_EX2_DJBCKYLD"]
["RO2_FLG_高压泵出口压力大","DR.RO2_EX2_FLG_GYBCKYLD"]
["RO2_FLG_过滤停机不冲洗","DR.RO2_EX2_FLG_TJBCX"]
["RO2_FLG_过滤停机整体冲洗","DR.RO2_EX2_FLG_TJZTCX"]
["RO2_FLG_膜里有药","DR.RO2_EX2_MLYY"]
["RO2_FLG_过滤停机冲二三段","DR.RO2_EX2_TJC23D"]
["加药间1噪音频率1","AR.ZZ_ZY_FR1"]
["加药间1噪音频率10","AR.ZZ_ZY_FR10"]
["加药间1噪音频率100","AR.ZZ_ZY_FR100"]
["加药间1噪音频率101","AR.ZZ_ZY_FR101"]
["加药间1噪音频率102","AR.ZZ_ZY_FR102"]
["加药间1噪音频率103","AR.ZZ_ZY_FR103"]
["加药间1噪音频率104","AR.ZZ_ZY_FR104"]
["加药间1噪音频率105","AR.ZZ_ZY_FR105"]
["加药间1噪音频率106","AR.ZZ_ZY_FR106"]
["加药间1噪音频率107","AR.ZZ_ZY_FR107"]
["加药间1噪音频率108","AR.ZZ_ZY_FR108"]
["加药间1噪音频率109","AR.ZZ_ZY_FR109"]
["加药间1噪音频率11","AR.ZZ_ZY_FR11"]
["加药间1噪音频率110","AR.ZZ_ZY_FR110"]
["加药间1噪音频率111","AR.ZZ_ZY_FR111"]
["加药间1噪音频率112","AR.ZZ_ZY_FR112"]
["加药间1噪音频率113","AR.ZZ_ZY_FR113"]
["加药间1噪音频率114","AR.ZZ_ZY_FR114"]
["加药间1噪音频率115","AR.ZZ_ZY_FR115"]
["加药间1噪音频率116","AR.ZZ_ZY_FR116"]
["加药间1噪音频率117","AR.ZZ_ZY_FR117"]
["加药间1噪音频率118","AR.ZZ_ZY_FR118"]
["加药间1噪音频率119","AR.ZZ_ZY_FR119"]
["加药间1噪音频率12","AR.ZZ_ZY_FR12"]
["加药间1噪音频率120","AR.ZZ_ZY_FR120"]
["加药间1噪音频率121","AR.ZZ_ZY_FR121"]
["加药间1噪音频率122","AR.ZZ_ZY_FR122"]
["加药间1噪音频率123","AR.ZZ_ZY_FR123"]
["加药间1噪音频率124","AR.ZZ_ZY_FR124"]
["加药间1噪音频率125","AR.ZZ_ZY_FR125"]
["加药间1噪音频率126","AR.ZZ_ZY_FR126"]
["加药间1噪音频率127","AR.ZZ_ZY_FR127"]
["加药间1噪音频率13","AR.ZZ_ZY_FR13"]
["加药间1噪音频率14","AR.ZZ_ZY_FR14"]
["加药间1噪音频率15","AR.ZZ_ZY_FR15"]
["加药间1噪音频率16","AR.ZZ_ZY_FR16"]
["加药间1噪音频率17","AR.ZZ_ZY_FR17"]
["加药间1噪音频率18","AR.ZZ_ZY_FR18"]
["加药间1噪音频率19","AR.ZZ_ZY_FR19"]
["加药间1噪音频率2","AR.ZZ_ZY_FR2"]
["加药间1噪音频率20","AR.ZZ_ZY_FR20"]
["加药间1噪音频率21","AR.ZZ_ZY_FR21"]
["加药间1噪音频率22","AR.ZZ_ZY_FR22"]
["加药间1噪音频率23","AR.ZZ_ZY_FR23"]
["加药间1噪音频率24","AR.ZZ_ZY_FR24"]
["加药间1噪音频率25","AR.ZZ_ZY_FR25"]
["加药间1噪音频率26","AR.ZZ_ZY_FR26"]
["加药间1噪音频率27","AR.ZZ_ZY_FR27"]
["加药间1噪音频率28","AR.ZZ_ZY_FR28"]
["加药间1噪音频率29","AR.ZZ_ZY_FR29"]
["加药间1噪音频率3","AR.ZZ_ZY_FR3"]
["加药间1噪音频率30","AR.ZZ_ZY_FR30"]
["加药间1噪音频率31","AR.ZZ_ZY_FR31"]
["加药间1噪音频率32","AR.ZZ_ZY_FR32"]
["加药间1噪音频率33","AR.ZZ_ZY_FR33"]
["加药间1噪音频率34","AR.ZZ_ZY_FR34"]
["加药间1噪音频率35","AR.ZZ_ZY_FR35"]
["加药间1噪音频率36","AR.ZZ_ZY_FR36"]
["加药间1噪音频率37","AR.ZZ_ZY_FR37"]
["加药间1噪音频率38","AR.ZZ_ZY_FR38"]
["加药间1噪音频率39","AR.ZZ_ZY_FR39"]
["加药间1噪音频率4","AR.ZZ_ZY_FR4"]
["加药间1噪音频率40","AR.ZZ_ZY_FR40"]
["加药间1噪音频率41","AR.ZZ_ZY_FR41"]
["加药间1噪音频率42","AR.ZZ_ZY_FR42"]
["加药间1噪音频率43","AR.ZZ_ZY_FR43"]
["加药间1噪音频率44","AR.ZZ_ZY_FR44"]
["加药间1噪音频率45","AR.ZZ_ZY_FR45"]
["加药间1噪音频率46","AR.ZZ_ZY_FR46"]
["加药间1噪音频率47","AR.ZZ_ZY_FR47"]
["加药间1噪音频率48","AR.ZZ_ZY_FR48"]
["加药间1噪音频率49","AR.ZZ_ZY_FR49"]
["加药间1噪音频率5","AR.ZZ_ZY_FR5"]
["加药间1噪音频率50","AR.ZZ_ZY_FR50"]
["加药间1噪音频率51","AR.ZZ_ZY_FR51"]
["加药间1噪音频率52","AR.ZZ_ZY_FR52"]
["加药间1噪音频率53","AR.ZZ_ZY_FR53"]
["加药间1噪音频率54","AR.ZZ_ZY_FR54"]
["加药间1噪音频率55","AR.ZZ_ZY_FR55"]
["加药间1噪音频率56","AR.ZZ_ZY_FR56"]
["加药间1噪音频率57","AR.ZZ_ZY_FR57"]
["加药间1噪音频率58","AR.ZZ_ZY_FR58"]
["加药间1噪音频率59","AR.ZZ_ZY_FR59"]
["加药间1噪音频率6","AR.ZZ_ZY_FR6"]
["加药间1噪音频率60","AR.ZZ_ZY_FR60"]
["加药间1噪音频率61","AR.ZZ_ZY_FR61"]
["加药间1噪音频率62","AR.ZZ_ZY_FR62"]
["加药间1噪音频率63","AR.ZZ_ZY_FR63"]
["加药间1噪音频率64","AR.ZZ_ZY_FR64"]
["加药间1噪音频率65","AR.ZZ_ZY_FR65"]
["加药间1噪音频率66","AR.ZZ_ZY_FR66"]
["加药间1噪音频率67","AR.ZZ_ZY_FR67"]
["加药间1噪音频率68","AR.ZZ_ZY_FR68"]
["加药间1噪音频率69","AR.ZZ_ZY_FR69"]
["加药间1噪音频率7","AR.ZZ_ZY_FR7"]
["加药间1噪音频率70","AR.ZZ_ZY_FR70"]
["加药间1噪音频率71","AR.ZZ_ZY_FR71"]
["加药间1噪音频率72","AR.ZZ_ZY_FR72"]
["加药间1噪音频率73","AR.ZZ_ZY_FR73"]
["加药间1噪音频率74","AR.ZZ_ZY_FR74"]
["加药间1噪音频率75","AR.ZZ_ZY_FR75"]
["加药间1噪音频率76","AR.ZZ_ZY_FR76"]
["加药间1噪音频率77","AR.ZZ_ZY_FR77"]
["加药间1噪音频率78","AR.ZZ_ZY_FR78"]
["加药间1噪音频率79","AR.ZZ_ZY_FR79"]
["加药间1噪音频率8","AR.ZZ_ZY_FR8"]
["加药间1噪音频率80","AR.ZZ_ZY_FR80"]
["加药间1噪音频率81","AR.ZZ_ZY_FR81"]
["加药间1噪音频率82","AR.ZZ_ZY_FR82"]
["加药间1噪音频率83","AR.ZZ_ZY_FR83"]
["加药间1噪音频率84","AR.ZZ_ZY_FR84"]
["加药间1噪音频率85","AR.ZZ_ZY_FR85"]
["加药间1噪音频率86","AR.ZZ_ZY_FR86"]
["加药间1噪音频率87","AR.ZZ_ZY_FR87"]
["加药间1噪音频率88","AR.ZZ_ZY_FR88"]
["加药间1噪音频率89","AR.ZZ_ZY_FR89"]
["加药间1噪音频率9","AR.ZZ_ZY_FR9"]
["加药间1噪音频率90","AR.ZZ_ZY_FR90"]
["加药间1噪音频率91","AR.ZZ_ZY_FR91"]
["加药间1噪音频率92","AR.ZZ_ZY_FR92"]
["加药间1噪音频率93","AR.ZZ_ZY_FR93"]
["加药间1噪音频率94","AR.ZZ_ZY_FR94"]
["加药间1噪音频率95","AR.ZZ_ZY_FR95"]
["加药间1噪音频率96","AR.ZZ_ZY_FR96"]
["加药间1噪音频率97","AR.ZZ_ZY_FR97"]
["加药间1噪音频率98","AR.ZZ_ZY_FR98"]
["加药间1噪音频率99","AR.ZZ_ZY_FR99"]
["加药间2噪音频率1","AR.ZZ_ZY2_FR1"]
["加药间2噪音频率10","AR.ZZ_ZY2_FR10"]
["加药间2噪音频率100","AR.ZZ_ZY2_FR100"]
["加药间2噪音频率101","AR.ZZ_ZY2_FR101"]
["加药间2噪音频率102","AR.ZZ_ZY2_FR102"]
["加药间2噪音频率103","AR.ZZ_ZY2_FR103"]
["加药间2噪音频率104","AR.ZZ_ZY2_FR104"]
["加药间2噪音频率105","AR.ZZ_ZY2_FR105"]
["加药间2噪音频率106","AR.ZZ_ZY2_FR106"]
["加药间2噪音频率107","AR.ZZ_ZY2_FR107"]
["加药间2噪音频率108","AR.ZZ_ZY2_FR108"]
["加药间2噪音频率109","AR.ZZ_ZY2_FR109"]
["加药间2噪音频率11","AR.ZZ_ZY2_FR11"]
["加药间2噪音频率110","AR.ZZ_ZY2_FR110"]
["加药间2噪音频率111","AR.ZZ_ZY2_FR111"]
["加药间2噪音频率112","AR.ZZ_ZY2_FR112"]
["加药间2噪音频率113","AR.ZZ_ZY2_FR113"]
["加药间2噪音频率114","AR.ZZ_ZY2_FR114"]
["加药间2噪音频率115","AR.ZZ_ZY2_FR115"]
["加药间2噪音频率116","AR.ZZ_ZY2_FR116"]
["加药间2噪音频率117","AR.ZZ_ZY2_FR117"]
["加药间2噪音频率118","AR.ZZ_ZY2_FR118"]
["加药间2噪音频率119","AR.ZZ_ZY2_FR119"]
["加药间2噪音频率12","AR.ZZ_ZY2_FR12"]
["加药间2噪音频率120","AR.ZZ_ZY2_FR120"]
["加药间2噪音频率121","AR.ZZ_ZY2_FR121"]
["加药间2噪音频率122","AR.ZZ_ZY2_FR122"]
["加药间2噪音频率123","AR.ZZ_ZY2_FR123"]
["加药间2噪音频率124","AR.ZZ_ZY2_FR124"]
["加药间2噪音频率125","AR.ZZ_ZY2_FR125"]
["加药间2噪音频率126","AR.ZZ_ZY2_FR126"]
["加药间2噪音频率127","AR.ZZ_ZY2_FR127"]
["加药间2噪音频率13","AR.ZZ_ZY2_FR13"]
["加药间2噪音频率14","AR.ZZ_ZY2_FR14"]
["加药间2噪音频率15","AR.ZZ_ZY2_FR15"]
["加药间2噪音频率16","AR.ZZ_ZY2_FR16"]
["加药间2噪音频率17","AR.ZZ_ZY2_FR17"]
["加药间2噪音频率18","AR.ZZ_ZY2_FR18"]
["加药间2噪音频率19","AR.ZZ_ZY2_FR19"]
["加药间2噪音频率2","AR.ZZ_ZY2_FR2"]
["加药间2噪音频率20","AR.ZZ_ZY2_FR20"]
["加药间2噪音频率21","AR.ZZ_ZY2_FR21"]
["加药间2噪音频率22","AR.ZZ_ZY2_FR22"]
["加药间2噪音频率23","AR.ZZ_ZY2_FR23"]
["加药间2噪音频率24","AR.ZZ_ZY2_FR24"]
["加药间2噪音频率25","AR.ZZ_ZY2_FR25"]
["加药间2噪音频率26","AR.ZZ_ZY2_FR26"]
["加药间2噪音频率27","AR.ZZ_ZY2_FR27"]
["加药间2噪音频率28","AR.ZZ_ZY2_FR28"]
["加药间2噪音频率29","AR.ZZ_ZY2_FR29"]
["加药间2噪音频率3","AR.ZZ_ZY2_FR3"]
["加药间2噪音频率30","AR.ZZ_ZY2_FR30"]
["加药间2噪音频率31","AR.ZZ_ZY2_FR31"]
["加药间2噪音频率32","AR.ZZ_ZY2_FR32"]
["加药间2噪音频率33","AR.ZZ_ZY2_FR33"]
["加药间2噪音频率34","AR.ZZ_ZY2_FR34"]
["加药间2噪音频率35","AR.ZZ_ZY2_FR35"]
["加药间2噪音频率36","AR.ZZ_ZY2_FR36"]
["加药间2噪音频率37","AR.ZZ_ZY2_FR37"]
["加药间2噪音频率38","AR.ZZ_ZY2_FR38"]
["加药间2噪音频率39","AR.ZZ_ZY2_FR39"]
["加药间2噪音频率4","AR.ZZ_ZY2_FR4"]
["加药间2噪音频率40","AR.ZZ_ZY2_FR40"]
["加药间2噪音频率41","AR.ZZ_ZY2_FR41"]
["加药间2噪音频率42","AR.ZZ_ZY2_FR42"]
["加药间2噪音频率43","AR.ZZ_ZY2_FR43"]
["加药间2噪音频率44","AR.ZZ_ZY2_FR44"]
["加药间2噪音频率45","AR.ZZ_ZY2_FR45"]
["加药间2噪音频率46","AR.ZZ_ZY2_FR46"]
["加药间2噪音频率47","AR.ZZ_ZY2_FR47"]
["加药间2噪音频率48","AR.ZZ_ZY2_FR48"]
["加药间2噪音频率49","AR.ZZ_ZY2_FR49"]
["加药间2噪音频率5","AR.ZZ_ZY2_FR5"]
["加药间2噪音频率50","AR.ZZ_ZY2_FR50"]
["加药间2噪音频率51","AR.ZZ_ZY2_FR51"]
["加药间2噪音频率52","AR.ZZ_ZY2_FR52"]
["加药间2噪音频率53","AR.ZZ_ZY2_FR53"]
["加药间2噪音频率54","AR.ZZ_ZY2_FR54"]
["加药间2噪音频率55","AR.ZZ_ZY2_FR55"]
["加药间2噪音频率56","AR.ZZ_ZY2_FR56"]
["加药间2噪音频率57","AR.ZZ_ZY2_FR57"]
["加药间2噪音频率58","AR.ZZ_ZY2_FR58"]
["加药间2噪音频率59","AR.ZZ_ZY2_FR59"]
["加药间2噪音频率6","AR.ZZ_ZY2_FR6"]
["加药间2噪音频率60","AR.ZZ_ZY2_FR60"]
["加药间2噪音频率61","AR.ZZ_ZY2_FR61"]
["加药间2噪音频率62","AR.ZZ_ZY2_FR62"]
["加药间2噪音频率63","AR.ZZ_ZY2_FR63"]
["加药间2噪音频率64","AR.ZZ_ZY2_FR64"]
["加药间2噪音频率65","AR.ZZ_ZY2_FR65"]
["加药间2噪音频率66","AR.ZZ_ZY2_FR66"]
["加药间2噪音频率67","AR.ZZ_ZY2_FR67"]
["加药间2噪音频率68","AR.ZZ_ZY2_FR68"]
["加药间2噪音频率69","AR.ZZ_ZY2_FR69"]
["加药间2噪音频率7","AR.ZZ_ZY2_FR7"]
["加药间2噪音频率70","AR.ZZ_ZY2_FR70"]
["加药间2噪音频率71","AR.ZZ_ZY2_FR71"]
["加药间2噪音频率72","AR.ZZ_ZY2_FR72"]
["加药间2噪音频率73","AR.ZZ_ZY2_FR73"]
["加药间2噪音频率74","AR.ZZ_ZY2_FR74"]
["加药间2噪音频率75","AR.ZZ_ZY2_FR75"]
["加药间2噪音频率76","AR.ZZ_ZY2_FR76"]
["加药间2噪音频率77","AR.ZZ_ZY2_FR77"]
["加药间2噪音频率78","AR.ZZ_ZY2_FR78"]
["加药间2噪音频率79","AR.ZZ_ZY2_FR79"]
["加药间2噪音频率8","AR.ZZ_ZY2_FR8"]
["加药间2噪音频率80","AR.ZZ_ZY2_FR80"]
["加药间2噪音频率81","AR.ZZ_ZY2_FR81"]
["加药间2噪音频率82","AR.ZZ_ZY2_FR82"]
["加药间2噪音频率83","AR.ZZ_ZY2_FR83"]
["加药间2噪音频率84","AR.ZZ_ZY2_FR84"]
["加药间2噪音频率85","AR.ZZ_ZY2_FR85"]
["加药间2噪音频率86","AR.ZZ_ZY2_FR86"]
["加药间2噪音频率87","AR.ZZ_ZY2_FR87"]
["加药间2噪音频率88","AR.ZZ_ZY2_FR88"]
["加药间2噪音频率89","AR.ZZ_ZY2_FR89"]
["加药间2噪音频率9","AR.ZZ_ZY2_FR9"]
["加药间2噪音频率90","AR.ZZ_ZY2_FR90"]
["加药间2噪音频率91","AR.ZZ_ZY2_FR91"]
["加药间2噪音频率92","AR.ZZ_ZY2_FR92"]
["加药间2噪音频率93","AR.ZZ_ZY2_FR93"]
["加药间2噪音频率94","AR.ZZ_ZY2_FR94"]
["加药间2噪音频率95","AR.ZZ_ZY2_FR95"]
["加药间2噪音频率96","AR.ZZ_ZY2_FR96"]
["加药间2噪音频率97","AR.ZZ_ZY2_FR97"]
["加药间2噪音频率98","AR.ZZ_ZY2_FR98"]
["加药间2噪音频率99","AR.ZZ_ZY2_FR99"]
["前端补水泵——自动启动","DR.QD_BSB_AUTOSTART"]
["前端补水泵—自动","DR.QD_BSB_BT_AUTO"]
["前端补水泵——故障复位","DR.QD_BSB_BT_RESET"]
["前端补水泵——启动","DR.QD_BSB_BT_START"]
["前端补水泵——停止","DR.QD_BSB_BT_STOP"]
["前端补水泵——故障","DR.QD_BSB_FAULT"]
["前端补水泵——输出","DR.QD_BSB_OUTPUT"]
["前端补水泵——ready","DR.QD_BSB_READY"]
["前端补水泵——远程","DR.QD_BSB_REM"]
["前端补水泵——运行反馈","DR.QD_BSB_RFB"]
["前端补水阀——自动","DR.QD_BSF_BT_AUTO"]
["前端补水阀——开阀","DR.QD_BSF_BT_CLOSE"]
["前端补水阀——关阀","DR.QD_BSF_BT_OPEN"]
["前端补水阀——故障复位","DR.QD_BSF_BT_RESET"]
["前端补水阀——关到位","DR.QD_BSF_CFB"]
["前端补水阀——关ing","DR.QD_BSF_CING"]
["前端补水阀——自动关","DR.QD_BSF_CLOSEAUTO"]
["前端补水阀——故障 ","DR.QD_BSF_ERR"]
["前端补水阀——总故障 ","DR.QD_BSF_ERRT"]
["前端补水阀开到位","DR.QD_BSF_OFB"]
["前端补水阀打开中","DR.QD_BSF_OING"]
["前端补水阀自动打开","DR.QD_BSF_OPENAUTO"]
["前端补水阀关闭","DR.QD_BSF_OUT_CLOSE"]
["前端补水阀打开","DR.QD_BSF_OUT_OPEN"]
["前端补水阀准备好","DR.QD_BSF_READY"]
["前端补水阀远程","DR.QD_BSF_REM"]
["RO产水PH PID 调节选择按钮","DR.QD_LD_BT_ROCSPH_PID"]
["RO进水ORP PID 调节选择按钮","DR.QD_LD_BT_ROHYJ_PID"]
["前端排气阀手自动","DR.QD_PQF_BT_AUTO"]
["前端排气阀手动关","DR.QD_PQF_BT_CLOSE"]
["前端排气阀手动开","DR.QD_PQF_BT_OPEN"]
["前端排气阀故障复位","DR.QD_PQF_BT_RESET"]
["前端排气阀关到位","DR.QD_PQF_CFB"]
["前端排气阀关闭中","DR.QD_PQF_CING"]
["前端排气阀自动关闭","DR.QD_PQF_CLOSEAUTO"]
["前端排气阀故障","DR.QD_PQF_ERR"]
["前端排气阀总故障","DR.QD_PQF_ERRT"]
["前端排气阀开到位","DR.QD_PQF_OFB"]
["前端排气阀打开中","DR.QD_PQF_OING"]
["前端排气阀自动打开","DR.QD_PQF_OPENAUTO"]
["前端排气阀关闭","DR.QD_PQF_OUT_CLOSE"]
["前端排气阀打开","DR.QD_PQF_OUT_OPEN"]
["前端排气阀准备好","DR.QD_PQF_OUT_READY"]
["前端排气阀远程","DR.QD_PQF_REM"]
["前端破真空阀手自动","DR.QD_PZKF_BT_AUTO"]
["前端破真空阀手动关","DR.QD_PZKF_BT_CLOSE"]
["前端破真空阀手动开","DR.QD_PZKF_BT_OPEN"]
["前端破真空阀故障复位","DR.QD_PZKF_BT_RESET"]
["前端破真空阀关到位","DR.QD_PZKF_CFB"]
["前端破真空阀关闭中","DR.QD_PZKF_CING"]
["前端破真空阀自动关闭","DR.QD_PZKF_CLOSEAUTO"]
["前端破真空阀故障","DR.QD_PZKF_ERR"]
["前端破真空阀总故障","DR.QD_PZKF_ERRT"]
["前端破真空阀开到位","DR.QD_PZKF_OFB"]
["前端破真空阀打开中","DR.QD_PZKF_OING"]
["前端破真空阀自动打开","DR.QD_PZKF_OPENAUTO"]
["前端破真空阀关闭","DR.QD_PZKF_OUT_CLOSE"]
["前端破真空阀打开","DR.QD_PZKF_OUT_OPEN"]
["前端破真空阀准备好","DR.QD_PZKF_OUT_READY"]
["前端破真空阀远程","DR.QD_PZKF_REM"]
["前端补水液位开关LS_00","DR.QD_QT_44_0"]
["Flag_QD排气执行中","DR.QD_QT_44_1"]
["Flag_QD排气中，超滤不允许","DR.QD_QT_44_2"]
["故障_引水装置补水超时","DR.QD_QT_44_3"]
["前端排气——备用","DR.QD_QT_44_4"]
["前端排气——备用","DR.QD_QT_44_5"]
["前端排气——备用","DR.QD_QT_44_6"]
["前端排气——备用","DR.QD_QT_44_7"]
["用户华晟-流量计温度","AI.WG_FLOW_HS2_00"]
["用户华晟-流量计压力","AI.WG_FLOW_HS2_01"]
["用户华晟-补偿前流量","AI.WG_FLOW_HS2_02"]
["用户华晟-补偿后流量","AI.WG_FLOW_HS2_03"]
["用户华晟-累计流量","AI.WG_FLOW_HS2_04"]
["用户芯动-流量计温度","AI.WG_FLOW_XD_00"]
["用户芯动-流量计压力","AI.WG_FLOW_XD_01"]
["用户芯动-补偿前流量","AI.WG_FLOW_XD_02"]
["用户芯动-补偿后流量","AI.WG_FLOW_XD_03"]
["用户芯动-累计流量","AI.WG_FLOW_XD_04"]
["前端补水泵","AR.QD_BSB_FRE_FB"]
["前端补水泵","AR.QD_BSB_FRESET"]
["前端补水泵","AR.QD_BSB_RUNTIME"]
["RO产水加碱频率1套","AR.QD_LD_R164"]
["RO产水加碱频率2套","AR.QD_LD_R168"]
["RO产水加碱频率备1","AR.QD_LD_R172"]
["RO产水加碱频率备2","AR.QD_LD_R176"]
["前端补水参照时间","AR.QD_QT_BSTIMESET"]
["前端液位触发后延时补水时间设置","AR.QD_QT_LSTIMEDELAYSET"]
["前端补水计时","AR.QD_QT_TIMEADD"]
["前端液位触发后延时补水计时","AR.QD_QT_TIMEDELAYADD"]
["备","AR.UF_LD_R152"]
["备","AR.UF_LD_R156"]
["备","AR.UF_LD_R182"]
["极电外供水流量计备用1","AI.WG_FLOW_JD_00"]
["极电外供水流量计备用2","AI.WG_FLOW_JD_01"]
["极电外供水流量计备用3","AI.WG_FLOW_JD_02"]
["极电外供水流量计备用4","AI.WG_FLOW_JD_03"]
["极点总供水流量计","AI.WG_FLOW_JD_04"]
["F1空调地址设定","AR.ZZ_AC1C_AD"]
["F1空调波特率设定","AR.ZZ_AC1C_BD"]
["F1空调风向设定","AR.ZZ_AC1C_DIR"]
["F1空调风速设定","AR.ZZ_AC1C_F"]
["F1空调开关模式","AR.ZZ_AC1C_MOD"]
["F1空调开关操作","AR.ZZ_AC1C_ON/OFF"]
["F1空调温度设定","AR.ZZ_AC1C_T"]
["F1空调地址","AI.ZZ_AC1S_ADR"]
["F1空调波特率","AI.ZZ_AC1S_BD"]
["F1空调红外状态","AI.ZZ_AC1S_IR"]
["F1空调开关状态","AI.ZZ_AC1S_ON/OFF"]
["F1空调湿度","AI.ZZ_AC1S_RH"]
["F1空调温度","AI.ZZ_AC1S_T"]
["F1空调运行状态检测信号类型","AI.ZZ_AC1S_TYPE"]
["F1空调运行状态检测信号值","AI.ZZ_AC1S_VALUE"]
["F2电控柜侧空调地址设定","AR.ZZ_AC2C_AD"]
["F2电控柜侧空调波特率设定","AR.ZZ_AC2C_BD"]
["F2电控柜侧空调风向设定","AR.ZZ_AC2C_DIR"]
["F2电控柜侧空调风速设定","AR.ZZ_AC2C_F"]
["F2电控柜侧空调开关模式","AR.ZZ_AC2C_MOD"]
["F2电控柜侧空调开关操作","AR.ZZ_AC2C_ON/OFF"]
["F2电控柜侧空调温度设定","AR.ZZ_AC2C_T"]
["F2电控柜侧空调地址","AI.ZZ_AC2S_ADR"]
["F2电控柜侧空调波特率","AI.ZZ_AC2S_BD"]
["F2电控柜侧空调红外状态","AI.ZZ_AC2S_IR"]
["F2电控柜侧空调开关状态","AI.ZZ_AC2S_ON/OFF"]
["F2电控柜侧空调湿度","AI.ZZ_AC2S_RH"]
["F2电控柜侧空调温度","AI.ZZ_AC2S_T"]
["F2电控柜侧空调运行状态检测信号类型","AI.ZZ_AC2S_TYPE"]
["F2电控柜侧空调运行状态检测信号值","AI.ZZ_AC2S_VALUE"]
["F2空调地址设定","AR.ZZ_AC3C_AD"]
["F2空调波特率设定","AR.ZZ_AC3C_BD"]
["F2空调风向设定","AR.ZZ_AC3C_DIR"]
["F2空调风速设定","AR.ZZ_AC3C_F"]
["F2空调开关模式","AR.ZZ_AC3C_MOD"]
["F2空调开关操作","AR.ZZ_AC3C_ON/OFF"]
["F2空调温度设定","AR.ZZ_AC3C_T"]
["F2空调地址","AI.ZZ_AC3S_ADR"]
["F2空调波特率","AI.ZZ_AC3S_BD"]
["F2空调红外状态","AI.ZZ_AC3S_IR"]
["F2空调开关状态","AI.ZZ_AC3S_ON/OFF"]
["F2空调湿度","AI.ZZ_AC3S_RH"]
["F2空调温度","AI.ZZ_AC3S_T"]
["F2空调运行状态检测信号类型","AI.ZZ_AC3S_TYPE"]
["F2空调运行状态检测信号值","AI.ZZ_AC3S_VALUE"]
["ORP-X0","AR.ROHYJ_ARR_X_ORP0"]
["ORP-X1","AR.ROHYJ_ARR_X_ORP1"]
["ORP-X10","AR.ROHYJ_ARR_X_ORP10"]
["ORP-X11","AR.ROHYJ_ARR_X_ORP11"]
["ORP-X12","AR.ROHYJ_ARR_X_ORP12"]
["ORP-X13","AR.ROHYJ_ARR_X_ORP13"]
["ORP-X14","AR.ROHYJ_ARR_X_ORP14"]
["ORP-X15","AR.ROHYJ_ARR_X_ORP15"]
["ORP-X2","AR.ROHYJ_ARR_X_ORP2"]
["ORP-X3","AR.ROHYJ_ARR_X_ORP3"]
["ORP-X4","AR.ROHYJ_ARR_X_ORP4"]
["ORP-X5","AR.ROHYJ_ARR_X_ORP5"]
["ORP-X6","AR.ROHYJ_ARR_X_ORP6"]
["ORP-X7","AR.ROHYJ_ARR_X_ORP7"]
["ORP-X8","AR.ROHYJ_ARR_X_ORP8"]
["ORP-X9","AR.ROHYJ_ARR_X_ORP9"]
["HYJ—Y——0","AR.ROHYJ_ARR_Y1_HYJ0"]
["HYJ—Y——1","AR.ROHYJ_ARR_Y1_HYJ1"]
["HYJ—Y——10","AR.ROHYJ_ARR_Y1_HYJ10"]
["HYJ—Y——11","AR.ROHYJ_ARR_Y1_HYJ11"]
["HYJ—Y——12","AR.ROHYJ_ARR_Y1_HYJ12"]
["HYJ—Y——13","AR.ROHYJ_ARR_Y1_HYJ13"]
["HYJ—Y——14","AR.ROHYJ_ARR_Y1_HYJ14"]
["HYJ—Y——15","AR.ROHYJ_ARR_Y1_HYJ15"]
["HYJ—Y——2","AR.ROHYJ_ARR_Y1_HYJ2"]
["HYJ—Y——3","AR.ROHYJ_ARR_Y1_HYJ3"]
["HYJ—Y——4","AR.ROHYJ_ARR_Y1_HYJ4"]
["HYJ—Y——5","AR.ROHYJ_ARR_Y1_HYJ5"]
["HYJ—Y——6","AR.ROHYJ_ARR_Y1_HYJ6"]
["HYJ—Y——7","AR.ROHYJ_ARR_Y1_HYJ7"]
["HYJ—Y——8","AR.ROHYJ_ARR_Y1_HYJ8"]
["HYJ—Y——9","AR.ROHYJ_ARR_Y1_HYJ9"]
["还原剂额定加药量","AR.ROHYJ_HYJJYBRATEDDO"]
["HYJ—1台泵需要量","AR.ROHYJ_JS_HY1P_NEED"]
["HYJ—原药需要量","AR.ROHYJ_JS_HYJ100_NEED"]
["还原剂药液流量","AR.ROHYJ_JS_HYJFLOWNEED"]
["进水流量修正系数","AR.ROHYJ_K_FLOWWATER"]
["ORP中间值","AR.ROHYJ_ORP_MID"]
["ORP实验值","AR.ROHYJ_ORP_SYZ"]
["还原剂泵数量","AR.ROHYJ_SET_BASICHYJ_N"]
["进水流量修正后值","AR.ROHYJ_SSD_FLOWW_XZ"]
["进水流量","AR.ROHYJ_SSD_FLOWWATER"]
["还原剂浓度","AR.ROHYJ_SSD_HYJ_ND"]
["还原剂流量计（如有）","AR.ROHYJ_SSD_HYJND_FLOW"]
["还原剂Y1","AR.ROHYJ_Y1_OUT"]
["加药量标定指标—0","DR.ROHYJ_ARR_FLAG_X0"]
["加药量标定指标—1","DR.ROHYJ_ARR_FLAG_X1"]
["加药量标定指标—10","DR.ROHYJ_ARR_FLAG_X10"]
["加药量标定指标—11","DR.ROHYJ_ARR_FLAG_X11"]
["加药量标定指标—12","DR.ROHYJ_ARR_FLAG_X12"]
["加药量标定指标—13","DR.ROHYJ_ARR_FLAG_X13"]
["加药量标定指标—14","DR.ROHYJ_ARR_FLAG_X14"]
["加药量标定指标—15","DR.ROHYJ_ARR_FLAG_X15"]
["加药量标定指标—2","DR.ROHYJ_ARR_FLAG_X2"]
["加药量标定指标—3","DR.ROHYJ_ARR_FLAG_X3"]
["加药量标定指标—4","DR.ROHYJ_ARR_FLAG_X4"]
["加药量标定指标—5","DR.ROHYJ_ARR_FLAG_X5"]
["加药量标定指标—6","DR.ROHYJ_ARR_FLAG_X6"]
["加药量标定指标—7","DR.ROHYJ_ARR_FLAG_X7"]
["加药量标定指标—8","DR.ROHYJ_ARR_FLAG_X8"]
["加药量标定指标—9","DR.ROHYJ_ARR_FLAG_X9"]
["按钮还原剂—选择实际值","DR.ROHYJ_BT_HYJ0"]
["按钮-还原剂ORP联动 —投用","DR.ROHYJ_BT_HYJ1"]
["华盛瞬时流量","AR.WGLL_HS_SSLL"]
["华盛流体速度","AR.WGLL_HS_LTSD"]
["华盛累计流量","AR.WGLL_HS_LJLL"]
["芯动补偿前流量","AR.WGLL_XD_BCQLL"]
["芯动补偿后流量","AR.WGLL_XD_BCHLL"]
["芯动累计流量","AR.WGLL_XD_LJLL"]
["极光累计流量","AR.WGLL_JG_LJLL"]
["反渗透回收率","ROHSL"]