{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":2249,"n_cols":2,"rows_kept":2249,"cut":false,"hidden":false,"merged":[]}
["item_alias","item_name"]
["UF步序和产水时长","UF_DB"]
["RO步序和产水时长","RO_DB"]
["进水量","water_in"]
["外供水流量","water_out"]
["UF反洗前压差","UF_BW_Before_TMP"]
["UF反洗后压差","UF_BW_After_TMP"]
["加药进线电流1A","JY_JXDL_1A"]
["加药进线电流1B","JY_JXDL_1B"]
["加药进线电流1C","JY_JXDL_1C"]
["RO进线电流1A","RO_JXDL_1A"]
["RO进线电流1B","RO_JXDL_1B"]
["RO进线电流1C","RO_JXDL_1C"]
["UF进线电流1A","UF_JXDL_1A"]
["UF进线电流1B","UF_JXDL_1B"]
["UF进线电流1C","UF_JXDL_1C"]
["测试故障报警点位，请忽略","CSGZDW"]
["UF运行过滤压差","UF_FF_TMP"]
["空压机压变1高报警","ns=6;s=AI_JYAIRYL1_H"]
["空压机压变1高高报警","ns=6;s=AI_JYAIRYL1_HH"]
["空压机压变1低报警","ns=6;s=AI_JYAIRYL1_L"]
["空压机压变1低低报警","ns=6;s=AI_JYAIRYL1_LL"]
["空压机压变2高报警","ns=6;s=AI_JYAIRYL2_H"]
["空压机压变2高高报警","ns=6;s=AI_JYAIRYL2_HH"]
["空压机压变2低报警","ns=6;s=AI_JYAIRYL2_L"]
["空压机压变2低低报警","ns=6;s=AI_JYAIRYL2_LL"]
["备用3高报警","ns=6;s=AI_JYBY3_H"]
["备用3高高报警","ns=6;s=AI_JYBY3_HH"]
["备用3低报警","ns=6;s=AI_JYBY3_L"]
["备用3低低报警","ns=6;s=AI_JYBY3_LL"]
["备用4高报警","ns=6;s=AI_JYBY4_H"]
["备用4高高报警","ns=6;s=AI_JYBY4_HH"]
["备用4低报警","ns=6;s=AI_JYBY4_L"]
["备用4低低报警","ns=6;s=AI_JYBY4_LL"]
["备用5高报警","ns=6;s=AI_JYBY5_H"]
["备用5高高报警","ns=6;s=AI_JYBY5_HH"]
["备用5低报警","ns=6;s=AI_JYBY5_L"]
["备用5低低报警","ns=6;s=AI_JYBY5_LL"]
["CIP PH高报警","ns=6;s=AI_JYCIPPH_H"]
["CIP PH高高报警","ns=6;s=AI_JYCIPPH_HH"]
["CIP PH低报警","ns=6;s=AI_JYCIPPH_L"]
["CIP PH低低报警","ns=6;s=AI_JYCIPPH_LL"]
["次钠液位高报警","ns=6;s=AI_JYCNYW_H"]
["次钠液位高高报警","ns=6;s=AI_JYCNYW_HH"]
["次钠液位低报警","ns=6;s=AI_JYCNYW_L"]
["次钠液位低低报警","ns=6;s=AI_JYCNYW_LL"]
["产水电导高报警","ns=6;s=AI_JYCSDD_H"]
["产水电导高高报警","ns=6;s=AI_JYCSDD_HH"]
["产水电导低报警","ns=6;s=AI_JYCSDD_L"]
["产水电导低低报警","ns=6;s=AI_JYCSDD_LL"]
["产水PH高报警","ns=6;s=AI_JYCSPH_H"]
["产水PH高高报警","ns=6;s=AI_JYCSPH_HH"]
["产水PH低报警","ns=6;s=AI_JYCSPH_L"]
["产水PH低低报警","ns=6;s=AI_JYCSPH_LL"]
["产水温度高报警","ns=6;s=AI_JYCSWD_H"]
["产水温度高高报警","ns=6;s=AI_JYCSWD_HH"]
["产水温度低报警","ns=6;s=AI_JYCSWD_L"]
["产水温度低低报警","ns=6;s=AI_JYCSWD_LL"]
["产水压力高报警","ns=6;s=AI_JYCSYL_H"]
["产水压力高高报警","ns=6;s=AI_JYCSYL_HH"]
["产水压力低报警","ns=6;s=AI_JYCSYL_L"]
["产水压力低低报警","ns=6;s=AI_JYCSYL_LL"]
["还原剂液位高报警","ns=6;s=AI_JYHYJYW_H"]
["还原剂液位高高报警","ns=6;s=AI_JYHYJYW_HH"]
["还原剂液位低报警","ns=6;s=AI_JYHYJYW_L"]
["还原剂液位低低报警","ns=6;s=AI_JYHYJYW_LL"]
["高级生物进水流量计高报警","ns=6;s=AI_JYJSLL1_H"]
["高级生物进水流量计高高报警","ns=6;s=AI_JYJSLL1_HH"]
["高级生物进水流量计低报警","ns=6;s=AI_JYJSLL1_L"]
["高级生物进水流量计低低报警","ns=6;s=AI_JYJSLL1_LL"]
["Y2B进水流量计高报警","ns=6;s=AI_JYJSLL2_H"]
["Y2B进水流量计高高报警","ns=6;s=AI_JYJSLL2_HH"]
["Y2B进水流量计低报警","ns=6;s=AI_JYJSLL2_L"]
["Y2B进水流量计低低报警","ns=6;s=AI_JYJSLL2_LL"]
["碱液位高报警","ns=6;s=AI_JYJYW_H"]
["碱液位高高报警","ns=6;s=AI_JYJYW_HH"]
["碱液位低报警","ns=6;s=AI_JYJYW_L"]
["碱液位低低报警","ns=6;s=AI_JYJYW_LL"]
["浓水流量计高报警","ns=6;s=AI_JYNS_H"]
["浓水流量计高高报警","ns=6;s=AI_JYNS_HH"]
["浓水流量计低报警","ns=6;s=AI_JYNS_L"]
["浓水流量计低低报警","ns=6;s=AI_JYNS_LL"]
["清洗水箱液位高报警","ns=6;s=AI_JYQXSXYW_H"]
["清洗水箱液位高高报警","ns=6;s=AI_JYQXSXYW_HH"]
["清洗水箱液位低报警","ns=6;s=AI_JYQXSXYW_L"]
["清洗水箱液位低低报警","ns=6;s=AI_JYQXSXYW_LL"]
["RO产水液位高报警","ns=6;s=AI_JYROCSYW_H"]
["RO产水液位高高报警","ns=6;s=AI_JYROCSYW_HH"]
["RO产水液位低报警","ns=6;s=AI_JYROCSYW_L"]
["RO产水液位低低报警","ns=6;s=AI_JYROCSYW_LL"]
["杀菌剂液位高报警","ns=6;s=AI_JYSJJYW_H"]
["杀菌剂液位高高报警","ns=6;s=AI_JYSJJYW_HH"]
["杀菌剂液位低报警","ns=6;s=AI_JYSJJYW_L"]
["杀菌剂液位低低报警","ns=6;s=AI_JYSJJYW_LL"]
["酸液位高报警","ns=6;s=AI_JYSYW_H"]
["酸液位高高报警","ns=6;s=AI_JYSYW_HH"]
["酸液位低报警","ns=6;s=AI_JYSYW_L"]
["酸液位低低报警","ns=6;s=AI_JYSYW_LL"]
["UF产水液位高报警","ns=6;s=AI_JYUFCSYW_H"]
["UF产水液位高高报警","ns=6;s=AI_JYUFCSYW_HH"]
["UF产水液位低报警","ns=6;s=AI_JYUFCSYW_L"]
["UF产水液位低低报警","ns=6;s=AI_JYUFCSYW_LL"]
["超滤提升泵液位高报警","ns=6;s=AI_JYUFTSBYW_H"]
["超滤提升泵液位高高报警","ns=6;s=AI_JYUFTSBYW_HH"]
["超滤提升泵液位低报警","ns=6;s=AI_JYUFTSBYW_L"]
["超滤提升泵液位低低报警","ns=6;s=AI_JYUFTSBYW_LL"]
["阻垢剂液位高报警","ns=6;s=AI_JYZGJYW_H"]
["阻垢剂液位高高报警","ns=6;s=AI_JYZGJYW_HH"]
["阻垢剂液位低报警","ns=6;s=AI_JYZGJYW_L"]
["阻垢剂液位低低报警","ns=6;s=AI_JYZGJYW_LL"]
["RO备用高报警","ns=6;s=AI_ROBY_H"]
["RO备用高高报警","ns=6;s=AI_ROBY_HH"]
["RO备用低报警","ns=6;s=AI_ROBY_L"]
["RO备用低低报警","ns=6;s=AI_ROBY_LL"]
["RO产水电导高报警","ns=6;s=AI_ROCSDD_H"]
["RO产水电导高高报警","ns=6;s=AI_ROCSDD_HH"]
["RO产水电导低报警","ns=6;s=AI_ROCSDD_L"]
["RO产水电导低低报警","ns=6;s=AI_ROCSDD_LL"]
["RO产水压力高报警","ns=6;s=AI_ROCSYL_H"]
["RO产水压力高高报警","ns=6;s=AI_ROCSYL_HH"]
["RO产水压力低报警","ns=6;s=AI_ROCSYL_L"]
["RO产水压力低低报警","ns=6;s=AI_ROCSYL_LL"]
["RO段间泵进口压力高报警","ns=6;s=AI_RODJJKYL_H"]
["RO段间泵进口压力高高报警","ns=6;s=AI_RODJJKYL_HH"]
["RO段间泵进口压力低报警","ns=6;s=AI_RODJJKYL_L"]
["RO段间泵进口压力低低报警","ns=6;s=AI_RODJJKYL_LL"]
["RO段间压力高报警","ns=6;s=AI_RODJYL_H"]
["RO段间压力高高报警","ns=6;s=AI_RODJYL_HH"]
["RO段间压力低报警","ns=6;s=AI_RODJYL_L"]
["RO段间压力低低报警","ns=6;s=AI_RODJYL_LL"]
["RO进水电导高报警","ns=6;s=AI_ROJSDD_H"]
["RO进水电导高高报警","ns=6;s=AI_ROJSDD_HH"]
["RO进水电导低报警","ns=6;s=AI_ROJSDD_L"]
["RO进水电导低低报警","ns=6;s=AI_ROJSDD_LL"]
["RO进水ORP高报警","ns=6;s=AI_ROJSORP_H"]
["RO进水ORP高高报警","ns=6;s=AI_ROJSORP_HH"]
["RO进水ORP低报警","ns=6;s=AI_ROJSORP_L"]
["RO进水ORP低低报警","ns=6;s=AI_ROJSORP_LL"]
["RO进水PH高报警","ns=6;s=AI_ROJSPH_H"]
["RO进水PH高高报警","ns=6;s=AI_ROJSPH_HH"]
["RO进水PH低报警","ns=6;s=AI_ROJSPH_L"]
["RO进水PH低低报警","ns=6;s=AI_ROJSPH_LL"]
["RO进水压力高报警","ns=6;s=AI_ROJSYL_H"]
["RO进水压力高高报警","ns=6;s=AI_ROJSYL_HH"]
["RO进水压力低报警","ns=6;s=AI_ROJSYL_L"]
["RO进水压力低低报警","ns=6;s=AI_ROJSYL_LL"]
["RO浓水压力高报警","ns=6;s=AI_RONSYL_H"]
["RO浓水压力高高报警","ns=6;s=AI_RONSYL_HH"]
["RO浓水压力低报警","ns=6;s=AI_RONSYL_L"]
["RO浓水压力低低报警","ns=6;s=AI_RONSYL_LL"]
["超滤空气流量高报警","ns=6;s=AI_UFAIR_H"]
["超滤空气流量高高报警","ns=6;s=AI_UFAIR_HH"]
["超滤空气流量低报警","ns=6;s=AI_UFAIR_L"]
["超滤空气流量低低报警","ns=6;s=AI_UFAIR_LL"]
["超滤备用高报警","ns=6;s=AI_UFBY1_H"]
["超滤备用高高报警","ns=6;s=AI_UFBY1_HH"]
["超滤备用低报警","ns=6;s=AI_UFBY1_L"]
["超滤备用低低报警","ns=6;s=AI_UFBY1_LL"]
["超滤备用2高报警","ns=6;s=AI_UFBY2_H"]
["超滤备用2高高报警","ns=6;s=AI_UFBY2_HH"]
["超滤备用2低报警","ns=6;s=AI_UFBY2_L"]
["超滤备用2低低报警","ns=6;s=AI_UFBY2_LL"]
["超滤备用3高报警","ns=6;s=AI_UFBY3_H"]
["超滤备用3高高报警","ns=6;s=AI_UFBY3_HH"]
["超滤备用3低报警","ns=6;s=AI_UFBY3_L"]
["超滤备用3低低报警","ns=6;s=AI_UFBY3_LL"]
["超滤备用4高报警","ns=6;s=AI_UFBY4_H"]
["超滤备用4高高报警","ns=6;s=AI_UFBY4_HH"]
["超滤备用4低报警","ns=6;s=AI_UFBY4_L"]
["超滤备用4低低报警","ns=6;s=AI_UFBY4_LL"]
["超滤进水ORP高报警","ns=6;s=AI_UFJSORP_H"]
["超滤进水ORP高高报警","ns=6;s=AI_UFJSORP_HH"]
["超滤进水ORP低报警","ns=6;s=AI_UFJSORP_L"]
["超滤进水ORP低低报警","ns=6;s=AI_UFJSORP_LL"]
["超滤进水PH高报警","ns=6;s=AI_UFJSPH_H"]
["超滤进水PH高高报警","ns=6;s=AI_UFJSPH_HH"]
["超滤进水PH低报警","ns=6;s=AI_UFJSPH_L"]
["超滤进水PH低低报警","ns=6;s=AI_UFJSPH_LL"]
["超滤进水液位高报警","ns=6;s=AI_UFJSYW_H"]
["超滤进水液位高高报警","ns=6;s=AI_UFJSYW_HH"]
["超滤进水液位低报警","ns=6;s=AI_UFJSYW_L"]
["超滤进水液位低低报警","ns=6;s=AI_UFJSYW_LL"]
["超滤进水浊度高报警","ns=6;s=AI_UFJSZD_H"]
["超滤进水浊度高高报警","ns=6;s=AI_UFJSZD_HH"]
["超滤进水浊度低报警","ns=6;s=AI_UFJSZD_L"]
["超滤进水浊度低低报警","ns=6;s=AI_UFJSZD_LL"]
["超滤膜堆液位高报警","ns=6;s=AI_UFMDYW_H"]
["超滤膜堆液位高高报警","ns=6;s=AI_UFMDYW_HH"]
["超滤膜堆液位低报警","ns=6;s=AI_UFMDYW_L"]
["超滤膜堆液位低低报警","ns=6;s=AI_UFMDYW_LL"]
["超滤真空管液位高报警","ns=6;s=AI_UFZKGYW_H"]
["超滤真空管液位高高报警","ns=6;s=AI_UFZKGYW_HH"]
["超滤真空管液位低报警","ns=6;s=AI_UFZKGYW_L"]
["超滤真空管液位低低报警","ns=6;s=AI_UFZKGYW_LL"]
["中和水箱高报警","ns=6;s=ALARM_ZHSX_H"]
["中和水箱超高报警","ns=6;s=ALARM_ZHSX_HH"]
["中和水箱低报警","ns=6;s=ALARM_ZHSX_L"]
["中和水箱超低报警","ns=6;s=ALARM_ZHSX_LL"]
["APPLY_13","ns=6;s=APPLY_13"]
["APPLY_14","ns=6;s=APPLY_14"]
["APPLY_15","ns=6;s=APPLY_15"]
["Apply_9","ns=6;s=APPLY_9"]
["Apply_BW_入栈","ns=6;s=APPLY_BW_PUSH"]
["Apply_BWCEB_出栈","ns=6;s=APPLY_BWCEB_POP"]
["Apply_CEB_入栈","ns=6;s=APPLY_CEB_PUSH"]
["Apply_次钠加药","ns=6;s=APPLY_CNJY"]
["Apply反洗泵BW","ns=6;s=APPLY_FXB_BW"]
["Apply反洗泵CEB","ns=6;s=APPLY_FXB_CEB"]
["Apply公共阀BW阀","ns=6;s=APPLY_GGF_BWV"]
["Apply公共阀CEB阀","ns=6;s=APPLY_GGF_CEBV"]
["Apply供水泵FW","ns=6;s=APPLY_GSB_FW"]
["Apply_碱加药","ns=6;s=APPLY_JJY"]
["Apply_PAC加药","ns=6;s=APPLY_PACJY"]
["Apply_酸加药","ns=6;s=APPLY_SJY"]
["Apply提升泵1","ns=6;s=APPLY_TSB1"]
["Apply提升泵2","ns=6;s=APPLY_TSB2"]
["药剂残留","ns=6;s=DRUG_ERR"]
["ERR_5","ns=6;s=ERR_5"]
["ERR_6","ns=6;s=ERR_6"]
["ERR_7","ns=6;s=ERR_7"]
["FLAG_17","ns=6;s=FLAG_17"]
["FLAG_18","ns=6;s=FLAG_18"]
["FLAG_19","ns=6;s=FLAG_19"]
["自动启动标志","ns=6;s=FLAG_AUTOSTART"]
["反洗CEB阀准备好","ns=6;s=FLAG_BWCEB_V_READY"]
["flag_CEB冲洗ing","ns=6;s=FLAG_CEB_CX_ING"]
["flag_CEBing","ns=6;s=FLAG_CEB_ING"]
["flag_CEB加药ing","ns=6;s=FLAG_CEB_JY_ING"]
["flag_冲水过滤ing","ns=6;s=FLAG_CSGL_ING"]
["flag_反洗ing","ns=6;s=FLAG_FX_ING"]
["反洗准备好","ns=6;s=FLAG_FX_READY"]
["flag_过滤end","ns=6;s=FLAG_GL_END"]
["flag_过滤ing","ns=6;s=FLAG_GL_ING"]
["过滤准备好","ns=6;s=FLAG_GL_READY"]
["盐酸准备好","ns=6;s=FLAG_HCL_READY"]
["碱洗准备好","ns=6;s=FLAG_JX_READY"]
["产水池A连锁","ns=6;s=FLAG_LS_CSCA"]
["产水池B连锁","ns=6;s=FLAG_LS_CSCB"]
["进水池A连锁","ns=6;s=FLAG_LS_JSCA"]
["进水池B连锁","ns=6;s=FLAG_LS_JSCB"]
["反洗电机洗准备好","ns=6;s=FLAG_M_BW_READY"]
["过滤电机准备好","ns=6;s=FLAG_M_GL_READY"]
["flag_膜内有药ing","ns=6;s=FLAG_MNYY_ING"]
["PAC洗准备好","ns=6;s=FLAG_PAC_READY"]
["气洗准备好","ns=6;s=FLAG_QX_READY"]
["水射器允许","ns=6;s=FLAG_SSQ_ALLOW"]
["酸洗准备好","ns=6;s=FLAG_SX_READY"]
["flag_全自动Ready","ns=6;s=FLAG_TY_READT"]
["阀门准备好","ns=6;s=FLAG_V_READY"]
["水洗准备好","ns=6;s=FLAG_WW_READY"]
["还原剂搅拌器自动启动","ns=6;s=JBQ_JY_HYJ_AUTOSTART"]
["还原剂搅拌器手自动","ns=6;s=JBQ_JY_HYJ_BT_AUTO"]
["还原剂搅拌器故障复位","ns=6;s=JBQ_JY_HYJ_BT_RESET"]
["还原剂搅拌器手动启动","ns=6;s=JBQ_JY_HYJ_BT_START"]
["还原剂搅拌器手动停止","ns=6;s=JBQ_JY_HYJ_BT_STOP"]
["还原剂搅拌器故障","ns=6;s=JBQ_JY_HYJ_FAULT"]
["还原剂搅拌器启动","ns=6;s=JBQ_JY_HYJ_OUTPUT"]
["还原剂搅拌器启动准备好","ns=6;s=JBQ_JY_HYJ_READY"]
["还原剂搅拌器泵远程","ns=6;s=JBQ_JY_HYJ_REM"]
["还原剂搅拌器运行","ns=6;s=JBQ_JY_HYJ_RFB"]
["加热器1手自动","ns=6;s=JBQ_JY_JRQ1_BT_AUTO"]
["加热器1故障复位","ns=6;s=JBQ_JY_JRQ1_BT_RESET"]
["加热器1手动启动","ns=6;s=JBQ_JY_JRQ1_BT_START"]
["加热器1手动停止","ns=6;s=JBQ_JY_JRQ1_BT_STOP"]
["加热器1故障","ns=6;s=JBQ_JY_JRQ1_FAULT"]
["加热器1启动","ns=6;s=JBQ_JY_JRQ1_OUTPUT"]
["加热器1启动准备好","ns=6;s=JBQ_JY_JRQ1_READY"]
["加热器1泵远程","ns=6;s=JBQ_JY_JRQ1_REM"]
["加热器1运行","ns=6;s=JBQ_JY_JRQ1_RFB"]
["加热器2手自动","ns=6;s=JBQ_JY_JRQ2_BT_AUTO"]
["加热器2故障复位","ns=6;s=JBQ_JY_JRQ2_BT_RESET"]
["加热器2手动启动","ns=6;s=JBQ_JY_JRQ2_BT_START"]
["加热器2手动停止","ns=6;s=JBQ_JY_JRQ2_BT_STOP"]
["加热器2故障","ns=6;s=JBQ_JY_JRQ2_FAULT"]
["加热器2启动","ns=6;s=JBQ_JY_JRQ2_OUTPUT"]
["加热器2启动准备好","ns=6;s=JBQ_JY_JRQ2_READY"]
["加热器2泵远程","ns=6;s=JBQ_JY_JRQ2_REM"]
["加热器2运行","ns=6;s=JBQ_JY_JRQ2_RFB"]
["溶药箱搅拌器自动启动","ns=6;s=JBQ_JY_RYX_AUTOSTART"]
["溶药箱搅拌器手自动","ns=6;s=JBQ_JY_RYX_BT_AUTO"]
["溶药箱搅拌器故障复位","ns=6;s=JBQ_JY_RYX_BT_RESET"]
["溶药箱搅拌器手动启动","ns=6;s=JBQ_JY_RYX_BT_START"]
["溶药箱搅拌器手动停止","ns=6;s=JBQ_JY_RYX_BT_STOP"]
["溶药箱搅拌器故障","ns=6;s=JBQ_JY_RYX_FAULT"]
["溶药箱搅拌器启动","ns=6;s=JBQ_JY_RYX_OUTPUT"]
["溶药箱搅拌器启动准备好","ns=6;s=JBQ_JY_RYX_READY"]
["溶药箱搅拌器泵远程","ns=6;s=JBQ_JY_RYX_REM"]
["溶药箱搅拌器运行","ns=6;s=JBQ_JY_RYX_RFB"]
["酸搅拌器自动启动","ns=6;s=JBQ_JY_S_AUTOSTART"]
["酸搅拌器手自动","ns=6;s=JBQ_JY_S_BT_AUTO"]
["酸搅拌器故障复位","ns=6;s=JBQ_JY_S_BT_RESET"]
["酸搅拌器手动启动","ns=6;s=JBQ_JY_S_BT_START"]
["酸搅拌器手动停止","ns=6;s=JBQ_JY_S_BT_STOP"]
["酸搅拌器故障","ns=6;s=JBQ_JY_S_FAULT"]
["酸搅拌器启动","ns=6;s=JBQ_JY_S_OUTPUT"]
["酸搅拌器启动准备好","ns=6;s=JBQ_JY_S_READY"]
["酸搅拌器泵远程","ns=6;s=JBQ_JY_S_REM"]
["酸搅拌器运行","ns=6;s=JBQ_JY_S_RFB"]
["杀菌剂搅拌器自动启动","ns=6;s=JBQ_JY_SJJ_AUTOSTART"]
["杀菌剂搅拌器手自动","ns=6;s=JBQ_JY_SJJ_BT_AUTO"]
["杀菌剂搅拌器故障复位","ns=6;s=JBQ_JY_SJJ_BT_RESET"]
["杀菌剂搅拌器手动启动","ns=6;s=JBQ_JY_SJJ_BT_START"]
["杀菌剂搅拌器手动停止","ns=6;s=JBQ_JY_SJJ_BT_STOP"]
["杀菌剂搅拌器故障","ns=6;s=JBQ_JY_SJJ_FAULT"]
["杀菌剂搅拌器启动","ns=6;s=JBQ_JY_SJJ_OUTPUT"]
["杀菌剂搅拌器启动准备好","ns=6;s=JBQ_JY_SJJ_READY"]
["杀菌剂搅拌器泵远程","ns=6;s=JBQ_JY_SJJ_REM"]
["杀菌剂搅拌器运行","ns=6;s=JBQ_JY_SJJ_RFB"]
["阻垢剂搅拌器自动启动","ns=6;s=JBQ_JY_ZGJ_AUTOSTART"]
["阻垢剂搅拌器手自动","ns=6;s=JBQ_JY_ZGJ_BT_AUTO"]
["阻垢剂搅拌器故障复位","ns=6;s=JBQ_JY_ZGJ_BT_RESET"]
["阻垢剂搅拌器手动启动","ns=6;s=JBQ_JY_ZGJ_BT_START"]
["阻垢剂搅拌器手动停止","ns=6;s=JBQ_JY_ZGJ_BT_STOP"]
["阻垢剂搅拌器故障","ns=6;s=JBQ_JY_ZGJ_FAULT"]
["阻垢剂搅拌器启动","ns=6;s=JBQ_JY_ZGJ_OUTPUT"]
["阻垢剂搅拌器启动准备好","ns=6;s=JBQ_JY_ZGJ_READY"]
["阻垢剂搅拌器泵远程","ns=6;s=JBQ_JY_ZGJ_REM"]
["阻垢剂搅拌器运行","ns=6;s=JBQ_JY_ZGJ_RFB"]
["CEB还原剂加药泵1手自动","ns=6;s=P_CEB_HYJ1_BT_AUTO"]
["CEB还原剂加药泵1故障复位","ns=6;s=P_CEB_HYJ1_BT_RESET"]
["CEB还原剂加药泵1手动启动","ns=6;s=P_CEB_HYJ1_BT_START"]
["CEB还原剂加药泵1手动停止","ns=6;s=P_CEB_HYJ1_BT_STOP"]
["CEB还原剂加药泵1故障","ns=6;s=P_CEB_HYJ1_FAULT"]
["CEB还原剂加药泵1启动","ns=6;s=P_CEB_HYJ1_OUTPUT"]
["CEB还原剂加药泵1启动准备好","ns=6;s=P_CEB_HYJ1_READY"]
["CEB还原剂加药泵1泵远程","ns=6;s=P_CEB_HYJ1_REM"]
["CEB还原剂加药泵1运行","ns=6;s=P_CEB_HYJ1_RFB"]
["CEB还原剂加药泵2手自动","ns=6;s=P_CEB_HYJ2_BT_AUTO"]
["CEB还原剂加药泵2故障复位","ns=6;s=P_CEB_HYJ2_BT_RESET"]
["CEB还原剂加药泵2手动启动","ns=6;s=P_CEB_HYJ2_BT_START"]
["CEB还原剂加药泵2手动停止","ns=6;s=P_CEB_HYJ2_BT_STOP"]
["CEB还原剂加药泵2故障","ns=6;s=P_CEB_HYJ2_FAULT"]
["CEB还原剂加药泵2启动","ns=6;s=P_CEB_HYJ2_OUTPUT"]
["CEB还原剂加药泵2启动准备好","ns=6;s=P_CEB_HYJ2_READY"]
["CEB还原剂加药泵2泵远程","ns=6;s=P_CEB_HYJ2_REM"]
["CEB还原剂加药泵2运行","ns=6;s=P_CEB_HYJ2_RFB"]
["备用气动隔膜泵1手自动","ns=6;s=P_JY_BY1_BT_AUTO"]
["备用气动隔膜泵1故障复位","ns=6;s=P_JY_BY1_BT_RESET"]
["备用气动隔膜泵1手动启动","ns=6;s=P_JY_BY1_BT_START"]
["备用气动隔膜泵1手动停止","ns=6;s=P_JY_BY1_BT_STOP"]
["备用气动隔膜泵1故障","ns=6;s=P_JY_BY1_FAULT"]
["备用气动隔膜泵1启动","ns=6;s=P_JY_BY1_OUTPUT"]
["备用气动隔膜泵1启动准备好","ns=6;s=P_JY_BY1_READY"]
["备用气动隔膜泵1泵远程","ns=6;s=P_JY_BY1_REM"]
["备用气动隔膜泵1运行","ns=6;s=P_JY_BY1_RFB"]
["备用气动隔膜泵2手自动","ns=6;s=P_JY_BY2_BT_AUTO"]
["备用气动隔膜泵2故障复位","ns=6;s=P_JY_BY2_BT_RESET"]
["备用气动隔膜泵2手动启动","ns=6;s=P_JY_BY2_BT_START"]
["备用气动隔膜泵2手动停止","ns=6;s=P_JY_BY2_BT_STOP"]
["备用气动隔膜泵2故障","ns=6;s=P_JY_BY2_FAULT"]
["备用气动隔膜泵2启动","ns=6;s=P_JY_BY2_OUTPUT"]
["备用气动隔膜泵2启动准备好","ns=6;s=P_JY_BY2_READY"]
["备用气动隔膜泵2泵远程","ns=6;s=P_JY_BY2_REM"]
["备用气动隔膜泵2运行","ns=6;s=P_JY_BY2_RFB"]
["备用气动隔膜泵3手自动","ns=6;s=P_JY_BY3_BT_AUTO"]
["备用气动隔膜泵3故障复位","ns=6;s=P_JY_BY3_BT_RESET"]
["备用气动隔膜泵3手动启动","ns=6;s=P_JY_BY3_BT_START"]
["备用气动隔膜泵3手动停止","ns=6;s=P_JY_BY3_BT_STOP"]
["备用气动隔膜泵3故障","ns=6;s=P_JY_BY3_FAULT"]
["备用气动隔膜泵3启动","ns=6;s=P_JY_BY3_OUTPUT"]
["备用气动隔膜泵3启动准备好","ns=6;s=P_JY_BY3_READY"]
["备用气动隔膜泵3泵远程","ns=6;s=P_JY_BY3_REM"]
["备用气动隔膜泵3运行","ns=6;s=P_JY_BY3_RFB"]
["CIP泵自动启动","ns=6;s=P_JY_CIPB_AUTOSTART"]
["CIP泵手自动","ns=6;s=P_JY_CIPB_BT_AUTO"]
["CIP泵故障复位","ns=6;s=P_JY_CIPB_BT_RESET"]
["CIP泵手动启动","ns=6;s=P_JY_CIPB_BT_START"]
["CIP泵手动停止","ns=6;s=P_JY_CIPB_BT_STOP"]
["CIP泵故障","ns=6;s=P_JY_CIPB_FAULT"]
["CIP泵启动","ns=6;s=P_JY_CIPB_OUTPUT"]
["CIP泵启动准备好","ns=6;s=P_JY_CIPB_READY"]
["CIP泵泵远程","ns=6;s=P_JY_CIPB_REM"]
["CIP泵运行","ns=6;s=P_JY_CIPB_RFB"]
["次钠加药泵1手自动","ns=6;s=P_JY_CN1_BT_AUTO"]
["次钠加药泵1故障复位","ns=6;s=P_JY_CN1_BT_RESET"]
["次钠加药泵1手动启动","ns=6;s=P_JY_CN1_BT_START"]
["次钠加药泵1手动停止","ns=6;s=P_JY_CN1_BT_STOP"]
["次钠加药泵1故障","ns=6;s=P_JY_CN1_FAULT"]
["次钠加药泵1启动","ns=6;s=P_JY_CN1_OUTPUT"]
["次钠加药泵1启动准备好","ns=6;s=P_JY_CN1_READY"]
["次钠加药泵1泵远程","ns=6;s=P_JY_CN1_REM"]
["次钠加药泵1运行","ns=6;s=P_JY_CN1_RFB"]
["次钠加药泵2手自动","ns=6;s=P_JY_CN2_BT_AUTO"]
["次钠加药泵2故障复位","ns=6;s=P_JY_CN2_BT_RESET"]
["次钠加药泵2手动启动","ns=6;s=P_JY_CN2_BT_START"]
["次钠加药泵2手动停止","ns=6;s=P_JY_CN2_BT_STOP"]
["次钠加药泵2故障","ns=6;s=P_JY_CN2_FAULT"]
["次钠加药泵2启动","ns=6;s=P_JY_CN2_OUTPUT"]
["次钠加药泵2启动准备好","ns=6;s=P_JY_CN2_READY"]
["次钠加药泵2泵远程","ns=6;s=P_JY_CN2_REM"]
["次钠加药泵2运行","ns=6;s=P_JY_CN2_RFB"]
["反洗风机自动启动","ns=6;s=P_JY_FX_FJ_AUTOSTART"]
["反洗风机手自动","ns=6;s=P_JY_FX_FJ_BT_AUTO"]
["反洗风机故障复位","ns=6;s=P_JY_FX_FJ_BT_RESET"]
["反洗风机手动启动","ns=6;s=P_JY_FX_FJ_BT_START"]
["反洗风机手动停止","ns=6;s=P_JY_FX_FJ_BT_STOP"]
["反洗风机故障","ns=6;s=P_JY_FX_FJ_FAULT"]
["反洗风机启动","ns=6;s=P_JY_FX_FJ_OUTPUT"]
["反洗风机启动准备好","ns=6;s=P_JY_FX_FJ_READY"]
["反洗风机泵远程","ns=6;s=P_JY_FX_FJ_REM"]
["反洗风机运行","ns=6;s=P_JY_FX_FJ_RFB"]
["还原剂加药泵手自动","ns=6;s=P_JY_HYJ_BT_AUTO"]
["还原剂加药泵故障复位","ns=6;s=P_JY_HYJ_BT_RESET"]
["还原剂加药泵手动启动","ns=6;s=P_JY_HYJ_BT_START"]
["还原剂加药泵手动停止","ns=6;s=P_JY_HYJ_BT_STOP"]
["还原剂加药泵故障","ns=6;s=P_JY_HYJ_FAULT"]
["还原剂加药泵启动","ns=6;s=P_JY_HYJ_OUTPUT"]
["还原剂加药泵启动准备好","ns=6;s=P_JY_HYJ_READY"]
["还原剂加药泵泵远程","ns=6;s=P_JY_HYJ_REM"]
["还原剂加药泵运行","ns=6;s=P_JY_HYJ_RFB"]
["碱加药泵1手自动","ns=6;s=P_JY_JJ1_BT_AUTO"]
["碱加药泵1故障复位","ns=6;s=P_JY_JJ1_BT_RESET"]
["碱加药泵1手动启动","ns=6;s=P_JY_JJ1_BT_START"]
["碱加药泵1手动停止","ns=6;s=P_JY_JJ1_BT_STOP"]
["碱加药泵1故障","ns=6;s=P_JY_JJ1_FAULT"]
["碱加药泵1启动","ns=6;s=P_JY_JJ1_OUTPUT"]
["碱加药泵1启动准备好","ns=6;s=P_JY_JJ1_READY"]
["碱加药泵1泵远程","ns=6;s=P_JY_JJ1_REM"]
["碱加药泵1运行","ns=6;s=P_JY_JJ1_RFB"]
["碱加药泵2手自动","ns=6;s=P_JY_JJ2_BT_AUTO"]
["碱加药泵2故障复位","ns=6;s=P_JY_JJ2_BT_RESET"]
["碱加药泵2手动启动","ns=6;s=P_JY_JJ2_BT_START"]
["碱加药泵2手动停止","ns=6;s=P_JY_JJ2_BT_STOP"]
["碱加药泵2故障","ns=6;s=P_JY_JJ2_FAULT"]
["碱加药泵2启动","ns=6;s=P_JY_JJ2_OUTPUT"]
["碱加药泵2启动准备好","ns=6;s=P_JY_JJ2_READY"]
["碱加药泵2泵远程","ns=6;s=P_JY_JJ2_REM"]
["碱加药泵2运行","ns=6;s=P_JY_JJ2_RFB"]
["酸加药泵1手自动","ns=6;s=P_JY_JS1_BT_AUTO"]
["酸加药泵1故障复位","ns=6;s=P_JY_JS1_BT_RESET"]
["酸加药泵1手动启动","ns=6;s=P_JY_JS1_BT_START"]
["酸加药泵1手动停止","ns=6;s=P_JY_JS1_BT_STOP"]
["酸加药泵1故障","ns=6;s=P_JY_JS1_FAULT"]
["酸加药泵1启动","ns=6;s=P_JY_JS1_OUTPUT"]
["酸加药泵1启动准备好","ns=6;s=P_JY_JS1_READY"]
["酸加药泵1泵远程","ns=6;s=P_JY_JS1_REM"]
["酸加药泵1运行","ns=6;s=P_JY_JS1_RFB"]
["酸加药泵2手自动","ns=6;s=P_JY_JS2_BT_AUTO"]
["酸加药泵2故障复位","ns=6;s=P_JY_JS2_BT_RESET"]
["酸加药泵2手动启动","ns=6;s=P_JY_JS2_BT_START"]
["酸加药泵2手动停止","ns=6;s=P_JY_JS2_BT_STOP"]
["酸加药泵2故障","ns=6;s=P_JY_JS2_FAULT"]
["酸加药泵2启动","ns=6;s=P_JY_JS2_OUTPUT"]
["酸加药泵2启动准备好","ns=6;s=P_JY_JS2_READY"]
["酸加药泵2泵远程","ns=6;s=P_JY_JS2_REM"]
["酸加药泵2运行","ns=6;s=P_JY_JS2_RFB"]
["泵坑潜污泵1手自动","ns=6;s=P_JY_QWB1_BT_AUTO"]
["泵坑潜污泵1故障复位","ns=6;s=P_JY_QWB1_BT_RESET"]
["泵坑潜污泵1手动启动","ns=6;s=P_JY_QWB1_BT_START"]
["泵坑潜污泵1手动停止","ns=6;s=P_JY_QWB1_BT_STOP"]
["泵坑潜污泵1故障","ns=6;s=P_JY_QWB1_FAULT"]
["泵坑潜污泵1启动","ns=6;s=P_JY_QWB1_OUTPUT"]
["泵坑潜污泵1启动准备好","ns=6;s=P_JY_QWB1_READY"]
["泵坑潜污泵1泵远程","ns=6;s=P_JY_QWB1_REM"]
["泵坑潜污泵1运行","ns=6;s=P_JY_QWB1_RFB"]
["泵坑潜污泵2手自动","ns=6;s=P_JY_QWB2_BT_AUTO"]
["泵坑潜污泵2故障复位","ns=6;s=P_JY_QWB2_BT_RESET"]
["泵坑潜污泵2手动启动","ns=6;s=P_JY_QWB2_BT_START"]
["泵坑潜污泵2手动停止","ns=6;s=P_JY_QWB2_BT_STOP"]
["泵坑潜污泵2故障","ns=6;s=P_JY_QWB2_FAULT"]
["泵坑潜污泵2启动","ns=6;s=P_JY_QWB2_OUTPUT"]
["泵坑潜污泵2启动准备好","ns=6;s=P_JY_QWB2_READY"]
["泵坑潜污泵2泵远程","ns=6;s=P_JY_QWB2_REM"]
["泵坑潜污泵2运行","ns=6;s=P_JY_QWB2_RFB"]
["杀菌剂加药泵手自动","ns=6;s=P_JY_SJJ_BT_AUTO"]
["杀菌剂加药泵故障复位","ns=6;s=P_JY_SJJ_BT_RESET"]
["杀菌剂加药泵手动启动","ns=6;s=P_JY_SJJ_BT_START"]
["杀菌剂加药泵手动停止","ns=6;s=P_JY_SJJ_BT_STOP"]
["杀菌剂加药泵故障","ns=6;s=P_JY_SJJ_FAULT"]
["杀菌剂加药泵启动","ns=6;s=P_JY_SJJ_OUTPUT"]
["杀菌剂加药泵启动准备好","ns=6;s=P_JY_SJJ_READY"]
["杀菌剂加药泵泵远程","ns=6;s=P_JY_SJJ_REM"]
["杀菌剂加药泵运行","ns=6;s=P_JY_SJJ_RFB"]
["塑料泵自动启动","ns=6;s=P_JY_SLB_AUTOSTART"]
["塑料泵手自动","ns=6;s=P_JY_SLB_BT_AUTO"]
["塑料泵故障复位","ns=6;s=P_JY_SLB_BT_RESET"]
["塑料泵手动启动","ns=6;s=P_JY_SLB_BT_START"]
["塑料泵手动停止","ns=6;s=P_JY_SLB_BT_STOP"]
["塑料泵故障","ns=6;s=P_JY_SLB_FAULT"]
["塑料泵启动","ns=6;s=P_JY_SLB_OUTPUT"]
["塑料泵启动准备好","ns=6;s=P_JY_SLB_READY"]
["塑料泵泵远程","ns=6;s=P_JY_SLB_REM"]
["塑料泵运行","ns=6;s=P_JY_SLB_RFB"]
["外供水碱加药泵1手自动","ns=6;s=P_JY_WGSJ1_BT_AUTO"]
["外供水碱加药泵1故障复位","ns=6;s=P_JY_WGSJ1_BT_RESET"]
["外供水碱加药泵1手动启动","ns=6;s=P_JY_WGSJ1_BT_START"]
["外供水碱加药泵1手动停止","ns=6;s=P_JY_WGSJ1_BT_STOP"]
["外供水碱加药泵1故障","ns=6;s=P_JY_WGSJ1_FAULT"]
["外供水碱加药泵1启动","ns=6;s=P_JY_WGSJ1_OUTPUT"]
["外供水碱加药泵1启动准备好","ns=6;s=P_JY_WGSJ1_READY"]
["外供水碱加药泵1泵远程","ns=6;s=P_JY_WGSJ1_REM"]
["外供水碱加药泵1运行","ns=6;s=P_JY_WGSJ1_RFB"]
["外供水碱加药泵2手自动","ns=6;s=P_JY_WGSJ2_BT_AUTO"]
["外供水碱加药泵2故障复位","ns=6;s=P_JY_WGSJ2_BT_RESET"]
["外供水碱加药泵2手动启动","ns=6;s=P_JY_WGSJ2_BT_START"]
["外供水碱加药泵2手动停止","ns=6;s=P_JY_WGSJ2_BT_STOP"]
["外供水碱加药泵2故障","ns=6;s=P_JY_WGSJ2_FAULT"]
["外供水碱加药泵2启动","ns=6;s=P_JY_WGSJ2_OUTPUT"]
["外供水碱加药泵2启动准备好","ns=6;s=P_JY_WGSJ2_READY"]
["外供水碱加药泵2泵远程","ns=6;s=P_JY_WGSJ2_REM"]
["外供水碱加药泵2运行","ns=6;s=P_JY_WGSJ2_RFB"]
["阻垢剂加药泵手自动","ns=6;s=P_JY_ZGJ_BT_AUTO"]
["阻垢剂加药泵故障复位","ns=6;s=P_JY_ZGJ_BT_RESET"]
["阻垢剂加药泵手动启动","ns=6;s=P_JY_ZGJ_BT_START"]
["阻垢剂加药泵手动停止","ns=6;s=P_JY_ZGJ_BT_STOP"]
["阻垢剂加药泵故障","ns=6;s=P_JY_ZGJ_FAULT"]
["阻垢剂加药泵启动","ns=6;s=P_JY_ZGJ_OUTPUT"]
["阻垢剂加药泵启动准备好","ns=6;s=P_JY_ZGJ_READY"]
["阻垢剂加药泵泵远程","ns=6;s=P_JY_ZGJ_REM"]
["阻垢剂加药泵运行","ns=6;s=P_JY_ZGJ_RFB"]
["反渗透段间泵自动启动","ns=6;s=P_RO_DJB_AUTOSTART"]
["反渗透段间泵手自动","ns=6;s=P_RO_DJB_BT_AUTO"]
["反渗透段间泵故障复位","ns=6;s=P_RO_DJB_BT_RESET"]
["反渗透段间泵手动启动","ns=6;s=P_RO_DJB_BT_START"]
["反渗透段间泵手动停止","ns=6;s=P_RO_DJB_BT_STOP"]
["反渗透段间泵故障","ns=6;s=P_RO_DJB_FAULT"]
["反渗透段间泵启动","ns=6;s=P_RO_DJB_OUTPUT"]
["反渗透段间泵启动准备好","ns=6;s=P_RO_DJB_READY"]
["反渗透段间泵泵远程","ns=6;s=P_RO_DJB_REM"]
["反渗透段间泵运行","ns=6;s=P_RO_DJB_RFB"]
["反渗透供水泵自动启动","ns=6;s=P_RO_GSB_AUTOSTART"]
["反渗透供水泵手自动","ns=6;s=P_RO_GSB_BT_AUTO"]
["反渗透供水泵故障复位","ns=6;s=P_RO_GSB_BT_RESET"]
["反渗透供水泵手动启动","ns=6;s=P_RO_GSB_BT_START"]
["反渗透供水泵手动停止","ns=6;s=P_RO_GSB_BT_STOP"]
["反渗透供水泵故障","ns=6;s=P_RO_GSB_FAULT"]
["反渗透供水泵启动","ns=6;s=P_RO_GSB_OUTPUT"]
["反渗透供水泵启动准备好","ns=6;s=P_RO_GSB_READY"]
["反渗透供水泵泵远程","ns=6;s=P_RO_GSB_REM"]
["反渗透供水泵运行","ns=6;s=P_RO_GSB_RFB"]
["反渗透高压泵自动启动","ns=6;s=P_RO_GYB_AUTOSTART"]
["反渗透高压泵手自动","ns=6;s=P_RO_GYB_BT_AUTO"]
["反渗透高压泵故障复位","ns=6;s=P_RO_GYB_BT_RESET"]
["反渗透高压泵手动启动","ns=6;s=P_RO_GYB_BT_START"]
["反渗透高压泵手动停止","ns=6;s=P_RO_GYB_BT_STOP"]
["反渗透高压泵故障","ns=6;s=P_RO_GYB_FAULT"]
["反渗透高压泵启动","ns=6;s=P_RO_GYB_OUTPUT"]
["反渗透高压泵启动准备好","ns=6;s=P_RO_GYB_READY"]
["反渗透高压泵泵远程","ns=6;s=P_RO_GYB_REM"]
["反渗透高压泵运行","ns=6;s=P_RO_GYB_RFB"]
["超滤产水泵自动启动","ns=6;s=P_UF_CSB_AUTOSTART"]
["超滤产水泵手自动","ns=6;s=P_UF_CSB_BT_AUTO"]
["超滤产水泵故障复位","ns=6;s=P_UF_CSB_BT_RESET"]
["超滤产水泵手动启动","ns=6;s=P_UF_CSB_BT_START"]
["超滤产水泵手动停止","ns=6;s=P_UF_CSB_BT_STOP"]
["超滤产水泵故障","ns=6;s=P_UF_CSB_FAULT"]
["超滤产水泵启动","ns=6;s=P_UF_CSB_OUTPUT"]
["超滤产水泵启动准备好","ns=6;s=P_UF_CSB_READY"]
["超滤产水泵泵远程","ns=6;s=P_UF_CSB_REM"]
["超滤产水泵运行","ns=6;s=P_UF_CSB_RFB"]
["超滤反洗泵自动启动","ns=6;s=P_UF_FXB_AUTOSTART"]
["超滤反洗泵手自动","ns=6;s=P_UF_FXB_BT_AUTO"]
["超滤反洗泵故障复位","ns=6;s=P_UF_FXB_BT_RESET"]
["超滤反洗泵手动启动","ns=6;s=P_UF_FXB_BT_START"]
["超滤反洗泵手动停止","ns=6;s=P_UF_FXB_BT_STOP"]
["超滤反洗泵故障","ns=6;s=P_UF_FXB_FAULT"]
["超滤反洗泵启动","ns=6;s=P_UF_FXB_OUTPUT"]
["超滤反洗泵启动准备好","ns=6;s=P_UF_FXB_READY"]
["超滤反洗泵泵远程","ns=6;s=P_UF_FXB_REM"]
["超滤反洗泵运行","ns=6;s=P_UF_FXB_RFB"]
["UF供水泵1手自动","ns=6;s=P_UF_GSB1_BT_AUTO"]
["UF供水泵1故障复位","ns=6;s=P_UF_GSB1_BT_RESET"]
["UF供水泵1手动启动","ns=6;s=P_UF_GSB1_BT_START"]
["UF供水泵1手动停止","ns=6;s=P_UF_GSB1_BT_STOP"]
["UF供水泵1故障","ns=6;s=P_UF_GSB1_FAULT"]
["UF供水泵1启动","ns=6;s=P_UF_GSB1_OUTPUT"]
["UF供水泵1启动准备好","ns=6;s=P_UF_GSB1_READY"]
["UF供水泵1泵远程","ns=6;s=P_UF_GSB1_REM"]
["UF供水泵1运行","ns=6;s=P_UF_GSB1_RFB"]
["UF供水泵2手自动","ns=6;s=P_UF_GSB2_BT_AUTO"]
["UF供水泵2故障复位","ns=6;s=P_UF_GSB2_BT_RESET"]
["UF供水泵2手动启动","ns=6;s=P_UF_GSB2_BT_START"]
["UF供水泵2手动停止","ns=6;s=P_UF_GSB2_BT_STOP"]
["UF供水泵2故障","ns=6;s=P_UF_GSB2_FAULT"]
["UF供水泵2启动","ns=6;s=P_UF_GSB2_OUTPUT"]
["UF供水泵2启动准备好","ns=6;s=P_UF_GSB2_READY"]
["UF供水泵2泵远程","ns=6;s=P_UF_GSB2_REM"]
["UF供水泵2运行","ns=6;s=P_UF_GSB2_RFB"]
["超滤排空泵自动启动","ns=6;s=P_UF_PKB_AUTOSTART"]
["超滤排空泵手自动","ns=6;s=P_UF_PKB_BT_AUTO"]
["超滤排空泵故障复位","ns=6;s=P_UF_PKB_BT_RESET"]
["超滤排空泵手动启动","ns=6;s=P_UF_PKB_BT_START"]
["超滤排空泵手动停止","ns=6;s=P_UF_PKB_BT_STOP"]
["超滤排空泵故障","ns=6;s=P_UF_PKB_FAULT"]
["超滤排空泵启动","ns=6;s=P_UF_PKB_OUTPUT"]
["超滤排空泵启动准备好","ns=6;s=P_UF_PKB_READY"]
["超滤排空泵泵远程","ns=6;s=P_UF_PKB_REM"]
["超滤排空泵运行","ns=6;s=P_UF_PKB_RFB"]
["超滤提升泵1自动启动","ns=6;s=P_UF_TSB1_AUTOSTART"]
["超滤提升泵1手自动","ns=6;s=P_UF_TSB1_BT_AUTO"]
["超滤提升泵1故障复位","ns=6;s=P_UF_TSB1_BT_RESET"]
["超滤提升泵1手动启动","ns=6;s=P_UF_TSB1_BT_START"]
["超滤提升泵1手动停止","ns=6;s=P_UF_TSB1_BT_STOP"]
["超滤提升泵1故障","ns=6;s=P_UF_TSB1_FAULT"]
["超滤提升泵1启动","ns=6;s=P_UF_TSB1_OUTPUT"]
["超滤提升泵1启动准备好","ns=6;s=P_UF_TSB1_READY"]
["超滤提升泵1泵远程","ns=6;s=P_UF_TSB1_REM"]
["超滤提升泵1运行","ns=6;s=P_UF_TSB1_RFB"]
["超滤提升泵2自动启动","ns=6;s=P_UF_TSB2_AUTOSTART"]
["超滤提升泵2手自动","ns=6;s=P_UF_TSB2_BT_AUTO"]
["超滤提升泵2故障复位","ns=6;s=P_UF_TSB2_BT_RESET"]
["超滤提升泵2手动启动","ns=6;s=P_UF_TSB2_BT_START"]
["超滤提升泵2手动停止","ns=6;s=P_UF_TSB2_BT_STOP"]
["超滤提升泵2故障","ns=6;s=P_UF_TSB2_FAULT"]
["超滤提升泵2启动","ns=6;s=P_UF_TSB2_OUTPUT"]
["超滤提升泵2启动准备好","ns=6;s=P_UF_TSB2_READY"]
["超滤提升泵2泵远程","ns=6;s=P_UF_TSB2_REM"]
["超滤提升泵2运行","ns=6;s=P_UF_TSB2_RFB"]
["RO_19_ERR","ns=6;s=RO_19_ERR"]
["RO_20_ERR","ns=6;s=RO_20_ERR"]
["RO_21_ERR","ns=6;s=RO_21_ERR"]
["RO_22_ERR","ns=6;s=RO_22_ERR"]
["RO_23_ERR","ns=6;s=RO_23_ERR"]
["RO_24_ERR","ns=6;s=RO_24_ERR"]
["RO_25_ERR","ns=6;s=RO_25_ERR"]
["RO_26_ERR","ns=6;s=RO_26_ERR"]
["RO_27_ERR","ns=6;s=RO_27_ERR"]
["RO_28_ERR","ns=6;s=RO_28_ERR"]
["RO_29_ERR","ns=6;s=RO_29_ERR"]
["RO_30_ERR","ns=6;s=RO_30_ERR"]
["RO_31_ERR","ns=6;s=RO_31_ERR"]
["RO_32_ERR","ns=6;s=RO_32_ERR"]
["反洗入栈","ns=6;s=RO_APPLY_BW_PUSH"]
["CEB入栈","ns=6;s=RO_APPLY_CEB_PUSH"]
["启动冲洗泵","ns=6;s=RO_APPLY_CXB_ON"]
["启动段间泵","ns=6;s=RO_APPLY_DJB_ON"]
["启用供水泵","ns=6;s=RO_APPLY_GSB_ON"]
["启动还原剂","ns=6;s=RO_APPLY_HYJ_ON"]
["出栈","ns=6;s=RO_APPLY_POP"]
["启动杀菌剂","ns=6;s=RO_APPLY_SJJ_ON"]
["启动出水排气阀","ns=6;s=RO_APPLY_V_CSPQ"]
["启动进水排气阀","ns=6;s=RO_APPLY_V_JSPQ"]
["启动浓水排气阀","ns=6;s=RO_APPLY_V_NSPQ"]
["启动阻垢剂","ns=6;s=RO_APPLY_ZGJ_ON"]
["启用增压泵","ns=6;s=RO_APPLY_ZYB_ON"]
["RO_APPLY1","ns=6;s=RO_APPLY1"]
["RO_APPLY2","ns=6;s=RO_APPLY2"]
["RO_APPLY20","ns=6;s=RO_APPLY20"]
["RO_APPLY24","ns=6;s=RO_APPLY24"]
["RO_APPLY25","ns=6;s=RO_APPLY25"]
["RO_APPLY26","ns=6;s=RO_APPLY26"]
["RO_APPLY27","ns=6;s=RO_APPLY27"]
["RO_APPLY28","ns=6;s=RO_APPLY28"]
["RO_APPLY29","ns=6;s=RO_APPLY29"]
["RO_APPLY3","ns=6;s=RO_APPLY3"]
["RO_APPLY30","ns=6;s=RO_APPLY30"]
["RO_APPLY31","ns=6;s=RO_APPLY31"]
["RO_APPLY4","ns=6;s=RO_APPLY4"]
["RO_APPLY5","ns=6;s=RO_APPLY5"]
["RO_APPLY6","ns=6;s=RO_APPLY6"]
["RO_APPLY7","ns=6;s=RO_APPLY7"]
["RO_APPLY8","ns=6;s=RO_APPLY8"]
["RO_BTN_10","ns=6;s=RO_BTN_10"]
["RO_BTN_11","ns=6;s=RO_BTN_11"]
["RO_BTN_20","ns=6;s=RO_BTN_20"]
["RO_BTN_22","ns=6;s=RO_BTN_22"]
["RO_BTN_23","ns=6;s=RO_BTN_23"]
["RO_BTN_24","ns=6;s=RO_BTN_24"]
["RO_BTN_25","ns=6;s=RO_BTN_25"]
["RO_BTN_26","ns=6;s=RO_BTN_26"]
["RO_BTN_27","ns=6;s=RO_BTN_27"]
["RO_BTN_28","ns=6;s=RO_BTN_28"]
["RO_BTN_29","ns=6;s=RO_BTN_29"]
["RO_BTN_30","ns=6;s=RO_BTN_30"]
["RO_BTN_31","ns=6;s=RO_BTN_31"]
["RO_BTN_5","ns=6;s=RO_BTN_5"]
["RO_BTN_6","ns=6;s=RO_BTN_6"]
["RO_BTN_7","ns=6;s=RO_BTN_7"]
["CIP清洗：启动/停止","ns=6;s=RO_BTN_CIP"]
["半自动：反洗（脉冲）","ns=6;s=RO_BTN_CX"]
["段间泵PID选择","ns=6;s=RO_BTN_DJB_PID"]
["急停","ns=6;s=RO_BTN_EMG"]
["故障复位","ns=6;s=RO_BTN_FAULT_RST"]
["高压泵PID选择","ns=6;s=RO_BTN_GYB_PID"]
["还原剂PID选择","ns=6;s=RO_BTN_HYJ_PID"]
["初始化","ns=6;s=RO_BTN_INITIAL"]
["累计流量清零","ns=6;s=RO_BTN_LJLL_CLEAR"]
["半自动：CEB（脉冲）","ns=6;s=RO_BTN_SJX"]
["半自动：开机 (置位)","ns=6;s=RO_BTN_START"]
["半自动：停止（脉冲，复位01/03）","ns=6;s=RO_BTN_STOP"]
["全自动：投运/停机","ns=6;s=RO_BTN_TY"]
["仪表屏蔽","ns=6;s=RO_BTN_YBDIS"]
["阀门自动","ns=6;s=RO_BTN_YVS_AUTO"]
["阻垢剂PID选择","ns=6;s=RO_BTN_ZGJ_PID"]
["ERR_电导率H","ns=6;s=RO_DDL_H_ERR"]
["ERR_电导率HH","ns=6;s=RO_DDL_HH_ERR"]
["Flag_16","ns=6;s=RO_FLAG_16"]
["RO_FLAG_22","ns=6;s=RO_FLAG_22"]
["RO_FLAG_23","ns=6;s=RO_FLAG_23"]
["RO_FLAG_25","ns=6;s=RO_FLAG_25"]
["RO_FLAG_26","ns=6;s=RO_FLAG_26"]
["RO_FLAG_27","ns=6;s=RO_FLAG_27"]
["RO_FLAG_28","ns=6;s=RO_FLAG_28"]
["RO_FLAG_29","ns=6;s=RO_FLAG_29"]
["自动启动标志","ns=6;s=RO_FLAG_AUTOSTART"]
["Flag_CSF_Allow","ns=6;s=RO_FLAG_CSF_ALLOW"]
["Flag_冲水过滤ing","ns=6;s=RO_FLAG_CSGL_ING"]
["flag_冲洗ready","ns=6;s=RO_FLAG_CX_READY"]
["Flag_冲洗泵run","ns=6;s=RO_FLAG_CXB_RUN"]
["Flag_DJB_Allow","ns=6;s=RO_FLAG_DJB_ALLOW"]
["Flag_过滤完成","ns=6;s=RO_FLAG_GL_FIN"]
["Flag_过滤ing","ns=6;s=RO_FLAG_GL_ING"]
["flag_过滤ready","ns=6;s=RO_FLAG_GL_READY"]
["Flag_供水泵run","ns=6;s=RO_FLAG_GSB_RUN"]
["Flag_GYB_Allow","ns=6;s=RO_FLAG_GYB_ALLOW"]
["Flag_还原剂run","ns=6;s=RO_FLAG_HYJ_RUN"]
["flag_冲洗电机Ready","ns=6;s=RO_FLAG_M_CX_READY"]
["flag_过滤电机Ready","ns=6;s=RO_FLAG_M_GL_READY"]
["flag_模组准备好Ready","ns=6;s=RO_FLAG_MZ_READY"]
["flag_模组水泵Ready","ns=6;s=RO_FLAG_MZP_READY"]
["Flag_模组设备ready","ns=6;s=RO_FLAG_MZSB_READY"]
["flag_模组仪表Ready","ns=6;s=RO_FLAG_MZYB_READY"]
["flag_模组阀门Ready","ns=6;s=RO_FLAG_MZYVS_READY"]
["Flag_杀菌冲洗ing","ns=6;s=RO_FLAG_SJCX_ING"]
["杀菌剂允许","ns=6;s=RO_FLAG_SJJ_ALLOW"]
["Flag_杀菌剂run","ns=6;s=RO_FLAG_SJJ_RUN"]
["Flag_停机冲洗ing","ns=6;s=RO_FLAG_TJCX_ING"]
["Flag_全自动过滤ready","ns=6;s=RO_FLAG_TY_READY"]
["flag_药洗Ready","ns=6;s=RO_FLAG_YX_READY"]
["Flag_阻垢剂run","ns=6;s=RO_FLAG_ZGJ_RUN"]
["ERR_膜内有药","ns=6;s=RO_MNYY_ERR"]
["段间泵出口压力高","ns=6;s=RO_PDJB_CK_H"]
["段间泵进口压力低","ns=6;s=RO_PDJB_JK_L"]
["ERR_水泵故障","ns=6;s=RO_PUMP_ERR"]
["增压泵出口压力高","ns=6;s=RO_PZYB_CK_H"]
["增压泵进口压力低","ns=6;s=RO_PZYB_JK_L"]
["ERR_系统故障","ns=6;s=RO_SYSTEM_ERR"]
["ERR_压差I_H","ns=6;s=RO_TMP1_H_ERR"]
["ERR_压差I_HH","ns=6;s=RO_TMP1_HH_ERR"]
["ERR_压差II_H","ns=6;s=RO_TMP2_H_ERR"]
["ERR_压差II_HH","ns=6;s=RO_TMP2_HH_ERR"]
["ERR_压差III_H","ns=6;s=RO_TMP3_H_ERR"]
["ERR_压差III_HH","ns=6;s=RO_TMP3_HH_ERR"]
["ERR_压差高故障","ns=6;s=RO_TMPHH_ERR"]
["ERR_仪表故障","ns=6;s=RO_YB_ERR"]
["ERR_阀门故障","ns=6;s=RO_YV_ERR"]
["系统故障","ns=6;s=SYSTEM_ERR"]
["压差H","ns=6;s=TMP_H_ERR"]
["压差HH","ns=6;s=TMP_HH_ERR"]
["APPLY_13","ns=6;s=UF_APPLY_13"]
["APPLY_14","ns=6;s=UF_APPLY_14"]
["APPLY_15","ns=6;s=UF_APPLY_15"]
["Apply_9","ns=6;s=UF_APPLY_9"]
["Apply_BW_入栈","ns=6;s=UF_APPLY_BW_PUSH"]
["Apply_BWCEB_出栈","ns=6;s=UF_APPLY_BWCEB_POP"]
["Apply_CEB_入栈","ns=6;s=UF_APPLY_CEB_PUSH"]
["Apply_次钠加药","ns=6;s=UF_APPLY_CNJY"]
["Apply反洗泵BW","ns=6;s=UF_APPLY_FXB_BW"]
["Apply反洗泵CEB","ns=6;s=UF_APPLY_FXB_CEB"]
["Apply公共阀BW阀","ns=6;s=UF_APPLY_GGF_BWV"]
["Apply公共阀CEB阀","ns=6;s=UF_APPLY_GGF_CEBV"]
["Apply供水泵FW","ns=6;s=UF_APPLY_GSB_FW"]
["Apply_碱加药","ns=6;s=UF_APPLY_JJY"]
["Apply_PAC加药","ns=6;s=UF_APPLY_PACJY"]
["Apply_酸加药","ns=6;s=UF_APPLY_SJY"]
["Apply提升泵1","ns=6;s=UF_APPLY_TSB1"]
["Apply提升泵2","ns=6;s=UF_APPLY_TSB2"]
["UF_BTN_12","ns=6;s=UF_BTN_12"]
["UF_BTN_13","ns=6;s=UF_BTN_13"]
["UF_BTN_14","ns=6;s=UF_BTN_14"]
["UF_BTN_15","ns=6;s=UF_BTN_15"]
["UF_BTN_16","ns=6;s=UF_BTN_16"]
["UF_BTN_20","ns=6;s=UF_BTN_20"]
["UF_BTN_21","ns=6;s=UF_BTN_21"]
["UF_BTN_22","ns=6;s=UF_BTN_22"]
["UF_BTN_23","ns=6;s=UF_BTN_23"]
["CIP清洗：启动/停止","ns=6;s=UF_BTN_CIP"]
["半自动：反洗（脉冲）","ns=6;s=UF_BTN_CX"]
["急停","ns=6;s=UF_BTN_EMG"]
["故障复位","ns=6;s=UF_BTN_FAULT_RST"]
["初始化","ns=6;s=UF_BTN_INITIAL"]
["半自动：碱洗选择","ns=6;s=UF_BTN_JXZ"]
["累计流量清零","ns=6;s=UF_BTN_LL_CLEAR"]
["气擦洗屏蔽","ns=6;s=UF_BTN_QCXDIS"]
["半自动：CEB（脉冲）","ns=6;s=UF_BTN_SJX"]
["半自动：开机 (置位)","ns=6;s=UF_BTN_START"]
["半自动：停止（脉冲，复位01/03）","ns=6;s=UF_BTN_STOP"]
["半自动：水洗选择","ns=6;s=UF_BTN_SXXZ"]
["半自动：酸洗选择","ns=6;s=UF_BTN_SXZ"]
["全自动：投运/停机","ns=6;s=UF_BTN_TY"]
["液位开关屏蔽","ns=6;s=UF_BTN_YWKGDIS"]
["药剂残留","ns=6;s=UF_DRUG_ERR"]
["ERR_5","ns=6;s=UF_ERR_5"]
["ERR_6","ns=6;s=UF_ERR_6"]
["ERR_7","ns=6;s=UF_ERR_7"]
["FLAG_17","ns=6;s=UF_FLAG_17"]
["FLAG_18","ns=6;s=UF_FLAG_18"]
["FLAG_19","ns=6;s=UF_FLAG_19"]
["自动启动标志","ns=6;s=UF_FLAG_AUTOSTART"]
["反洗CEB阀准备好","ns=6;s=UF_FLAG_BWCEB_V_RY"]
["flag_CEB冲洗ing","ns=6;s=UF_FLAG_CEB_CX_ING"]
["flag_CEBing","ns=6;s=UF_FLAG_CEB_ING"]
["flag_CEB加药ing","ns=6;s=UF_FLAG_CEB_JY_ING"]
["flag_冲水过滤ing","ns=6;s=UF_FLAG_CSGL_ING"]
["flag_反洗ing","ns=6;s=UF_FLAG_FX_ING"]
["反洗准备好","ns=6;s=UF_FLAG_FX_READY"]
["flag_过滤end","ns=6;s=UF_FLAG_GL_END"]
["flag_过滤ing","ns=6;s=UF_FLAG_GL_ING"]
["过滤准备好","ns=6;s=UF_FLAG_GL_READY"]
["盐酸准备好","ns=6;s=UF_FLAG_HCL_READY"]
["碱洗准备好","ns=6;s=UF_FLAG_JX_READY"]
["产水池A连锁","ns=6;s=UF_FLAG_LS_CSCA"]
["产水池B连锁","ns=6;s=UF_FLAG_LS_CSCB"]
["进水池A连锁","ns=6;s=UF_FLAG_LS_JSCA"]
["进水池B连锁","ns=6;s=UF_FLAG_LS_JSCB"]
["反洗电机洗准备好","ns=6;s=UF_FLAG_M_BW_READY"]
["过滤电机准备好","ns=6;s=UF_FLAG_M_GL_READY"]
["flag_膜内有药ing","ns=6;s=UF_FLAG_MNYY_ING"]
["PAC洗准备好","ns=6;s=UF_FLAG_PAC_READY"]
["气洗准备好","ns=6;s=UF_FLAG_QX_READY"]
["水射器允许","ns=6;s=UF_FLAG_SSQ_ALLOW"]
["酸洗准备好","ns=6;s=UF_FLAG_SX_READY"]
["flag_全自动Ready","ns=6;s=UF_FLAG_TY_READT"]
["阀门准备好","ns=6;s=UF_FLAG_V_READY"]
["水洗准备好","ns=6;s=UF_FLAG_WW_READY"]
["系统故障","ns=6;s=UF_SYSTEM_ERR"]
["压差H","ns=6;s=UF_TMP_H_ERR"]
["压差HH","ns=6;s=UF_TMP_HH_ERR"]
["膜组阀门故障","ns=6;s=UF_VALVE_ERR"]
["加药间CIP补水阀手自动","ns=6;s=V_JY_CIPBS_BT_AUTO"]
["加药间CIP补水阀手动关","ns=6;s=V_JY_CIPBS_BT_CLOSE"]
["加药间CIP补水阀手动开","ns=6;s=V_JY_CIPBS_BT_OPEN"]
["加药间CIP补水阀故障复位","ns=6;s=V_JY_CIPBS_BT_RESET"]
["加药间CIP补水阀关到位","ns=6;s=V_JY_CIPBS_CFB"]
["加药间CIP补水阀关闭中","ns=6;s=V_JY_CIPBS_CING"]
["加药间CIP补水阀自动关闭","ns=6;s=V_JY_CIPBS_CLOSEAUTO"]
["加药间CIP补水阀故障","ns=6;s=V_JY_CIPBS_ERR"]
["加药间CIP补水阀总故障","ns=6;s=V_JY_CIPBS_ERRT"]
["加药间CIP补水阀开到位","ns=6;s=V_JY_CIPBS_OFB"]
["加药间CIP补水阀打开中","ns=6;s=V_JY_CIPBS_OING"]
["加药间CIP补水阀自动打开","ns=6;s=V_JY_CIPBS_OPENAUTO"]
["加药间CIP补水阀关闭","ns=6;s=V_JY_CIPBS_OUT_CLOSE"]
["加药间CIP补水阀打开","ns=6;s=V_JY_CIPBS_OUT_OPEN"]
["加药间CIP补水阀准备好","ns=6;s=V_JY_CIPBS_OUT_READY"]
["加药间CIP补水阀远程","ns=6;s=V_JY_CIPBS_REM"]
["加药间CIP排放阀手自动","ns=6;s=V_JY_CIPPF_BT_AUTO"]
["加药间CIP排放阀手动关","ns=6;s=V_JY_CIPPF_BT_CLOSE"]
["加药间CIP排放阀手动开","ns=6;s=V_JY_CIPPF_BT_OPEN"]
["加药间CIP排放阀故障复位","ns=6;s=V_JY_CIPPF_BT_RESET"]
["加药间CIP排放阀关到位","ns=6;s=V_JY_CIPPF_CFB"]
["加药间CIP排放阀关闭中","ns=6;s=V_JY_CIPPF_CING"]
["加药间CIP排放阀自动关闭","ns=6;s=V_JY_CIPPF_CLOSEAUTO"]
["加药间CIP排放阀故障","ns=6;s=V_JY_CIPPF_ERR"]
["加药间CIP排放阀总故障","ns=6;s=V_JY_CIPPF_ERRT"]
["加药间CIP排放阀开到位","ns=6;s=V_JY_CIPPF_OFB"]
["加药间CIP排放阀打开中","ns=6;s=V_JY_CIPPF_OING"]
["加药间CIP排放阀自动打开","ns=6;s=V_JY_CIPPF_OPENAUTO"]
["加药间CIP排放阀关闭","ns=6;s=V_JY_CIPPF_OUT_CLOSE"]
["加药间CIP排放阀打开","ns=6;s=V_JY_CIPPF_OUT_OPEN"]
["加药间CIP排放阀准备好","ns=6;s=V_JY_CIPPF_OUT_READY"]
["加药间CIP排放阀远程","ns=6;s=V_JY_CIPPF_REM"]
["RO产水箱补水阀手自动","ns=6;s=V_JY_CSBS_BT_AUTO"]
["RO产水箱补水阀手动关","ns=6;s=V_JY_CSBS_BT_CLOSE"]
["RO产水箱补水阀手动开","ns=6;s=V_JY_CSBS_BT_OPEN"]
["RO产水箱补水阀故障复位","ns=6;s=V_JY_CSBS_BT_RESET"]
["RO产水箱补水阀关到位","ns=6;s=V_JY_CSBS_CFB"]
["RO产水箱补水阀关闭中","ns=6;s=V_JY_CSBS_CING"]
["RO产水箱补水阀自动关闭","ns=6;s=V_JY_CSBS_CLOSEAUTO"]
["RO产水箱补水阀故障","ns=6;s=V_JY_CSBS_ERR"]
["RO产水箱补水阀总故障","ns=6;s=V_JY_CSBS_ERRT"]
["RO产水箱补水阀开到位","ns=6;s=V_JY_CSBS_OFB"]
["RO产水箱补水阀打开中","ns=6;s=V_JY_CSBS_OING"]
["RO产水箱补水阀自动打开","ns=6;s=V_JY_CSBS_OPENAUTO"]
["RO产水箱补水阀关闭","ns=6;s=V_JY_CSBS_OUT_CLOSE"]
["RO产水箱补水阀打开","ns=6;s=V_JY_CSBS_OUT_OPEN"]
["RO产水箱补水阀准备好","ns=6;s=V_JY_CSBS_OUT_READY"]
["RO产水箱补水阀远程","ns=6;s=V_JY_CSBS_REM"]
["加药间冲洗阀手自动","ns=6;s=V_JY_CX_BT_AUTO"]
["加药间冲洗阀手动关","ns=6;s=V_JY_CX_BT_CLOSE"]
["加药间冲洗阀手动开","ns=6;s=V_JY_CX_BT_OPEN"]
["加药间冲洗阀故障复位","ns=6;s=V_JY_CX_BT_RESET"]
["加药间冲洗阀关到位","ns=6;s=V_JY_CX_CFB"]
["加药间冲洗阀关闭中","ns=6;s=V_JY_CX_CING"]
["加药间冲洗阀自动关闭","ns=6;s=V_JY_CX_CLOSEAUTO"]
["加药间冲洗阀故障","ns=6;s=V_JY_CX_ERR"]
["加药间冲洗阀总故障","ns=6;s=V_JY_CX_ERRT"]
["加药间冲洗阀开到位","ns=6;s=V_JY_CX_OFB"]
["加药间冲洗阀打开中","ns=6;s=V_JY_CX_OING"]
["加药间冲洗阀自动打开","ns=6;s=V_JY_CX_OPENAUTO"]
["加药间冲洗阀关闭","ns=6;s=V_JY_CX_OUT_CLOSE"]
["加药间冲洗阀打开","ns=6;s=V_JY_CX_OUT_OPEN"]
["加药间冲洗阀准备好","ns=6;s=V_JY_CX_OUT_READY"]
["加药间冲洗阀远程","ns=6;s=V_JY_CX_REM"]
["UF废水外排阀手自动","ns=6;s=V_JY_UFFS_BT_AUTO"]
["UF废水外排阀手动关","ns=6;s=V_JY_UFFS_BT_CLOSE"]
["UF废水外排阀手动开","ns=6;s=V_JY_UFFS_BT_OPEN"]
["UF废水外排阀故障复位","ns=6;s=V_JY_UFFS_BT_RESET"]
["UF废水外排阀关到位","ns=6;s=V_JY_UFFS_CFB"]
["UF废水外排阀关闭中","ns=6;s=V_JY_UFFS_CING"]
["UF废水外排阀自动关闭","ns=6;s=V_JY_UFFS_CLOSEAUTO"]
["UF废水外排阀故障","ns=6;s=V_JY_UFFS_ERR"]
["UF废水外排阀总故障","ns=6;s=V_JY_UFFS_ERRT"]
["UF废水外排阀开到位","ns=6;s=V_JY_UFFS_OFB"]
["UF废水外排阀打开中","ns=6;s=V_JY_UFFS_OING"]
["UF废水外排阀自动打开","ns=6;s=V_JY_UFFS_OPENAUTO"]
["UF废水外排阀关闭","ns=6;s=V_JY_UFFS_OUT_CLOSE"]
["UF废水外排阀打开","ns=6;s=V_JY_UFFS_OUT_OPEN"]
["UF废水外排阀准备好","ns=6;s=V_JY_UFFS_OUT_READY"]
["UF废水外排阀远程","ns=6;s=V_JY_UFFS_REM"]
["加药间CIP循环阀手自动","ns=6;s=V_JY_VIPXH_BT_AUTO"]
["加药间CIP循环阀手动关","ns=6;s=V_JY_VIPXH_BT_CLOSE"]
["加药间CIP循环阀手动开","ns=6;s=V_JY_VIPXH_BT_OPEN"]
["加药间CIP循环阀故障复位","ns=6;s=V_JY_VIPXH_BT_RESET"]
["加药间CIP循环阀关到位","ns=6;s=V_JY_VIPXH_CFB"]
["加药间CIP循环阀关闭中","ns=6;s=V_JY_VIPXH_CING"]
["加药间CIP循环阀自动关闭","ns=6;s=V_JY_VIPXH_CLOSEAUTO"]
["加药间CIP循环阀故障","ns=6;s=V_JY_VIPXH_ERR"]
["加药间CIP循环阀总故障","ns=6;s=V_JY_VIPXH_ERRT"]
["加药间CIP循环阀开到位","ns=6;s=V_JY_VIPXH_OFB"]
["加药间CIP循环阀打开中","ns=6;s=V_JY_VIPXH_OING"]
["加药间CIP循环阀自动打开","ns=6;s=V_JY_VIPXH_OPENAUTO"]
["加药间CIP循环阀关闭","ns=6;s=V_JY_VIPXH_OUT_CLOSE"]
["加药间CIP循环阀打开","ns=6;s=V_JY_VIPXH_OUT_OPEN"]
["加药间CIP循环阀准备好","ns=6;s=V_JY_VIPXH_OUT_READY"]
["加药间CIP循环阀远程","ns=6;s=V_JY_VIPXH_REM"]
["RO外供水阀手自动","ns=6;s=V_JY_WG_BT_AUTO"]
["RO外供水阀手动关","ns=6;s=V_JY_WG_BT_CLOSE"]
["RO外供水阀手动开","ns=6;s=V_JY_WG_BT_OPEN"]
["RO外供水阀故障复位","ns=6;s=V_JY_WG_BT_RESET"]
["RO外供水阀关到位","ns=6;s=V_JY_WG_CFB"]
["RO外供水阀关闭中","ns=6;s=V_JY_WG_CING"]
["RO外供水阀自动关闭","ns=6;s=V_JY_WG_CLOSEAUTO"]
["RO外供水阀故障","ns=6;s=V_JY_WG_ERR"]
["RO外供水阀总故障","ns=6;s=V_JY_WG_ERRT"]
["RO外供水阀开到位","ns=6;s=V_JY_WG_OFB"]
["RO外供水阀打开中","ns=6;s=V_JY_WG_OING"]
["RO外供水阀自动打开","ns=6;s=V_JY_WG_OPENAUTO"]
["RO外供水阀关闭","ns=6;s=V_JY_WG_OUT_CLOSE"]
["RO外供水阀打开","ns=6;s=V_JY_WG_OUT_OPEN"]
["RO外供水阀准备好","ns=6;s=V_JY_WG_OUT_READY"]
["RO外供水阀远程","ns=6;s=V_JY_WG_REM"]
["加药间外供碱阀手自动","ns=6;s=V_JY_WGJ_BT_AUTO"]
["加药间外供碱阀手动关","ns=6;s=V_JY_WGJ_BT_CLOSE"]
["加药间外供碱阀手动开","ns=6;s=V_JY_WGJ_BT_OPEN"]
["加药间外供碱阀故障复位","ns=6;s=V_JY_WGJ_BT_RESET"]
["加药间外供碱阀关到位","ns=6;s=V_JY_WGJ_CFB"]
["加药间外供碱阀关闭中","ns=6;s=V_JY_WGJ_CING"]
["加药间外供碱阀自动关闭","ns=6;s=V_JY_WGJ_CLOSEAUTO"]
["加药间外供碱阀故障","ns=6;s=V_JY_WGJ_ERR"]
["加药间外供碱阀总故障","ns=6;s=V_JY_WGJ_ERRT"]
["加药间外供碱阀开到位","ns=6;s=V_JY_WGJ_OFB"]
["加药间外供碱阀打开中","ns=6;s=V_JY_WGJ_OING"]
["加药间外供碱阀自动打开","ns=6;s=V_JY_WGJ_OPENAUTO"]
["加药间外供碱阀关闭","ns=6;s=V_JY_WGJ_OUT_CLOSE"]
["加药间外供碱阀打开","ns=6;s=V_JY_WGJ_OUT_OPEN"]
["加药间外供碱阀准备好","ns=6;s=V_JY_WGJ_OUT_READY"]
["加药间外供碱阀远程","ns=6;s=V_JY_WGJ_REM"]
["RO不合格水阀手自动","ns=6;s=V_RO_BHGF_BT_AUTO"]
["RO不合格水阀手动关","ns=6;s=V_RO_BHGF_BT_CLOSE"]
["RO不合格水阀手动开","ns=6;s=V_RO_BHGF_BT_OPEN"]
["RO不合格水阀故障复位","ns=6;s=V_RO_BHGF_BT_RESET"]
["RO不合格水阀关到位","ns=6;s=V_RO_BHGF_CFB"]
["RO不合格水阀关闭中","ns=6;s=V_RO_BHGF_CING"]
["RO不合格水阀自动关闭","ns=6;s=V_RO_BHGF_CLOSEAUTO"]
["RO不合格水阀故障","ns=6;s=V_RO_BHGF_ERR"]
["RO不合格水阀总故障","ns=6;s=V_RO_BHGF_ERRT"]
["RO不合格水阀开到位","ns=6;s=V_RO_BHGF_OFB"]
["RO不合格水阀打开中","ns=6;s=V_RO_BHGF_OING"]
["RO不合格水阀自动打开","ns=6;s=V_RO_BHGF_OPENAUTO"]
["RO不合格水阀关闭","ns=6;s=V_RO_BHGF_OUT_CLOSE"]
["RO不合格水阀打开","ns=6;s=V_RO_BHGF_OUT_OPEN"]
["RO不合格水阀准备好","ns=6;s=V_RO_BHGF_OUT_READY"]
["RO不合格水阀远程","ns=6;s=V_RO_BHGF_REM"]
["RO备用阀3手自动","ns=6;s=V_RO_BY3_BT_AUTO"]
["RO备用阀3手动关","ns=6;s=V_RO_BY3_BT_CLOSE"]
["RO备用阀3手动开","ns=6;s=V_RO_BY3_BT_OPEN"]
["RO备用阀3故障复位","ns=6;s=V_RO_BY3_BT_RESET"]
["RO备用阀3关到位","ns=6;s=V_RO_BY3_CFB"]
["RO备用阀3关闭中","ns=6;s=V_RO_BY3_CING"]
["RO备用阀3自动关闭","ns=6;s=V_RO_BY3_CLOSEAUTO"]
["RO备用阀3故障","ns=6;s=V_RO_BY3_ERR"]
["RO备用阀3总故障","ns=6;s=V_RO_BY3_ERRT"]
["RO备用阀3开到位","ns=6;s=V_RO_BY3_OFB"]
["RO备用阀3打开中","ns=6;s=V_RO_BY3_OING"]
["RO备用阀3自动打开","ns=6;s=V_RO_BY3_OPENAUTO"]
["RO备用阀3关闭","ns=6;s=V_RO_BY3_OUT_CLOSE"]
["RO备用阀3打开","ns=6;s=V_RO_BY3_OUT_OPEN"]
["RO备用阀3准备好","ns=6;s=V_RO_BY3_OUT_READY"]
["RO备用阀3远程","ns=6;s=V_RO_BY3_REM"]
["RO备用阀4手自动","ns=6;s=V_RO_BY4_BT_AUTO"]
["RO备用阀4手动关","ns=6;s=V_RO_BY4_BT_CLOSE"]
["RO备用阀4手动开","ns=6;s=V_RO_BY4_BT_OPEN"]
["RO备用阀4故障复位","ns=6;s=V_RO_BY4_BT_RESET"]
["RO备用阀4关到位","ns=6;s=V_RO_BY4_CFB"]
["RO备用阀4关闭中","ns=6;s=V_RO_BY4_CING"]
["RO备用阀4自动关闭","ns=6;s=V_RO_BY4_CLOSEAUTO"]
["RO备用阀4故障","ns=6;s=V_RO_BY4_ERR"]
["RO备用阀4总故障","ns=6;s=V_RO_BY4_ERRT"]
["RO备用阀4开到位","ns=6;s=V_RO_BY4_OFB"]
["RO备用阀4打开中","ns=6;s=V_RO_BY4_OING"]
["RO备用阀4自动打开","ns=6;s=V_RO_BY4_OPENAUTO"]
["RO备用阀4关闭","ns=6;s=V_RO_BY4_OUT_CLOSE"]
["RO备用阀4打开","ns=6;s=V_RO_BY4_OUT_OPEN"]
["RO备用阀4准备好","ns=6;s=V_RO_BY4_OUT_READY"]
["RO备用阀4远程","ns=6;s=V_RO_BY4_REM"]
["RO生化进水阀手自动","ns=6;s=V_RO_BYF1_BT_AUTO"]
["RO生化进水阀手动关","ns=6;s=V_RO_BYF1_BT_CLOSE"]
["RO生化进水阀手动开","ns=6;s=V_RO_BYF1_BT_OPEN"]
["RO生化进水阀故障复位","ns=6;s=V_RO_BYF1_BT_RESET"]
["RO生化进水阀关到位","ns=6;s=V_RO_BYF1_CFB"]
["RO生化进水阀关闭中","ns=6;s=V_RO_BYF1_CING"]
["RO生化进水阀自动关闭","ns=6;s=V_RO_BYF1_CLOSEAUTO"]
["RO生化进水阀故障","ns=6;s=V_RO_BYF1_ERR"]
["RO生化进水阀总故障","ns=6;s=V_RO_BYF1_ERRT"]
["RO生化进水阀开到位","ns=6;s=V_RO_BYF1_OFB"]
["RO生化进水阀打开中","ns=6;s=V_RO_BYF1_OING"]
["RO生化进水阀自动打开","ns=6;s=V_RO_BYF1_OPENAUTO"]
["RO生化进水阀关闭","ns=6;s=V_RO_BYF1_OUT_CLOSE"]
["RO生化进水阀打开","ns=6;s=V_RO_BYF1_OUT_OPEN"]
["RO生化进水阀准备好","ns=6;s=V_RO_BYF1_OUT_READY"]
["RO生化进水阀远程","ns=6;s=V_RO_BYF1_REM"]
["RO备用阀手自动","ns=6;s=V_RO_BYF2_BT_AUTO"]
["RO备用阀手动关","ns=6;s=V_RO_BYF2_BT_CLOSE"]
["RO备用阀手动开","ns=6;s=V_RO_BYF2_BT_OPEN"]
["RO备用阀故障复位","ns=6;s=V_RO_BYF2_BT_RESET"]
["RO备用阀关到位","ns=6;s=V_RO_BYF2_CFB"]
["RO备用阀关闭中","ns=6;s=V_RO_BYF2_CING"]
["RO备用阀自动关闭","ns=6;s=V_RO_BYF2_CLOSEAUTO"]
["RO备用阀故障","ns=6;s=V_RO_BYF2_ERR"]
["RO备用阀总故障","ns=6;s=V_RO_BYF2_ERRT"]
["RO备用阀开到位","ns=6;s=V_RO_BYF2_OFB"]
["RO备用阀打开中","ns=6;s=V_RO_BYF2_OING"]
["RO备用阀自动打开","ns=6;s=V_RO_BYF2_OPENAUTO"]
["RO备用阀关闭","ns=6;s=V_RO_BYF2_OUT_CLOSE"]
["RO备用阀打开","ns=6;s=V_RO_BYF2_OUT_OPEN"]
["RO备用阀准备好","ns=6;s=V_RO_BYF2_OUT_READY"]
["RO备用阀远程","ns=6;s=V_RO_BYF2_REM"]
["RO产水阀手自动","ns=6;s=V_RO_CSF_BT_AUTO"]
["RO产水阀手动关","ns=6;s=V_RO_CSF_BT_CLOSE"]
["RO产水阀手动开","ns=6;s=V_RO_CSF_BT_OPEN"]
["RO产水阀故障复位","ns=6;s=V_RO_CSF_BT_RESET"]
["RO产水阀关到位","ns=6;s=V_RO_CSF_CFB"]
["RO产水阀关闭中","ns=6;s=V_RO_CSF_CING"]
["RO产水阀自动关闭","ns=6;s=V_RO_CSF_CLOSEAUTO"]
["RO产水阀故障","ns=6;s=V_RO_CSF_ERR"]
["RO产水阀总故障","ns=6;s=V_RO_CSF_ERRT"]
["RO产水阀开到位","ns=6;s=V_RO_CSF_OFB"]
["RO产水阀打开中","ns=6;s=V_RO_CSF_OING"]
["RO产水阀自动打开","ns=6;s=V_RO_CSF_OPENAUTO"]
["RO产水阀关闭","ns=6;s=V_RO_CSF_OUT_CLOSE"]
["RO产水阀打开","ns=6;s=V_RO_CSF_OUT_OPEN"]
["RO产水阀准备好","ns=6;s=V_RO_CSF_OUT_READY"]
["RO产水阀远程","ns=6;s=V_RO_CSF_REM"]
["RO冲洗进水阀手自动","ns=6;s=V_RO_CXJSF_BT_AUTO"]
["RO冲洗进水阀手动关","ns=6;s=V_RO_CXJSF_BT_CLOSE"]
["RO冲洗进水阀手动开","ns=6;s=V_RO_CXJSF_BT_OPEN"]
["RO冲洗进水阀故障复位","ns=6;s=V_RO_CXJSF_BT_RESET"]
["RO冲洗进水阀关到位","ns=6;s=V_RO_CXJSF_CFB"]
["RO冲洗进水阀关闭中","ns=6;s=V_RO_CXJSF_CING"]
["RO冲洗进水阀自动关闭","ns=6;s=V_RO_CXJSF_CLOSEAUTO"]
["RO冲洗进水阀故障","ns=6;s=V_RO_CXJSF_ERR"]
["RO冲洗进水阀总故障","ns=6;s=V_RO_CXJSF_ERRT"]
["RO冲洗进水阀开到位","ns=6;s=V_RO_CXJSF_OFB"]
["RO冲洗进水阀打开中","ns=6;s=V_RO_CXJSF_OING"]
["RO冲洗进水阀自动打开","ns=6;s=V_RO_CXJSF_OPENAUTO"]
["RO冲洗进水阀关闭","ns=6;s=V_RO_CXJSF_OUT_CLOSE"]
["RO冲洗进水阀打开","ns=6;s=V_RO_CXJSF_OUT_OPEN"]
["RO冲洗进水阀准备好","ns=6;s=V_RO_CXJSF_OUT_READY"]
["RO冲洗进水阀远程","ns=6;s=V_RO_CXJSF_REM"]
["RO冲洗排水阀手自动","ns=6;s=V_RO_CXPSF_BT_AUTO"]
["RO冲洗排水阀手动关","ns=6;s=V_RO_CXPSF_BT_CLOSE"]
["RO冲洗排水阀手动开","ns=6;s=V_RO_CXPSF_BT_OPEN"]
["RO冲洗排水阀故障复位","ns=6;s=V_RO_CXPSF_BT_RESET"]
["RO冲洗排水阀关到位","ns=6;s=V_RO_CXPSF_CFB"]
["RO冲洗排水阀关闭中","ns=6;s=V_RO_CXPSF_CING"]
["RO冲洗排水阀自动关闭","ns=6;s=V_RO_CXPSF_CLOSEAUTO"]
["RO冲洗排水阀故障","ns=6;s=V_RO_CXPSF_ERR"]
["RO冲洗排水阀总故障","ns=6;s=V_RO_CXPSF_ERRT"]
["RO冲洗排水阀开到位","ns=6;s=V_RO_CXPSF_OFB"]
["RO冲洗排水阀打开中","ns=6;s=V_RO_CXPSF_OING"]
["RO冲洗排水阀自动打开","ns=6;s=V_RO_CXPSF_OPENAUTO"]
["RO冲洗排水阀关闭","ns=6;s=V_RO_CXPSF_OUT_CLOSE"]
["RO冲洗排水阀打开","ns=6;s=V_RO_CXPSF_OUT_OPEN"]
["RO冲洗排水阀准备好","ns=6;s=V_RO_CXPSF_OUT_READY"]
["RO冲洗排水阀远程","ns=6;s=V_RO_CXPSF_REM"]
["RO一段反洗进水阀手自动","ns=6;s=V_RO_FJSF_BT_AUTO"]
["RO一段反洗进水阀手动关","ns=6;s=V_RO_FJSF_BT_CLOSE"]
["RO一段反洗进水阀手动开","ns=6;s=V_RO_FJSF_BT_OPEN"]
["RO一段反洗进水阀故障复位","ns=6;s=V_RO_FJSF_BT_RESET"]
["RO一段反洗进水阀关到位","ns=6;s=V_RO_FJSF_CFB"]
["RO一段反洗进水阀关闭中","ns=6;s=V_RO_FJSF_CING"]
["RO一段反洗进水阀自动关闭","ns=6;s=V_RO_FJSF_CLOSEAUTO"]
["RO一段反洗进水阀故障","ns=6;s=V_RO_FJSF_ERR"]
["RO一段反洗进水阀总故障","ns=6;s=V_RO_FJSF_ERRT"]
["RO一段反洗进水阀开到位","ns=6;s=V_RO_FJSF_OFB"]
["RO一段反洗进水阀打开中","ns=6;s=V_RO_FJSF_OING"]
["RO一段反洗进水阀自动打开","ns=6;s=V_RO_FJSF_OPENAUTO"]
["RO一段反洗进水阀关闭","ns=6;s=V_RO_FJSF_OUT_CLOSE"]
["RO一段反洗进水阀打开","ns=6;s=V_RO_FJSF_OUT_OPEN"]
["RO一段反洗进水阀准备好","ns=6;s=V_RO_FJSF_OUT_READY"]
["RO一段反洗进水阀远程","ns=6;s=V_RO_FJSF_REM"]
["RO一段反洗排水阀手自动","ns=6;s=V_RO_FPSF_BT_AUTO"]
["RO一段反洗排水阀手动关","ns=6;s=V_RO_FPSF_BT_CLOSE"]
["RO一段反洗排水阀手动开","ns=6;s=V_RO_FPSF_BT_OPEN"]
["RO一段反洗排水阀故障复位","ns=6;s=V_RO_FPSF_BT_RESET"]
["RO一段反洗排水阀关到位","ns=6;s=V_RO_FPSF_CFB"]
["RO一段反洗排水阀关闭中","ns=6;s=V_RO_FPSF_CING"]
["RO一段反洗排水阀自动关闭","ns=6;s=V_RO_FPSF_CLOSEAUTO"]
["RO一段反洗排水阀故障","ns=6;s=V_RO_FPSF_ERR"]
["RO一段反洗排水阀总故障","ns=6;s=V_RO_FPSF_ERRT"]
["RO一段反洗排水阀开到位","ns=6;s=V_RO_FPSF_OFB"]
["RO一段反洗排水阀打开中","ns=6;s=V_RO_FPSF_OING"]
["RO一段反洗排水阀自动打开","ns=6;s=V_RO_FPSF_OPENAUTO"]
["RO一段反洗排水阀关闭","ns=6;s=V_RO_FPSF_OUT_CLOSE"]
["RO一段反洗排水阀打开","ns=6;s=V_RO_FPSF_OUT_OPEN"]
["RO一段反洗排水阀准备好","ns=6;s=V_RO_FPSF_OUT_READY"]
["RO一段反洗排水阀远程","ns=6;s=V_RO_FPSF_REM"]
["RO还原剂阀手自动","ns=6;s=V_RO_HYJF_BT_AUTO"]
["RO还原剂阀手动关","ns=6;s=V_RO_HYJF_BT_CLOSE"]
["RO还原剂阀手动开","ns=6;s=V_RO_HYJF_BT_OPEN"]
["RO还原剂阀故障复位","ns=6;s=V_RO_HYJF_BT_RESET"]
["RO还原剂阀关到位","ns=6;s=V_RO_HYJF_CFB"]
["RO还原剂阀关闭中","ns=6;s=V_RO_HYJF_CING"]
["RO还原剂阀自动关闭","ns=6;s=V_RO_HYJF_CLOSEAUTO"]
["RO还原剂阀故障","ns=6;s=V_RO_HYJF_ERR"]
["RO还原剂阀总故障","ns=6;s=V_RO_HYJF_ERRT"]
["RO还原剂阀开到位","ns=6;s=V_RO_HYJF_OFB"]
["RO还原剂阀打开中","ns=6;s=V_RO_HYJF_OING"]
["RO还原剂阀自动打开","ns=6;s=V_RO_HYJF_OPENAUTO"]
["RO还原剂阀关闭","ns=6;s=V_RO_HYJF_OUT_CLOSE"]
["RO还原剂阀打开","ns=6;s=V_RO_HYJF_OUT_OPEN"]
["RO还原剂阀准备好","ns=6;s=V_RO_HYJF_OUT_READY"]
["RO还原剂阀远程","ns=6;s=V_RO_HYJF_REM"]
["RO进水阀手自动","ns=6;s=V_RO_JSF_BT_AUTO"]
["RO进水阀手动关","ns=6;s=V_RO_JSF_BT_CLOSE"]
["RO进水阀手动开","ns=6;s=V_RO_JSF_BT_OPEN"]
["RO进水阀故障复位","ns=6;s=V_RO_JSF_BT_RESET"]
["RO进水阀关到位","ns=6;s=V_RO_JSF_CFB"]
["RO进水阀关闭中","ns=6;s=V_RO_JSF_CING"]
["RO进水阀自动关闭","ns=6;s=V_RO_JSF_CLOSEAUTO"]
["RO进水阀故障","ns=6;s=V_RO_JSF_ERR"]
["RO进水阀总故障","ns=6;s=V_RO_JSF_ERRT"]
["RO进水阀开到位","ns=6;s=V_RO_JSF_OFB"]
["RO进水阀打开中","ns=6;s=V_RO_JSF_OING"]
["RO进水阀自动打开","ns=6;s=V_RO_JSF_OPENAUTO"]
["RO进水阀关闭","ns=6;s=V_RO_JSF_OUT_CLOSE"]
["RO进水阀打开","ns=6;s=V_RO_JSF_OUT_OPEN"]
["RO进水阀准备好","ns=6;s=V_RO_JSF_OUT_READY"]
["RO进水阀远程","ns=6;s=V_RO_JSF_REM"]
["RO排气阀1手自动","ns=6;s=V_RO_PQF1_BT_AUTO"]
["RO排气阀1手动关","ns=6;s=V_RO_PQF1_BT_CLOSE"]
["RO排气阀1手动开","ns=6;s=V_RO_PQF1_BT_OPEN"]
["RO排气阀1故障复位","ns=6;s=V_RO_PQF1_BT_RESET"]
["RO排气阀1关到位","ns=6;s=V_RO_PQF1_CFB"]
["RO排气阀1关闭中","ns=6;s=V_RO_PQF1_CING"]
["RO排气阀1自动关闭","ns=6;s=V_RO_PQF1_CLOSEAUTO"]
["RO排气阀1故障","ns=6;s=V_RO_PQF1_ERR"]
["RO排气阀1总故障","ns=6;s=V_RO_PQF1_ERRT"]
["RO排气阀1开到位","ns=6;s=V_RO_PQF1_OFB"]
["RO排气阀1打开中","ns=6;s=V_RO_PQF1_OING"]
["RO排气阀1自动打开","ns=6;s=V_RO_PQF1_OPENAUTO"]
["RO排气阀1关闭","ns=6;s=V_RO_PQF1_OUT_CLOSE"]
["RO排气阀1打开","ns=6;s=V_RO_PQF1_OUT_OPEN"]
["RO排气阀1准备好","ns=6;s=V_RO_PQF1_OUT_READY"]
["RO排气阀1远程","ns=6;s=V_RO_PQF1_REM"]
["RO排气阀2手自动","ns=6;s=V_RO_PQF2_BT_AUTO"]
["RO排气阀2手动关","ns=6;s=V_RO_PQF2_BT_CLOSE"]
["RO排气阀2手动开","ns=6;s=V_RO_PQF2_BT_OPEN"]
["RO排气阀2故障复位","ns=6;s=V_RO_PQF2_BT_RESET"]
["RO排气阀2关到位","ns=6;s=V_RO_PQF2_CFB"]
["RO排气阀2关闭中","ns=6;s=V_RO_PQF2_CING"]
["RO排气阀2自动关闭","ns=6;s=V_RO_PQF2_CLOSEAUTO"]
["RO排气阀2故障","ns=6;s=V_RO_PQF2_ERR"]
["RO排气阀2总故障","ns=6;s=V_RO_PQF2_ERRT"]
["RO排气阀2开到位","ns=6;s=V_RO_PQF2_OFB"]
["RO排气阀2打开中","ns=6;s=V_RO_PQF2_OING"]
["RO排气阀2自动打开","ns=6;s=V_RO_PQF2_OPENAUTO"]
["RO排气阀2关闭","ns=6;s=V_RO_PQF2_OUT_CLOSE"]
["RO排气阀2打开","ns=6;s=V_RO_PQF2_OUT_OPEN"]
["RO排气阀2准备好","ns=6;s=V_RO_PQF2_OUT_READY"]
["RO排气阀2远程","ns=6;s=V_RO_PQF2_REM"]
["RO排气阀3手自动","ns=6;s=V_RO_PQF3_BT_AUTO"]
["RO排气阀3手动关","ns=6;s=V_RO_PQF3_BT_CLOSE"]
["RO排气阀3手动开","ns=6;s=V_RO_PQF3_BT_OPEN"]
["RO排气阀3故障复位","ns=6;s=V_RO_PQF3_BT_RESET"]
["RO排气阀3关到位","ns=6;s=V_RO_PQF3_CFB"]
["RO排气阀3关闭中","ns=6;s=V_RO_PQF3_CING"]
["RO排气阀3自动关闭","ns=6;s=V_RO_PQF3_CLOSEAUTO"]
["RO排气阀3故障","ns=6;s=V_RO_PQF3_ERR"]
["RO排气阀3总故障","ns=6;s=V_RO_PQF3_ERRT"]
["RO排气阀3开到位","ns=6;s=V_RO_PQF3_OFB"]
["RO排气阀3打开中","ns=6;s=V_RO_PQF3_OING"]
["RO排气阀3自动打开","ns=6;s=V_RO_PQF3_OPENAUTO"]
["RO排气阀3关闭","ns=6;s=V_RO_PQF3_OUT_CLOSE"]
["RO排气阀3打开","ns=6;s=V_RO_PQF3_OUT_OPEN"]
["RO排气阀3准备好","ns=6;s=V_RO_PQF3_OUT_READY"]
["RO排气阀3远程","ns=6;s=V_RO_PQF3_REM"]
["RO排气阀4手自动","ns=6;s=V_RO_PQF4_BT_AUTO"]
["RO排气阀4手动关","ns=6;s=V_RO_PQF4_BT_CLOSE"]
["RO排气阀4手动开","ns=6;s=V_RO_PQF4_BT_OPEN"]
["RO排气阀4故障复位","ns=6;s=V_RO_PQF4_BT_RESET"]
["RO排气阀4关到位","ns=6;s=V_RO_PQF4_CFB"]
["RO排气阀4关闭中","ns=6;s=V_RO_PQF4_CING"]
["RO排气阀4自动关闭","ns=6;s=V_RO_PQF4_CLOSEAUTO"]
["RO排气阀4故障","ns=6;s=V_RO_PQF4_ERR"]
["RO排气阀4总故障","ns=6;s=V_RO_PQF4_ERRT"]
["RO排气阀4开到位","ns=6;s=V_RO_PQF4_OFB"]
["RO排气阀4打开中","ns=6;s=V_RO_PQF4_OING"]
["RO排气阀4自动打开","ns=6;s=V_RO_PQF4_OPENAUTO"]
["RO排气阀4关闭","ns=6;s=V_RO_PQF4_OUT_CLOSE"]
["RO排气阀4打开","ns=6;s=V_RO_PQF4_OUT_OPEN"]
["RO排气阀4准备好","ns=6;s=V_RO_PQF4_OUT_READY"]
["RO排气阀4远程","ns=6;s=V_RO_PQF4_REM"]
["RO排气阀5手自动","ns=6;s=V_RO_PQF5_BT_AUTO"]
["RO排气阀5手动关","ns=6;s=V_RO_PQF5_BT_CLOSE"]
["RO排气阀5手动开","ns=6;s=V_RO_PQF5_BT_OPEN"]
["RO排气阀5故障复位","ns=6;s=V_RO_PQF5_BT_RESET"]
["RO排气阀5关到位","ns=6;s=V_RO_PQF5_CFB"]
["RO排气阀5关闭中","ns=6;s=V_RO_PQF5_CING"]
["RO排气阀5自动关闭","ns=6;s=V_RO_PQF5_CLOSEAUTO"]
["RO排气阀5故障","ns=6;s=V_RO_PQF5_ERR"]
["RO排气阀5总故障","ns=6;s=V_RO_PQF5_ERRT"]
["RO排气阀5开到位","ns=6;s=V_RO_PQF5_OFB"]
["RO排气阀5打开中","ns=6;s=V_RO_PQF5_OING"]
["RO排气阀5自动打开","ns=6;s=V_RO_PQF5_OPENAUTO"]
["RO排气阀5关闭","ns=6;s=V_RO_PQF5_OUT_CLOSE"]
["RO排气阀5打开","ns=6;s=V_RO_PQF5_OUT_OPEN"]
["RO排气阀5准备好","ns=6;s=V_RO_PQF5_OUT_READY"]
["RO排气阀5远程","ns=6;s=V_RO_PQF5_REM"]
["RO排气阀6手自动","ns=6;s=V_RO_PQF6_BT_AUTO"]
["RO排气阀6手动关","ns=6;s=V_RO_PQF6_BT_CLOSE"]
["RO排气阀6手动开","ns=6;s=V_RO_PQF6_BT_OPEN"]
["RO排气阀6故障复位","ns=6;s=V_RO_PQF6_BT_RESET"]
["RO排气阀6关到位","ns=6;s=V_RO_PQF6_CFB"]
["RO排气阀6关闭中","ns=6;s=V_RO_PQF6_CING"]
["RO排气阀6自动关闭","ns=6;s=V_RO_PQF6_CLOSEAUTO"]
["RO排气阀6故障","ns=6;s=V_RO_PQF6_ERR"]
["RO排气阀6总故障","ns=6;s=V_RO_PQF6_ERRT"]
["RO排气阀6开到位","ns=6;s=V_RO_PQF6_OFB"]
["RO排气阀6打开中","ns=6;s=V_RO_PQF6_OING"]
["RO排气阀6自动打开","ns=6;s=V_RO_PQF6_OPENAUTO"]
["RO排气阀6关闭","ns=6;s=V_RO_PQF6_OUT_CLOSE"]
["RO排气阀6打开","ns=6;s=V_RO_PQF6_OUT_OPEN"]
["RO排气阀6准备好","ns=6;s=V_RO_PQF6_OUT_READY"]
["RO排气阀6远程","ns=6;s=V_RO_PQF6_REM"]
["RO排气阀7手自动","ns=6;s=V_RO_PQF7_BT_AUTO"]
["RO排气阀7手动关","ns=6;s=V_RO_PQF7_BT_CLOSE"]
["RO排气阀7手动开","ns=6;s=V_RO_PQF7_BT_OPEN"]
["RO排气阀7故障复位","ns=6;s=V_RO_PQF7_BT_RESET"]
["RO排气阀7关到位","ns=6;s=V_RO_PQF7_CFB"]
["RO排气阀7关闭中","ns=6;s=V_RO_PQF7_CING"]
["RO排气阀7自动关闭","ns=6;s=V_RO_PQF7_CLOSEAUTO"]
["RO排气阀7故障","ns=6;s=V_RO_PQF7_ERR"]
["RO排气阀7总故障","ns=6;s=V_RO_PQF7_ERRT"]
["RO排气阀7开到位","ns=6;s=V_RO_PQF7_OFB"]
["RO排气阀7打开中","ns=6;s=V_RO_PQF7_OING"]
["RO排气阀7自动打开","ns=6;s=V_RO_PQF7_OPENAUTO"]
["RO排气阀7关闭","ns=6;s=V_RO_PQF7_OUT_CLOSE"]
["RO排气阀7打开","ns=6;s=V_RO_PQF7_OUT_OPEN"]
["RO排气阀7准备好","ns=6;s=V_RO_PQF7_OUT_READY"]
["RO排气阀7远程","ns=6;s=V_RO_PQF7_REM"]
["RO排气阀8手自动","ns=6;s=V_RO_PQF8_BT_AUTO"]
["RO排气阀8手动关","ns=6;s=V_RO_PQF8_BT_CLOSE"]
["RO排气阀8手动开","ns=6;s=V_RO_PQF8_BT_OPEN"]
["RO排气阀8故障复位","ns=6;s=V_RO_PQF8_BT_RESET"]
["RO排气阀8关到位","ns=6;s=V_RO_PQF8_CFB"]
["RO排气阀8关闭中","ns=6;s=V_RO_PQF8_CING"]
["RO排气阀8自动关闭","ns=6;s=V_RO_PQF8_CLOSEAUTO"]
["RO排气阀8故障","ns=6;s=V_RO_PQF8_ERR"]
["RO排气阀8总故障","ns=6;s=V_RO_PQF8_ERRT"]
["RO排气阀8开到位","ns=6;s=V_RO_PQF8_OFB"]
["RO排气阀8打开中","ns=6;s=V_RO_PQF8_OING"]
["RO排气阀8自动打开","ns=6;s=V_RO_PQF8_OPENAUTO"]
["RO排气阀8关闭","ns=6;s=V_RO_PQF8_OUT_CLOSE"]
["RO排气阀8打开","ns=6;s=V_RO_PQF8_OUT_OPEN"]
["RO排气阀8准备好","ns=6;s=V_RO_PQF8_OUT_READY"]
["RO排气阀8远程","ns=6;s=V_RO_PQF8_REM"]
["RO排气阀9手自动","ns=6;s=V_RO_PQF9_BT_AUTO"]
["RO排气阀9手动关","ns=6;s=V_RO_PQF9_BT_CLOSE"]
["RO排气阀9手动开","ns=6;s=V_RO_PQF9_BT_OPEN"]
["RO排气阀9故障复位","ns=6;s=V_RO_PQF9_BT_RESET"]
["RO排气阀9关到位","ns=6;s=V_RO_PQF9_CFB"]
["RO排气阀9关闭中","ns=6;s=V_RO_PQF9_CING"]
["RO排气阀9自动关闭","ns=6;s=V_RO_PQF9_CLOSEAUTO"]
["RO排气阀9故障","ns=6;s=V_RO_PQF9_ERR"]
["RO排气阀9总故障","ns=6;s=V_RO_PQF9_ERRT"]
["RO排气阀9开到位","ns=6;s=V_RO_PQF9_OFB"]
["RO排气阀9打开中","ns=6;s=V_RO_PQF9_OING"]
["RO排气阀9自动打开","ns=6;s=V_RO_PQF9_OPENAUTO"]
["RO排气阀9关闭","ns=6;s=V_RO_PQF9_OUT_CLOSE"]
["RO排气阀9打开","ns=6;s=V_RO_PQF9_OUT_OPEN"]
["RO排气阀9准备好","ns=6;s=V_RO_PQF9_OUT_READY"]
["RO排气阀9远程","ns=6;s=V_RO_PQF9_REM"]
["RO杀菌剂阀手自动","ns=6;s=V_RO_SJJF_BT_AUTO"]
["RO杀菌剂阀手动关","ns=6;s=V_RO_SJJF_BT_CLOSE"]
["RO杀菌剂阀手动开","ns=6;s=V_RO_SJJF_BT_OPEN"]
["RO杀菌剂阀故障复位","ns=6;s=V_RO_SJJF_BT_RESET"]
["RO杀菌剂阀关到位","ns=6;s=V_RO_SJJF_CFB"]
["RO杀菌剂阀关闭中","ns=6;s=V_RO_SJJF_CING"]
["RO杀菌剂阀自动关闭","ns=6;s=V_RO_SJJF_CLOSEAUTO"]
["RO杀菌剂阀故障","ns=6;s=V_RO_SJJF_ERR"]
["RO杀菌剂阀总故障","ns=6;s=V_RO_SJJF_ERRT"]
["RO杀菌剂阀开到位","ns=6;s=V_RO_SJJF_OFB"]
["RO杀菌剂阀打开中","ns=6;s=V_RO_SJJF_OING"]
["RO杀菌剂阀自动打开","ns=6;s=V_RO_SJJF_OPENAUTO"]
["RO杀菌剂阀关闭","ns=6;s=V_RO_SJJF_OUT_CLOSE"]
["RO杀菌剂阀打开","ns=6;s=V_RO_SJJF_OUT_OPEN"]
["RO杀菌剂阀准备好","ns=6;s=V_RO_SJJF_OUT_READY"]
["RO杀菌剂阀远程","ns=6;s=V_RO_SJJF_REM"]
["RO阻垢剂阀手自动","ns=6;s=V_RO_ZGJF_BT_AUTO"]
["RO阻垢剂阀手动关","ns=6;s=V_RO_ZGJF_BT_CLOSE"]
["RO阻垢剂阀手动开","ns=6;s=V_RO_ZGJF_BT_OPEN"]
["RO阻垢剂阀故障复位","ns=6;s=V_RO_ZGJF_BT_RESET"]
["RO阻垢剂阀关到位","ns=6;s=V_RO_ZGJF_CFB"]
["RO阻垢剂阀关闭中","ns=6;s=V_RO_ZGJF_CING"]
["RO阻垢剂阀自动关闭","ns=6;s=V_RO_ZGJF_CLOSEAUTO"]
["RO阻垢剂阀故障","ns=6;s=V_RO_ZGJF_ERR"]
["RO阻垢剂阀总故障","ns=6;s=V_RO_ZGJF_ERRT"]
["RO阻垢剂阀开到位","ns=6;s=V_RO_ZGJF_OFB"]
["RO阻垢剂阀打开中","ns=6;s=V_RO_ZGJF_OING"]
["RO阻垢剂阀自动打开","ns=6;s=V_RO_ZGJF_OPENAUTO"]
["RO阻垢剂阀关闭","ns=6;s=V_RO_ZGJF_OUT_CLOSE"]
["RO阻垢剂阀打开","ns=6;s=V_RO_ZGJF_OUT_OPEN"]
["RO阻垢剂阀准备好","ns=6;s=V_RO_ZGJF_OUT_READY"]
["RO阻垢剂阀远程","ns=6;s=V_RO_ZGJF_REM"]
["UF曝气阀手自动","ns=6;s=V_UF_BQF_BT_AUTO"]
["UF曝气阀手动关","ns=6;s=V_UF_BQF_BT_CLOSE"]
["UF曝气阀手动开","ns=6;s=V_UF_BQF_BT_OPEN"]
["UF曝气阀故障复位","ns=6;s=V_UF_BQF_BT_RESET"]
["UF曝气阀关到位","ns=6;s=V_UF_BQF_CFB"]
["UF曝气阀关闭中","ns=6;s=V_UF_BQF_CING"]
["UF曝气阀自动关闭","ns=6;s=V_UF_BQF_CLOSEAUTO"]
["UF曝气阀故障","ns=6;s=V_UF_BQF_ERR"]
["UF曝气阀总故障","ns=6;s=V_UF_BQF_ERRT"]
["UF曝气阀开到位","ns=6;s=V_UF_BQF_OFB"]
["UF曝气阀打开中","ns=6;s=V_UF_BQF_OING"]
["UF曝气阀自动打开","ns=6;s=V_UF_BQF_OPENAUTO"]
["UF曝气阀关闭","ns=6;s=V_UF_BQF_OUT_CLOSE"]
["UF曝气阀打开","ns=6;s=V_UF_BQF_OUT_OPEN"]
["UF曝气阀准备好","ns=6;s=V_UF_BQF_OUT_READY"]
["UF曝气阀远程","ns=6;s=V_UF_BQF_REM"]
["UF备用阀手自动","ns=6;s=V_UF_BYF_BT_AUTO"]
["UF备用阀手动关","ns=6;s=V_UF_BYF_BT_CLOSE"]
["UF备用阀手动开","ns=6;s=V_UF_BYF_BT_OPEN"]
["UF备用阀故障复位","ns=6;s=V_UF_BYF_BT_RESET"]
["UF备用阀关到位","ns=6;s=V_UF_BYF_CFB"]
["UF备用阀关闭中","ns=6;s=V_UF_BYF_CING"]
["UF备用阀自动关闭","ns=6;s=V_UF_BYF_CLOSEAUTO"]
["UF备用阀故障","ns=6;s=V_UF_BYF_ERR"]
["UF备用阀总故障","ns=6;s=V_UF_BYF_ERRT"]
["UF备用阀开到位","ns=6;s=V_UF_BYF_OFB"]
["UF备用阀打开中","ns=6;s=V_UF_BYF_OING"]
["UF备用阀自动打开","ns=6;s=V_UF_BYF_OPENAUTO"]
["UF备用阀关闭","ns=6;s=V_UF_BYF_OUT_CLOSE"]
["UF备用阀打开","ns=6;s=V_UF_BYF_OUT_OPEN"]
["UF备用阀准备好","ns=6;s=V_UF_BYF_OUT_READY"]
["UF备用阀远程","ns=6;s=V_UF_BYF_REM"]
["UF次钠加药阀手自动","ns=6;s=V_UF_CNF_BT_AUTO"]
["UF次钠加药阀手动关","ns=6;s=V_UF_CNF_BT_CLOSE"]
["UF次钠加药阀手动开","ns=6;s=V_UF_CNF_BT_OPEN"]
["UF次钠加药阀故障复位","ns=6;s=V_UF_CNF_BT_RESET"]
["UF次钠加药阀关到位","ns=6;s=V_UF_CNF_CFB"]
["UF次钠加药阀关闭中","ns=6;s=V_UF_CNF_CING"]
["UF次钠加药阀自动关闭","ns=6;s=V_UF_CNF_CLOSEAUTO"]
["UF次钠加药阀故障","ns=6;s=V_UF_CNF_ERR"]
["UF次钠加药阀总故障","ns=6;s=V_UF_CNF_ERRT"]
["UF次钠加药阀开到位","ns=6;s=V_UF_CNF_OFB"]
["UF次钠加药阀打开中","ns=6;s=V_UF_CNF_OING"]
["UF次钠加药阀自动打开","ns=6;s=V_UF_CNF_OPENAUTO"]
["UF次钠加药阀关闭","ns=6;s=V_UF_CNF_OUT_CLOSE"]
["UF次钠加药阀打开","ns=6;s=V_UF_CNF_OUT_OPEN"]
["UF次钠加药阀准备好","ns=6;s=V_UF_CNF_OUT_READY"]
["UF次钠加药阀远程","ns=6;s=V_UF_CNF_REM"]
["UF产水阀手自动","ns=6;s=V_UF_CSF_BT_AUTO"]
["UF产水阀手动关","ns=6;s=V_UF_CSF_BT_CLOSE"]
["UF产水阀手动开","ns=6;s=V_UF_CSF_BT_OPEN"]
["UF产水阀故障复位","ns=6;s=V_UF_CSF_BT_RESET"]
["UF产水阀关到位","ns=6;s=V_UF_CSF_CFB"]
["UF产水阀关闭中","ns=6;s=V_UF_CSF_CING"]
["UF产水阀自动关闭","ns=6;s=V_UF_CSF_CLOSEAUTO"]
["UF产水阀故障","ns=6;s=V_UF_CSF_ERR"]
["UF产水阀总故障","ns=6;s=V_UF_CSF_ERRT"]
["UF产水阀开到位","ns=6;s=V_UF_CSF_OFB"]
["UF产水阀打开中","ns=6;s=V_UF_CSF_OING"]
["UF产水阀自动打开","ns=6;s=V_UF_CSF_OPENAUTO"]
["UF产水阀关闭","ns=6;s=V_UF_CSF_OUT_CLOSE"]
["UF产水阀打开","ns=6;s=V_UF_CSF_OUT_OPEN"]
["UF产水阀准备好","ns=6;s=V_UF_CSF_OUT_READY"]
["UF产水阀远程","ns=6;s=V_UF_CSF_REM"]
["UF反洗阀手自动","ns=6;s=V_UF_FXF_BT_AUTO"]
["UF反洗阀手动关","ns=6;s=V_UF_FXF_BT_CLOSE"]
["UF反洗阀手动开","ns=6;s=V_UF_FXF_BT_OPEN"]
["UF反洗阀故障复位","ns=6;s=V_UF_FXF_BT_RESET"]
["UF反洗阀关到位","ns=6;s=V_UF_FXF_CFB"]
["UF反洗阀关闭中","ns=6;s=V_UF_FXF_CING"]
["UF反洗阀自动关闭","ns=6;s=V_UF_FXF_CLOSEAUTO"]
["UF反洗阀故障","ns=6;s=V_UF_FXF_ERR"]
["UF反洗阀总故障","ns=6;s=V_UF_FXF_ERRT"]
["UF反洗阀开到位","ns=6;s=V_UF_FXF_OFB"]
["UF反洗阀打开中","ns=6;s=V_UF_FXF_OING"]
["UF反洗阀自动打开","ns=6;s=V_UF_FXF_OPENAUTO"]
["UF反洗阀关闭","ns=6;s=V_UF_FXF_OUT_CLOSE"]
["UF反洗阀打开","ns=6;s=V_UF_FXF_OUT_OPEN"]
["UF反洗阀准备好","ns=6;s=V_UF_FXF_OUT_READY"]
["UF反洗阀远程","ns=6;s=V_UF_FXF_REM"]
["UF还原阀手自动","ns=6;s=V_UF_HYF_BT_AUTO"]
["UF还原阀手动关","ns=6;s=V_UF_HYF_BT_CLOSE"]
["UF还原阀手动开","ns=6;s=V_UF_HYF_BT_OPEN"]
["UF还原阀故障复位","ns=6;s=V_UF_HYF_BT_RESET"]
["UF还原阀关到位","ns=6;s=V_UF_HYF_CFB"]
["UF还原阀关闭中","ns=6;s=V_UF_HYF_CING"]
["UF还原阀自动关闭","ns=6;s=V_UF_HYF_CLOSEAUTO"]
["UF还原阀故障","ns=6;s=V_UF_HYF_ERR"]
["UF还原阀总故障","ns=6;s=V_UF_HYF_ERRT"]
["UF还原阀开到位","ns=6;s=V_UF_HYF_OFB"]
["UF还原阀打开中","ns=6;s=V_UF_HYF_OING"]
["UF还原阀自动打开","ns=6;s=V_UF_HYF_OPENAUTO"]
["UF还原阀关闭","ns=6;s=V_UF_HYF_OUT_CLOSE"]
["UF还原阀打开","ns=6;s=V_UF_HYF_OUT_OPEN"]
["UF还原阀准备好","ns=6;s=V_UF_HYF_OUT_READY"]
["UF还原阀远程","ns=6;s=V_UF_HYF_REM"]
["UF碱加药阀手自动","ns=6;s=V_UF_JF_BT_AUTO"]
["UF碱加药阀手动关","ns=6;s=V_UF_JF_BT_CLOSE"]
["UF碱加药阀手动开","ns=6;s=V_UF_JF_BT_OPEN"]
["UF碱加药阀故障复位","ns=6;s=V_UF_JF_BT_RESET"]
["UF碱加药阀关到位","ns=6;s=V_UF_JF_CFB"]
["UF碱加药阀关闭中","ns=6;s=V_UF_JF_CING"]
["UF碱加药阀自动关闭","ns=6;s=V_UF_JF_CLOSEAUTO"]
["UF碱加药阀故障","ns=6;s=V_UF_JF_ERR"]
["UF碱加药阀总故障","ns=6;s=V_UF_JF_ERRT"]
["UF碱加药阀开到位","ns=6;s=V_UF_JF_OFB"]
["UF碱加药阀打开中","ns=6;s=V_UF_JF_OING"]
["UF碱加药阀自动打开","ns=6;s=V_UF_JF_OPENAUTO"]
["UF碱加药阀关闭","ns=6;s=V_UF_JF_OUT_CLOSE"]
["UF碱加药阀打开","ns=6;s=V_UF_JF_OUT_OPEN"]
["UF碱加药阀准备好","ns=6;s=V_UF_JF_OUT_READY"]
["UF碱加药阀远程","ns=6;s=V_UF_JF_REM"]
["UF进水阀手自动","ns=6;s=V_UF_JSF_BT_AUTO"]
["UF进水阀手动关","ns=6;s=V_UF_JSF_BT_CLOSE"]
["UF进水阀手动开","ns=6;s=V_UF_JSF_BT_OPEN"]
["UF进水阀故障复位","ns=6;s=V_UF_JSF_BT_RESET"]
["UF进水阀关到位","ns=6;s=V_UF_JSF_CFB"]
["UF进水阀关闭中","ns=6;s=V_UF_JSF_CING"]
["UF进水阀自动关闭","ns=6;s=V_UF_JSF_CLOSEAUTO"]
["UF进水阀故障","ns=6;s=V_UF_JSF_ERR"]
["UF进水阀总故障","ns=6;s=V_UF_JSF_ERRT"]
["UF进水阀开到位","ns=6;s=V_UF_JSF_OFB"]
["UF进水阀打开中","ns=6;s=V_UF_JSF_OING"]
["UF进水阀自动打开","ns=6;s=V_UF_JSF_OPENAUTO"]
["UF进水阀关闭","ns=6;s=V_UF_JSF_OUT_CLOSE"]
["UF进水阀打开","ns=6;s=V_UF_JSF_OUT_OPEN"]
["UF进水阀准备好","ns=6;s=V_UF_JSF_OUT_READY"]
["UF进水阀远程","ns=6;s=V_UF_JSF_REM"]
["UF排空阀手自动","ns=6;s=V_UF_PKF_BT_AUTO"]
["UF排空阀手动关","ns=6;s=V_UF_PKF_BT_CLOSE"]
["UF排空阀手动开","ns=6;s=V_UF_PKF_BT_OPEN"]
["UF排空阀故障复位","ns=6;s=V_UF_PKF_BT_RESET"]
["UF排空阀关到位","ns=6;s=V_UF_PKF_CFB"]
["UF排空阀关闭中","ns=6;s=V_UF_PKF_CING"]
["UF排空阀自动关闭","ns=6;s=V_UF_PKF_CLOSEAUTO"]
["UF排空阀故障","ns=6;s=V_UF_PKF_ERR"]
["UF排空阀总故障","ns=6;s=V_UF_PKF_ERRT"]
["UF排空阀开到位","ns=6;s=V_UF_PKF_OFB"]
["UF排空阀打开中","ns=6;s=V_UF_PKF_OING"]
["UF排空阀自动打开","ns=6;s=V_UF_PKF_OPENAUTO"]
["UF排空阀关闭","ns=6;s=V_UF_PKF_OUT_CLOSE"]
["UF排空阀打开","ns=6;s=V_UF_PKF_OUT_OPEN"]
["UF排空阀准备好","ns=6;s=V_UF_PKF_OUT_READY"]
["UF排空阀远程","ns=6;s=V_UF_PKF_REM"]
["UF酸加药阀手自动","ns=6;s=V_UF_SF_BT_AUTO"]
["UF酸加药阀手动关","ns=6;s=V_UF_SF_BT_CLOSE"]
["UF酸加药阀手动开","ns=6;s=V_UF_SF_BT_OPEN"]
["UF酸加药阀故障复位","ns=6;s=V_UF_SF_BT_RESET"]
["UF酸加药阀关到位","ns=6;s=V_UF_SF_CFB"]
["UF酸加药阀关闭中","ns=6;s=V_UF_SF_CING"]
["UF酸加药阀自动关闭","ns=6;s=V_UF_SF_CLOSEAUTO"]
["UF酸加药阀故障","ns=6;s=V_UF_SF_ERR"]
["UF酸加药阀总故障","ns=6;s=V_UF_SF_ERRT"]
["UF酸加药阀开到位","ns=6;s=V_UF_SF_OFB"]
["UF酸加药阀打开中","ns=6;s=V_UF_SF_OING"]
["UF酸加药阀自动打开","ns=6;s=V_UF_SF_OPENAUTO"]
["UF酸加药阀关闭","ns=6;s=V_UF_SF_OUT_CLOSE"]
["UF酸加药阀打开","ns=6;s=V_UF_SF_OUT_OPEN"]
["UF酸加药阀准备好","ns=6;s=V_UF_SF_OUT_READY"]
["UF酸加药阀远程","ns=6;s=V_UF_SF_REM"]
["UF水射器电磁阀手自动","ns=6;s=V_UF_SSQF_BT_AUTO"]
["UF水射器电磁阀手动关","ns=6;s=V_UF_SSQF_BT_CLOSE"]
["UF水射器电磁阀手动开","ns=6;s=V_UF_SSQF_BT_OPEN"]
["UF水射器电磁阀故障复位","ns=6;s=V_UF_SSQF_BT_RESET"]
["UF水射器电磁阀关到位","ns=6;s=V_UF_SSQF_CFB"]
["UF水射器电磁阀关闭中","ns=6;s=V_UF_SSQF_CING"]
["UF水射器电磁阀自动关闭","ns=6;s=V_UF_SSQF_CLOSEAUTO"]
["UF水射器电磁阀故障","ns=6;s=V_UF_SSQF_ERR"]
["UF水射器电磁阀总故障","ns=6;s=V_UF_SSQF_ERRT"]
["UF水射器电磁阀开到位","ns=6;s=V_UF_SSQF_OFB"]
["UF水射器电磁阀打开中","ns=6;s=V_UF_SSQF_OING"]
["UF水射器电磁阀自动打开","ns=6;s=V_UF_SSQF_OPENAUTO"]
["UF水射器电磁阀关闭","ns=6;s=V_UF_SSQF_OUT_CLOSE"]
["UF水射器电磁阀打开","ns=6;s=V_UF_SSQF_OUT_OPEN"]
["UF水射器电磁阀准备好","ns=6;s=V_UF_SSQF_OUT_READY"]
["UF水射器电磁阀远程","ns=6;s=V_UF_SSQF_REM"]
["UF中和外排阀手自动","ns=6;s=V_UF_ZHWPF_BT_AUTO"]
["UF中和外排阀手动关","ns=6;s=V_UF_ZHWPF_BT_CLOSE"]
["UF中和外排阀手动开","ns=6;s=V_UF_ZHWPF_BT_OPEN"]
["UF中和外排阀故障复位","ns=6;s=V_UF_ZHWPF_BT_RESET"]
["UF中和外排阀关到位","ns=6;s=V_UF_ZHWPF_CFB"]
["UF中和外排阀关闭中","ns=6;s=V_UF_ZHWPF_CING"]
["UF中和外排阀自动关闭","ns=6;s=V_UF_ZHWPF_CLOSEAUTO"]
["UF中和外排阀故障","ns=6;s=V_UF_ZHWPF_ERR"]
["UF中和外排阀总故障","ns=6;s=V_UF_ZHWPF_ERRT"]
["UF中和外排阀开到位","ns=6;s=V_UF_ZHWPF_OFB"]
["UF中和外排阀打开中","ns=6;s=V_UF_ZHWPF_OING"]
["UF中和外排阀自动打开","ns=6;s=V_UF_ZHWPF_OPENAUTO"]
["UF中和外排阀关闭","ns=6;s=V_UF_ZHWPF_OUT_CLOSE"]
["UF中和外排阀打开","ns=6;s=V_UF_ZHWPF_OUT_OPEN"]
["UF中和外排阀准备好","ns=6;s=V_UF_ZHWPF_OUT_READY"]
["UF中和外排阀远程","ns=6;s=V_UF_ZHWPF_REM"]
["UF中和循环阀手自动","ns=6;s=V_UF_ZHXHF_BT_AUTO"]
["UF中和循环阀手动关","ns=6;s=V_UF_ZHXHF_BT_CLOSE"]
["UF中和循环阀手动开","ns=6;s=V_UF_ZHXHF_BT_OPEN"]
["UF中和循环阀故障复位","ns=6;s=V_UF_ZHXHF_BT_RESET"]
["UF中和循环阀关到位","ns=6;s=V_UF_ZHXHF_CFB"]
["UF中和循环阀关闭中","ns=6;s=V_UF_ZHXHF_CING"]
["UF中和循环阀自动关闭","ns=6;s=V_UF_ZHXHF_CLOSEAUTO"]
["UF中和循环阀故障","ns=6;s=V_UF_ZHXHF_ERR"]
["UF中和循环阀总故障","ns=6;s=V_UF_ZHXHF_ERRT"]
["UF中和循环阀开到位","ns=6;s=V_UF_ZHXHF_OFB"]
["UF中和循环阀打开中","ns=6;s=V_UF_ZHXHF_OING"]
["UF中和循环阀自动打开","ns=6;s=V_UF_ZHXHF_OPENAUTO"]
["UF中和循环阀关闭","ns=6;s=V_UF_ZHXHF_OUT_CLOSE"]
["UF中和循环阀打开","ns=6;s=V_UF_ZHXHF_OUT_OPEN"]
["UF中和循环阀准备好","ns=6;s=V_UF_ZHXHF_OUT_READY"]
["UF中和循环阀远程","ns=6;s=V_UF_ZHXHF_REM"]
["膜组阀门故障","ns=6;s=VALVE_ERR"]
["空气流量计反馈","ns=3;s=AI_JYAIR_OUT"]
["空压机压变1反馈","ns=3;s=AI_JYAIRYL1_OUT"]
["空压机压变2反馈","ns=3;s=AI_JYAIRYL2_OUT"]
["反馈","ns=3;s=AI_JYBY1_OUT"]
["反馈","ns=3;s=AI_JYBY2_OUT"]
["反馈备用","ns=3;s=AI_JYBY3_OUT"]
["备用反馈","ns=3;s=AI_JYBY4_OUT"]
["备用反馈","ns=3;s=AI_JYBY5_OUT"]
["CIP泵频率反馈","ns=3;s=AI_JYCIPB_FR_OUT"]
["CIPph反馈","ns=3;s=AI_JYCIPPH_OUT"]
["cip清洗流量计反馈","ns=3;s=AI_JYCIPQXLL_OUT"]
["次钠液位反馈","ns=3;s=AI_JYCNYW_OUT"]
["外供水电导反馈","ns=3;s=AI_JYCSDD_OUT"]
["产水流量计1反馈","ns=3;s=AI_JYCSLL1_OUT"]
["产水流量计2反馈","ns=3;s=AI_JYCSLL2_OUT"]
["外供水PH反馈","ns=3;s=AI_JYCSPH_OUT"]
["产水温度反馈","ns=3;s=AI_JYCSWD_OUT"]
["产水压力变送器反馈","ns=3;s=AI_JYCSYL_OUT"]
["反洗风机频率反馈","ns=3;s=AI_JYFJ_FR_OUT"]
["还原剂液位反馈","ns=3;s=AI_JYHYJYW_OUT"]
["高级生物进水流量计反馈","ns=3;s=AI_JYJSLL1_OUT"]
["Y2B进水流量计反馈","ns=3;s=AI_JYJSLL2_OUT"]
["碱液位反馈","ns=3;s=AI_JYJYW_OUT"]
["备用反馈","ns=3;s=AI_JYNS_OUT"]
["清洗水箱液位计反馈","ns=3;s=AI_JYQXSXYW_OUT"]
["反渗透产水液位计反馈","ns=3;s=AI_JYROCSYW_OUT"]
["杀菌剂液位反馈","ns=3;s=AI_JYSJJYW_OUT"]
["酸液位反馈","ns=3;s=AI_JYSYW_OUT"]
["超滤产水液位计反馈","ns=3;s=AI_JYUFCSYW_OUT"]
["超滤提升泵液位计反馈","ns=3;s=AI_JYUFTSBYW_OUT"]
["尾水排放流量计反馈","ns=3;s=AI_JYWSLL_OUT"]
["阻垢剂液位反馈","ns=3;s=AI_JYZGJYW_OUT"]
["二段产水流量反馈","ns=3;s=AI_RO2DCSLL_OUT"]
["备用反馈1","ns=3;s=AI_ROBY_OUT"]
["产水电导反馈","ns=3;s=AI_ROCSDD_OUT"]
["产水压力反馈","ns=3;s=AI_ROCSYL_OUT"]
["RO段间泵频率反馈","ns=3;s=AI_RODJB_FR_OUT"]
["段间泵进口压力反馈","ns=3;s=AI_RODJJKYL_OUT"]
["段间压力反馈","ns=3;s=AI_RODJYL_OUT"]
["RO供水泵频率反馈","ns=3;s=AI_ROGSB_FR_OUT"]
["RO高压泵频率反馈","ns=3;s=AI_ROGYB_FR_OUT"]
["进水电导反馈","ns=3;s=AI_ROJSDD_OUT"]
["进水流量反馈","ns=3;s=AI_ROJSLL_OUT"]
["进水ORP反馈","ns=3;s=AI_ROJSORP_OUT"]
["进水PH反馈","ns=3;s=AI_ROJSPH_OUT"]
["进水压力反馈","ns=3;s=AI_ROJSYL_OUT"]
["浓水流量反馈","ns=3;s=AI_RONSLL_OUT"]
["浓水压力反馈","ns=3;s=AI_RONSYL_OUT"]
["空压机流量反馈","ns=3;s=AI_UFAIR_OUT"]
["反馈备用1","ns=3;s=AI_UFBY1_OUT"]
["反馈备用2","ns=3;s=AI_UFBY2_OUT"]
["反馈备用3","ns=3;s=AI_UFBY3_OUT"]
["反馈备用4","ns=3;s=AI_UFBY4_OUT"]
["UF产水泵频率反馈","ns=3;s=AI_UFCSB_FR_OUT"]
["UF产水流量反馈","ns=3;s=AI_UFCSLL_OUT"]
["UF产水压力反馈","ns=3;s=AI_UFCSYL_OUT"]
["UF产水浊度反馈","ns=3;s=AI_UFCSZD_OUT"]
["UF反洗泵频率反馈","ns=3;s=AI_UFFXB_FR_OUT"]
["UF反洗流量反馈","ns=3;s=AI_UFFXLL_OUT"]
["UF进水ORP反馈","ns=3;s=AI_UFJSORP_OUT"]
["UF进水ph反馈","ns=3;s=AI_UFJSPH_OUT"]
["UF进水温度反馈","ns=3;s=AI_UFJSYW_OUT"]
["UF进水浊度反馈","ns=3;s=AI_UFJSZD_OUT"]
["UF膜堆液位反馈","ns=3;s=AI_UFMDYW_OUT"]
["UF排空泵频率反馈","ns=3;s=AI_UFPKB_FR_OUT"]
["UF提升泵1频率反馈","ns=3;s=AI_UFTSB1_FR_OUT"]
["UF提升泵2频率反馈","ns=3;s=AI_UFTSB2_FR_OUT"]
["真空管液位反馈","ns=3;s=AI_UFZKGYW_OUT"]
["中和水箱液位高高限值","ns=3;s=ALARM_ZHSX_HHR"]
["中和水箱液位高限值","ns=3;s=ALARM_ZHSX_HR"]
["中和水箱液位","ns=3;s=ALARM_ZHSX_IN"]
["中和水箱液位低低限值","ns=3;s=ALARM_ZHSX_LLR"]
["中和水箱液位低限值","ns=3;s=ALARM_ZHSX_LR"]
["还原剂搅拌器频率反馈","ns=3;s=JBQ_JY_HYJ_FRE_FB"]
["还原剂搅拌器频率设定","ns=3;s=JBQ_JY_HYJ_FRESET"]
["还原剂搅拌器运行时间","ns=3;s=JBQ_JY_HYJ_RUNTIME"]
["加热器1频率反馈","ns=3;s=JBQ_JY_JRQ1_FRE_FB"]
["加热器1频率设定","ns=3;s=JBQ_JY_JRQ1_FRESET"]
["加热器1运行时间","ns=3;s=JBQ_JY_JRQ1_RUNTIME"]
["加热器2频率反馈","ns=3;s=JBQ_JY_JRQ2_FRE_FB"]
["加热器2频率设定","ns=3;s=JBQ_JY_JRQ2_FRESET"]
["加热器2运行时间","ns=3;s=JBQ_JY_JRQ2_RUNTIME"]
["溶药箱搅拌器频率反馈","ns=3;s=JBQ_JY_RYX_FRE_FB"]
["溶药箱搅拌器频率设定","ns=3;s=JBQ_JY_RYX_FRESET"]
["溶药箱搅拌器运行时间","ns=3;s=JBQ_JY_RYX_RUNTIME"]
["酸搅拌器频率反馈","ns=3;s=JBQ_JY_S_FRE_FB"]
["酸搅拌器频率设定","ns=3;s=JBQ_JY_S_FRESET"]
["酸搅拌器运行时间","ns=3;s=JBQ_JY_S_RUNTIME"]
["杀菌剂搅拌器频率反馈","ns=3;s=JBQ_JY_SJJ_FRE_FB"]
["杀菌剂搅拌器频率设定","ns=3;s=JBQ_JY_SJJ_FRESET"]
["杀菌剂搅拌器运行时间","ns=3;s=JBQ_JY_SJJ_RUNTIME"]
["阻垢剂搅拌器频率反馈","ns=3;s=JBQ_JY_ZGJ_FRE_FB"]
["阻垢剂搅拌器频率设定","ns=3;s=JBQ_JY_ZGJ_FRESET"]
["阻垢剂搅拌器运行时间","ns=3;s=JBQ_JY_ZGJ_RUNTIME"]
["备用高设定","ns=3;s=LOCK_BY_H"]
["备用高高设定","ns=3;s=LOCK_BY_HH"]
["备用低设定","ns=3;s=LOCK_BY_L"]
["备用低低设定","ns=3;s=LOCK_BY_LL"]
["备用中设定","ns=3;s=LOCK_BY_M"]
["CIP液位高设定","ns=3;s=LOCK_CIPYW_H"]
["CIP液位高高设定","ns=3;s=LOCK_CIPYW_HH"]
["CIP液位低设定","ns=3;s=LOCK_CIPYW_L"]
["CIP液位低低设定","ns=3;s=LOCK_CIPYW_LL"]
["CIP液位中设定","ns=3;s=LOCK_CIPYW_M"]
["膜池液位高设定","ns=3;s=LOCK_MCYW_H"]
["膜池液位高高设定","ns=3;s=LOCK_MCYW_HH"]
["膜池液位低设定","ns=3;s=LOCK_MCYW_L"]
["膜池液位低低设定","ns=3;s=LOCK_MCYW_LL"]
["膜池液位中设定","ns=3;s=LOCK_MCYW_M"]
["RO产水电导高设定","ns=3;s=LOCK_ROCSDD_H"]
["RO产水电导高高设定","ns=3;s=LOCK_ROCSDD_HH"]
["RO产水电导低设定","ns=3;s=LOCK_ROCSDD_L"]
["RO产水电导低低设定","ns=3;s=LOCK_ROCSDD_LL"]
["RO产水电导中设定","ns=3;s=LOCK_ROCSDD_M"]
["RO产水池液位高设定","ns=3;s=LOCK_ROCSYW_H"]
["RO产水池液位高高设定","ns=3;s=LOCK_ROCSYW_HH"]
["RO产水池液位低设定","ns=3;s=LOCK_ROCSYW_L"]
["RO产水池液位低低设定","ns=3;s=LOCK_ROCSYW_LL"]
["RO产水池液位中设定","ns=3;s=LOCK_ROCSYW_M"]
["水射器液位高设定","ns=3;s=LOCK_SSQYW_H"]
["水射器液位高高设定","ns=3;s=LOCK_SSQYW_HH"]
["水射器液位低设定","ns=3;s=LOCK_SSQYW_L"]
["水射器液位低低设定","ns=3;s=LOCK_SSQYW_LL"]
["水射器液位中设定","ns=3;s=LOCK_SSQYW_M"]
["UF产水池液位高设定","ns=3;s=LOCK_UFCSYW_H"]
["UF产水池液位高高设定","ns=3;s=LOCK_UFCSYW_HH"]
["UF产水池液位低设定","ns=3;s=LOCK_UFCSYW_L"]
["UF产水池液位低低设定","ns=3;s=LOCK_UFCSYW_LL"]
["UF产水池液位中设定","ns=3;s=LOCK_UFCSYW_M"]
["UF进水池液位高设定","ns=3;s=LOCK_UFJSYW_H"]
["UF进水池液位高高设定","ns=3;s=LOCK_UFJSYW_HH"]
["UF进水池液位低设定","ns=3;s=LOCK_UFJSYW_L"]
["UF进水池液位低低设定","ns=3;s=LOCK_UFJSYW_LL"]
["UF进水池液位中设定","ns=3;s=LOCK_UFJSYW_M"]
["UF ORP值高设定","ns=3;s=LOCK_UFORP_H"]
["UF ORP值高高设定","ns=3;s=LOCK_UFORP_HH"]
["UF ORP值低设定","ns=3;s=LOCK_UFORP_L"]
["UF ORP值低低设定","ns=3;s=LOCK_UFORP_LL"]
["UF ORP值中设定","ns=3;s=LOCK_UFORP_M"]
["UF PH值高设定","ns=3;s=LOCK_UFPH_H"]
["UF PH值高高设定","ns=3;s=LOCK_UFPH_HH"]
["UF PH值低设定","ns=3;s=LOCK_UFPH_L"]
["UF PH值低低设定","ns=3;s=LOCK_UFPH_LL"]
["UF PH值中设定","ns=3;s=LOCK_UFPH_M"]
["CEB还原剂加药泵1频率反馈","ns=3;s=P_CEB_HYJ1_FRE_FB"]
["CEB还原剂加药泵1频率设定","ns=3;s=P_CEB_HYJ1_FRESET"]
["CEB还原剂加药泵1运行时间","ns=3;s=P_CEB_HYJ1_RUNTIME"]
["CEB还原剂加药泵2频率反馈","ns=3;s=P_CEB_HYJ2_FRE_FB"]
["CEB还原剂加药泵2频率设定","ns=3;s=P_CEB_HYJ2_FRESET"]
["CEB还原剂加药泵2运行时间","ns=3;s=P_CEB_HYJ2_RUNTIME"]
["备用气动隔膜泵1频率反馈","ns=3;s=P_JY_BY1_FRE_FB"]
["备用气动隔膜泵1频率设定","ns=3;s=P_JY_BY1_FRESET"]
["备用气动隔膜泵1运行时间","ns=3;s=P_JY_BY1_RUNTIME"]
["备用气动隔膜泵2频率反馈","ns=3;s=P_JY_BY2_FRE_FB"]
["备用气动隔膜泵2频率设定","ns=3;s=P_JY_BY2_FRESET"]
["备用气动隔膜泵2运行时间","ns=3;s=P_JY_BY2_RUNTIME"]
["备用气动隔膜泵3频率反馈","ns=3;s=P_JY_BY3_FRE_FB"]
["备用气动隔膜泵3频率设定","ns=3;s=P_JY_BY3_FRESET"]
["备用气动隔膜泵3运行时间","ns=3;s=P_JY_BY3_RUNTIME"]
["CIP泵频率反馈","ns=3;s=P_JY_CIPB_FRE_FB"]
["CIP泵频率设定","ns=3;s=P_JY_CIPB_FRESET"]
["CIP泵运行时间","ns=3;s=P_JY_CIPB_RUNTIME"]
["次钠加药泵1频率反馈","ns=3;s=P_JY_CN1_FRE_FB"]
["次钠加药泵1频率设定","ns=3;s=P_JY_CN1_FRESET"]
["次钠加药泵1运行时间","ns=3;s=P_JY_CN1_RUNTIME"]
["次钠加药泵2频率反馈","ns=3;s=P_JY_CN2_FRE_FB"]
["次钠加药泵2频率设定","ns=3;s=P_JY_CN2_FRESET"]
["次钠加药泵2运行时间","ns=3;s=P_JY_CN2_RUNTIME"]
["反洗风机频率反馈","ns=3;s=P_JY_FX_FJ_FRE_FB"]
["反洗风机频率设定","ns=3;s=P_JY_FX_FJ_FRESET"]
["反洗风机运行时间","ns=3;s=P_JY_FX_FJ_RUNTIME"]
["还原剂加药泵频率反馈","ns=3;s=P_JY_HYJ_FRE_FB"]
["还原剂加药泵频率设定","ns=3;s=P_JY_HYJ_FRESET"]
["还原剂加药泵运行时间","ns=3;s=P_JY_HYJ_RUNTIME"]
["碱加药泵1频率反馈","ns=3;s=P_JY_JJ1_FRE_FB"]
["碱加药泵1频率设定","ns=3;s=P_JY_JJ1_FRESET"]
["碱加药泵1运行时间","ns=3;s=P_JY_JJ1_RUNTIME"]
["碱加药泵2频率反馈","ns=3;s=P_JY_JJ2_FRE_FB"]
["碱加药泵2频率设定","ns=3;s=P_JY_JJ2_FRESET"]
["碱加药泵2运行时间","ns=3;s=P_JY_JJ2_RUNTIME"]
["酸加药泵1频率反馈","ns=3;s=P_JY_JS1_FRE_FB"]
["酸加药泵1频率设定","ns=3;s=P_JY_JS1_FRESET"]
["酸加药泵1运行时间","ns=3;s=P_JY_JS1_RUNTIME"]
["酸加药泵2频率反馈","ns=3;s=P_JY_JS2_FRE_FB"]
["酸加药泵2频率设定","ns=3;s=P_JY_JS2_FRESET"]
["酸加药泵2运行时间","ns=3;s=P_JY_JS2_RUNTIME"]
["潜污泵1频率反馈","ns=3;s=P_JY_QWB1_FRE_FB"]
["潜污泵1频率设定","ns=3;s=P_JY_QWB1_FRESET"]
["潜污泵1运行时间","ns=3;s=P_JY_QWB1_RUNTIME"]
["潜污泵2频率反馈","ns=3;s=P_JY_QWB2_FRE_FB"]
["潜污泵2频率设定","ns=3;s=P_JY_QWB2_FRESET"]
["潜污泵2运行时间","ns=3;s=P_JY_QWB2_RUNTIME"]
["杀菌剂加药泵频率反馈","ns=3;s=P_JY_SJJ_FRE_FB"]
["杀菌剂加药泵频率设定","ns=3;s=P_JY_SJJ_FRESET"]
["杀菌剂加药泵运行时间","ns=3;s=P_JY_SJJ_RUNTIME"]
["塑料泵频率反馈","ns=3;s=P_JY_SLB_FRE_FB"]
["塑料泵频率设定","ns=3;s=P_JY_SLB_FRESET"]
["塑料泵运行时间","ns=3;s=P_JY_SLB_RUNTIME"]
["外供水碱加药泵1频率反馈","ns=3;s=P_JY_WGSJ1_FRE_FB"]
["外供水碱加药泵1频率设定","ns=3;s=P_JY_WGSJ1_FRESET"]
["外供水碱加药泵1运行时间","ns=3;s=P_JY_WGSJ1_RUNTIME"]
["外供水碱加药泵2频率反馈","ns=3;s=P_JY_WGSJ2_FRE_FB"]
["外供水碱加药泵2频率设定","ns=3;s=P_JY_WGSJ2_FRESET"]
["外供水碱加药泵2运行时间","ns=3;s=P_JY_WGSJ2_RUNTIME"]
["阻垢剂加药泵频率反馈","ns=3;s=P_JY_ZGJ_FRE_FB"]
["阻垢剂加药泵频率设定","ns=3;s=P_JY_ZGJ_FRESET"]
["阻垢剂加药泵运行时间","ns=3;s=P_JY_ZGJ_RUNTIME"]
["RO段间泵频率反馈","ns=3;s=P_RO_DJB_FRE_FB"]
["RO段间泵频率设定","ns=3;s=P_RO_DJB_FRESET"]
["RO段间泵运行时间","ns=3;s=P_RO_DJB_RUNTIME"]
["RO供水泵频率反馈","ns=3;s=P_RO_GSB_FRE_FB"]
["RO供水泵频率设定","ns=3;s=P_RO_GSB_FRESET"]
["RO供水泵运行时间","ns=3;s=P_RO_GSB_RUNTIME"]
["RO高压泵频率反馈","ns=3;s=P_RO_GYB_FRE_FB"]
["RO高压泵频率设定","ns=3;s=P_RO_GYB_FRESET"]
["RO高压泵运行时间","ns=3;s=P_RO_GYB_RUNTIME"]
["UF产水泵频率反馈","ns=3;s=P_UF_CSB_FRE_FB"]
["UF产水泵频率设定","ns=3;s=P_UF_CSB_FRESET"]
["UF产水泵运行时间","ns=3;s=P_UF_CSB_RUNTIME"]
["UF反洗泵频率反馈","ns=3;s=P_UF_FXB_FRE_FB"]
["UF反洗泵频率设定","ns=3;s=P_UF_FXB_FRESET"]
["UF反洗泵运行时间","ns=3;s=P_UF_FXB_RUNTIME"]
["UF供水泵1频率反馈","ns=3;s=P_UF_GSB1_FRE_FB"]
["UF供水泵1频率设定","ns=3;s=P_UF_GSB1_FRESET"]
["UF供水泵1运行时间","ns=3;s=P_UF_GSB1_RUNTIME"]
["UF供水泵2频率反馈","ns=3;s=P_UF_GSB2_FRE_FB"]
["UF供水泵2频率设定","ns=3;s=P_UF_GSB2_FRESET"]
["UF供水泵2运行时间","ns=3;s=P_UF_GSB2_RUNTIME"]
["UF排空泵频率反馈","ns=3;s=P_UF_PKB_FRE_FB"]
["UF排空泵频率设定","ns=3;s=P_UF_PKB_FRESET"]
["UF排空泵运行时间","ns=3;s=P_UF_PKB_RUNTIME"]
["UF提升泵1频率反馈","ns=3;s=P_UF_TSB1_FRE_FB"]
["UF提升泵1频率设定","ns=3;s=P_UF_TSB1_FRESET"]
["UF提升泵1运行时间","ns=3;s=P_UF_TSB1_RUNTIME"]
["UF提升泵2频率反馈","ns=3;s=P_UF_TSB2_FRE_FB"]
["UF提升泵2频率设定","ns=3;s=P_UF_TSB2_FRESET"]
["UF提升泵2运行时间","ns=3;s=P_UF_TSB2_RUNTIME"]
["SSD_Press_12dj","ns=3;s=RO_12DJYL_SSD"]
["SSD_Flow_1dcs","ns=3;s=RO_1DCSLL_SSD"]
["SSD_Flow_1djs","ns=3;s=RO_1DJSLL_SSD"]
["SSD_Press_23dj","ns=3;s=RO_23DJYL_SSD"]
["SSD_Flow_2dcs","ns=3;s=RO_2DCSLL_SSD"]
["SSD_Flow_2djs","ns=3;s=RO_2DJSLL_SSD"]
["SSD_Flow_3dcs","ns=3;s=RO_3DCSLL_SSD"]
["SSD_Flow_3djs","ns=3;s=RO_3DJSLL_SSD"]
["反洗码","ns=3;s=RO_BW_CODE"]
["SSD_Press_by","ns=3;s=RO_BYYL_SSD"]
["CEB码","ns=3;s=RO_CEB_CODE"]
["SSD_PressCha1","ns=3;s=RO_CHA1YL_SSD"]
["SSD_PressCha2","ns=3;s=RO_CHA2YL_SSD"]
["SSD_PressCha3","ns=3;s=RO_CHA3YL_SSD"]
["SSD_产水率","ns=3;s=RO_CS_RATE_SSD"]
["Set充水时间","ns=3;s=RO_CS_TIME_SET"]
["SSD_csddl","ns=3;s=RO_CSDDL_SSD"]
["SSD_产水量累计Dint","ns=3;s=RO_CSLJ_OUT"]
["SSD_产水量累计","ns=3;s=RO_CSLJ_SSD"]
["Set充水时排气时间","ns=3;s=RO_CSPQ_TIME_SET"]
["SSD_Press_cs","ns=3;s=RO_CSYL_SSD"]
["提示","ns=3;s=RO_CUE"]
["Set冲洗时间","ns=3;s=RO_CX_TIME_SET"]
["SSD_冲洗量累计","ns=3;s=RO_CXLJ_SSD"]
["SSD_冲洗流量","ns=3;s=RO_CXLL_SSD"]
["Set_ddl_HR","ns=3;s=RO_DDL_H_SET"]
["Set_ddl_HHR","ns=3;s=RO_DDL_HH_SET"]
["HZ_Pdjb_HH","ns=3;s=RO_DJB_FRE_HH_SET"]
["HZ_Pdjb_LL","ns=3;s=RO_DJB_FRE_LL_SET"]
["段间泵固定频率设定","ns=3;s=RO_DJB_FRE_MANSET"]
["HZ_Pdjb_PIDOut","ns=3;s=RO_DJB_FRE_PID_OUT"]
["OUT_段间泵流量Need","ns=3;s=RO_DJBLL_NEED_OUT"]
["Set_段间泵过滤流量","ns=3;s=RO_DJGLLL_SET"]
["报错","ns=3;s=RO_FAULT"]
["Set反洗时间I","ns=3;s=RO_FX1_TIME_SET"]
["Set反洗时间II","ns=3;s=RO_FX2_TIME_SET"]
["Set反洗时间III","ns=3;s=RO_FX3_TIME_SET"]
["OUT_过滤时间","ns=3;s=RO_GL_TIME_OUT"]
["Set过滤时间","ns=3;s=RO_GL_TIME_SET"]
["Out_过滤次数","ns=3;s=RO_GL_TIMES_OUT"]
["HZ_Pgyb_HH","ns=3;s=RO_GYB_FRE_HH_SET"]
["HZ_Pgyb_LL","ns=3;s=RO_GYB_FRE_LL_SET"]
["HZ_Pdjb_ManSet","ns=3;s=RO_GYB_FRE_MANSET"]
["HZ_Pgyb_PIDOut","ns=3;s=RO_GYB_FRE_PID_OUT"]
["Out_故障时间","ns=3;s=RO_GZ_TIME_OUT"]
["SSD_jsddl","ns=3;s=RO_JSDDL_SSD"]
["OUT_进水流量need","ns=3;s=RO_JSLL_NEED_OUT"]
["SSD_Press_js","ns=3;s=RO_JSYL_SSD"]
["Set_开机冲洗流量","ns=3;s=RO_KJCXLL_SET"]
["模式","ns=3;s=RO_MODE"]
["SSD_Flow_ns","ns=3;s=RO_NS_SSD"]
["SSD_Flow_nshl","ns=3;s=RO_NSH1_SSD"]
["SSD_Press_ns","ns=3;s=RO_NSYL_SSD"]
["Out_12","ns=3;s=RO_OUT_12"]
["Out_13","ns=3;s=RO_OUT_13"]
["Out_14","ns=3;s=RO_OUT_14"]
["Out_15","ns=3;s=RO_OUT_15"]
["Out_16","ns=3;s=RO_OUT_16"]
["Out_17","ns=3;s=RO_OUT_17"]
["Out_20","ns=3;s=RO_OUT_20"]
["Set_PressPump_ck_H","ns=3;s=RO_P_CK_H_SET"]
["Set_PressPump_jk_L","ns=3;s=RO_P_JK_L_SET"]
["Set_排气时间1","ns=3;s=RO_PQ1_TIME_SET"]
["Set_排气时间2","ns=3;s=RO_PQ2_TIME_SET"]
["Set_排气时间3","ns=3;s=RO_PQ3_TIME_SET"]
["Set_排气时间4","ns=3;s=RO_PQ4_TIME_SET"]
["Set_排气时间5","ns=3;s=RO_PQ5_TIME_SET"]
["Set_排气时间6","ns=3;s=RO_PQ6_TIME_SET"]
["Out_设定时间","ns=3;s=RO_SET_TIME_OUT"]
["Set_R16","ns=3;s=RO_SET16"]
["Set杀菌冲洗时间","ns=3;s=RO_SJCX_TIME_SET"]
["Set_杀菌冲洗流量","ns=3;s=RO_SJCXLL_SET"]
["Set杀菌浸泡时间","ns=3;s=RO_SJJP_TIME_SET"]
["Set杀菌加药时间","ns=3;s=RO_SJJY_TIME_SET"]
["Set_杀菌加药流量","ns=3;s=RO_SJJYLL_SET"]
["步序","ns=3;s=RO_STEP"]
["Out_系统时间","ns=3;s=RO_SYSTEM_TIME_OUT"]
["Set_压差I_H","ns=3;s=RO_TMP1H_SET"]
["Set_压差I_HH","ns=3;s=RO_TMP1HH_SET"]
["Set_压差II_H","ns=3;s=RO_TMP2H_SET"]
["Set_压差II_HH","ns=3;s=RO_TMP2HH_SET"]
["Set_压差III_H","ns=3;s=RO_TMP3H_SET"]
["Set_压差III_HH","ns=3;s=RO_TMP3HH_SET"]
["SSD_脱盐率","ns=3;s=RO_TYL_SSD"]
["ZBY_R10","ns=3;s=RO_ZBY_R10"]
["ZBY_R11","ns=3;s=RO_ZBY_R11"]
["ZBY_R12","ns=3;s=RO_ZBY_R12"]
["ZBY_R14","ns=3;s=RO_ZBY_R14"]
["ZBY_R15","ns=3;s=RO_ZBY_R15"]
["ZBY_R16","ns=3;s=RO_ZBY_R16"]
["ZBY_R17","ns=3;s=RO_ZBY_R17"]
["ZBY_R5","ns=3;s=RO_ZBY_R5"]
["ZBY_R6","ns=3;s=RO_ZBY_R6"]
["ZBY_R7","ns=3;s=RO_ZBY_R7"]
["ZBY_R8","ns=3;s=RO_ZBY_R8"]
["SSD_Flow_zcs","ns=3;s=RO_ZCS_SSD"]
["OUT_增压泵流量Need","ns=3;s=RO_ZYBLL_NEED_OUT"]
["Set_增压泵过滤流量","ns=3;s=RO_ZYGLLL_SET"]
["0ut_动作时间","ns=3;s=UF_ACTION_TIME_OUT"]
["UF_BWCODE","ns=3;s=UF_BWCODE"]
["Out_反洗用水累计","ns=3;s=UF_BWLJ_FLOW"]
["Set反洗流量","ns=3;s=UF_BWLL_SET"]
["备用关键字","ns=3;s=UF_BY"]
["UF_CEBCODE","ns=3;s=UF_CEBCODE"]
["CEB碱洗冲洗时间1","ns=3;s=UF_CEBJCX1_TIME_SET"]
["CEB碱洗冲洗时间2","ns=3;s=UF_CEBJCX2_TIME_SET"]
["CEB碱洗浸泡时间","ns=3;s=UF_CEBJJP_TIME_SET"]
["CEB碱加药时间","ns=3;s=UF_CEBJJY_TIME_SET"]
["CEB碱气洗时间","ns=3;s=UF_CEBJX_TIME_SET"]
["SetCEB流量","ns=3;s=UF_CEBLL_SET"]
["CEB酸洗冲洗时间1","ns=3;s=UF_CEBSCX1_TIME_SET"]
["CEB酸洗冲洗时间2","ns=3;s=UF_CEBSCX2_TIME_SET"]
["CEB酸洗浸泡时间","ns=3;s=UF_CEBSJP_TIME_SET"]
["CEB酸加药时间","ns=3;s=UF_CEBSJY_TIME_SET"]
["CEB酸气洗时间","ns=3;s=UF_CEBSQX_TIME_SET"]
["SSDCIP清洗流量计","ns=3;s=UF_CIPQX_FLOW"]
["SSD产水浊度","ns=3;s=UF_CS_NTU"]
["SSD产水压力","ns=3;s=UF_CS_PRESS"]
["提示关键字","ns=3;s=UF_CUE"]
["DInt_10","ns=3;s=UF_DINT10"]
["DInt_3","ns=3;s=UF_DINT3"]
["DInt_4","ns=3;s=UF_DINT4"]
["DInt_5","ns=3;s=UF_DINT5"]
["DInt_6","ns=3;s=UF_DINT6"]
["DInt_7","ns=3;s=UF_DINT7"]
["DInt_8","ns=3;s=UF_DINT8"]
["DInt_9","ns=3;s=UF_DINT9"]
["故障关键字","ns=3;s=UF_FAULT"]
["SSD反洗流量计","ns=3;s=UF_FX_FLOW"]
["Out_过滤时间","ns=3;s=UF_GL_TIME_OUT"]
["Set过滤时间","ns=3;s=UF_GL_TIME_SET"]
["Out_过滤次数","ns=3;s=UF_GL_TIMES_OUT"]
["过滤次数设定","ns=3;s=UF_GL_TIMES_SET"]
["Out_过滤总次数","ns=3;s=UF_GL_TTS_OUT"]
["Out_过滤产水累计","ns=3;s=UF_GLLJ_FLOW"]
["Set过滤流量","ns=3;s=UF_GLLL_SET"]
["Oot延时过滤次数","ns=3;s=UF_GLYS_TIMES_OUT"]
["Set延时过滤次数","ns=3;s=UF_GLYS_TIMES_SET"]
["Set后冲CEB时间1","ns=3;s=UF_HC1_TIME_SET"]
["Set后冲CEB时间2","ns=3;s=UF_HC2_TIME_SET"]
["Set后冲CEB气洗时间","ns=3;s=UF_HCQX_TIME_SET"]
["SSD进水流量计","ns=3;s=UF_JS_FLOW"]
["SSD进水压力","ns=3;s=UF_JS_PRESS"]
["SSD进水累计流量","ns=3;s=UF_JSLJ_FLOW"]
["膜组模式","ns=3;s=UF_MODE"]
["Set过滤次数设定","ns=3;s=UF_PQ_TIME_SET"]
["SSD气擦洗流量","ns=3;s=UF_QCX_FLOW"]
["Set气擦洗时间","ns=3;s=UF_QCX_TIME_SET"]
["UF_REAL1","ns=3;s=UF_REAL1"]
["UF_REAL10","ns=3;s=UF_REAL10"]
["UF_REAL11","ns=3;s=UF_REAL11"]
["UF_REAL12","ns=3;s=UF_REAL12"]
["UF_REAL2","ns=3;s=UF_REAL2"]
["UF_REAL3","ns=3;s=UF_REAL3"]
["UF_REAL4","ns=3;s=UF_REAL4"]
["UF_REAL5","ns=3;s=UF_REAL5"]
["UF_REAL6","ns=3;s=UF_REAL6"]
["UF_REAL7","ns=3;s=UF_REAL7"]
["UF_REAL8","ns=3;s=UF_REAL8"]
["UF_REAL9","ns=3;s=UF_REAL9"]
["Out_设定时间","ns=3;s=UF_SET_TIME_OUT"]
["UF_SET1","ns=3;s=UF_SET1"]
["UF_SET2","ns=3;s=UF_SET2"]
["UF_SET3","ns=3;s=UF_SET3"]
["步序关键字","ns=3;s=UF_STEP"]
["Out_系统时间","ns=3;s=UF_SYSTEM_TIME_OUT"]
["SSD调节阀开度","ns=3;s=UF_TJV_KD"]
["SSD跨膜压差","ns=3;s=UF_TMP"]
["Set压差HR","ns=3;s=UF_TMP_H_SET"]
["Set压差HHR","ns=3;s=UF_TMP_HH_SET"]
["Set水反洗时间1","ns=3;s=UF_WBW1_TIME_SET"]
["Set水反洗时间2","ns=3;s=UF_WBW2_TIME_SET"]
["Set正冲流量","ns=3;s=UF_ZCLL_SET"]
["废水收集槽高液位","ns=6;s=DI_JY_FQ_FS_H"]
["废水收集槽低液位","ns=6;s=DI_JY_FQ_FS_L"]
["集水坑浮球高液位开关","ns=6;s=DI_JY_FQ_JSK_H"]
["集水坑浮球低液位开关","ns=6;s=DI_JY_FQ_JSK_L"]
["反渗透产水池高液位开关","ns=6;s=DI_JY_FQ_ROCS_H"]
["反渗透产水池高液位开关","ns=6;s=DI_JY_FQ_ROCS_L"]
["T2B水池高液位","ns=6;s=DI_JY_FQ_T2B_H"]
["T2B水池低液位","ns=6;s=DI_JY_FQ_T2B_L"]
["提升泵高液位开关","ns=6;s=DI_JY_FQ_TSB_H"]
["提升泵低液位开关","ns=6;s=DI_JY_FQ_TSB_L"]
["超滤产水池液位高液位开关","ns=6;s=DI_JY_FQ_UFCS_H"]
["超滤产水池液位低液位开关","ns=6;s=DI_JY_FQ_UFCS_L"]
["1#空压机故障","ns=6;s=DI_JY_KYJ_1_ERR"]
["1#空压机运行","ns=6;s=DI_JY_KYJ_1_RUN"]
["1#空压机故障","ns=6;s=DI_JY_KYJ_2_ERR"]
["2#空压机运行","ns=6;s=DI_JY_KYJ_2_RUN"]
["段间泵进口低压开关","ns=6;s=DI_RO_PI_DB_L"]
["段间泵出口高压开关","ns=6;s=DI_RO_PI_DJB_H"]
["高压泵出口高压开关","ns=6;s=DI_RO_PI_GYB_H"]
["高压泵进口低压开关","ns=6;s=DI_RO_PI_GYB_L"]
["膜池浮球_高液位","ns=6;s=DI_UF_YW_H"]
["膜池浮球_低液位","ns=6;s=DI_UF_YW_L"]
["流量累计备用2","ns=3;s=LJ_FLOW_BY2"]
["流量累计备用3","ns=3;s=LJ_FLOW_BY3"]
["流量累计备用4","ns=3;s=LJ_FLOW_BY4"]
["流量累计备用5","ns=3;s=LJ_FLOW_BY5"]
["流量累计备用6","ns=3;s=LJ_FLOW_BY6"]
["RO产水流量累计1","ns=3;s=LJ_FLOW_ROCS1"]
["RO产水流量累计2","ns=3;s=LJ_FLOW_ROCS2"]
["RO冲洗流量累计","ns=3;s=LJ_FLOW_ROCX"]
["RO浓水水流量累计1","ns=3;s=LJ_FLOW_RONS1"]
["RO浓水水流量累计2","ns=3;s=LJ_FLOW_RONS2"]
["杀菌剂加药箱液位H","ns=6;s=DI_JY_SJJ_H"]
["杀菌剂加药箱液位L","ns=6;s=DI_JY_SJJ_L"]
["还原剂加药箱液位H","ns=6;s=DI_JY_HYJ_H"]
["还原剂加药箱液位L","ns=6;s=DI_JY_HYJ_L"]
["阻垢剂加药箱液位H","ns=6;s=DI_JY_ZGJ_H"]
["阻垢剂加药箱液位L","ns=6;s=DI_JY_ZGJ_L"]
["中和池高液位","ns=6;s=DI_JY_ZHCYW_H"]
["中和池低液位","ns=6;s=DI_JY_ZHCYW_L"]
["次钠加药箱液位H","ns=6;s=DI_JY_CN_H"]
["次钠加药箱液位L","ns=6;s=DI_JY_CN_L"]
["氢氧化钠加药箱液位H","ns=6;s=DI_JY_NAOH_H"]
["氢氧化钠加药箱液位L","ns=6;s=DI_JY_NAOH_L"]
["柠檬酸加药箱液位H","ns=6;s=DI_JY_NMS_H"]
["柠檬酸加药箱液位L","ns=6;s=DI_JY_NMS_L"]
["RO外供水池高液位","ns=6;s=DI_JY_ROWGSCYW_H"]
["RO外供水池低液位","ns=6;s=DI_JY_ROWGSCYW_L"]
["RO供水泵温度","ns=3;s=VB1_TEM"]
["RO供水泵X轴速度","ns=3;s=VB1_X_Z_SD"]
["RO供水泵X轴位移","ns=3;s=VB1_X_Z_WY"]
["RO供水泵Y轴速度","ns=3;s=VB1_Y_Z_SD"]
["RO供水泵Y轴位移","ns=3;s=VB1_Y_Z_WY"]
["RO供水泵Z轴速度","ns=3;s=VB1_Z_Z_SD"]
["RO供水泵Z轴位移","ns=3;s=VB1_Z_Z_WY"]
["RO段间泵温度","ns=3;s=VB2_TEM"]
["RO段间泵X轴速度","ns=3;s=VB2_X_Z_SD"]
["RO段间泵X轴位移","ns=3;s=VB2_X_Z_WY"]
["RO段间泵Y轴速度","ns=3;s=VB2_Y_Z_SD"]
["RO段间泵Y轴位移","ns=3;s=VB2_Y_Z_WY"]
["RO段间泵Z轴速度","ns=3;s=VB2_Z_Z_SD"]
["RO段间泵Z轴位移","ns=3;s=VB2_Z_Z_WY"]
["UF反洗泵温度","ns=3;s=VB3_TEM"]
["UF反洗泵X轴速度","ns=3;s=VB3_X_Z_SD"]
["UF反洗泵X轴位移","ns=3;s=VB3_X_Z_WY"]
["UF反洗泵Y轴速度","ns=3;s=VB3_Y_Z_SD"]
["UF反洗泵Y轴位移","ns=3;s=VB3_Y_Z_WY"]
["UF反洗泵Z轴速度","ns=3;s=VB3_Z_Z_SD"]
["UF反洗泵Z轴位移","ns=3;s=VB3_Z_Z_WY"]
["UF排空泵温度","ns=3;s=VB4_TEM"]
["UF排空泵X轴速度","ns=3;s=VB4_X_Z_SD"]
["UF排空泵X轴位移","ns=3;s=VB4_X_Z_WY"]
["UF排空泵Y轴速度","ns=3;s=VB4_Y_Z_SD"]
["UF排空泵Y轴位移","ns=3;s=VB4_Y_Z_WY"]
["UF排空泵Z轴速度","ns=3;s=VB4_Z_Z_SD"]
["UF排空泵Z轴位移","ns=3;s=VB4_Z_Z_WY"]
["UF产水泵温度","ns=3;s=VB5_TEM"]
["UF产水泵X轴速度","ns=3;s=VB5_X_Z_SD"]
["UF产水泵X轴位移","ns=3;s=VB5_X_Z_WY"]
["UF产水泵Y轴速度","ns=3;s=VB5_Y_Z_SD"]
["UF产水泵Y轴位移","ns=3;s=VB5_Y_Z_WY"]
["UF产水泵Z轴速度","ns=3;s=VB5_Z_Z_SD"]
["UF产水泵Z轴位移","ns=3;s=VB5_Z_Z_WY"]
["CIP清洗水泵温度","ns=3;s=VB6_TEM"]
["CIP清洗水泵X轴速度","ns=3;s=VB6_X_Z_SD"]
["CIP清洗水泵X轴位移","ns=3;s=VB6_X_Z_WY"]
["CIP清洗水泵Y轴速度","ns=3;s=VB6_Y_Z_SD"]
["CIP清洗水泵Y轴位移","ns=3;s=VB6_Y_Z_WY"]
["CIP清洗水泵Z轴速度","ns=3;s=VB6_Z_Z_SD"]
["CIP清洗水泵Z轴位移","ns=3;s=VB6_Z_Z_WY"]
["反洗风机温度","ns=3;s=VB7_TEM"]
["反洗风机X轴速度","ns=3;s=VB7_X_Z_SD"]
["反洗风机X轴位移","ns=3;s=VB7_X_Z_WY"]
["反洗风机Y轴速度","ns=3;s=VB7_Y_Z_SD"]
["反洗风机Y轴位移","ns=3;s=VB7_Y_Z_WY"]
["反洗风机Z轴速度","ns=3;s=VB7_Z_Z_SD"]
["反洗风机Z轴位移","ns=3;s=VB7_Z_Z_WY"]
["RO高压泵温度","ns=3;s=VB8_TEM"]
["RO高压泵X轴速度","ns=3;s=VB8_X_Z_SD"]
["RO高压泵X轴位移","ns=3;s=VB8_X_Z_WY"]
["RO高压泵Y轴速度","ns=3;s=VB8_Y_Z_SD"]
["RO高压泵Y轴位移","ns=3;s=VB8_Y_Z_WY"]
["RO高压泵Z轴速度","ns=3;s=VB8_Z_Z_SD"]
["RO高压泵Z轴位移","ns=3;s=VB8_Z_Z_WY"]
["超滤进水上方烟感","ns=3;s=YG1_ALARM"]
["通道设置","ns=3;s=YG1_ID"]
["RO模架上方烟感","ns=3;s=YG2_ALARM"]
["通道设置","ns=3;s=YG2_ID"]
["RO控制柜上方烟感","ns=3;s=YG3_ALARM"]
["通道设置","ns=3;s=YG3_ID"]
["加药间上方烟感","ns=3;s=YG4_ALARM"]
["通道","ns=3;s=YG4_ID"]
["加药间控制柜总进线功率因数","ns=3;s=Z1_COSΘ"]
["加药间控制柜总进线电能","ns=3;s=Z1_EP"]
["加药间控制柜总进线IA","ns=3;s=Z1_IA"]
["加药间控制柜总进线IB","ns=3;s=Z1_IB"]
["加药间控制柜总进线IC","ns=3;s=Z1_IC"]
["加药间控制柜总进线总功率","ns=3;s=Z1_POWER"]
["加药间控制柜总进线UA","ns=3;s=Z1_UA"]
["加药间控制柜总进线UB","ns=3;s=Z1_UB"]
["加药间控制柜总进线UC","ns=3;s=Z1_UC"]
["反洗风机功率因数","ns=3;s=Z2_COSΘ"]
["反洗风机电能","ns=3;s=Z2_EP"]
["反洗风机IA","ns=3;s=Z2_IA"]
["反洗风机IB","ns=3;s=Z2_IB"]
["反洗风机IC","ns=3;s=Z2_IC"]
["反洗风机总功率","ns=3;s=Z2_POWER"]
["反洗风机UA","ns=3;s=Z2_UA"]
["反洗风机UB","ns=3;s=Z2_UB"]
["反洗风机UC","ns=3;s=Z2_UC"]
["CIP泵功率因数","ns=3;s=Z3_COSΘ"]
["CIP泵电能","ns=3;s=Z3_EP"]
["CIP泵IA","ns=3;s=Z3_IA"]
["CIP泵IB","ns=3;s=Z3_IB"]
["CIP泵IC","ns=3;s=Z3_IC"]
["CIP泵总功率","ns=3;s=Z3_POWER"]
["CIP泵UA","ns=3;s=Z3_UA"]
["CIP泵UB","ns=3;s=Z3_UB"]
["CIP泵UC","ns=3;s=Z3_UC"]
["1#电加热器功率因数","ns=3;s=Z4_COSΘ"]
["1#电加热器电能","ns=3;s=Z4_EP"]
["1#电加热器IA","ns=3;s=Z4_IA"]
["1#电加热器IB","ns=3;s=Z4_IB"]
["1#电加热器IC","ns=3;s=Z4_IC"]
["1#电加热器总功率","ns=3;s=Z4_POWER"]
["1#电加热器UA","ns=3;s=Z4_UA"]
["1#电加热器UB","ns=3;s=Z4_UB"]
["1#电加热器UC","ns=3;s=Z4_UC"]
["2#电加热器功率因数","ns=3;s=Z5_COSΘ"]
["2#电加热器电能","ns=3;s=Z5_EP"]
["2#电加热器IA","ns=3;s=Z5_IA"]
["2#电加热器IB","ns=3;s=Z5_IB"]
["2#电加热器IC","ns=3;s=Z5_IC"]
["2#电加热器总功率","ns=3;s=Z5_POWER"]
["2#电加热器UA","ns=3;s=Z5_UA"]
["2#电加热器UB","ns=3;s=Z5_UB"]
["2#电加热器UC","ns=3;s=Z5_UC"]
["RO控制柜总进线功率因数","ns=3;s=Z6_COSΘ"]
["RO控制柜总进线电能","ns=3;s=Z6_EP"]
["RO控制柜总进线IA","ns=3;s=Z6_IA"]
["RO控制柜总进线IB","ns=3;s=Z6_IB"]
["RO控制柜总进线IC","ns=3;s=Z6_IC"]
["RO控制柜总进线总功率","ns=3;s=Z6_POWER"]
["RO控制柜总进线UA","ns=3;s=Z6_UA"]
["RO控制柜总进线UB","ns=3;s=Z6_UB"]
["RO控制柜总进线UC","ns=3;s=Z6_UC"]
["RO高压泵功率因数","ns=3;s=Z7_COSΘ"]
["RO高压泵电能","ns=3;s=Z7_EP"]
["RO高压泵IA","ns=3;s=Z7_IA"]
["RO高压泵IB","ns=3;s=Z7_IB"]
["RO高压泵IC","ns=3;s=Z7_IC"]
["RO高压泵总功率","ns=3;s=Z7_POWER"]
["RO高压泵UA","ns=3;s=Z7_UA"]
["RO高压泵UB","ns=3;s=Z7_UB"]
["RO高压泵UC","ns=3;s=Z7_UC"]
["RO供水泵功率因数","ns=3;s=Z8_COSΘ"]
["RO供水泵电能","ns=3;s=Z8_EP"]
["RO供水泵IA","ns=3;s=Z8_IA"]
["RO供水泵IB","ns=3;s=Z8_IB"]
["RO供水泵IC","ns=3;s=Z8_IC"]
["RO供水泵总功率","ns=3;s=Z8_POWER"]
["RO供水泵UA","ns=3;s=Z8_UA"]
["RO供水泵UB","ns=3;s=Z8_UB"]
["RO供水泵UC","ns=3;s=Z8_UC"]
["RO供段间泵功率因数","ns=3;s=Z9_COSΘ"]
["RO供段间泵电能","ns=3;s=Z9_EP"]
["RO供段间泵IA","ns=3;s=Z9_IA"]
["RO供段间泵IB","ns=3;s=Z9_IB"]
["RO供段间泵IC","ns=3;s=Z9_IC"]
["RO供段间泵总功率","ns=3;s=Z9_POWER"]
["RO供段间泵UA","ns=3;s=Z9_UA"]
["RO供段间泵UB","ns=3;s=Z9_UB"]
["RO供段间泵UC","ns=3;s=Z9_UC"]
["UF控制柜总进线功率因数","ns=3;s=Z10_COSΘ"]
["UF控制柜总进线电能","ns=3;s=Z10_EP"]
["UF控制柜总进线IA","ns=3;s=Z10_IA"]
["UF控制柜总进线IB","ns=3;s=Z10_IB"]
["UF控制柜总进线IC","ns=3;s=Z10_IC"]
["UF控制柜总进线总功率","ns=3;s=Z10_POWER"]
["UF控制柜总进线UA","ns=3;s=Z10_UA"]
["UF控制柜总进线UB","ns=3;s=Z10_UB"]
["UF控制柜总进线UC","ns=3;s=Z10_UC"]
["UF产水泵功率因数","ns=3;s=Z11_COSΘ"]
["UF产水泵电能","ns=3;s=Z11_EP"]
["UF产水泵IA","ns=3;s=Z11_IA"]
["UF产水泵IB","ns=3;s=Z11_IB"]
["UF产水泵IC","ns=3;s=Z11_IC"]
["UF产水泵总功率","ns=3;s=Z11_POWER"]
["UF产水泵UA","ns=3;s=Z11_UA"]
["UF产水泵UB","ns=3;s=Z11_UB"]
["UF产水泵UC","ns=3;s=Z11_UC"]
["UF排空泵功率因数","ns=3;s=Z12_COSΘ"]
["UF排空泵电能","ns=3;s=Z12_EP"]
["UF排空泵IA","ns=3;s=Z12_IA"]
["UF排空泵IB","ns=3;s=Z12_IB"]
["UF排空泵IC","ns=3;s=Z12_IC"]
["UF排空泵总功率","ns=3;s=Z12_POWER"]
["UF排空泵UA","ns=3;s=Z12_UA"]
["UF排空泵UB","ns=3;s=Z12_UB"]
["UF排空泵UC","ns=3;s=Z12_UC"]
["UF反洗泵功率因数","ns=3;s=Z13_COSΘ"]
["UF反洗泵电能","ns=3;s=Z13_EP"]
["UF反洗泵IA","ns=3;s=Z13_IA"]
["UF反洗泵IB","ns=3;s=Z13_IB"]
["UF反洗泵IC","ns=3;s=Z13_IC"]
["UF反洗泵总功率","ns=3;s=Z13_POWER"]
["UF反洗泵UA","ns=3;s=Z13_UA"]
["UF反洗泵UB","ns=3;s=Z13_UB"]
["UF反洗泵UC","ns=3;s=Z13_UC"]
["UF 1#提升泵功率因数","ns=3;s=Z14_COSΘ"]
["UF 1#提升泵电能","ns=3;s=Z14_EP"]
["UF 1#提升泵IA","ns=3;s=Z14_IA"]
["UF 1#提升泵IB","ns=3;s=Z14_IB"]
["UF 1#提升泵IC","ns=3;s=Z14_IC"]
["UF 1#提升泵总功率","ns=3;s=Z14_POWER"]
["UF 1#提升泵UA","ns=3;s=Z14_UA"]
["UF 1#提升泵UB","ns=3;s=Z14_UB"]
["UF 1#提升泵UC","ns=3;s=Z14_UC"]
["UF 2#提升泵功率因数","ns=3;s=Z15_COSΘ"]
["UF 2#提升泵电能","ns=3;s=Z15_EP"]
["UF 2#提升泵IA","ns=3;s=Z15_IA"]
["UF 2#提升泵IB","ns=3;s=Z15_IB"]
["UF 2#提升泵IC","ns=3;s=Z15_IC"]
["UF 2#提升泵总功率","ns=3;s=Z15_POWER"]
["UF 2#提升泵UA","ns=3;s=Z15_UA"]
["UF 2#提升泵UB","ns=3;s=Z15_UB"]
["UF 2#提升泵UC","ns=3;s=Z15_UC"]
["RO外供水碱泵HZ0","ns=3;s=RO_WGS_JB_A0"]
["RO外供水碱泵HZ1","ns=3;s=RO_WGS_JB_A1"]
["RO外供水碱泵HZ10","ns=3;s=RO_WGS_JB_A10"]
["RO外供水碱泵HZ11","ns=3;s=RO_WGS_JB_A11"]
["RO外供水碱泵HZ12","ns=3;s=RO_WGS_JB_A12"]
["RO外供水碱泵HZ13","ns=3;s=RO_WGS_JB_A13"]
["RO外供水碱泵HZ14","ns=3;s=RO_WGS_JB_A14"]
["RO外供水碱泵HZ15","ns=3;s=RO_WGS_JB_A15"]
["RO外供水碱泵HZ2","ns=3;s=RO_WGS_JB_A2"]
["RO外供水碱泵HZ3","ns=3;s=RO_WGS_JB_A3"]
["RO外供水碱泵HZ4","ns=3;s=RO_WGS_JB_A4"]
["RO外供水碱泵HZ5","ns=3;s=RO_WGS_JB_A5"]
["RO外供水碱泵HZ6","ns=3;s=RO_WGS_JB_A6"]
["RO外供水碱泵HZ7","ns=3;s=RO_WGS_JB_A7"]
["RO外供水碱泵HZ8","ns=3;s=RO_WGS_JB_A8"]
["RO外供水碱泵HZ9","ns=3;s=RO_WGS_JB_A9"]
["备用11高设定","ns=3;s=LOCK_BY11_H"]
["备用11高高设定","ns=3;s=LOCK_BY11_HH"]
["备用11低设定","ns=3;s=LOCK_BY11_L"]
["备用11低低设定","ns=3;s=LOCK_BY11_LL"]
["备用11中设定","ns=3;s=LOCK_BY11_M"]
["备用12高设定","ns=3;s=LOCK_BY12_H"]
["备用12高高设定","ns=3;s=LOCK_BY12_HH"]
["备用12低设定","ns=3;s=LOCK_BY12_L"]
["备用12低低设定","ns=3;s=LOCK_BY12_LL"]
["备用12中设定","ns=3;s=LOCK_BY12_M"]
["备用13高设定","ns=3;s=LOCK_BY13_H"]
["备用13高高设定","ns=3;s=LOCK_BY13_HH"]
["备用13低设定","ns=3;s=LOCK_BY13_L"]
["备用13低低设定","ns=3;s=LOCK_BY13_LL"]
["备用13中设定","ns=3;s=LOCK_BY13_M"]
["备用14高设定","ns=3;s=LOCK_BY14_H"]
["备用14高高设定","ns=3;s=LOCK_BY14_HH"]
["备用14低设定","ns=3;s=LOCK_BY14_L"]
["备用14低低设定","ns=3;s=LOCK_BY14_LL"]
["备用14中设定","ns=3;s=LOCK_BY14_M"]
["备用15高设定","ns=3;s=LOCK_BY15_H"]
["备用15高高设定","ns=3;s=LOCK_BY15_HH"]
["备用15低设定","ns=3;s=LOCK_BY15_L"]
["备用15低低设定","ns=3;s=LOCK_BY15_LL"]
["备用15中设定","ns=3;s=LOCK_BY15_M"]
["备用16高设定","ns=3;s=LOCK_BY16_H"]
["备用16高高设定","ns=3;s=LOCK_BY16_HH"]
["备用16低设定","ns=3;s=LOCK_BY16_L"]
["备用16低低设定","ns=3;s=LOCK_BY16_LL"]
["备用16中设定","ns=3;s=LOCK_BY16_M"]
["备用17高设定","ns=3;s=LOCK_BY17_H"]
["备用17高高设定","ns=3;s=LOCK_BY17_HH"]
["备用17低设定","ns=3;s=LOCK_BY17_L"]
["备用17低低设定","ns=3;s=LOCK_BY17_LL"]
["备用17中设定","ns=3;s=LOCK_BY17_M"]
["备用18高设定","ns=3;s=LOCK_BY18_H"]
["备用18高高设定","ns=3;s=LOCK_BY18_HH"]
["备用18低设定","ns=3;s=LOCK_BY18_L"]
["备用18低低设定","ns=3;s=LOCK_BY18_LL"]
["备用18中设定","ns=3;s=LOCK_BY18_M"]
["备用19高设定","ns=3;s=LOCK_BY19_H"]
["备用19高高设定","ns=3;s=LOCK_BY19_HH"]
["备用19低设定","ns=3;s=LOCK_BY19_L"]
["备用19低低设定","ns=3;s=LOCK_BY19_LL"]
["备用19中设定","ns=3;s=LOCK_BY19_M"]
["RO进水PH高设定","ns=3;s=LOCK_ROJSPH_H"]
["RO进水PH高高设定","ns=3;s=LOCK_ROJSPH_HH"]
["RO进水PH低设定","ns=3;s=LOCK_ROJSPH_L"]
["RO进水PH低低设定","ns=3;s=LOCK_ROJSPH_LL"]
["RO进水PH中设定","ns=3;s=LOCK_ROJSPH_M"]
["反渗透进水ORP超高（组态弹窗用）","ORP_CX"]
["反渗透回收率","ROHSL"]