{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":3676,"n_cols":2,"rows_kept":3676,"cut":false,"hidden":false,"merged":[]}
["item_alias","item_name"]
["进水量","water_in"]
["外供水流量","water_out"]
["RO1脱盐率","RO1_TYL"]
["RO2脱盐率","RO2_TYL"]
["UF1渗透率","UF1Per"]
["UF2渗透率","UF2Per"]
["次钠加药箱高报警","ns=6;s=ALARM_CN_H"]
["次钠加药箱超高报警","ns=6;s=ALARM_CN_HH"]
["次钠加药箱低报警","ns=6;s=ALARM_CN_L"]
["次钠加药箱超低报警","ns=6;s=ALARM_CN_LL"]
["反洗废水箱高报警","ns=6;s=ALARM_FSX_H"]
["反洗废水箱超高报警","ns=6;s=ALARM_FSX_HH"]
["反洗废水箱低报警","ns=6;s=ALARM_FSX_L"]
["反洗废水箱超低报警","ns=6;s=ALARM_FSX_LL"]
["还原剂加药箱高报警","ns=6;s=ALARM_HYJ_H"]
["还原剂加药箱超高报警","ns=6;s=ALARM_HYJ_HH"]
["还原剂加药箱低报警","ns=6;s=ALARM_HYJ_L"]
["还原剂加药箱超低报警","ns=6;s=ALARM_HYJ_LL"]
["碱加药箱高报警","ns=6;s=ALARM_J_H"]
["碱加药箱超高报警","ns=6;s=ALARM_J_HH"]
["碱加药箱低报警","ns=6;s=ALARM_J_L"]
["碱加药箱超低报警","ns=6;s=ALARM_J_LL"]
["超滤原水箱1高报警","ns=6;s=ALARM_JSX1_H"]
["超滤原水箱1超高报警","ns=6;s=ALARM_JSX1_HH"]
["超滤原水箱1低报警","ns=6;s=ALARM_JSX1_L"]
["超滤原水箱1超低报警","ns=6;s=ALARM_JSX1_LL"]
["超滤原水箱2高报警","ns=6;s=ALARM_JSX2_H"]
["超滤原水箱2超高报警","ns=6;s=ALARM_JSX2_HH"]
["超滤原水箱2低报警","ns=6;s=ALARM_JSX2_L"]
["超滤原水箱2超低报警","ns=6;s=ALARM_JSX2_LL"]
["PAC加药箱高报警","ns=6;s=ALARM_PAC_H"]
["PAC加药箱超高报警","ns=6;s=ALARM_PAC_HH"]
["PAC加药箱低报警","ns=6;s=ALARM_PAC_L"]
["PAC加药箱超低报警","ns=6;s=ALARM_PAC_LL"]
["清洗水箱高报警","ns=6;s=ALARM_QXSX_H"]
["清洗水箱超高报警","ns=6;s=ALARM_QXSX_HH"]
["清洗水箱低报警","ns=6;s=ALARM_QXSX_L"]
["清洗水箱超低报警","ns=6;s=ALARM_QXSX_LL"]
["反渗透产水箱高报警","ns=6;s=ALARM_RO_CSX_H"]
["反渗透产水箱超高报警","ns=6;s=ALARM_RO_CSX_HH"]
["反渗透产水箱低报警","ns=6;s=ALARM_RO_CSX_L"]
["反渗透产水箱超低报警","ns=6;s=ALARM_RO_CSX_LL"]
["酸加药箱高报警","ns=6;s=ALARM_S_H"]
["酸加药箱超高报警","ns=6;s=ALARM_S_HH"]
["酸加药箱低报警","ns=6;s=ALARM_S_L"]
["酸加药箱超低报警","ns=6;s=ALARM_S_LL"]
["杀菌剂加药箱高报警","ns=6;s=ALARM_SJJ_H"]
["杀菌剂加药箱超高报警","ns=6;s=ALARM_SJJ_HH"]
["杀菌剂加药箱低报警","ns=6;s=ALARM_SJJ_L"]
["杀菌剂加药箱超低报警","ns=6;s=ALARM_SJJ_LL"]
["超滤产水箱高报警","ns=6;s=ALARM_UF_CSX_H"]
["超滤产水箱超高报警","ns=6;s=ALARM_UF_CSX_HH"]
["超滤产水箱低报警","ns=6;s=ALARM_UF_CSX_L"]
["超滤产水箱超低报警","ns=6;s=ALARM_UF_CSX_LL"]
["阻垢剂加药箱高报警","ns=6;s=ALARM_ZGJ_H"]
["阻垢剂加药箱超高报警","ns=6;s=ALARM_ZGJ_HH"]
["阻垢剂加药箱低报警","ns=6;s=ALARM_ZGJ_L"]
["阻垢剂加药箱超低报警","ns=6;s=ALARM_ZGJ_LL"]
["中和水箱高报警","ns=6;s=ALARM_ZHSX_H"]
["中和水箱超高报警","ns=6;s=ALARM_ZHSX_HH"]
["中和水箱低报警","ns=6;s=ALARM_ZHSX_L"]
["中和水箱超低报警","ns=6;s=ALARM_ZHSX_LL"]
["还原剂搅拌器自动启动","ns=6;s=JBQ_HYJ_AUTOSTART"]
["还原剂搅拌器手自动","ns=6;s=JBQ_HYJ_BT_AUTO"]
["还原剂搅拌器故障复位","ns=6;s=JBQ_HYJ_BT_RESET"]
["还原剂搅拌器手动启动","ns=6;s=JBQ_HYJ_BT_START"]
["还原剂搅拌器手动停止","ns=6;s=JBQ_HYJ_BT_STOP"]
["还原剂搅拌器故障","ns=6;s=JBQ_HYJ_FAULT"]
["还原剂搅拌器启动","ns=6;s=JBQ_HYJ_OUTPUT"]
["还原剂搅拌器启动准备好","ns=6;s=JBQ_HYJ_READY"]
["还原剂搅拌器远程","ns=6;s=JBQ_HYJ_REM"]
["还原剂搅拌器运行","ns=6;s=JBQ_HYJ_RFB"]
["PAC搅拌器自动启动","ns=6;s=JBQ_PAC_AUTOSTART"]
["PAC搅拌器手自动","ns=6;s=JBQ_PAC_BT_AUTO"]
["PAC搅拌器故障复位","ns=6;s=JBQ_PAC_BT_RESET"]
["PAC搅拌器手动启动","ns=6;s=JBQ_PAC_BT_START"]
["PAC搅拌器手动停止","ns=6;s=JBQ_PAC_BT_STOP"]
["PAC搅拌器故障","ns=6;s=JBQ_PAC_FAULT"]
["PAC搅拌器启动","ns=6;s=JBQ_PAC_OUTPUT"]
["PAC搅拌器启动准备好","ns=6;s=JBQ_PAC_READY"]
["PAC搅拌器远程","ns=6;s=JBQ_PAC_REM"]
["PAC搅拌器运行","ns=6;s=JBQ_PAC_RFB"]
["酸搅拌器自动启动","ns=6;s=JBQ_S_AUTOSTART"]
["酸搅拌器手自动","ns=6;s=JBQ_S_BT_AUTO"]
["酸搅拌器故障复位","ns=6;s=JBQ_S_BT_RESET"]
["酸搅拌器手动启动","ns=6;s=JBQ_S_BT_START"]
["酸搅拌器手动停止","ns=6;s=JBQ_S_BT_STOP"]
["酸搅拌器故障","ns=6;s=JBQ_S_FAULT"]
["酸搅拌器启动","ns=6;s=JBQ_S_OUTPUT"]
["酸搅拌器启动准备好","ns=6;s=JBQ_S_READY"]
["酸搅拌器远程","ns=6;s=JBQ_S_REM"]
["酸搅拌器运行","ns=6;s=JBQ_S_RFB"]
["阻垢剂搅拌器自动启动","ns=6;s=JBQ_ZGJ_AUTOSTART"]
["阻垢剂搅拌器手自动","ns=6;s=JBQ_ZGJ_BT_AUTO"]
["阻垢剂搅拌器故障复位","ns=6;s=JBQ_ZGJ_BT_RESET"]
["阻垢剂搅拌器手动启动","ns=6;s=JBQ_ZGJ_BT_START"]
["阻垢剂搅拌器手动停止","ns=6;s=JBQ_ZGJ_BT_STOP"]
["阻垢剂搅拌器故障","ns=6;s=JBQ_ZGJ_FAULT"]
["阻垢剂搅拌器启动","ns=6;s=JBQ_ZGJ_OUTPUT"]
["阻垢剂搅拌器启动准备好","ns=6;s=JBQ_ZGJ_READY"]
["阻垢剂搅拌器远程","ns=6;s=JBQ_ZGJ_REM"]
["阻垢剂搅拌器运行","ns=6;s=JBQ_ZGJ_RFB"]
["1#次钠加药泵自动启动","ns=6;s=P_1#CNB_AUTOSTART"]
["1#次钠加药泵手自动","ns=6;s=P_1#CNB_BT_AUTO"]
["1#次钠加药泵故障复位","ns=6;s=P_1#CNB_BT_RESET"]
["1#次钠加药泵手动启动","ns=6;s=P_1#CNB_BT_START"]
["1#次钠加药泵手动停止","ns=6;s=P_1#CNB_BT_STOP"]
["1#次钠加药泵故障","ns=6;s=P_1#CNB_FAULT"]
["1#次钠加药泵启动","ns=6;s=P_1#CNB_OUTPUT"]
["1#次钠加药泵启动准备好","ns=6;s=P_1#CNB_READY"]
["1#次钠加药泵远程","ns=6;s=P_1#CNB_REM"]
["1#次钠加药泵运行","ns=6;s=P_1#CNB_RFB"]
["1#出水碱加药泵自动启动","ns=6;s=P_1#CSJB_AUTOSTART"]
["1#出水碱加药泵手自动","ns=6;s=P_1#CSJB_BT_AUTO"]
["1#出水碱加药泵故障复位","ns=6;s=P_1#CSJB_BT_RESET"]
["1#出水碱加药泵手动启动","ns=6;s=P_1#CSJB_BT_START"]
["1#出水碱加药泵手动停止","ns=6;s=P_1#CSJB_BT_STOP"]
["1#出水碱加药泵故障","ns=6;s=P_1#CSJB_FAULT"]
["1#出水碱加药泵启动","ns=6;s=P_1#CSJB_OUTPUT"]
["1#出水碱加药泵启动准备好","ns=6;s=P_1#CSJB_READY"]
["1#出水碱加药泵远程","ns=6;s=P_1#CSJB_REM"]
["1#出水碱加药泵运行","ns=6;s=P_1#CSJB_RFB"]
["1#回用水泵自动启动","ns=6;s=P_1#HYSB_AUTOSTART"]
["1#回用水泵手自动","ns=6;s=P_1#HYSB_BT_AUTO"]
["1#回用水泵故障复位","ns=6;s=P_1#HYSB_BT_RESET"]
["1#回用水泵手动启动","ns=6;s=P_1#HYSB_BT_START"]
["1#回用水泵手动停止","ns=6;s=P_1#HYSB_BT_STOP"]
["1#回用水泵故障","ns=6;s=P_1#HYSB_FAULT"]
["1#回用水泵启动","ns=6;s=P_1#HYSB_OUTPUT"]
["1#回用水泵启动准备好","ns=6;s=P_1#HYSB_READY"]
["1#回用水泵远程","ns=6;s=P_1#HYSB_REM"]
["1#回用水泵运行","ns=6;s=P_1#HYSB_RFB"]
["1#PAC加药泵自动启动","ns=6;s=P_1#PACB_AUTOSTART"]
["1#PAC加药泵手自动","ns=6;s=P_1#PACB_BT_AUTO"]
["1#PAC加药泵故障复位","ns=6;s=P_1#PACB_BT_RESET"]
["1#PAC加药泵手动启动","ns=6;s=P_1#PACB_BT_START"]
["1#PAC加药泵手动停止","ns=6;s=P_1#PACB_BT_STOP"]
["1#PAC加药泵故障","ns=6;s=P_1#PACB_FAULT"]
["1#PAC加药泵启动","ns=6;s=P_1#PACB_OUTPUT"]
["1#PAC加药泵启动准备好","ns=6;s=P_1#PACB_READY"]
["1#PAC加药泵远程","ns=6;s=P_1#PACB_REM"]
["1#PAC加药泵运行","ns=6;s=P_1#PACB_RFB"]
["1#RO段间泵自动启动","ns=6;s=P_1#RODJB_AUTOSTART"]
["1#RO段间泵手自动","ns=6;s=P_1#RODJB_BT_AUTO"]
["1#RO段间泵故障复位","ns=6;s=P_1#RODJB_BT_RESET"]
["1#RO段间泵手动启动","ns=6;s=P_1#RODJB_BT_START"]
["1#RO段间泵手动停止","ns=6;s=P_1#RODJB_BT_STOP"]
["1#RO段间泵故障","ns=6;s=P_1#RODJB_FAULT"]
["1#RO段间泵启动","ns=6;s=P_1#RODJB_OUTPUT"]
["1#RO段间泵启动准备好","ns=6;s=P_1#RODJB_READY"]
["1#RO段间泵远程","ns=6;s=P_1#RODJB_REM"]
["1#RO段间泵运行","ns=6;s=P_1#RODJB_RFB"]
["1#RO高压泵自动启动","ns=6;s=P_1#ROGYB_AUTOSTART"]
["1#RO高压泵手自动","ns=6;s=P_1#ROGYB_BT_AUTO"]
["1#RO高压泵故障复位","ns=6;s=P_1#ROGYB_BT_RESET"]
["1#RO高压泵手动启动","ns=6;s=P_1#ROGYB_BT_START"]
["1#RO高压泵手动停止","ns=6;s=P_1#ROGYB_BT_STOP"]
["1#RO高压泵故障","ns=6;s=P_1#ROGYB_FAULT"]
["1#RO高压泵启动","ns=6;s=P_1#ROGYB_OUTPUT"]
["1#RO高压泵启动准备好","ns=6;s=P_1#ROGYB_READY"]
["1#RO高压泵远程","ns=6;s=P_1#ROGYB_REM"]
["1#RO高压泵运行","ns=6;s=P_1#ROGYB_RFB"]
["1#RO还原剂加药泵自动启动","ns=6;s=P_1#HYJB_AUTOSTART"]
["1#RO还原剂加药泵手自动","ns=6;s=P_1#HYJB_BT_AUTO"]
["1#RO还原剂加药泵故障复位","ns=6;s=P_1#HYJB_BT_RESET"]
["1#RO还原剂加药泵手动启动","ns=6;s=P_1#HYJB_BT_START"]
["1#RO还原剂加药泵手动停止","ns=6;s=P_1#HYJB_BT_STOP"]
["1#RO还原剂加药泵故障","ns=6;s=P_1#HYJB_FAULT"]
["1#RO还原剂加药泵启动","ns=6;s=P_1#HYJB_OUTPUT"]
["1#RO还原剂加药泵启动准备好","ns=6;s=P_1#HYJB_READY"]
["1#RO还原剂加药泵远程","ns=6;s=P_1#HYJB_REM"]
["1#RO还原剂加药泵运行","ns=6;s=P_1#HYJB_RFB"]
["1#酸加药泵自动启动","ns=6;s=P_1#SB_AUTOSTART"]
["1#酸加药泵手自动","ns=6;s=P_1#SB_BT_AUTO"]
["1#酸加药泵故障复位","ns=6;s=P_1#SB_BT_RESET"]
["1#酸加药泵手动启动","ns=6;s=P_1#SB_BT_START"]
["1#酸加药泵手动停止","ns=6;s=P_1#SB_BT_STOP"]
["1#酸加药泵故障","ns=6;s=P_1#SB_FAULT"]
["1#酸加药泵启动","ns=6;s=P_1#SB_OUTPUT"]
["1#酸加药泵启动准备好","ns=6;s=P_1#SB_READY"]
["1#酸加药泵远程","ns=6;s=P_1#SB_REM"]
["1#酸加药泵运行","ns=6;s=P_1#SB_RFB"]
["1#杀菌剂加药泵自动启动","ns=6;s=P_1#SJB_AUTOSTART"]
["1#杀菌剂加药泵手自动","ns=6;s=P_1#SJB_BT_AUTO"]
["1#杀菌剂加药泵故障复位","ns=6;s=P_1#SJB_BT_RESET"]
["1#杀菌剂加药泵手动启动","ns=6;s=P_1#SJB_BT_START"]
["1#杀菌剂加药泵手动停止","ns=6;s=P_1#SJB_BT_STOP"]
["1#杀菌剂加药泵故障","ns=6;s=P_1#SJB_FAULT"]
["1#杀菌剂加药泵启动","ns=6;s=P_1#SJB_OUTPUT"]
["1#杀菌剂加药泵启动准备好","ns=6;s=P_1#SJB_READY"]
["1#杀菌剂加药泵远程","ns=6;s=P_1#SJB_REM"]
["1#杀菌剂加药泵运行","ns=6;s=P_1#SJB_RFB"]
["1#超滤碱加药泵自动启动","ns=6;s=P_1#UF_JB_AUTOSTART"]
["1#超滤碱加药泵手自动","ns=6;s=P_1#UF_JB_BT_AUTO"]
["1#超滤碱加药泵故障复位","ns=6;s=P_1#UF_JB_BT_RESET"]
["1#超滤碱加药泵手动启动","ns=6;s=P_1#UF_JB_BT_START"]
["1#超滤碱加药泵手动停止","ns=6;s=P_1#UF_JB_BT_STOP"]
["1#超滤碱加药泵故障","ns=6;s=P_1#UF_JB_FAULT"]
["1#超滤碱加药泵启动","ns=6;s=P_1#UF_JB_OUTPUT"]
["1#超滤碱加药泵启动准备好","ns=6;s=P_1#UF_JB_READY"]
["1#超滤碱加药泵远程","ns=6;s=P_1#UF_JB_REM"]
["1#超滤碱加药泵运行","ns=6;s=P_1#UF_JB_RFB"]
["1#超滤反洗泵自动启动","ns=6;s=P_1#UFBWB_AUTOSTART"]
["1#超滤反洗泵手自动","ns=6;s=P_1#UFBWB_BT_AUTO"]
["1#超滤反洗泵故障复位","ns=6;s=P_1#UFBWB_BT_RESET"]
["1#超滤反洗泵手动启动","ns=6;s=P_1#UFBWB_BT_START"]
["1#超滤反洗泵手动停止","ns=6;s=P_1#UFBWB_BT_STOP"]
["1#超滤反洗泵故障","ns=6;s=P_1#UFBWB_FAULT"]
["1#超滤反洗泵启动","ns=6;s=P_1#UFBWB_OUTPUT"]
["1#超滤反洗泵启动准备好","ns=6;s=P_1#UFBWB_READY"]
["1#超滤反洗泵远程","ns=6;s=P_1#UFBWB_REM"]
["1#超滤反洗泵运行","ns=6;s=P_1#UFBWB_RFB"]
["1#阻垢剂加药泵自动启动","ns=6;s=P_1#ZGJB_AUTOSTART"]
["1#阻垢剂加药泵手自动","ns=6;s=P_1#ZGJB_BT_AUTO"]
["1#阻垢剂加药泵故障复位","ns=6;s=P_1#ZGJB_BT_RESET"]
["1#阻垢剂加药泵手动启动","ns=6;s=P_1#ZGJB_BT_START"]
["1#阻垢剂加药泵手动停止","ns=6;s=P_1#ZGJB_BT_STOP"]
["1#阻垢剂加药泵故障","ns=6;s=P_1#ZGJB_FAULT"]
["1#阻垢剂加药泵启动","ns=6;s=P_1#ZGJB_OUTPUT"]
["1#阻垢剂加药泵启动准备好","ns=6;s=P_1#ZGJB_READY"]
["1#阻垢剂加药泵远程","ns=6;s=P_1#ZGJB_REM"]
["1#阻垢剂加药泵运行","ns=6;s=P_1#ZGJB_RFB"]
["1#中和还原剂加药泵自动启动","ns=6;s=P_1#ZH_HYJ_AUTOSTART"]
["1#中和还原剂加药泵手自动","ns=6;s=P_1#ZH_HYJ_BT_AUTO"]
["1#中和还原剂加药泵故障复位","ns=6;s=P_1#ZH_HYJ_BT_RESET"]
["1#中和还原剂加药泵手动启动","ns=6;s=P_1#ZH_HYJ_BT_START"]
["1#中和还原剂加药泵手动停止","ns=6;s=P_1#ZH_HYJ_BT_STOP"]
["1#中和还原剂加药泵故障","ns=6;s=P_1#ZH_HYJ_FAULT"]
["1#中和还原剂加药泵启动","ns=6;s=P_1#ZH_HYJ_OUTPUT"]
["1#中和还原剂加药泵启动准备好","ns=6;s=P_1#ZH_HYJ_READY"]
["1#中和还原剂加药泵远程","ns=6;s=P_1#ZH_HYJ_REM"]
["1#中和还原剂加药泵运行","ns=6;s=P_1#ZH_HYJ_RFB"]
["2#次钠加药泵自动启动","ns=6;s=P_2#CNB_AUTOSTART"]
["2#次钠加药泵手自动","ns=6;s=P_2#CNB_BT_AUTO"]
["2#次钠加药泵故障复位","ns=6;s=P_2#CNB_BT_RESET"]
["2#次钠加药泵手动启动","ns=6;s=P_2#CNB_BT_START"]
["2#次钠加药泵手动停止","ns=6;s=P_2#CNB_BT_STOP"]
["2#次钠加药泵故障","ns=6;s=P_2#CNB_FAULT"]
["2#次钠加药泵启动","ns=6;s=P_2#CNB_OUTPUT"]
["2#次钠加药泵启动准备好","ns=6;s=P_2#CNB_READY"]
["2#次钠加药泵远程","ns=6;s=P_2#CNB_REM"]
["2#次钠加药泵运行","ns=6;s=P_2#CNB_RFB"]
["2#出水碱加药泵自动启动","ns=6;s=P_2#CSJB_AUTOSTART"]
["2#出水碱加药泵手自动","ns=6;s=P_2#CSJB_BT_AUTO"]
["2#出水碱加药泵故障复位","ns=6;s=P_2#CSJB_BT_RESET"]
["2#出水碱加药泵手动启动","ns=6;s=P_2#CSJB_BT_START"]
["2#出水碱加药泵手动停止","ns=6;s=P_2#CSJB_BT_STOP"]
["2#出水碱加药泵故障","ns=6;s=P_2#CSJB_FAULT"]
["2#出水碱加药泵启动","ns=6;s=P_2#CSJB_OUTPUT"]
["2#出水碱加药泵启动准备好","ns=6;s=P_2#CSJB_READY"]
["2#出水碱加药泵远程","ns=6;s=P_2#CSJB_REM"]
["2#出水碱加药泵运行","ns=6;s=P_2#CSJB_RFB"]
["2#回用水泵自动启动","ns=6;s=P_2#HYSB_AUTOSTART"]
["2#回用水泵手自动","ns=6;s=P_2#HYSB_BT_AUTO"]
["2#回用水泵故障复位","ns=6;s=P_2#HYSB_BT_RESET"]
["2#回用水泵手动启动","ns=6;s=P_2#HYSB_BT_START"]
["2#回用水泵手动停止","ns=6;s=P_2#HYSB_BT_STOP"]
["2#回用水泵故障","ns=6;s=P_2#HYSB_FAULT"]
["2#回用水泵启动","ns=6;s=P_2#HYSB_OUTPUT"]
["2#回用水泵启动准备好","ns=6;s=P_2#HYSB_READY"]
["2#回用水泵远程","ns=6;s=P_2#HYSB_REM"]
["2#回用水泵运行","ns=6;s=P_2#HYSB_RFB"]
["2#PAC加药泵自动启动","ns=6;s=P_2#PACB_AUTOSTART"]
["2#PAC加药泵手自动","ns=6;s=P_2#PACB_BT_AUTO"]
["2#PAC加药泵故障复位","ns=6;s=P_2#PACB_BT_RESET"]
["2#PAC加药泵手动启动","ns=6;s=P_2#PACB_BT_START"]
["2#PAC加药泵手动停止","ns=6;s=P_2#PACB_BT_STOP"]
["2#PAC加药泵故障","ns=6;s=P_2#PACB_FAULT"]
["2#PAC加药泵启动","ns=6;s=P_2#PACB_OUTPUT"]
["2#PAC加药泵启动准备好","ns=6;s=P_2#PACB_READY"]
["2#PAC加药泵远程","ns=6;s=P_2#PACB_REM"]
["2#PAC加药泵运行","ns=6;s=P_2#PACB_RFB"]
["2#RO段间泵自动启动","ns=6;s=P_2#RODJB_AUTOSTART"]
["2#RO段间泵手自动","ns=6;s=P_2#RODJB_BT_AUTO"]
["2#RO段间泵故障复位","ns=6;s=P_2#RODJB_BT_RESET"]
["2#RO段间泵手动启动","ns=6;s=P_2#RODJB_BT_START"]
["2#RO段间泵手动停止","ns=6;s=P_2#RODJB_BT_STOP"]
["2#RO段间泵故障","ns=6;s=P_2#RODJB_FAULT"]
["2#RO段间泵启动","ns=6;s=P_2#RODJB_OUTPUT"]
["2#RO段间泵启动准备好","ns=6;s=P_2#RODJB_READY"]
["2#RO段间泵远程","ns=6;s=P_2#RODJB_REM"]
["2#RO段间泵运行","ns=6;s=P_2#RODJB_RFB"]
["2#RO高压泵自动启动","ns=6;s=P_2#ROGYB_AUTOSTART"]
["2#RO高压泵手自动","ns=6;s=P_2#ROGYB_BT_AUTO"]
["2#RO高压泵故障复位","ns=6;s=P_2#ROGYB_BT_RESET"]
["2#RO高压泵手动启动","ns=6;s=P_2#ROGYB_BT_START"]
["2#RO高压泵手动停止","ns=6;s=P_2#ROGYB_BT_STOP"]
["2#RO高压泵故障","ns=6;s=P_2#ROGYB_FAULT"]
["2#RO高压泵启动","ns=6;s=P_2#ROGYB_OUTPUT"]
["2#RO高压泵启动准备好","ns=6;s=P_2#ROGYB_READY"]
["2#RO高压泵远程","ns=6;s=P_2#ROGYB_REM"]
["2#RO高压泵运行","ns=6;s=P_2#ROGYB_RFB"]
["2#RO还原剂加药泵自动启动","ns=6;s=P_2#HYJB_AUTOSTART"]
["2#RO还原剂加药泵手自动","ns=6;s=P_2#HYJB_BT_AUTO"]
["2#RO还原剂加药泵故障复位","ns=6;s=P_2#HYJB_BT_RESET"]
["2#RO还原剂加药泵手动启动","ns=6;s=P_2#HYJB_BT_START"]
["2#RO还原剂加药泵手动停止","ns=6;s=P_2#HYJB_BT_STOP"]
["2#RO还原剂加药泵故障","ns=6;s=P_2#HYJB_FAULT"]
["2#RO还原剂加药泵启动","ns=6;s=P_2#HYJB_OUTPUT"]
["2#RO还原剂加药泵启动准备好","ns=6;s=P_2#HYJB_READY"]
["2#RO还原剂加药泵远程","ns=6;s=P_2#HYJB_REM"]
["2#RO还原剂加药泵运行","ns=6;s=P_2#HYJB_RFB"]
["2#酸加药泵自动启动","ns=6;s=P_2#SB_AUTOSTART"]
["2#酸加药泵手自动","ns=6;s=P_2#SB_BT_AUTO"]
["2#酸加药泵故障复位","ns=6;s=P_2#SB_BT_RESET"]
["2#酸加药泵手动启动","ns=6;s=P_2#SB_BT_START"]
["2#酸加药泵手动停止","ns=6;s=P_2#SB_BT_STOP"]
["2#酸加药泵故障","ns=6;s=P_2#SB_FAULT"]
["2#酸加药泵启动","ns=6;s=P_2#SB_OUTPUT"]
["2#酸加药泵启动准备好","ns=6;s=P_2#SB_RE"]
["2#酸加药泵远程","ns=6;s=P_2#SB_READY"]
["2#酸加药泵运行","ns=6;s=P_2#SB_RFB"]
["2#杀菌剂加药泵自动启动","ns=6;s=P_2#SJB_AUTOSTART"]
["2#杀菌剂加药泵手自动","ns=6;s=P_2#SJB_BT_AUTO"]
["2#杀菌剂加药泵故障复位","ns=6;s=P_2#SJB_BT_RESET"]
["2#杀菌剂加药泵手动启动","ns=6;s=P_2#SJB_BT_START"]
["2#杀菌剂加药泵手动停止","ns=6;s=P_2#SJB_BT_STOP"]
["2#杀菌剂加药泵故障","ns=6;s=P_2#SJB_FAULT"]
["2#杀菌剂加药泵启动","ns=6;s=P_2#SJB_OUTPUT"]
["2#杀菌剂加药泵启动准备好","ns=6;s=P_2#SJB_READY"]
["2#杀菌剂加药泵远程","ns=6;s=P_2#SJB_REM"]
["2#杀菌剂加药泵运行","ns=6;s=P_2#SJB_RFB"]
["2#超滤碱加药泵自动启动","ns=6;s=P_2#UF_JB_AUTOSTART"]
["2#超滤碱加药泵手自动","ns=6;s=P_2#UF_JB_BT_AUTO"]
["2#超滤碱加药泵故障复位","ns=6;s=P_2#UF_JB_BT_RESET"]
["2#超滤碱加药泵手动启动","ns=6;s=P_2#UF_JB_BT_START"]
["2#超滤碱加药泵手动停止","ns=6;s=P_2#UF_JB_BT_STOP"]
["2#超滤碱加药泵故障","ns=6;s=P_2#UF_JB_FAULT"]
["2#超滤碱加药泵启动","ns=6;s=P_2#UF_JB_OUTPUT"]
["2#超滤碱加药泵启动准备好","ns=6;s=P_2#UF_JB_READY"]
["2#超滤碱加药泵远程","ns=6;s=P_2#UF_JB_REM"]
["2#超滤碱加药泵运行","ns=6;s=P_2#UF_JB_RFB"]
["2#超滤反洗泵自动启动","ns=6;s=P_2#UFBWB_AUTOSTART"]
["2#超滤反洗泵手自动","ns=6;s=P_2#UFBWB_BT_AUTO"]
["2#超滤反洗泵故障复位","ns=6;s=P_2#UFBWB_BT_RESET"]
["2#超滤反洗泵手动启动","ns=6;s=P_2#UFBWB_BT_START"]
["2#超滤反洗泵手动停止","ns=6;s=P_2#UFBWB_BT_STOP"]
["2#超滤反洗泵故障","ns=6;s=P_2#UFBWB_FAULT"]
["2#超滤反洗泵启动","ns=6;s=P_2#UFBWB_OUTPUT"]
["2#超滤反洗泵启动准备好","ns=6;s=P_2#UFBWB_READY"]
["2#超滤反洗泵远程","ns=6;s=P_2#UFBWB_REM"]
["2#超滤反洗泵运行","ns=6;s=P_2#UFBWB_RFB"]
["2#阻垢剂加药泵自动启动","ns=6;s=P_2#ZGJB_AUTOSTART"]
["2#阻垢剂加药泵手自动","ns=6;s=P_2#ZGJB_BT_AUTO"]
["2#阻垢剂加药泵故障复位","ns=6;s=P_2#ZGJB_BT_RESET"]
["2#阻垢剂加药泵手动启动","ns=6;s=P_2#ZGJB_BT_START"]
["2#阻垢剂加药泵手动停止","ns=6;s=P_2#ZGJB_BT_STOP"]
["2#阻垢剂加药泵故障","ns=6;s=P_2#ZGJB_FAULT"]
["2#阻垢剂加药泵启动","ns=6;s=P_2#ZGJB_OUTPUT"]
["2#阻垢剂加药泵启动准备好","ns=6;s=P_2#ZGJB_READY"]
["2#阻垢剂加药泵远程","ns=6;s=P_2#ZGJB_REM"]
["2#阻垢剂加药泵运行","ns=6;s=P_2#ZGJB_RFB"]
["2#中和还原剂加药泵自动启动","ns=6;s=P_2#ZH_HYJ_AUTOSTART"]
["2#中和还原剂加药泵手自动","ns=6;s=P_2#ZH_HYJ_BT_AUTO"]
["2#中和还原剂加药泵故障复位","ns=6;s=P_2#ZH_HYJ_BT_RESET"]
["2#中和还原剂加药泵手动启动","ns=6;s=P_2#ZH_HYJ_BT_START"]
["2#中和还原剂加药泵手动停止","ns=6;s=P_2#ZH_HYJ_BT_STOP"]
["2#中和还原剂加药泵故障","ns=6;s=P_2#ZH_HYJ_FAULT"]
["2#中和还原剂加药泵启动","ns=6;s=P_2#ZH_HYJ_OUTPUT"]
["2#中和还原剂加药泵启动准备好","ns=6;s=P_2#ZH_HYJ_READY"]
["2#中和还原剂加药泵远程","ns=6;s=P_2#ZH_HYJ_REM"]
["2#中和还原剂加药泵运行","ns=6;s=P_2#ZH_HYJ_RFB"]
["3#阻垢剂加药泵自动启动","ns=6;s=P_3#ZGJB_AUTOSTART"]
["3#阻垢剂加药泵手自动","ns=6;s=P_3#ZGJB_BT_AUTO"]
["3#阻垢剂加药泵故障复位","ns=6;s=P_3#ZGJB_BT_RESET"]
["3#阻垢剂加药泵手动启动","ns=6;s=P_3#ZGJB_BT_START"]
["3#阻垢剂加药泵手动停止","ns=6;s=P_3#ZGJB_BT_STOP"]
["3#阻垢剂加药泵故障","ns=6;s=P_3#ZGJB_FAULT"]
["3#阻垢剂加药泵启动","ns=6;s=P_3#ZGJB_OUTPUT"]
["3#阻垢剂加药泵启动准备好","ns=6;s=P_3#ZGJB_READY"]
["3#阻垢剂加药泵远程","ns=6;s=P_3#ZGJB_REM"]
["3#阻垢剂加药泵运行","ns=6;s=P_3#ZGJB_RFB"]
["废水泵自动启动","ns=6;s=P_FSB_AUTOSTART"]
["废水泵手自动","ns=6;s=P_FSB_BT_AUTO"]
["废水泵故障复位","ns=6;s=P_FSB_BT_RESET"]
["废水泵手动启动","ns=6;s=P_FSB_BT_START"]
["废水泵手动停止","ns=6;s=P_FSB_BT_STOP"]
["废水泵故障","ns=6;s=P_FSB_FAULT"]
["废水泵启动","ns=6;s=P_FSB_OUTPUT"]
["废水泵启动准备好","ns=6;s=P_FSB_READY"]
["废水泵远程","ns=6;s=P_FSB_REM"]
["废水泵运行","ns=6;s=P_FSB_RFB"]
["加热器自动启动","ns=6;s=P_JRQ_AUTOSTART"]
["加热器手自动","ns=6;s=P_JRQ_BT_AUTO"]
["加热器故障复位","ns=6;s=P_JRQ_BT_RESET"]
["加热器手动启动","ns=6;s=P_JRQ_BT_START"]
["加热器手动停止","ns=6;s=P_JRQ_BT_STOP"]
["加热器故障","ns=6;s=P_JRQ_FAULT"]
["加热器启动","ns=6;s=P_JRQ_OUTPUT"]
["加热器启动准备好","ns=6;s=P_JRQ_READY"]
["加热器远程","ns=6;s=P_JRQ_REM"]
["加热器运行","ns=6;s=P_JRQ_RFB"]
["潜污泵自动启动","ns=6;s=P_QWB_AUTOSTART"]
["潜污泵手自动","ns=6;s=P_QWB_BT_AUTO"]
["潜污泵故障复位","ns=6;s=P_QWB_BT_RESET"]
["潜污泵手动启动","ns=6;s=P_QWB_BT_START"]
["潜污泵手动停止","ns=6;s=P_QWB_BT_STOP"]
["潜污泵故障","ns=6;s=P_QWB_FAULT"]
["潜污泵启动","ns=6;s=P_QWB_OUTPUT"]
["潜污泵启动准备好","ns=6;s=P_QWB_READY"]
["潜污泵远程","ns=6;s=P_QWB_REM"]
["潜污泵运行","ns=6;s=P_QWB_RFB"]
["清洗水泵自动启动","ns=6;s=P_QXSB_AUTOSTART"]
["清洗水泵手自动","ns=6;s=P_QXSB_BT_AUTO"]
["清洗水泵故障复位","ns=6;s=P_QXSB_BT_RESET"]
["清洗水泵手动启动","ns=6;s=P_QXSB_BT_START"]
["清洗水泵手动停止","ns=6;s=P_QXSB_BT_STOP"]
["清洗水泵故障","ns=6;s=P_QXSB_FAULT"]
["清洗水泵启动","ns=6;s=P_QXSB_OUTPUT"]
["清洗水泵启动准备好","ns=6;s=P_QXSB_READY"]
["清洗水泵远程","ns=6;s=P_QXSB_REM"]
["清洗水泵运行","ns=6;s=P_QXSB_RFB"]
["反渗透供水泵自动启动","ns=6;s=P_ROGSB_AUTOSTART"]
["反渗透供水泵手自动","ns=6;s=P_ROGSB_BT_AUTO"]
["反渗透供水泵故障复位","ns=6;s=P_ROGSB_BT_RESET"]
["反渗透供水泵手动启动","ns=6;s=P_ROGSB_BT_START"]
["反渗透供水泵手动停止","ns=6;s=P_ROGSB_BT_STOP"]
["反渗透供水泵故障","ns=6;s=P_ROGSB_FAULT"]
["反渗透供水泵启动","ns=6;s=P_ROGSB_OUTPUT"]
["反渗透供水泵启动准备好","ns=6;s=P_ROGSB_READY"]
["反渗透供水泵远程","ns=6;s=P_ROGSB_REM"]
["反渗透供水泵运行","ns=6;s=P_ROGSB_RFB"]
["超滤供水泵自动启动","ns=6;s=P_UFGSB_AUTOSTART"]
["超滤供水泵手自动","ns=6;s=P_UFGSB_BT_AUTO"]
["超滤供水泵故障复位","ns=6;s=P_UFGSB_BT_RESET"]
["超滤供水泵手动启动","ns=6;s=P_UFGSB_BT_START"]
["超滤供水泵手动停止","ns=6;s=P_UFGSB_BT_STOP"]
["超滤供水泵故障","ns=6;s=P_UFGSB_FAULT"]
["超滤供水泵启动","ns=6;s=P_UFGSB_OUTPUT"]
["超滤供水泵启动准备好","ns=6;s=P_UFGSB_READY"]
["超滤供水泵远程","ns=6;s=P_UFGSB_REM"]
["超滤供水泵运行","ns=6;s=P_UFGSB_RFB"]
["中和泵自动启动","ns=6;s=P_ZH_AUTOSTART"]
["中和泵手自动","ns=6;s=P_ZH_BT_AUTO"]
["中和泵故障复位","ns=6;s=P_ZH_BT_RESET"]
["中和泵手动启动","ns=6;s=P_ZH_BT_START"]
["中和泵手动停止","ns=6;s=P_ZH_BT_STOP"]
["中和泵故障","ns=6;s=P_ZH_FAULT"]
["中和泵启动","ns=6;s=P_ZH_OUTPUT"]
["中和泵启动准备好","ns=6;s=P_ZH_READY"]
["中和泵远程","ns=6;s=P_ZH_REM"]
["中和泵运行","ns=6;s=P_ZH_RFB"]
["RO1一段压差高","ns=6;s=RO1_1D_YC_HIGH"]
["RO1二三段碱维护按键","ns=6;s=RO1_2/3DJWH"]
["RO1二段压差高","ns=6;s=RO1_2D_YC_HIGH"]
["RO1执行一段碱维护","ns=6;s=RO1_ACT_1DJWH"]
["RO1执行一段杀菌","ns=6;s=RO1_ACT_1DSJ"]
["RO1执行一段酸维护","ns=6;s=RO1_ACT_1DSWH"]
["RO1执行二三段碱维护","ns=6;s=RO1_ACT_2/3DJWH"]
["RO1执行二三段杀菌维护","ns=6;s=RO1_ACT_2/3DSJWH"]
["RO1执行二三段酸维护","ns=6;s=RO1_ACT_2/3DSWH"]
["RO1执行冲洗","ns=6;s=RO1_ACT_CX"]
["RO1执行超越过滤","ns=6;s=RO1_ACT_CYGL"]
["RO1执行超越停机冲洗","ns=6;s=RO1_ACT_CYTJCX"]
["RO1执行超越停机加药冲洗","ns=6;s=RO1_ACT_CYTJJYCX"]
["RO1执行非正常停机冲洗","ns=6;s=RO1_ACT_FZCTJCX"]
["RO1执行过滤","ns=6;s=RO1_ACT_GL"]
["RO1执行长时间停机加药冲洗","ns=6;s=RO1_ACT_LONGTIME_CEB"]
["RO1允许冲洗","ns=6;s=RO1_ALLOW_CX"]
["RO1允许过滤","ns=6;s=RO1_ALLOW_GL"]
["RO1允许杀菌","ns=6;s=RO1_ALLOW_SJ"]
["RO1出栈","ns=6;s=RO1_APPLY_POP"]
["RO1清零出栈代码","ns=6;s=RO1_APPLY_POP_CLEAR"]
["RO1入栈","ns=6;s=RO1_APPLY_PUSH"]
["RO1启用反洗泵","ns=6;s=RO1_APPLY_RO_FXB"]
["RO1启用供水泵","ns=6;s=RO1_APPLY_RO_GSB"]
["RO1启用还原剂泵","ns=6;s=RO1_APPLY_RO_HYJB"]
["RO1启用还原剂阀","ns=6;s=RO1_APPLY_RO_HYJF"]
["RO1启用气洗阀","ns=6;s=RO1_APPLY_RO_QXF"]
["RO1启用阻垢剂泵","ns=6;s=RO1_APPLY_RO_ZGJB"]
["RO1启用杀菌泵","ns=6;s=RO1_APPLY_SJB"]
["RO1启用杀菌阀","ns=6;s=RO1_APPLY_SJF"]
["RO1启用维护碱泵","ns=6;s=RO1_APPLY_WHJB"]
["RO1启用维护碱阀","ns=6;s=RO1_APPLY_WHJF"]
["RO1启用维护酸泵","ns=6;s=RO1_APPLY_WHSB"]
["RO1启用维护酸阀","ns=6;s=RO1_APPLY_WHSF"]
["RO1自动启动","ns=6;s=RO1_AUTO_START"]
["RO1一段碱维护按键","ns=6;s=RO1_BT_1DJWH"]
["RO1一段酸维护按键","ns=6;s=RO1_BT_1DSWH"]
["RO1一段杀菌按键","ns=6;s=RO1_BT_1DXJ"]
["RO1二三段碱维护","ns=6;s=RO1_BT_2/3DJWH"]
["RO1二三段杀菌按键","ns=6;s=RO1_BT_2/3DSJ"]
["RO1二三段酸维护按键","ns=6;s=RO1_BT_2/3DSWH"]
["RO1自动维护按键","ns=6;s=RO1_BT_AUTO_WH"]
["RO1正常冲洗按键","ns=6;s=RO1_BT_CX"]
["RO1超越过滤按键","ns=6;s=RO1_BT_CYGL"]
["RO1超越模式按键","ns=6;s=RO1_BT_CYMS"]
["RO1超越停机冲洗按键","ns=6;s=RO1_BT_CYTJCX"]
["RO1超越停机加药冲洗按键","ns=6;s=RO1_BT_CYTJJYCX"]
["RO1急停按键","ns=6;s=RO1_BT_EMERGENCY"]
["RO1非正常冲洗按键","ns=6;s=RO1_BT_FZCCX"]
["RO1过滤按键","ns=6;s=RO1_BT_GL"]
["RO1初始化按键","ns=6;s=RO1_BT_INITIAL"]
["RO1复位按键","ns=6;s=RO1_BT_RESET"]
["RO1杀菌按键","ns=6;s=RO1_BT_SJ"]
["RO1启动按键","ns=6;s=RO1_BT_START"]
["RO1停止按键","ns=6;s=RO1_BT_STOP"]
["RO1自动按键","ns=6;s=RO1_BT_SYSTEMAUTO"]
["RO1手动按键","ns=6;s=RO1_BT_SYSTEMMANU"]
["RO1停机加药冲洗按键","ns=6;s=RO1_BT_TJJYCX"]
["RO1阀自动按键","ns=6;s=RO1_BT_VALVE_AUTO"]
["RO1电导率高","ns=6;s=RO1_DDL_HIGH"]
["RO1段间泵出口压力开关","ns=6;s=RO1_DJB_CKYLKG_OPEN"]
["RO1段间泵进口压力开关","ns=6;s=RO1_DJB_JKYLKG_CLOSE"]
["RO1正在过滤标记","ns=6;s=RO1_FLAG_GLING"]
["RO1系统准备好标记","ns=6;s=RO1_FLAG_SYS_READY"]
["RO1高压泵出口压力开关","ns=6;s=RO1_GYB_CKYLKG_OPEN"]
["RO1高压泵进口压力开关","ns=6;s=RO1_GYB_JKYLKG_CLOSE"]
["RO1系统报错","ns=6;s=RO1_SYSTEM_ERROR"]
["RO1该杀菌了","ns=6;s=RO1_TIME_FOR_SJ"]
["RO1阀准备好","ns=6;s=RO1_V_READY"]
["RO2一段压差高","ns=6;s=RO2_1D_YC_HIGH"]
["RO2二三段碱维护按键","ns=6;s=RO2_2/3DJWH"]
["RO2二段压差高","ns=6;s=RO2_2D_YC_HIGH"]
["RO2执行一段碱维护","ns=6;s=RO2_ACT_1DJWH"]
["RO2执行一段杀菌","ns=6;s=RO2_ACT_1DSJ"]
["RO2执行一段酸维护","ns=6;s=RO2_ACT_1DSWH"]
["RO2执行二三段碱维护","ns=6;s=RO2_ACT_2/3DJWH"]
["RO2执行二三段杀菌维护","ns=6;s=RO2_ACT_2/3DSJWH"]
["RO2执行二三段酸维护","ns=6;s=RO2_ACT_2/3DSWH"]
["RO2执行冲洗","ns=6;s=RO2_ACT_CX"]
["RO2执行超越过滤","ns=6;s=RO2_ACT_CYGL"]
["RO2执行超越停机冲洗","ns=6;s=RO2_ACT_CYTJCX"]
["RO2执行超越停机加药冲洗","ns=6;s=RO2_ACT_CYTJJYCX"]
["RO2执行非正常停机冲洗","ns=6;s=RO2_ACT_FZCTJCX"]
["RO2执行过滤","ns=6;s=RO2_ACT_GL"]
["RO2执行长时间停机加药冲洗","ns=6;s=RO2_ACT_LONGTIME_CEB"]
["RO2允许冲洗","ns=6;s=RO2_ALLOW_CX"]
["RO2允许过滤","ns=6;s=RO2_ALLOW_GL"]
["RO2允许杀菌","ns=6;s=RO2_ALLOW_SJ"]
["RO2出栈","ns=6;s=RO2_APPLY_POP"]
["RO2清零出栈代码","ns=6;s=RO2_APPLY_POP_CLEAR"]
["RO2入栈","ns=6;s=RO2_APPLY_PUSH"]
["RO2启用反洗泵","ns=6;s=RO2_APPLY_RO_FXB"]
["RO2启用供水泵","ns=6;s=RO2_APPLY_RO_GSB"]
["RO2启用还原剂泵","ns=6;s=RO2_APPLY_RO_HYJB"]
["RO2启用还原剂阀","ns=6;s=RO2_APPLY_RO_HYJF"]
["RO2启用气洗阀","ns=6;s=RO2_APPLY_RO_QXF"]
["RO2启用阻垢剂泵","ns=6;s=RO2_APPLY_RO_ZGJB"]
["RO2启用杀菌泵","ns=6;s=RO2_APPLY_SJB"]
["RO2启用杀菌阀","ns=6;s=RO2_APPLY_SJF"]
["RO2启用维护碱泵","ns=6;s=RO2_APPLY_WHJB"]
["RO2启用维护碱阀","ns=6;s=RO2_APPLY_WHJF"]
["RO2启用维护酸泵","ns=6;s=RO2_APPLY_WHSB"]
["RO2启用维护酸阀","ns=6;s=RO2_APPLY_WHSF"]
["RO2自动启动","ns=6;s=RO2_AUTO_START"]
["RO2一段碱维护按键","ns=6;s=RO2_BT_1DJWH"]
["RO2一段酸维护按键","ns=6;s=RO2_BT_1DSWH"]
["RO2一段杀菌按键","ns=6;s=RO2_BT_1DXJ"]
["RO2二三段碱维护","ns=6;s=RO2_BT_2/3DJWH"]
["RO2二三段杀菌按键","ns=6;s=RO2_BT_2/3DSJ"]
["RO2二三段酸维护按键","ns=6;s=RO2_BT_2/3DSWH"]
["RO2自动维护按键","ns=6;s=RO2_BT_AUTO_WH"]
["RO2正常冲洗按键","ns=6;s=RO2_BT_CX"]
["RO2超越过滤按键","ns=6;s=RO2_BT_CYGL"]
["RO2超越模式按键","ns=6;s=RO2_BT_CYMS"]
["RO2超越停机冲洗按键","ns=6;s=RO2_BT_CYTJCX"]
["RO2超越停机加药冲洗按键","ns=6;s=RO2_BT_CYTJJYCX"]
["RO2急停按键","ns=6;s=RO2_BT_EMERGENCY"]
["RO2非正常冲洗按键","ns=6;s=RO2_BT_FZCCX"]
["RO2过滤按键","ns=6;s=RO2_BT_GL"]
["RO2初始化按键","ns=6;s=RO2_BT_INITIAL"]
["RO2复位按键","ns=6;s=RO2_BT_RESET"]
["RO2杀菌按键","ns=6;s=RO2_BT_SJ"]
["RO2启动按键","ns=6;s=RO2_BT_START"]
["RO2停止按键","ns=6;s=RO2_BT_STOP"]
["RO2自动按键","ns=6;s=RO2_BT_SYSTEMAUTO"]
["RO2手动按键","ns=6;s=RO2_BT_SYSTEMMANU"]
["RO2停机加药冲洗按键","ns=6;s=RO2_BT_TJJYCX"]
["RO2阀自动按键","ns=6;s=RO2_BT_VALVE_AUTO"]
["RO2电导率高","ns=6;s=RO2_DDL_HIGH"]
["RO2段间泵出口压力开关","ns=6;s=RO2_DJB_CKYLKG_OPEN"]
["RO2段间泵进口压力开关","ns=6;s=RO2_DJB_JKYLKG_CLOSE"]
["RO2正在过滤标记","ns=6;s=RO2_FLAG_GLING"]
["RO2系统准备好标记","ns=6;s=RO2_FLAG_SYS_READY"]
["RO2高压泵出口压力开关","ns=6;s=RO2_GYB_CKYLKG_OPEN"]
["RO2高压泵进口压力开关","ns=6;s=RO2_GYB_JKYLKG_CLOSE"]
["RO2系统报错","ns=6;s=RO2_SYSTEM_ERROR"]
["RO2该杀菌了","ns=6;s=RO2_TIME_FOR_SJ"]
["RO2阀准备好","ns=6;s=RO2_V_READY"]
["UF1允许反洗","ns=6;s=UF1_ALLOW_BW"]
["UF1允许反洗气冲洗","ns=6;s=UF1_ALLOW_BWQCX"]
["UF1允许备用1","ns=6;s=UF1_ALLOW_BY1"]
["UF1允许备用2","ns=6;s=UF1_ALLOW_BY2"]
["UF1允许备用3","ns=6;s=UF1_ALLOW_BY3"]
["UF1允许CEB","ns=6;s=UF1_ALLOW_CEB"]
["UF1允许过滤","ns=6;s=UF1_ALLOW_GL"]
["UF1允许PAC","ns=6;s=UF1_ALLOW_PAC"]
["UF1启用供水泵","ns=6;s=UF1_APPLY_GSB"]
["UF1启用PAC泵","ns=6;s=UF1_APPLY_PAC_B"]
["UF1启用PAC阀","ns=6;s=UF1_APPLY_PAC-V"]
["UF1启用调节阀","ns=6;s=UF1_APPLY_TJV"]
["UF1自动过滤启动","ns=6;s=UF1_AUTOSTART_GL"]
["UF1手动反洗操作","ns=6;s=UF1_BT_BW"]
["UF1手动CEB操作","ns=6;s=UF1_BT_CEB"]
["UF1手动CIP操作","ns=6;s=UF1_BT_CIP"]
["UF1手动冲水操作","ns=6;s=UF1_BT_CS"]
["UF1手动清除过滤流量","ns=6;s=UF1_BT_ERASE_GLFLOW"]
["UF1停止操作","ns=6;s=UF1_BT_ESTOP"]
["UF1手动过滤操作","ns=6;s=UF1_BT_GL"]
["UF1手动初始化操作","ns=6;s=UF1_BT_INAI"]
["UF1手动屏蔽液位开关","ns=6;s=UF1_BT_PB_YWKG"]
["UF1故障复位操作","ns=6;s=UF1_BT_RESET"]
["UF1手自动模式操作","ns=6;s=UF1_BT_SYS_AUTO"]
["UF1阀门手自动操作","ns=6;s=UF1_BT_V_AUTO"]
["UF1 CEB碱选择","ns=6;s=UF1_CEB_J"]
["UF1 CEB酸选择","ns=6;s=UF1_CEB_S"]
["UF1压差高限值报错","ns=6;s=UF1_ERR_YC_H"]
["UF1压差高高值报错","ns=6;s=UF1_ERR_YC_HH"]
["UF1药剂残留报错","ns=6;s=UF1_ERR_YJCL"]
["UF1过滤准备好标志","ns=6;s=UF1_FLAG_GL_READY"]
["UF1膜内有药标志","ns=6;s=UF1_FLAG_MNYY"]
["UF1无它CEB标志","ns=6;s=UF1_FLAG_NOOTHERCEB"]
["UF1阀准备好标志","ns=6;s=UF1_FLAG_V_RRADY"]
["UF1系统报错","ns=6;s=UF1_SYS_ERR"]
["UF2允许反洗","ns=6;s=UF2_ALLOW_BW"]
["UF2允许反洗气冲洗","ns=6;s=UF2_ALLOW_BWQCX"]
["UF2允许备用1","ns=6;s=UF2_ALLOW_BY1"]
["UF2允许备用2","ns=6;s=UF2_ALLOW_BY2"]
["UF2允许备用3","ns=6;s=UF2_ALLOW_BY3"]
["UF2允许CEB","ns=6;s=UF2_ALLOW_CEB"]
["UF2允许过滤","ns=6;s=UF2_ALLOW_GL"]
["UF2允许PAC","ns=6;s=UF2_ALLOW_PAC"]
["UF2启用PAC泵","ns=6;s=UF2_APPLY_PAC_B"]
["UF2启用PAC阀","ns=6;s=UF2_APPLY_PAC_V"]
["UF2自动过滤启动","ns=6;s=UF2_AUTOSTART_GL"]
["UF2手动反洗操作","ns=6;s=UF2_BT_BW"]
["UF2手动CEB操作","ns=6;s=UF2_BT_CEB"]
["UF2手动CIP操作","ns=6;s=UF2_BT_CIP"]
["UF2手动冲水操作","ns=6;s=UF2_BT_CS"]
["UF2手动清除过滤流量","ns=6;s=UF2_BT_ERASE_GLFLOW"]
["UF2停止操作","ns=6;s=UF2_BT_ESTOP"]
["UF2手动过滤操作","ns=6;s=UF2_BT_GL"]
["UF2手动初始化操作","ns=6;s=UF2_BT_INAI"]
["UF2故障复位操作","ns=6;s=UF2_BT_RESET"]
["UF2手动屏蔽液位开关","ns=6;s=UF2_BT_PB_YWKG"]
["UF2手自动模式操作","ns=6;s=UF2_BT_SYS_AUTO"]
["UF2阀门手自动操作","ns=6;s=UF2_BT_V_AUTO"]
["UF2 CEB碱选择","ns=6;s=UF2_CEB_J"]
["UF2 CEB酸选择","ns=6;s=UF2_CEB_S"]
["UF2压差高限值报错","ns=6;s=UF2_ERR_YC_H"]
["UF2压差高高值报错","ns=6;s=UF2_ERR_YC_HH"]
["UF2药剂残留报错","ns=6;s=UF2_ERR_YJCL"]
["UF2过滤准备好标志","ns=6;s=UF2_FLAG_GL_READY"]
["UF2膜内有药标志","ns=6;s=UF2_FLAG_MNYY"]
["UF2无它CEB标志","ns=6;s=UF2_FLAG_NOOTHERCEB"]
["UF2阀准备好标志","ns=6;s=UF2_FLAG_V_READY"]
["UF2系统报错","ns=6;s=UF2_SYS_ERR"]
["UF1反洗进水阀手自动","ns=6;s=V_1#UF_BWJS_BT_AUTO"]
["UF1反洗进水阀手动关","ns=6;s=V_1#UF_BWJS_BT_CLOSE"]
["UF1反洗进水阀手动开","ns=6;s=V_1#UF_BWJS_BT_OPEN"]
["UF1反洗进水阀故障复位","ns=6;s=V_1#UF_BWJS_BT_RESET"]
["UF1反洗进水阀关到位","ns=6;s=V_1#UF_BWJS_CFB"]
["UF1反洗进水阀关闭中","ns=6;s=V_1#UF_BWJS_CING"]
["UF1反洗进水阀自动关闭","ns=6;s=V_1#UF_BWJS_CLOSEAUT"]
["UF1反洗进水阀故障","ns=6;s=V_1#UF_BWJS_ERR"]
["UF1反洗进水阀总故障","ns=6;s=V_1#UF_BWJS_ERRT"]
["UF1反洗进水阀开到位","ns=6;s=V_1#UF_BWJS_OFB"]
["UF1反洗进水阀打开中","ns=6;s=V_1#UF_BWJS_OING"]
["UF1反洗进水阀自动打开","ns=6;s=V_1#UF_BWJS_OPENAUTO"]
["UF1反洗进水阀关闭","ns=6;s=V_1#UF_BWJS_OUT_CLOS"]
["UF1反洗进水阀打开","ns=6;s=V_1#UF_BWJS_OUT_OPEN"]
["UF1反洗进水阀准备好","ns=6;s=V_1#UF_BWJS_READY"]
["UF1反洗进水阀远程","ns=6;s=V_1#UF_BWJS_REM"]
["UF1反洗排水阀手自动","ns=6;s=V_1#UF_BWPS_BT_AUTO"]
["UF1反洗排水阀手动关","ns=6;s=V_1#UF_BWPS_BT_CLOSE"]
["UF1反洗排水阀手动开","ns=6;s=V_1#UF_BWPS_BT_OPEN"]
["UF1反洗排水阀故障复位","ns=6;s=V_1#UF_BWPS_BT_RESET"]
["UF1反洗排水阀关到位","ns=6;s=V_1#UF_BWPS_CFB"]
["UF1反洗排水阀关闭中","ns=6;s=V_1#UF_BWPS_CING"]
["UF1反洗排水阀自动关闭","ns=6;s=V_1#UF_BWPS_CLOSEAUT"]
["UF1反洗排水阀故障","ns=6;s=V_1#UF_BWPS_ERR"]
["UF1反洗排水阀总故障","ns=6;s=V_1#UF_BWPS_ERRT"]
["UF1反洗排水阀开到位","ns=6;s=V_1#UF_BWPS_OFB"]
["UF1反洗排水阀打开中","ns=6;s=V_1#UF_BWPS_OING"]
["UF1反洗排水阀自动打开","ns=6;s=V_1#UF_BWPS_OPENAUTO"]
["UF1反洗排水阀关闭","ns=6;s=V_1#UF_BWPS_OUT_CLOS"]
["UF1反洗排水阀打开","ns=6;s=V_1#UF_BWPS_OUT_OPEN"]
["UF1反洗排水阀准备好","ns=6;s=V_1#UF_BWPS_READY"]
["UF1反洗排水阀远程","ns=6;s=V_1#UF_BWPS_REM"]
["UF1产水阀手自动","ns=6;s=V_1#UF_CS_BT_AUTO"]
["UF1产水阀手动关","ns=6;s=V_1#UF_CS_BT_CLOSE"]
["UF1产水阀手动开","ns=6;s=V_1#UF_CS_BT_OPEN"]
["UF1产水阀故障复位","ns=6;s=V_1#UF_CS_BT_RESET"]
["UF1产水阀关到位","ns=6;s=V_1#UF_CS_CFB"]
["UF1产水阀关闭中","ns=6;s=V_1#UF_CS_CING"]
["UF1产水阀自动关闭","ns=6;s=V_1#UF_CS_CLOSEAUTO"]
["UF1产水阀故障","ns=6;s=V_1#UF_CS_ERR"]
["UF1产水阀总故障","ns=6;s=V_1#UF_CS_ERRT"]
["UF1产水阀开到位","ns=6;s=V_1#UF_CS_OFB"]
["UF1产水阀打开中","ns=6;s=V_1#UF_CS_OING"]
["UF1产水阀自动打开","ns=6;s=V_1#UF_CS_OPENAUTO"]
["UF1产水阀关闭","ns=6;s=V_1#UF_CS_OUT_CLOSE"]
["UF1产水阀打开","ns=6;s=V_1#UF_CS_OUT_OPEN"]
["UF1产水阀准备好","ns=6;s=V_1#UF_CS_OUT_READY"]
["UF1产水阀远程","ns=6;s=V_1#UF_CS_REM"]
["UF1排气阀1手自动","ns=6;s=V_1#UF_PQ1_BT_AUTO"]
["UF1排气阀1手动关","ns=6;s=V_1#UF_PQ1_BT_CLOSE"]
["UF1排气阀1手动开","ns=6;s=V_1#UF_PQ1_BT_OPEN"]
["UF1排气阀1故障复位","ns=6;s=V_1#UF_PQ1_BT_RESET"]
["UF1排气阀1关到位","ns=6;s=V_1#UF_PQ1_CFB"]
["UF1排气阀1关闭中","ns=6;s=V_1#UF_PQ1_CING"]
["UF1排气阀1自动关闭","ns=6;s=V_1#UF_PQ1_CLOSEAUTO"]
["UF1排气阀1故障","ns=6;s=V_1#UF_PQ1_ERR"]
["UF1排气阀1总故障","ns=6;s=V_1#UF_PQ1_ERRT"]
["UF1排气阀1开到位","ns=6;s=V_1#UF_PQ1_OFB"]
["UF1排气阀1打开中","ns=6;s=V_1#UF_PQ1_OING"]
["UF1排气阀1自动打开","ns=6;s=V_1#UF_PQ1_OPENAUTO"]
["UF1排气阀1关闭","ns=6;s=V_1#UF_PQ1_OUT_CLOSE"]
["UF1排气阀1打开","ns=6;s=V_1#UF_PQ1_OUT_OPEN"]
["UF1排气阀1准备好","ns=6;s=V_1#UF_PQ1_OUT_READY"]
["UF1排气阀1远程","ns=6;s=V_1#UF_PQ1_REM"]
["UF1排气阀2手自动","ns=6;s=V_1#UF_PQ2_BT_AUTO"]
["UF1排气阀2手动关","ns=6;s=V_1#UF_PQ2_BT_CLOSE"]
["UF1排气阀2手动开","ns=6;s=V_1#UF_PQ2_BT_OPEN"]
["UF1排气阀2故障复位","ns=6;s=V_1#UF_PQ2_BT_RESET"]
["UF1排气阀2关到位","ns=6;s=V_1#UF_PQ2_CFB"]
["UF1排气阀2关闭中","ns=6;s=V_1#UF_PQ2_CING"]
["UF1排气阀2自动关闭","ns=6;s=V_1#UF_PQ2_CLOSEAUTO"]
["UF1排气阀2故障","ns=6;s=V_1#UF_PQ2_ERR"]
["UF1排气阀2总故障","ns=6;s=V_1#UF_PQ2_ERRT"]
["UF1排气阀2开到位","ns=6;s=V_1#UF_PQ2_OFB"]
["UF1排气阀2打开中","ns=6;s=V_1#UF_PQ2_OING"]
["UF1排气阀2自动打开","ns=6;s=V_1#UF_PQ2_OPENAUTO"]
["UF1排气阀2关闭","ns=6;s=V_1#UF_PQ2_OUT_CLOSE"]
["UF1排气阀2打开","ns=6;s=V_1#UF_PQ2_OUT_OPEN"]
["UF1排气阀2准备好","ns=6;s=V_1#UF_PQ2_OUT_READY"]
["UF1排气阀2远程","ns=6;s=V_1#UF_PQ2_REM"]
["UF1排气阀3手自动","ns=6;s=V_1#UF_PQ3_BT_AUTO"]
["UF1排气阀3手动关","ns=6;s=V_1#UF_PQ3_BT_CLOSE"]
["UF1排气阀3手动开","ns=6;s=V_1#UF_PQ3_BT_OPEN"]
["UF1排气阀3故障复位","ns=6;s=V_1#UF_PQ3_BT_RESET"]
["UF1排气阀3关到位","ns=6;s=V_1#UF_PQ3_CFB"]
["UF1排气阀3关闭中","ns=6;s=V_1#UF_PQ3_CING"]
["UF1排气阀3自动关闭","ns=6;s=V_1#UF_PQ3_CLOSEAUTO"]
["UF1排气阀3故障","ns=6;s=V_1#UF_PQ3_ERR"]
["UF1排气阀3总故障","ns=6;s=V_1#UF_PQ3_ERRT"]
["UF1排气阀3开到位","ns=6;s=V_1#UF_PQ3_OFB"]
["UF1排气阀3打开中","ns=6;s=V_1#UF_PQ3_OING"]
["UF1排气阀3自动打开","ns=6;s=V_1#UF_PQ3_OPENAUTO"]
["UF1排气阀3关闭","ns=6;s=V_1#UF_PQ3_OUT_CLOSE"]
["UF1排气阀3打开","ns=6;s=V_1#UF_PQ3_OUT_OPEN"]
["UF1排气阀3准备好","ns=6;s=V_1#UF_PQ3_READY"]
["UF1排气阀3远程","ns=6;s=V_1#UF_PQ3_REM"]
["UF1排气阀4手自动","ns=6;s=V_1#UF_PQ4_BT_AUTO"]
["UF1排气阀4手动关","ns=6;s=V_1#UF_PQ4_BT_CLOSE"]
["UF1排气阀4手动开","ns=6;s=V_1#UF_PQ4_BT_OPEN"]
["UF1排气阀4故障复位","ns=6;s=V_1#UF_PQ4_BT_RESET"]
["UF1排气阀4关到位","ns=6;s=V_1#UF_PQ4_CFB"]
["UF1排气阀4关闭中","ns=6;s=V_1#UF_PQ4_CING"]
["UF1排气阀4自动关闭","ns=6;s=V_1#UF_PQ4_CLOSEAUTO"]
["UF1排气阀4故障","ns=6;s=V_1#UF_PQ4_ERR"]
["UF1排气阀4总故障","ns=6;s=V_1#UF_PQ4_ERRT"]
["UF1排气阀4开到位","ns=6;s=V_1#UF_PQ4_OFB"]
["UF1排气阀4打开中","ns=6;s=V_1#UF_PQ4_OING"]
["UF1排气阀4自动打开","ns=6;s=V_1#UF_PQ4_OPENAUTO"]
["UF1排气阀4关闭","ns=6;s=V_1#UF_PQ4_OUT_CLOSE"]
["UF1排气阀4打开","ns=6;s=V_1#UF_PQ4_OUT_OPEN"]
["UF1排气阀4准备好","ns=6;s=V_1#UF_PQ4_OUT_READY"]
["UF1排气阀4远程","ns=6;s=V_1#UF_PQ4_REM"]
["UF1隔断阀手自动","ns=6;s=V_1#UFCIPGL_BT_AUTO"]
["UF1隔断阀手动关","ns=6;s=V_1#UFCIPGL_BT_CLOSE"]
["UF1隔断阀手动开","ns=6;s=V_1#UFCIPGL_BT_OPEN"]
["UF1隔断阀故障复位","ns=6;s=V_1#UFCIPGL_BT_RESET"]
["UF1隔断阀关到位","ns=6;s=V_1#UFCIPGL_CFB"]
["UF1隔断阀关闭中","ns=6;s=V_1#UFCIPGL_CING"]
["UF1隔断阀自动关闭","ns=6;s=V_1#UFCIPGL_CLOSEA"]
["UF1隔断阀故障","ns=6;s=V_1#UFCIPGL_EER"]
["UF1隔断阀总故障","ns=6;s=V_1#UFCIPGL_ERRT"]
["UF1隔断阀开到位","ns=6;s=V_1#UFCIPGL_OFB"]
["UF1隔断阀打开中","ns=6;s=V_1#UFCIPGL_OING"]
["UF1隔断阀自动打开","ns=6;s=V_1#UFCIPGL_OPENAU"]
["UF1隔断阀关闭","ns=6;s=V_1#UFCIPGL_OUT_CL"]
["UF1隔断阀打开","ns=6;s=V_1#UFCIPGL_OUT_OP"]
["UF1隔断阀准备好","ns=6;s=V_1#UFCIPGL_READY"]
["UF1隔断阀远程","ns=6;s=V_1#UFCIPGL_REM"]
["RO1不合格阀手自动","ns=6;s=V_1RO_BHG_BT_AUTO"]
["RO1不合格阀手动关","ns=6;s=V_1RO_BHG_BT_CLOSE"]
["RO1不合格阀手动开","ns=6;s=V_1RO_BHG_BT_OPEN"]
["RO1不合格阀故障复位","ns=6;s=V_1RO_BHG_BT_RESET"]
["RO1不合格阀关到位","ns=6;s=V_1RO_BHG_CFB"]
["RO1不合格阀关闭中","ns=6;s=V_1RO_BHG_CING"]
["RO1不合格阀自动关闭","ns=6;s=V_1RO_BHG_CLOSEAUTO"]
["RO1不合格阀故障","ns=6;s=V_1RO_BHG_ERR"]
["RO1不合格阀总故障","ns=6;s=V_1RO_BHG_ERRT"]
["RO1不合格阀开到位","ns=6;s=V_1RO_BHG_OFB"]
["RO1不合格阀打开中","ns=6;s=V_1RO_BHG_OING"]
["RO1不合格阀自动打开","ns=6;s=V_1RO_BHG_OPENAUTO"]
["RO1不合格阀关闭","ns=6;s=V_1RO_BHG_OUT_CLOSE"]
["RO1不合格阀打开","ns=6;s=V_1RO_BHG_OUT_OPEN"]
["RO1不合格阀准备好","ns=6;s=V_1RO_BHG_OUT_READY"]
["RO1不合格阀远程","ns=6;s=V_1RO_BHG_REM"]
["RO1产水阀手自动","ns=6;s=V_1RO_CS_BT_AUTO"]
["RO1产水阀手动关","ns=6;s=V_1RO_CS_BT_CLOSE"]
["RO1产水阀手动开","ns=6;s=V_1RO_CS_BT_OPEN"]
["RO1产水阀故障复位","ns=6;s=V_1RO_CS_BT_RESET"]
["RO1产水阀关到位","ns=6;s=V_1RO_CS_CFB"]
["RO1产水阀关闭中","ns=6;s=V_1RO_CS_CING"]
["RO1产水阀自动关闭","ns=6;s=V_1RO_CS_CLOSEAUTO"]
["RO1产水阀故障","ns=6;s=V_1RO_CS_ERR"]
["RO1产水阀总故障","ns=6;s=V_1RO_CS_ERRT"]
["RO1产水阀开到位","ns=6;s=V_1RO_CS_OFB"]
["RO1产水阀打开中","ns=6;s=V_1RO_CS_OING"]
["RO1产水阀自动打开","ns=6;s=V_1RO_CS_OPENAUTO"]
["RO1产水阀关闭","ns=6;s=V_1RO_CS_OUT_CLOSE"]
["RO1产水阀打开","ns=6;s=V_1RO_CS_OUT_OPEN"]
["RO1产水阀准备好","ns=6;s=V_1RO_CS_OUT_READY"]
["RO1产水阀远程","ns=6;s=V_1RO_CS_REM"]
["RO1进水阀手自动","ns=6;s=V_1RO_JS_BT_AUTO"]
["RO1进水阀手动关","ns=6;s=V_1RO_JS_BT_CLOSE"]
["RO1进水阀手动开","ns=6;s=V_1RO_JS_BT_OPEN"]
["RO1进水阀故障复位","ns=6;s=V_1RO_JS_BT_RESET"]
["RO1进水阀关到位","ns=6;s=V_1RO_JS_CFB"]
["RO1进水阀关闭中","ns=6;s=V_1RO_JS_CING"]
["RO1进水阀自动关闭","ns=6;s=V_1RO_JS_CLOSEA"]
["RO1进水阀故障","ns=6;s=V_1RO_JS_ERR"]
["RO1进水阀总故障","ns=6;s=V_1RO_JS_ERRT"]
["RO1进水阀开到位","ns=6;s=V_1RO_JS_OFB"]
["RO1进水阀打开中","ns=6;s=V_1RO_JS_OING"]
["RO1进水阀自动打开","ns=6;s=V_1RO_JS_OPENA"]
["RO1进水阀关闭","ns=6;s=V_1RO_JS_OUT_CLOSE"]
["RO1进水阀打开","ns=6;s=V_1RO_JS_OUT_OPEN"]
["RO1进水阀准备好","ns=6;s=V_1RO_JS_OUT_READY"]
["RO1进水阀远程","ns=6;s=V_1RO_JS_REM"]
["RO1二段产水排气阀手自动","ns=6;s=V_1ROEDCSPQ_BT_AUTO"]
["RO1二段产水排气阀手动关","ns=6;s=V_1ROEDCSPQ_BT_CLOSE"]
["RO1二段产水排气阀手动开","ns=6;s=V_1ROEDCSPQ_BT_OPEN"]
["RO1二段产水排气阀故障复位","ns=6;s=V_1ROEDCSPQ_BT_RESET"]
["RO1二段产水排气阀关到位","ns=6;s=V_1ROEDCSPQ_CFB"]
["RO1二段产水排气阀关闭中","ns=6;s=V_1ROEDCSPQ_CING"]
["RO1二段产水排气阀自动关闭","ns=6;s=V_1ROEDCSPQ_CLOSEA"]
["RO1二段产水排气阀故障","ns=6;s=V_1ROEDCSPQ_ERR"]
["RO1二段产水排气阀总故障","ns=6;s=V_1ROEDCSPQ_ERRT"]
["RO1二段产水排气阀开到位","ns=6;s=V_1ROEDCSPQ_OFB"]
["RO1二段产水排气阀打开中","ns=6;s=V_1ROEDCSPQ_OING"]
["RO1二段产水排气阀自动打开","ns=6;s=V_1ROEDCSPQ_OPENA"]
["RO1二段产水排气阀关闭","ns=6;s=V_1ROEDCSPQ_OUT_C"]
["RO1二段产水排气阀打开","ns=6;s=V_1ROEDCSPQ_OUT_O"]
["RO1二段产水排气阀准备好","ns=6;s=V_1ROEDCSPQ_READY"]
["RO1二段产水排气阀远程","ns=6;s=V_1ROEDCSPQ_REM"]
["RO1二段进水排气阀手自动","ns=6;s=V_1ROEDJSPQ_BT_AUTO"]
["RO1二段进水排气阀手动关","ns=6;s=V_1ROEDJSPQ_BT_CLOSE"]
["RO1二段进水排气阀手动开","ns=6;s=V_1ROEDJSPQ_BT_OPEN"]
["RO1二段进水排气阀故障复位","ns=6;s=V_1ROEDJSPQ_BT_RESET"]
["RO1二段进水排气阀关到位","ns=6;s=V_1ROEDJSPQ_CFB"]
["RO1二段进水排气阀关闭中","ns=6;s=V_1ROEDJSPQ_CING"]
["RO1二段进水排气阀自动关闭","ns=6;s=V_1ROEDJSPQ_CLOSE"]
["RO1二段进水排气阀故障","ns=6;s=V_1ROEDJSPQ_ERR"]
["RO1二段进水排气阀总故障","ns=6;s=V_1ROEDJSPQ_ERRT"]
["RO1二段进水排气阀开到位","ns=6;s=V_1ROEDJSPQ_OFB"]
["RO1二段进水排气阀打开中","ns=6;s=V_1ROEDJSPQ_OING"]
["RO1二段进水排气阀自动打开","ns=6;s=V_1ROEDJSPQ_OPENA"]
["RO1二段进水排气阀关闭","ns=6;s=V_1ROEDJSPQ_OUT_C"]
["RO1二段进水排气阀打开","ns=6;s=V_1ROEDJSPQ_OUT_O"]
["RO1二段进水排气阀准备好","ns=6;s=V_1ROEDJSPQ_READY"]
["RO1二段进水排气阀远程","ns=6;s=V_1ROEDJSPQ_REM"]
["RO1二段浓水排气阀手自动","ns=6;s=V_1ROEDNSPQ_BT_AUTO"]
["RO1二段浓水排气阀手动关","ns=6;s=V_1ROEDNSPQ_BT_CLOSE"]
["RO1二段浓水排气阀手动开","ns=6;s=V_1ROEDNSPQ_BT_OPEN"]
["RO1二段浓水排气阀故障复位","ns=6;s=V_1ROEDNSPQ_BT_RESET"]
["RO1二段浓水排气阀关到位","ns=6;s=V_1ROEDNSPQ_CFB"]
["RO1二段浓水排气阀关闭中","ns=6;s=V_1ROEDNSPQ_CING"]
["RO1二段浓水排气阀自动关闭","ns=6;s=V_1ROEDNSPQ_CLOSE"]
["RO1二段浓水排气阀故障","ns=6;s=V_1ROEDNSPQ_ERR"]
["RO1二段浓水排气阀总故障","ns=6;s=V_1ROEDNSPQ_ERRT"]
["RO1二段浓水排气阀开到位","ns=6;s=V_1ROEDNSPQ_OFB"]
["RO1二段浓水排气阀打开中","ns=6;s=V_1ROEDNSPQ_OING"]
["RO1二段浓水排气阀自动打开","ns=6;s=V_1ROEDNSPQ_OPENA"]
["RO1二段浓水排气阀关闭","ns=6;s=V_1ROEDNSPQ_OUT_C"]
["RO1二段浓水排气阀打开","ns=6;s=V_1ROEDNSPQ_OUT_O"]
["RO1二段浓水排气阀准备好","ns=6;s=V_1ROEDNSPQ_READY"]
["RO1二段浓水排气阀远程","ns=6;s=V_1ROEDNSPQ_REM"]
["RO1三段产水排气阀手自动","ns=6;s=V_1ROSDCSPQ_BT_AUTO"]
["RO1三段产水排气阀手动关","ns=6;s=V_1ROSDCSPQ_BT_CLOSE"]
["RO1三段产水排气阀手动开","ns=6;s=V_1ROSDCSPQ_BT_OPEN"]
["RO1三段产水排气阀故障复位","ns=6;s=V_1ROSDCSPQ_BT_RESET"]
["RO1三段产水排气阀关到位","ns=6;s=V_1ROSDCSPQ_CFB"]
["RO1三段产水排气阀关闭中","ns=6;s=V_1ROSDCSPQ_CING"]
["RO1三段产水排气阀自动关闭","ns=6;s=V_1ROSDCSPQ_CLOSEA"]
["RO1三段产水排气阀故障","ns=6;s=V_1ROSDCSPQ_ERR"]
["RO1三段产水排气阀总故障","ns=6;s=V_1ROSDCSPQ_ERRT"]
["RO1三段产水排气阀开到位","ns=6;s=V_1ROSDCSPQ_OFB"]
["RO1三段产水排气阀打开中","ns=6;s=V_1ROSDCSPQ_OING"]
["RO1三段产水排气阀自动打开","ns=6;s=V_1ROSDCSPQ_OPENA"]
["RO1三段产水排气阀关闭","ns=6;s=V_1ROSDCSPQ_OUT_C"]
["RO1三段产水排气阀打开","ns=6;s=V_1ROSDCSPQ_OUT_O"]
["RO1三段产水排气阀准备好","ns=6;s=V_1ROSDCSPQ_READY"]
["RO1三段产水排气阀远程","ns=6;s=V_1ROSDCSPQ_REM"]
["RO1三段冲洗排水阀手自动","ns=6;s=V_1ROSDCXPS_BT_AUTO"]
["RO1三段冲洗排水阀手动关","ns=6;s=V_1ROSDCXPS_BT_CLOSE"]
["RO1三段冲洗排水阀手动开","ns=6;s=V_1ROSDCXPS_BT_OPEN"]
["RO1三段冲洗排水阀故障复位","ns=6;s=V_1ROSDCXPS_BT_RESET"]
["RO1三段冲洗排水阀关到位","ns=6;s=V_1ROSDCXPS_CFB"]
["RO1三段冲洗排水阀关闭中","ns=6;s=V_1ROSDCXPS_CING"]
["RO1三段冲洗排水阀自动关闭","ns=6;s=V_1ROSDCXPS_CLOSEA"]
["RO1三段冲洗排水阀故障","ns=6;s=V_1ROSDCXPS_ERR"]
["RO1三段冲洗排水阀总故障","ns=6;s=V_1ROSDCXPS_ERRT"]
["RO1三段冲洗排水阀开到位","ns=6;s=V_1ROSDCXPS_OFB"]
["RO1三段冲洗排水阀打开中","ns=6;s=V_1ROSDCXPS_OING"]
["RO1三段冲洗排水阀自动打开","ns=6;s=V_1ROSDCXPS_OPENA"]
["RO1三段冲洗排水阀关闭","ns=6;s=V_1ROSDCXPS_OUT_C"]
["RO1三段冲洗排水阀打开","ns=6;s=V_1ROSDCXPS_OUT_O"]
["RO1三段冲洗排水阀准备好","ns=6;s=V_1ROSDCXPS_READY"]
["RO1三段冲洗排水阀远程","ns=6;s=V_1ROSDCXPS_REM"]
["RO1三段进水排气阀手自动","ns=6;s=V_1ROSDJSPQ_BT_AUTO"]
["RO1三段进水排气阀手动关","ns=6;s=V_1ROSDJSPQ_BT_CLOSE"]
["RO1三段进水排气阀手动开","ns=6;s=V_1ROSDJSPQ_BT_OPEN"]
["RO1三段进水排气阀故障复位","ns=6;s=V_1ROSDJSPQ_BT_RESET"]
["RO1三段进水排气阀关到位","ns=6;s=V_1ROSDJSPQ_CFB"]
["RO1三段进水排气阀关闭中","ns=6;s=V_1ROSDJSPQ_CING"]
["RO1三段进水排气阀自动关闭","ns=6;s=V_1ROSDJSPQ_CLOSEA"]
["RO1三段进水排气阀故障","ns=6;s=V_1ROSDJSPQ_ERR"]
["RO1三段进水排气阀总故障","ns=6;s=V_1ROSDJSPQ_ERRT"]
["RO1三段进水排气阀开到位","ns=6;s=V_1ROSDJSPQ_OFB"]
["RO1三段进水排气阀打开中","ns=6;s=V_1ROSDJSPQ_OING"]
["RO1三段进水排气阀自动打开","ns=6;s=V_1ROSDJSPQ_OPENA"]
["RO1三段进水排气阀关闭","ns=6;s=V_1ROSDJSPQ_OUT_C"]
["RO1三段进水排气阀打开","ns=6;s=V_1ROSDJSPQ_OUT_O"]
["RO1三段进水排气阀准备好","ns=6;s=V_1ROSDJSPQ_READY"]
["RO1三段进水排气阀远程","ns=6;s=V_1ROSDJSPQ_REM"]
["RO1三段浓水排气阀手自动","ns=6;s=V_1ROSDNSPQ_BT_AUTO"]
["RO1三段浓水排气阀手动关","ns=6;s=V_1ROSDNSPQ_BT_CLOSE"]
["RO1三段浓水排气阀手动开","ns=6;s=V_1ROSDNSPQ_BT_OPEN"]
["RO1三段浓水排气阀故障复位","ns=6;s=V_1ROSDNSPQ_BT_RESET"]
["RO1三段浓水排气阀关到位","ns=6;s=V_1ROSDNSPQ_CFB"]
["RO1三段浓水排气阀关闭中","ns=6;s=V_1ROSDNSPQ_CING"]
["RO1三段浓水排气阀自动关闭","ns=6;s=V_1ROSDNSPQ_CLOSEA"]
["RO1三段浓水排气阀故障","ns=6;s=V_1ROSDNSPQ_ERR"]
["RO1三段浓水排气阀总故障","ns=6;s=V_1ROSDNSPQ_ERRT"]
["RO1三段浓水排气阀开到位","ns=6;s=V_1ROSDNSPQ_OFB"]
["RO1三段浓水排气阀打开中","ns=6;s=V_1ROSDNSPQ_OING"]
["RO1三段浓水排气阀自动打开","ns=6;s=V_1ROSDNSPQ_OPENA"]
["RO1三段浓水排气阀关闭","ns=6;s=V_1ROSDNSPQ_OUT_C"]
["RO1三段浓水排气阀打开","ns=6;s=V_1ROSDNSPQ_OUT_O"]
["RO1三段浓水排气阀准备好","ns=6;s=V_1ROSDNSPQ_READY"]
["RO1三段浓水排气阀远程","ns=6;s=V_1ROSDNSPQ_REM"]
["RO1一段冲洗进水阀手自动","ns=6;s=V_1ROYDBWJS_BT_AUTO"]
["RO1一段冲洗进水阀手动关","ns=6;s=V_1ROYDBWJS_BT_CLOSE"]
["RO1一段冲洗进水阀手动开","ns=6;s=V_1ROYDBWJS_BT_OPEN"]
["RO1一段冲洗进水阀故障复位","ns=6;s=V_1ROYDBWJS_BT_RESET"]
["RO1一段冲洗进水阀关到位","ns=6;s=V_1ROYDBWJS_CFB"]
["RO1一段冲洗进水阀关闭中","ns=6;s=V_1ROYDBWJS_CING"]
["RO1一段冲洗进水阀自动关闭","ns=6;s=V_1ROYDBWJS_CLOSEA"]
["RO1一段冲洗进水阀故障","ns=6;s=V_1ROYDBWJS_ERR"]
["RO1一段冲洗进水阀总故障","ns=6;s=V_1ROYDBWJS_ERRT"]
["RO1一段冲洗进水阀开到位","ns=6;s=V_1ROYDBWJS_OFB"]
["RO1一段冲洗进水阀打开中","ns=6;s=V_1ROYDBWJS_OING"]
["RO1一段冲洗进水阀自动打开","ns=6;s=V_1ROYDBWJS_OPENA"]
["RO1一段冲洗进水阀关闭","ns=6;s=V_1ROYDBWJS_OUT_C"]
["RO1一段冲洗进水阀打开","ns=6;s=V_1ROYDBWJS_OUT_O"]
["RO1一段冲洗进水阀准备好","ns=6;s=V_1ROYDBWJS_READY"]
["RO1一段冲洗进水阀远程","ns=6;s=V_1ROYDBWJS_REM"]
["RO1一段冲洗排水阀手自动","ns=6;s=V_1ROYDBWPS_BT_AUTO"]
["RO1一段冲洗排水阀手动关","ns=6;s=V_1ROYDBWPS_BT_CLOSE"]
["RO1一段冲洗排水阀手动开","ns=6;s=V_1ROYDBWPS_BT_OPEN"]
["RO1一段冲洗排水阀故障复位","ns=6;s=V_1ROYDBWPS_BT_RESET"]
["RO1一段冲洗排水阀关到位","ns=6;s=V_1ROYDBWPS_CFB"]
["RO1一段冲洗排水阀关闭中","ns=6;s=V_1ROYDBWPS_CING"]
["RO1一段冲洗排水阀自动关闭","ns=6;s=V_1ROYDBWPS_CLOSEA"]
["RO1一段冲洗排水阀故障","ns=6;s=V_1ROYDBWPS_ERR"]
["RO1一段冲洗排水阀总故障","ns=6;s=V_1ROYDBWPS_ERRT"]
["RO1一段冲洗排水阀开到位","ns=6;s=V_1ROYDBWPS_OFB"]
["RO1一段冲洗排水阀打开中","ns=6;s=V_1ROYDBWPS_OING"]
["RO1一段冲洗排水阀自动打开","ns=6;s=V_1ROYDBWPS_OPENA"]
["RO1一段冲洗排水阀关闭","ns=6;s=V_1ROYDBWPS_OUT_C"]
["RO1一段冲洗排水阀打开","ns=6;s=V_1ROYDBWPS_OUT_O"]
["RO1一段冲洗排水阀准备好","ns=6;s=V_1ROYDBWPS_READY"]
["RO1一段冲洗排水阀远程","ns=6;s=V_1ROYDBWPS_REM"]
["RO1一段产水排气阀1手自动","ns=6;s=V_1ROYDCSP1_BT_AUTO"]
["RO1一段产水排气阀1手动关","ns=6;s=V_1ROYDCSP1_BT_CLOSE"]
["RO1一段产水排气阀1手动开","ns=6;s=V_1ROYDCSP1_BT_OPEN"]
["RO1一段产水排气阀1故障复位","ns=6;s=V_1ROYDCSP1_BT_RESET"]
["RO1一段产水排气阀1关到位","ns=6;s=V_1ROYDCSP1_CFB"]
["RO1一段产水排气阀1关闭中","ns=6;s=V_1ROYDCSP1_CING"]
["RO1一段产水排气阀1自动关闭","ns=6;s=V_1ROYDCSP1_CLOSA"]
["RO1一段产水排气阀1故障","ns=6;s=V_1ROYDCSP1_ERR"]
["RO1一段产水排气阀1总故障","ns=6;s=V_1ROYDCSP1_ERRT"]
["RO1一段产水排气阀1开到位","ns=6;s=V_1ROYDCSP1_OFB"]
["RO1一段产水排气阀1打开中","ns=6;s=V_1ROYDCSP1_OING"]
["RO1一段产水排气阀1自动打开","ns=6;s=V_1ROYDCSP1_OPEN"]
["RO1一段产水排气阀1关闭","ns=6;s=V_1ROYDCSP1_OUT_CL"]
["RO1一段产水排气阀1打开","ns=6;s=V_1ROYDCSP1_OUT_OP"]
["RO1一段产水排气阀1准备好","ns=6;s=V_1ROYDCSP1_READ"]
["RO1一段产水排气阀1远程","ns=6;s=V_1ROYDCSP1_REM"]
["RO1一段产水排气阀2手自动","ns=6;s=V_1ROYDCSP2_BT_AUTO"]
["RO1一段产水排气阀2手动关","ns=6;s=V_1ROYDCSP2_BT_CLOSE"]
["RO1一段产水排气阀2手动开","ns=6;s=V_1ROYDCSP2_BT_OPEN"]
["RO1一段产水排气阀2故障复位","ns=6;s=V_1ROYDCSP2_BT_RESET"]
["RO1一段产水排气阀2关到位","ns=6;s=V_1ROYDCSP2_CFB"]
["RO1一段产水排气阀2关闭中","ns=6;s=V_1ROYDCSP2_CING"]
["RO1一段产水排气阀2自动关闭","ns=6;s=V_1ROYDCSP2_CLOS"]
["RO1一段产水排气阀2故障","ns=6;s=V_1ROYDCSP2_ERR"]
["RO1一段产水排气阀2总故障","ns=6;s=V_1ROYDCSP2_ERRT"]
["RO1一段产水排气阀2开到位","ns=6;s=V_1ROYDCSP2_OFB"]
["RO1一段产水排气阀2打开中","ns=6;s=V_1ROYDCSP2_OING"]
["RO1一段产水排气阀2自动打开","ns=6;s=V_1ROYDCSP2_OPEN"]
["RO1一段产水排气阀2关闭","ns=6;s=V_1ROYDCSP2_OUTC"]
["RO1一段产水排气阀2打开","ns=6;s=V_1ROYDCSP2_OUTO"]
["RO1一段产水排气阀2准备好","ns=6;s=V_1ROYDCSP2_READY"]
["RO1一段产水排气阀2远程","ns=6;s=V_1ROYDCSP2_REM"]
["RO1一段超越旁路阀手自动","ns=6;s=V_1ROYDCYPL_BT_AUTO"]
["RO1一段超越旁路阀手动关","ns=6;s=V_1ROYDCYPL_BT_CLOSE"]
["RO1一段超越旁路阀手动开","ns=6;s=V_1ROYDCYPL_BT_OPEN"]
["RO1一段超越旁路阀故障复位","ns=6;s=V_1ROYDCYPL_BT_RESET"]
["RO1一段超越旁路阀关到位","ns=6;s=V_1ROYDCYPL_CFB"]
["RO1一段超越旁路阀关闭中","ns=6;s=V_1ROYDCYPL_CING"]
["RO1一段超越旁路阀自动关闭","ns=6;s=V_1ROYDCYPL_CLOSEA"]
["RO1一段超越旁路阀故障","ns=6;s=V_1ROYDCYPL_ERR"]
["RO1一段超越旁路阀总故障","ns=6;s=V_1ROYDCYPL_ERRT"]
["RO1一段超越旁路阀开到位","ns=6;s=V_1ROYDCYPL_OFB"]
["RO1一段超越旁路阀打开中","ns=6;s=V_1ROYDCYPL_OING"]
["RO1一段超越旁路阀自动打开","ns=6;s=V_1ROYDCYPL_OPENA"]
["RO1一段超越旁路阀关闭","ns=6;s=V_1ROYDCYPL_OUTC"]
["RO1一段超越旁路阀打开","ns=6;s=V_1ROYDCYPL_OUTO"]
["RO1一段超越旁路阀准备好","ns=6;s=V_1ROYDCYPL_READY"]
["RO1一段超越旁路阀远程","ns=6;s=V_1ROYDCYPL_REM"]
["RO1一段进水排气阀1手自动","ns=6;s=V_1ROYDJSP1_BT_AUTO"]
["RO1一段进水排气阀1手动关","ns=6;s=V_1ROYDJSP1_BT_CLOSE"]
["RO1一段进水排气阀1手动开","ns=6;s=V_1ROYDJSP1_BT_OPEN"]
["RO1一段进水排气阀1故障复位","ns=6;s=V_1ROYDJSP1_BT_RESET"]
["RO1一段进水排气阀1关到位","ns=6;s=V_1ROYDJSP1_CFB"]
["RO1一段进水排气阀1关闭中","ns=6;s=V_1ROYDJSP1_CING"]
["RO1一段进水排气阀1自动关闭","ns=6;s=V_1ROYDJSP1_CLOS"]
["RO1一段进水排气阀1故障","ns=6;s=V_1ROYDJSP1_ERR"]
["RO1一段进水排气阀1总故障","ns=6;s=V_1ROYDJSP1_ERRT"]
["RO1一段进水排气阀1开到位","ns=6;s=V_1ROYDJSP1_OFB"]
["RO1一段进水排气阀1打开中","ns=6;s=V_1ROYDJSP1_OING"]
["RO1一段进水排气阀1自动打开","ns=6;s=V_1ROYDJSP1_OPEN"]
["RO1一段进水排气阀1关闭","ns=6;s=V_1ROYDJSP1_OUTC"]
["RO1一段进水排气阀1打开","ns=6;s=V_1ROYDJSP1_OUTO"]
["RO1一段进水排气阀1准备好","ns=6;s=V_1ROYDJSP1_READY"]
["RO1一段进水排气阀1远程","ns=6;s=V_1ROYDJSP1_REM"]
["RO1一段进水排气阀2手自动","ns=6;s=V_1ROYDJSP2_BT_AUTO"]
["RO1一段进水排气阀2手动关","ns=6;s=V_1ROYDJSP2_BT_CLOSE"]
["RO1一段进水排气阀2手动开","ns=6;s=V_1ROYDJSP2_BT_OPEN"]
["RO1一段进水排气阀2故障复位","ns=6;s=V_1ROYDJSP2_BT_RESET"]
["RO1一段进水排气阀2关到位","ns=6;s=V_1ROYDJSP2_CFB"]
["RO1一段进水排气阀2关闭中","ns=6;s=V_1ROYDJSP2_CING"]
["RO1一段进水排气阀2自动关闭","ns=6;s=V_1ROYDJSP2_CLOSEA"]
["RO1一段进水排气阀2故障","ns=6;s=V_1ROYDJSP2_ERR"]
["RO1一段进水排气阀2总故障","ns=6;s=V_1ROYDJSP2_ERRT"]
["RO1一段进水排气阀2开到位","ns=6;s=V_1ROYDJSP2_OFB"]
["RO1一段进水排气阀2打开中","ns=6;s=V_1ROYDJSP2_OING"]
["RO1一段进水排气阀2自动打开","ns=6;s=V_1ROYDJSP2_OPENA"]
["RO1一段进水排气阀2关闭","ns=6;s=V_1ROYDJSP2_OUTC"]
["RO1一段进水排气阀2打开","ns=6;s=V_1ROYDJSP2_OUTO"]
["RO1一段进水排气阀2准备好","ns=6;s=V_1ROYDJSP2_READY"]
["RO1一段进水排气阀2远程","ns=6;s=V_1ROYDJSP2_REM"]
["RO1一段浓水排气阀1手自动","ns=6;s=V_1ROYDNSP1_BT_AUTO"]
["RO1一段浓水排气阀1手动关","ns=6;s=V_1ROYDNSP1_BT_CLOSE"]
["RO1一段浓水排气阀1手动开","ns=6;s=V_1ROYDNSP1_BT_OPEN"]
["RO1一段浓水排气阀1故障复位","ns=6;s=V_1ROYDNSP1_BT_RESET"]
["RO1一段浓水排气阀1关到位","ns=6;s=V_1ROYDNSP1_CFB"]
["RO1一段浓水排气阀1关闭中","ns=6;s=V_1ROYDNSP1_CING"]
["RO1一段浓水排气阀1自动关闭","ns=6;s=V_1ROYDNSP1_CLOS"]
["RO1一段浓水排气阀1故障","ns=6;s=V_1ROYDNSP1_ERR"]
["RO1一段浓水排气阀1总故障","ns=6;s=V_1ROYDNSP1_ERRT"]
["RO1一段浓水排气阀1开到位","ns=6;s=V_1ROYDNSP1_OFB"]
["RO1一段浓水排气阀1打开中","ns=6;s=V_1ROYDNSP1_OING"]
["RO1一段浓水排气阀1自动打开","ns=6;s=V_1ROYDNSP1_OPEN"]
["RO1一段浓水排气阀1关闭","ns=6;s=V_1ROYDNSP1_OUTC"]
["RO1一段浓水排气阀1打开","ns=6;s=V_1ROYDNSP1_OUTO"]
["RO1一段浓水排气阀1准备好","ns=6;s=V_1ROYDNSP1_READ"]
["RO1一段浓水排气阀1远程","ns=6;s=V_1ROYDNSP1_REM"]
["RO1一段浓水排气阀2手自动","ns=6;s=V_1ROYDNSP2_BT_AUTO"]
["RO1一段浓水排气阀2手动关","ns=6;s=V_1ROYDNSP2_BT_CLOSE"]
["RO1一段浓水排气阀2手动开","ns=6;s=V_1ROYDNSP2_BT_OPEN"]
["RO1一段浓水排气阀2故障复位","ns=6;s=V_1ROYDNSP2_BT_RESET"]
["RO1一段浓水排气阀2关到位","ns=6;s=V_1ROYDNSP2_CFB"]
["RO1一段浓水排气阀2关闭中","ns=6;s=V_1ROYDNSP2_CING"]
["RO1一段浓水排气阀2自动关闭","ns=6;s=V_1ROYDNSP2_CLOSEA"]
["RO1一段浓水排气阀2故障","ns=6;s=V_1ROYDNSP2_ERR"]
["RO1一段浓水排气阀2总故障","ns=6;s=V_1ROYDNSP2_ERRT"]
["RO1一段浓水排气阀2开到位","ns=6;s=V_1ROYDNSP2_OFB"]
["RO1一段浓水排气阀2打开中","ns=6;s=V_1ROYDNSP2_OING"]
["RO1一段浓水排气阀2自动打开","ns=6;s=V_1ROYDNSP2_OPEN"]
["RO1一段浓水排气阀2关闭","ns=6;s=V_1ROYDNSP2_OUTC"]
["RO1一段浓水排气阀2打开","ns=6;s=V_1ROYDNSP2_OUTO"]
["RO1一段浓水排气阀2准备好","ns=6;s=V_1ROYDNSP2_READY"]
["RO1一段浓水排气阀2远程","ns=6;s=V_1ROYDNSP2_REM"]
["RO1一段隔离阀手自动","ns=6;s=V_1ROYDQXGL_BT_AUTO"]
["RO1一段隔离阀手动关","ns=6;s=V_1ROYDQXGL_BT_CLOSE"]
["RO1一段隔离阀手动开","ns=6;s=V_1ROYDQXGL_BT_OPEN"]
["RO1一段隔离阀故障复位","ns=6;s=V_1ROYDQXGL_BT_RESET"]
["RO1一段隔离阀关到位","ns=6;s=V_1ROYDQXGL_CFB"]
["RO1一段隔离阀关闭中","ns=6;s=V_1ROYDQXGL_CING"]
["RO1一段隔离阀自动关闭","ns=6;s=V_1ROYDQXGL_CLOSEA"]
["RO1一段隔离阀故障","ns=6;s=V_1ROYDQXGL_ERR"]
["RO1一段隔离阀总故障","ns=6;s=V_1ROYDQXGL_ERRT"]
["RO1一段隔离阀开到位","ns=6;s=V_1ROYDQXGL_OFB"]
["RO1一段隔离阀打开中","ns=6;s=V_1ROYDQXGL_OING"]
["RO1一段隔离阀自动打开","ns=6;s=V_1ROYDQXGL_OPENA"]
["RO1一段隔离阀关闭","ns=6;s=V_1ROYDQXGL_OUT_C"]
["RO1一段隔离阀打开","ns=6;s=V_1ROYDQXGL_OUT_O"]
["RO1一段隔离阀准备好","ns=6;s=V_1ROYDQXGL_READY"]
["RO1一段隔离阀远程","ns=6;s=V_1ROYDQXGL_REM"]
["UF2反洗进水阀手自动","ns=6;s=V_2#UF_BWJS_BT_AUTO"]
["UF2反洗进水阀手动关","ns=6;s=V_2#UF_BWJS_BT_CLOSE"]
["UF2反洗进水阀手动开","ns=6;s=V_2#UF_BWJS_BT_OPEN"]
["UF2反洗进水阀故障复位","ns=6;s=V_2#UF_BWJS_BT_RESET"]
["UF2反洗进水阀关到位","ns=6;s=V_2#UF_BWJS_CFB"]
["UF2反洗进水阀关闭中","ns=6;s=V_2#UF_BWJS_CING"]
["UF2反洗进水阀自动关闭","ns=6;s=V_2#UF_BWJS_CLOSEAUT"]
["UF2反洗进水阀故障","ns=6;s=V_2#UF_BWJS_ERR"]
["UF2反洗进水阀总故障","ns=6;s=V_2#UF_BWJS_ERRT"]
["UF2反洗进水阀开到位","ns=6;s=V_2#UF_BWJS_OFB"]
["UF2反洗进水阀打开中","ns=6;s=V_2#UF_BWJS_OING"]
["UF2反洗进水阀自动打开","ns=6;s=V_2#UF_BWJS_OPENAUTO"]
["UF2反洗进水阀关闭","ns=6;s=V_2#UF_BWJS_OUT_CLOS"]
["UF2反洗进水阀打开","ns=6;s=V_2#UF_BWJS_OUT_OPEN"]
["UF2反洗进水阀准备好","ns=6;s=V_2#UF_BWJS_READY"]
["UF2反洗进水阀远程","ns=6;s=V_2#UF_BWJS_REM"]
["UF2反洗排水阀手自动","ns=6;s=V_2#UF_BWPS_BT_AUTO"]
["UF2反洗排水阀手动关","ns=6;s=V_2#UF_BWPS_BT_CLOSE"]
["UF2反洗排水阀手动开","ns=6;s=V_2#UF_BWPS_BT_OPEN"]
["UF2反洗排水阀故障复位","ns=6;s=V_2#UF_BWPS_BT_RESET"]
["UF2反洗排水阀关到位","ns=6;s=V_2#UF_BWPS_CFB"]
["UF2反洗排水阀关闭中","ns=6;s=V_2#UF_BWPS_CING"]
["UF2反洗排水阀自动关闭","ns=6;s=V_2#UF_BWPS_CLOSEAUT"]
["UF2反洗排水阀故障","ns=6;s=V_2#UF_BWPS_ERR"]
["UF2反洗排水阀总故障","ns=6;s=V_2#UF_BWPS_ERRT"]
["UF2反洗排水阀开到位","ns=6;s=V_2#UF_BWPS_OFB"]
["UF2反洗排水阀打开中","ns=6;s=V_2#UF_BWPS_OING"]
["UF2反洗排水阀自动打开","ns=6;s=V_2#UF_BWPS_OPENAUTO"]
["UF2反洗排水阀关闭","ns=6;s=V_2#UF_BWPS_OUT_CLOS"]
["UF2反洗排水阀打开","ns=6;s=V_2#UF_BWPS_OUT_OPEN"]
["UF2反洗排水阀准备好","ns=6;s=V_2#UF_BWPS_READY"]
["UF2反洗排水阀远程","ns=6;s=V_2#UF_BWPS_REM"]
["UF2产水阀手自动","ns=6;s=V_2#UF_CS_BT_AUTO"]
["UF2产水阀手动关","ns=6;s=V_2#UF_CS_BT_CLOSE"]
["UF2产水阀手动开","ns=6;s=V_2#UF_CS_BT_OPEN"]
["UF2产水阀故障复位","ns=6;s=V_2#UF_CS_BT_RESET"]
["UF2产水阀关到位","ns=6;s=V_2#UF_CS_CFB"]
["UF2产水阀关闭中","ns=6;s=V_2#UF_CS_CING"]
["UF2产水阀自动关闭","ns=6;s=V_2#UF_CS_CLOSEAUTO"]
["UF2产水阀故障","ns=6;s=V_2#UF_CS_ERR"]
["UF2产水阀总故障","ns=6;s=V_2#UF_CS_ERRT"]
["UF2产水阀开到位","ns=6;s=V_2#UF_CS_OFB"]
["UF2产水阀打开中","ns=6;s=V_2#UF_CS_OING"]
["UF2产水阀自动打开","ns=6;s=V_2#UF_CS_OPENAUTO"]
["UF2产水阀关闭","ns=6;s=V_2#UF_CS_OUT_CLOSE"]
["UF2产水阀打开","ns=6;s=V_2#UF_CS_OUT_OPEN"]
["UF2产水阀准备好","ns=6;s=V_2#UF_CS_READY"]
["UF2产水阀远程","ns=6;s=V_2#UF_CS_REM"]
["UF2排气阀1手自动","ns=6;s=V_2#UF_PQ1_BT_AUTO"]
["UF2排气阀1手动关","ns=6;s=V_2#UF_PQ1_BT_CLOSE"]
["UF2排气阀1手动开","ns=6;s=V_2#UF_PQ1_BT_OPEN"]
["UF2排气阀1故障复位","ns=6;s=V_2#UF_PQ1_BT_RESET"]
["UF2排气阀1关到位","ns=6;s=V_2#UF_PQ1_CFB"]
["UF2排气阀1关闭中","ns=6;s=V_2#UF_PQ1_CING"]
["UF2排气阀1自动关闭","ns=6;s=V_2#UF_PQ1_CLOSEAUTO"]
["UF2排气阀1故障","ns=6;s=V_2#UF_PQ1_ERR"]
["UF2排气阀1总故障","ns=6;s=V_2#UF_PQ1_ERRT"]
["UF2排气阀1开到位","ns=6;s=V_2#UF_PQ1_OFB"]
["UF2排气阀1打开中","ns=6;s=V_2#UF_PQ1_OING"]
["UF2排气阀1自动打开","ns=6;s=V_2#UF_PQ1_OPENAUTO"]
["UF2排气阀1关闭","ns=6;s=V_2#UF_PQ1_OUT_CLOSE"]
["UF2排气阀1打开","ns=6;s=V_2#UF_PQ1_OUT_OPEN"]
["UF2排气阀1准备好","ns=6;s=V_2#UF_PQ1_READY"]
["UF2排气阀1远程","ns=6;s=V_2#UF_PQ1_REM"]
["UF2排气阀2手自动","ns=6;s=V_2#UF_PQ2_BT_AUTO"]
["UF2排气阀2手动关","ns=6;s=V_2#UF_PQ2_BT_CLOSE"]
["UF2排气阀2手动开","ns=6;s=V_2#UF_PQ2_BT_OPEN"]
["UF2排气阀2故障复位","ns=6;s=V_2#UF_PQ2_BT_RESET"]
["UF2排气阀2关到位","ns=6;s=V_2#UF_PQ2_CFB"]
["UF2排气阀2关闭中","ns=6;s=V_2#UF_PQ2_CING"]
["UF2排气阀2自动关闭","ns=6;s=V_2#UF_PQ2_CLOSEAUTO"]
["UF2排气阀2故障","ns=6;s=V_2#UF_PQ2_ERR"]
["UF2排气阀2总故障","ns=6;s=V_2#UF_PQ2_ERRT"]
["UF2排气阀2开到位","ns=6;s=V_2#UF_PQ2_OFB"]
["UF2排气阀2打开中","ns=6;s=V_2#UF_PQ2_OING"]
["UF2排气阀2自动打开","ns=6;s=V_2#UF_PQ2_OPENAUTO"]
["UF2排气阀2关闭","ns=6;s=V_2#UF_PQ2_OUT_CLOSE"]
["UF2排气阀2打开","ns=6;s=V_2#UF_PQ2_OUT_OPEN"]
["UF2排气阀2准备好","ns=6;s=V_2#UF_PQ2_READY"]
["UF2排气阀2远程","ns=6;s=V_2#UF_PQ2_REM"]
["UF2排气阀3手自动","ns=6;s=V_2#UF_PQ3_BT_AUTO"]
["UF2排气阀3手动关","ns=6;s=V_2#UF_PQ3_BT_CLOSE"]
["UF2排气阀3手动开","ns=6;s=V_2#UF_PQ3_BT_OPEN"]
["UF2排气阀3故障复位","ns=6;s=V_2#UF_PQ3_BT_RESET"]
["UF2排气阀3关到位","ns=6;s=V_2#UF_PQ3_CFB"]
["UF2排气阀3关闭中","ns=6;s=V_2#UF_PQ3_CING"]
["UF2排气阀3自动关闭","ns=6;s=V_2#UF_PQ3_CLOSEAUTO"]
["UF2排气阀3故障","ns=6;s=V_2#UF_PQ3_ERR"]
["UF2排气阀3总故障","ns=6;s=V_2#UF_PQ3_ERRT"]
["UF2排气阀3开到位","ns=6;s=V_2#UF_PQ3_OFB"]
["UF2排气阀3打开中","ns=6;s=V_2#UF_PQ3_OING"]
["UF2排气阀3自动打开","ns=6;s=V_2#UF_PQ3_OPENAUTO"]
["UF2排气阀3关闭","ns=6;s=V_2#UF_PQ3_OUT_CLOSE"]
["UF2排气阀3打开","ns=6;s=V_2#UF_PQ3_OUT_OPEN"]
["UF2排气阀3准备好","ns=6;s=V_2#UF_PQ3_READY"]
["UF2排气阀3远程","ns=6;s=V_2#UF_PQ3_REM"]
["UF2排气阀4手自动","ns=6;s=V_2#UF_PQ4_BT_AUTO"]
["UF2排气阀4手动关","ns=6;s=V_2#UF_PQ4_BT_CLOSE"]
["UF2排气阀4手动开","ns=6;s=V_2#UF_PQ4_BT_OPEN"]
["UF2排气阀4故障复位","ns=6;s=V_2#UF_PQ4_BT_RESET"]
["UF2排气阀4关到位","ns=6;s=V_2#UF_PQ4_CFB"]
["UF2排气阀4关闭中","ns=6;s=V_2#UF_PQ4_CING"]
["UF2排气阀4自动关闭","ns=6;s=V_2#UF_PQ4_CLOSEAUTO"]
["UF2排气阀4故障","ns=6;s=V_2#UF_PQ4_ERR"]
["UF2排气阀4总故障","ns=6;s=V_2#UF_PQ4_ERRT"]
["UF2排气阀4开到位","ns=6;s=V_2#UF_PQ4_OFB"]
["UF2排气阀4打开中","ns=6;s=V_2#UF_PQ4_OING"]
["UF2排气阀4自动打开","ns=6;s=V_2#UF_PQ4_OPENAUTO"]
["UF2排气阀4关闭","ns=6;s=V_2#UF_PQ4_OUT_CLOSE"]
["UF2排气阀4打开","ns=6;s=V_2#UF_PQ4_OUT_OPEN"]
["UF2排气阀4准备好","ns=6;s=V_2#UF_PQ4_READY"]
["UF2排气阀4远程","ns=6;s=V_2#UF_PQ4_REM"]
["UF2隔断阀手自动","ns=6;s=V_2#UFCIPGL_BT_AUTO"]
["UF2隔断阀手动关","ns=6;s=V_2#UFCIPGL_BT_CLOSE"]
["UF2隔断阀手动开","ns=6;s=V_2#UFCIPGL_BT_OPEN"]
["UF2隔断阀故障复位","ns=6;s=V_2#UFCIPGL_BT_RESET"]
["UF2隔断阀关到位","ns=6;s=V_2#UFCIPGL_CFB"]
["UF2隔断阀关闭中","ns=6;s=V_2#UFCIPGL_CING"]
["UF2隔断阀自动关闭","ns=6;s=V_2#UFCIPGL_CLOSEA"]
["UF2隔断阀故障","ns=6;s=V_2#UFCIPGL_ERR"]
["UF2隔断阀总故障","ns=6;s=V_2#UFCIPGL_ERRT"]
["UF2隔断阀开到位","ns=6;s=V_2#UFCIPGL_OFB"]
["UF2隔断阀打开中","ns=6;s=V_2#UFCIPGL_OING"]
["UF2隔断阀自动打开","ns=6;s=V_2#UFCIPGL_OPENAU"]
["UF2隔断阀关闭","ns=6;s=V_2#UFCIPGL_OUT_CL"]
["UF2隔断阀打开","ns=6;s=V_2#UFCIPGL_OUT_OP"]
["UF2隔断阀准备好","ns=6;s=V_2#UFCIPGL_READY"]
["UF2隔断阀远程","ns=6;s=V_2#UFCIPGL_REM"]
["RO2不合格阀手自动","ns=6;s=V_2RO_BHG_BT_AUTO"]
["RO2不合格阀手动关","ns=6;s=V_2RO_BHG_BT_CLOSE"]
["RO2不合格阀手动开","ns=6;s=V_2RO_BHG_BT_OPEN"]
["RO2不合格阀故障复位","ns=6;s=V_2RO_BHG_BT_RESET"]
["RO2不合格阀关到位","ns=6;s=V_2RO_BHG_CFB"]
["RO2不合格阀关闭中","ns=6;s=V_2RO_BHG_CING"]
["RO2不合格阀自动关闭","ns=6;s=V_2RO_BHG_CLOSEAUTO"]
["RO2不合格阀故障","ns=6;s=V_2RO_BHG_ERR"]
["RO2不合格阀总故障","ns=6;s=V_2RO_BHG_ERRT"]
["RO2不合格阀开到位","ns=6;s=V_2RO_BHG_OFB"]
["RO2不合格阀打开中","ns=6;s=V_2RO_BHG_OING"]
["RO2不合格阀自动打开","ns=6;s=V_2RO_BHG_OPENAUTO"]
["RO2不合格阀关闭","ns=6;s=V_2RO_BHG_OUT_CLOSE"]
["RO2不合格阀打开","ns=6;s=V_2RO_BHG_OUT_OPEN"]
["RO2不合格阀准备好","ns=6;s=V_2RO_BHG_OUT_READY"]
["RO2不合格阀远程","ns=6;s=V_2RO_BHG_REM"]
["RO2产水阀手自动","ns=6;s=V_2RO_CS_BT_AUTO"]
["RO2产水阀手动关","ns=6;s=V_2RO_CS_BT_CLOSE"]
["RO2产水阀手动开","ns=6;s=V_2RO_CS_BT_OPEN"]
["RO2产水阀故障复位","ns=6;s=V_2RO_CS_BT_RESET"]
["RO2产水阀关到位","ns=6;s=V_2RO_CS_CFB"]
["RO2产水阀关闭中","ns=6;s=V_2RO_CS_CING"]
["RO2产水阀自动关闭","ns=6;s=V_2RO_CS_CLOSEAUTO"]
["RO2产水阀故障","ns=6;s=V_2RO_CS_ERR"]
["RO2产水阀总故障","ns=6;s=V_2RO_CS_ERRT"]
["RO2产水阀开到位","ns=6;s=V_2RO_CS_OFB"]
["RO2产水阀打开中","ns=6;s=V_2RO_CS_OING"]
["RO2产水阀自动打开","ns=6;s=V_2RO_CS_OPENAUTO"]
["RO2产水阀关闭","ns=6;s=V_2RO_CS_OUT_CLOSE"]
["RO2产水阀打开","ns=6;s=V_2RO_CS_OUT_OPEN"]
["RO2产水阀准备好","ns=6;s=V_2RO_CS_OUT_READY"]
["RO2产水阀远程","ns=6;s=V_2RO_CS_REM"]
["RO2进水阀手自动","ns=6;s=V_2RO_JS_BT_AUTO"]
["RO2进水阀手动关","ns=6;s=V_2RO_JS_BT_CLOSE"]
["RO2进水阀手动开","ns=6;s=V_2RO_JS_BT_OPEN"]
["RO2进水阀故障复位","ns=6;s=V_2RO_JS_BT_RESET"]
["RO2进水阀关到位","ns=6;s=V_2RO_JS_CFB"]
["RO2进水阀关闭中","ns=6;s=V_2RO_JS_CING"]
["RO2进水阀自动关闭","ns=6;s=V_2RO_JS_CLOSEAUTO"]
["RO2进水阀故障","ns=6;s=V_2RO_JS_ERR"]
["RO2进水阀总故障","ns=6;s=V_2RO_JS_ERRT"]
["RO2进水阀开到位","ns=6;s=V_2RO_JS_OFB"]
["RO2进水阀打开中","ns=6;s=V_2RO_JS_OING"]
["RO2进水阀自动打开","ns=6;s=V_2RO_JS_OPENAUTO"]
["RO2进水阀关闭","ns=6;s=V_2RO_JS_OUT_CLOSE"]
["RO2进水阀打开","ns=6;s=V_2RO_JS_OUT_OPEN"]
["RO2进水阀准备好","ns=6;s=V_2RO_JS_OUT_READY"]
["RO2进水阀远程","ns=6;s=V_2RO_JS_REM"]
["RO2二段产水排气阀手自动","ns=6;s=V_2ROEDCSPQ_BT_AUTO"]
["RO2二段产水排气阀手动关","ns=6;s=V_2ROEDCSPQ_BT_CLOSE"]
["RO2二段产水排气阀手动开","ns=6;s=V_2ROEDCSPQ_BT_OPEN"]
["RO2二段产水排气阀故障复位","ns=6;s=V_2ROEDCSPQ_BT_RESET"]
["RO2二段产水排气阀关到位","ns=6;s=V_2ROEDCSPQ_CFB"]
["RO2二段产水排气阀关闭中","ns=6;s=V_2ROEDCSPQ_CING"]
["RO2二段产水排气阀自动关闭","ns=6;s=V_2ROEDCSPQ_CLOSEA"]
["RO2二段产水排气阀故障","ns=6;s=V_2ROEDCSPQ_ERR"]
["RO2二段产水排气阀总故障","ns=6;s=V_2ROEDCSPQ_ERRT"]
["RO2二段产水排气阀开到位","ns=6;s=V_2ROEDCSPQ_OFB"]
["RO2二段产水排气阀打开中","ns=6;s=V_2ROEDCSPQ_OING"]
["RO2二段产水排气阀自动打开","ns=6;s=V_2ROEDCSPQ_OPENA"]
["RO2二段产水排气阀关闭","ns=6;s=V_2ROEDCSPQ_OUT_C"]
["RO2二段产水排气阀打开","ns=6;s=V_2ROEDCSPQ_OUT_O"]
["RO2二段产水排气阀准备好","ns=6;s=V_2ROEDCSPQ_READY"]
["RO2二段产水排气阀远程","ns=6;s=V_2ROEDCSPQ_REM"]
["RO2二段进水排气阀手自动","ns=6;s=V_2ROEDJSPQ_BT_AUTO"]
["RO2二段进水排气阀手动关","ns=6;s=V_2ROEDJSPQ_BT_CLOSE"]
["RO2二段进水排气阀手动开","ns=6;s=V_2ROEDJSPQ_BT_OPEN"]
["RO2二段进水排气阀故障复位","ns=6;s=V_2ROEDJSPQ_BT_RESET"]
["RO2二段进水排气阀关到位","ns=6;s=V_2ROEDJSPQ_CFB"]
["RO2二段进水排气阀关闭中","ns=6;s=V_2ROEDJSPQ_CING"]
["RO2二段进水排气阀自动关闭","ns=6;s=V_2ROEDJSPQ_CLOSEA"]
["RO2二段进水排气阀故障","ns=6;s=V_2ROEDJSPQ_ERR"]
["RO2二段进水排气阀总故障","ns=6;s=V_2ROEDJSPQ_ERRT"]
["RO2二段进水排气阀开到位","ns=6;s=V_2ROEDJSPQ_OFB"]
["RO2二段进水排气阀打开中","ns=6;s=V_2ROEDJSPQ_OING"]
["RO2二段进水排气阀自动打开","ns=6;s=V_2ROEDJSPQ_OPENA"]
["RO2二段进水排气阀关闭","ns=6;s=V_2ROEDJSPQ_OUT_C"]
["RO2二段进水排气阀打开","ns=6;s=V_2ROEDJSPQ_OUT_O"]
["RO2二段进水排气阀准备好","ns=6;s=V_2ROEDJSPQ_READY"]
["RO2二段进水排气阀远程","ns=6;s=V_2ROEDJSPQ_REM"]
["RO2二段浓水排气阀手自动","ns=6;s=V_2ROEDNSPQ_BT_AUTO"]
["RO2二段浓水排气阀手动关","ns=6;s=V_2ROEDNSPQ_BT_CLOSE"]
["RO2二段浓水排气阀手动开","ns=6;s=V_2ROEDNSPQ_BT_OPEN"]
["RO2二段浓水排气阀故障复位","ns=6;s=V_2ROEDNSPQ_BT_RESET"]
["RO2二段浓水排气阀关到位","ns=6;s=V_2ROEDNSPQ_CFB"]
["RO2二段浓水排气阀关闭中","ns=6;s=V_2ROEDNSPQ_CING"]
["RO2二段浓水排气阀自动关闭","ns=6;s=V_2ROEDNSPQ_CLOSE"]
["RO2二段浓水排气阀故障","ns=6;s=V_2ROEDNSPQ_ERR"]
["RO2二段浓水排气阀总故障","ns=6;s=V_2ROEDNSPQ_ERRT"]
["RO2二段浓水排气阀开到位","ns=6;s=V_2ROEDNSPQ_OFB"]
["RO2二段浓水排气阀打开中","ns=6;s=V_2ROEDNSPQ_OING"]
["RO2二段浓水排气阀自动打开","ns=6;s=V_2ROEDNSPQ_OPENA"]
["RO2二段浓水排气阀关闭","ns=6;s=V_2ROEDNSPQ_OUT_C"]
["RO2二段浓水排气阀打开","ns=6;s=V_2ROEDNSPQ_OUT_O"]
["RO2二段浓水排气阀准备好","ns=6;s=V_2ROEDNSPQ_READY"]
["RO2二段浓水排气阀远程","ns=6;s=V_2ROEDNSPQ_REM"]
["RO2三段产水排气阀手自动","ns=6;s=V_2ROSDCSPQ_BT_AUTO"]
["RO2三段产水排气阀手动关","ns=6;s=V_2ROSDCSPQ_BT_CLOSE"]
["RO2三段产水排气阀手动开","ns=6;s=V_2ROSDCSPQ_BT_OPEN"]
["RO2三段产水排气阀故障复位","ns=6;s=V_2ROSDCSPQ_BT_RESET"]
["RO2三段产水排气阀关到位","ns=6;s=V_2ROSDCSPQ_CFB"]
["RO2三段产水排气阀关闭中","ns=6;s=V_2ROSDCSPQ_CING"]
["RO2三段产水排气阀自动关闭","ns=6;s=V_2ROSDCSPQ_CLOSE"]
["RO2三段产水排气阀故障","ns=6;s=V_2ROSDCSPQ_ERR"]
["RO2三段产水排气阀总故障","ns=6;s=V_2ROSDCSPQ_ERRT"]
["RO2三段产水排气阀开到位","ns=6;s=V_2ROSDCSPQ_OFB"]
["RO2三段产水排气阀打开中","ns=6;s=V_2ROSDCSPQ_OING"]
["RO2三段产水排气阀自动打开","ns=6;s=V_2ROSDCSPQ_OPENA"]
["RO2三段产水排气阀关闭","ns=6;s=V_2ROSDCSPQ_OUT_C"]
["RO2三段产水排气阀打开","ns=6;s=V_2ROSDCSPQ_OUT_O"]
["RO2三段产水排气阀准备好","ns=6;s=V_2ROSDCSPQ_READY"]
["RO2三段产水排气阀远程","ns=6;s=V_2ROSDCSPQ_REM"]
["RO2三段冲洗排水阀手自动","ns=6;s=V_2ROSDCXPS_BT_AUTO"]
["RO2三段冲洗排水阀手动关","ns=6;s=V_2ROSDCXPS_BT_CLOSE"]
["RO2三段冲洗排水阀手动开","ns=6;s=V_2ROSDCXPS_BT_OPEN"]
["RO2三段冲洗排水阀故障复位","ns=6;s=V_2ROSDCXPS_BT_RESET"]
["RO2三段冲洗排水阀关到位","ns=6;s=V_2ROSDCXPS_CFB"]
["RO2三段冲洗排水阀关闭中","ns=6;s=V_2ROSDCXPS_CING"]
["RO2三段冲洗排水阀自动关闭","ns=6;s=V_2ROSDCXPS_CLOSE"]
["RO2三段冲洗排水阀故障","ns=6;s=V_2ROSDCXPS_ERR"]
["RO2三段冲洗排水阀总故障","ns=6;s=V_2ROSDCXPS_ERRT"]
["RO2三段冲洗排水阀开到位","ns=6;s=V_2ROSDCXPS_OFB"]
["RO2三段冲洗排水阀打开中","ns=6;s=V_2ROSDCXPS_OING"]
["RO2三段冲洗排水阀自动打开","ns=6;s=V_2ROSDCXPS_OPENA"]
["RO2三段冲洗排水阀关闭","ns=6;s=V_2ROSDCXPS_OUT_C"]
["RO2三段冲洗排水阀打开","ns=6;s=V_2ROSDCXPS_OUT_O"]
["RO2三段冲洗排水阀准备好","ns=6;s=V_2ROSDCXPS_READY"]
["RO2三段冲洗排水阀远程","ns=6;s=V_2ROSDCXPS_REM"]
["RO2三段进水排气阀手自动","ns=6;s=V_2ROSDJSPQ_BT_AUTO"]
["RO2三段进水排气阀手动关","ns=6;s=V_2ROSDJSPQ_BT_CLOSE"]
["RO2三段进水排气阀手动开","ns=6;s=V_2ROSDJSPQ_BT_OPEN"]
["RO2三段进水排气阀故障复位","ns=6;s=V_2ROSDJSPQ_BT_RESET"]
["RO2三段进水排气阀关到位","ns=6;s=V_2ROSDJSPQ_CFB"]
["RO2三段进水排气阀关闭中","ns=6;s=V_2ROSDJSPQ_CING"]
["RO2三段进水排气阀自动关闭","ns=6;s=V_2ROSDJSPQ_CLOSE"]
["RO2三段进水排气阀故障","ns=6;s=V_2ROSDJSPQ_ERR"]
["RO2三段进水排气阀总故障","ns=6;s=V_2ROSDJSPQ_ERRT"]
["RO2三段进水排气阀开到位","ns=6;s=V_2ROSDJSPQ_OFB"]
["RO2三段进水排气阀打开中","ns=6;s=V_2ROSDJSPQ_OING"]
["RO2三段进水排气阀自动打开","ns=6;s=V_2ROSDJSPQ_OPENA"]
["RO2三段进水排气阀关闭","ns=6;s=V_2ROSDJSPQ_OUT_C"]
["RO2三段进水排气阀打开","ns=6;s=V_2ROSDJSPQ_OUT_O"]
["RO2三段进水排气阀准备好","ns=6;s=V_2ROSDJSPQ_READY"]
["RO2三段进水排气阀远程","ns=6;s=V_2ROSDJSPQ_REM"]
["RO2三段浓水排气阀手自动","ns=6;s=V_2ROSDNSPQ_BT_AUTO"]
["RO2三段浓水排气阀手动关","ns=6;s=V_2ROSDNSPQ_BT_CLOSE"]
["RO2三段浓水排气阀手动开","ns=6;s=V_2ROSDNSPQ_BT_OPEN"]
["RO2三段浓水排气阀故障复位","ns=6;s=V_2ROSDNSPQ_BT_RESET"]
["RO2三段浓水排气阀关到位","ns=6;s=V_2ROSDNSPQ_CFB"]
["RO2三段浓水排气阀关闭中","ns=6;s=V_2ROSDNSPQ_CING"]
["RO2三段浓水排气阀自动关闭","ns=6;s=V_2ROSDNSPQ_CLOSE"]
["RO2三段浓水排气阀故障","ns=6;s=V_2ROSDNSPQ_ERR"]
["RO2三段浓水排气阀总故障","ns=6;s=V_2ROSDNSPQ_ERRT"]
["RO2三段浓水排气阀开到位","ns=6;s=V_2ROSDNSPQ_OFB"]
["RO2三段浓水排气阀打开中","ns=6;s=V_2ROSDNSPQ_OING"]
["RO2三段浓水排气阀自动打开","ns=6;s=V_2ROSDNSPQ_OPENA"]
["RO2三段浓水排气阀关闭","ns=6;s=V_2ROSDNSPQ_OUT_C"]
["RO2三段浓水排气阀打开","ns=6;s=V_2ROSDNSPQ_OUT_O"]
["RO2三段浓水排气阀准备好","ns=6;s=V_2ROSDNSPQ_READY"]
["RO2三段浓水排气阀远程","ns=6;s=V_2ROSDNSPQ_REM"]
["RO2一段冲洗进水阀手自动","ns=6;s=V_2ROYDBWJS_BT_AUTO"]
["RO2一段冲洗进水阀手动关","ns=6;s=V_2ROYDBWJS_BT_CLOSE"]
["RO2一段冲洗进水阀手动开","ns=6;s=V_2ROYDBWJS_BT_OPEN"]
["RO2一段冲洗进水阀故障复位","ns=6;s=V_2ROYDBWJS_BT_RESET"]
["RO2一段冲洗进水阀关到位","ns=6;s=V_2ROYDBWJS_CFB"]
["RO2一段冲洗进水阀关闭中","ns=6;s=V_2ROYDBWJS_CING"]
["RO2一段冲洗进水阀自动关闭","ns=6;s=V_2ROYDBWJS_CLOSEA"]
["RO2一段冲洗进水阀故障","ns=6;s=V_2ROYDBWJS_ERR"]
["RO2一段冲洗进水阀总故障","ns=6;s=V_2ROYDBWJS_ERRT"]
["RO2一段冲洗进水阀开到位","ns=6;s=V_2ROYDBWJS_OFB"]
["RO2一段冲洗进水阀打开中","ns=6;s=V_2ROYDBWJS_OING"]
["RO2一段冲洗进水阀自动打开","ns=6;s=V_2ROYDBWJS_OPENA"]
["RO2一段冲洗进水阀关闭","ns=6;s=V_2ROYDBWJS_OUT_C"]
["RO2一段冲洗进水阀打开","ns=6;s=V_2ROYDBWJS_OUT_O"]
["RO2一段冲洗进水阀准备好","ns=6;s=V_2ROYDBWJS_READY"]
["RO2一段冲洗进水阀远程","ns=6;s=V_2ROYDBWJS_REM"]
["RO2一段冲洗排水阀手自动","ns=6;s=V_2ROYDBWPS_BT_AUTO"]
["RO2一段冲洗排水阀手动关","ns=6;s=V_2ROYDBWPS_BT_CLOSE"]
["RO2一段冲洗排水阀手动开","ns=6;s=V_2ROYDBWPS_BT_OPEN"]
["RO2一段冲洗排水阀故障复位","ns=6;s=V_2ROYDBWPS_BT_RESET"]
["RO2一段冲洗排水阀关到位","ns=6;s=V_2ROYDBWPS_CFB"]
["RO2一段冲洗排水阀关闭中","ns=6;s=V_2ROYDBWPS_CING"]
["RO2一段冲洗排水阀自动关闭","ns=6;s=V_2ROYDBWPS_CLOSE"]
["RO2一段冲洗排水阀故障","ns=6;s=V_2ROYDBWPS_ERR"]
["RO2一段冲洗排水阀总故障","ns=6;s=V_2ROYDBWPS_ERRT"]
["RO2一段冲洗排水阀开到位","ns=6;s=V_2ROYDBWPS_OFB"]
["RO2一段冲洗排水阀打开中","ns=6;s=V_2ROYDBWPS_OING"]
["RO2一段冲洗排水阀自动打开","ns=6;s=V_2ROYDBWPS_OPENA"]
["RO2一段冲洗排水阀关闭","ns=6;s=V_2ROYDBWPS_OUT_C"]
["RO2一段冲洗排水阀打开","ns=6;s=V_2ROYDBWPS_OUT_O"]
["RO2一段冲洗排水阀准备好","ns=6;s=V_2ROYDBWPS_READY"]
["RO2一段冲洗排水阀远程","ns=6;s=V_2ROYDBWPS_REM"]
["RO2一段产水排气阀1手自动","ns=6;s=V_2ROYDCSP1_BT_AUTO"]
["RO2一段产水排气阀1手动关","ns=6;s=V_2ROYDCSP1_BT_CLOSE"]
["RO2一段产水排气阀1手动开","ns=6;s=V_2ROYDCSP1_BT_OPEN"]
["RO2一段产水排气阀1故障复位","ns=6;s=V_2ROYDCSP1_BT_RESET"]
["RO2一段产水排气阀1关到位","ns=6;s=V_2ROYDCSP1_CFB"]
["RO2一段产水排气阀1关闭中","ns=6;s=V_2ROYDCSP1_CING"]
["RO2一段产水排气阀1自动关闭","ns=6;s=V_2ROYDCSP1_CLOS"]
["RO2一段产水排气阀1故障","ns=6;s=V_2ROYDCSP1_ERR"]
["RO2一段产水排气阀1总故障","ns=6;s=V_2ROYDCSP1_ERRT"]
["RO2一段产水排气阀1开到位","ns=6;s=V_2ROYDCSP1_OFB"]
["RO2一段产水排气阀1打开中","ns=6;s=V_2ROYDCSP1_OING"]
["RO2一段产水排气阀1自动打开","ns=6;s=V_2ROYDCSP1_OPEN"]
["RO2一段产水排气阀1关闭","ns=6;s=V_2ROYDCSP1_OUTC"]
["RO2一段产水排气阀1打开","ns=6;s=V_2ROYDCSP1_OUTO"]
["RO2一段产水排气阀1准备好","ns=6;s=V_2ROYDCSP1_READY"]
["RO2一段产水排气阀1远程","ns=6;s=V_2ROYDCSP1_REM"]
["RO2一段产水排气阀2手自动","ns=6;s=V_2ROYDCSP2_BT_AUTO"]
["RO2一段产水排气阀2手动关","ns=6;s=V_2ROYDCSP2_BT_CLOSE"]
["RO2一段产水排气阀2手动开","ns=6;s=V_2ROYDCSP2_BT_OPEN"]
["RO2一段产水排气阀2故障复位","ns=6;s=V_2ROYDCSP2_BT_RESET"]
["RO2一段产水排气阀2关到位","ns=6;s=V_2ROYDCSP2_CFB"]
["RO2一段产水排气阀2关闭中","ns=6;s=V_2ROYDCSP2_CING"]
["RO2一段产水排气阀2自动关闭","ns=6;s=V_2ROYDCSP2_CLOSEA"]
["RO2一段产水排气阀2故障","ns=6;s=V_2ROYDCSP2_ERR"]
["RO2一段产水排气阀2总故障","ns=6;s=V_2ROYDCSP2_ERRT"]
["RO2一段产水排气阀2开到位","ns=6;s=V_2ROYDCSP2_OFB"]
["RO2一段产水排气阀2打开中","ns=6;s=V_2ROYDCSP2_OING"]
["RO2一段产水排气阀2自动打开","ns=6;s=V_2ROYDCSP2_OPEN"]
["RO2一段产水排气阀2关闭","ns=6;s=V_2ROYDCSP2_OUTC"]
["RO2一段产水排气阀2打开","ns=6;s=V_2ROYDCSP2_OUTO"]
["RO2一段产水排气阀2准备好","ns=6;s=V_2ROYDCSP2_READY"]
["RO2一段产水排气阀2远程","ns=6;s=V_2ROYDCSP2_REM"]
["RO2一段超越旁路阀手自动","ns=6;s=V_2ROYDCYPL_BT_AUTO"]
["RO2一段超越旁路阀手动关","ns=6;s=V_2ROYDCYPL_BT_CLOSE"]
["RO2一段超越旁路阀手动开","ns=6;s=V_2ROYDCYPL_BT_OPEN"]
["RO2一段超越旁路阀故障复位","ns=6;s=V_2ROYDCYPL_BT_RESET"]
["RO2一段超越旁路阀关到位","ns=6;s=V_2ROYDCYPL_CFB"]
["RO2一段超越旁路阀关闭中","ns=6;s=V_2ROYDCYPL_CING"]
["RO2一段超越旁路阀自动关闭","ns=6;s=V_2ROYDCYPL_CLOSEA"]
["RO2一段超越旁路阀故障","ns=6;s=V_2ROYDCYPL_ERR"]
["RO2一段超越旁路阀总故障","ns=6;s=V_2ROYDCYPL_ERRT"]
["RO2一段超越旁路阀开到位","ns=6;s=V_2ROYDCYPL_OFB"]
["RO2一段超越旁路阀打开中","ns=6;s=V_2ROYDCYPL_OING"]
["RO2一段超越旁路阀自动打开","ns=6;s=V_2ROYDCYPL_OPENA"]
["RO2一段超越旁路阀关闭","ns=6;s=V_2ROYDCYPL_OUT_C"]
["RO2一段超越旁路阀打开","ns=6;s=V_2ROYDCYPL_OUT_O"]
["RO2一段超越旁路阀准备好","ns=6;s=V_2ROYDCYPL_READY"]
["RO2一段超越旁路阀远程","ns=6;s=V_2ROYDCYPL_REM"]
["RO2一段进水排气阀1手自动","ns=6;s=V_2ROYDJSP1_BT_AUTO"]
["RO2一段进水排气阀1手动关","ns=6;s=V_2ROYDJSP1_BT_CLOSE"]
["RO2一段进水排气阀1手动开","ns=6;s=V_2ROYDJSP1_BT_OPEN"]
["RO2一段进水排气阀1故障复位","ns=6;s=V_2ROYDJSP1_BT_RESET"]
["RO2一段进水排气阀1关到位","ns=6;s=V_2ROYDJSP1_CFB"]
["RO2一段进水排气阀1关闭中","ns=6;s=V_2ROYDJSP1_CING"]
["RO2一段进水排气阀1自动关闭","ns=6;s=V_2ROYDJSP1_CLOSEA"]
["RO2一段进水排气阀1故障","ns=6;s=V_2ROYDJSP1_ERR"]
["RO2一段进水排气阀1总故障","ns=6;s=V_2ROYDJSP1_ERRT"]
["RO2一段进水排气阀1开到位","ns=6;s=V_2ROYDJSP1_OFB"]
["RO2一段进水排气阀1打开中","ns=6;s=V_2ROYDJSP1_OING"]
["RO2一段进水排气阀1自动打开","ns=6;s=V_2ROYDJSP1_OPEN"]
["RO2一段进水排气阀1关闭","ns=6;s=V_2ROYDJSP1_OUTC"]
["RO2一段进水排气阀1打开","ns=6;s=V_2ROYDJSP1_OUTO"]
["RO2一段进水排气阀1准备好","ns=6;s=V_2ROYDJSP1_READY"]
["RO2一段进水排气阀1远程","ns=6;s=V_2ROYDJSP1_REM"]
["RO2一段进水排气阀2手自动","ns=6;s=V_2ROYDJSP2_BT_AUTO"]
["RO2一段进水排气阀2手动关","ns=6;s=V_2ROYDJSP2_BT_CLOSE"]
["RO2一段进水排气阀2手动开","ns=6;s=V_2ROYDJSP2_BT_OPEN"]
["RO2一段进水排气阀2故障复位","ns=6;s=V_2ROYDJSP2_BT_RESET"]
["RO2一段进水排气阀2关到位","ns=6;s=V_2ROYDJSP2_CFB"]
["RO2一段进水排气阀2关闭中","ns=6;s=V_2ROYDJSP2_CING"]
["RO2一段进水排气阀2自动关闭","ns=6;s=V_2ROYDJSP2_CLOS"]
["RO2一段进水排气阀2故障","ns=6;s=V_2ROYDJSP2_ERR"]
["RO2一段进水排气阀2总故障","ns=6;s=V_2ROYDJSP2_ERRT"]
["RO2一段进水排气阀2开到位","ns=6;s=V_2ROYDJSP2_OFB"]
["RO2一段进水排气阀2打开中","ns=6;s=V_2ROYDJSP2_OING"]
["RO2一段进水排气阀2自动打开","ns=6;s=V_2ROYDJSP2_OPEN"]
["RO2一段进水排气阀2关闭","ns=6;s=V_2ROYDJSP2_OUTC"]
["RO2一段进水排气阀2打开","ns=6;s=V_2ROYDJSP2_OUTO"]
["RO2一段进水排气阀2准备好","ns=6;s=V_2ROYDJSP2_READY"]
["RO2一段进水排气阀2远程","ns=6;s=V_2ROYDJSP2_REM"]
["RO2一段浓水排气阀1手自动","ns=6;s=V_2ROYDNSP1_BT_AUTO"]
["RO2一段浓水排气阀1手动关","ns=6;s=V_2ROYDNSP1_BT_CLOSE"]
["RO2一段浓水排气阀1手动开","ns=6;s=V_2ROYDNSP1_BT_OPEN"]
["RO2一段浓水排气阀1故障复位","ns=6;s=V_2ROYDNSP1_BT_RESET"]
["RO2一段浓水排气阀1关到位","ns=6;s=V_2ROYDNSP1_CFB"]
["RO2一段浓水排气阀1关闭中","ns=6;s=V_2ROYDNSP1_CING"]
["RO2一段浓水排气阀1自动关闭","ns=6;s=V_2ROYDNSP1_CLOSEA"]
["RO2一段浓水排气阀1故障","ns=6;s=V_2ROYDNSP1_ERR"]
["RO2一段浓水排气阀1总故障","ns=6;s=V_2ROYDNSP1_ERRT"]
["RO2一段浓水排气阀1开到位","ns=6;s=V_2ROYDNSP1_OFB"]
["RO2一段浓水排气阀1打开中","ns=6;s=V_2ROYDNSP1_OING"]
["RO2一段浓水排气阀1自动打开","ns=6;s=V_2ROYDNSP1_OPENA"]
["RO2一段浓水排气阀1关闭","ns=6;s=V_2ROYDNSP1_OUTC"]
["RO2一段浓水排气阀1打开","ns=6;s=V_2ROYDNSP1_OUTO"]
["RO2一段浓水排气阀1准备好","ns=6;s=V_2ROYDNSP1_READY"]
["RO2一段浓水排气阀1远程","ns=6;s=V_2ROYDNSP1_REM"]
["RO2一段浓水排气阀2手自动","ns=6;s=V_2ROYDNSP2_BT_AUTO"]
["RO2一段浓水排气阀2手动关","ns=6;s=V_2ROYDNSP2_BT_CLOSE"]
["RO2一段浓水排气阀2手动开","ns=6;s=V_2ROYDNSP2_BT_OPEN"]
["RO2一段浓水排气阀2故障复位","ns=6;s=V_2ROYDNSP2_BT_RESET"]
["RO2一段浓水排气阀2关到位","ns=6;s=V_2ROYDNSP2_CFB"]
["RO2一段浓水排气阀2关闭中","ns=6;s=V_2ROYDNSP2_CING"]
["RO2一段浓水排气阀2自动关闭","ns=6;s=V_2ROYDNSP2_CLOSEA"]
["RO2一段浓水排气阀2故障","ns=6;s=V_2ROYDNSP2_ERR"]
["RO2一段浓水排气阀2总故障","ns=6;s=V_2ROYDNSP2_ERRT"]
["RO2一段浓水排气阀2开到位","ns=6;s=V_2ROYDNSP2_OFB"]
["RO2一段浓水排气阀2打开中","ns=6;s=V_2ROYDNSP2_OING"]
["RO2一段浓水排气阀2自动打开","ns=6;s=V_2ROYDNSP2_OPEN"]
["RO2一段浓水排气阀2关闭","ns=6;s=V_2ROYDNSP2_OUTC"]
["RO2一段浓水排气阀2打开","ns=6;s=V_2ROYDNSP2_OUTO"]
["RO2一段浓水排气阀2准备好","ns=6;s=V_2ROYDNSP2_READY"]
["RO2一段浓水排气阀2远程","ns=6;s=V_2ROYDNSP2_REM"]
["RO2一段隔离阀手自动","ns=6;s=V_2ROYDQXGL_BT_AUTO"]
["RO2一段隔离阀手动关","ns=6;s=V_2ROYDQXGL_BT_CLOSE"]
["RO2一段隔离阀手动开","ns=6;s=V_2ROYDQXGL_BT_OPEN"]
["RO2一段隔离阀故障复位","ns=6;s=V_2ROYDQXGL_BT_RESET"]
["RO2一段隔离阀关到位","ns=6;s=V_2ROYDQXGL_CFB"]
["RO2一段隔离阀关闭中","ns=6;s=V_2ROYDQXGL_CING"]
["RO2一段隔离阀自动关闭","ns=6;s=V_2ROYDQXGL_CLOSEA"]
["RO2一段隔离阀故障","ns=6;s=V_2ROYDQXGL_ERR"]
["RO2一段隔离阀总故障","ns=6;s=V_2ROYDQXGL_ERRT"]
["RO2一段隔离阀开到位","ns=6;s=V_2ROYDQXGL_OFB"]
["RO2一段隔离阀打开中","ns=6;s=V_2ROYDQXGL_OING"]
["RO2一段隔离阀自动打开","ns=6;s=V_2ROYDQXGL_OPENA"]
["RO2一段隔离阀关闭","ns=6;s=V_2ROYDQXGL_OUT_C"]
["RO2一段隔离阀打开","ns=6;s=V_2ROYDQXGL_OUT_O"]
["RO2一段隔离阀准备好","ns=6;s=V_2ROYDQXGL_READY"]
["RO2一段隔离阀远程","ns=6;s=V_2ROYDQXGL_REM"]
["反洗废水外排阀手自动","ns=6;s=V_BW_WP_BT_AUTO"]
["反洗废水外排阀手动关","ns=6;s=V_BW_WP_BT_CLOSE"]
["反洗废水外排阀手动开","ns=6;s=V_BW_WP_BT_OPEN"]
["反洗废水外排阀故障复位","ns=6;s=V_BW_WP_BT_RESET"]
["反洗废水外排阀关到位","ns=6;s=V_BW_WP_CFB"]
["反洗废水外排阀关闭中","ns=6;s=V_BW_WP_CING"]
["反洗废水外排阀自动关闭","ns=6;s=V_BW_WP_CLOSEAUTO"]
["反洗废水外排阀故障","ns=6;s=V_BW_WP_ERR"]
["反洗废水外排阀总故障","ns=6;s=V_BW_WP_ERRT"]
["反洗废水外排阀开到位","ns=6;s=V_BW_WP_OFB"]
["反洗废水外排阀打开中","ns=6;s=V_BW_WP_OING"]
["反洗废水外排阀自动打开","ns=6;s=V_BW_WP_OPENAUTO"]
["反洗废水外排阀关闭","ns=6;s=V_BW_WP_OUT_CLOSE"]
["反洗废水外排阀打开","ns=6;s=V_BW_WP_OUT_OPEN"]
["反洗废水外排阀准备好","ns=6;s=V_BW_WP_READY"]
["反洗废水外排阀远程","ns=6;s=V_BW_WP_REM"]
["CEB次钠加药阀手自动","ns=6;s=V_CEB_CN_BT_AUTO"]
["CEB次钠加药阀手动关","ns=6;s=V_CEB_CN_BT_CLOSE"]
["CEB次钠加药阀手动开","ns=6;s=V_CEB_CN_BT_OPEN"]
["CEB次钠加药阀故障复位","ns=6;s=V_CEB_CN_BT_RESET"]
["CEB次钠加药阀关到位","ns=6;s=V_CEB_CN_CFB"]
["CEB次钠加药阀关闭中","ns=6;s=V_CEB_CN_CING"]
["CEB次钠加药阀自动关闭","ns=6;s=V_CEB_CN_CLOSEAUTO"]
["CEB次钠加药阀故障","ns=6;s=V_CEB_CN_ERR"]
["CEB次钠加药阀总故障","ns=6;s=V_CEB_CN_ERRT"]
["CEB次钠加药阀开到位","ns=6;s=V_CEB_CN_OFB"]
["CEB次钠加药阀打开中","ns=6;s=V_CEB_CN_OING"]
["CEB次钠加药阀自动打开","ns=6;s=V_CEB_CN_OPENAUTO"]
["CEB次钠加药阀关闭","ns=6;s=V_CEB_CN_OUT_CLOSE"]
["CEB次钠加药阀打开","ns=6;s=V_CEB_CN_OUT_OPEN"]
["CEB次钠加药阀准备好","ns=6;s=V_CEB_CN_READY"]
["CEB次钠加药阀远程","ns=6;s=V_CEB_CN_REM"]
["CEB碱加药阀手自动","ns=6;s=V_CEB_J_BT_AUTO"]
["CEB碱加药阀手动关","ns=6;s=V_CEB_J_BT_CLOSE"]
["CEB碱加药阀手动开","ns=6;s=V_CEB_J_BT_OPEN"]
["CEB碱加药阀故障复位","ns=6;s=V_CEB_J_BT_RESET"]
["CEB碱加药阀关到位","ns=6;s=V_CEB_J_CFB"]
["CEB碱加药阀关闭中","ns=6;s=V_CEB_J_CING"]
["CEB碱加药阀自动关闭","ns=6;s=V_CEB_J_CLOSEAUTO"]
["CEB碱加药阀故障","ns=6;s=V_CEB_J_ERR"]
["CEB碱加药阀总故障","ns=6;s=V_CEB_J_ERRT"]
["CEB碱加药阀开到位","ns=6;s=V_CEB_J_OFB"]
["CEB碱加药阀打开中","ns=6;s=V_CEB_J_OING"]
["CEB碱加药阀自动打开","ns=6;s=V_CEB_J_OPENAUTO"]
["CEB碱加药阀关闭","ns=6;s=V_CEB_J_OUT_CLOSE"]
["CEB碱加药阀打开","ns=6;s=V_CEB_J_OUT_OPEN"]
["CEB碱加药阀准备好","ns=6;s=V_CEB_J_READY"]
["CEB碱加药阀远程","ns=6;s=V_CEB_J_REM"]
["CEB酸加药阀手自动","ns=6;s=V_CEB_S_BT_AUTO"]
["CEB酸加药阀手动关","ns=6;s=V_CEB_S_BT_CLOSE"]
["CEB酸加药阀手动开","ns=6;s=V_CEB_S_BT_OPEN"]
["CEB酸加药阀故障复位","ns=6;s=V_CEB_S_BT_RESET"]
["CEB酸加药阀关到位","ns=6;s=V_CEB_S_CFB"]
["CEB酸加药阀关闭中","ns=6;s=V_CEB_S_CING"]
["CEB酸加药阀自动关闭","ns=6;s=V_CEB_S_CLOSEAUTO"]
["CEB酸加药阀故障","ns=6;s=V_CEB_S_ERR"]
["CEB酸加药阀总故障","ns=6;s=V_CEB_S_ERRT"]
["CEB酸加药阀开到位","ns=6;s=V_CEB_S_OFB"]
["CEB酸加药阀打开中","ns=6;s=V_CEB_S_OING"]
["CEB酸加药阀自动打开","ns=6;s=V_CEB_S_OPENAUTO"]
["CEB酸加药阀关闭","ns=6;s=V_CEB_S_OUT_CLOSE"]
["CEB酸加药阀打开","ns=6;s=V_CEB_S_OUT_OPEN"]
["CEB酸加药阀准备好","ns=6;s=V_CEB_S_READY"]
["CEB酸加药阀远程","ns=6;s=V_CEB_S_REM"]
["CEB排放阀手自动","ns=6;s=V_CEB_WP_BT_AUTO"]
["CEB排放阀手动关","ns=6;s=V_CEB_WP_BT_CLOSE"]
["CEB排放阀手动开","ns=6;s=V_CEB_WP_BT_OPEN"]
["CEB排放阀故障复位","ns=6;s=V_CEB_WP_BT_RESET"]
["CEB排放阀关到位","ns=6;s=V_CEB_WP_CFB"]
["CEB排放阀关闭中","ns=6;s=V_CEB_WP_CING"]
["CEB排放阀自动关闭","ns=6;s=V_CEB_WP_CLOSEAUTO"]
["CEB排放阀故障","ns=6;s=V_CEB_WP_ERR"]
["CEB排放阀总故障","ns=6;s=V_CEB_WP_ERRT"]
["CEB排放阀开到位","ns=6;s=V_CEB_WP_OFB"]
["CEB排放阀打开中","ns=6;s=V_CEB_WP_OING"]
["CEB排放阀自动打开","ns=6;s=V_CEB_WP_OPENAUTO"]
["CEB排放阀关闭","ns=6;s=V_CEB_WP_OUT_CLOSE"]
["CEB排放阀打开","ns=6;s=V_CEB_WP_OUT_OPEN"]
["CEB排放阀准备好","ns=6;s=V_CEB_WP_READY"]
["CEB排放阀远程","ns=6;s=V_CEB_WP_REM"]
["回用水碱加药阀手自动","ns=6;s=V_HYS_JJ_BT_AUTO"]
["回用水碱加药阀手动关","ns=6;s=V_HYS_JJ_BT_CLOSE"]
["回用水碱加药阀手动开","ns=6;s=V_HYS_JJ_BT_OPEN"]
["回用水碱加药阀故障复位","ns=6;s=V_HYS_JJ_BT_RESET"]
["回用水碱加药阀关到位","ns=6;s=V_HYS_JJ_CFB"]
["回用水碱加药阀关闭中","ns=6;s=V_HYS_JJ_CING"]
["回用水碱加药阀自动关闭","ns=6;s=V_HYS_JJ_CLOSEAUTO"]
["回用水碱加药阀故障","ns=6;s=V_HYS_JJ_ERR"]
["回用水碱加药阀总故障","ns=6;s=V_HYS_JJ_ERRT"]
["回用水碱加药阀开到位","ns=6;s=V_HYS_JJ_OFB"]
["回用水碱加药阀打开中","ns=6;s=V_HYS_JJ_OING"]
["回用水碱加药阀自动打开","ns=6;s=V_HYS_JJ_OPENAUTO"]
["回用水碱加药阀关闭","ns=6;s=V_HYS_JJ_OUT_CLOSE"]
["回用水碱加药阀打开","ns=6;s=V_HYS_JJ_OUT_OPEN"]
["回用水碱加药阀准备好","ns=6;s=V_HYS_JJ_READY"]
["回用水碱加药阀远程","ns=6;s=V_HYS_JJ_REM"]
["絮凝剂加药阀手自动","ns=6;s=V_PAC_BT_AUTO"]
["絮凝剂加药阀手动关","ns=6;s=V_PAC_BT_CLOSE"]
["絮凝剂加药阀手动开","ns=6;s=V_PAC_BT_OPEN"]
["絮凝剂加药阀故障复位","ns=6;s=V_PAC_BT_RESET"]
["絮凝剂加药阀关到位","ns=6;s=V_PAC_CFB"]
["絮凝剂加药阀关闭中","ns=6;s=V_PAC_CING"]
["絮凝剂加药阀自动关闭","ns=6;s=V_PAC_CLOSEAUTO"]
["絮凝剂加药阀故障","ns=6;s=V_PAC_ERR"]
["絮凝剂加药阀总故障","ns=6;s=V_PAC_ERRT"]
["絮凝剂加药阀开到位","ns=6;s=V_PAC_OFB"]
["絮凝剂加药阀打开中","ns=6;s=V_PAC_OING"]
["絮凝剂加药阀自动打开","ns=6;s=V_PAC_OPENAUTO"]
["絮凝剂加药阀关闭","ns=6;s=V_PAC_OUT_CLOSE"]
["絮凝剂加药阀打开","ns=6;s=V_PAC_OUT_OPEN"]
["絮凝剂加药阀准备好","ns=6;s=V_PAC_OUT_READY"]
["絮凝剂加药阀远程","ns=6;s=V_PAC_REM"]
["RO还原剂加药阀手自动","ns=6;s=V_RO_HYJ_BT_AUTO"]
["RO还原剂加药阀手动关","ns=6;s=V_RO_HYJ_BT_CLOSE"]
["RO还原剂加药阀手动开","ns=6;s=V_RO_HYJ_BT_OPEN"]
["RO还原剂加药阀故障复位","ns=6;s=V_RO_HYJ_BT_RESET"]
["RO还原剂加药阀关到位","ns=6;s=V_RO_HYJ_CFB"]
["RO还原剂加药阀关闭中","ns=6;s=V_RO_HYJ_CING"]
["RO还原剂加药阀自动关闭","ns=6;s=V_RO_HYJ_CLOSEAUTO"]
["RO还原剂加药阀故障","ns=6;s=V_RO_HYJ_ERR"]
["RO还原剂加药阀总故障","ns=6;s=V_RO_HYJ_ERRT"]
["RO还原剂加药阀开到位","ns=6;s=V_RO_HYJ_OFB"]
["RO还原剂加药阀打开中","ns=6;s=V_RO_HYJ_OING"]
["RO还原剂加药阀自动打开","ns=6;s=V_RO_HYJ_OPENAUTO"]
["RO还原剂加药阀关闭","ns=6;s=V_RO_HYJ_OUT_CLOSE"]
["RO还原剂加药阀打开","ns=6;s=V_RO_HYJ_OUT_OPEN"]
["RO还原剂加药阀准备好","ns=6;s=V_RO_HYJ_OUT_READY"]
["RO还原剂加药阀远程","ns=6;s=V_RO_HYJ_REM"]
["RO维护碱加药阀手自动","ns=6;s=V_RO_J_BT_AUTO"]
["RO维护碱加药阀手动关","ns=6;s=V_RO_J_BT_CLOSE"]
["RO维护碱加药阀手动开","ns=6;s=V_RO_J_BT_OPEN"]
["RO维护碱加药阀故障复位","ns=6;s=V_RO_J_BT_RESET"]
["RO维护碱加药阀关到位","ns=6;s=V_RO_J_CFB"]
["RO维护碱加药阀关闭中","ns=6;s=V_RO_J_CING"]
["RO维护碱加药阀自动关闭","ns=6;s=V_RO_J_CLOSEA"]
["RO维护碱加药阀故障","ns=6;s=V_RO_J_ERR"]
["RO维护碱加药阀总故障","ns=6;s=V_RO_J_ERRT"]
["RO维护碱加药阀开到位","ns=6;s=V_RO_J_OFB"]
["RO维护碱加药阀打开中","ns=6;s=V_RO_J_OING"]
["RO维护碱加药阀自动打开","ns=6;s=V_RO_J_OPENA"]
["RO维护碱加药阀关闭","ns=6;s=V_RO_J_OUTCLOSE"]
["RO维护碱加药阀打开","ns=6;s=V_RO_J_OUTOPEN"]
["RO维护碱加药阀准备好","ns=6;s=V_RO_J_READY"]
["RO维护碱加药阀远程","ns=6;s=V_RO_J_REM"]
["RO气洗阀手自动","ns=6;s=V_RO_QX_BT_AUTO"]
["RO气洗阀手动关","ns=6;s=V_RO_QX_BT_CLOSE"]
["RO气洗阀手动开","ns=6;s=V_RO_QX_BT_OPEN"]
["RO气洗阀故障复位","ns=6;s=V_RO_QX_BT_RESET"]
["RO气洗阀关到位","ns=6;s=V_RO_QX_CFB"]
["RO气洗阀关闭中","ns=6;s=V_RO_QX_CING"]
["RO气洗阀自动关闭","ns=6;s=V_RO_QX_CLOSEAUTO"]
["RO气洗阀故障","ns=6;s=V_RO_QX_ERR"]
["RO气洗阀总故障","ns=6;s=V_RO_QX_ERRT"]
["RO气洗阀开到位","ns=6;s=V_RO_QX_OFB"]
["RO气洗阀打开中","ns=6;s=V_RO_QX_OING"]
["RO气洗阀自动打开","ns=6;s=V_RO_QX_OPENAUTO"]
["RO气洗阀关闭","ns=6;s=V_RO_QX_OUT_CLOSE"]
["RO气洗阀打开","ns=6;s=V_RO_QX_OUT_OPEN"]
["RO气洗阀准备好","ns=6;s=V_RO_QX_READY"]
["RO气洗阀远程","ns=6;s=V_RO_QX_REM"]
["RO维护酸加药阀手自动","ns=6;s=V_RO_S_BT_AUTO"]
["RO维护酸加药阀手动关","ns=6;s=V_RO_S_BT_CLOSE"]
["RO维护酸加药阀手动开","ns=6;s=V_RO_S_BT_OPEN"]
["RO维护酸加药阀故障复位","ns=6;s=V_RO_S_BT_RESET"]
["RO维护酸加药阀关到位","ns=6;s=V_RO_S_CFB"]
["RO维护酸加药阀关闭中","ns=6;s=V_RO_S_CING"]
["RO维护酸加药阀自动关闭","ns=6;s=V_RO_S_CLOSEA"]
["RO维护酸加药阀故障","ns=6;s=V_RO_S_ERR"]
["RO维护酸加药阀总故障","ns=6;s=V_RO_S_ERRT"]
["RO维护酸加药阀开到位","ns=6;s=V_RO_S_OFB"]
["RO维护酸加药阀打开中","ns=6;s=V_RO_S_OING"]
["RO维护酸加药阀自动打开","ns=6;s=V_RO_S_OPENA"]
["RO维护酸加药阀关闭","ns=6;s=V_RO_S_OUTCLOSE"]
["RO维护酸加药阀打开","ns=6;s=V_RO_S_OUTOPEN"]
["RO维护酸加药阀准备好","ns=6;s=V_RO_S_READY"]
["RO维护酸加药阀远程","ns=6;s=V_RO_S_REM"]
["杀菌剂加药阀手自动","ns=6;s=V_SJJ_BT_AUTO"]
["杀菌剂加药阀手动关","ns=6;s=V_SJJ_BT_CLOSE"]
["杀菌剂加药阀手动开","ns=6;s=V_SJJ_BT_OPEN"]
["杀菌剂加药阀故障复位","ns=6;s=V_SJJ_BT_RESET"]
["杀菌剂加药阀关到位","ns=6;s=V_SJJ_CFB"]
["杀菌剂加药阀关闭中","ns=6;s=V_SJJ_CING"]
["杀菌剂加药阀自动关闭","ns=6;s=V_SJJ_CLOSEAUTO"]
["杀菌剂加药阀故障","ns=6;s=V_SJJ_ERR"]
["杀菌剂加药阀总故障","ns=6;s=V_SJJ_ERRT"]
["杀菌剂加药阀开到位","ns=6;s=V_SJJ_OFB"]
["杀菌剂加药阀打开中","ns=6;s=V_SJJ_OING"]
["杀菌剂加药阀自动打开","ns=6;s=V_SJJ_OPENAUTO"]
["杀菌剂加药阀关闭","ns=6;s=V_SJJ_OUT_CLOSE"]
["杀菌剂加药阀打开","ns=6;s=V_SJJ_OUT_OPEN"]
["杀菌剂加药阀准备好","ns=6;s=V_SJJ_READY"]
["杀菌剂加药阀远程","ns=6;s=V_SJJ_REM"]
["UF1进水调节阀备用1","ns=6;s=V_UF1_TJV_AUTO_CLOSE"]
["UF1进水调节阀备用2","ns=6;s=V_UF1_TJV_AUTO_OPEN"]
["UF1进水调节阀手自动","ns=6;s=V_UF1_TJV_BT_AUTO"]
["UF1进水调节阀备用3","ns=6;s=V_UF1_TJV_BT_CLOSE"]
["UF1进水调节阀备用4","ns=6;s=V_UF1_TJV_BT_OPEN"]
["UF1进水调节阀备用5","ns=6;s=V_UF1_TJV_BT_RESET"]
["UF1进水调节阀关状态","ns=6;s=V_UF1_TJV_CFB"]
["UF1进水调节阀备用6","ns=6;s=V_UF1_TJV_CLOSE"]
["UF1进水调节阀备用7","ns=6;s=V_UF1_TJV_FAULT"]
["UF1进水调节阀开状态","ns=6;s=V_UF1_TJV_OFB"]
["UF1进水调节阀备用8","ns=6;s=V_UF1_TJV_OPEN"]
["UF1进水调节阀备用9","ns=6;s=V_UF1_TJV_READY"]
["UF1进水调节阀备用10","ns=6;s=V_UF1_TJV_REM"]
["UF2进水调节阀备用1","ns=6;s=V_UF2_TJV_AUTO_CLOSE"]
["UF2进水调节阀备用2","ns=6;s=V_UF2_TJV_AUTO_OPEN"]
["UF2进水调节阀手自动","ns=6;s=V_UF2_TJV_BT_AUTO"]
["UF2进水调节阀备用3","ns=6;s=V_UF2_TJV_BT_CLOSE"]
["UF2进水调节阀备用4","ns=6;s=V_UF2_TJV_BT_OPEN"]
["UF2进水调节阀备用5","ns=6;s=V_UF2_TJV_BT_RESET"]
["UF2进水调节阀关状态","ns=6;s=V_UF2_TJV_CFB"]
["UF2进水调节阀备用6","ns=6;s=V_UF2_TJV_CLOSE"]
["UF2进水调节阀备用7","ns=6;s=V_UF2_TJV_FAULT"]
["UF2进水调节阀开状态","ns=6;s=V_UF2_TJV_OFB"]
["UF2进水调节阀备用8","ns=6;s=V_UF2_TJV_OPEN"]
["UF2进水调节阀备用9","ns=6;s=V_UF2_TJV_READY"]
["UF2进水调节阀备用10","ns=6;s=V_UF2_TJV_REM"]
["阻垢剂加药阀A手自动","ns=6;s=V_ZGJ_A_BT_AUTO"]
["阻垢剂加药阀A手动关","ns=6;s=V_ZGJ_A_BT_CLOSE"]
["阻垢剂加药阀A手动开","ns=6;s=V_ZGJ_A_BT_OPEN"]
["阻垢剂加药阀A故障复位","ns=6;s=V_ZGJ_A_BT_RESET"]
["阻垢剂加药阀A关到位","ns=6;s=V_ZGJ_A_CFB"]
["阻垢剂加药阀A关闭中","ns=6;s=V_ZGJ_A_CING"]
["阻垢剂加药阀A自动关闭","ns=6;s=V_ZGJ_A_CLOSEAUTO"]
["阻垢剂加药阀A故障","ns=6;s=V_ZGJ_A_ERR"]
["阻垢剂加药阀A总故障","ns=6;s=V_ZGJ_A_ERRT"]
["阻垢剂加药阀A开到位","ns=6;s=V_ZGJ_A_OFB"]
["阻垢剂加药阀A打开中","ns=6;s=V_ZGJ_A_OING"]
["阻垢剂加药阀A自动打开","ns=6;s=V_ZGJ_A_OPENAUTO"]
["阻垢剂加药阀A关闭","ns=6;s=V_ZGJ_A_OUT_CLOSE"]
["阻垢剂加药阀A打开","ns=6;s=V_ZGJ_A_OUT_OPEN"]
["阻垢剂加药阀A准备好","ns=6;s=V_ZGJ_A_OUT_READY"]
["阻垢剂加药阀A远程","ns=6;s=V_ZGJ_A_REM"]
["阻垢剂加药阀B手自动","ns=6;s=V_ZGJ_B_BT_AUTO"]
["阻垢剂加药阀B手动关","ns=6;s=V_ZGJ_B_BT_CLOSE"]
["阻垢剂加药阀B手动开","ns=6;s=V_ZGJ_B_BT_OPEN"]
["阻垢剂加药阀B故障复位","ns=6;s=V_ZGJ_B_BT_RESET"]
["阻垢剂加药阀B关到位","ns=6;s=V_ZGJ_B_CFB"]
["阻垢剂加药阀B关闭中","ns=6;s=V_ZGJ_B_CING"]
["阻垢剂加药阀B自动关闭","ns=6;s=V_ZGJ_B_CLOSEAUTO"]
["阻垢剂加药阀B故障","ns=6;s=V_ZGJ_B_ERR"]
["阻垢剂加药阀B总故障","ns=6;s=V_ZGJ_B_ERRT"]
["阻垢剂加药阀B开到位","ns=6;s=V_ZGJ_B_OFB"]
["阻垢剂加药阀B打开中","ns=6;s=V_ZGJ_B_OING"]
["阻垢剂加药阀B自动打开","ns=6;s=V_ZGJ_B_OPENAUTO"]
["阻垢剂加药阀B关闭","ns=6;s=V_ZGJ_B_OUT_CLOSE"]
["阻垢剂加药阀B打开","ns=6;s=V_ZGJ_B_OUT_OPEN"]
["阻垢剂加药阀B准备好","ns=6;s=V_ZGJ_B_OUT_READY"]
["阻垢剂加药阀B远程","ns=6;s=V_ZGJ_B_REM"]
["中和还原剂加药阀手自动","ns=6;s=V_ZH_HYJ_BT_AUTO"]
["中和还原剂加药阀手动关","ns=6;s=V_ZH_HYJ_BT_CLOSE"]
["中和还原剂加药阀手动开","ns=6;s=V_ZH_HYJ_BT_OPEN"]
["中和还原剂加药阀故障复位","ns=6;s=V_ZH_HYJ_BT_RESET"]
["中和还原剂加药阀关到位","ns=6;s=V_ZH_HYJ_CFB"]
["中和还原剂加药阀关闭中","ns=6;s=V_ZH_HYJ_CING"]
["中和还原剂加药阀自动关闭","ns=6;s=V_ZH_HYJ_CLOSEAUTO"]
["中和还原剂加药阀故障","ns=6;s=V_ZH_HYJ_ERR"]
["中和还原剂加药阀总故障","ns=6;s=V_ZH_HYJ_ERRT"]
["中和还原剂加药阀开到位","ns=6;s=V_ZH_HYJ_OFB"]
["中和还原剂加药阀打开中","ns=6;s=V_ZH_HYJ_OING"]
["中和还原剂加药阀自动打开","ns=6;s=V_ZH_HYJ_OPENAUTO"]
["中和还原剂加药阀关闭","ns=6;s=V_ZH_HYJ_OUT_CLOSE"]
["中和还原剂加药阀打开","ns=6;s=V_ZH_HYJ_OUT_OPEN"]
["中和还原剂加药阀准备好","ns=6;s=V_ZH_HYJ_OUT_READY"]
["中和还原剂加药阀远程","ns=6;s=V_ZH_HYJ_REM"]
["中和碱加药阀手自动","ns=6;s=V_ZH_J_BT_AUTO"]
["中和碱加药阀手动关","ns=6;s=V_ZH_J_BT_CLOSE"]
["中和碱加药阀手动开","ns=6;s=V_ZH_J_BT_OPEN"]
["中和碱加药阀故障复位","ns=6;s=V_ZH_J_BT_RESET"]
["中和碱加药阀关到位","ns=6;s=V_ZH_J_CFB"]
["中和碱加药阀关闭中","ns=6;s=V_ZH_J_CING"]
["中和碱加药阀自动关闭","ns=6;s=V_ZH_J_CLOSEAUTO"]
["中和碱加药阀故障","ns=6;s=V_ZH_J_ERR"]
["中和碱加药阀总故障","ns=6;s=V_ZH_J_ERRT"]
["中和碱加药阀开到位","ns=6;s=V_ZH_J_OFB"]
["中和碱加药阀打开中","ns=6;s=V_ZH_J_OING"]
["中和碱加药阀自动打开","ns=6;s=V_ZH_J_OPENAUTO"]
["中和碱加药阀关闭","ns=6;s=V_ZH_J_OUT_CLOSE"]
["中和碱加药阀打开","ns=6;s=V_ZH_J_OUT_OPEN"]
["中和碱加药阀准备好","ns=6;s=V_ZH_J_OUT_READY"]
["中和碱加药阀远程","ns=6;s=V_ZH_J_REM"]
["中和酸加药阀手自动","ns=6;s=V_ZH_S_BT_AUTO"]
["中和酸加药阀手动关","ns=6;s=V_ZH_S_BT_CLOSE"]
["中和酸加药阀手动开","ns=6;s=V_ZH_S_BT_OPEN"]
["中和酸加药阀故障复位","ns=6;s=V_ZH_S_BT_RESET"]
["中和酸加药阀关到位","ns=6;s=V_ZH_S_CFB"]
["中和酸加药阀关闭中","ns=6;s=V_ZH_S_CING"]
["中和酸加药阀自动关闭","ns=6;s=V_ZH_S_CLOSEAUTO"]
["中和酸加药阀故障","ns=6;s=V_ZH_S_ERR"]
["中和酸加药阀总故障","ns=6;s=V_ZH_S_ERRT"]
["中和酸加药阀开到位","ns=6;s=V_ZH_S_OFB"]
["中和酸加药阀打开中","ns=6;s=V_ZH_S_OING"]
["中和酸加药阀自动打开","ns=6;s=V_ZH_S_OPENAUTO"]
["中和酸加药阀关闭","ns=6;s=V_ZH_S_OUT_CLOSE"]
["中和酸加药阀打开","ns=6;s=V_ZH_S_OUT_OPEN"]
["中和酸加药阀准备好","ns=6;s=V_ZH_S_OUT_READY"]
["中和酸加药阀远程","ns=6;s=V_ZH_S_REM"]
["中和外排阀手自动","ns=6;s=V_ZH_WP_BT_AUTO"]
["中和外排阀手动关","ns=6;s=V_ZH_WP_BT_CLOSE"]
["中和外排阀手动开","ns=6;s=V_ZH_WP_BT_OPEN"]
["中和外排阀故障复位","ns=6;s=V_ZH_WP_BT_RESET"]
["中和外排阀关到位","ns=6;s=V_ZH_WP_CFB"]
["中和外排阀关闭中","ns=6;s=V_ZH_WP_CING"]
["中和外排阀自动关闭","ns=6;s=V_ZH_WP_CLOSEAUTO"]
["中和外排阀故障","ns=6;s=V_ZH_WP_ERR"]
["中和外排阀总故障","ns=6;s=V_ZH_WP_ERRT"]
["中和外排阀开到位","ns=6;s=V_ZH_WP_OFB"]
["中和外排阀打开中","ns=6;s=V_ZH_WP_OING"]
["中和外排阀自动打开","ns=6;s=V_ZH_WP_OPENAUTO"]
["中和外排阀关闭","ns=6;s=V_ZH_WP_OUT_CLOSE"]
["中和外排阀打开","ns=6;s=V_ZH_WP_OUT_OPEN"]
["中和外排阀准备好","ns=6;s=V_ZH_WP_OUT_READY"]
["中和外排阀远程","ns=6;s=V_ZH_WP_REM"]
["中和循环阀手自动","ns=6;s=V_ZHXH_BT_AUTO"]
["中和循环阀手动关","ns=6;s=V_ZHXH_BT_CLOSE"]
["中和循环阀手动开","ns=6;s=V_ZHXH_BT_OPEN"]
["中和循环阀故障复位","ns=6;s=V_ZHXH_BT_RESET"]
["中和循环阀关到位","ns=6;s=V_ZHXH_CFB"]
["中和循环阀关闭中","ns=6;s=V_ZHXH_CING"]
["中和循环阀自动关闭","ns=6;s=V_ZHXH_CLOSEAUTO"]
["中和循环阀故障","ns=6;s=V_ZHXH_ERR"]
["中和循环阀总故障","ns=6;s=V_ZHXH_ERRT"]
["中和循环阀开到位","ns=6;s=V_ZHXH_OFB"]
["中和循环阀打开中","ns=6;s=V_ZHXH_OING"]
["中和循环阀自动打开","ns=6;s=V_ZHXH_OPENAUTO"]
["中和循环阀关闭","ns=6;s=V_ZHXH_OUT_CLOSE"]
["中和循环阀打开","ns=6;s=V_ZHXH_OUT_OPEN"]
["中和循环阀准备好","ns=6;s=V_ZHXH_OUT_READY"]
["中和循环阀远程","ns=6;s=V_ZHXH_REM"]
["1#出水碱加药泵频率反馈","ns=3;s=1#CSJB_FRE_FB_O"]
["1#回用水泵电流反馈","ns=3;s=1#HYSB_CUR_FB_O"]
["1#回用水泵频率反馈","ns=3;s=1#HYSB_FRE_FB_O"]
["1#回用水泵后轴温度","ns=3;s=1#HYSB_HZ_TEMP_O"]
["1#回用水泵前轴温度","ns=3;s=1#HYSB_QZ_TEMP_O"]
["1#PAC加药泵频率反馈","ns=3;s=1#PAC_FRE_FB_O"]
["1#RO产水电导","ns=3;s=1#RO_CSDD_O"]
["1#RO产水压力","ns=3;s=1#RO_CSPRESS_O"]
["1#RO二段产水流量","ns=3;s=1#RO_EDCSFLOW_O"]
["1#RO二段进水压力","ns=3;s=1#RO_EDJSPRESS_O"]
["1#RO二段浓水压力","ns=3;s=1#RO_EDNSPRESS_O"]
["1#RO进水流量","ns=3;s=1#RO_JSFLOW_O"]
["1#RO进水压力","ns=3;s=1#RO_JSPRESS_O"]
["1#RO浓水流量","ns=3;s=1#RO_NSFLOW_O"]
["1#RO三段产水流量","ns=3;s=1#RO_SDCSFLOW_O"]
["1#RO三段进水压力","ns=3;s=1#RO_SDJSPRESS_O"]
["1#RO三段浓水压力","ns=3;s=1#RO_SDNSPRESS_O"]
["1#RO段间泵电流反馈","ns=3;s=1#RODJB_CUR_FB_O"]
["1#RO段间泵测振反馈","ns=3;s=1#RODJB_CZ_O"]
["1#RO段间泵频率反馈","ns=3;s=1#RODJB_FRE_FB_O"]
["1#RO段间泵后轴温度","ns=3;s=1#RODJB_HZ_TEMP_O"]
["1#RO段间泵前轴温度","ns=3;s=1#RODJB_QZ_TEMP_O"]
["1#RO高压泵电流反馈","ns=3;s=1#ROGYB_CUR_FB_O"]
["1#RO高压泵测振反馈","ns=3;s=1#ROGYB_CZ_O"]
["1#RO高压泵频率反馈","ns=3;s=1#ROGYB_FRE_FB_O"]
["1#RO高压泵后轴温度反馈","ns=3;s=1#ROGYB_HZ_TEMP_O"]
["1#RO高压泵前轴温度反馈","ns=3;s=1#ROGYB_QZ_TEMP_O"]
["1#RO还原剂加药泵频率反馈","ns=3;s=1#ROHYJ_FRE_FB_O"]
["1#杀菌剂加药泵频率反馈","ns=3;s=1#SJB_FRE_FB_O"]
["1#UF产水压力","ns=3;s=1#UF_CSPRESS_O"]
["1#UF进水流量","ns=3;s=1#UF_JSFLOW_O"]
["1#UF进水压力","ns=3;s=1#UF_JSPRESS_O"]
["1#UF调节阀开度反馈","ns=3;s=1#UF_V_FB_O"]
["1#UF反洗泵电流反馈","ns=3;s=1#UFBWB_CUR_FB_O"]
["1#UF反洗泵频率反馈","ns=3;s=1#UFBWB_FRE_FB_O"]
["1#UF反洗泵后轴温度反馈","ns=3;s=1#UFBWB_HZ_TEMP_O"]
["1#UF反洗泵前轴温度反馈","ns=3;s=1#UFBWB_QZ_TEMP_O"]
["1#阻垢剂流量","ns=3;s=1#ZGJ_FLOW_O"]
["1#阻垢剂加药泵频率反馈","ns=3;s=1#ZGJ_FRE_FB_O"]
["2#出水碱加药泵频率反馈","ns=3;s=2#CSJB_FRE_FB_O"]
["2#回用水泵电流反馈","ns=3;s=2#HYSB_CUR_FB_O"]
["2#回用水泵频率反馈","ns=3;s=2#HYSB_FRE_FB_O"]
["2#回用水泵后轴温度","ns=3;s=2#HYSB_HZ_TEMP_O"]
["2#回用水泵前轴温度","ns=3;s=2#HYSB_QZ_TEMP_O"]
["2#PAC加药泵频率反馈","ns=3;s=2#PAC_FRE_FB_O"]
["2#RO产水电导","ns=3;s=2#RO_CSDD_O"]
["2#RO产水压力","ns=3;s=2#RO_CSPRESS_O"]
["2#RO二段产水流量","ns=3;s=2#RO_EDCSFLOW_O"]
["2#RO二段进水压力","ns=3;s=2#RO_EDJSPRESS_O"]
["2#RO二段浓水压力","ns=3;s=2#RO_EDNSPRESS_O"]
["2#RO进水流量","ns=3;s=2#RO_JSFLOW_O"]
["2#RO进水压力","ns=3;s=2#RO_JSPRESS_O"]
["2#RO浓水流量","ns=3;s=2#RO_NSFLOW_O"]
["2#RO三段产水流量","ns=3;s=2#RO_SDCSFLOW_O"]
["2#RO三段进水压力","ns=3;s=2#RO_SDJSPRESS_O"]
["2#RO三段浓水压力","ns=3;s=2#RO_SDNSPRESS_O"]
["2#RO段间泵电流反馈","ns=3;s=2#RODJB_CUR_FB_O"]
["2#RO段间泵测振反馈","ns=3;s=2#RODJB_CZ_O"]
["2#RO段间泵频率反馈","ns=3;s=2#RODJB_FRE_FB_O"]
["2#RO段间泵后轴温度","ns=3;s=2#RODJB_HZ_TEMP_O"]
["2#RO段间泵前轴温度","ns=3;s=2#RODJB_QZ_TEMP_O"]
["2#RO高压泵电流反馈","ns=3;s=2#ROGYB_CUR_FB_O"]
["2#RO高压泵测振反馈","ns=3;s=2#ROGYB_CZ_O"]
["2#RO高压泵频率反馈","ns=3;s=2#ROGYB_FRE_FB_O"]
["2#RO高压泵后轴温度反馈","ns=3;s=2#ROGYB_HZ_TEMP_O"]
["2#RO高压泵前轴温度反馈","ns=3;s=2#ROGYB_QZ_TEMP_O"]
["2#RO还原剂加药泵频率反馈","ns=3;s=2#ROHYJ_FRE_FB_O"]
["2#杀菌剂加药泵频率反馈","ns=3;s=2#SJB_FRE_FB_O"]
["2#UF产水压力","ns=3;s=2#UF_CSPRESS_O"]
["2#UF进水流量","ns=3;s=2#UF_JSFLOW_O"]
["2#UF进水压力","ns=3;s=2#UF_JSPRESS_O"]
["2#UF调节阀开度反馈","ns=3;s=2#UF_V_FB_O"]
["2#UF反洗泵电流反馈","ns=3;s=2#UFBWB_CUR_FB_O"]
["2#UF反洗泵频率反馈","ns=3;s=2#UFBWB_FRE_FB_O"]
["2#UF反洗泵后轴温度反馈","ns=3;s=2#UFBWB_HZ_TEMP_O"]
["2#UF反洗泵前轴温度反馈","ns=3;s=2#UFBWB_QZ_TEMP_O"]
["2#阻垢剂流量","ns=3;s=2#ZGJ_FLOW_O"]
["2#阻垢剂加药泵频率反馈","ns=3;s=2#ZGJ_FRE_FB_O"]
["3#阻垢剂加药泵频率反馈","ns=3;s=3#ZGJ_FRE_FB_O"]
["空气压力","ns=3;s=AIR_PRESS_O"]
["次钠液位高高限值","ns=3;s=ALARM_CN_HHR"]
["次钠液位高限值","ns=3;s=ALARM_CN_HR"]
["次钠液位","ns=3;s=ALARM_CN_IN"]
["次钠液位低低限值","ns=3;s=ALARM_CN_LLR"]
["次钠液位低限值","ns=3;s=ALARM_CN_LR"]
["废水箱液位高高限值","ns=3;s=ALARM_FSX_HHR"]
["废水箱液位高限值","ns=3;s=ALARM_FSX_HR"]
["废水箱液位","ns=3;s=ALARM_FSX_IN"]
["废水箱液位低低限值","ns=3;s=ALARM_FSX_LLR"]
["废水箱液位低限值","ns=3;s=ALARM_FSX_LR"]
["还原剂液位高高限值","ns=3;s=ALARM_HYJ_HHR"]
["还原剂液位高限值","ns=3;s=ALARM_HYJ_HR"]
["还原剂液位","ns=3;s=ALARM_HYJ_IN"]
["还原剂液位低低限值","ns=3;s=ALARM_HYJ_LLR"]
["还原剂液位低限值","ns=3;s=ALARM_HYJ_LR"]
["碱液位高高限值","ns=3;s=ALARM_J_HHR"]
["碱液位高限值","ns=3;s=ALARM_J_HR"]
["碱液位","ns=3;s=ALARM_J_IN"]
["碱液位低低限值","ns=3;s=ALARM_J_LLR"]
["碱液位低限值","ns=3;s=ALARM_J_LR"]
["进水箱1液位高高限值","ns=3;s=ALARM_JSX1_HHR"]
["进水箱1液位高限值","ns=3;s=ALARM_JSX1_HR"]
["进水箱1液位","ns=3;s=ALARM_JSX1_IN"]
["进水箱1液位低低限值","ns=3;s=ALARM_JSX1_LLR"]
["进水箱1液位低限值","ns=3;s=ALARM_JSX1_LR"]
["进水箱2液位高高限值","ns=3;s=ALARM_JSX2_HHR"]
["进水箱2液位高限值","ns=3;s=ALARM_JSX2_HR"]
["进水箱2液位","ns=3;s=ALARM_JSX2_IN"]
["进水箱2液位低低限值","ns=3;s=ALARM_JSX2_LLR"]
["进水箱2液位低限值","ns=3;s=ALARM_JSX2_LR"]
["絮凝剂液位高高限值","ns=3;s=ALARM_PAC_HHR"]
["絮凝剂液位高限值","ns=3;s=ALARM_PAC_HR"]
["絮凝剂液位","ns=3;s=ALARM_PAC_IN"]
["絮凝剂液位低低限值","ns=3;s=ALARM_PAC_LLR"]
["絮凝剂液位低限值","ns=3;s=ALARM_PAC_LR"]
["CIP水箱液位高高限值","ns=3;s=ALARM_QXSX_HHR"]
["CIP水箱液位高限值","ns=3;s=ALARM_QXSX_HR"]
["CIP水箱液位","ns=3;s=ALARM_QXSX_IN"]
["CIP水箱液位低低限值","ns=3;s=ALARM_QXSX_LLR"]
["CIP水箱液位低限值","ns=3;s=ALARM_QXSX_LR"]
["RO产水箱液位高高限值","ns=3;s=ALARM_RO_CSX_HHR"]
["RO产水箱液位高限值","ns=3;s=ALARM_RO_CSX_HR"]
["RO产水箱液位","ns=3;s=ALARM_RO_CSX_IN"]
["RO产水箱液位低低限值","ns=3;s=ALARM_RO_CSX_LLR"]
["RO产水箱液位低限值","ns=3;s=ALARM_RO_CSX_LR"]
["酸液位高高限值","ns=3;s=ALARM_S_HHR"]
["酸液位高限值","ns=3;s=ALARM_S_HR"]
["酸液位","ns=3;s=ALARM_S_IN"]
["酸液位低低限值","ns=3;s=ALARM_S_LLR"]
["酸液位低限值","ns=3;s=ALARM_S_LR"]
["杀菌剂液位高高限值","ns=3;s=ALARM_SJJ_HHR"]
["杀菌剂液位高限值","ns=3;s=ALARM_SJJ_HR"]
["杀菌剂液位","ns=3;s=ALARM_SJJ_IN"]
["杀菌剂液位低低限值","ns=3;s=ALARM_SJJ_LLR"]
["杀菌剂液位低限值","ns=3;s=ALARM_SJJ_LR"]
["UF产水箱液位高高限值","ns=3;s=ALARM_UF_CSX_HHR"]
["UF产水箱液位高限值","ns=3;s=ALARM_UF_CSX_HR"]
["UF产水箱液位","ns=3;s=ALARM_UF_CSX_IN"]
["UF产水箱液位低低限值","ns=3;s=ALARM_UF_CSX_LLR"]
["UF产水箱液位低限值","ns=3;s=ALARM_UF_CSX_LR"]
["阻垢剂液位高高限值","ns=3;s=ALARM_ZGJ_HHR"]
["阻垢剂液位高限值","ns=3;s=ALARM_ZGJ_HR"]
["阻垢剂液位","ns=3;s=ALARM_ZGJ_IN"]
["阻垢剂液位低低限值","ns=3;s=ALARM_ZGJ_LLR"]
["阻垢剂液位低限值","ns=3;s=ALARM_ZGJ_LR"]
["中和水箱液位高高限值","ns=3;s=ALARM_ZHSX_HHR"]
["中和水箱液位高限值","ns=3;s=ALARM_ZHSX_HR"]
["中和水箱液位","ns=3;s=ALARM_ZHSX_IN"]
["中和水箱液位低低限值","ns=3;s=ALARM_ZHSX_LLR"]
["中和水箱液位低限值","ns=3;s=ALARM_ZHSX_LR"]
["反洗流量","ns=3;s=BW_FLOW_O"]
["反洗压力","ns=3;s=BW_PRESS_O"]
["次钠液位","ns=3;s=CN_LEVEL_O"]
["RO产水箱液位","ns=3;s=CS_LEVEL_O"]
["排队输出码","ns=3;s=FIFO_OUTCODE"]
["排队数量","ns=3;s=FIFO_QUE_NUMB"]
["排队1号码","ns=3;s=FIFO_QUE1"]
["排队10号码","ns=3;s=FIFO_QUE10"]
["排队11号码","ns=3;s=FIFO_QUE11"]
["排队2号码","ns=3;s=FIFO_QUE2"]
["排队3号码","ns=3;s=FIFO_QUE3"]
["排队4号码","ns=3;s=FIFO_QUE4"]
["排队5号码","ns=3;s=FIFO_QUE5"]
["排队6号码","ns=3;s=FIFO_QUE6"]
["排队7号码","ns=3;s=FIFO_QUE7"]
["排队8号码","ns=3;s=FIFO_QUE8"]
["排队9号码","ns=3;s=FIFO_QUE9"]
["排队等待码","ns=3;s=FIFO_WAITCODE"]
["废水箱液位","ns=3;s=FS_LEVEL_O"]
["废水泵后轴温度","ns=3;s=FSB_HZ_TEMP_O"]
["废水泵前轴温度","ns=3;s=FSB_QZ_TEMP_O"]
["还原剂液位","ns=3;s=HYJ_LEVEL_O"]
["回用水A流量","ns=3;s=HYS_A_FLOW_O"]
["回用水B流量","ns=3;s=HYS_B_FLOW_O"]
["回用水PH","ns=3;s=HYS_PH_O"]
["碱液位","ns=3;s=J_LEVEL_O"]
["还原剂搅拌器频率反馈","ns=3;s=JBQ_HYJ_FRE_FB"]
["还原剂搅拌器频率设定","ns=3;s=JBQ_HYJ_FRESET"]
["还原剂搅拌器运行时间","ns=3;s=JBQ_HYJ_RUNTIME"]
["PAC搅拌器频率反馈","ns=3;s=JBQ_PAC_FRE_FB"]
["PAC搅拌器频率设定","ns=3;s=JBQ_PAC_FRESET"]
["PAC搅拌器运行时间","ns=3;s=JBQ_PAC_RUNTIME"]
["酸搅拌器频率反馈","ns=3;s=JBQ_S_FRE_FB"]
["酸搅拌器频率设定","ns=3;s=JBQ_S_FRESET"]
["酸搅拌器运行时间","ns=3;s=JBQ_S_RUNTIME"]
["阻垢剂搅拌器频率反馈","ns=3;s=JBQ_ZGJ_FRE_FB"]
["阻垢剂搅拌器频率设定","ns=3;s=JBQ_ZGJ_FRESET"]
["阻垢剂搅拌器运行时间","ns=3;s=JBQ_ZGJ_RUNTIME"]
["进水箱1液位","ns=3;s=JSX1_LEVEL_O"]
["进水箱2液位","ns=3;s=JSX2_LEVEL_O"]
["1#次钠加药泵频率反馈","ns=3;s=P_1#CNB_FRE_FB"]
["1#次钠加药泵频率设定","ns=3;s=P_1#CNB_FRESET"]
["1#次钠加药泵运行时间","ns=3;s=P_1#CNB_RUNTIME"]
["1#出水碱加药泵频率反馈","ns=3;s=P_1#CSJB_FRE_FB"]
["1#出水碱加药泵频率设定","ns=3;s=P_1#CSJB_FRESET"]
["1#出水碱加药泵运行时间","ns=3;s=P_1#CSJB_RUNTIME"]
["1#回用水泵频率反馈","ns=3;s=P_1#HYSB_FRE_FB"]
["1#回用水泵频率设定","ns=3;s=P_1#HYSB_FRESET"]
["1#回用水泵运行时间","ns=3;s=P_1#HYSB_RUNTIME"]
["1#PAC加药泵频率反馈","ns=3;s=P_1#PACB_FRE_FB"]
["1#PAC加药泵频率设定","ns=3;s=P_1#PACB_FRESET"]
["1#PAC加药泵运行时间","ns=3;s=P_1#PACB_RUNTIME"]
["1#RO段间泵频率反馈","ns=3;s=P_1#RODJB_FRE_FB"]
["1#RO段间泵频率设定","ns=3;s=P_1#RODJB_FRESET"]
["1#RO段间泵运行时间","ns=3;s=P_1#RODJB_RUNTIME"]
["1#RO高压泵频率反馈","ns=3;s=P_1#ROGYB_FRE_FB"]
["1#RO高压泵频率设定","ns=3;s=P_1#ROGYB_FRESET"]
["1#RO高压泵运行时间","ns=3;s=P_1#ROGYB_RUNTIME"]
["1#RO还原剂加药泵频率反馈","ns=3;s=P_1#HYJB_FRE_FB"]
["1#RO还原剂加药泵频率设定","ns=3;s=P_1#HYJB_FRESET"]
["1#RO还原剂加药泵运行时间","ns=3;s=P_1#HYJB_RUNTIME"]
["1#酸加药泵频率反馈","ns=3;s=P_1#SB_FRE_FB"]
["1#酸加药泵频率设定","ns=3;s=P_1#SB_FRESET"]
["1#酸加药泵运行时间","ns=3;s=P_1#SB_RUNTIME"]
["1#杀菌剂加药泵频率反馈","ns=3;s=P_1#SJB_FRE_FB"]
["1#杀菌剂加药泵频率设定","ns=3;s=P_1#SJB_FRESET"]
["1#杀菌剂加药泵运行时间","ns=3;s=P_1#SJB_RUNTIME"]
["1#超滤碱加药泵频率反馈","ns=3;s=P_1#UF_JB_FRE_FB"]
["1#超滤碱加药泵频率设定","ns=3;s=P_1#UF_JB_FRESET"]
["1#超滤碱加药泵运行时间","ns=3;s=P_1#UF_JB_RUNTIME"]
["1#UF反洗泵频率反馈","ns=3;s=P_1#UFBWB_FRE_FB"]
["1#UF反洗泵频率设定","ns=3;s=P_1#UFBWB_FRESET"]
["1#UF反洗泵运行时间","ns=3;s=P_1#UFBWB_RUNTIME"]
["1#阻垢剂加药泵频率反馈","ns=3;s=P_1#ZGJB_FRE_FB"]
["1#阻垢剂加药泵频率设定","ns=3;s=P_1#ZGJB_FRESET"]
["1#阻垢剂加药泵运行时间","ns=3;s=P_1#ZGJB_RUNTIME"]
["1#中和还原剂加药泵频率反馈","ns=3;s=P_1#ZH_HYJ_FRE_FB"]
["1#中和还原剂加药泵频率设定","ns=3;s=P_1#ZH_HYJ_FRESET"]
["1#中和还原剂加药泵运行时间","ns=3;s=P_1#ZH_HYJ_RUNTIME"]
["2#次钠加药泵频率反馈","ns=3;s=P_2#CNB_FRE_FB"]
["2#次钠加药泵频率设定","ns=3;s=P_2#CNB_FRESET"]
["2#次钠加药泵运行时间","ns=3;s=P_2#CNB_RUNTIME"]
["2#出水碱加药泵频率反馈","ns=3;s=P_2#CSJB_FRE_FB"]
["2#出水碱加药泵频率设定","ns=3;s=P_2#CSJB_FRESET"]
["2#出水碱加药泵运行时间","ns=3;s=P_2#CSJB_RUNTIME"]
["2#回用水泵频率反馈","ns=3;s=P_2#HYSB_FRE_FB"]
["2#回用水泵频率设定","ns=3;s=P_2#HYSB_FRESET"]
["2#回用水泵运行时间","ns=3;s=P_2#HYSB_RUNTIME"]
["2#PAC加药泵频率反馈","ns=3;s=P_2#PACB_FRE_FB"]
["2#PAC加药泵频率设定","ns=3;s=P_2#PACB_FRESET"]
["2#PAC加药泵运行时间","ns=3;s=P_2#PACB_RUNTIME"]
["2#RO段间泵频率反馈","ns=3;s=P_2#RODJB_FRE_FB"]
["2#RO段间泵频率设定","ns=3;s=P_2#RODJB_FRESET"]
["2#RO段间泵运行时间","ns=3;s=P_2#RODJB_RUNTIME"]
["2#RO高压泵频率反馈","ns=3;s=P_2#ROGYB_FRE_FB"]
["2#RO高压泵频率设定","ns=3;s=P_2#ROGYB_FRESET"]
["2#RO高压泵运行时间","ns=3;s=P_2#ROGYB_RUNTIME"]
["2#RO还原剂加药泵频率反馈","ns=3;s=P_2#HYJB_FRE_FB"]
["2#RO还原剂加药泵频率设定","ns=3;s=P_2#HYJB_FRESET"]
["2#RO还原剂加药泵运行时间","ns=3;s=P_2#HYJB_RUNTIME"]
["2#酸加药泵频率反馈","ns=3;s=P_2#SB_FRE_FB"]
["2#酸加药泵频率设定","ns=3;s=P_2#SB_FRESET"]
["2#酸加药泵运行时间","ns=3;s=P_2#SB_RUNTIME"]
["2#杀菌剂加药泵频率反馈","ns=3;s=P_2#SJB_FRE_FB"]
["2#杀菌剂加药泵频率设定","ns=3;s=P_2#SJB_FRESET"]
["2#杀菌剂加药泵运行时间","ns=3;s=P_2#SJB_RUNTIME"]
["2#超滤碱加药泵频率反馈","ns=3;s=P_2#UF_JB_FRE_FB"]
["2#超滤碱加药泵频率设定","ns=3;s=P_2#UF_JB_FRESET"]
["2#超滤碱加药泵运行时间","ns=3;s=P_2#UF_JB_RUNTIME"]
["2#UF反洗泵频率反馈","ns=3;s=P_2#UFBWB_FRE_FB"]
["2#UF反洗泵频率设定","ns=3;s=P_2#UFBWB_FRESET"]
["2#UF反洗泵运行时间","ns=3;s=P_2#UFBWB_RUNTIME"]
["2#阻垢剂加药泵频率反馈","ns=3;s=P_2#ZGJB_FRE_FB"]
["2#阻垢剂加药泵频率设定","ns=3;s=P_2#ZGJB_FRESET"]
["2#阻垢剂加药泵运行时间","ns=3;s=P_2#ZGJB_RUNTIME"]
["2#中和还原剂加药泵频率反馈","ns=3;s=P_2#ZH_HYJ_FRE_FB"]
["2#中和还原剂加药泵频率设定","ns=3;s=P_2#ZH_HYJ_FRESET"]
["2#中和还原剂加药泵运行时间","ns=3;s=P_2#ZH_HYJ_RUNTIME"]
["3#阻垢剂加药泵频率反馈","ns=3;s=P_3#ZGJB_FRE_FB"]
["3#阻垢剂加药泵频率设定","ns=3;s=P_3#ZGJB_FRESET"]
["3#阻垢剂加药泵运行时间","ns=3;s=P_3#ZGJB_RUNTIME"]
["废水泵频率反馈","ns=3;s=P_FSB_FRE_FB"]
["废水泵频率设定","ns=3;s=P_FSB_FRESET"]
["废水泵运行时间","ns=3;s=P_FSB_RUNTIME"]
["加热器频率反馈","ns=3;s=P_JRQ_FRE_FB"]
["加热器频率设定","ns=3;s=P_JRQ_FRESET"]
["加热器运行时间","ns=3;s=P_JRQ_RUNTIME"]
["潜污泵频率反馈","ns=3;s=P_QWB_FRE_FB"]
["潜污泵频率设定","ns=3;s=P_QWB_FRESET"]
["潜污泵运行时间","ns=3;s=P_QWB_RUNTIME"]
["清洗水泵频率反馈","ns=3;s=P_QXSB_FRE_FB"]
["清洗水泵频率设定","ns=3;s=P_QXSB_FRESET"]
["清洗水泵运行时间","ns=3;s=P_QXSB_RUNTIME"]
["RO供水泵频率反馈","ns=3;s=P_ROGSB_FRE_FB"]
["RO供水泵频率设定","ns=3;s=P_ROGSB_FRESET"]
["RO供水泵运行时间","ns=3;s=P_ROGSB_RUNTIME"]
["UF供水泵频率反馈","ns=3;s=P_UFGSB_FRE_FB"]
["UF供水泵频率设定","ns=3;s=P_UFGSB_FRESET"]
["UF供水泵运行时间","ns=3;s=P_UFGSB_RUNTIME"]
["中和泵频率反馈","ns=3;s=P_ZH_FRE_FB"]
["中和泵频率设定","ns=3;s=P_ZH_FRESET"]
["中和泵运行时间","ns=3;s=P_ZH_RUNTIME"]
["絮凝剂液位","ns=3;s=PAC_LEVEL_O"]
["CIP水箱液位","ns=3;s=QXS_LEVEL_O"]
["CIP水PH","ns=3;s=QXS_PH_O"]
["CIP水温度","ns=3;s=QXS_TEMP_O"]
["清洗水泵电流","ns=3;s=QXSB_CUR_FB_O"]
["清洗水泵频率反馈","ns=3;s=QXSB_FRE_FB_O"]
["清洗水泵后轴温度反馈","ns=3;s=QXSB_HZ_TEMP_O"]
["清洗水泵前轴温度反馈","ns=3;s=QXSB_QZ_TEMP_O"]
["RO供水泵后轴温度反馈","ns=3;s=RO_GSB_HZ_TEMP_O"]
["RO供水泵前轴温度反馈","ns=3;s=RO_GSB_QZ_TEMP_0"]
["RO进水电导","ns=3;s=RO_JSDD_O"]
["RO进水ORP","ns=3;s=RO_JSORP_O"]
["RO进水PH","ns=3;s=RO_JSPH_O"]
["RO外供水电导","ns=3;s=RO_WSDD_O"]
["RO1一段压差","ns=3;s=RO1_1D_YC"]
["RO1一段压差设定","ns=3;s=RO1_1D_YC_SET"]
["RO1一段产水流量","ns=3;s=RO1_1DUAN_CS_FLOW"]
["RO1一段已碱维护天数","ns=3;s=RO1_1DYJWH_DAYS"]
["RO1一段已杀菌天数","ns=3;s=RO1_1DYSJ_DAYS"]
["RO1一段已酸维护天数","ns=3;s=RO1_1DYSWH_DAYS"]
["RO1二三段已碱维护天数","ns=3;s=RO1_23DYJWH_DAYS"]
["RO1二三段已杀菌天数","ns=3;s=RO1_23DYSJ_DAYS"]
["RO1二三段已酸维护天数","ns=3;s=RO1_23DYSWH_DAYS"]
["RO1二段压差","ns=3;s=RO1_2D_YC"]
["RO1二段压差设定","ns=3;s=RO1_2D_YC_SET"]
["RO1CODE_一段碱维护","ns=3;s=RO1_CODE_1DJWH"]
["RO1CODE_一段杀菌","ns=3;s=RO1_CODE_1DSJ"]
["RO1CODE_一段酸维护","ns=3;s=RO1_CODE_1DSWH"]
["RO1CODE_二三段碱维护","ns=3;s=RO1_CODE_23DJWH"]
["RO1CODE_二三段杀菌","ns=3;s=RO1_CODE_23DSJ"]
["RO1CODE_二三段酸维护","ns=3;s=RO1_CODE_23DSWH"]
["RO1CODE_冲洗","ns=3;s=RO1_CODE_CX"]
["RO1设定段间泵启动频率","ns=3;s=RO1_GSB_FR_OUT"]
["1#RO高压泵频率输出","ns=3;s=RO1_GYB_FR_OUT"]
["RO1系统定时","ns=3;s=RO1_HMI_SET_TIME"]
["RO1系统计时","ns=3;s=RO1_HMI_SYSTEM_TIME"]
["RO1需要冲洗流量","ns=3;s=RO1_NEED_CXLL"]
["RO1需要段间泵流量","ns=3;s=RO1_NEED_DJBLL"]
["RO1需要供水流量","ns=3;s=RO1_NEED_GSLL"]
["RO1需要高压泵流量","ns=3;s=RO1_NEED_GYBLL"]
["RO1产水率","ns=3;s=RO1_RATE_CS"]
["RO1SET_一段碱维护天数","ns=3;s=RO1_SET_1DJWH_DAYS"]
["RO1SET_一段碱维后气水混洗时间","ns=3;s=RO1_SET_1DJWHHX_TIME"]
["RO1SET_一段碱维后水洗时间","ns=3;s=RO1_SET_1DJWHSX_TIME"]
["RO1SET_一段碱维加碱时间","ns=3;s=RO1_SET_1DJWJJ_TIME"]
["RO1SET_一段碱维浸泡时间","ns=3;s=RO1_SET_1DJWJP_TIME"]
["RO1SET_一段杀菌天数","ns=3;s=RO1_SET_1DSJ_DAYS"]
["RO1Set一段杀菌时间","ns=3;s=RO1_SET_1DSJ_TIME"]
["RO1Set_一段杀菌浸泡时间","ns=3;s=RO1_SET_1DSJJP_TIME"]
["RO1Set一段杀菌结束反冲排气时间","ns=3;s=RO1_SET_1DSJJS_TIME"]
["RO1Set一段杀菌结束气水冲时间","ns=3;s=RO1_SET_1DSJJSQ_TIME"]
["RO1SET_一段酸维护天数","ns=3;s=RO1_SET_1DSWH_DAYS"]
["RO1SET_一段酸维后气水混洗时间","ns=3;s=RO1_SET_1DSWHHX_TIME"]
["RO1SET_一段酸维后水洗时间","ns=3;s=RO1_SET_1DSWHSX_TIME"]
["RO1SET_一段酸维浸泡时间","ns=3;s=RO1_SET_1DSWJP_TIME"]
["RO1SET_一段酸维加酸时间","ns=3;s=RO1_SET_1DSWJS_TIME"]
["RO1Set_二三段正冲时间","ns=3;s=RO1_SET_2/3DZC_TIME"]
["RO1SET_二三段碱维护天数","ns=3;s=RO1_SET_23DJWH_DAYS"]
["RO1SET_二三段碱维护时间","ns=3;s=RO1_SET_23DJWH_TIME"]
["RO1SET_二三段碱维护后冲洗时间","ns=3;s=RO1_SET_23DJWHHCX_T"]
["RO1SET_二三段碱维护浸泡时间","ns=3;s=RO1_SET_23DJWHJ_TIME"]
["RO1SET_二三段杀菌天数","ns=3;s=RO1_SET_23DSJ_DAYS"]
["RO1SET_二三段杀菌后冲洗时间","ns=3;s=RO1_SET_23DSJCX_TIME"]
["RO1SET_二三段杀菌浸泡时间","ns=3;s=RO1_SET_23DSJJP_TIME"]
["RO1SET_二三段杀菌维护时间","ns=3;s=RO1_SET_23DSJWH_TIME"]
["RO1SET_二三段酸维护天数","ns=3;s=RO1_SET_23DSWH_DAYS"]
["RO1SET_二三段酸维护时间","ns=3;s=RO1_SET_23DSWH_TIME"]
["RO1SET_二三段酸维护后冲洗时间","ns=3;s=RO1_SET_23SWHHC_TIME"]
["RO1SET_二三段酸维护浸泡时间","ns=3;s=RO1_SET_23SWHJP_TIME"]
["RO1SET_超越过滤冲水排气时间","ns=3;s=RO1_SET_CYSGLCSPQ_T"]
["RO1SET_超越停机冲洗时间","ns=3;s=RO1_SET_CYTJCX_T"]
["RO1SET_超越停机加药冲洗时间","ns=3;s=RO1_SET_CYTJJYCX_T"]
["RO1SET_电导率","ns=3;s=RO1_SET_DDL"]
["RO1段间泵流量设定","ns=3;s=RO1_SET_DJBLL"]
["RO1Set反冲时间","ns=3;s=RO1_SET_FC_TIME"]
["RO1Set过滤产水时间","ns=3;s=RO1_SET_GLCS_TIME"]
["RO1供水流量设定","ns=3;s=RO1_SET_GSL"]
["RO1SET_GSPump_频率_L","ns=3;s=RO1_SET_GSPUMP_FR_L"]
["RO1SET_GYPump_频率","ns=3;s=RO1_SET_GYPUMP_FR"]
["RO1SET_GYPump_频率_H","ns=3;s=RO1_SET_GYPUMP_FR_H"]
["RO1SET_GYPump_频率_L","ns=3;s=RO1_SET_GYPUMP_FR_L"]
["RO1SET_加药冲洗反冲洗时间","ns=3;s=RO1_SET_JYCXFC_T"]
["RO1SET_加药冲洗正冲洗时间","ns=3;s=RO1_SET_JYCXZC_TIME"]
["RO1Set开机冲洗时间","ns=3;s=RO1_SET_KJCX_TIME"]
["RO1SET_ORP","ns=3;s=RO1_SET_ORP"]
["RO1SET_气水混洗时间","ns=3;s=RO1_SET_QSHX_TIEM"]
["RO1Set_水反洗排气时间","ns=3;s=RO1_SET_SFXPQ_TIME"]
["RO1SET_杀菌后反冲时间","ns=3;s=RO1_SET_SJHFC_TIME"]
["RO1SET_杀菌后正冲时间","ns=3;s=RO1_SET_SJHZC_TIME"]
["RO1杀菌浸泡时间设定","ns=3;s=RO1_SET_SJJP_TIME"]
["RO1SET杀菌流量","ns=3;s=RO1_SET_SJLL"]
["RO1Set停机加药冲洗时间","ns=3;s=RO1_SET_TJJYCX_TIME"]
["RO1SET_预杀菌天数","ns=3;s=RO1_SET_YSJ_DAYS"]
["RO1Set正冲时间","ns=3;s=RO1_SET_ZC_TIME"]
["RO1SET正冲流量","ns=3;s=RO1_SET_ZCLL"]
["RO1步序","ns=3;s=RO1_STEP"]
["RO1总产水流量","ns=3;s=RO1_TOTAL_CSLL"]
["RO1总过滤次数","ns=3;s=RO1_TOTAL_GL_CS"]
["RO1总进水流量","ns=3;s=RO1_TOTAL_JSLL"]
["RO1总浓水流量","ns=3;s=RO1_TOTAL_NSLL"]
["RO2一段压差","ns=3;s=RO2_1D_YC"]
["RO2一段压差设定","ns=3;s=RO2_1D_YC_SET"]
["RO2一段产水流量","ns=3;s=RO2_1DUAN_CS_FLOW"]
["RO2一段已碱维护天数","ns=3;s=RO2_1DYJWH_DAYS"]
["RO2一段已杀菌天数","ns=3;s=RO2_1DYSJ_DAYS"]
["RO2一段已酸维护天数","ns=3;s=RO2_1DYSWH_DAYS"]
["RO2二三段已碱维护天数","ns=3;s=RO2_23DYJWH_DAYS"]
["RO2二三段已杀菌天数","ns=3;s=RO2_23DYSJ_DAYS"]
["RO2二三段已酸维护天数","ns=3;s=RO2_23DYSWH_DAYS"]
["RO2二段压差","ns=3;s=RO2_2D_YC"]
["RO2二段压差设定","ns=3;s=RO2_2D_YC_SET"]
["RO2CODE_一段碱维护","ns=3;s=RO2_CODE_1DJWH"]
["RO2CODE_一段杀菌","ns=3;s=RO2_CODE_1DSJ"]
["RO2CODE_一段酸维护","ns=3;s=RO2_CODE_1DSWH"]
["RO2CODE_二三段碱维护","ns=3;s=RO2_CODE_23DJWH"]
["RO2CODE_二三段杀菌","ns=3;s=RO2_CODE_23DSJ"]
["RO2CODE_二三段酸维护","ns=3;s=RO2_CODE_23DSWH"]
["RO2CODE_冲洗","ns=3;s=RO2_CODE_CX"]
["2#RO供水泵频率输出","ns=3;s=RO2_GSB_FR_OUT"]
["2#RO高压泵频率输出","ns=3;s=RO2_GYB_FR_OUT"]
["RO2系统定时","ns=3;s=RO2_HMI_SET_TIME"]
["RO2系统计时","ns=3;s=RO2_HMI_SYSTEM_TIME"]
["RO2需要冲洗流量","ns=3;s=RO2_NEED_CXLL"]
["RO2需要段间泵流量","ns=3;s=RO2_NEED_DJBLL"]
["RO2需要供水流量","ns=3;s=RO2_NEED_GSLL"]
["RO2需要高压泵流量","ns=3;s=RO2_NEED_GYBLL"]
["RO2产水率","ns=3;s=RO2_RATE_CS"]
["RO2SET_一段碱维护天数","ns=3;s=RO2_SET_1DJWH_DAYS"]
["RO2SET_一段碱维后气水混洗时间","ns=3;s=RO2_SET_1DJWHHX_TIME"]
["RO2SET_一段碱维后水洗时间","ns=3;s=RO2_SET_1DJWHSX_TIME"]
["RO2SET_一段碱维加碱时间","ns=3;s=RO2_SET_1DJWJJ_TIME"]
["RO2SET_一段碱维浸泡时间","ns=3;s=RO2_SET_1DJWJP_TIME"]
["RO2SET_一段杀菌天数","ns=3;s=RO2_SET_1DSJ_DAYS"]
["RO2Set一段杀菌时间","ns=3;s=RO2_SET_1DSJ_TIME"]
["RO2Set_一段杀菌浸泡时间","ns=3;s=RO2_SET_1DSJJP_TIME"]
["RO2Set一段杀菌结束反冲排气时间","ns=3;s=RO2_SET_1DSJJS_TIME"]
["RO2Set一段杀菌结束气水冲时间","ns=3;s=RO2_SET_1DSJJSQ_TIME"]
["RO2SET_一段酸维护天数","ns=3;s=RO2_SET_1DSWH_DAYS"]
["RO2SET_一段酸维后气水混洗时间","ns=3;s=RO2_SET_1DSWHHX_TIME"]
["RO2SET_一段酸维后水洗时间","ns=3;s=RO2_SET_1DSWHSX_TIME"]
["RO2SET_一段酸维浸泡时间","ns=3;s=RO2_SET_1DSWJP_TIME"]
["RO2SET_一段酸维加酸时间","ns=3;s=RO2_SET_1DSWJS_TIME"]
["RO2Set_二三段正冲时间","ns=3;s=RO2_SET_2/3DZC_TIME"]
["RO2SET_二三段碱维护天数","ns=3;s=RO2_SET_23DJWH_DAYS"]
["RO2SET_二三段碱维护时间","ns=3;s=RO2_SET_23DJWH_TIME"]
["RO2SET_二三段碱维护后冲洗时间","ns=3;s=RO2_SET_23DJWHHCX_T"]
["RO2SET_二三段碱维护浸泡时间","ns=3;s=RO2_SET_23DJWHJ_TIME"]
["RO2SET_二三段杀菌天数","ns=3;s=RO2_SET_23DSJ_DAYS"]
["RO2SET_二三段杀菌后冲洗时间","ns=3;s=RO2_SET_23DSJCX_TIME"]
["RO2SET_二三段杀菌浸泡时间","ns=3;s=RO2_SET_23DSJJP_TIME"]
["RO2SET_二三段杀菌维护时间","ns=3;s=RO2_SET_23DSJWH_TIME"]
["RO2SET_二三段酸维护天数","ns=3;s=RO2_SET_23DSWH_DAYS"]
["RO2SET_二三段酸维护时间","ns=3;s=RO2_SET_23DSWH_TIME"]
["RO2SET_二三段酸维护后冲洗时间","ns=3;s=RO2_SET_23SWHHC_TIME"]
["RO2SET_二三段酸维护浸泡时间","ns=3;s=RO2_SET_23SWHJP_TIME"]
["RO2SET_超越过滤冲水排气时间","ns=3;s=RO2_SET_CYSGLCSPQ_T"]
["RO2SET_超越停机冲洗时间","ns=3;s=RO2_SET_CYTJCX_T"]
["RO2SET_超越停机加药冲洗时间","ns=3;s=RO2_SET_CYTJJYCX_T"]
["RO2SET_电导率","ns=3;s=RO2_SET_DDL"]
["RO2段间泵流量设定","ns=3;s=RO2_SET_DJBLL"]
["RO2Set反冲时间","ns=3;s=RO2_SET_FC_TIME"]
["RO2Set过滤产水时间","ns=3;s=RO2_SET_GLCS_TIME"]
["RO2供水流量设定","ns=3;s=RO2_SET_GSL"]
["RO2SET_GSPump_频率_L","ns=3;s=RO2_SET_GSPUMP_FR_L"]
["RO2SET_GYPump_频率","ns=3;s=RO2_SET_GYPUMP_FR"]
["RO2SET_GYPump_频率_H","ns=3;s=RO2_SET_GYPUMP_FR_H"]
["RO2SET_GYPump_频率_L","ns=3;s=RO2_SET_GYPUMP_FR_L"]
["RO2SET_加药冲洗反冲洗时间","ns=3;s=RO2_SET_JYCXFC_T"]
["RO2SET_加药冲洗正冲洗时间","ns=3;s=RO2_SET_JYCXZC_TIME"]
["RO2Set开机冲洗时间","ns=3;s=RO2_SET_KJCX_TIME"]
["RO2SET_ORP","ns=3;s=RO2_SET_ORP"]
["RO2SET_气水混洗时间","ns=3;s=RO2_SET_QSHX_TIEM"]
["RO2Set_水反洗排气时间","ns=3;s=RO2_SET_SFXPQ_TIME"]
["RO2SET_杀菌后反冲时间","ns=3;s=RO2_SET_SJHFC_TIME"]
["RO2SET_杀菌后正冲时间","ns=3;s=RO2_SET_SJHZC_TIME"]
["RO2杀菌浸泡时间设定","ns=3;s=RO2_SET_SJJP_TIME"]
["RO2SET杀菌流量","ns=3;s=RO2_SET_SJLL"]
["RO2Set停机加药冲洗时间","ns=3;s=RO2_SET_TJJYCX_TIME"]
["RO2SET_预杀菌天数","ns=3;s=RO2_SET_YSJ_DAYS"]
["RO2Set正冲时间","ns=3;s=RO2_SET_ZC_TIME"]
["RO2SET正冲流量","ns=3;s=RO2_SET_ZCLL"]
["RO2步序","ns=3;s=RO2_STEP"]
["RO2总产水流量","ns=3;s=RO2_TOTAL_CSLL"]
["RO2总过滤次数","ns=3;s=RO2_TOTAL_GL_CS"]
["RO2总进水流量","ns=3;s=RO2_TOTAL_JSLL"]
["RO2总浓水流量","ns=3;s=RO2_TOTAL_NSLL"]
["RO供水泵电流","ns=3;s=ROGSB_CUR_FB_O"]
["RO供水泵频率反馈","ns=3;s=ROGSB_FRE_FB_O"]
["酸液位","ns=3;s=S_LEVEL_O"]
["杀菌剂液位","ns=3;s=SJJ_LEVEL_O"]
["UF产水浊度","ns=3;s=UF_CS_ZD_O"]
["UF产水箱液位","ns=3;s=UF_CSLEVEL_O"]
["UF1反洗次数显示","ns=3;s=UF1_OUT_BW_CS"]
["UF1反洗流量累计","ns=3;s=UF1_OUT_BW_FLOW_ADD"]
["UF1反洗总次数累计","ns=3;s=UF1_OUT_BW_ZCS"]
["UF1过滤流量累计","ns=3;s=UF1_OUT_GL_FLOW_ADD"]
["UF1系统设置时间","ns=3;s=UF1_OUT_SET_TIME"]
["UF1系统显示时间","ns=3;s=UF1_OUT_SYS_TIME"]
["UF1设置反洗次数","ns=3;s=UF1_SET_BW_CS"]
["UF1设置反洗流量","ns=3;s=UF1_SET_BW_FLOW"]
["UF1设置冲水排气流量","ns=3;s=UF1_SET_CS_FLOW"]
["UF1设置冲水排气时间","ns=3;s=UF1_SET_CSPQ_TIME"]
["UF1设置过滤流量","ns=3;s=UF1_SET_GL_FLOW"]
["UF1设置过滤时间","ns=3;s=UF1_SET_GL_TIME"]
["UF1设置加药流量","ns=3;s=UF1_SET_JY_FLOW"]
["UF1设置跨膜压差高高值","ns=3;s=UF1_SET_KMYC_HHR"]
["UF1设置跨膜压差高值","ns=3;s=UF1_SET_KMYC_HR"]
["UF1设置酸反洗时间","ns=3;s=UF1_SET_S_BW_TIME"]
["UF1设置CEB后冲时间","ns=3;s=UF1_SETCEB_HC_TIME"]
["UF1设置CEB浸泡时间","ns=3;s=UF1_SETCEB_JP_TIME"]
["UF1设置CEB加药时间","ns=3;s=UF1_SETCEB_JY_TIME"]
["UF1设置CEB前冲时间","ns=3;s=UF1_SETCEB_QC_TIME"]
["UF1跨膜压差","ns=3;s=UF1_SSD_KMYC"]
["UF1步序","ns=3;s=UF1_STEP"]
["UF2反洗次数显示","ns=3;s=UF2_OUT_BW_CS"]
["UF2反洗流量累计","ns=3;s=UF2_OUT_BW_FLOW_ADD"]
["UF2反洗总次数累计","ns=3;s=UF2_OUT_BW_ZCS"]
["UF2过滤流量累计","ns=3;s=UF2_OUT_GL_FLOW_ADD"]
["UF2系统设置时间","ns=3;s=UF2_OUT_SET_TIME"]
["UF2系统显示时间","ns=3;s=UF2_OUT_SYS_TIME"]
["UF2设置反洗次数","ns=3;s=UF2_SET_BW_CS"]
["UF2设置反洗流量","ns=3;s=UF2_SET_BW_FLOW"]
["UF2设置冲水排气流量","ns=3;s=UF2_SET_CS_FLOW"]
["UF2设置冲水排气时间","ns=3;s=UF2_SET_CSPQ_TIME"]
["UF2设置过滤流量","ns=3;s=UF2_SET_GL_FLOW"]
["UF2设置过滤时间","ns=3;s=UF2_SET_GL_TIME"]
["UF2设置加药流量","ns=3;s=UF2_SET_JY_FLOW"]
["UF2设置跨膜压差高高值","ns=3;s=UF2_SET_KMYC_HHR"]
["UF2设置跨膜压差高值","ns=3;s=UF2_SET_KMYC_HR"]
["UF2设置酸反洗时间","ns=3;s=UF2_SET_S_BW_TIME"]
["UF2设置CEB后冲时间","ns=3;s=UF2_SETCEB_HC_TIME"]
["UF2设置CEB浸泡时间","ns=3;s=UF2_SETCEB_JP_TIME"]
["UF2设置CEB加药时间","ns=3;s=UF2_SETCEB_JY_TIME"]
["UF2设置CEB前冲时间","ns=3;s=UF2_SETCEB_QC_TIME"]
["UF2跨膜压差","ns=3;s=UF2_SSD_KMYC"]
["UF2步序","ns=3;s=UF2_STEP"]
["UF供水泵电流","ns=3;s=UFGSB_CUR_FB_O"]
["UF供水泵频率反馈","ns=3;s=UFGSB_FRE_FB_O"]
["UF供水泵后轴温度反馈","ns=3;s=UFGSB_HZ_TEMP_O"]
["UF供水泵前轴温度反馈","ns=3;s=UFGSB_QZ_TEMP_O"]
["UF1调节阀开度反馈","ns=3;s=V_UF1_TJV_KD_FB"]
["UF1调节阀开度设定","ns=3;s=V_UF1_TJV_KD_SET"]
["UF2调节阀开度反馈","ns=3;s=V_UF2_TJV_KD_FB"]
["UF2调节阀开度设定","ns=3;s=V_UF2_TJV_KD_SET"]
["阻垢剂液位","ns=3;s=ZGJ_LEVEL_O"]
["中和水箱液位","ns=3;s=ZH_LEVEL_O"]
["中和水箱ORP","ns=3;s=ZH_ORP_O"]
["中和水箱PH","ns=3;s=ZH_PH_O"]
["中和泵后轴温度","ns=3;s=ZHB_HZ_TEMP_O"]
["中和泵前轴温度","ns=3;s=ZHB_QZ_TEMP_O"]
["进水压力","ns=3;s=ZJS_PRESS_O"]
["进水温度","ns=3;s=ZJS_TEMP_O"]
["UF进水浊度","ns=3;s=ZJS_ZD_O"]
["2号阻垢剂泵给RO1用","ns=6;s=PUBLIC_BYZGJB4_1"]
["2号阻垢剂泵给RO2用","ns=6;s=PUBLIC_BYZGJB4_2"]
["UF其它设备CEB中","ns=6;s=PUBLIC_OTHER_CEBING"]
["UF其它设备反洗中","ns=6;s=PUBLIC_OTHER_BWING"]
["其它RO在过滤中","ns=6;s=PUBLIC_OTHERRO_GLING"]
["RO_回用水泵PID选择","ns=6;s=PUBLIC_RO_HYSB_PID"]
["RO其他设备杀菌中","ns=6;s=PUBLIC_RO_OTHER_SJ"]
["RO其他设备冲洗中","ns=6;s=PUBLIC_RO_OTHER_CX"]
["RO_系统自动","ns=6;s=PUBLIC_RO_SYS_AUOTO"]
["RO_系统手动","ns=6;s=PUBLIC_RO_SYS_MAN"]
["RO1_允许冲洗","ns=6;s=PUBLIC_RO1_ALLOW_CX"]
["RO1_允许过滤","ns=6;s=PUBLIC_RO1_ALLOW_GL"]
["RO1_允许杀菌","ns=6;s=PUBLIC_RO1_ALLOW_SJ"]
["RO1_段间泵PID选择","ns=6;s=PUBLIC_RO1_DJB_PID"]
["RO1_高压泵PID选择","ns=6;s=PUBLIC_RO1_GYB_PID"]
["RO2_允许冲洗","ns=6;s=PUBLIC_RO2_ALLOW_CX"]
["RO2_允许过滤","ns=6;s=PUBLIC_RO2_ALLOW_GL"]
["RO2_允许杀菌","ns=6;s=PUBLIC_RO2_ALLOW_SJ"]
["RO2_段间泵PID选择","ns=6;s=PUBLIC_RO2_DJB_PID"]
["RO2_高压泵PID选择","ns=6;s=PUBLIC_RO2_GYB_PID"]
["UF_反洗泵PID模式选择","ns=6;s=PUBLIC_UF_FXB_PID"]
["UF系统自动","ns=6;s=PUBLIC_UF_SYS_AUTO"]
["UF系统手动","ns=6;s=PUBLIC_UF_SYS_MAN"]
["UF允许反洗","ns=6;s=PUBLIC_UF1_ALLOW_BW"]
["UF1允许CEB","ns=6;s=PUBLIC_UF1_ALLOW_CEB"]
["UF允许过滤","ns=6;s=PUBLIC_UF1_ALLOW_GL"]
["UF1_TJF_PID模式","ns=6;s=PUBLIC_UF1_TJF_PID"]
["UF2允许反洗","ns=6;s=PUBLIC_UF2_ALLOW_BW"]
["UF2允许CEB","ns=6;s=PUBLIC_UF2_ALLOW_CEB"]
["UF2允许过滤","ns=6;s=PUBLIC_UF2_ALLOW_GL"]
["UF2_TJF_PID模式","ns=6;s=PUBLIC_UF2_TJF_PID"]
["RO1系统报错","ns=6;s=PUBLIC_BY_B00L_1"]
["RO2系统报错","ns=6;s=PUBLIC_BY_BOOL_2"]
["离散变量备用3","ns=6;s=PUBLIC_BY_BOOL_3"]
["离散变量备用4","ns=6;s=PUBLIC_BY_BOOL_4"]
["离散变量备用5","ns=6;s=PUBLIC_BY_BOOL_5"]
["离散变量备用6","ns=6;s=PUBLIC_BY_BOOL_6"]
["离散变量备用7","ns=6;s=PUBLIC_BY_BOOL_7"]
["离散变量备用8","ns=6;s=PUBLIC_BY_BOOL_8"]
["离散变量备用9","ns=6;s=PUBLIC_BY_BOOL_9"]
["离散变量备用10","ns=6;s=PUBLIC_BY_BOOL_10"]
["离散变量备用11","ns=6;s=PUBLIC_BY_BOOL_11"]
["离散变量备用12","ns=6;s=PUBLIC_BY_BOOL_12"]
["离散变量备用13","ns=6;s=PUBLIC_BY_BOOL_13"]
["离散变量备用14","ns=6;s=PUBLIC_BY_BOOL_14"]
["离散变量备用15","ns=6;s=PUBLIC_BY_BOOL_15"]
["离散变量备用16","ns=6;s=PUBLIC_BY_BOOL_16"]
["离散变量备用17","ns=6;s=PUBLIC_BY_BOOL_17"]
["离散变量备用18","ns=6;s=PUBLIC_BY_BOOL_18"]
["离散变量备用19","ns=6;s=PUBLIC_BY_BOOL_19"]
["离散变量备用20","ns=6;s=PUBLIC_BY_BOOL_20"]
["离散变量备用21","ns=6;s=PUBLIC_BY_BOOL_21"]
["离散变量备用22","ns=6;s=PUBLIC_BY_BOOL_22"]
["离散变量备用23","ns=6;s=PUBLIC_BY_BOOL_23"]
["离散变量备用24","ns=6;s=PUBLIC_BY_BOOL_24"]
["离散变量备用25","ns=6;s=PUBLIC_BY_BOOL_25"]
["离散变量备用26","ns=6;s=PUBLIC_BY_BOOL_26"]
["离散变量备用27","ns=6;s=PUBLIC_BY_BOOL_27"]
["离散变量备用28","ns=6;s=PUBLIC_BY_BOOL_28"]
["离散变量备用29","ns=6;s=PUBLIC_BY_BOOL_29"]
["离散变量备用30","ns=6;s=PUBLIC_BY_BOOL_30"]
["离散变量备用31","ns=6;s=PUBLIC_BY_BOOL_31"]
["离散变量备用32","ns=6;s=PUBLIC_BY_BOOL_32"]
["UF2 PID频率输出","ns=3;s=PUBLIC_2#UF_FXB_PID"]
["2号垢剂泵切换","ns=3;s=PUBLIC_BYZGJB_QH"]
["RO_回用水泵频率PID输出","ns=3;s=PUBLIC_RO_HYSB_PID_S"]
["RO_手动输入运行数量","ns=3;s=PUBLIC_RO_MAN_SETNUM"]
["RO1_段间泵频率PID输出","ns=3;s=PUBLIC_RO1_DJB_PID_S"]
["RO1_高压泵频率PID输出","ns=3;s=PUBLIC_RO1_GYB_PID_S"]
["RO1膜通量","ns=3;s=PUBLIC_RO1_MTL"]
["RO2_段间泵频率PID输出","ns=3;s=PUBLIC_RO2_DJB_PID_S"]
["RO2_高压泵频率PID输出","ns=3;s=PUBLIC_RO2_GYB_PID_S"]
["RO2膜通量","ns=3;s=PUBLIC_RO2_MTL"]
["RO反洗泵定频OUT","ns=3;s=PUBLIC_RO_FXB_FRE_S"]
["RO反洗泵频率设定[0]","ns=3;s=PUBLIC_RO_FXB_FRE_0"]
["RO反洗泵频率设定[1]","ns=3;s=PUBLIC_RO_FXB_FRE_1"]
["RO反洗泵频率设定[2]","ns=3;s=PUBLIC_RO_FXB_FRE_2"]
["RO反洗泵频率设定[3]","ns=3;s=PUBLIC_RO_FXB_FRE_3"]
["RO反洗泵频率设定[4]","ns=3;s=PUBLIC_RO_FXB_FRE_4"]
["RO反洗泵频率设定[5]","ns=3;s=PUBLIC_RO_FXB_FRE_5"]
["RO反洗泵频率设定[6]","ns=3;s=PUBLIC_RO_FXB_FRE_6"]
["RO反洗泵频率设定[7]","ns=3;s=PUBLIC_RO_FXB_FRE_7"]
["RO反洗泵频率设定[8]","ns=3;s=PUBLIC_RO_FXB_FRE_8"]
["RO反洗泵频率设定[9]","ns=3;s=PUBLIC_RO_FXB_FRE_9"]
["RO供水泵定频OUT","ns=3;s=PUBLIC_RO_GSB_FRE_S"]
["RO供水泵频率设定[0]","ns=3;s=PUBLIC_RO_GSB_FRE_0"]
["RO供水泵频率设定[1]","ns=3;s=PUBLIC_RO_GSB_FRE_1"]
["RO供水泵频率设定[2]","ns=3;s=PUBLIC_RO_GSB_FRE_2"]
["RO供水泵频率设定[3]","ns=3;s=PUBLIC_RO_GSB_FRE_3"]
["RO供水泵频率设定[4]","ns=3;s=PUBLIC_RO_GSB_FRE_4"]
["RO供水泵频率设定[5]","ns=3;s=PUBLIC_RO_GSB_FRE_5"]
["RO供水泵频率设定[6]","ns=3;s=PUBLIC_RO_GSB_FRE_6"]
["RO供水泵频率设定[7]","ns=3;s=PUBLIC_RO_GSB_FRE_7"]
["RO供水泵频率设定[8]","ns=3;s=PUBLIC_RO_GSB_FRE_8"]
["RO供水泵频率设定[9]","ns=3;s=PUBLIC_RO_GSB_FRE_9"]
["RO回用水泵恒压值SP","ns=3;s=PUBLIC_RO_HYSB_SP"]
["RO回用水泵频率设定[0]","ns=3;s=PUBLIC_RO_HYSB_FRE_0"]
["RO回用水泵频率设定[1]","ns=3;s=PUBLIC_RO_HYSB_FRE_1"]
["RO回用水泵频率设定[2]","ns=3;s=PUBLIC_RO_HYSB_FRE_2"]
["RO回用水泵频率设定[3]","ns=3;s=PUBLIC_RO_HYSB_FRE_3"]
["UF1 PID频率输出","ns=3;s=PUBLIC_1#UF_FXB_PID"]
["UF手动输入运行数量","ns=3;s=PUBLIC_UF_MAN_SETNUM"]
["UF1调节阀PID开度","ns=3;s=PUBLIC_UF1_TJV_PID_O"]
["UF1冲水排气调节阀开度set","ns=3;s=PUBLIC_UF1TJFCSPQSET"]
["UF1过滤起始调节阀PID开度set","ns=3;s=PUBLIC_UF1TJFGLSET"]
["UF2调节阀PID开度","ns=3;s=PUBLIC_UF2_TJV_PID_O"]
["UF2冲水排气调节阀开度set","ns=3;s=PUBLIC_UF2TJFCSPQSET"]
["UF2过滤起始调节阀PID开度set","ns=3;s=PUBLIC_UF2TJFGLSET"]
["UF反洗泵流量SP","ns=3;s=PUBLIC_UF_FXB_LL_S"]
["UF反洗泵频率设定[0]","ns=3;s=PUBLIC_UF_FXB_FRE_0"]
["UF反洗泵频率设定[1]","ns=3;s=PUBLIC_UF_FXB_FRE_1"]
["UF反洗泵频率设定[2]","ns=3;s=PUBLIC_UF_FXB_FRE_2"]
["UF反洗泵频率设定[3]","ns=3;s=PUBLIC_UF_FXB_FRE_3"]
["UF反洗泵频率设定[4]","ns=3;s=PUBLIC_UF_FXB_FRE_4"]
["UF反洗泵频率设定[5]","ns=3;s=PUBLIC_UF_FXB_FRE_5"]
["UF反洗泵频率设定[6]","ns=3;s=PUBLIC_UF_FXB_FRE_6"]
["UF反洗泵频率设定[7]","ns=3;s=PUBLIC_UF_FXB_FRE_7"]
["UF反洗泵频率设定[8]","ns=3;s=PUBLIC_UF_FXB_FRE_8"]
["UF反洗泵频率设定[9]","ns=3;s=PUBLIC_UF_FXB_FRE_9"]
["UF反洗泵频率OUT","ns=3;s=PUBLIC_UF_FXB_FRE_S"]
["UF供水泵频率设定[0]","ns=3;s=PUBLIC_UF_GSB_FRE_0"]
["UF供水泵频率设定[1]","ns=3;s=PUBLIC_UF_GSB_FRE_1"]
["UF供水泵频率设定[2]","ns=3;s=PUBLIC_UF_GSB_FRE_2"]
["UF供水泵频率设定[3]","ns=3;s=PUBLIC_UF_GSB_FRE_3"]
["UF供水泵频率设定[4]","ns=3;s=PUBLIC_UF_GSB_FRE_4"]
["UF供水泵频率设定[5]","ns=3;s=PUBLIC_UF_GSB_FRE_5"]
["UF供水泵频率设定[6]","ns=3;s=PUBLIC_UF_GSB_FRE_6"]
["UF供水泵频率设定[7]","ns=3;s=PUBLIC_UF_GSB_FRE_7"]
["UF供水泵频率设定[8]","ns=3;s=PUBLIC_UF_GSB_FRE_8"]
["UF供水泵频率设定[9]","ns=3;s=PUBLIC_UF_GSB_FRE_9"]
["UF供水泵频率OUT","ns=3;s=PUBLIC_UF_GSB_FRE_S"]
["RO1三段压差","ns=3;s=PUBLIC_BY_REAL_1"]
["RO2三段压差","ns=3;s=PUBLIC_BY_REAL_2"]
["实数变量备用3","ns=3;s=PUBLIC_BY_REAL_3"]
["实数变量备用4","ns=3;s=PUBLIC_BY_REAL_4"]
["实数变量备用5","ns=3;s=PUBLIC_BY_REAL_5"]
["实数变量备用6","ns=3;s=PUBLIC_BY_REAL_6"]
["实数变量备用7","ns=3;s=PUBLIC_BY_REAL_7"]
["实数变量备用8","ns=3;s=PUBLIC_BY_REAL_8"]
["实数变量备用9","ns=3;s=PUBLIC_BY_REAL_9"]
["实数变量备用10","ns=3;s=PUBLIC_BY_REAL_10"]
["实数变量备用11","ns=3;s=PUBLIC_BY_REAL_11"]
["实数变量备用12","ns=3;s=PUBLIC_BY_REAL_12"]
["实数变量备用13","ns=3;s=PUBLIC_BY_REAL_13"]
["实数变量备用14","ns=3;s=PUBLIC_BY_REAL_14"]
["实数变量备用15","ns=3;s=PUBLIC_BY_REAL_15"]
["实数变量备用16","ns=3;s=PUBLIC_BY_REAL_16"]
["实数变量备用17","ns=3;s=PUBLIC_BY_REAL_17"]
["实数变量备用18","ns=3;s=PUBLIC_BY_REAL_18"]
["实数变量备用19","ns=3;s=PUBLIC_BY_REAL_19"]
["实数变量备用20","ns=3;s=PUBLIC_BY_REAL_20"]
["实数变量备用21","ns=3;s=PUBLIC_BY_REAL_21"]
["实数变量备用22","ns=3;s=PUBLIC_BY_REAL_22"]
["实数变量备用23","ns=3;s=PUBLIC_BY_REAL_23"]
["实数变量备用24","ns=3;s=PUBLIC_BY_REAL_24"]
["实数变量备用25","ns=3;s=PUBLIC_BY_REAL_25"]
["实数变量备用26","ns=3;s=PUBLIC_BY_REAL_26"]
["实数变量备用27","ns=3;s=PUBLIC_BY_REAL_27"]
["实数变量备用28","ns=3;s=PUBLIC_BY_REAL_28"]
["实数变量备用29","ns=3;s=PUBLIC_BY_REAL_29"]
["实数变量备用30","ns=3;s=PUBLIC_BY_REAL_30"]
["实数变量备用31","ns=3;s=PUBLIC_BY_REAL_31"]
["实数变量备用32","ns=3;s=PUBLIC_BY_REAL_32"]
["反渗透外供泵功率因数","ns=3;s=ZZ_ROWGB_COSΘ"]
["反渗透外供泵正向有功电能","ns=3;s=ZZ_ROWGB_EP"]
["反渗透外供泵相电流Ia","ns=3;s=ZZ_ROWGB_IA"]
["反渗透外供泵相电流Ib","ns=3;s=ZZ_ROWGB_IB"]
["反渗透外供泵相电流Ic","ns=3;s=ZZ_ROWGB_IC"]
["反渗透外供泵总功率","ns=3;s=ZZ_ROWGB_POWER"]
["反渗透外供泵相电压Ua","ns=3;s=ZZ_ROWGB_UA"]
["反渗透外供泵相电压Ub","ns=3;s=ZZ_ROWGB_UB"]
["反渗透外供泵相电压Uc","ns=3;s=ZZ_ROWGB_UC"]
["1#RO段间泵功率因数","ns=3;s=ZZ_1#RODJB_COSΘ"]
["1#RO段间泵正向有功电能","ns=3;s=ZZ_1#RODJB_EP"]
["1#RO段间泵相电流Ia","ns=3;s=ZZ_1#RODJB_IA"]
["1#RO段间泵相电流Ib","ns=3;s=ZZ_1#RODJB_IB"]
["1#RO段间泵相电流Ic","ns=3;s=ZZ_1#RODJB_IC"]
["1#RO段间泵总功率","ns=3;s=ZZ_1#RODJB_POWER"]
["1#RO段间泵相电压Ua","ns=3;s=ZZ_1#RODJB_UA"]
["1#RO段间泵相电压Ub","ns=3;s=ZZ_1#RODJB_UB"]
["1#RO段间泵相电压Uc","ns=3;s=ZZ_1#RODJB_UC"]
["1#RO高压泵功率因数","ns=3;s=ZZ_1#ROGYB_COSΘ"]
["1#RO高压泵正向有功电能","ns=3;s=ZZ_1#ROGYB_EP"]
["1#RO高压泵相电流Ia","ns=3;s=ZZ_1#ROGYB_IA"]
["1#RO高压泵相电流Ib","ns=3;s=ZZ_1#ROGYB_IB"]
["1#RO高压泵相电流Ic","ns=3;s=ZZ_1#ROGYB_IC"]
["1#RO高压泵总功率","ns=3;s=ZZ_1#ROGYB_POWER"]
["1#RO高压泵相电压Ua","ns=3;s=ZZ_1#ROGYB_UA"]
["1#RO高压泵相电压Ub","ns=3;s=ZZ_1#ROGYB_UB"]
["1#RO高压泵相电压Uc","ns=3;s=ZZ_1#ROGYB_UC"]
["1#UF反洗泵功率因数","ns=3;s=ZZ_1#UFBWB_COSΘ"]
["1#UF反洗泵正向有功电能","ns=3;s=ZZ_1#UFBWB_EP"]
["1#UF反洗泵相电流Ia","ns=3;s=ZZ_1#UFBWB_IA"]
["1#UF反洗泵相电流Ib","ns=3;s=ZZ_1#UFBWB_IB"]
["1#UF反洗泵相电流Ic","ns=3;s=ZZ_1#UFBWB_IC"]
["1#UF反洗泵总功率","ns=3;s=ZZ_1#UFBWB_POWER"]
["1#UF反洗泵相电压Ua","ns=3;s=ZZ_1#UFBWB_UA"]
["1#UF反洗泵相电压Ub","ns=3;s=ZZ_1#UFBWB_UB"]
["1#UF反洗泵相电压Uc","ns=3;s=ZZ_1#UFBWB_UC"]
["大流量冲洗泵功率因数","ns=3;s=ZZ_DLLCXB_COSΘ"]
["大流量冲洗泵正向有功电能","ns=3;s=ZZ_DLLCXB_EP"]
["大流量冲洗泵相电流Ia","ns=3;s=ZZ_DLLCXB_IA"]
["大流量冲洗泵相电流Ib","ns=3;s=ZZ_DLLCXB_IB"]
["大流量冲洗泵相电流Ic","ns=3;s=ZZ_DLLCXB_IC"]
["大流量冲洗泵总功率","ns=3;s=ZZ_DLLCXB_POWER"]
["大流量冲洗泵相电压Ua","ns=3;s=ZZ_DLLCXB_UA"]
["大流量冲洗泵相电压Ub","ns=3;s=ZZ_DLLCXB_UB"]
["大流量冲洗泵相电压Uc","ns=3;s=ZZ_DLLCXB_UC"]
["2#RO段间泵功率因数","ns=3;s=ZZ_2#RODJB_COSΘ"]
["2#RO段间泵正向有功电能","ns=3;s=ZZ_2#RODJB_EP"]
["2#RO段间泵相电流Ia","ns=3;s=ZZ_2#RODJB_IA"]
["2#RO段间泵相电流Ib","ns=3;s=ZZ_2#RODJB_IB"]
["2#RO段间泵相电流Ic","ns=3;s=ZZ_2#RODJB_IC"]
["2#RO段间泵总功率","ns=3;s=ZZ_2#RODJB_POWER"]
["2#RO段间泵相电压Ua","ns=3;s=ZZ_2#RODJB_UA"]
["2#RO段间泵相电压Ub","ns=3;s=ZZ_2#RODJB_UB"]
["2#RO段间泵相电压Uc","ns=3;s=ZZ_2#RODJB_UC"]
["2#RO高压泵功率因数","ns=3;s=ZZ_2#ROGYB_COSΘ"]
["2#RO高压泵正向有功电能","ns=3;s=ZZ_2#ROGYB_EP"]
["2#RO高压泵相电流Ia","ns=3;s=ZZ_2#ROGYB_IA"]
["2#RO高压泵相电流Ib","ns=3;s=ZZ_2#ROGYB_IB"]
["2#RO高压泵相电流Ic","ns=3;s=ZZ_2#ROGYB_IC"]
["2#RO高压泵总功率","ns=3;s=ZZ_2#ROGYB_POWER"]
["2#RO高压泵相电压Ua","ns=3;s=ZZ_2#ROGYB_UA"]
["2#RO高压泵相电压Ub","ns=3;s=ZZ_2#ROGYB_UB"]
["2#RO高压泵相电压Uc","ns=3;s=ZZ_2#ROGYB_UC"]
["2#UF反洗泵功率因数","ns=3;s=ZZ_2#UFBWB_COSΘ"]
["2#UF反洗泵正向有功电能","ns=3;s=ZZ_2#UFBWB_EP"]
["2#UF反洗泵相电流Ia","ns=3;s=ZZ_2#UFBWB_IA"]
["2#UF反洗泵相电流Ib","ns=3;s=ZZ_2#UFBWB_IB"]
["2#UF反洗泵相电流Ic","ns=3;s=ZZ_2#UFBWB_IC"]
["2#UF反洗泵总功率","ns=3;s=ZZ_2#UFBWB_POWER"]
["2#UF反洗泵相电压Ua","ns=3;s=ZZ_2#UFBWB_UA"]
["2#UF反洗泵相电压Ub","ns=3;s=ZZ_2#UFBWB_UB"]
["2#UF反洗泵相电压Uc","ns=3;s=ZZ_2#UFBWB_UC"]
["泵房柜总进线功率因数","ns=3;s=ZZ_BFGZJX_COSΘ"]
["泵房柜总进线正向有功电能","ns=3;s=ZZ_BFGZJX_EP"]
["泵房柜总进线相电流Ia","ns=3;s=ZZ_BFGZJX_IA"]
["泵房柜总进线相电流Ib","ns=3;s=ZZ_BFGZJX_IB"]
["泵房柜总进线相电流Ic","ns=3;s=ZZ_BFGZJX_IC"]
["泵房柜总进线总功率","ns=3;s=ZZ_BFGZJX_POWER"]
["泵房柜总进线相电压Ua","ns=3;s=ZZ_BFGZJX_UA"]
["泵房柜总进线相电压Ub","ns=3;s=ZZ_BFGZJX_UB"]
["泵房柜总进线相电压Uc","ns=3;s=ZZ_BFGZJX_UC"]
["超滤柜总进线功率因数","ns=3;s=ZZ_UFGZJX_COSΘ"]
["超滤柜总进线正向有功电能","ns=3;s=ZZ_UFGZJX_EP"]
["超滤柜总进线相电流Ia","ns=3;s=ZZ_UFGZJX_IA"]
["超滤柜总进线相电流Ib","ns=3;s=ZZ_UFGZJX_IB"]
["超滤柜总进线相电流Ic","ns=3;s=ZZ_UFGZJX_IC"]
["超滤柜总进线总功率","ns=3;s=ZZ_UFGZJX_POWER"]
["超滤柜总进线相电压Ua","ns=3;s=ZZ_UFGZJX_UA"]
["超滤柜总进线相电压Ub","ns=3;s=ZZ_UFGZJX_UB"]
["超滤柜总进线相电压Uc","ns=3;s=ZZ_UFGZJX_UC"]
["2#反渗透柜总进线功率因数","ns=3;s=ZZ_2#ROGZJX_COSΘ"]
["2#反渗透柜总进线正向有功电能","ns=3;s=ZZ_2#ROGZJX_EP"]
["2#反渗透柜总进线相电流Ia","ns=3;s=ZZ_2#ROGZJX_IA"]
["2#反渗透柜总进线相电流Ib","ns=3;s=ZZ_2#ROGZJX_IB"]
["2#反渗透柜总进线相电流Ic","ns=3;s=ZZ_2#ROGZJX_IC"]
["2#反渗透柜总进线总功率","ns=3;s=ZZ_2#ROGZJX_POWER"]
["2#反渗透柜总进线相电压Ua","ns=3;s=ZZ_2#ROGZJX_UA"]
["2#反渗透柜总进线相电压Ub","ns=3;s=ZZ_2#ROGZJX_UB"]
["2#反渗透柜总进线相电压Uc","ns=3;s=ZZ_2#ROGZJX_UC"]
["废水排放泵功率因数","ns=3;s=ZZ_FSPFB_COSΘ"]
["废水排放泵正向有功电能","ns=3;s=ZZ_FSPFB_EP"]
["废水排放泵相电流Ia","ns=3;s=ZZ_FSPFB_IA"]
["废水排放泵相电流Ib","ns=3;s=ZZ_FSPFB_IB"]
["废水排放泵相电流Ic","ns=3;s=ZZ_FSPFB_IC"]
["废水排放泵总功率","ns=3;s=ZZ_FSPFB_POWER"]
["废水排放泵相电压Ua","ns=3;s=ZZ_FSPFB_UA"]
["废水排放泵相电压Ub","ns=3;s=ZZ_FSPFB_UB"]
["废水排放泵相电压Uc","ns=3;s=ZZ_FSPFB_UC"]
["加药柜总进线功率因数","ns=3;s=ZZ_JYGZJX_COSΘ"]
["加药柜总进线正向有功电能","ns=3;s=ZZ_JYGZJX_EP"]
["加药柜总进线相电流Ia","ns=3;s=ZZ_JYGZJX_IA"]
["加药柜总进线相电流Ib","ns=3;s=ZZ_JYGZJX_IB"]
["加药柜总进线相电流Ic","ns=3;s=ZZ_JYGZJX_IC"]
["加药柜总进线总功率","ns=3;s=ZZ_JYGZJX_POWER"]
["加药柜总进线相电压Ua","ns=3;s=ZZ_JYGZJX_UA"]
["加药柜总进线相电压Ub","ns=3;s=ZZ_JYGZJX_UB"]
["加药柜总进线相电压Uc","ns=3;s=ZZ_JYGZJX_UC"]
["1#反渗透柜总进线功率因数","ns=3;s=ZZ_1#ROGZJX_COSΘ"]
["1#反渗透柜总进线正向有功电能","ns=3;s=ZZ_1#ROGZJX_EP"]
["1#反渗透柜总进线相电流Ia","ns=3;s=ZZ_1#ROGZJX_IA"]
["1#反渗透柜总进线相电流Ib","ns=3;s=ZZ_1#ROGZJX_IB"]
["1#反渗透柜总进线相电流Ic","ns=3;s=ZZ_1#ROGZJX_IC"]
["1#反渗透柜总进线总功率","ns=3;s=ZZ_1#ROGZJX_POWER"]
["1#反渗透柜总进线相电压Ua","ns=3;s=ZZ_1#ROGZJX_UA"]
["1#反渗透柜总进线相电压Ub","ns=3;s=ZZ_1#ROGZJX_UB"]
["1#反渗透柜总进线相电压Uc","ns=3;s=ZZ_1#ROGZJX_UC"]
["1#照明模块第一路","ns=3;s=ZZ_MB_1#ZM1"]
["1#照明模块第二路","ns=3;s=ZZ_MB_1#ZM2"]
["1#照明模块第三路","ns=3;s=ZZ_MB_1#ZM3"]
["1#照明模块第四路","ns=3;s=ZZ_MB_1#ZM4"]
["1#照明模块第五路","ns=3;s=ZZ_MB_1#ZM5"]
["1#照明模块第六路","ns=3;s=ZZ_MB_1#ZM6"]
["2#照明模块第一路","ns=3;s=ZZ_MB_2#ZM1"]
["2#照明模块第二路","ns=3;s=ZZ_MB_2#ZM2"]
["2#照明模块第三路","ns=3;s=ZZ_MB_2#ZM3"]
["2#照明模块第四路","ns=3;s=ZZ_MB_2#ZM4"]
["2#照明模块第五路","ns=3;s=ZZ_MB_2#ZM5"]
["2#照明模块第六路","ns=3;s=ZZ_MB_2#ZM6"]
["3#照明模块第一路","ns=3;s=ZZ_MB_3#ZM1"]
["3#照明模块第二路","ns=3;s=ZZ_MB_3#ZM2"]
["3#照明模块第三路","ns=3;s=ZZ_MB_3#ZM3"]
["3#照明模块第四路","ns=3;s=ZZ_MB_3#ZM4"]
["3#照明模块第五路","ns=3;s=ZZ_MB_3#ZM5"]
["3#照明模块第六路","ns=3;s=ZZ_MB_3#ZM6"]
["4#照明模块第一路","ns=3;s=ZZ_MB_4#ZM1"]
["4#照明模块第二路","ns=3;s=ZZ_MB_4#ZM2"]
["4#照明模块第三路","ns=3;s=ZZ_MB_4#ZM3"]
["4#照明模块第四路","ns=3;s=ZZ_MB_4#ZM4"]
["4#照明模块第五路","ns=3;s=ZZ_MB_4#ZM5"]
["4#照明模块第六路","ns=3;s=ZZ_MB_4#ZM6"]
["湿度9#","ns=3;s=ZZ_MB_SD9"]
["温度9#","ns=3;s=ZZ_MB_WD9"]
["湿度4#","ns=3;s=ZZ_MB_SD4"]
["温度4#","ns=3;s=ZZ_MB_WD4"]
["湿度10#","ns=3;s=ZZ_MB_SD10"]
["温度10#","ns=3;s=ZZ_MB_WD10"]
["烟感9#","ns=3;s=ZZ_MB_YG9"]
["烟感4#","ns=3;s=ZZ_MB_YG4"]
["烟感10#","ns=3;s=ZZ_MB_YG10"]
["湿度11#","ns=3;s=ZZ_MB_SD11"]
["温度11#","ns=3;s=ZZ_MB_WD11"]
["湿度5#","ns=3;s=ZZ_MB_SD5"]
["温度5#","ns=3;s=ZZ_MB_WD5"]
["烟感11#","ns=3;s=ZZ_MB_YG11"]
["烟感5#","ns=3;s=ZZ_MB_YG5"]
["RO供水泵功率因数","ns=3;s=ZZ_ROGSB_COSΘ"]
["RO供水泵正向有功电能","ns=3;s=ZZ_ROGSB_EP"]
["RO供水泵相电流Ia","ns=3;s=ZZ_ROGSB_IA"]
["RO供水泵相电流Ib","ns=3;s=ZZ_ROGSB_IB"]
["RO供水泵相电流Ic","ns=3;s=ZZ_ROGSB_IC"]
["RO供水泵总功率","ns=3;s=ZZ_ROGSB_POWER"]
["RO供水泵相电压Ua","ns=3;s=ZZ_ROGSB_UA"]
["RO供水泵相电压Ub","ns=3;s=ZZ_ROGSB_UB"]
["RO供水泵相电压Uc","ns=3;s=ZZ_ROGSB_UC"]
["UF供水泵功率因数","ns=3;s=ZZ_UFGSB_COSΘ"]
["UF供水泵正向有功电能","ns=3;s=ZZ_UFGSB_EP"]
["UF供水泵相电流Ia","ns=3;s=ZZ_UFGSB_IA"]
["UF供水泵相电流Ib","ns=3;s=ZZ_UFGSB_IB"]
["UF供水泵相电流Ic","ns=3;s=ZZ_UFGSB_IC"]
["UF供水泵总功率","ns=3;s=ZZ_UFGSB_POWER"]
["UF供水泵相电压Ua","ns=3;s=ZZ_UFGSB_UA"]
["UF供水泵相电压Ub","ns=3;s=ZZ_UFGSB_UB"]
["UF供水泵相电压Uc","ns=3;s=ZZ_UFGSB_UC"]
["中和废水泵功率因数","ns=3;s=ZZ_ZHFSB_COSΘ"]
["中和废水泵正向有功电能","ns=3;s=ZZ_ZHFSB_EP"]
["中和废水泵相电流Ia","ns=3;s=ZZ_ZHFSB_IA"]
["中和废水泵相电流Ib","ns=3;s=ZZ_ZHFSB_IB"]
["中和废水泵相电流Ic","ns=3;s=ZZ_ZHFSB_IC"]
["中和废水泵总功率","ns=3;s=ZZ_ZHFSB_POWER"]
["中和废水泵相电压Ua","ns=3;s=ZZ_ZHFSB_UA"]
["中和废水泵相电压Ub","ns=3;s=ZZ_ZHFSB_UB"]
["中和废水泵相电压Uc","ns=3;s=ZZ_ZHFSB_UC"]
["RO1三段压差设定","ns=3;s=RO1_EX_3DYACHASET"]
["RO1三段压差读取","ns=3;s=RO1_EX_3DYCREAD"]
["RO1压力设置HH1","ns=3;s=RO1_EX_DPT1_HHR"]
["RO1压力设置HH2","ns=3;s=RO1_EX_DPT2_HHR"]
["RO1压力设置HH3","ns=3;s=RO1_EX_DPT3_HHR"]
["RO1一段进水压力设置","ns=3;s=RO1_EX_PRESSHHR_11"]
["RO1一段浓水压力设置","ns=3;s=RO1_EX_PRESSHHR_12"]
["RO1二段压力设定","ns=3;s=RO1_EX_PRESSHHR_22"]
["RO1三段进水压力设定","ns=3;s=RO1_EX_PRESSHHR_31"]
["RO1三段浓水压力设定","ns=3;s=RO1_EX_PRESSHHR_32"]
["RO1产水压力设定","ns=3;s=RO1_EX_PRESSHHR_CS"]
["RO1实数备用1","ns=3;s=RO1_EX_ZBY_R8"]
["RO1实数备用2","ns=3;s=RO1_EX_ZBY_R9"]
["RO1过滤停机不冲洗时间设定","ns=3;s=RO1_EX2_TJBCX_TIME"]
["RO1过滤停机冲23段洗时间设定","ns=3;s=RO1_EX2_TJC23D_TIME"]
["RO1停机整体冲洗时间设定","ns=3;s=RO1_EX2_TJZTCS_TIME"]
["RO1双整备用7","ns=3;s=RO1_EX2_ZBY_DINT10"]
["RO1双整备用1","ns=3;s=RO1_EX2_ZBY_DINT4"]
["RO1双整备用2","ns=3;s=RO1_EX2_ZBY_DINT5"]
["RO1双整备用3","ns=3;s=RO1_EX2_ZBY_DINT6"]
["RO1双整备用4","ns=3;s=RO1_EX2_ZBY_DINT7"]
["RO1双整备用5","ns=3;s=RO1_EX2_ZBY_DINT8"]
["RO1双整备用6","ns=3;s=RO1_EX2_ZBY_DINT9"]
["RO1实数备用EX21","ns=3;s=RO1_EX2_ZBY_R1"]
["RO1实数备用10","ns=3;s=RO1_EX2_ZBY_R10"]
["RO1实数备用EX22","ns=3;s=RO1_EX2_ZBY_R2"]
["RO1实数备用3","ns=3;s=RO1_EX2_ZBY_R3"]
["RO1实数备用4","ns=3;s=RO1_EX2_ZBY_R4"]
["RO1实数备用5","ns=3;s=RO1_EX2_ZBY_R5"]
["RO1实数备用6","ns=3;s=RO1_EX2_ZBY_R6"]
["RO1实数备用7","ns=3;s=RO1_EX2_ZBY_R7"]
["RO1实数备用8","ns=3;s=RO1_EX2_ZBY_R8"]
["RO1实数备用9","ns=3;s=RO1_EX2_ZBY_R9"]
["RO2三段压差设定","ns=3;s=RO2_EX_3DYACHASET"]
["RO2三段压差读取","ns=3;s=RO2_EX_3DYCREAD"]
["RO2压力设置HH1","ns=3;s=RO2_EX_DPT1_HHR"]
["RO2压力设置HH2","ns=3;s=RO2_EX_DPT2_HHR"]
["RO2压力设置HH3","ns=3;s=RO2_EX_DPT3_HHR"]
["RO2一段进水压力设置","ns=3;s=RO2_EX_PRESSHHR_11"]
["RO2一段浓水压力设置","ns=3;s=RO2_EX_PRESSHHR_12"]
["RO2二段压力设定","ns=3;s=RO2_EX_PRESSHHR_22"]
["RO2三段进水压力设定","ns=3;s=RO2_EX_PRESSHHR_31"]
["RO2三段浓水压力设定","ns=3;s=RO2_EX_PRESSHHR_32"]
["RO2产水压力设定","ns=3;s=RO2_EX_PRESSHHR_CS"]
["RO2实数备用1","ns=3;s=RO2_EX_ZBY_R8"]
["RO2实数备用2","ns=3;s=RO2_EX_ZBY_R9"]
["RO2过滤停机不冲洗时间设定","ns=3;s=RO2_EX2_TJBCX_TIME"]
["RO2过滤停机冲23段洗时间设定","ns=3;s=RO2_EX2_TJC23D_TIME"]
["RO2停机整体冲洗时间设定","ns=3;s=RO2_EX2_TJZTCS_TIME"]
["RO2双整备用7","ns=3;s=RO2_EX2_ZBY_DINT10"]
["RO2双整备用1","ns=3;s=RO2_EX2_ZBY_DINT4"]
["RO2双整备用2","ns=3;s=RO2_EX2_ZBY_DINT5"]
["RO2双整备用3","ns=3;s=RO2_EX2_ZBY_DINT6"]
["RO2双整备用4","ns=3;s=RO2_EX2_ZBY_DINT7"]
["RO2双整备用5","ns=3;s=RO2_EX2_ZBY_DINT8"]
["RO2双整备用6","ns=3;s=RO2_EX2_ZBY_DINT9"]
["RO2实数备用EX21","ns=3;s=RO2_EX2_ZBY_R1"]
["RO2实数备用10","ns=3;s=RO2_EX2_ZBY_R10"]
["RO2实数备用EX22","ns=3;s=RO2_EX2_ZBY_R2"]
["RO2实数备用3","ns=3;s=RO2_EX2_ZBY_R3"]
["RO2实数备用4","ns=3;s=RO2_EX2_ZBY_R4"]
["RO2实数备用5","ns=3;s=RO2_EX2_ZBY_R5"]
["RO2实数备用6","ns=3;s=RO2_EX2_ZBY_R6"]
["RO2实数备用7","ns=3;s=RO2_EX2_ZBY_R7"]
["RO2实数备用8","ns=3;s=RO2_EX2_ZBY_R8"]
["RO2实数备用9","ns=3;s=RO2_EX2_ZBY_R9"]
["RO产水池启动RO数量0","ns=3;s=YWLD_RO_CSC_LDUPNUM0"]
["RO产水池启动RO数量1","ns=3;s=YWLD_RO_CSC_LDUPNUM1"]
["RO产水池启动RO数量2","ns=3;s=YWLD_RO_CSC_LDUPNUM2"]
["RO产水池启动二套RO液位","ns=3;s=YWLD_RO_CSC_LDYWR[0]"]
["RO产水池启动一套RO液位","ns=3;s=YWLD_RO_CSC_LDYWR[1]"]
["RO产水池停止RO液位","ns=3;s=YWLD_RO_CSC_LDYWR[2]"]
["RO进水池启动数量0","ns=3;s=YWLD_RO_JSC_LDUPNUM0"]
["RO进水池启动RO数量1","ns=3;s=YWLD_RO_JSC_LDUPNUM1"]
["RO进水池启动RO数量2","ns=3;s=YWLD_RO_JSC_LDUPNUM2"]
["RO进水箱停RO液位","ns=3;s=YWLD_RO_JSC_LDYWR[0]"]
["RO进水箱启动一套RO液位","ns=3;s=YWLD_RO_JSC_LDYWR[1]"]
["RO进水箱启动二套RO液位","ns=3;s=YWLD_RO_JSC_LDYWR[2]"]
["RO冲洗不允许液位","ns=3;s=YWLD_ROCSC_BW_LLR"]
["RO冲洗允许液位","ns=3;s=YWLD_ROCSC_BW_LR"]
["RO产水池启动RO数量","ns=3;s=YWLD_SSDROCSCNEEDNUM"]
["RO进水池启动RO数量","ns=3;s=YWLD_SSDROJSCNEEDNUM"]
["RO联动液位自动启动数量","ns=3;s=YWLD_SSDRONEEDNUM_YW"]
["UF产水池启动UF数量","ns=3;s=YWLD_SSDUFCSCNEEDNUM"]
["UF进水池启动UF数量","ns=3;s=YWLD_SSDUFJSCNEEDNUM"]
["UF自动液位启动数量","ns=3;s=YWLD_SSDUFNEEDNUM_YW"]
["UF产水池启动UF数量0","ns=3;s=YWLD_UF_CSC_LDUPNUM0"]
["UF产水池启动UF数量1","ns=3;s=YWLD_UF_CSC_LDUPNUM1"]
["UF产水池启动UF数量2","ns=3;s=YWLD_UF_CSC_LDUPNUM2"]
["UF产水箱启两套UF液位","ns=3;s=YWLD_UF_CSC_LDYWR[0]"]
["UF产水箱启一套UF液位","ns=3;s=YWLD_UF_CSC_LDYWR[1]"]
["UF产水箱启零套UF液位","ns=3;s=YWLD_UF_CSC_LDYWR[2]"]
["UF进水池启动数量0","ns=3;s=YWLD_UF_JSC_LDUPNUM0"]
["UF进水池启动数量1","ns=3;s=YWLD_UF_JSC_LDUPNUM1"]
["UF进水池启动数量2","ns=3;s=YWLD_UF_JSC_LDUPNUM2"]
["UF进水池停UF液位","ns=3;s=YWLD_UF_JSC_LDYWR[0]"]
["UF进水池启动一套UF液位","ns=3;s=YWLD_UF_JSC_LDYWR[1]"]
["UF进水池启动二套UF液位","ns=3;s=YWLD_UF_JSC_LDYWR[2]"]
["BW不允许液位","ns=3;s=YWLD_UFCSC_BW_LLR"]
["BW允许液位","ns=3;s=YWLD_UFCSC_BW_LR"]
["CEB允许液位","ns=3;s=YWLD_UFCSC_CEB_ALLOW"]
["YWLD实数备用1","ns=3;s=YWLD_ZBYR1"]
["YWLD实数备用2","ns=3;s=YWLD_ZBYR2"]
["YWLD实数备用3","ns=3;s=YWLD_ZBYR3"]
["YWLD实数备用4","ns=3;s=YWLD_ZBYR4"]
["YWLD实数备用5","ns=3;s=YWLD_ZBYR5"]
["YWLD实数备用6","ns=3;s=YWLD_ZBYR6"]
["YWLD实数备用7","ns=3;s=YWLD_ZBYR7"]
["反洗水泵A震动温度","ns=3;s=ZZ_FXSB_A_ZD_WD"]
["反洗水泵A震动X轴速度","ns=3;s=ZZ_FXSB_A_ZD_XZSD"]
["反洗水泵A震动X轴位移","ns=3;s=ZZ_FXSB_A_ZD_XZWY"]
["反洗水泵A震动Y轴速度","ns=3;s=ZZ_FXSB_A_ZD_YZSD"]
["反洗水泵A震动Y轴位移","ns=3;s=ZZ_FXSB_A_ZD_YZWY"]
["反洗水泵A震动Z轴速度","ns=3;s=ZZ_FXSB_A_ZD_ZZSD"]
["反洗水泵A震动Z轴位移","ns=3;s=ZZ_FXSB_A_ZD_ZZWY"]
["反洗水泵B震动温度","ns=3;s=ZZ_FXSB_B_ZD_WD"]
["反洗水泵B震动X轴速度","ns=3;s=ZZ_FXSB_B_ZD_XZSD"]
["反洗水泵B震动X轴位移","ns=3;s=ZZ_FXSB_B_ZD_XZWY"]
["反洗水泵B震动Y轴速度","ns=3;s=ZZ_FXSB_B_ZD_YZSD"]
["反洗水泵B震动Y轴位移","ns=3;s=ZZ_FXSB_B_ZD_YZWY"]
["反洗水泵B震动Z轴速度","ns=3;s=ZZ_FXSB_B_ZD_ZZSD"]
["反洗水泵B震动Z轴位移","ns=3;s=ZZ_FXSB_B_ZD_ZZWY"]
["大流量冲洗泵震动温度","ns=3;s=ZZ_DLLCXB_ZD_WD"]
["大流量冲洗泵震动X轴速度","ns=3;s=ZZ_DLLCXB_ZD_XZSD"]
["大流量冲洗泵震动X轴位移","ns=3;s=ZZ_DLLCXB_ZD_XZWY"]
["大流量冲洗泵震动Y轴速度","ns=3;s=ZZ_DLLCXB_ZD_YZSD"]
["大流量冲洗泵震动Y轴位移","ns=3;s=ZZ_DLLCXB_ZD_YZWY"]
["大流量冲洗泵震动Z轴速度","ns=3;s=ZZ_DLLCXB_ZD_ZZSD"]
["大流量冲洗泵震动Z轴位移","ns=3;s=ZZ_DLLCXB_ZD_ZZWY"]
["超滤供水泵震动温度","ns=3;s=ZZ_UFGSB_ZD_WD"]
["超滤供水泵震动X轴速度","ns=3;s=ZZ_UFGSB_ZD_XZSD"]
["超滤供水泵震动X轴位移","ns=3;s=ZZ_UFGSB_ZD_XZWY"]
["超滤供水泵震动Y轴速度","ns=3;s=ZZ_UFGSB_ZD_YZSD"]
["超滤供水泵震动Y轴位移","ns=3;s=ZZ_UFGSB_ZD_YZWY"]
["超滤供水泵震动Z轴速度","ns=3;s=ZZ_UFGSB_ZD_ZZSD"]
["超滤供水泵震动Z轴位移","ns=3;s=ZZ_UFGSB_ZD_ZZWY"]
["RO供水泵震动温度","ns=3;s=ZZ_ROGSB_ZD_WD"]
["RO供水泵震动X轴速度","ns=3;s=ZZ_ROGSB_ZD_XZSD"]
["RO供水泵震动X轴位移","ns=3;s=ZZ_ROGSB_ZD_XZWY"]
["RO供水泵震动Y轴速度","ns=3;s=ZZ_ROGSB_ZD_YZSD"]
["RO供水泵震动Y轴位移","ns=3;s=ZZ_ROGSB_ZD_YZWY"]
["RO供水泵震动Z轴速度","ns=3;s=ZZ_ROGSB_ZD_ZZSD"]
["RO供水泵震动Z轴位移","ns=3;s=ZZ_ROGSB_ZD_ZZWY"]
["外供水泵震动温度","ns=3;s=ZZ_WGSB_ZD_WD"]
["外供水泵震动X轴速度","ns=3;s=ZZ_WGSB_ZD_XZSD"]
["外供水泵震动X轴位移","ns=3;s=ZZ_WGSB_ZD_XZWY"]
["外供水泵震动Y轴速度","ns=3;s=ZZ_WGSB_ZD_YZSD"]
["外供水泵震动Y轴位移","ns=3;s=ZZ_WGSB_ZD_YZWY"]
["外供水泵震动Z轴速度","ns=3;s=ZZ_WGSB_ZD_ZZSD"]
["外供水泵震动Z轴位移","ns=3;s=ZZ_WGSB_ZD_ZZWY"]
["RO1三段压差高","ns=6;s=RO1_EX_3DYCG"]
["RO1压差HH报警1","ns=6;s=RO1_EX_DPT1_HH"]
["RO1压差HH报警2","ns=6;s=RO1_EX_DPT2_HH"]
["RO1压差HH报警3","ns=6;s=RO1_EX_DPT3_HH"]
["RO1一段进水压力高","ns=6;s=RO1_EX_PRESSHH_11"]
["RO1一段浓水压力高","ns=6;s=RO1_EX_PRESSHH_12"]
["RO1二段压力高","ns=6;s=RO1_EX_PRESSHH_22"]
["RO1三段进水压力高","ns=6;s=RO1_EX_PRESSHH_31"]
["RO1三段浓水压力高","ns=6;s=RO1_EX_PRESSHH_32"]
["RO1产水压力高报警","ns=6;s=RO1_EX_PRESSHH_CS"]
["RO1备用1压力高报警","ns=6;s=RO1_EX_ZFLAG_BY11"]
["RO1备用2压力高报警","ns=6;s=RO1_EX_ZFLAG_BY12"]
["RO1备用3压力高报警","ns=6;s=RO1_EX_ZFLAG_BY13"]
["RO1备用4压力高报警","ns=6;s=RO1_EX_ZFLAG_BY14"]
["RO1备用5压力高报警","ns=6;s=RO1_EX_ZFLAG_BY15"]
["RO1_BT_半自动时停机按钮","ns=6;s=RO1_EX2_BT_BZDTJ"]
["RO1_备用4按钮","ns=6;s=RO1_EX2_BT_ZZBY12"]
["RO1_备用按钮5","ns=6;s=RO1_EX2_BT_ZZBY13"]
["RO1_备用按钮6","ns=6;s=RO1_EX2_BT_ZZBY14"]
["RO1_备用按钮7","ns=6;s=RO1_EX2_BT_ZZBY15"]
["RO1_备用按钮8","ns=6;s=RO1_EX2_BT_ZZBY16"]
["RO1_备用1按钮","ns=6;s=RO1_EX2_BT_ZZBY5"]
["RO1_备用2按钮","ns=6;s=RO1_EX2_BT_ZZBY6"]
["RO1_备用3按钮","ns=6;s=RO1_EX2_BT_ZZBY7"]
["RO1_冲洗申请","ns=6;s=RO1_EX2_CXSQ"]
["RO1_FLG_段间泵出口压力大","ns=6;s=RO1_EX2_DJBCKYLD"]
["RO1_FLG_高压泵出口压力大","ns=6;s=RO1_EX2_FLG_GYBCKYLD"]
["RO1_FLG_过滤停机不冲洗","ns=6;s=RO1_EX2_FLG_TJBCX"]
["RO1_FLG_过滤停机整体冲洗","ns=6;s=RO1_EX2_FLG_TJZTCX"]
["RO1_FLG_膜里有药","ns=6;s=RO1_EX2_MLYY"]
["RO1_FLG_过滤停机冲二三段","ns=6;s=RO1_EX2_TJC23D"]
["RO2三段压差高","ns=6;s=RO2_EX_3DYCG"]
["RO2压差HH报警1","ns=6;s=RO2_EX_DPT1_HH"]
["RO2压差HH报警2","ns=6;s=RO2_EX_DPT2_HH"]
["RO2压差HH报警3","ns=6;s=RO2_EX_DPT3_HH"]
["RO2一段进水压力高","ns=6;s=RO2_EX_PRESSHH_11"]
["RO2一段浓水压力高","ns=6;s=RO2_EX_PRESSHH_12"]
["RO2二段压力高","ns=6;s=RO2_EX_PRESSHH_22"]
["RO2三段进水压力高","ns=6;s=RO2_EX_PRESSHH_31"]
["RO2三段浓水压力高","ns=6;s=RO2_EX_PRESSHH_32"]
["RO2产水压力高报警","ns=6;s=RO2_EX_PRESSHH_CS"]
["RO2备用1压力高报警","ns=6;s=RO2_EX_ZFLAG_BY11"]
["RO2备用2压力高报警","ns=6;s=RO2_EX_ZFLAG_BY12"]
["RO2备用3压力高报警","ns=6;s=RO2_EX_ZFLAG_BY13"]
["RO2备用4压力高报警","ns=6;s=RO2_EX_ZFLAG_BY14"]
["RO2备用5压力高报警","ns=6;s=RO2_EX_ZFLAG_BY15"]
["RO2_BT_半自动时停机按钮","ns=6;s=RO2_EX2_BT_BZDTJ"]
["RO2_备用4按钮","ns=6;s=RO2_EX2_BT_ZZBY12"]
["RO2_备用按钮5","ns=6;s=RO2_EX2_BT_ZZBY13"]
["RO2_备用按钮6","ns=6;s=RO2_EX2_BT_ZZBY14"]
["RO2_备用按钮7","ns=6;s=RO2_EX2_BT_ZZBY15"]
["RO2_备用按钮8","ns=6;s=RO2_EX2_BT_ZZBY16"]
["RO2_备用1按钮","ns=6;s=RO2_EX2_BT_ZZBY5"]
["RO2_备用2按钮","ns=6;s=RO2_EX2_BT_ZZBY6"]
["RO2_备用3按钮","ns=6;s=RO2_EX2_BT_ZZBY7"]
["RO2_冲洗申请","ns=6;s=RO2_EX2_CXSQ"]
["RO2_FLG_段间泵出口压力大","ns=6;s=RO2_EX2_DJBCKYLD"]
["RO2_FLG_高压泵出口压力大","ns=6;s=RO2_EX2_FLG_GYBCKYLD"]
["RO2_FLG_过滤停机不冲洗","ns=6;s=RO2_EX2_FLG_TJBCX"]
["RO2_FLG_过滤停机整体冲洗","ns=6;s=RO2_EX2_FLG_TJZTCX"]
["RO2_FLG_膜里有药","ns=6;s=RO2_EX2_MLYY"]
["RO2_FLG_过滤停机冲二三段","ns=6;s=RO2_EX2_TJC23D"]
["加药间1噪音频率1","ns=3;s=ZZ_ZY_FR1"]
["加药间1噪音频率10","ns=3;s=ZZ_ZY_FR10"]
["加药间1噪音频率100","ns=3;s=ZZ_ZY_FR100"]
["加药间1噪音频率101","ns=3;s=ZZ_ZY_FR101"]
["加药间1噪音频率102","ns=3;s=ZZ_ZY_FR102"]
["加药间1噪音频率103","ns=3;s=ZZ_ZY_FR103"]
["加药间1噪音频率104","ns=3;s=ZZ_ZY_FR104"]
["加药间1噪音频率105","ns=3;s=ZZ_ZY_FR105"]
["加药间1噪音频率106","ns=3;s=ZZ_ZY_FR106"]
["加药间1噪音频率107","ns=3;s=ZZ_ZY_FR107"]
["加药间1噪音频率108","ns=3;s=ZZ_ZY_FR108"]
["加药间1噪音频率109","ns=3;s=ZZ_ZY_FR109"]
["加药间1噪音频率11","ns=3;s=ZZ_ZY_FR11"]
["加药间1噪音频率110","ns=3;s=ZZ_ZY_FR110"]
["加药间1噪音频率111","ns=3;s=ZZ_ZY_FR111"]
["加药间1噪音频率112","ns=3;s=ZZ_ZY_FR112"]
["加药间1噪音频率113","ns=3;s=ZZ_ZY_FR113"]
["加药间1噪音频率114","ns=3;s=ZZ_ZY_FR114"]
["加药间1噪音频率115","ns=3;s=ZZ_ZY_FR115"]
["加药间1噪音频率116","ns=3;s=ZZ_ZY_FR116"]
["加药间1噪音频率117","ns=3;s=ZZ_ZY_FR117"]
["加药间1噪音频率118","ns=3;s=ZZ_ZY_FR118"]
["加药间1噪音频率119","ns=3;s=ZZ_ZY_FR119"]
["加药间1噪音频率12","ns=3;s=ZZ_ZY_FR12"]
["加药间1噪音频率120","ns=3;s=ZZ_ZY_FR120"]
["加药间1噪音频率121","ns=3;s=ZZ_ZY_FR121"]
["加药间1噪音频率122","ns=3;s=ZZ_ZY_FR122"]
["加药间1噪音频率123","ns=3;s=ZZ_ZY_FR123"]
["加药间1噪音频率124","ns=3;s=ZZ_ZY_FR124"]
["加药间1噪音频率125","ns=3;s=ZZ_ZY_FR125"]
["加药间1噪音频率126","ns=3;s=ZZ_ZY_FR126"]
["加药间1噪音频率127","ns=3;s=ZZ_ZY_FR127"]
["加药间1噪音频率13","ns=3;s=ZZ_ZY_FR13"]
["加药间1噪音频率14","ns=3;s=ZZ_ZY_FR14"]
["加药间1噪音频率15","ns=3;s=ZZ_ZY_FR15"]
["加药间1噪音频率16","ns=3;s=ZZ_ZY_FR16"]
["加药间1噪音频率17","ns=3;s=ZZ_ZY_FR17"]
["加药间1噪音频率18","ns=3;s=ZZ_ZY_FR18"]
["加药间1噪音频率19","ns=3;s=ZZ_ZY_FR19"]
["加药间1噪音频率2","ns=3;s=ZZ_ZY_FR2"]
["加药间1噪音频率20","ns=3;s=ZZ_ZY_FR20"]
["加药间1噪音频率21","ns=3;s=ZZ_ZY_FR21"]
["加药间1噪音频率22","ns=3;s=ZZ_ZY_FR22"]
["加药间1噪音频率23","ns=3;s=ZZ_ZY_FR23"]
["加药间1噪音频率24","ns=3;s=ZZ_ZY_FR24"]
["加药间1噪音频率25","ns=3;s=ZZ_ZY_FR25"]
["加药间1噪音频率26","ns=3;s=ZZ_ZY_FR26"]
["加药间1噪音频率27","ns=3;s=ZZ_ZY_FR27"]
["加药间1噪音频率28","ns=3;s=ZZ_ZY_FR28"]
["加药间1噪音频率29","ns=3;s=ZZ_ZY_FR29"]
["加药间1噪音频率3","ns=3;s=ZZ_ZY_FR3"]
["加药间1噪音频率30","ns=3;s=ZZ_ZY_FR30"]
["加药间1噪音频率31","ns=3;s=ZZ_ZY_FR31"]
["加药间1噪音频率32","ns=3;s=ZZ_ZY_FR32"]
["加药间1噪音频率33","ns=3;s=ZZ_ZY_FR33"]
["加药间1噪音频率34","ns=3;s=ZZ_ZY_FR34"]
["加药间1噪音频率35","ns=3;s=ZZ_ZY_FR35"]
["加药间1噪音频率36","ns=3;s=ZZ_ZY_FR36"]
["加药间1噪音频率37","ns=3;s=ZZ_ZY_FR37"]
["加药间1噪音频率38","ns=3;s=ZZ_ZY_FR38"]
["加药间1噪音频率39","ns=3;s=ZZ_ZY_FR39"]
["加药间1噪音频率4","ns=3;s=ZZ_ZY_FR4"]
["加药间1噪音频率40","ns=3;s=ZZ_ZY_FR40"]
["加药间1噪音频率41","ns=3;s=ZZ_ZY_FR41"]
["加药间1噪音频率42","ns=3;s=ZZ_ZY_FR42"]
["加药间1噪音频率43","ns=3;s=ZZ_ZY_FR43"]
["加药间1噪音频率44","ns=3;s=ZZ_ZY_FR44"]
["加药间1噪音频率45","ns=3;s=ZZ_ZY_FR45"]
["加药间1噪音频率46","ns=3;s=ZZ_ZY_FR46"]
["加药间1噪音频率47","ns=3;s=ZZ_ZY_FR47"]
["加药间1噪音频率48","ns=3;s=ZZ_ZY_FR48"]
["加药间1噪音频率49","ns=3;s=ZZ_ZY_FR49"]
["加药间1噪音频率5","ns=3;s=ZZ_ZY_FR5"]
["加药间1噪音频率50","ns=3;s=ZZ_ZY_FR50"]
["加药间1噪音频率51","ns=3;s=ZZ_ZY_FR51"]
["加药间1噪音频率52","ns=3;s=ZZ_ZY_FR52"]
["加药间1噪音频率53","ns=3;s=ZZ_ZY_FR53"]
["加药间1噪音频率54","ns=3;s=ZZ_ZY_FR54"]
["加药间1噪音频率55","ns=3;s=ZZ_ZY_FR55"]
["加药间1噪音频率56","ns=3;s=ZZ_ZY_FR56"]
["加药间1噪音频率57","ns=3;s=ZZ_ZY_FR57"]
["加药间1噪音频率58","ns=3;s=ZZ_ZY_FR58"]
["加药间1噪音频率59","ns=3;s=ZZ_ZY_FR59"]
["加药间1噪音频率6","ns=3;s=ZZ_ZY_FR6"]
["加药间1噪音频率60","ns=3;s=ZZ_ZY_FR60"]
["加药间1噪音频率61","ns=3;s=ZZ_ZY_FR61"]
["加药间1噪音频率62","ns=3;s=ZZ_ZY_FR62"]
["加药间1噪音频率63","ns=3;s=ZZ_ZY_FR63"]
["加药间1噪音频率64","ns=3;s=ZZ_ZY_FR64"]
["加药间1噪音频率65","ns=3;s=ZZ_ZY_FR65"]
["加药间1噪音频率66","ns=3;s=ZZ_ZY_FR66"]
["加药间1噪音频率67","ns=3;s=ZZ_ZY_FR67"]
["加药间1噪音频率68","ns=3;s=ZZ_ZY_FR68"]
["加药间1噪音频率69","ns=3;s=ZZ_ZY_FR69"]
["加药间1噪音频率7","ns=3;s=ZZ_ZY_FR7"]
["加药间1噪音频率70","ns=3;s=ZZ_ZY_FR70"]
["加药间1噪音频率71","ns=3;s=ZZ_ZY_FR71"]
["加药间1噪音频率72","ns=3;s=ZZ_ZY_FR72"]
["加药间1噪音频率73","ns=3;s=ZZ_ZY_FR73"]
["加药间1噪音频率74","ns=3;s=ZZ_ZY_FR74"]
["加药间1噪音频率75","ns=3;s=ZZ_ZY_FR75"]
["加药间1噪音频率76","ns=3;s=ZZ_ZY_FR76"]
["加药间1噪音频率77","ns=3;s=ZZ_ZY_FR77"]
["加药间1噪音频率78","ns=3;s=ZZ_ZY_FR78"]
["加药间1噪音频率79","ns=3;s=ZZ_ZY_FR79"]
["加药间1噪音频率8","ns=3;s=ZZ_ZY_FR8"]
["加药间1噪音频率80","ns=3;s=ZZ_ZY_FR80"]
["加药间1噪音频率81","ns=3;s=ZZ_ZY_FR81"]
["加药间1噪音频率82","ns=3;s=ZZ_ZY_FR82"]
["加药间1噪音频率83","ns=3;s=ZZ_ZY_FR83"]
["加药间1噪音频率84","ns=3;s=ZZ_ZY_FR84"]
["加药间1噪音频率85","ns=3;s=ZZ_ZY_FR85"]
["加药间1噪音频率86","ns=3;s=ZZ_ZY_FR86"]
["加药间1噪音频率87","ns=3;s=ZZ_ZY_FR87"]
["加药间1噪音频率88","ns=3;s=ZZ_ZY_FR88"]
["加药间1噪音频率89","ns=3;s=ZZ_ZY_FR89"]
["加药间1噪音频率9","ns=3;s=ZZ_ZY_FR9"]
["加药间1噪音频率90","ns=3;s=ZZ_ZY_FR90"]
["加药间1噪音频率91","ns=3;s=ZZ_ZY_FR91"]
["加药间1噪音频率92","ns=3;s=ZZ_ZY_FR92"]
["加药间1噪音频率93","ns=3;s=ZZ_ZY_FR93"]
["加药间1噪音频率94","ns=3;s=ZZ_ZY_FR94"]
["加药间1噪音频率95","ns=3;s=ZZ_ZY_FR95"]
["加药间1噪音频率96","ns=3;s=ZZ_ZY_FR96"]
["加药间1噪音频率97","ns=3;s=ZZ_ZY_FR97"]
["加药间1噪音频率98","ns=3;s=ZZ_ZY_FR98"]
["加药间1噪音频率99","ns=3;s=ZZ_ZY_FR99"]
["加药间2噪音频率1","ns=3;s=ZZ_ZY2_FR1"]
["加药间2噪音频率10","ns=3;s=ZZ_ZY2_FR10"]
["加药间2噪音频率100","ns=3;s=ZZ_ZY2_FR100"]
["加药间2噪音频率101","ns=3;s=ZZ_ZY2_FR101"]
["加药间2噪音频率102","ns=3;s=ZZ_ZY2_FR102"]
["加药间2噪音频率103","ns=3;s=ZZ_ZY2_FR103"]
["加药间2噪音频率104","ns=3;s=ZZ_ZY2_FR104"]
["加药间2噪音频率105","ns=3;s=ZZ_ZY2_FR105"]
["加药间2噪音频率106","ns=3;s=ZZ_ZY2_FR106"]
["加药间2噪音频率107","ns=3;s=ZZ_ZY2_FR107"]
["加药间2噪音频率108","ns=3;s=ZZ_ZY2_FR108"]
["加药间2噪音频率109","ns=3;s=ZZ_ZY2_FR109"]
["加药间2噪音频率11","ns=3;s=ZZ_ZY2_FR11"]
["加药间2噪音频率110","ns=3;s=ZZ_ZY2_FR110"]
["加药间2噪音频率111","ns=3;s=ZZ_ZY2_FR111"]
["加药间2噪音频率112","ns=3;s=ZZ_ZY2_FR112"]
["加药间2噪音频率113","ns=3;s=ZZ_ZY2_FR113"]
["加药间2噪音频率114","ns=3;s=ZZ_ZY2_FR114"]
["加药间2噪音频率115","ns=3;s=ZZ_ZY2_FR115"]
["加药间2噪音频率116","ns=3;s=ZZ_ZY2_FR116"]
["加药间2噪音频率117","ns=3;s=ZZ_ZY2_FR117"]
["加药间2噪音频率118","ns=3;s=ZZ_ZY2_FR118"]
["加药间2噪音频率119","ns=3;s=ZZ_ZY2_FR119"]
["加药间2噪音频率12","ns=3;s=ZZ_ZY2_FR12"]
["加药间2噪音频率120","ns=3;s=ZZ_ZY2_FR120"]
["加药间2噪音频率121","ns=3;s=ZZ_ZY2_FR121"]
["加药间2噪音频率122","ns=3;s=ZZ_ZY2_FR122"]
["加药间2噪音频率123","ns=3;s=ZZ_ZY2_FR123"]
["加药间2噪音频率124","ns=3;s=ZZ_ZY2_FR124"]
["加药间2噪音频率125","ns=3;s=ZZ_ZY2_FR125"]
["加药间2噪音频率126","ns=3;s=ZZ_ZY2_FR126"]
["加药间2噪音频率127","ns=3;s=ZZ_ZY2_FR127"]
["加药间2噪音频率13","ns=3;s=ZZ_ZY2_FR13"]
["加药间2噪音频率14","ns=3;s=ZZ_ZY2_FR14"]
["加药间2噪音频率15","ns=3;s=ZZ_ZY2_FR15"]
["加药间2噪音频率16","ns=3;s=ZZ_ZY2_FR16"]
["加药间2噪音频率17","ns=3;s=ZZ_ZY2_FR17"]
["加药间2噪音频率18","ns=3;s=ZZ_ZY2_FR18"]
["加药间2噪音频率19","ns=3;s=ZZ_ZY2_FR19"]
["加药间2噪音频率2","ns=3;s=ZZ_ZY2_FR2"]
["加药间2噪音频率20","ns=3;s=ZZ_ZY2_FR20"]
["加药间2噪音频率21","ns=3;s=ZZ_ZY2_FR21"]
["加药间2噪音频率22","ns=3;s=ZZ_ZY2_FR22"]
["加药间2噪音频率23","ns=3;s=ZZ_ZY2_FR23"]
["加药间2噪音频率24","ns=3;s=ZZ_ZY2_FR24"]
["加药间2噪音频率25","ns=3;s=ZZ_ZY2_FR25"]
["加药间2噪音频率26","ns=3;s=ZZ_ZY2_FR26"]
["加药间2噪音频率27","ns=3;s=ZZ_ZY2_FR27"]
["加药间2噪音频率28","ns=3;s=ZZ_ZY2_FR28"]
["加药间2噪音频率29","ns=3;s=ZZ_ZY2_FR29"]
["加药间2噪音频率3","ns=3;s=ZZ_ZY2_FR3"]
["加药间2噪音频率30","ns=3;s=ZZ_ZY2_FR30"]
["加药间2噪音频率31","ns=3;s=ZZ_ZY2_FR31"]
["加药间2噪音频率32","ns=3;s=ZZ_ZY2_FR32"]
["加药间2噪音频率33","ns=3;s=ZZ_ZY2_FR33"]
["加药间2噪音频率34","ns=3;s=ZZ_ZY2_FR34"]
["加药间2噪音频率35","ns=3;s=ZZ_ZY2_FR35"]
["加药间2噪音频率36","ns=3;s=ZZ_ZY2_FR36"]
["加药间2噪音频率37","ns=3;s=ZZ_ZY2_FR37"]
["加药间2噪音频率38","ns=3;s=ZZ_ZY2_FR38"]
["加药间2噪音频率39","ns=3;s=ZZ_ZY2_FR39"]
["加药间2噪音频率4","ns=3;s=ZZ_ZY2_FR4"]
["加药间2噪音频率40","ns=3;s=ZZ_ZY2_FR40"]
["加药间2噪音频率41","ns=3;s=ZZ_ZY2_FR41"]
["加药间2噪音频率42","ns=3;s=ZZ_ZY2_FR42"]
["加药间2噪音频率43","ns=3;s=ZZ_ZY2_FR43"]
["加药间2噪音频率44","ns=3;s=ZZ_ZY2_FR44"]
["加药间2噪音频率45","ns=3;s=ZZ_ZY2_FR45"]
["加药间2噪音频率46","ns=3;s=ZZ_ZY2_FR46"]
["加药间2噪音频率47","ns=3;s=ZZ_ZY2_FR47"]
["加药间2噪音频率48","ns=3;s=ZZ_ZY2_FR48"]
["加药间2噪音频率49","ns=3;s=ZZ_ZY2_FR49"]
["加药间2噪音频率5","ns=3;s=ZZ_ZY2_FR5"]
["加药间2噪音频率50","ns=3;s=ZZ_ZY2_FR50"]
["加药间2噪音频率51","ns=3;s=ZZ_ZY2_FR51"]
["加药间2噪音频率52","ns=3;s=ZZ_ZY2_FR52"]
["加药间2噪音频率53","ns=3;s=ZZ_ZY2_FR53"]
["加药间2噪音频率54","ns=3;s=ZZ_ZY2_FR54"]
["加药间2噪音频率55","ns=3;s=ZZ_ZY2_FR55"]
["加药间2噪音频率56","ns=3;s=ZZ_ZY2_FR56"]
["加药间2噪音频率57","ns=3;s=ZZ_ZY2_FR57"]
["加药间2噪音频率58","ns=3;s=ZZ_ZY2_FR58"]
["加药间2噪音频率59","ns=3;s=ZZ_ZY2_FR59"]
["加药间2噪音频率6","ns=3;s=ZZ_ZY2_FR6"]
["加药间2噪音频率60","ns=3;s=ZZ_ZY2_FR60"]
["加药间2噪音频率61","ns=3;s=ZZ_ZY2_FR61"]
["加药间2噪音频率62","ns=3;s=ZZ_ZY2_FR62"]
["加药间2噪音频率63","ns=3;s=ZZ_ZY2_FR63"]
["加药间2噪音频率64","ns=3;s=ZZ_ZY2_FR64"]
["加药间2噪音频率65","ns=3;s=ZZ_ZY2_FR65"]
["加药间2噪音频率66","ns=3;s=ZZ_ZY2_FR66"]
["加药间2噪音频率67","ns=3;s=ZZ_ZY2_FR67"]
["加药间2噪音频率68","ns=3;s=ZZ_ZY2_FR68"]
["加药间2噪音频率69","ns=3;s=ZZ_ZY2_FR69"]
["加药间2噪音频率7","ns=3;s=ZZ_ZY2_FR7"]
["加药间2噪音频率70","ns=3;s=ZZ_ZY2_FR70"]
["加药间2噪音频率71","ns=3;s=ZZ_ZY2_FR71"]
["加药间2噪音频率72","ns=3;s=ZZ_ZY2_FR72"]
["加药间2噪音频率73","ns=3;s=ZZ_ZY2_FR73"]
["加药间2噪音频率74","ns=3;s=ZZ_ZY2_FR74"]
["加药间2噪音频率75","ns=3;s=ZZ_ZY2_FR75"]
["加药间2噪音频率76","ns=3;s=ZZ_ZY2_FR76"]
["加药间2噪音频率77","ns=3;s=ZZ_ZY2_FR77"]
["加药间2噪音频率78","ns=3;s=ZZ_ZY2_FR78"]
["加药间2噪音频率79","ns=3;s=ZZ_ZY2_FR79"]
["加药间2噪音频率8","ns=3;s=ZZ_ZY2_FR8"]
["加药间2噪音频率80","ns=3;s=ZZ_ZY2_FR80"]
["加药间2噪音频率81","ns=3;s=ZZ_ZY2_FR81"]
["加药间2噪音频率82","ns=3;s=ZZ_ZY2_FR82"]
["加药间2噪音频率83","ns=3;s=ZZ_ZY2_FR83"]
["加药间2噪音频率84","ns=3;s=ZZ_ZY2_FR84"]
["加药间2噪音频率85","ns=3;s=ZZ_ZY2_FR85"]
["加药间2噪音频率86","ns=3;s=ZZ_ZY2_FR86"]
["加药间2噪音频率87","ns=3;s=ZZ_ZY2_FR87"]
["加药间2噪音频率88","ns=3;s=ZZ_ZY2_FR88"]
["加药间2噪音频率89","ns=3;s=ZZ_ZY2_FR89"]
["加药间2噪音频率9","ns=3;s=ZZ_ZY2_FR9"]
["加药间2噪音频率90","ns=3;s=ZZ_ZY2_FR90"]
["加药间2噪音频率91","ns=3;s=ZZ_ZY2_FR91"]
["加药间2噪音频率92","ns=3;s=ZZ_ZY2_FR92"]
["加药间2噪音频率93","ns=3;s=ZZ_ZY2_FR93"]
["加药间2噪音频率94","ns=3;s=ZZ_ZY2_FR94"]
["加药间2噪音频率95","ns=3;s=ZZ_ZY2_FR95"]
["加药间2噪音频率96","ns=3;s=ZZ_ZY2_FR96"]
["加药间2噪音频率97","ns=3;s=ZZ_ZY2_FR97"]
["加药间2噪音频率98","ns=3;s=ZZ_ZY2_FR98"]
["加药间2噪音频率99","ns=3;s=ZZ_ZY2_FR99"]
["前端补水泵——自动启动","ns=6;s=QD_BSB_AUTOSTART"]
["前端补水泵—自动","ns=6;s=QD_BSB_BT_AUTO"]
["前端补水泵——故障复位","ns=6;s=QD_BSB_BT_RESET"]
["前端补水泵——启动","ns=6;s=QD_BSB_BT_START"]
["前端补水泵——停止","ns=6;s=QD_BSB_BT_STOP"]
["前端补水泵——故障","ns=6;s=QD_BSB_FAULT"]
["前端补水泵——输出","ns=6;s=QD_BSB_OUTPUT"]
["前端补水泵——ready","ns=6;s=QD_BSB_READY"]
["前端补水泵——远程","ns=6;s=QD_BSB_REM"]
["前端补水泵——运行反馈","ns=6;s=QD_BSB_RFB"]
["前端补水阀——自动","ns=6;s=QD_BSF_BT_AUTO"]
["前端补水阀——开阀","ns=6;s=QD_BSF_BT_CLOSE"]
["前端补水阀——关阀","ns=6;s=QD_BSF_BT_OPEN"]
["前端补水阀——故障复位","ns=6;s=QD_BSF_BT_RESET"]
["前端补水阀——关到位","ns=6;s=QD_BSF_CFB"]
["前端补水阀——关ing","ns=6;s=QD_BSF_CING"]
["前端补水阀——自动关","ns=6;s=QD_BSF_CLOSEAUTO"]
["前端补水阀——故障 ","ns=6;s=QD_BSF_ERR"]
["前端补水阀——总故障 ","ns=6;s=QD_BSF_ERRT"]
["前端补水阀开到位","ns=6;s=QD_BSF_OFB"]
["前端补水阀打开中","ns=6;s=QD_BSF_OING"]
["前端补水阀自动打开","ns=6;s=QD_BSF_OPENAUTO"]
["前端补水阀关闭","ns=6;s=QD_BSF_OUT_CLOSE"]
["前端补水阀打开","ns=6;s=QD_BSF_OUT_OPEN"]
["前端补水阀准备好","ns=6;s=QD_BSF_READY"]
["前端补水阀远程","ns=6;s=QD_BSF_REM"]
["RO产水PH PID 调节选择按钮","ns=6;s=QD_LD_BT_ROCSPH_PID"]
["RO进水ORP PID 调节选择按钮","ns=6;s=QD_LD_BT_ROHYJ_PID"]
["前端排气阀手自动","ns=6;s=QD_PQF_BT_AUTO"]
["前端排气阀手动关","ns=6;s=QD_PQF_BT_CLOSE"]
["前端排气阀手动开","ns=6;s=QD_PQF_BT_OPEN"]
["前端排气阀故障复位","ns=6;s=QD_PQF_BT_RESET"]
["前端排气阀关到位","ns=6;s=QD_PQF_CFB"]
["前端排气阀关闭中","ns=6;s=QD_PQF_CING"]
["前端排气阀自动关闭","ns=6;s=QD_PQF_CLOSEAUTO"]
["前端排气阀故障","ns=6;s=QD_PQF_ERR"]
["前端排气阀总故障","ns=6;s=QD_PQF_ERRT"]
["前端排气阀开到位","ns=6;s=QD_PQF_OFB"]
["前端排气阀打开中","ns=6;s=QD_PQF_OING"]
["前端排气阀自动打开","ns=6;s=QD_PQF_OPENAUTO"]
["前端排气阀关闭","ns=6;s=QD_PQF_OUT_CLOSE"]
["前端排气阀打开","ns=6;s=QD_PQF_OUT_OPEN"]
["前端排气阀准备好","ns=6;s=QD_PQF_OUT_READY"]
["前端排气阀远程","ns=6;s=QD_PQF_REM"]
["前端破真空阀手自动","ns=6;s=QD_PZKF_BT_AUTO"]
["前端破真空阀手动关","ns=6;s=QD_PZKF_BT_CLOSE"]
["前端破真空阀手动开","ns=6;s=QD_PZKF_BT_OPEN"]
["前端破真空阀故障复位","ns=6;s=QD_PZKF_BT_RESET"]
["前端破真空阀关到位","ns=6;s=QD_PZKF_CFB"]
["前端破真空阀关闭中","ns=6;s=QD_PZKF_CING"]
["前端破真空阀自动关闭","ns=6;s=QD_PZKF_CLOSEAUTO"]
["前端破真空阀故障","ns=6;s=QD_PZKF_ERR"]
["前端破真空阀总故障","ns=6;s=QD_PZKF_ERRT"]
["前端破真空阀开到位","ns=6;s=QD_PZKF_OFB"]
["前端破真空阀打开中","ns=6;s=QD_PZKF_OING"]
["前端破真空阀自动打开","ns=6;s=QD_PZKF_OPENAUTO"]
["前端破真空阀关闭","ns=6;s=QD_PZKF_OUT_CLOSE"]
["前端破真空阀打开","ns=6;s=QD_PZKF_OUT_OPEN"]
["前端破真空阀准备好","ns=6;s=QD_PZKF_OUT_READY"]
["前端破真空阀远程","ns=6;s=QD_PZKF_REM"]
["前端补水液位开关LS_00","ns=6;s=QD_QT_44_0"]
["Flag_QD排气执行中","ns=6;s=QD_QT_44_1"]
["Flag_QD排气中，超滤不允许","ns=6;s=QD_QT_44_2"]
["故障_引水装置补水超时","ns=6;s=QD_QT_44_3"]
["前端排气——备用","ns=6;s=QD_QT_44_4"]
["前端排气——备用","ns=6;s=QD_QT_44_5"]
["前端排气——备用","ns=6;s=QD_QT_44_6"]
["前端排气——备用","ns=6;s=QD_QT_44_7"]
["用户华晟-流量计温度","ns=1;s=WG_FLOW_HS2_00"]
["用户华晟-流量计压力","ns=1;s=WG_FLOW_HS2_01"]
["用户华晟-补偿前流量","ns=1;s=WG_FLOW_HS2_02"]
["用户华晟-补偿后流量","ns=1;s=WG_FLOW_HS2_03"]
["用户华晟-累计流量","ns=1;s=WG_FLOW_HS2_04"]
["用户芯动-流量计温度","ns=1;s=WG_FLOW_XD_00"]
["用户芯动-流量计压力","ns=1;s=WG_FLOW_XD_01"]
["用户芯动-补偿前流量","ns=1;s=WG_FLOW_XD_02"]
["用户芯动-补偿后流量","ns=1;s=WG_FLOW_XD_03"]
["用户芯动-累计流量","ns=1;s=WG_FLOW_XD_04"]
["前端补水泵","ns=3;s=QD_BSB_FRE_FB"]
["前端补水泵","ns=3;s=QD_BSB_FRESET"]
["前端补水泵","ns=3;s=QD_BSB_RUNTIME"]
["RO产水加碱频率1套","ns=3;s=QD_LD_R164"]
["RO产水加碱频率2套","ns=3;s=QD_LD_R168"]
["RO产水加碱频率备1","ns=3;s=QD_LD_R172"]
["RO产水加碱频率备2","ns=3;s=QD_LD_R176"]
["前端补水参照时间","ns=3;s=QD_QT_BSTIMESET"]
["前端液位触发后延时补水时间设置","ns=3;s=QD_QT_LSTIMEDELAYSET"]
["前端补水计时","ns=3;s=QD_QT_TIMEADD"]
["前端液位触发后延时补水计时","ns=3;s=QD_QT_TIMEDELAYADD"]
["备","ns=3;s=UF_LD_R152"]
["备","ns=3;s=UF_LD_R156"]
["备","ns=3;s=UF_LD_R182"]
["极电外供水流量计备用1","ns=1;s=WG_FLOW_JD_00"]
["极电外供水流量计备用2","ns=1;s=WG_FLOW_JD_01"]
["极电外供水流量计备用3","ns=1;s=WG_FLOW_JD_02"]
["极电外供水流量计备用4","ns=1;s=WG_FLOW_JD_03"]
["极点总供水流量计","ns=1;s=WG_FLOW_JD_04"]
["F1空调地址设定","ns=3;s=ZZ_AC1C_AD"]
["F1空调波特率设定","ns=3;s=ZZ_AC1C_BD"]
["F1空调风向设定","ns=3;s=ZZ_AC1C_DIR"]
["F1空调风速设定","ns=3;s=ZZ_AC1C_F"]
["F1空调开关模式","ns=3;s=ZZ_AC1C_MOD"]
["F1空调开关操作","ns=3;s=ZZ_AC1C_ON/OFF"]
["F1空调温度设定","ns=3;s=ZZ_AC1C_T"]
["F1空调地址","ns=1;s=ZZ_AC1S_ADR"]
["F1空调波特率","ns=1;s=ZZ_AC1S_BD"]
["F1空调红外状态","ns=1;s=ZZ_AC1S_IR"]
["F1空调开关状态","ns=1;s=ZZ_AC1S_ON/OFF"]
["F1空调湿度","ns=1;s=ZZ_AC1S_RH"]
["F1空调温度","ns=1;s=ZZ_AC1S_T"]
["F1空调运行状态检测信号类型","ns=1;s=ZZ_AC1S_TYPE"]
["F1空调运行状态检测信号值","ns=1;s=ZZ_AC1S_VALUE"]
["F2电控柜侧空调地址设定","ns=3;s=ZZ_AC2C_AD"]
["F2电控柜侧空调波特率设定","ns=3;s=ZZ_AC2C_BD"]
["F2电控柜侧空调风向设定","ns=3;s=ZZ_AC2C_DIR"]
["F2电控柜侧空调风速设定","ns=3;s=ZZ_AC2C_F"]
["F2电控柜侧空调开关模式","ns=3;s=ZZ_AC2C_MOD"]
["F2电控柜侧空调开关操作","ns=3;s=ZZ_AC2C_ON/OFF"]
["F2电控柜侧空调温度设定","ns=3;s=ZZ_AC2C_T"]
["F2电控柜侧空调地址","ns=1;s=ZZ_AC2S_ADR"]
["F2电控柜侧空调波特率","ns=1;s=ZZ_AC2S_BD"]
["F2电控柜侧空调红外状态","ns=1;s=ZZ_AC2S_IR"]
["F2电控柜侧空调开关状态","ns=1;s=ZZ_AC2S_ON/OFF"]
["F2电控柜侧空调湿度","ns=1;s=ZZ_AC2S_RH"]
["F2电控柜侧空调温度","ns=1;s=ZZ_AC2S_T"]
["F2电控柜侧空调运行状态检测信号类型","ns=1;s=ZZ_AC2S_TYPE"]
["F2电控柜侧空调运行状态检测信号值","ns=1;s=ZZ_AC2S_VALUE"]
["F2空调地址设定","ns=3;s=ZZ_AC3C_AD"]
["F2空调波特率设定","ns=3;s=ZZ_AC3C_BD"]
["F2空调风向设定","ns=3;s=ZZ_AC3C_DIR"]
["F2空调风速设定","ns=3;s=ZZ_AC3C_F"]
["F2空调开关模式","ns=3;s=ZZ_AC3C_MOD"]
["F2空调开关操作","ns=3;s=ZZ_AC3C_ON/OFF"]
["F2空调温度设定","ns=3;s=ZZ_AC3C_T"]
["F2空调地址","ns=1;s=ZZ_AC3S_ADR"]
["F2空调波特率","ns=1;s=ZZ_AC3S_BD"]
["F2空调红外状态","ns=1;s=ZZ_AC3S_IR"]
["F2空调开关状态","ns=1;s=ZZ_AC3S_ON/OFF"]
["F2空调湿度","ns=1;s=ZZ_AC3S_RH"]
["F2空调温度","ns=1;s=ZZ_AC3S_T"]
["F2空调运行状态检测信号类型","ns=1;s=ZZ_AC3S_TYPE"]
["F2空调运行状态检测信号值","ns=1;s=ZZ_AC3S_VALUE"]
["1#超滤 CIP进水手动阀开到位","ns=6;s=SF_UF1_CIPJSF_OFB"]
["1#超滤 CIP进水手动阀关到位","ns=6;s=SF_UF1_CIPJSF_CFB"]
["1#超滤 CIP浓水侧回水手动阀开到位","ns=6;s=SF_UF1_CIPNSF_OFB"]
["1#超滤 CIP浓水侧回水手动阀关到位","ns=6;s=SF_UF1_CIPNSF_CFB"]
["1#超滤 CIP产水侧回水手动阀开到位","ns=6;s=SF_UF1_CIPCSF_OFB"]
["1#超滤 CIP产水侧回水手动阀关到位","ns=6;s=SF_UF1_CIPCSF_CFB"]
["2#超滤 CIP进水手动阀开到位","ns=6;s=SF_UF2_CIPJSF_OFB"]
["2#超滤 CIP进水手动阀关到位","ns=6;s=SF_UF2_CIPJSF_CFB"]
["2#超滤 CIP浓水侧回水手动阀开到位","ns=6;s=SF_UF2_CIPNSF_OFB"]
["2#超滤 CIP浓水侧回水手动阀关到位","ns=6;s=SF_UF2_CIPNSF_CFB"]
["2#超滤 CIP产水侧回水手动阀开到位","ns=6;s=SF_UF2_CIPCSF_OFB"]
["2#超滤 CIP产水侧回水手动阀关到位","ns=6;s=SF_UF2_CIPCSF_CFB"]
["1#反渗透一二段CIP进水手动阀开到位","ns=6;s=SF_RO1_12DCIPJS_OFB"]
["1#反渗透一二段CIP进水手动阀关到位","ns=6;s=SF_RO1_12DCIPJS_CFB"]
["1#反渗透一段浓水侧CIP回水手动阀开到位","ns=6;s=SF_RO1_1DNSCIP_OFB"]
["1#反渗透一段浓水侧CIP回水手动阀关到位","ns=6;s=SF_RO1_1DNSCIP_CFB"]
["1#反渗透一段产水侧CIP回水手动阀开到位","ns=6;s=SF_RO1_1DCSCIP_OFB"]
["1#反渗透一段产水侧CIP回水手动阀关到位","ns=6;s=SF_RO1_1DCSCIP_CFB"]
["1#反渗透一段清洗产水隔断手动阀开到位","ns=6;s=SF_RO1_1DQXCSGD_OFB"]
["1#反渗透一段清洗产水隔断手动阀关到位","ns=6;s=SF_RO1_1DQXCSGD_CFB"]
["1#反渗透二段浓水侧CIP回水手动阀开到位","ns=6;s=SF_RO1_2DNSCIP_OFB"]
["1#反渗透二段浓水侧CIP回水手动阀关到位","ns=6;s=SF_RO1_2DNSCIP_CFB"]
["1#反渗透三段CIP进水手动阀开到位","ns=6;s=SF_RO1_3DCIPJS_OFB"]
["1#反渗透三段CIP进水手动阀关到位","ns=6;s=SF_RO1_3DCIPJS_CFB"]
["1#反渗透三段浓水侧CIP回水手动阀开到位","ns=6;s=SF_RO1_3DNSCIP_OFB"]
["1#反渗透三段浓水侧CIP回水手动阀关到位","ns=6;s=SF_RO1_3DNSCIP_CFB"]
["1#反渗透二三段产水侧CIP回水手动阀开到位","ns=6;s=SF_RO1_23CSCIP_OFB"]
["1#反渗透二三段产水侧CIP回水手动阀关到位","ns=6;s=SF_RO1_23CSCIP_CFB"]
["2#反渗透一二段CIP进水手动阀开到位","ns=6;s=SF_RO2_12DCIPJS_OFB"]
["2#反渗透一二段CIP进水手动阀关到位","ns=6;s=SF_RO2_12DCIPJS_CFB"]
["2#反渗透一段浓水侧CIP回水手动阀开到位","ns=6;s=SF_RO2_1DNSCIP_OFB"]
["2#反渗透一段浓水侧CIP回水手动阀关到位","ns=6;s=SF_RO2_1DNSCIP_CFB"]
["2#反渗透一段产水侧CIP回水手动阀开到位","ns=6;s=SF_RO2_1DCSCIP_OFB"]
["2#反渗透一段产水侧CIP回水手动阀关到位","ns=6;s=SF_RO2_1DCSCIP_CFB"]
["2#反渗透一段清洗产水隔断手动阀开到位","ns=6;s=SF_RO2_1DQXCSGD_OFB"]
["2#反渗透一段清洗产水隔断手动阀关到位","ns=6;s=SF_RO2_1DQXCSGD_CFB"]
["2#反渗透二段浓水侧CIP回水手动阀开到位","ns=6;s=SF_RO2_2DNSCIP_OFB"]
["2#反渗透二段浓水侧CIP回水手动阀关到位","ns=6;s=SF_RO2_2DNSCIP_CFB"]
["2#反渗透三段CIP进水手动阀开到位","ns=6;s=SF_RO2_3DCIPJS_OFB"]
["2#反渗透三段CIP进水手动阀关到位","ns=6;s=SF_RO2_3DCIPJS_CFB"]
["2#反渗透三段浓水侧CIP回水手动阀开到位","ns=6;s=SF_RO2_3DNSCIP_OFB"]
["2#反渗透三段浓水侧CIP回水手动阀关到位","ns=6;s=SF_RO2_3DNSCIP_CFB"]
["2#反渗透二三段产水侧CIP回水手动阀开到位","ns=6;s=SF_RO2_23CSCIP_OFB"]
["2#反渗透二三段产水侧CIP回水手动阀关到位","ns=6;s=SF_RO2_23CSCIP_CFB"]
["CIP补水阀手自动","ns=6;s=V_F_CIPBSF_BT_AUTO"]
["CIP补水阀手动关","ns=6;s=V_F_CIPBSF_BT_CLOSE"]
["CIP补水阀手动开","ns=6;s=V_F_CIPBSF_BT_OPEN"]
["CIP补水阀故障复位","ns=6;s=V_F_CIPBSF_BT_RESET"]
["CIP补水阀关到位","ns=6;s=V_F_CIPBSF_CFB"]
["CIP补水阀关闭中","ns=6;s=V_F_CIPBSF_CING"]
["CIP补水阀自动关闭","ns=6;s=V_F_CIPBSF_CLOSEAUTO"]
["CIP补水阀故障","ns=6;s=V_F_CIPBSF_ERR"]
["CIP补水阀总故障","ns=6;s=V_F_CIPBSF_ERRT"]
["CIP补水阀开到位","ns=6;s=V_F_CIPBSF_OFB"]
["CIP补水阀打开中","ns=6;s=V_F_CIPBSF_OING"]
["CIP补水阀自动打开","ns=6;s=V_F_CIPBSF_OPENAUTO"]
["CIP补水阀关闭","ns=6;s=V_F_CIPBSF_OUT_CLOSE"]
["CIP补水阀打开","ns=6;s=V_F_CIPBSF_OUT_OPEN"]
["CIP补水阀准备好","ns=6;s=V_F_CIPBSF_OUT_READY"]
["CIP补水阀远程","ns=6;s=V_F_CIPBSF_REM"]
["CIP次钠加药阀手自动","ns=6;s=V_F_CIPCNF_BT_AUTO"]
["CIP次钠加药阀手动关","ns=6;s=V_F_CIPCNF_BT_CLOSE"]
["CIP次钠加药阀手动开","ns=6;s=V_F_CIPCNF_BT_OPEN"]
["CIP次钠加药阀故障复位","ns=6;s=V_F_CIPCNF_BT_RESET"]
["CIP次钠加药阀关到位","ns=6;s=V_F_CIPCNF_CFB"]
["CIP次钠加药阀关闭中","ns=6;s=V_F_CIPCNF_CING"]
["CIP次钠加药阀自动关闭","ns=6;s=V_F_CIPCNF_CLOSEAUTO"]
["CIP次钠加药阀故障","ns=6;s=V_F_CIPCNF_ERR"]
["CIP次钠加药阀总故障","ns=6;s=V_F_CIPCNF_ERRT"]
["CIP次钠加药阀开到位","ns=6;s=V_F_CIPCNF_OFB"]
["CIP次钠加药阀打开中","ns=6;s=V_F_CIPCNF_OING"]
["CIP次钠加药阀自动打开","ns=6;s=V_F_CIPCNF_OPENAUTO"]
["CIP次钠加药阀关闭","ns=6;s=V_F_CIPCNF_OUT_CLOSE"]
["CIP次钠加药阀打开","ns=6;s=V_F_CIPCNF_OUT_OPEN"]
["CIP次钠加药阀准备好","ns=6;s=V_F_CIPCNF_OUT_READY"]
["CIP次钠加药阀远程","ns=6;s=V_F_CIPCNF_REM"]
["CIP碱加药阀手自动","ns=6;s=V_F_CIPJF_BT_AUTO"]
["CIP碱加药阀手动关","ns=6;s=V_F_CIPJF_BT_CLOSE"]
["CIP碱加药阀手动开","ns=6;s=V_F_CIPJF_BT_OPEN"]
["CIP碱加药阀故障复位","ns=6;s=V_F_CIPJF_BT_RESET"]
["CIP碱加药阀关到位","ns=6;s=V_F_CIPJF_CFB"]
["CIP碱加药阀关闭中","ns=6;s=V_F_CIPJF_CING"]
["CIP碱加药阀自动关闭","ns=6;s=V_F_CIPJF_CLOSEAUTO"]
["CIP碱加药阀故障","ns=6;s=V_F_CIPJF_ERR"]
["CIP碱加药阀总故障","ns=6;s=V_F_CIPJF_ERRT"]
["CIP碱加药阀开到位","ns=6;s=V_F_CIPJF_OFB"]
["CIP碱加药阀打开中","ns=6;s=V_F_CIPJF_OING"]
["CIP碱加药阀自动打开","ns=6;s=V_F_CIPJF_OPENAUTO"]
["CIP碱加药阀关闭","ns=6;s=V_F_CIPJF_OUT_CLOSE"]
["CIP碱加药阀打开","ns=6;s=V_F_CIPJF_OUT_OPEN"]
["CIP碱加药阀准备好","ns=6;s=V_F_CIPJF_OUT_READY"]
["CIP碱加药阀远程","ns=6;s=V_F_CIPJF_REM"]
["CIP酸加药阀手自动","ns=6;s=V_F_CIPSF_BT_AUTO"]
["CIP酸加药阀手动关","ns=6;s=V_F_CIPSF_BT_CLOSE"]
["CIP酸加药阀手动开","ns=6;s=V_F_CIPSF_BT_OPEN"]
["CIP酸加药阀故障复位","ns=6;s=V_F_CIPSF_BT_RESET"]
["CIP酸加药阀关到位","ns=6;s=V_F_CIPSF_CFB"]
["CIP酸加药阀关闭中","ns=6;s=V_F_CIPSF_CING"]
["CIP酸加药阀自动关闭","ns=6;s=V_F_CIPSF_CLOSEAUTO"]
["CIP酸加药阀故障","ns=6;s=V_F_CIPSF_ERR"]
["CIP酸加药阀总故障","ns=6;s=V_F_CIPSF_ERRT"]
["CIP酸加药阀开到位","ns=6;s=V_F_CIPSF_OFB"]
["CIP酸加药阀打开中","ns=6;s=V_F_CIPSF_OING"]
["CIP酸加药阀自动打开","ns=6;s=V_F_CIPSF_OPENAUTO"]
["CIP酸加药阀关闭","ns=6;s=V_F_CIPSF_OUT_CLOSE"]
["CIP酸加药阀打开","ns=6;s=V_F_CIPSF_OUT_OPEN"]
["CIP酸加药阀准备好","ns=6;s=V_F_CIPSF_OUT_READY"]
["CIP酸加药阀远程","ns=6;s=V_F_CIPSF_REM"]
["反渗透碱加药阀手自动","ns=6;s=V_F_ROJF_BT_AUTO"]
["反渗透碱加药阀手动关","ns=6;s=V_F_ROJF_BT_CLOSE"]
["反渗透碱加药阀手动开","ns=6;s=V_F_ROJF_BT_OPEN"]
["反渗透碱加药阀故障复位","ns=6;s=V_F_ROJF_BT_RESET"]
["反渗透碱加药阀关到位","ns=6;s=V_F_ROJF_CFB"]
["反渗透碱加药阀关闭中","ns=6;s=V_F_ROJF_CING"]
["反渗透碱加药阀自动关闭","ns=6;s=V_F_ROJF_CLOSEAUTO"]
["反渗透碱加药阀故障","ns=6;s=V_F_ROJF_ERR"]
["反渗透碱加药阀总故障","ns=6;s=V_F_ROJF_ERRT"]
["反渗透碱加药阀开到位","ns=6;s=V_F_ROJF_OFB"]
["反渗透碱加药阀打开中","ns=6;s=V_F_ROJF_OING"]
["反渗透碱加药阀自动打开","ns=6;s=V_F_ROJF_OPENAUTO"]
["反渗透碱加药阀关闭","ns=6;s=V_F_ROJF_OUT_CLOSE"]
["反渗透碱加药阀打开","ns=6;s=V_F_ROJF_OUT_OPEN"]
["反渗透碱加药阀准备好","ns=6;s=V_F_ROJF_OUT_READY"]
["反渗透碱加药阀远程","ns=6;s=V_F_ROJF_REM"]
["反渗透酸加药阀手自动","ns=6;s=V_F_ROSF_BT_AUTO"]
["反渗透酸加药阀手动关","ns=6;s=V_F_ROSF_BT_CLOSE"]
["反渗透酸加药阀手动开","ns=6;s=V_F_ROSF_BT_OPEN"]
["反渗透酸加药阀故障复位","ns=6;s=V_F_ROSF_BT_RESET"]
["反渗透酸加药阀关到位","ns=6;s=V_F_ROSF_CFB"]
["反渗透酸加药阀关闭中","ns=6;s=V_F_ROSF_CING"]
["反渗透酸加药阀自动关闭","ns=6;s=V_F_ROSF_CLOSEAUTO"]
["反渗透酸加药阀故障","ns=6;s=V_F_ROSF_ERR"]
["反渗透酸加药阀总故障","ns=6;s=V_F_ROSF_ERRT"]
["反渗透酸加药阀开到位","ns=6;s=V_F_ROSF_OFB"]
["反渗透酸加药阀打开中","ns=6;s=V_F_ROSF_OING"]
["反渗透酸加药阀自动打开","ns=6;s=V_F_ROSF_OPENAUTO"]
["反渗透酸加药阀关闭","ns=6;s=V_F_ROSF_OUT_CLOSE"]
["反渗透酸加药阀打开","ns=6;s=V_F_ROSF_OUT_OPEN"]
["反渗透酸加药阀准备好","ns=6;s=V_F_ROSF_OUT_READY"]
["反渗透酸加药阀远程","ns=6;s=V_F_ROSF_REM"]
["1#超滤提升泵自动启动","ns=6;s=P_1#UFTSB_AUTOSTART"]
["1#超滤提升泵手自动","ns=6;s=P_1#UFTSB_BT_AUTO"]
["1#超滤提升泵故障复位","ns=6;s=P_1#UFTSB_BT_RESET"]
["1#超滤提升泵手动启动","ns=6;s=P_1#UFTSB_BT_START"]
["1#超滤提升泵手动停止","ns=6;s=P_1#UFTSB_BT_STOP"]
["1#超滤提升泵故障","ns=6;s=P_1#UFTSB_FAULT"]
["1#超滤提升泵启动","ns=6;s=P_1#UFTSB_OUTPUT"]
["1#超滤提升泵启动准备好","ns=6;s=P_1#UFTSB_READY"]
["1#超滤提升泵远程","ns=6;s=P_1#UFTSB_REM"]
["1#超滤提升泵运行","ns=6;s=P_1#UFTSB_RFB"]
["1#超滤提升泵频率反馈","ns=3;s=P_1#UFTSB_FRE_FB"]
["1#超滤提升泵频率设定","ns=3;s=P_1#UFTSB_FRESET"]
["1#超滤提升泵运行时间","ns=3;s=P_1#UFTSB_RUNTIME"]
["2#超滤提升泵自动启动","ns=6;s=P_2#UFTSB_AUTOSTART"]
["2#超滤提升泵手自动","ns=6;s=P_2#UFTSB_BT_AUTO"]
["2#超滤提升泵故障复位","ns=6;s=P_2#UFTSB_BT_RESET"]
["2#超滤提升泵手动启动","ns=6;s=P_2#UFTSB_BT_START"]
["2#超滤提升泵手动停止","ns=6;s=P_2#UFTSB_BT_STOP"]
["2#超滤提升泵故障","ns=6;s=P_2#UFTSB_FAULT"]
["2#超滤提升泵启动","ns=6;s=P_2#UFTSB_OUTPUT"]
["2#超滤提升泵启动准备好","ns=6;s=P_2#UFTSB_READY"]
["2#超滤提升泵远程","ns=6;s=P_2#UFTSB_REM"]
["2#超滤提升泵运行","ns=6;s=P_2#UFTSB_RFB"]
["2#超滤提升泵频率反馈","ns=3;s=P_2#UFTSB_FRE_FB"]
["2#超滤提升泵频率设定","ns=3;s=P_2#UFTSB_FRESET"]
["2#超滤提升泵运行时间","ns=3;s=P_2#UFTSB_RUNTIME"]
["1#湿地提升泵自动启动","ns=6;s=P_1#SDTSB_AUTOSTART"]
["1#湿地提升泵手自动","ns=6;s=P_1#SDTSB_BT_AUTO"]
["1#湿地提升泵故障复位","ns=6;s=P_1#SDTSB_BT_RESET"]
["1#湿地提升泵手动启动","ns=6;s=P_1#SDTSB_BT_START"]
["1#湿地提升泵手动停止","ns=6;s=P_1#SDTSB_BT_STOP"]
["1#湿地提升泵故障","ns=6;s=P_1#SDTSB_FAULT"]
["1#湿地提升泵启动","ns=6;s=P_1#SDTSB_OUTPUT"]
["1#湿地提升泵启动准备好","ns=6;s=P_1#SDTSB_READY"]
["1#湿地提升泵远程","ns=6;s=P_1#SDTSB_REM"]
["1#湿地提升泵运行","ns=6;s=P_1#SDTSB_RFB"]
["1#湿地提升泵频率反馈","ns=3;s=P_1#SDTSB_FRE_FB"]
["1#湿地提升泵频率设定","ns=3;s=P_1#SDTSB_FRESET"]
["1#湿地提升泵运行时间","ns=3;s=P_1#SDTSB_RUNTIME"]
["2#湿地提升泵自动启动","ns=6;s=P_2#SDTSB_AUTOSTART"]
["2#湿地提升泵手自动","ns=6;s=P_2#SDTSB_BT_AUTO"]
["2#湿地提升泵故障复位","ns=6;s=P_2#SDTSB_BT_RESET"]
["2#湿地提升泵手动启动","ns=6;s=P_2#SDTSB_BT_START"]
["2#湿地提升泵手动停止","ns=6;s=P_2#SDTSB_BT_STOP"]
["2#湿地提升泵故障","ns=6;s=P_2#SDTSB_FAULT"]
["2#湿地提升泵启动","ns=6;s=P_2#SDTSB_OUTPUT"]
["2#湿地提升泵启动准备好","ns=6;s=P_2#SDTSB_READY"]
["2#湿地提升泵远程","ns=6;s=P_2#SDTSB_REM"]
["2#湿地提升泵运行","ns=6;s=P_2#SDTSB_RFB"]
["2#湿地提升泵频率反馈","ns=3;s=P_2#SDTSB_FRE_FB"]
["2#湿地提升泵频率设定","ns=3;s=P_2#SDTSB_FRESET"]
["2#湿地提升泵运行时间","ns=3;s=P_2#SDTSB_RUNTIME"]
["超滤进水取样阀手自动","ns=6;s=QYF_UFJS_BT_AUTO"]
["超滤进水取样阀手动关","ns=6;s=QYF_UFJS_BT_CLOSE"]
["超滤进水取样阀手动开","ns=6;s=QYF_UFJS_BT_OPEN"]
["超滤进水取样阀故障复位","ns=6;s=QYF_UFJS_BT_RESET"]
["超滤进水取样阀关到位","ns=6;s=QYF_UFJS_CFB"]
["超滤进水取样阀关闭中","ns=6;s=QYF_UFJS_CING"]
["超滤进水取样阀自动关闭","ns=6;s=QYF_UFJS_CLOSEAUTO"]
["超滤进水取样阀故障","ns=6;s=QYF_UFJS_ERR"]
["超滤进水取样阀总故障","ns=6;s=QYF_UFJS_ERRT"]
["超滤进水取样阀开到位","ns=6;s=QYF_UFJS_OFB"]
["超滤进水取样阀打开中","ns=6;s=QYF_UFJS_OING"]
["超滤进水取样阀自动打开","ns=6;s=QYF_UFJS_OPENAUTO"]
["超滤进水取样阀关闭","ns=6;s=QYF_UFJS_OUT_CLOSE"]
["超滤进水取样阀打开","ns=6;s=QYF_UFJS_OUT_OPEN"]
["超滤进水取样阀准备好","ns=6;s=QYF_UFJS_OUT_READY"]
["超滤进水取样阀远程","ns=6;s=QYF_UFJS_REM"]
["超滤产水取样阀手自动","ns=6;s=QYF_UFCS_BT_AUTO"]
["超滤产水取样阀手动关","ns=6;s=QYF_UFCS_BT_CLOSE"]
["超滤产水取样阀手动开","ns=6;s=QYF_UFCS_BT_OPEN"]
["超滤产水取样阀故障复位","ns=6;s=QYF_UFCS_BT_RESET"]
["超滤产水取样阀关到位","ns=6;s=QYF_UFCS_CFB"]
["超滤产水取样阀关闭中","ns=6;s=QYF_UFCS_CING"]
["超滤产水取样阀自动关闭","ns=6;s=QYF_UFCS_CLOSEAUTO"]
["超滤产水取样阀故障","ns=6;s=QYF_UFCS_ERR"]
["超滤产水取样阀总故障","ns=6;s=QYF_UFCS_ERRT"]
["超滤产水取样阀开到位","ns=6;s=QYF_UFCS_OFB"]
["超滤产水取样阀打开中","ns=6;s=QYF_UFCS_OING"]
["超滤产水取样阀自动打开","ns=6;s=QYF_UFCS_OPENAUTO"]
["超滤产水取样阀关闭","ns=6;s=QYF_UFCS_OUT_CLOSE"]
["超滤产水取样阀打开","ns=6;s=QYF_UFCS_OUT_OPEN"]
["超滤产水取样阀准备好","ns=6;s=QYF_UFCS_OUT_READY"]
["超滤产水取样阀远程","ns=6;s=QYF_UFCS_REM"]
["反渗透产水取样阀手自动","ns=6;s=QYF_ROCS_BT_AUTO"]
["反渗透产水取样阀手动关","ns=6;s=QYF_ROCS_BT_CLOSE"]
["反渗透产水取样阀手动开","ns=6;s=QYF_ROCS_BT_OPEN"]
["反渗透产水取样阀故障复位","ns=6;s=QYF_ROCS_BT_RESET"]
["反渗透产水取样阀关到位","ns=6;s=QYF_ROCS_CFB"]
["反渗透产水取样阀关闭中","ns=6;s=QYF_ROCS_CING"]
["反渗透产水取样阀自动关闭","ns=6;s=QYF_ROCS_CLOSEAUTO"]
["反渗透产水取样阀故障","ns=6;s=QYF_ROCS_ERR"]
["反渗透产水取样阀总故障","ns=6;s=QYF_ROCS_ERRT"]
["反渗透产水取样阀开到位","ns=6;s=QYF_ROCS_OFB"]
["反渗透产水取样阀打开中","ns=6;s=QYF_ROCS_OING"]
["反渗透产水取样阀自动打开","ns=6;s=QYF_ROCS_OPENAUTO"]
["反渗透产水取样阀关闭","ns=6;s=QYF_ROCS_OUT_CLOSE"]
["反渗透产水取样阀打开","ns=6;s=QYF_ROCS_OUT_OPEN"]
["反渗透产水取样阀准备好","ns=6;s=QYF_ROCS_OUT_READY"]
["反渗透产水取样阀远程","ns=6;s=QYF_ROCS_REM"]
["反渗透外供水取样阀手自动","ns=6;s=QYF_ROWG_BT_AUTO"]
["反渗透外供水取样阀手动关","ns=6;s=QYF_ROWG_BT_CLOSE"]
["反渗透外供水取样阀手动开","ns=6;s=QYF_ROWG_BT_OPEN"]
["反渗透外供水取样阀故障复位","ns=6;s=QYF_ROWG_BT_RESET"]
["反渗透外供水取样阀关到位","ns=6;s=QYF_ROWG_CFB"]
["反渗透外供水取样阀关闭中","ns=6;s=QYF_ROWG_CING"]
["反渗透外供水取样阀自动关闭","ns=6;s=QYF_ROWG_CLOSEAUTO"]
["反渗透外供水取样阀故障","ns=6;s=QYF_ROWG_ERR"]
["反渗透外供水取样阀总故障","ns=6;s=QYF_ROWG_ERRT"]
["反渗透外供水取样阀开到位","ns=6;s=QYF_ROWG_OFB"]
["反渗透外供水取样阀打开中","ns=6;s=QYF_ROWG_OING"]
["反渗透外供水取样阀自动打开","ns=6;s=QYF_ROWG_OPENAUTO"]
["反渗透外供水取样阀关闭","ns=6;s=QYF_ROWG_OUT_CLOSE"]
["反渗透外供水取样阀打开","ns=6;s=QYF_ROWG_OUT_OPEN"]
["反渗透外供水取样阀准备好","ns=6;s=QYF_ROWG_OUT_READY"]
["反渗透外供水取样阀远程","ns=6;s=QYF_ROWG_REM"]
["自动按钮","ns=6;s=ZH_BUTTON_AUTO"]
["直排按钮","ns=6;s=ZH_BUTTON_DISCHARGE"]
["复位按钮","ns=6;s=ZH_BUTTON_RESET"]
["3700","ns=6;s=ZH_END_HCL"]
["3701","ns=6;s=ZH_END_NAOH"]
["3702","ns=6;s=ZH_END_SBS"]
["3703","ns=6;s=ZH_END_TOTAL"]
["3704","ns=6;s=ZH_READY_HCL"]
["3705","ns=6;s=ZH_READY_NAOH"]
["3706","ns=6;s=ZH_READY_SBS"]
["3707","ns=6;s=ZH_READY_TOTAL"]
["3708","ns=6;s=ZH_READY_ZH"]
["3709","ns=3;s=ZH_LT_ZHC_H"]
["3710","ns=3;s=ZH_LT_ZHC_L"]
["3711","ns=3;s=ZH_ORP_H"]
["3712","ns=3;s=ZH_ORP_HH"]
["3713","ns=3;s=ZH_PH_H"]
["3714","ns=3;s=ZH_PH_HH"]
["3715","ns=3;s=ZH_PH_L"]
["3716","ns=3;s=ZH_PH_LL"]
["3717","ns=3;s=ZH_TIME_CYCLE"]
["3718","ns=3;s=ZH_TIME_FAULT"]
["3719","ns=3;s=ZH_TIME_ORP_H"]
["3720","ns=3;s=ZH_TIME_ORP_HH"]
["3721","ns=3;s=ZH_TIME_PH_H"]
["3722","ns=3;s=ZH_TIME_PH_HH"]
["3723","ns=3;s=ZH_TIME_PH_L"]
["3724","ns=3;s=ZH_TIME_PH_LL"]
["3725","ns=3;s=ZH_TIME_RUNING"]
["3726","ns=3;s=ZH_TIME_SET"]
["3727","ns=3;s=ZH_WORD_STEP"]
["2#RO段间泵效率","2#RODJB_Eff"]
["1#RO段间泵效率","1#RODJB_Eff"]
["反渗透外供泵效率","ROWGB_Eff"]
["2#RO高压泵效率","2#ROGYB_Eff"]
["1#RO高压泵效率","1#ROGYB_Eff"]
["反渗透回收率","ROHSL"]