{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":5379,"n_cols":2,"rows_kept":5379,"cut":false,"hidden":false,"merged":[]}
["item_alias","item_name"]
["超滤总进水量","water_in"]
["1#RO回收率","RO1HSL"]
["2#RO回收率","RO2HSL"]
["UF供水泵运行数量","UFGSB_shuliang"]
["超滤泵出水流量","UF_bump_avg"]
["超滤反洗泵运行数量","UFFXB_shuliang"]
["反洗泵出水流量","UFFXB_runFlow"]
["CIP清洗水泵运行数量","CIP_QXB_runnumber"]
["清洗水泵流量","CIP_QXB_runFlow"]
["1#超滤供水泵效率","UF_bump1_n"]
["2#超滤供水泵效率","UF_bump2_n"]
["3#超滤供水泵效率","UF_bump3_n"]
["4#超滤供水泵效率","UF_bump4_n"]
["UF1膜运行通量","UF1_FluxF"]
["UF2膜运行通量  ","UF2_FluxF"]
["UF3膜运行通量  ","UF3_FluxF"]
["UF4膜运行通量 ","UF4_FluxF"]
["自清洗过滤器压差","PFTMP"]
["UF1膜渗透率","UF1Per"]
["UF2膜渗透率","UF2Per"]
["UF3膜渗透率","UF3Per"]
["UF4膜渗透率","UF4Per"]
["反洗膜通量","UFFX_Flux"]
["RO总进水流量","RO_TotalFlow"]
["RO总产水流量","RO_TCHFlow"]
["3#RO回收率","RO3HSL"]
["4#RO回收率","RO4HSL"]
["3#清水外供泵效率","QSWGB3_n"]
["2#清水外供泵效率","QSWGB2_n"]
["1#清水外供泵效率","QSWGB1_n"]
["清水外供泵出水流量 ","QSWGB_Flow"]
["RO4脱盐率","RO4_TYL"]
["RO3脱盐率","RO3_TYL"]
["RO2脱盐率","RO2_TYL"]
["RO1脱盐率","RO1_TYL"]
["RO4膜运行通量","RO4_FluxF"]
["RO3膜运行通量","RO3_FluxF"]
["RO2膜运行通量","RO2_FluxF"]
["RO1膜运行通量","RO1_FluxF"]
["RO4一二段产水流量比值","RO4_SPK"]
["RO3一二段产水流量比值","RO3_SPK"]
["RO2一二段产水流量比值","RO2_SPK"]
["RO1一二段产水流量比值","RO1_SPK"]
["RO4段间泵效率","RO4_DJB_n"]
["RO3段间泵效率","RO3_DJB_n"]
["RO2段间泵效率","RO2_DJB_n"]
["RO1段间泵效率","RO1_DJB_n"]
["RO4高压泵效率","RO4_GYB_n"]
["RO3高压泵效率","RO3_GYB_n"]
["RO2高压泵效率","RO2_GYB_n"]
["RO1高压泵效率","RO1_GYB_n"]
["反渗透RO2步序和产水时长","C.M.RO2_DB@control_word_time"]
["反渗透RO1步序和产水时长","C.M.RO1_DB@control_word_time"]
["反渗透RO3步序和产水时长","C.M.RO3_DB@control_word_time"]
["反渗透RO4步序和产水时长","C.M.RO4_DB@control_word_time"]
["UF反洗时间显示","UF_DB@time_display"]
["清洗膜通量","UFQX_Flux"]
["UF反洗步序","UF_FXBX"]
["UF酸洗步序","UF_SXBX"]
["UF碱洗步序","UF_JXBX"]
["UF1步序和产水时长","C.M.UF1_DB@word_control_time"]
["UF2步序和产水时长","C.M.UF2_DB@word_control_time"]
["UF3步序和产水时长","C.M.UF3_DB@word_control_time"]
["UF4步序和产水时长","C.M.UF4_DB@word_control_time"]
["膜车间进出水流量校验","Flow_check"]
["RO1产水流量","RO1_CSFlow"]
["RO2产水流量","RO2_CSFlow"]
["RO3产水流量","RO3_CSFlow"]
["RO4产水流量","RO4_CSFlow"]
["UF1反洗压差","C.M.UF1_DW@press_PV"]
["UF2反洗压差","C.M.UF2_DW@press_PV"]
["UF3反洗压差","C.M.UF3_DW@press_PV"]
["UF4反洗压差","C.M.UF4_DW@press_PV"]
["UF1运行过滤压差","UF1_FF_TMP"]
["UF2运行过滤压差","UF2_FF_TMP"]
["UF3运行过滤压差","UF3_FF_TMP"]
["UF4运行过滤压差","UF4_FF_TMP"]
["UF1反洗前压差","UF1_BW_Before_TMP"]
["UF1反洗后压差","UF1_BW_After_TMP"]
["UF2反洗前压差","UF2_BW_Before_TMP"]
["UF3反洗前压差","UF3_BW_Before_TMP"]
["UF4反洗前压差","UF4_BW_Before_TMP"]
["UF2反洗后压差","UF2_BW_After_TMP"]
["UF3反洗后压差","UF3_BW_After_TMP"]
["UF4反洗后压差","UF4_BW_After_TMP"]
["UF1反洗前渗透率","UF1_BW_Before_Per"]
["UF1反洗后渗透率","UF1_BW_After_Per"]
["UF2反洗前渗透率","UF2_BW_Before_Per"]
["UF3反洗前渗透率","UF3_BW_Before_Per"]
["UF4反洗前渗透率","UF4_BW_Before_Per"]
["UF2反洗后渗透率","UF2_BW_After_Per"]
["UF3反洗后渗透率","UF3_BW_After_Per"]
["UF4反洗后渗透率","UF4_BW_After_Per"]
["水温校正因子","SW_ jzyz"]
["UF1膜渗透率（标准25℃）","UF1_BZ_Per"]
["UF2膜渗透率（标准25℃）","UF2_BZ_Per"]
["UF3膜渗透率（标准25℃）","UF3_BZ_Per"]
["UF4膜渗透率（标准25℃）","UF4_BZ_Per"]
["1#RO运行回收率","RO1_YX_HSL"]
["2#RO运行回收率","RO2_YX_HSL"]
["3#RO运行回收率","RO3_YX_HSL"]
["4#RO运行回收率","RO4_YX_HSL"]
["az_feed_in_flow","az_feed_in_flow"]
["az_feed_out_flow","az_feed_out_flow"]
["RO1过滤一段压差","RO1_FF_TMP1"]
["RO1过滤二段压差","RO1_FF_TMP2"]
["RO2过滤一段压差","RO2_FF_TMP1"]
["RO2过滤二段压差","RO2_FF_TMP2"]
["RO3过滤二段压差","RO3_FF_TMP2"]
["RO4过滤二段压差","RO4_FF_TMP2"]
["RO3过滤一段压差","RO3_FF_TMP1"]
["RO4过滤一段压差","RO4_FF_TMP1"]
["RO3冲洗后一段压差","RO3_CX_After_TMP1"]
["RO1冲洗前一段压差","RO1_CX_Before_TMP1"]
["RO3冲洗后时间节点","RO3_CX_After_TIme"]
["RO1冲洗后一段压差","RO1_CX_After_TMP1"]
["RO2冲洗后一段压差","RO2_CX_After_TMP1"]
["RO4冲洗后一段压差","RO4_CX_After_TMP1"]
["RO1冲洗后二段压差","RO1_CX_After_TMP2"]
["RO2冲洗后二段压差","RO2_CX_After_TMP2"]
["RO3冲洗后二段压差","RO3_CX_After_TMP2"]
["RO4冲洗后二段压差","RO4_CX_After_TMP2"]
["RO1冲洗前二段压差","RO1_CX_Before_TMP2"]
["RO2冲洗前一段压差","RO2_CX_Before_TMP1"]
["RO2冲洗前二段压差","RO2_CX_Before_TMP2"]
["RO3冲洗前一段压差","RO3_CX_Before_TMP1"]
["RO3冲洗前二段压差","RO3_CX_Before_TMP2"]
["RO4冲洗前一段压差","RO4_CX_Before_TMP1"]
["RO4冲洗前二段压差","RO4_CX_Before_TMP2"]
["反渗透进水ORP超高（组态弹窗用）","ORP_CX"]
["反渗透D产水电导率新","C.M.RO4_Cond_CS_filter@out"]
["反渗透C产水电导率新","C.M.RO3_Cond_CS_filter@out"]
["反渗透B产水电导率新","C.M.RO2_Cond_CS_filter@out"]
["反渗透A产水电导率新","C.M.RO1_Cond_CS_filter@out"]
["1#反渗透CIP状态","RO1_CIP_STATE"]
["2#反渗透CIP状态","RO2_CIP_STATE"]
["3#反渗透CIP状态","RO3_CIP_STATE"]
["4#反渗透CIP状态","RO4_CIP_STATE"]
["超滤回收率","UFHSL"]
["外供水PH报警定制","WGS_PH_CUSTOM_ALARM"]
["外供水ORP报警定制","WGS_ORP_CUSTOM_ALARM"]
["设定——反洗优先时间设定","C.M.BW_First_Left_Time"]
["设定——冲洗加药-一段碱频率","C.M.cxjy_FreSet[0]"]
["设定——冲洗加药-二段碱频率","C.M.cxjy_FreSet[1]"]
["设定——冲洗加药-一段非氧频率","C.M.cxjy_FreSet[2]"]
["设定——冲洗加药-二段非氧频率","C.M.cxjy_FreSet[3]"]
["设定——冲洗加药-一段酸频率","C.M.cxjy_FreSet[4]"]
["设定——冲洗加药-二段酸频率","C.M.cxjy_FreSet[5]"]
["反洗排队显示1","C.M.FIFOShow0"]
["反洗排队显示2","C.M.FIFOShow1"]
["反洗排队显示3","C.M.FIFOShow2"]
["反洗排队显示4","C.M.FIFOShow3"]
["水淹报警信号1","C.M.Flag_SY[0]"]
["水淹报警信号2","C.M.Flag_SY[1]"]
["水淹报警信号3","C.M.Flag_SY[2]"]
["水淹报警信号4","C.M.Flag_SY[3]"]
["水淹报警信号5","C.M.Flag_SY[4]"]
["水淹报警信号6","C.M.Flag_SY[5]"]
["水淹报警信号7","C.M.Flag_SY[6]"]
["水淹报警信号8","C.M.Flag_SY[7]"]
["非氧加药泵1——自动/手动","C.M.PRO_cxsx_FY1@auto_select"]
["非氧加药泵1——故障","C.M.PRO_cxsx_FY1@fault_total"]
["非氧加药泵1——远程","C.M.PRO_cxsx_FY1@rem"]
["非氧加药泵1——复位","C.M.PRO_cxsx_FY1@reset"]
["非氧加药泵1——运行反馈","C.M.PRO_cxsx_FY1@run"]
["非氧加药泵1——运行时间","C.M.PRO_cxsx_FY1@run_time"]
["非氧加药泵1——起泵","C.M.PRO_cxsx_FY1@start"]
["非氧加药泵1——停泵","C.M.PRO_cxsx_FY1@stop"]
["非氧加药泵1——手动频率","C.M.PRO_cxsx_FY1_AO_FB@spare"]
["非氧加药泵1——故障","C.M.PRO_cxsx_FY1_fre@Fault"]
["非氧加药泵1——频率反馈","C.M.PRO_cxsx_FY1_fre@out"]
["非氧加药泵2——自动/手动","C.M.PRO_cxsx_FY2@auto_select"]
["非氧加药泵2——故障","C.M.PRO_cxsx_FY2@fault_total"]
["非氧加药泵2——远程","C.M.PRO_cxsx_FY2@rem"]
["非氧加药泵2——复位","C.M.PRO_cxsx_FY2@reset"]
["非氧加药泵2——运行反馈","C.M.PRO_cxsx_FY2@run"]
["非氧加药泵2——运行时间","C.M.PRO_cxsx_FY2@run_time"]
["非氧加药泵2——起泵","C.M.PRO_cxsx_FY2@start"]
["非氧加药泵2——停泵","C.M.PRO_cxsx_FY2@stop"]
["非氧加药泵2——手动频率","C.M.PRO_cxsx_FY2_AO_FB@spare"]
["非氧加药泵2——故障","C.M.PRO_cxsx_FY2_fre@Fault"]
["非氧加药泵2——频率反馈","C.M.PRO_cxsx_FY2_fre@out"]
["冲洗碱加药泵1——自动/手动","C.M.PRO_cxsx_J1@auto_select"]
["冲洗碱加药泵1——故障","C.M.PRO_cxsx_J1@fault_total"]
["冲洗碱加药泵1——远程","C.M.PRO_cxsx_J1@rem"]
["冲洗碱加药泵1——复位","C.M.PRO_cxsx_J1@reset"]
["冲洗碱加药泵1——运行反馈","C.M.PRO_cxsx_J1@run"]
["冲洗碱加药泵1——运行时间","C.M.PRO_cxsx_J1@run_time"]
["冲洗碱加药泵1——起泵","C.M.PRO_cxsx_J1@start"]
["冲洗碱加药泵1——停泵","C.M.PRO_cxsx_J1@stop"]
["冲洗碱加药泵1——手动频率","C.M.PRO_cxsx_J1_AO_FB@spare"]
["冲洗碱加药泵1——故障","C.M.PRO_cxsx_J1_fre@Fault"]
["冲洗碱加药泵1——频率反馈","C.M.PRO_cxsx_J1_fre@out"]
["冲洗碱加药泵2——自动/手动","C.M.PRO_cxsx_J2@auto_select"]
["冲洗碱加药泵2——故障","C.M.PRO_cxsx_J2@fault_total"]
["冲洗碱加药泵2——远程","C.M.PRO_cxsx_J2@rem"]
["冲洗碱加药泵2——复位","C.M.PRO_cxsx_J2@reset"]
["冲洗碱加药泵2——运行反馈","C.M.PRO_cxsx_J2@run"]
["冲洗碱加药泵2——运行时间","C.M.PRO_cxsx_J2@run_time"]
["冲洗碱加药泵2——起泵","C.M.PRO_cxsx_J2@start"]
["冲洗碱加药泵2——停泵","C.M.PRO_cxsx_J2@stop"]
["冲洗碱加药泵2——手动频率","C.M.PRO_cxsx_J2_AO_FB@spare"]
["冲洗碱加药泵2——故障","C.M.PRO_cxsx_J2_fre@Fault"]
["冲洗碱加药泵2——频率反馈","C.M.PRO_cxsx_J2_fre@out"]
["冲洗酸加药泵1——自动/手动","C.M.PRO_cxsx_S1@auto_select"]
["冲洗酸加药泵1——故障","C.M.PRO_cxsx_S1@fault_total"]
["冲洗酸加药泵1——远程","C.M.PRO_cxsx_S1@rem"]
["冲洗酸加药泵1——复位","C.M.PRO_cxsx_S1@reset"]
["冲洗酸加药泵1——运行反馈","C.M.PRO_cxsx_S1@run"]
["冲洗酸加药泵1——运行时间","C.M.PRO_cxsx_S1@run_time"]
["冲洗酸加药泵1——起泵","C.M.PRO_cxsx_S1@start"]
["冲洗酸加药泵1——停泵","C.M.PRO_cxsx_S1@stop"]
["冲洗酸加药泵1——手动频率","C.M.PRO_cxsx_S1_AO_FB@spare"]
["冲洗酸加药泵1——故障","C.M.PRO_cxsx_S1_fre@Fault"]
["冲洗酸加药泵1——频率反馈","C.M.PRO_cxsx_S1_fre@out"]
["冲洗酸加药泵2——自动/手动","C.M.PRO_cxsx_S2@auto_select"]
["冲洗酸加药泵2——故障","C.M.PRO_cxsx_S2@fault_total"]
["冲洗酸加药泵2——远程","C.M.PRO_cxsx_S2@rem"]
["冲洗酸加药泵2——复位","C.M.PRO_cxsx_S2@reset"]
["冲洗酸加药泵2——运行反馈","C.M.PRO_cxsx_S2@run"]
["冲洗酸加药泵2——运行时间","C.M.PRO_cxsx_S2@run_time"]
["冲洗酸加药泵2——起泵","C.M.PRO_cxsx_S2@start"]
["冲洗酸加药泵2——停泵","C.M.PRO_cxsx_S2@stop"]
["冲洗酸加药泵2——手动频率","C.M.PRO_cxsx_S2_AO_FB@spare"]
["冲洗酸加药泵2——故障","C.M.PRO_cxsx_S2_fre@Fault"]
["冲洗酸加药泵2——频率反馈","C.M.PRO_cxsx_S2_fre@out"]
["非氧产水加药——水量","C.M.RO_FYcsJY[0]"]
["非氧产水加药——加药浓度设定","C.M.RO_FYcsJY[1]"]
["非氧产水加药——冲程设定","C.M.RO_FYcsJY[2]"]
["非氧产水加药——系数","C.M.RO_FYcsJY[3]"]
["非氧产水加药——频率输出","C.M.RO_FYcsJY[4]"]
["非氧产水加药——备用","C.M.RO_FYcsJY[5]"]
["RO产水池联动数量设置 L","C.M.ArrRO_cscLDnum_1_0"]
["RO产水池联动数量设置 H1","C.M.ArrRO_cscLDnum_1_1"]
["RO产水池联动数量设置 H2","C.M.ArrRO_cscLDnum_1_2"]
["RO产水池联动数量设置 H3","C.M.ArrRO_cscLDnum_1_3"]
["RO产水池联动数量设置 H4","C.M.ArrRO_cscLDnum_1_4"]
["RO进水池联动数量设置 L","C.M.ArrRO_jscLDnum_1_0"]
["RO进水池联动数量设置 H1","C.M.ArrRO_jscLDnum_1_1"]
["RO进水池联动数量设置 H2","C.M.ArrRO_jscLDnum_1_2"]
["RO进水池联动数量设置 H3","C.M.ArrRO_jscLDnum_1_3"]
["RO进水池联动数量设置 H4","C.M.ArrRO_jscLDnum_1_4"]
["RO产水池联动标志 L","C.M.ArrROcsc_LDFlag_1_0"]
["RO产水池联动标志 H1","C.M.ArrROcsc_LDFlag_1_1"]
["RO产水池联动标志 H2","C.M.ArrROcsc_LDFlag_1_2"]
["RO产水池联动标志 H3","C.M.ArrROcsc_LDFlag_1_3"]
["RO产水池联动标志 H4","C.M.ArrROcsc_LDFlag_1_4"]
["RO产水池联动液位设置 L","C.M.ArrROcsc_LDYW_1_0"]
["RO产水池联动液位设置 H1","C.M.ArrROcsc_LDYW_1_1"]
["RO产水池联动液位设置 H2","C.M.ArrROcsc_LDYW_1_2"]
["RO产水池联动液位设置 H3","C.M.ArrROcsc_LDYW_1_3"]
["RO产水池联动液位设置 H4","C.M.ArrROcsc_LDYW_1_4"]
["RO进水池联动标志 L","C.M.ArrROjsc_LDFlag_1_0"]
["RO进水池联动标志 H1","C.M.ArrROjsc_LDFlag_1_1"]
["RO进水池联动标志 H2","C.M.ArrROjsc_LDFlag_1_2"]
["RO进水池联动标志 H3","C.M.ArrROjsc_LDFlag_1_3"]
["RO进水池联动标志 H4","C.M.ArrROjsc_LDFlag_1_4"]
["RO进水池联动液位设置 L","C.M.ArrROjsc_LDYW_1_0"]
["RO进水池联动液位设置 H1","C.M.ArrROjsc_LDYW_1_1"]
["RO进水池联动液位设置 H2","C.M.ArrROjsc_LDYW_1_2"]
["RO进水池联动液位设置 H3","C.M.ArrROjsc_LDYW_1_3"]
["RO进水池联动液位设置 H4","C.M.ArrROjsc_LDYW_1_4"]
["还原剂 PID 选择","C.M.BT_hyj_PID"]
["PAC 加药阀 投用选择","C.M.BT_PACjyf_InUse"]
["RO 手动指定产水 按钮","C.M.BT_RO_ManCS"]
["RO流量联动产水 按钮","C.M.BT_ROFlowLD"]
["RO全自动启动 按钮","C.M.BT_ROsAuto"]
["RO液位联动选择","C.M.BT_ROYWLD"]
["BW优先 UF1","C.M.BW_First_Order[0]"]
["BW优先 UF2","C.M.BW_First_Order[1]"]
["BW优先 UF3","C.M.BW_First_Order[2]"]
["BW优先 UF4","C.M.BW_First_Order[3]"]
["CEB 申请 UF1","C.M.CEB_Apply[0]"]
["CEB 申请 UF2","C.M.CEB_Apply[1]"]
["CEB 申请 UF3","C.M.CEB_Apply[2]"]
["CEB 申请 UF4","C.M.CEB_Apply[3]"]
["CEB 应答 UF1","C.M.CEB_Apply[10]"]
["CEB 应答 UF2","C.M.CEB_Apply[11]"]
["CEB 应答 UF3","C.M.CEB_Apply[12]"]
["CEB 应答 UF4","C.M.CEB_Apply[13]"]
["外供流量 当天","C.M.FL_WG_day[0]"]
["外供流量 前1天","C.M.FL_WG_day[1]"]
["外供流量 前2天","C.M.FL_WG_day[2]"]
["外供流量 前3天","C.M.FL_WG_day[3]"]
["外供流量 前4天","C.M.FL_WG_day[4]"]
["备用","C.M.FL_WG_day[5]"]
["备用","C.M.FL_WG_day[6]"]
["备用","C.M.FL_WG_day[7]"]
["备用","C.M.FL_WG_day[8]"]
["备用","C.M.FL_WG_day[9]"]
["还原剂频率输出","C.M.HYJ_out_Final"]
["还原剂PID 设置 I值","C.M.HYJ_PID_I"]
["还原剂PID 设置 P值","C.M.HYJ_PID_P"]
["还原剂PID 目标值 ","C.M.HYJ_PID_SP"]
["PAC频率输出","C.M.PACFreSetRead[0]"]
["PAC频率设置 1","C.M.PACFreSetRead[1]"]
["PAC频率设置 2","C.M.PACFreSetRead[2]"]
["PAC频率设置 3","C.M.PACFreSetRead[3]"]
["PAC频率设置 4","C.M.PACFreSetRead[4]"]
["PAC数量输出","C.M.PACNumSetRead[0]"]
["PAC数量设置 1","C.M.PACNumSetRead[1]"]
["PAC数量设置 2","C.M.PACNumSetRead[2]"]
["PAC数量设置 3","C.M.PACNumSetRead[3]"]
["PAC数量设置 4","C.M.PACNumSetRead[4]"]
["RO产水数量","C.M.RO_CStotalNum"]
["单套产水基准值","C.M.RO_FlowLDBasicF"]
["清水池与外供联动后需要RO套数","C.M.RO_FLOWLDHNum"]
["外供流量需要RO套数","C.M.RO_FlowLDNum"]
["RO运行数量","C.M.RO_RunNum"]
["RO自动运行数量输出","C.M.RO_RunNumFinalSet"]
["RO联动UF数量","C.M.RO_UF_NeedNum"]
["RO自动可用数量","C.M.ROAutoReadyNumSSD"]
["RO自动运行数量输出","C.M.ROAutoRunNumSSD"]
["RO产水池联动数量","C.M.ROcscLDnum"]
["RO进水池联动数量","C.M.ROjscLDnum"]
["RO手动联动数量","C.M.ROManLDnum"]
["RO准备好数量","C.M.ROReadyRunNum"]
["RO液位联动数量","C.M.ROYWLDnum"]
["UF产水结束信号","C.M.UF_CSendingApply"]
["UF产水中数量","C.M.UF_CSingNum"]
["UF 准备好数量","C.M.UF_readyCSNum"]
["UF1 渗透率","C.M.UF1_Count[0]"]
["UF1 产水进度","C.M.UF1_Count[4]"]
["RO1 产水进度","C.M.UF1_Count[5]"]
["UF1 CEB 进度","C.M.UF1_Count[6]"]
["总进水流量","C.M.UF1_Count[7]"]
["UF2 渗透率","C.M.UF2_Count[0]"]
["中间值，不用读","C.M.UF2_Count[3]"]
["UF2 产水进度","C.M.UF2_Count[4]"]
["RO2 产水进度","C.M.UF2_Count[5]"]
["UF2 CEB 进度","C.M.UF2_Count[6]"]
["总进水流量","C.M.UF2_Count[7]"]
["UF3 渗透率","C.M.UF3_Count[0]"]
["中间值，不用读","C.M.UF3_Count[3]"]
["UF3 产水进度","C.M.UF3_Count[4]"]
["RO3 产水进度","C.M.UF3_Count[5]"]
["UF3 CEB 进度","C.M.UF3_Count[6]"]
["总进水流量","C.M.UF3_Count[7]"]
["UF4 渗透率","C.M.UF4_Count[0]"]
["中间值，不用读","C.M.UF4_Count[3]"]
["UF4 产水进度","C.M.UF4_Count[4]"]
["RO4 产水进度","C.M.UF4_Count[5]"]
["UF4 CEB 进度","C.M.UF4_Count[6]"]
["总进水流量","C.M.UF4_Count[7]"]
["暂留1（不确定）","C.M.AL_LS_CSMG_L"]
["暂留2（不确定）","C.M.AL_LS_HCl_L"]
["暂留3（不确定）","C.M.AL_LS_HYJ1_L"]
["暂留4（不确定）","C.M.AL_LS_HYJ2_L"]
["暂留5（不确定）","C.M.AL_LS_NaClO_L"]
["暂留6（不确定）","C.M.AL_LS_NaOH_L"]
["暂留7（不确定）","C.M.AL_LS_PAC_L"]
["暂留8（不确定）","C.M.AL_LS_QSC_L"]
["暂留9（不确定）","C.M.AL_LS_SJJ_L"]
["暂留10（不确定）","C.M.AL_LS_UFFXSC_L"]
["暂留11（不确定）","C.M.AL_LS_UFJSC_L"]
["暂留12（不确定）","C.M.AL_LS_ZGJ_L"]
["暂留13（不确定）","C.M.AL_RO_LS_JSZG_L"]
["暂留14（不确定）","C.M.AL_RO1_LS_DJB_H"]
["暂留15（不确定）","C.M.AL_RO1_LS_DJB_L"]
["暂留16（不确定）","C.M.AL_RO1_LS_GYB_H"]
["暂留17（不确定）","C.M.AL_RO1_LS_GYB_L"]
["暂留18（不确定）","C.M.AL_RO2_LS_DJB_H"]
["暂留19（不确定）","C.M.AL_RO2_LS_DJB_L"]
["暂留20（不确定）","C.M.AL_RO2_LS_GYB_H"]
["暂留21（不确定）","C.M.AL_RO2_LS_GYB_L"]
["暂留22（不确定）","C.M.AL_RO3_LS_DJB_H"]
["暂留23（不确定）","C.M.AL_RO3_LS_DJB_L"]
["暂留24（不确定）","C.M.AL_RO3_LS_GYB_H"]
["暂留25（不确定）","C.M.AL_RO3_LS_GYB_L"]
["暂留26（不确定）","C.M.AL_RO4_LS_DJB_H"]
["暂留27（不确定）","C.M.AL_RO4_LS_DJB_L"]
["暂留28（不确定）","C.M.AL_RO4_LS_GYB_H"]
["暂留29（不确定）","C.M.AL_RO4_LS_GYB_L"]
["暂留30（不确定）","C.M.AL_UF1_LS1"]
["暂留31（不确定）","C.M.AL_UF1_LS2"]
["暂留32（不确定）","C.M.AL_UF1_LS3"]
["暂留33（不确定）","C.M.AL_UF1_LS4"]
["暂留34（不确定）","C.M.AL_UF2_LS1"]
["暂留35（不确定）","C.M.AL_UF2_LS2"]
["暂留36（不确定）","C.M.AL_UF2_LS3"]
["暂留37（不确定）","C.M.AL_UF2_LS4"]
["暂留38（不确定）","C.M.AL_UF3_LS1"]
["暂留39（不确定）","C.M.AL_UF3_LS2"]
["暂留40（不确定）","C.M.AL_UF3_LS3"]
["暂留41（不确定）","C.M.AL_UF3_LS4"]
["暂留42（不确定）","C.M.AL_UF4_LS1"]
["暂留43（不确定）","C.M.AL_UF4_LS2"]
["暂留44（不确定）","C.M.AL_UF4_LS3"]
["暂留45（不确定）","C.M.AL_UF4_LS4"]
["盐酸加药阀(CEB)手自动","C.M.CEB_HCl@auto_select"]
["盐酸加药阀(CEB)关操作","C.M.CEB_HCl@close"]
["盐酸加药阀(CEB)关到位","C.M.CEB_HCl@close_feedback"]
["盐酸加药阀(CEB)故障","C.M.CEB_HCl@fault_total"]
["盐酸加药阀(CEB)开操作","C.M.CEB_HCl@open"]
["盐酸加药阀(CEB)开到位","C.M.CEB_HCl@open_feedback"]
["盐酸加药阀(CEB)远程","C.M.CEB_HCl@rem"]
["盐酸加药阀(CEB)复位","C.M.CEB_HCl@reset"]
["NaClO加药阀(CEB)手自动","C.M.CEB_NaClO@auto_select"]
["NaClO加药阀(CEB)关操作","C.M.CEB_NaClO@close"]
["NaClO加药阀(CEB)关到位","C.M.CEB_NaClO@close_feedback"]
["NaClO加药阀(CEB)故障","C.M.CEB_NaClO@fault_total"]
["NaClO加药阀(CEB)开操作","C.M.CEB_NaClO@open"]
["NaClO加药阀(CEB)开到位","C.M.CEB_NaClO@open_feedback"]
["NaClO加药阀(CEB)远程","C.M.CEB_NaClO@rem"]
["NaClO加药阀(CEB)复位","C.M.CEB_NaClO@reset"]
["NaOH加药阀(CEB)手自动","C.M.CEB_NaOH@auto_select"]
["NaOH加药阀(CEB)关操作","C.M.CEB_NaOH@close"]
["NaOH加药阀(CEB)关到位","C.M.CEB_NaOH@close_feedback"]
["NaOH加药阀(CEB)故障","C.M.CEB_NaOH@fault_total"]
["NaOH加药阀(CEB)开操作","C.M.CEB_NaOH@open"]
["NaOH加药阀(CEB)开到位","C.M.CEB_NaOH@open_feedback"]
["NaOH加药阀(CEB)远程","C.M.CEB_NaOH@rem"]
["NaOH加药阀(CEB)复位","C.M.CEB_NaOH@reset"]
["1#CIP清洗水泵手自动","C.M.CIP_QXB1@auto_select"]
["1#CIP清洗水泵故障","C.M.CIP_QXB1@fault_total"]
["1#CIP清洗水泵远程","C.M.CIP_QXB1@rem"]
["1#CIP清洗水泵复位","C.M.CIP_QXB1@reset"]
["1#CIP清洗水泵运行","C.M.CIP_QXB1@run"]
["1#CIP清洗水泵运行时间","C.M.CIP_QXB1@run_time"]
["1#CIP清洗水泵启动操作","C.M.CIP_QXB1@start"]
["1#CIP清洗水泵停止操作","C.M.CIP_QXB1@stop"]
["1#CIP清洗水泵电流报警","C.M.CIP_QXB1_A@Fault"]
["1#CIP清洗水泵电流高报警","C.M.CIP_QXB1_A@H_AL"]
["1#CIP清洗水泵电流高报警开关","C.M.CIP_QXB1_A@H_AL_ON"]
["1#CIP清洗水泵电流高限设置","C.M.CIP_QXB1_A@H_AL_set"]
["1#CIP清洗水泵电流低报警","C.M.CIP_QXB1_A@L_AL"]
["1#CIP清洗水泵电流低报警开关","C.M.CIP_QXB1_A@L_AL_ON"]
["1#CIP清洗水泵电流低限设置","C.M.CIP_QXB1_A@L_AL_set"]
["1#CIP清洗水泵运行电流","C.M.CIP_QXB1_A@out"]
["1#CIP清洗水泵设置频率","C.M.CIP_QXB1_AO_FB@spare"]
["1#CIP清洗水泵频率报警","C.M.CIP_QXB1_fre@Fault"]
["1#CIP清洗水泵频率高报警","C.M.CIP_QXB1_fre@H_AL"]
["1#CIP清洗水泵频率高报警开关","C.M.CIP_QXB1_fre@H_AL_ON"]
["1#CIP清洗水泵频率高限设置","C.M.CIP_QXB1_fre@H_AL_set"]
["1#CIP清洗水泵频率低报警","C.M.CIP_QXB1_fre@L_AL"]
["1#CIP清洗水泵频率低报警开关","C.M.CIP_QXB1_fre@L_AL_ON"]
["1#CIP清洗水泵频率低限设置","C.M.CIP_QXB1_fre@L_AL_set"]
["1#CIP清洗水泵运行频率","C.M.CIP_QXB1_fre@out"]
["2#CIP清洗水泵手自动","C.M.CIP_QXB2@auto_select"]
["2#CIP清洗水泵故障","C.M.CIP_QXB2@fault_total"]
["2#CIP清洗水泵远程","C.M.CIP_QXB2@rem"]
["2#CIP清洗水泵复位","C.M.CIP_QXB2@reset"]
["2#CIP清洗水泵运行","C.M.CIP_QXB2@run"]
["2#CIP清洗水泵运行时间","C.M.CIP_QXB2@run_time"]
["2#CIP清洗水泵启动操作","C.M.CIP_QXB2@start"]
["2#CIP清洗水泵停止操作","C.M.CIP_QXB2@stop"]
["2#CIP清洗水泵电流报警","C.M.CIP_QXB2_A@Fault"]
["2#CIP清洗水泵电流高报警","C.M.CIP_QXB2_A@H_AL"]
["2#CIP清洗水泵电流高报警开关","C.M.CIP_QXB2_A@H_AL_ON"]
["2#CIP清洗水泵电流高限设置","C.M.CIP_QXB2_A@H_AL_set"]
["2#CIP清洗水泵电流低报警","C.M.CIP_QXB2_A@L_AL"]
["2#CIP清洗水泵电流低报警开关","C.M.CIP_QXB2_A@L_AL_ON"]
["2#CIP清洗水泵电流低限设置","C.M.CIP_QXB2_A@L_AL_set"]
["2#CIP清洗水泵运行电流","C.M.CIP_QXB2_A@out"]
["2#CIP清洗水泵设置频率","C.M.CIP_QXB2_AO_FB@spare"]
["2#CIP清洗水泵频率报警","C.M.CIP_QXB2_fre@Fault"]
["2#CIP清洗水泵频率高报警","C.M.CIP_QXB2_fre@H_AL"]
["2#CIP清洗水泵频率高报警开关","C.M.CIP_QXB2_fre@H_AL_ON"]
["2#CIP清洗水泵频率高限设置","C.M.CIP_QXB2_fre@H_AL_set"]
["2#CIP清洗水泵频率低报警","C.M.CIP_QXB2_fre@L_AL"]
["2#CIP清洗水泵频率低报警开关","C.M.CIP_QXB2_fre@L_AL_ON"]
["2#CIP清洗水泵频率低限设置","C.M.CIP_QXB2_fre@L_AL_set"]
["2#CIP清洗水泵运行频率","C.M.CIP_QXB2_fre@out"]
["CIP出水阀手自动","C.M.CIP_QXCSF@auto_select"]
["CIP出水阀关操作","C.M.CIP_QXCSF@close"]
["CIP出水阀关到位","C.M.CIP_QXCSF@close_feedback"]
["CIP出水阀故障","C.M.CIP_QXCSF@fault_total"]
["CIP出水阀开操作","C.M.CIP_QXCSF@open"]
["CIP出水阀开到位","C.M.CIP_QXCSF@open_feedback"]
["CIP出水阀远程","C.M.CIP_QXCSF@rem"]
["CIP出水阀复位","C.M.CIP_QXCSF@reset"]
["CIP循环阀手自动","C.M.CIP_QXXHF@auto_select"]
["CIP循环阀关操作","C.M.CIP_QXXHF@close"]
["CIP循环阀关到位","C.M.CIP_QXXHF@close_feedback"]
["CIP循环阀故障","C.M.CIP_QXXHF@fault_total"]
["CIP循环阀开操作","C.M.CIP_QXXHF@open"]
["CIP循环阀开到位","C.M.CIP_QXXHF@open_feedback"]
["CIP循环阀远程","C.M.CIP_QXXHF@rem"]
["CIP循环阀复位","C.M.CIP_QXXHF@reset"]
["外排水余氯报警","C.M.Cl_WPS@fault"]
["外排水余氯高报警","C.M.Cl_WPS@H_AL"]
["外排水余氯高报警开关","C.M.Cl_WPS@H_AL_ON"]
["外排水余氯高限设置","C.M.Cl_WPS@H_AL_set"]
["外排水余氯低报警","C.M.Cl_WPS@L_AL"]
["外排水余氯低报警开关","C.M.Cl_WPS@L_AL_ON"]
["外排水余氯低限设置","C.M.Cl_WPS@L_AL_set"]
["外排水余氯","C.M.Cl_WPS@out"]
["1#NaClO加药泵(出水)手自动","C.M.CS_NaClO1@auto_select"]
["1#NaClO加药泵(出水)故障","C.M.CS_NaClO1@fault_total"]
["1#NaClO加药泵(出水)远程","C.M.CS_NaClO1@rem"]
["1#NaClO加药泵(出水)复位","C.M.CS_NaClO1@reset"]
["1#NaClO加药泵(出水)运行","C.M.CS_NaClO1@run"]
["1#NaClO加药泵(出水)运行时间","C.M.CS_NaClO1@run_time"]
["1#NaClO加药泵(出水)启动操作","C.M.CS_NaClO1@start"]
["1#NaClO加药泵(出水)停止操作","C.M.CS_NaClO1@stop"]
["1#NaClO加药泵(出水)设置频率","C.M.CS_NaClO1_AO_FB@spare"]
["1#NaClO加药泵(出水)频率报警","C.M.CS_NaClO1_fre@Fault"]
["1#NaClO加药泵(出水)频率高报警","C.M.CS_NaClO1_fre@H_AL"]
["1#NaClO加药泵(出水)频率高报警开关","C.M.CS_NaClO1_fre@H_AL_ON"]
["1#NaClO加药泵(出水)频率高限设置","C.M.CS_NaClO1_fre@H_AL_set"]
["1#NaClO加药泵(出水)频率低报警","C.M.CS_NaClO1_fre@L_AL"]
["1#NaClO加药泵(出水)频率低报警开关","C.M.CS_NaClO1_fre@L_AL_ON"]
["1#NaClO加药泵(出水)频率低限设置","C.M.CS_NaClO1_fre@L_AL_set"]
["1#NaClO加药泵(出水)运行频率","C.M.CS_NaClO1_fre@out"]
["2#NaClO加药泵(出水)手自动","C.M.CS_NaClO2@auto_select"]
["2#NaClO加药泵(出水)故障","C.M.CS_NaClO2@fault_total"]
["2#NaClO加药泵(出水)远程","C.M.CS_NaClO2@rem"]
["2#NaClO加药泵(出水)复位","C.M.CS_NaClO2@reset"]
["2#NaClO加药泵(出水)运行","C.M.CS_NaClO2@run"]
["2#NaClO加药泵(出水)运行时间","C.M.CS_NaClO2@run_time"]
["2#NaClO加药泵(出水)启动操作","C.M.CS_NaClO2@start"]
["2#NaClO加药泵(出水)停止操作","C.M.CS_NaClO2@stop"]
["2#NaClO加药泵(出水)设置频率","C.M.CS_NaClO2_AO_FB@spare"]
["2#NaClO加药泵(出水)频率报警","C.M.CS_NaClO2_fre@Fault"]
["2#NaClO加药泵(出水)频率高报警","C.M.CS_NaClO2_fre@H_AL"]
["2#NaClO加药泵(出水)频率高报警开关","C.M.CS_NaClO2_fre@H_AL_ON"]
["2#NaClO加药泵(出水)频率高限设置","C.M.CS_NaClO2_fre@H_AL_set"]
["2#NaClO加药泵(出水)频率低报警","C.M.CS_NaClO2_fre@L_AL"]
["2#NaClO加药泵(出水)频率低报警开关","C.M.CS_NaClO2_fre@L_AL_ON"]
["2#NaClO加药泵(出水)频率低限设置","C.M.CS_NaClO2_fre@L_AL_set"]
["2#NaClO加药泵(出水)运行频率","C.M.CS_NaClO2_fre@out"]
["膜车间1#排风扇手自动","C.M.Fan1@auto_select"]
["膜车间1#排风扇故障","C.M.Fan1@fault_total"]
["膜车间1#排风扇远程","C.M.Fan1@rem"]
["膜车间1#排风扇复位","C.M.Fan1@reset"]
["膜车间1#排风扇运行","C.M.Fan1@run"]
["膜车间1#排风扇运行时间","C.M.Fan1@run_time"]
["膜车间1#排风扇启动操作","C.M.Fan1@start"]
["膜车间1#排风扇停止操作","C.M.Fan1@stop"]
["膜车间2#排风扇手自动","C.M.Fan2@auto_select"]
["膜车间2#排风扇故障","C.M.Fan2@fault_total"]
["膜车间2#排风扇远程","C.M.Fan2@rem"]
["膜车间2#排风扇复位","C.M.Fan2@reset"]
["膜车间2#排风扇运行","C.M.Fan2@run"]
["膜车间2#排风扇运行时间","C.M.Fan2@run_time"]
["膜车间2#排风扇启动操作","C.M.Fan2@start"]
["膜车间2#排风扇停止操作","C.M.Fan2@stop"]
["膜车间3#排风扇手自动","C.M.Fan3@auto_select"]
["膜车间3#排风扇故障","C.M.Fan3@fault_total"]
["膜车间3#排风扇远程","C.M.Fan3@rem"]
["膜车间3#排风扇复位","C.M.Fan3@reset"]
["膜车间3#排风扇运行","C.M.Fan3@run"]
["膜车间3#排风扇运行时间","C.M.Fan3@run_time"]
["膜车间3#排风扇启动操作","C.M.Fan3@start"]
["膜车间3#排风扇停止操作","C.M.Fan3@stop"]
["膜车间4#排风扇手自动","C.M.Fan4@auto_select"]
["膜车间4#排风扇故障","C.M.Fan4@fault_total"]
["膜车间4#排风扇远程","C.M.Fan4@rem"]
["膜车间4#排风扇复位","C.M.Fan4@reset"]
["膜车间4#排风扇运行","C.M.Fan4@run"]
["膜车间4#排风扇运行时间","C.M.Fan4@run_time"]
["膜车间4#排风扇启动操作","C.M.Fan4@start"]
["膜车间4#排风扇停止操作","C.M.Fan4@stop"]
["膜车间5#排风扇手自动","C.M.Fan5@auto_select"]
["膜车间5#排风扇故障","C.M.Fan5@fault_total"]
["膜车间5#排风扇远程","C.M.Fan5@rem"]
["膜车间5#排风扇复位","C.M.Fan5@reset"]
["膜车间5#排风扇运行","C.M.Fan5@run"]
["膜车间5#排风扇运行时间","C.M.Fan5@run_time"]
["膜车间5#排风扇启动操作","C.M.Fan5@start"]
["膜车间5#排风扇停止操作","C.M.Fan5@stop"]
["膜车间6#排风扇手自动","C.M.Fan6@auto_select"]
["膜车间6#排风扇故障","C.M.Fan6@fault_total"]
["膜车间6#排风扇远程","C.M.Fan6@rem"]
["膜车间6#排风扇复位","C.M.Fan6@reset"]
["膜车间6#排风扇运行","C.M.Fan6@run"]
["膜车间6#排风扇运行时间","C.M.Fan6@run_time"]
["膜车间6#排风扇启动操作","C.M.Fan6@start"]
["膜车间6#排风扇停止操作","C.M.Fan6@stop"]
["水泵间1#排风扇手自动","C.M.Fan7@auto_select"]
["水泵间1#排风扇故障","C.M.Fan7@fault_total"]
["水泵间1#排风扇远程","C.M.Fan7@rem"]
["水泵间1#排风扇复位","C.M.Fan7@reset"]
["水泵间1#排风扇运行","C.M.Fan7@run"]
["水泵间1#排风扇运行时间","C.M.Fan7@run_time"]
["水泵间1#排风扇启动操作","C.M.Fan7@start"]
["水泵间1#排风扇停止操作","C.M.Fan7@stop"]
["水泵间2#排风扇手自动","C.M.Fan8@auto_select"]
["水泵间2#排风扇故障","C.M.Fan8@fault_total"]
["水泵间2#排风扇远程","C.M.Fan8@rem"]
["水泵间2#排风扇复位","C.M.Fan8@reset"]
["水泵间2#排风扇运行","C.M.Fan8@run"]
["水泵间2#排风扇运行时间","C.M.Fan8@run_time"]
["水泵间2#排风扇启动操作","C.M.Fan8@start"]
["水泵间2#排风扇停止操作","C.M.Fan8@stop"]
["水泵间3#排风扇手自动","C.M.Fan9@auto_select"]
["水泵间3#排风扇故障","C.M.Fan9@fault_total"]
["水泵间3#排风扇远程","C.M.Fan9@rem"]
["水泵间3#排风扇复位","C.M.Fan9@reset"]
["水泵间3#排风扇运行","C.M.Fan9@run"]
["水泵间3#排风扇运行时间","C.M.Fan9@run_time"]
["水泵间3#排风扇启动操作","C.M.Fan9@start"]
["水泵间3#排风扇停止操作","C.M.Fan9@stop"]
["水泵间4#排风扇手自动","C.M.Fan10@auto_select"]
["水泵间4#排风扇故障","C.M.Fan10@fault_total"]
["水泵间4#排风扇远程","C.M.Fan10@rem"]
["水泵间4#排风扇复位","C.M.Fan10@reset"]
["水泵间4#排风扇运行","C.M.Fan10@run"]
["水泵间4#排风扇运行时间","C.M.Fan10@run_time"]
["水泵间4#排风扇启动操作","C.M.Fan10@start"]
["水泵间4#排风扇停止操作","C.M.Fan10@stop"]
["水泵间5#排风扇手自动","C.M.Fan11@auto_select"]
["水泵间5#排风扇故障","C.M.Fan11@fault_total"]
["水泵间5#排风扇远程","C.M.Fan11@rem"]
["水泵间5#排风扇复位","C.M.Fan11@reset"]
["水泵间5#排风扇运行","C.M.Fan11@run"]
["水泵间5#排风扇运行时间","C.M.Fan11@run_time"]
["水泵间5#排风扇启动操作","C.M.Fan11@start"]
["水泵间5#排风扇停止操作","C.M.Fan11@stop"]
["水泵间6#排风扇手自动","C.M.Fan12@auto_select"]
["水泵间6#排风扇故障","C.M.Fan12@fault_total"]
["水泵间6#排风扇远程","C.M.Fan12@rem"]
["水泵间6#排风扇复位","C.M.Fan12@reset"]
["水泵间6#排风扇运行","C.M.Fan12@run"]
["水泵间6#排风扇运行时间","C.M.Fan12@run_time"]
["水泵间6#排风扇启动操作","C.M.Fan12@start"]
["水泵间6#排风扇停止操作","C.M.Fan12@stop"]
["水泵间7#排风扇手自动","C.M.Fan13@auto_select"]
["水泵间7#排风扇故障","C.M.Fan13@fault_total"]
["水泵间7#排风扇远程","C.M.Fan13@rem"]
["水泵间7#排风扇复位","C.M.Fan13@reset"]
["水泵间7#排风扇运行","C.M.Fan13@run"]
["水泵间7#排风扇运行时间","C.M.Fan13@run_time"]
["水泵间7#排风扇启动操作","C.M.Fan13@start"]
["水泵间7#排风扇停止操作","C.M.Fan13@stop"]
["水泵间8#排风扇手自动","C.M.Fan14@auto_select"]
["水泵间8#排风扇故障","C.M.Fan14@fault_total"]
["水泵间8#排风扇远程","C.M.Fan14@rem"]
["水泵间8#排风扇复位","C.M.Fan14@reset"]
["水泵间8#排风扇运行","C.M.Fan14@run"]
["水泵间8#排风扇运行时间","C.M.Fan14@run_time"]
["水泵间8#排风扇启动操作","C.M.Fan14@start"]
["水泵间8#排风扇停止操作","C.M.Fan14@stop"]
["中控室排风扇手自动","C.M.Fan15@auto_select"]
["中控室排风扇故障","C.M.Fan15@fault_total"]
["中控室排风扇远程","C.M.Fan15@rem"]
["中控室排风扇复位","C.M.Fan15@reset"]
["中控室排风扇运行","C.M.Fan15@run"]
["中控室排风扇运行时间","C.M.Fan15@run_time"]
["中控室排风扇启动操作","C.M.Fan15@start"]
["中控室排风扇停止操作","C.M.Fan15@stop"]
["楼梯间1#排风扇手自动","C.M.Fan16@auto_select"]
["楼梯间1#排风扇故障","C.M.Fan16@fault_total"]
["楼梯间1#排风扇远程","C.M.Fan16@rem"]
["楼梯间1#排风扇复位","C.M.Fan16@reset"]
["楼梯间1#排风扇运行","C.M.Fan16@run"]
["楼梯间1#排风扇运行时间","C.M.Fan16@run_time"]
["楼梯间1#排风扇启动操作","C.M.Fan16@start"]
["楼梯间1#排风扇停止操作","C.M.Fan16@stop"]
["楼梯间2#排风扇手自动","C.M.Fan17@auto_select"]
["楼梯间2#排风扇故障","C.M.Fan17@fault_total"]
["楼梯间2#排风扇远程","C.M.Fan17@rem"]
["楼梯间2#排风扇复位","C.M.Fan17@reset"]
["楼梯间2#排风扇运行","C.M.Fan17@run"]
["楼梯间2#排风扇运行时间","C.M.Fan17@run_time"]
["楼梯间2#排风扇启动操作","C.M.Fan17@start"]
["楼梯间2#排风扇停止操作","C.M.Fan17@stop"]
["高配室排风扇手自动","C.M.Fan18@auto_select"]
["高配室排风扇故障","C.M.Fan18@fault_total"]
["高配室排风扇远程","C.M.Fan18@rem"]
["高配室排风扇复位","C.M.Fan18@reset"]
["高配室排风扇运行","C.M.Fan18@run"]
["高配室排风扇运行时间","C.M.Fan18@run_time"]
["高配室排风扇启动操作","C.M.Fan18@start"]
["高配室排风扇停止操作","C.M.Fan18@stop"]
["低配室1#排风扇手自动","C.M.Fan19@auto_select"]
["低配室1#排风扇故障","C.M.Fan19@fault_total"]
["低配室1#排风扇远程","C.M.Fan19@rem"]
["低配室1#排风扇复位","C.M.Fan19@reset"]
["低配室1#排风扇运行","C.M.Fan19@run"]
["低配室1#排风扇运行时间","C.M.Fan19@run_time"]
["低配室1#排风扇启动操作","C.M.Fan19@start"]
["低配室1#排风扇停止操作","C.M.Fan19@stop"]
["低配室2#排风扇手自动","C.M.Fan20@auto_select"]
["低配室2#排风扇故障","C.M.Fan20@fault_total"]
["低配室2#排风扇远程","C.M.Fan20@rem"]
["低配室2#排风扇复位","C.M.Fan20@reset"]
["低配室2#排风扇运行","C.M.Fan20@run"]
["低配室2#排风扇运行时间","C.M.Fan20@run_time"]
["低配室2#排风扇启动操作","C.M.Fan20@start"]
["低配室2#排风扇停止操作","C.M.Fan20@stop"]
["加药间1#排风扇手自动","C.M.Fan21@auto_select"]
["加药间1#排风扇故障","C.M.Fan21@fault_total"]
["加药间1#排风扇远程","C.M.Fan21@rem"]
["加药间1#排风扇复位","C.M.Fan21@reset"]
["加药间1#排风扇运行","C.M.Fan21@run"]
["加药间1#排风扇运行时间","C.M.Fan21@run_time"]
["加药间1#排风扇启动操作","C.M.Fan21@start"]
["加药间1#排风扇停止操作","C.M.Fan21@stop"]
["加药间2#排风扇手自动","C.M.Fan22@auto_select"]
["加药间2#排风扇故障","C.M.Fan22@fault_total"]
["加药间2#排风扇远程","C.M.Fan22@rem"]
["加药间2#排风扇复位","C.M.Fan22@reset"]
["加药间2#排风扇运行","C.M.Fan22@run"]
["加药间2#排风扇运行时间","C.M.Fan22@run_time"]
["加药间2#排风扇启动操作","C.M.Fan22@start"]
["加药间2#排风扇停止操作","C.M.Fan22@stop"]
["小加药间1#排风扇手自动","C.M.Fan23@auto_select"]
["小加药间1#排风扇故障","C.M.Fan23@fault_total"]
["小加药间1#排风扇远程","C.M.Fan23@rem"]
["小加药间1#排风扇复位","C.M.Fan23@reset"]
["小加药间1#排风扇运行","C.M.Fan23@run"]
["小加药间1#排风扇运行时间","C.M.Fan23@run_time"]
["小加药间1#排风扇启动操作","C.M.Fan23@start"]
["小加药间1#排风扇停止操作","C.M.Fan23@stop"]
["小加药间2#排风扇手自动","C.M.Fan24@auto_select"]
["小加药间2#排风扇故障","C.M.Fan24@fault_total"]
["小加药间2#排风扇远程","C.M.Fan24@rem"]
["小加药间2#排风扇复位","C.M.Fan24@reset"]
["小加药间2#排风扇运行","C.M.Fan24@run"]
["小加药间2#排风扇运行时间","C.M.Fan24@run_time"]
["小加药间2#排风扇启动操作","C.M.Fan24@start"]
["小加药间2#排风扇停止操作","C.M.Fan24@stop"]
["外供累计流量","C.M.flow_ZCS_acc"]
["外供累计流量清零","C.M.flow_ZCS_acc_reset"]
["CIP流量报警","C.M.FT_CIP@fault"]
["CIP流量高报警","C.M.FT_CIP@H_AL"]
["CIP流量高报警开关","C.M.FT_CIP@H_AL_ON"]
["CIP流量高限设置","C.M.FT_CIP@H_AL_set"]
["CIP流量低报警","C.M.FT_CIP@L_AL"]
["CIP流量低报警开关","C.M.FT_CIP@L_AL_ON"]
["CIP流量低限设置","C.M.FT_CIP@L_AL_set"]
["CIP流量","C.M.FT_CIP@out"]
["补水流量报警","C.M.FT_FXSC@fault"]
["补水流量高报警","C.M.FT_FXSC@H_AL"]
["补水流量高报警开关","C.M.FT_FXSC@H_AL_ON"]
["补水流量高限设置","C.M.FT_FXSC@H_AL_set"]
["补水流量低报警","C.M.FT_FXSC@L_AL"]
["补水流量低报警开关","C.M.FT_FXSC@L_AL_ON"]
["补水流量低限设置","C.M.FT_FXSC@L_AL_set"]
["补水流量","C.M.FT_FXSC@out"]
["补水流量设定值","C.M.FT_FXSCBS_set"]
["还原剂流量报警","C.M.FT_HYJJY1@fault"]
["还原剂流量高报警","C.M.FT_HYJJY1@H_AL"]
["还原剂流量高报警开关","C.M.FT_HYJJY1@H_AL_ON"]
["还原剂流量高限设置","C.M.FT_HYJJY1@H_AL_set"]
["还原剂流量低报警","C.M.FT_HYJJY1@L_AL"]
["还原剂流量低报警开关","C.M.FT_HYJJY1@L_AL_ON"]
["还原剂流量低限设置","C.M.FT_HYJJY1@L_AL_set"]
["还原剂流量","C.M.FT_HYJJY1@out"]
["总浓水排水流量报警","C.M.FT_NSPS@fault"]
["总浓水排水流量高报警","C.M.FT_NSPS@H_AL"]
["总浓水排水流量高报警开关","C.M.FT_NSPS@H_AL_ON"]
["总浓水排水流量高限设置","C.M.FT_NSPS@H_AL_set"]
["总浓水排水流量低报警","C.M.FT_NSPS@L_AL"]
["总浓水排水流量低报警开关","C.M.FT_NSPS@L_AL_ON"]
["总浓水排水流量低限设置","C.M.FT_NSPS@L_AL_set"]
["总浓水排水流量","C.M.FT_NSPS@out"]
["清水池流量报警","C.M.FT_QSC@fault"]
["清水池流量高报警","C.M.FT_QSC@H_AL"]
["清水池流量高报警开关","C.M.FT_QSC@H_AL_ON"]
["清水池流量高限设置","C.M.FT_QSC@H_AL_set"]
["清水池流量低报警","C.M.FT_QSC@L_AL"]
["清水池流量低报警开关","C.M.FT_QSC@L_AL_ON"]
["清水池流量低限设置","C.M.FT_QSC@L_AL_set"]
["清水池流量","C.M.FT_QSC@out"]
["未知1流量报警（不确定）","C.M.FT_ZGJ1@fault"]
["未知1流量高报警（不确定）","C.M.FT_ZGJ1@H_AL"]
["未知1流量高报警开关（不确定）","C.M.FT_ZGJ1@H_AL_ON"]
["未知1流量高限设置（不确定）","C.M.FT_ZGJ1@H_AL_set"]
["未知1流量低报警（不确定）","C.M.FT_ZGJ1@L_AL"]
["未知1流量低报警开关（不确定）","C.M.FT_ZGJ1@L_AL_ON"]
["未知1流量低限设置（不确定）","C.M.FT_ZGJ1@L_AL_set"]
["未知1流量（不确定）","C.M.FT_ZGJ1@out"]
["未知2流量报警（不确定）","C.M.FT_ZGJ2@fault"]
["未知2流量高报警（不确定）","C.M.FT_ZGJ2@H_AL"]
["未知2流量高报警开关（不确定）","C.M.FT_ZGJ2@H_AL_ON"]
["未知2流量高限设置（不确定）","C.M.FT_ZGJ2@H_AL_set"]
["未知2流量低报警（不确定）","C.M.FT_ZGJ2@L_AL"]
["未知2流量低报警开关（不确定）","C.M.FT_ZGJ2@L_AL_ON"]
["未知2流量低限设置（不确定）","C.M.FT_ZGJ2@L_AL_set"]
["未知2流量（不确定）","C.M.FT_ZGJ2@out"]
["未知3流量报警（不确定）","C.M.FT_ZGJ3@fault"]
["未知3流量高报警（不确定）","C.M.FT_ZGJ3@H_AL"]
["未知3流量高报警开关（不确定）","C.M.FT_ZGJ3@H_AL_ON"]
["未知3流量高限设置（不确定）","C.M.FT_ZGJ3@H_AL_set"]
["未知3流量低报警（不确定）","C.M.FT_ZGJ3@L_AL"]
["未知3流量低报警开关（不确定）","C.M.FT_ZGJ3@L_AL_ON"]
["未知3流量低限设置（不确定）","C.M.FT_ZGJ3@L_AL_set"]
["未知3流量（不确定）","C.M.FT_ZGJ3@out"]
["未知4流量报警（不确定）","C.M.FT_ZGJ4@fault"]
["未知4流量高报警（不确定）","C.M.FT_ZGJ4@H_AL"]
["未知4流量高报警开关（不确定）","C.M.FT_ZGJ4@H_AL_ON"]
["未知4流量高限设置（不确定）","C.M.FT_ZGJ4@H_AL_set"]
["未知4流量低报警（不确定）","C.M.FT_ZGJ4@L_AL"]
["未知4流量低报警开关（不确定）","C.M.FT_ZGJ4@L_AL_ON"]
["未知4流量低限设置（不确定）","C.M.FT_ZGJ4@L_AL_set"]
["未知4流量（不确定）","C.M.FT_ZGJ4@out"]
["未知5流量报警（不确定）","C.M.FT_ZGJ5@fault"]
["未知5流量高报警（不确定）","C.M.FT_ZGJ5@H_AL"]
["未知5流量高报警开关（不确定）","C.M.FT_ZGJ5@H_AL_ON"]
["未知5流量高限设置（不确定）","C.M.FT_ZGJ5@H_AL_set"]
["未知5流量低报警（不确定）","C.M.FT_ZGJ5@L_AL"]
["未知5流量低报警开关（不确定）","C.M.FT_ZGJ5@L_AL_ON"]
["未知5流量低限设置（不确定）","C.M.FT_ZGJ5@L_AL_set"]
["未知5流量（不确定）","C.M.FT_ZGJ5@out"]
["1#反渗透阻垢剂流量报警","C.M.FT_ZGJJY1@fault"]
["1#反渗透阻垢剂流量高报警","C.M.FT_ZGJJY1@H_AL"]
["1#反渗透阻垢剂流量高报警开关","C.M.FT_ZGJJY1@H_AL_ON"]
["1#反渗透阻垢剂流量高限设置","C.M.FT_ZGJJY1@H_AL_set"]
["1#反渗透阻垢剂流量低报警","C.M.FT_ZGJJY1@L_AL"]
["1#反渗透阻垢剂流量低报警开关","C.M.FT_ZGJJY1@L_AL_ON"]
["1#反渗透阻垢剂流量低限设置","C.M.FT_ZGJJY1@L_AL_set"]
["1#反渗透阻垢剂流量","C.M.FT_ZGJJY1@out"]
["2#反渗透阻垢剂流量报警","C.M.FT_ZGJJY2@fault"]
["2#反渗透阻垢剂流量高报警","C.M.FT_ZGJJY2@H_AL"]
["2#反渗透阻垢剂流量高报警开关","C.M.FT_ZGJJY2@H_AL_ON"]
["2#反渗透阻垢剂流量高限设置","C.M.FT_ZGJJY2@H_AL_set"]
["2#反渗透阻垢剂流量低报警","C.M.FT_ZGJJY2@L_AL"]
["2#反渗透阻垢剂流量低报警开关","C.M.FT_ZGJJY2@L_AL_ON"]
["2#反渗透阻垢剂流量低限设置","C.M.FT_ZGJJY2@L_AL_set"]
["2#反渗透阻垢剂流量","C.M.FT_ZGJJY2@out"]
["3#反渗透阻垢剂流量报警","C.M.FT_ZGJJY3@fault"]
["3#反渗透阻垢剂流量高报警","C.M.FT_ZGJJY3@H_AL"]
["3#反渗透阻垢剂流量高报警开关","C.M.FT_ZGJJY3@H_AL_ON"]
["3#反渗透阻垢剂流量高限设置","C.M.FT_ZGJJY3@H_AL_set"]
["3#反渗透阻垢剂流量低报警","C.M.FT_ZGJJY3@L_AL"]
["3#反渗透阻垢剂流量低报警开关","C.M.FT_ZGJJY3@L_AL_ON"]
["3#反渗透阻垢剂流量低限设置","C.M.FT_ZGJJY3@L_AL_set"]
["3#反渗透阻垢剂流量","C.M.FT_ZGJJY3@out"]
["4#反渗透阻垢剂流量报警","C.M.FT_ZGJJY4@fault"]
["4#反渗透阻垢剂流量高报警","C.M.FT_ZGJJY4@H_AL"]
["4#反渗透阻垢剂流量高报警开关","C.M.FT_ZGJJY4@H_AL_ON"]
["4#反渗透阻垢剂流量高限设置","C.M.FT_ZGJJY4@H_AL_set"]
["4#反渗透阻垢剂流量低报警","C.M.FT_ZGJJY4@L_AL"]
["4#反渗透阻垢剂流量低报警开关","C.M.FT_ZGJJY4@L_AL_ON"]
["4#反渗透阻垢剂流量低限设置","C.M.FT_ZGJJY4@L_AL_set"]
["4#反渗透阻垢剂流量","C.M.FT_ZGJJY4@out"]
["总进水流量报警","C.M.FT_ZJS@fault"]
["总进水流量高报警","C.M.FT_ZJS@H_AL"]
["总进水流量高报警开关","C.M.FT_ZJS@H_AL_ON"]
["总进水流量高限设置","C.M.FT_ZJS@H_AL_set"]
["总进水流量低报警","C.M.FT_ZJS@L_AL"]
["总进水流量低报警开关","C.M.FT_ZJS@L_AL_ON"]
["总进水流量低限设置","C.M.FT_ZJS@L_AL_set"]
["总进水流量","C.M.FT_ZJS@out"]
["1#自清洗过滤器反洗","C.M.GLQ1_FX"]
["1#自清洗过滤器过滤","C.M.GLQ1_GL"]
["1#自清洗过滤器故障","C.M.GLQ1_GZ"]
["2#自清洗过滤器反洗","C.M.GLQ2_FX"]
["2#自清洗过滤器过滤","C.M.GLQ2_GL"]
["2#自清洗过滤器故障","C.M.GLQ2_GZ"]
["3#自清洗过滤器反洗","C.M.GLQ3_FX"]
["3#自清洗过滤器过滤","C.M.GLQ3_GL"]
["3#自清洗过滤器故障","C.M.GLQ3_GZ"]
["还原剂药箱1搅拌器手自动","C.M.JBQ_HYJ@auto_select"]
["还原剂药箱1搅拌器故障","C.M.JBQ_HYJ@fault_total"]
["还原剂药箱1搅拌器远程","C.M.JBQ_HYJ@rem"]
["还原剂药箱1搅拌器复位","C.M.JBQ_HYJ@reset"]
["还原剂药箱1搅拌器运行","C.M.JBQ_HYJ@run"]
["还原剂药箱1搅拌器运行时间","C.M.JBQ_HYJ@run_time"]
["还原剂药箱1搅拌器启动操作","C.M.JBQ_HYJ@start"]
["还原剂药箱1搅拌器停止操作","C.M.JBQ_HYJ@stop"]
["还原剂药箱2搅拌器手自动","C.M.JBQ_HYJ2@auto_select"]
["还原剂药箱2搅拌器故障","C.M.JBQ_HYJ2@fault_total"]
["还原剂药箱2搅拌器远程","C.M.JBQ_HYJ2@rem"]
["还原剂药箱2搅拌器复位","C.M.JBQ_HYJ2@reset"]
["还原剂药箱2搅拌器运行","C.M.JBQ_HYJ2@run"]
["还原剂药箱2搅拌器运行时间","C.M.JBQ_HYJ2@run_time"]
["还原剂药箱2搅拌器启动操作","C.M.JBQ_HYJ2@start"]
["还原剂药箱2搅拌器停止操作","C.M.JBQ_HYJ2@stop"]
["氢氧化钠药箱搅拌器手自动","C.M.JBQ_NaOH@auto_select"]
["氢氧化钠药箱搅拌器故障","C.M.JBQ_NaOH@fault_total"]
["氢氧化钠药箱搅拌器远程","C.M.JBQ_NaOH@rem"]
["氢氧化钠药箱搅拌器复位","C.M.JBQ_NaOH@reset"]
["氢氧化钠药箱搅拌器运行","C.M.JBQ_NaOH@run"]
["氢氧化钠药箱搅拌器运行时间","C.M.JBQ_NaOH@run_time"]
["氢氧化钠药箱搅拌器启动操作","C.M.JBQ_NaOH@start"]
["氢氧化钠药箱搅拌器停止操作","C.M.JBQ_NaOH@stop"]
["溶药箱搅拌器手自动","C.M.JBQ_RYX@auto_select"]
["溶药箱搅拌器故障","C.M.JBQ_RYX@fault_total"]
["溶药箱搅拌器远程","C.M.JBQ_RYX@rem"]
["溶药箱搅拌器复位","C.M.JBQ_RYX@reset"]
["溶药箱搅拌器运行","C.M.JBQ_RYX@run"]
["溶药箱搅拌器运行时间","C.M.JBQ_RYX@run_time"]
["溶药箱搅拌器启动操作","C.M.JBQ_RYX@start"]
["溶药箱搅拌器停止操作","C.M.JBQ_RYX@stop"]
["杀菌剂药箱搅拌器手自动","C.M.JBQ_SJJ@auto_select"]
["杀菌剂药箱搅拌器故障","C.M.JBQ_SJJ@fault_total"]
["杀菌剂药箱搅拌器远程","C.M.JBQ_SJJ@rem"]
["杀菌剂药箱搅拌器复位","C.M.JBQ_SJJ@reset"]
["杀菌剂药箱搅拌器运行","C.M.JBQ_SJJ@run"]
["杀菌剂药箱搅拌器运行时间","C.M.JBQ_SJJ@run_time"]
["杀菌剂药箱搅拌器启动操作","C.M.JBQ_SJJ@start"]
["杀菌剂药箱搅拌器停止操作","C.M.JBQ_SJJ@stop"]
["絮凝剂药箱搅拌器手自动","C.M.JBQ_XNJ@auto_select"]
["絮凝剂药箱搅拌器故障","C.M.JBQ_XNJ@fault_total"]
["絮凝剂药箱搅拌器远程","C.M.JBQ_XNJ@rem"]
["絮凝剂药箱搅拌器复位","C.M.JBQ_XNJ@reset"]
["絮凝剂药箱搅拌器运行","C.M.JBQ_XNJ@run"]
["絮凝剂药箱搅拌器运行时间","C.M.JBQ_XNJ@run_time"]
["絮凝剂药箱搅拌器启动操作","C.M.JBQ_XNJ@start"]
["絮凝剂药箱搅拌器停止操作","C.M.JBQ_XNJ@stop"]
["阻垢剂药箱搅拌器手自动","C.M.JBQ_ZGJ@auto_select"]
["阻垢剂药箱搅拌器故障","C.M.JBQ_ZGJ@fault_total"]
["阻垢剂药箱搅拌器远程","C.M.JBQ_ZGJ@rem"]
["阻垢剂药箱搅拌器复位","C.M.JBQ_ZGJ@reset"]
["阻垢剂药箱搅拌器运行","C.M.JBQ_ZGJ@run"]
["阻垢剂药箱搅拌器运行时间","C.M.JBQ_ZGJ@run_time"]
["阻垢剂药箱搅拌器启动操作","C.M.JBQ_ZGJ@start"]
["阻垢剂药箱搅拌器停止操作","C.M.JBQ_ZGJ@stop"]
["CIP水箱1#电加热器搅拌器手自动","C.M.JRQ1@auto_select"]
["CIP水箱1#电加热器搅拌器故障","C.M.JRQ1@fault_total"]
["CIP水箱1#电加热器搅拌器远程","C.M.JRQ1@rem"]
["CIP水箱1#电加热器搅拌器复位","C.M.JRQ1@reset"]
["CIP水箱1#电加热器搅拌器运行","C.M.JRQ1@run"]
["CIP水箱1#电加热器搅拌器运行时间","C.M.JRQ1@run_time"]
["CIP水箱1#电加热器搅拌器启动操作","C.M.JRQ1@start"]
["CIP水箱1#电加热器搅拌器停止操作","C.M.JRQ1@stop"]
["CIP水箱2#电加热器搅拌器手自动","C.M.JRQ2@auto_select"]
["CIP水箱2#电加热器搅拌器故障","C.M.JRQ2@fault_total"]
["CIP水箱2#电加热器搅拌器远程","C.M.JRQ2@rem"]
["CIP水箱2#电加热器搅拌器复位","C.M.JRQ2@reset"]
["CIP水箱2#电加热器搅拌器运行","C.M.JRQ2@run"]
["CIP水箱2#电加热器搅拌器运行时间","C.M.JRQ2@run_time"]
["CIP水箱2#电加热器搅拌器启动操作","C.M.JRQ2@start"]
["CIP水箱2#电加热器搅拌器停止操作","C.M.JRQ2@stop"]
["1#NaClO加药泵(进水)手自动","C.M.JS_NaClO1@auto_select"]
["1#NaClO加药泵(进水)故障","C.M.JS_NaClO1@fault_total"]
["1#NaClO加药泵(进水)远程","C.M.JS_NaClO1@rem"]
["1#NaClO加药泵(进水)复位","C.M.JS_NaClO1@reset"]
["1#NaClO加药泵(进水)运行","C.M.JS_NaClO1@run"]
["1#NaClO加药泵(进水)运行时间","C.M.JS_NaClO1@run_time"]
["1#NaClO加药泵(进水)启动操作","C.M.JS_NaClO1@start"]
["1#NaClO加药泵(进水)停止操作","C.M.JS_NaClO1@stop"]
["1#NaClO加药泵(进水)设置频率","C.M.JS_NaClO1_AO_FB@spare"]
["1#NaClO加药泵(进水)频率报警","C.M.JS_NaClO1_fre@Fault"]
["1#NaClO加药泵(进水)频率高报警","C.M.JS_NaClO1_fre@H_AL"]
["1#NaClO加药泵(进水)频率高报警开关","C.M.JS_NaClO1_fre@H_AL_ON"]
["1#NaClO加药泵(进水)频率高限设置","C.M.JS_NaClO1_fre@H_AL_set"]
["1#NaClO加药泵(进水)频率低报警","C.M.JS_NaClO1_fre@L_AL"]
["1#NaClO加药泵(进水)频率低报警开关","C.M.JS_NaClO1_fre@L_AL_ON"]
["1#NaClO加药泵(进水)频率低限设置","C.M.JS_NaClO1_fre@L_AL_set"]
["1#NaClO加药泵(进水)运行频率","C.M.JS_NaClO1_fre@out"]
["2#NaClO加药泵(进水)手自动","C.M.JS_NaClO2@auto_select"]
["2#NaClO加药泵(进水)故障","C.M.JS_NaClO2@fault_total"]
["2#NaClO加药泵(进水)远程","C.M.JS_NaClO2@rem"]
["2#NaClO加药泵(进水)复位","C.M.JS_NaClO2@reset"]
["2#NaClO加药泵(进水)运行","C.M.JS_NaClO2@run"]
["2#NaClO加药泵(进水)运行时间","C.M.JS_NaClO2@run_time"]
["2#NaClO加药泵(进水)启动操作","C.M.JS_NaClO2@start"]
["2#NaClO加药泵(进水)停止操作","C.M.JS_NaClO2@stop"]
["2#NaClO加药泵(进水)设置频率","C.M.JS_NaClO2_AO_FB@spare"]
["2#NaClO加药泵(进水)频率报警","C.M.JS_NaClO2_fre@Fault"]
["2#NaClO加药泵(进水)频率高报警","C.M.JS_NaClO2_fre@H_AL"]
["2#NaClO加药泵(进水)频率高报警开关","C.M.JS_NaClO2_fre@H_AL_ON"]
["2#NaClO加药泵(进水)频率高限设置","C.M.JS_NaClO2_fre@H_AL_set"]
["2#NaClO加药泵(进水)频率低报警","C.M.JS_NaClO2_fre@L_AL"]
["2#NaClO加药泵(进水)频率低报警开关","C.M.JS_NaClO2_fre@L_AL_ON"]
["2#NaClO加药泵(进水)频率低限设置","C.M.JS_NaClO2_fre@L_AL_set"]
["2#NaClO加药泵(进水)运行频率","C.M.JS_NaClO2_fre@out"]
["未知1手自动（不确定）","C.M.JSKB1@auto_select"]
["未知1故障（不确定）","C.M.JSKB1@fault_total"]
["未知1远程（不确定）","C.M.JSKB1@rem"]
["未知1复位（不确定）","C.M.JSKB1@reset"]
["未知1运行（不确定）","C.M.JSKB1@run"]
["未知1运行时间（不确定）","C.M.JSKB1@run_time"]
["未知1启动操作（不确定）","C.M.JSKB1@start"]
["未知1停止操作（不确定）","C.M.JSKB1@stop"]
["未知2手自动（不确定）","C.M.JSKB2@auto_select"]
["未知2故障（不确定）","C.M.JSKB2@fault_total"]
["未知2远程（不确定）","C.M.JSKB2@rem"]
["未知2复位（不确定）","C.M.JSKB2@reset"]
["未知2运行（不确定）","C.M.JSKB2@run"]
["未知2运行时间（不确定）","C.M.JSKB2@run_time"]
["未知2启动操作（不确定）","C.M.JSKB2@start"]
["未知2停止操作（不确定）","C.M.JSKB2@stop"]
["未知3手自动（不确定）","C.M.JSKB3@auto_select"]
["未知3故障（不确定）","C.M.JSKB3@fault_total"]
["未知3远程（不确定）","C.M.JSKB3@rem"]
["未知3复位（不确定）","C.M.JSKB3@reset"]
["未知3运行（不确定）","C.M.JSKB3@run"]
["未知3运行时间（不确定）","C.M.JSKB3@run_time"]
["未知3启动操作（不确定）","C.M.JSKB3@start"]
["未知3停止操作（不确定）","C.M.JSKB3@stop"]
["未知4手自动（不确定）","C.M.JSKB4@auto_select"]
["未知4故障（不确定）","C.M.JSKB4@fault_total"]
["未知4远程（不确定）","C.M.JSKB4@rem"]
["未知4复位（不确定）","C.M.JSKB4@reset"]
["未知4运行（不确定）","C.M.JSKB4@run"]
["未知4运行时间（不确定）","C.M.JSKB4@run_time"]
["未知4启动操作（不确定）","C.M.JSKB4@start"]
["未知4停止操作（不确定）","C.M.JSKB4@stop"]
["1#盐酸加药泵手自动","C.M.JYB1_HCl1@auto_select"]
["1#盐酸加药泵故障","C.M.JYB1_HCl1@fault_total"]
["1#盐酸加药泵远程","C.M.JYB1_HCl1@rem"]
["1#盐酸加药泵复位","C.M.JYB1_HCl1@reset"]
["1#盐酸加药泵运行","C.M.JYB1_HCl1@run"]
["1#盐酸加药泵运行时间","C.M.JYB1_HCl1@run_time"]
["1#盐酸加药泵启动操作","C.M.JYB1_HCl1@start"]
["1#盐酸加药泵停止操作","C.M.JYB1_HCl1@stop"]
["2#盐酸加药泵手自动","C.M.JYB1_HCl2@auto_select"]
["2#盐酸加药泵故障","C.M.JYB1_HCl2@fault_total"]
["2#盐酸加药泵远程","C.M.JYB1_HCl2@rem"]
["2#盐酸加药泵复位","C.M.JYB1_HCl2@reset"]
["2#盐酸加药泵运行","C.M.JYB1_HCl2@run"]
["2#盐酸加药泵运行时间","C.M.JYB1_HCl2@run_time"]
["2#盐酸加药泵启动操作","C.M.JYB1_HCl2@start"]
["2#盐酸加药泵停止操作","C.M.JYB1_HCl2@stop"]
["1#还原剂加药泵(中和)手自动","C.M.JYB1_HYJ1@auto_select"]
["1#还原剂加药泵(中和)故障","C.M.JYB1_HYJ1@fault_total"]
["1#还原剂加药泵(中和)远程","C.M.JYB1_HYJ1@rem"]
["1#还原剂加药泵(中和)复位","C.M.JYB1_HYJ1@reset"]
["1#还原剂加药泵(中和)运行","C.M.JYB1_HYJ1@run"]
["1#还原剂加药泵(中和)运行时间","C.M.JYB1_HYJ1@run_time"]
["1#还原剂加药泵(中和)启动操作","C.M.JYB1_HYJ1@start"]
["1#还原剂加药泵(中和)停止操作","C.M.JYB1_HYJ1@stop"]
["2#还原剂加药泵(中和)手自动","C.M.JYB1_HYJ2@auto_select"]
["2#还原剂加药泵(中和)故障","C.M.JYB1_HYJ2@fault_total"]
["2#还原剂加药泵(中和)远程","C.M.JYB1_HYJ2@rem"]
["2#还原剂加药泵(中和)复位","C.M.JYB1_HYJ2@reset"]
["2#还原剂加药泵(中和)运行","C.M.JYB1_HYJ2@run"]
["2#还原剂加药泵(中和)运行时间","C.M.JYB1_HYJ2@run_time"]
["2#还原剂加药泵(中和)启动操作","C.M.JYB1_HYJ2@start"]
["2#还原剂加药泵(中和)停止操作","C.M.JYB1_HYJ2@stop"]
["1#NaClO加药泵手自动","C.M.JYB1_NaClO1@auto_select"]
["1#NaClO加药泵故障","C.M.JYB1_NaClO1@fault_total"]
["1#NaClO加药泵远程","C.M.JYB1_NaClO1@rem"]
["1#NaClO加药泵复位","C.M.JYB1_NaClO1@reset"]
["1#NaClO加药泵运行","C.M.JYB1_NaClO1@run"]
["1#NaClO加药泵运行时间","C.M.JYB1_NaClO1@run_time"]
["1#NaClO加药泵启动操作","C.M.JYB1_NaClO1@start"]
["1#NaClO加药泵停止操作","C.M.JYB1_NaClO1@stop"]
["2#NaClO加药泵手自动","C.M.JYB1_NaClO2@auto_select"]
["2#NaClO加药泵故障","C.M.JYB1_NaClO2@fault_total"]
["2#NaClO加药泵远程","C.M.JYB1_NaClO2@rem"]
["2#NaClO加药泵复位","C.M.JYB1_NaClO2@reset"]
["2#NaClO加药泵运行","C.M.JYB1_NaClO2@run"]
["2#NaClO加药泵运行时间","C.M.JYB1_NaClO2@run_time"]
["2#NaClO加药泵启动操作","C.M.JYB1_NaClO2@start"]
["2#NaClO加药泵停止操作","C.M.JYB1_NaClO2@stop"]
["1#NaOH加药泵(中和)手自动","C.M.JYB1_NaOH1@auto_select"]
["1#NaOH加药泵(中和)故障","C.M.JYB1_NaOH1@fault_total"]
["1#NaOH加药泵(中和)远程","C.M.JYB1_NaOH1@rem"]
["1#NaOH加药泵(中和)复位","C.M.JYB1_NaOH1@reset"]
["1#NaOH加药泵(中和)运行","C.M.JYB1_NaOH1@run"]
["1#NaOH加药泵(中和)运行时间","C.M.JYB1_NaOH1@run_time"]
["1#NaOH加药泵(中和)启动操作","C.M.JYB1_NaOH1@start"]
["1#NaOH加药泵(中和)停止操作","C.M.JYB1_NaOH1@stop"]
["2#NaOH加药泵(CEB)手自动","C.M.JYB1_NaOH2@auto_select"]
["2#NaOH加药泵(CEB)故障","C.M.JYB1_NaOH2@fault_total"]
["2#NaOH加药泵(CEB)远程","C.M.JYB1_NaOH2@rem"]
["2#NaOH加药泵(CEB)复位","C.M.JYB1_NaOH2@reset"]
["2#NaOH加药泵(CEB)运行","C.M.JYB1_NaOH2@run"]
["2#NaOH加药泵(CEB)运行时间","C.M.JYB1_NaOH2@run_time"]
["2#NaOH加药泵(CEB)启动操作","C.M.JYB1_NaOH2@start"]
["2#NaOH加药泵(CEB)停止操作","C.M.JYB1_NaOH2@stop"]
["1#还原剂加药泵(RO)手自动","C.M.JYB2_HYJ1@auto_select"]
["1#还原剂加药泵(RO)故障","C.M.JYB2_HYJ1@fault_total"]
["1#还原剂加药泵(RO)远程","C.M.JYB2_HYJ1@rem"]
["1#还原剂加药泵(RO)复位","C.M.JYB2_HYJ1@reset"]
["1#还原剂加药泵(RO)运行","C.M.JYB2_HYJ1@run"]
["1#还原剂加药泵(RO)运行时间","C.M.JYB2_HYJ1@run_time"]
["1#还原剂加药泵(RO)启动操作","C.M.JYB2_HYJ1@start"]
["1#还原剂加药泵(RO)停止操作","C.M.JYB2_HYJ1@stop"]
["1#还原剂加药泵(RO)设置频率","C.M.JYB2_HYJ1_AO_FB@spare"]
["1#还原剂加药泵(RO)频率报警","C.M.JYB2_HYJ1_fre@Fault"]
["1#还原剂加药泵(RO)频率高报警","C.M.JYB2_HYJ1_fre@H_AL"]
["1#还原剂加药泵(RO)频率高报警开关","C.M.JYB2_HYJ1_fre@H_AL_ON"]
["1#还原剂加药泵(RO)频率高限设置","C.M.JYB2_HYJ1_fre@H_AL_set"]
["1#还原剂加药泵(RO)频率低报警","C.M.JYB2_HYJ1_fre@L_AL"]
["1#还原剂加药泵(RO)频率低报警开关","C.M.JYB2_HYJ1_fre@L_AL_ON"]
["1#还原剂加药泵(RO)频率低限设置","C.M.JYB2_HYJ1_fre@L_AL_set"]
["1#还原剂加药泵(RO)运行频率","C.M.JYB2_HYJ1_fre@out"]
["2#还原剂加药泵(RO)手自动","C.M.JYB2_HYJ2@auto_select"]
["2#还原剂加药泵(RO)故障","C.M.JYB2_HYJ2@fault_total"]
["2#还原剂加药泵(RO)远程","C.M.JYB2_HYJ2@rem"]
["2#还原剂加药泵(RO)复位","C.M.JYB2_HYJ2@reset"]
["2#还原剂加药泵(RO)运行","C.M.JYB2_HYJ2@run"]
["2#还原剂加药泵(RO)运行时间","C.M.JYB2_HYJ2@run_time"]
["2#还原剂加药泵(RO)启动操作","C.M.JYB2_HYJ2@start"]
["2#还原剂加药泵(RO)停止操作","C.M.JYB2_HYJ2@stop"]
["2#还原剂加药泵(RO)设置频率","C.M.JYB2_HYJ2_AO_FB@spare"]
["2#还原剂加药泵(RO)频率报警","C.M.JYB2_HYJ2_fre@Fault"]
["2#还原剂加药泵(RO)频率高报警","C.M.JYB2_HYJ2_fre@H_AL"]
["2#还原剂加药泵(RO)频率高报警开关","C.M.JYB2_HYJ2_fre@H_AL_ON"]
["2#还原剂加药泵(RO)频率高限设置","C.M.JYB2_HYJ2_fre@H_AL_set"]
["2#还原剂加药泵(RO)频率低报警","C.M.JYB2_HYJ2_fre@L_AL"]
["2#还原剂加药泵(RO)频率低报警开关","C.M.JYB2_HYJ2_fre@L_AL_ON"]
["2#还原剂加药泵(RO)频率低限设置","C.M.JYB2_HYJ2_fre@L_AL_set"]
["2#还原剂加药泵(RO)运行频率","C.M.JYB2_HYJ2_fre@out"]
["3#还原剂加药泵(RO)手自动","C.M.JYB2_HYJ3@auto_select"]
["3#还原剂加药泵(RO)故障","C.M.JYB2_HYJ3@fault_total"]
["3#还原剂加药泵(RO)远程","C.M.JYB2_HYJ3@rem"]
["3#还原剂加药泵(RO)复位","C.M.JYB2_HYJ3@reset"]
["3#还原剂加药泵(RO)运行","C.M.JYB2_HYJ3@run"]
["3#还原剂加药泵(RO)运行时间","C.M.JYB2_HYJ3@run_time"]
["3#还原剂加药泵(RO)启动操作","C.M.JYB2_HYJ3@start"]
["3#还原剂加药泵(RO)停止操作","C.M.JYB2_HYJ3@stop"]
["3#还原剂加药泵(RO)设置频率","C.M.JYB2_HYJ3_AO_FB@spare"]
["3#还原剂加药泵(RO)频率报警","C.M.JYB2_HYJ3_fre@Fault"]
["3#还原剂加药泵(RO)频率高报警","C.M.JYB2_HYJ3_fre@H_AL"]
["3#还原剂加药泵(RO)频率高报警开关","C.M.JYB2_HYJ3_fre@H_AL_ON"]
["3#还原剂加药泵(RO)频率高限设置","C.M.JYB2_HYJ3_fre@H_AL_set"]
["3#还原剂加药泵(RO)频率低报警","C.M.JYB2_HYJ3_fre@L_AL"]
["3#还原剂加药泵(RO)频率低报警开关","C.M.JYB2_HYJ3_fre@L_AL_ON"]
["3#还原剂加药泵(RO)频率低限设置","C.M.JYB2_HYJ3_fre@L_AL_set"]
["3#还原剂加药泵(RO)运行频率","C.M.JYB2_HYJ3_fre@out"]
["1#NaOH加药泵(出水)手自动","C.M.JYB2_NaOH1@auto_select"]
["1#NaOH加药泵(出水)故障","C.M.JYB2_NaOH1@fault_total"]
["1#NaOH加药泵(出水)远程","C.M.JYB2_NaOH1@rem"]
["1#NaOH加药泵(出水)复位","C.M.JYB2_NaOH1@reset"]
["1#NaOH加药泵(出水)运行","C.M.JYB2_NaOH1@run"]
["1#NaOH加药泵(出水)运行时间","C.M.JYB2_NaOH1@run_time"]
["1#NaOH加药泵(出水)启动操作","C.M.JYB2_NaOH1@start"]
["1#NaOH加药泵(出水)停止操作","C.M.JYB2_NaOH1@stop"]
["1#NaOH加药泵(出水)设置频率","C.M.JYB2_NaOH1_AO_FB@spare"]
["1#NaOH加药泵(出水)频率报警","C.M.JYB2_NaOH1_fre@Fault"]
["1#NaOH加药泵(出水)频率高报警","C.M.JYB2_NaOH1_fre@H_AL"]
["1#NaOH加药泵(出水)频率高报警开关","C.M.JYB2_NaOH1_fre@H_AL_ON"]
["1#NaOH加药泵(出水)频率高限设置","C.M.JYB2_NaOH1_fre@H_AL_set"]
["1#NaOH加药泵(出水)频率低报警","C.M.JYB2_NaOH1_fre@L_AL"]
["1#NaOH加药泵(出水)频率低报警开关","C.M.JYB2_NaOH1_fre@L_AL_ON"]
["1#NaOH加药泵(出水)频率低限设置","C.M.JYB2_NaOH1_fre@L_AL_set"]
["1#NaOH加药泵(出水)运行频率","C.M.JYB2_NaOH1_fre@out"]
["2#NaOH加药泵(出水)手自动","C.M.JYB2_NaOH2@auto_select"]
["2#NaOH加药泵(出水)故障","C.M.JYB2_NaOH2@fault_total"]
["2#NaOH加药泵(出水)远程","C.M.JYB2_NaOH2@rem"]
["2#NaOH加药泵(出水)复位","C.M.JYB2_NaOH2@reset"]
["2#NaOH加药泵(出水)运行","C.M.JYB2_NaOH2@run"]
["2#NaOH加药泵(出水)运行时间","C.M.JYB2_NaOH2@run_time"]
["2#NaOH加药泵(出水)启动操作","C.M.JYB2_NaOH2@start"]
["2#NaOH加药泵(出水)停止操作","C.M.JYB2_NaOH2@stop"]
["2#NaOH加药泵(出水)设置频率","C.M.JYB2_NaOH2_AO_FB@spare"]
["2#NaOH加药泵(出水)频率报警","C.M.JYB2_NaOH2_fre@Fault"]
["2#NaOH加药泵(出水)频率高报警","C.M.JYB2_NaOH2_fre@H_AL"]
["2#NaOH加药泵(出水)频率高报警开关","C.M.JYB2_NaOH2_fre@H_AL_ON"]
["2#NaOH加药泵(出水)频率高限设置","C.M.JYB2_NaOH2_fre@H_AL_set"]
["2#NaOH加药泵(出水)频率低报警","C.M.JYB2_NaOH2_fre@L_AL"]
["2#NaOH加药泵(出水)频率低报警开关","C.M.JYB2_NaOH2_fre@L_AL_ON"]
["2#NaOH加药泵(出水)频率低限设置","C.M.JYB2_NaOH2_fre@L_AL_set"]
["2#NaOH加药泵(出水)运行频率","C.M.JYB2_NaOH2_fre@out"]
["1#絮凝剂加药泵(UF)手自动","C.M.JYB2_XNJ1@auto_select"]
["1#絮凝剂加药泵(UF)故障","C.M.JYB2_XNJ1@fault_total"]
["1#絮凝剂加药泵(UF)远程","C.M.JYB2_XNJ1@rem"]
["1#絮凝剂加药泵(UF)复位","C.M.JYB2_XNJ1@reset"]
["1#絮凝剂加药泵(UF)运行","C.M.JYB2_XNJ1@run"]
["1#絮凝剂加药泵(UF)运行时间","C.M.JYB2_XNJ1@run_time"]
["1#絮凝剂加药泵(UF)启动操作","C.M.JYB2_XNJ1@start"]
["1#絮凝剂加药泵(UF)停止操作","C.M.JYB2_XNJ1@stop"]
["1#絮凝剂加药泵(UF)设置频率","C.M.JYB2_XNJ1_AO_FB@spare"]
["1#絮凝剂加药泵(UF)频率报警","C.M.JYB2_XNJ1_fre@Fault"]
["1#絮凝剂加药泵(UF)频率高报警","C.M.JYB2_XNJ1_fre@H_AL"]
["1#絮凝剂加药泵(UF)频率高报警开关","C.M.JYB2_XNJ1_fre@H_AL_ON"]
["1#絮凝剂加药泵(UF)频率高限设置","C.M.JYB2_XNJ1_fre@H_AL_set"]
["1#絮凝剂加药泵(UF)频率低报警","C.M.JYB2_XNJ1_fre@L_AL"]
["1#絮凝剂加药泵(UF)频率低报警开关","C.M.JYB2_XNJ1_fre@L_AL_ON"]
["1#絮凝剂加药泵(UF)频率低限设置","C.M.JYB2_XNJ1_fre@L_AL_set"]
["1#絮凝剂加药泵(UF)运行频率","C.M.JYB2_XNJ1_fre@out"]
["2#絮凝剂加药泵(UF)手自动","C.M.JYB2_XNJ2@auto_select"]
["2#絮凝剂加药泵(UF)故障","C.M.JYB2_XNJ2@fault_total"]
["2#絮凝剂加药泵(UF)远程","C.M.JYB2_XNJ2@rem"]
["2#絮凝剂加药泵(UF)复位","C.M.JYB2_XNJ2@reset"]
["2#絮凝剂加药泵(UF)运行","C.M.JYB2_XNJ2@run"]
["2#絮凝剂加药泵(UF)运行时间","C.M.JYB2_XNJ2@run_time"]
["2#絮凝剂加药泵(UF)启动操作","C.M.JYB2_XNJ2@start"]
["2#絮凝剂加药泵(UF)停止操作","C.M.JYB2_XNJ2@stop"]
["2#絮凝剂加药泵(UF)设置频率","C.M.JYB2_XNJ2_AO_FB@spare"]
["2#絮凝剂加药泵(UF)频率报警","C.M.JYB2_XNJ2_fre@Fault"]
["2#絮凝剂加药泵(UF)频率高报警","C.M.JYB2_XNJ2_fre@H_AL"]
["2#絮凝剂加药泵(UF)频率高报警开关","C.M.JYB2_XNJ2_fre@H_AL_ON"]
["2#絮凝剂加药泵(UF)频率高限设置","C.M.JYB2_XNJ2_fre@H_AL_set"]
["2#絮凝剂加药泵(UF)频率低报警","C.M.JYB2_XNJ2_fre@L_AL"]
["2#絮凝剂加药泵(UF)频率低报警开关","C.M.JYB2_XNJ2_fre@L_AL_ON"]
["2#絮凝剂加药泵(UF)频率低限设置","C.M.JYB2_XNJ2_fre@L_AL_set"]
["2#絮凝剂加药泵(UF)运行频率","C.M.JYB2_XNJ2_fre@out"]
["1#阻垢剂加药泵(RO)手自动","C.M.JYB2_ZGJ1@auto_select"]
["1#阻垢剂加药泵(RO)故障","C.M.JYB2_ZGJ1@fault_total"]
["1#阻垢剂加药泵(RO)远程","C.M.JYB2_ZGJ1@rem"]
["1#阻垢剂加药泵(RO)复位","C.M.JYB2_ZGJ1@reset"]
["1#阻垢剂加药泵(RO)运行","C.M.JYB2_ZGJ1@run"]
["1#阻垢剂加药泵(RO)运行时间","C.M.JYB2_ZGJ1@run_time"]
["1#阻垢剂加药泵(RO)启动操作","C.M.JYB2_ZGJ1@start"]
["1#阻垢剂加药泵(RO)停止操作","C.M.JYB2_ZGJ1@stop"]
["1#阻垢剂加药泵(RO)设置频率","C.M.JYB2_ZGJ1_AO_FB@spare"]
["1#阻垢剂加药泵(RO)频率报警","C.M.JYB2_ZGJ1_fre@Fault"]
["1#阻垢剂加药泵(RO)频率高报警","C.M.JYB2_ZGJ1_fre@H_AL"]
["1#阻垢剂加药泵(RO)频率高报警开关","C.M.JYB2_ZGJ1_fre@H_AL_ON"]
["1#阻垢剂加药泵(RO)频率高限设置","C.M.JYB2_ZGJ1_fre@H_AL_set"]
["1#阻垢剂加药泵(RO)频率低报警","C.M.JYB2_ZGJ1_fre@L_AL"]
["1#阻垢剂加药泵(RO)频率低报警开关","C.M.JYB2_ZGJ1_fre@L_AL_ON"]
["1#阻垢剂加药泵(RO)频率低限设置","C.M.JYB2_ZGJ1_fre@L_AL_set"]
["1#阻垢剂加药泵(RO)运行频率","C.M.JYB2_ZGJ1_fre@out"]
["2#阻垢剂加药泵(RO)手自动","C.M.JYB2_ZGJ2@auto_select"]
["2#阻垢剂加药泵(RO)故障","C.M.JYB2_ZGJ2@fault_total"]
["2#阻垢剂加药泵(RO)远程","C.M.JYB2_ZGJ2@rem"]
["2#阻垢剂加药泵(RO)复位","C.M.JYB2_ZGJ2@reset"]
["2#阻垢剂加药泵(RO)运行","C.M.JYB2_ZGJ2@run"]
["2#阻垢剂加药泵(RO)运行时间","C.M.JYB2_ZGJ2@run_time"]
["2#阻垢剂加药泵(RO)启动操作","C.M.JYB2_ZGJ2@start"]
["2#阻垢剂加药泵(RO)停止操作","C.M.JYB2_ZGJ2@stop"]
["2#阻垢剂加药泵(RO)设置频率","C.M.JYB2_ZGJ2_AO_FB@spare"]
["2#阻垢剂加药泵(RO)频率报警","C.M.JYB2_ZGJ2_fre@Fault"]
["2#阻垢剂加药泵(RO)频率高报警","C.M.JYB2_ZGJ2_fre@H_AL"]
["2#阻垢剂加药泵(RO)频率高报警开关","C.M.JYB2_ZGJ2_fre@H_AL_ON"]
["2#阻垢剂加药泵(RO)频率高限设置","C.M.JYB2_ZGJ2_fre@H_AL_set"]
["2#阻垢剂加药泵(RO)频率低报警","C.M.JYB2_ZGJ2_fre@L_AL"]
["2#阻垢剂加药泵(RO)频率低报警开关","C.M.JYB2_ZGJ2_fre@L_AL_ON"]
["2#阻垢剂加药泵(RO)频率低限设置","C.M.JYB2_ZGJ2_fre@L_AL_set"]
["2#阻垢剂加药泵(RO)运行频率","C.M.JYB2_ZGJ2_fre@out"]
["3#阻垢剂加药泵(RO)手自动","C.M.JYB2_ZGJ3@auto_select"]
["3#阻垢剂加药泵(RO)故障","C.M.JYB2_ZGJ3@fault_total"]
["3#阻垢剂加药泵(RO)远程","C.M.JYB2_ZGJ3@rem"]
["3#阻垢剂加药泵(RO)复位","C.M.JYB2_ZGJ3@reset"]
["3#阻垢剂加药泵(RO)运行","C.M.JYB2_ZGJ3@run"]
["3#阻垢剂加药泵(RO)运行时间","C.M.JYB2_ZGJ3@run_time"]
["3#阻垢剂加药泵(RO)启动操作","C.M.JYB2_ZGJ3@start"]
["3#阻垢剂加药泵(RO)停止操作","C.M.JYB2_ZGJ3@stop"]
["3#阻垢剂加药泵(RO)设置频率","C.M.JYB2_ZGJ3_AO_FB@spare"]
["3#阻垢剂加药泵(RO)频率报警","C.M.JYB2_ZGJ3_fre@Fault"]
["3#阻垢剂加药泵(RO)频率高报警","C.M.JYB2_ZGJ3_fre@H_AL"]
["3#阻垢剂加药泵(RO)频率高报警开关","C.M.JYB2_ZGJ3_fre@H_AL_ON"]
["3#阻垢剂加药泵(RO)频率高限设置","C.M.JYB2_ZGJ3_fre@H_AL_set"]
["3#阻垢剂加药泵(RO)频率低报警","C.M.JYB2_ZGJ3_fre@L_AL"]
["3#阻垢剂加药泵(RO)频率低报警开关","C.M.JYB2_ZGJ3_fre@L_AL_ON"]
["3#阻垢剂加药泵(RO)频率低限设置","C.M.JYB2_ZGJ3_fre@L_AL_set"]
["3#阻垢剂加药泵(RO)运行频率","C.M.JYB2_ZGJ3_fre@out"]
["4#阻垢剂加药泵(RO)手自动","C.M.JYB2_ZGJ4@auto_select"]
["4#阻垢剂加药泵(RO)故障","C.M.JYB2_ZGJ4@fault_total"]
["4#阻垢剂加药泵(RO)远程","C.M.JYB2_ZGJ4@rem"]
["4#阻垢剂加药泵(RO)复位","C.M.JYB2_ZGJ4@reset"]
["4#阻垢剂加药泵(RO)运行","C.M.JYB2_ZGJ4@run"]
["4#阻垢剂加药泵(RO)运行时间","C.M.JYB2_ZGJ4@run_time"]
["4#阻垢剂加药泵(RO)启动操作","C.M.JYB2_ZGJ4@start"]
["4#阻垢剂加药泵(RO)停止操作","C.M.JYB2_ZGJ4@stop"]
["4#阻垢剂加药泵(RO)设置频率","C.M.JYB2_ZGJ4_AO_FB@spare"]
["4#阻垢剂加药泵(RO)频率报警","C.M.JYB2_ZGJ4_fre@Fault"]
["4#阻垢剂加药泵(RO)频率高报警","C.M.JYB2_ZGJ4_fre@H_AL"]
["4#阻垢剂加药泵(RO)频率高报警开关","C.M.JYB2_ZGJ4_fre@H_AL_ON"]
["4#阻垢剂加药泵(RO)频率高限设置","C.M.JYB2_ZGJ4_fre@H_AL_set"]
["4#阻垢剂加药泵(RO)频率低报警","C.M.JYB2_ZGJ4_fre@L_AL"]
["4#阻垢剂加药泵(RO)频率低报警开关","C.M.JYB2_ZGJ4_fre@L_AL_ON"]
["4#阻垢剂加药泵(RO)频率低限设置","C.M.JYB2_ZGJ4_fre@L_AL_set"]
["4#阻垢剂加药泵(RO)运行频率","C.M.JYB2_ZGJ4_fre@out"]
["5#阻垢剂加药泵(RO)手自动","C.M.JYB2_ZGJ5@auto_select"]
["5#阻垢剂加药泵(RO)故障","C.M.JYB2_ZGJ5@fault_total"]
["5#阻垢剂加药泵(RO)远程","C.M.JYB2_ZGJ5@rem"]
["5#阻垢剂加药泵(RO)复位","C.M.JYB2_ZGJ5@reset"]
["5#阻垢剂加药泵(RO)运行","C.M.JYB2_ZGJ5@run"]
["5#阻垢剂加药泵(RO)运行时间","C.M.JYB2_ZGJ5@run_time"]
["5#阻垢剂加药泵(RO)启动操作","C.M.JYB2_ZGJ5@start"]
["5#阻垢剂加药泵(RO)停止操作","C.M.JYB2_ZGJ5@stop"]
["5#阻垢剂加药泵(RO)设置频率","C.M.JYB2_ZGJ5_AO_FB@spare"]
["5#阻垢剂加药泵(RO)频率报警","C.M.JYB2_ZGJ5_fre@Fault"]
["5#阻垢剂加药泵(RO)频率高报警","C.M.JYB2_ZGJ5_fre@H_AL"]
["5#阻垢剂加药泵(RO)频率高报警开关","C.M.JYB2_ZGJ5_fre@H_AL_ON"]
["5#阻垢剂加药泵(RO)频率高限设置","C.M.JYB2_ZGJ5_fre@H_AL_set"]
["5#阻垢剂加药泵(RO)频率低报警","C.M.JYB2_ZGJ5_fre@L_AL"]
["5#阻垢剂加药泵(RO)频率低报警开关","C.M.JYB2_ZGJ5_fre@L_AL_ON"]
["5#阻垢剂加药泵(RO)频率低限设置","C.M.JYB2_ZGJ5_fre@L_AL_set"]
["5#阻垢剂加药泵(RO)运行频率","C.M.JYB2_ZGJ5_fre@out"]
["CIP水箱低液位开关","C.M.LS_CIP_L_I"]
["超滤产水母管开关","C.M.LS_CSMG_L_I"]
["盐酸药箱液位开关","C.M.LS_HCl_L_I"]
["还原剂药箱1液位开关","C.M.LS_HYJ1_L_I"]
["还原剂药箱2液位开关","C.M.LS_HYJ2_L_I"]
["次氯酸钠药箱液位开关","C.M.LS_NaClO_L_I"]
["氢氧化钠药箱液位开关","C.M.LS_NaOH_L_I"]
["絮凝剂药箱液位开关","C.M.LS_PAC_L_I"]
["清水池液位开关","C.M.LS_QSC_L_I"]
["杀菌剂药箱液位开关","C.M.LS_SJJ_L_I"]
["超滤反洗水池低液位开关","C.M.LS_UFFXSC_L_I"]
["超滤原水池低液位开关","C.M.LS_UFJSC_L_I"]
["阻垢剂药箱液位开关","C.M.LS_ZGJ_L_I"]
["CIP水箱液位报警","C.M.LT_CIP@fault"]
["CIP水箱液位高报警","C.M.LT_CIP@H_AL"]
["CIP水箱液位高报警开关","C.M.LT_CIP@H_AL_ON"]
["CIP水箱液位高限设置","C.M.LT_CIP@H_AL_set"]
["CIP水箱液位低报警","C.M.LT_CIP@L_AL"]
["CIP水箱液位低报警开关","C.M.LT_CIP@L_AL_ON"]
["CIP水箱液位低限设置","C.M.LT_CIP@L_AL_set"]
["CIP水箱液位","C.M.LT_CIP@out"]
["超滤反洗水池液位报警","C.M.LT_FXSC@fault"]
["超滤反洗水池液位高报警","C.M.LT_FXSC@H_AL"]
["超滤反洗水池液位高报警开关","C.M.LT_FXSC@H_AL_ON"]
["超滤反洗水池液位高限设置","C.M.LT_FXSC@H_AL_set"]
["超滤反洗水池液位低报警","C.M.LT_FXSC@L_AL"]
["超滤反洗水池液位低报警开关","C.M.LT_FXSC@L_AL_ON"]
["超滤反洗水池液位低限设置","C.M.LT_FXSC@L_AL_set"]
["超滤反洗水池液位","C.M.LT_FXSC@out"]
["超滤反洗水池液位设定值","C.M.LT_FXSC_set"]
["盐酸药箱液位报警","C.M.LT_HCl@fault"]
["盐酸药箱液位高报警","C.M.LT_HCl@H_AL"]
["盐酸药箱液位高报警开关","C.M.LT_HCl@H_AL_ON"]
["盐酸药箱液位高限设置","C.M.LT_HCl@H_AL_set"]
["盐酸药箱液位低报警","C.M.LT_HCl@L_AL"]
["盐酸药箱液位低报警开关","C.M.LT_HCl@L_AL_ON"]
["盐酸药箱液位低限设置","C.M.LT_HCl@L_AL_set"]
["盐酸药箱液位","C.M.LT_HCl@out"]
["还原剂药箱2液位报警","C.M.LT_HYJ1@fault"]
["还原剂药箱2液位高报警","C.M.LT_HYJ1@H_AL"]
["还原剂药箱2液位高报警开关","C.M.LT_HYJ1@H_AL_ON"]
["还原剂药箱2液位高限设置","C.M.LT_HYJ1@H_AL_set"]
["还原剂药箱2液位低报警","C.M.LT_HYJ1@L_AL"]
["还原剂药箱2液位低报警开关","C.M.LT_HYJ1@L_AL_ON"]
["还原剂药箱2液位低限设置","C.M.LT_HYJ1@L_AL_set"]
["还原剂药箱2液位","C.M.LT_HYJ1@out"]
["还原剂药箱1液位报警","C.M.LT_HYJ2@fault"]
["还原剂药箱1液位高报警","C.M.LT_HYJ2@H_AL"]
["还原剂药箱1液位高报警开关","C.M.LT_HYJ2@H_AL_ON"]
["还原剂药箱1液位高限设置","C.M.LT_HYJ2@H_AL_set"]
["还原剂药箱1液位低报警","C.M.LT_HYJ2@L_AL"]
["还原剂药箱1液位低报警开关","C.M.LT_HYJ2@L_AL_ON"]
["还原剂药箱1液位低限设置","C.M.LT_HYJ2@L_AL_set"]
["还原剂药箱1液位","C.M.LT_HYJ2@out"]
["超滤原水池液位报警","C.M.LT_JSC@fault"]
["超滤原水池液位高报警","C.M.LT_JSC@H_AL"]
["超滤原水池液位高报警开关","C.M.LT_JSC@H_AL_ON"]
["超滤原水池液位高限设置","C.M.LT_JSC@H_AL_set"]
["超滤原水池液位低报警","C.M.LT_JSC@L_AL"]
["超滤原水池液位低报警开关","C.M.LT_JSC@L_AL_ON"]
["超滤原水池液位低限设置","C.M.LT_JSC@L_AL_set"]
["超滤原水池液位","C.M.LT_JSC@out"]
["次氯酸钠药箱液位报警","C.M.LT_NaClO@fault"]
["次氯酸钠药箱液位高报警","C.M.LT_NaClO@H_AL"]
["次氯酸钠药箱液位高报警开关","C.M.LT_NaClO@H_AL_ON"]
["次氯酸钠药箱液位高限设置","C.M.LT_NaClO@H_AL_set"]
["次氯酸钠药箱液位低报警","C.M.LT_NaClO@L_AL"]
["次氯酸钠药箱液位低报警开关","C.M.LT_NaClO@L_AL_ON"]
["次氯酸钠药箱液位低限设置","C.M.LT_NaClO@L_AL_set"]
["次氯酸钠药箱液位","C.M.LT_NaClO@out"]
["氢氧化钠药箱液位报警","C.M.LT_NaOH@fault"]
["氢氧化钠药箱液位高报警","C.M.LT_NaOH@H_AL"]
["氢氧化钠药箱液位高报警开关","C.M.LT_NaOH@H_AL_ON"]
["氢氧化钠药箱液位高限设置","C.M.LT_NaOH@H_AL_set"]
["氢氧化钠药箱液位低报警","C.M.LT_NaOH@L_AL"]
["氢氧化钠药箱液位低报警开关","C.M.LT_NaOH@L_AL_ON"]
["氢氧化钠药箱液位低限设置","C.M.LT_NaOH@L_AL_set"]
["氢氧化钠药箱液位","C.M.LT_NaOH@out"]
["絮凝剂药箱液位报警","C.M.LT_PAC@fault"]
["絮凝剂药箱液位高报警","C.M.LT_PAC@H_AL"]
["絮凝剂药箱液位高报警开关","C.M.LT_PAC@H_AL_ON"]
["絮凝剂药箱液位高限设置","C.M.LT_PAC@H_AL_set"]
["絮凝剂药箱液位低报警","C.M.LT_PAC@L_AL"]
["絮凝剂药箱液位低报警开关","C.M.LT_PAC@L_AL_ON"]
["絮凝剂药箱液位低限设置","C.M.LT_PAC@L_AL_set"]
["絮凝剂药箱液位","C.M.LT_PAC@out"]
["清水池液位报警","C.M.LT_QSC@fault"]
["清水池液位高报警","C.M.LT_QSC@H_AL"]
["清水池液位高报警开关","C.M.LT_QSC@H_AL_ON"]
["清水池液位高限设置","C.M.LT_QSC@H_AL_set"]
["清水池液位低报警","C.M.LT_QSC@L_AL"]
["清水池液位低报警开关","C.M.LT_QSC@L_AL_ON"]
["清水池液位低限设置","C.M.LT_QSC@L_AL_set"]
["清水池液位","C.M.LT_QSC@out"]
["杀菌剂药箱液位报警","C.M.LT_SJJ@fault"]
["杀菌剂药箱液位高报警","C.M.LT_SJJ@H_AL"]
["杀菌剂药箱液位高报警开关","C.M.LT_SJJ@H_AL_ON"]
["杀菌剂药箱液位高限设置","C.M.LT_SJJ@H_AL_set"]
["杀菌剂药箱液位低报警","C.M.LT_SJJ@L_AL"]
["杀菌剂药箱液位低报警开关","C.M.LT_SJJ@L_AL_ON"]
["杀菌剂药箱液位低限设置","C.M.LT_SJJ@L_AL_set"]
["杀菌剂药箱液位","C.M.LT_SJJ@out"]
["阻垢剂药箱液位报警","C.M.LT_ZGJ@fault"]
["阻垢剂药箱液位高报警","C.M.LT_ZGJ@H_AL"]
["阻垢剂药箱液位高报警开关","C.M.LT_ZGJ@H_AL_ON"]
["阻垢剂药箱液位高限设置","C.M.LT_ZGJ@H_AL_set"]
["阻垢剂药箱液位低报警","C.M.LT_ZGJ@L_AL"]
["阻垢剂药箱液位低报警开关","C.M.LT_ZGJ@L_AL_ON"]
["阻垢剂药箱液位低限设置","C.M.LT_ZGJ@L_AL_set"]
["阻垢剂药箱液位","C.M.LT_ZGJ@out"]
["中和池液位报警","C.M.LT_ZHC@fault"]
["中和池液位高报警","C.M.LT_ZHC@H_AL"]
["中和池液位高报警开关","C.M.LT_ZHC@H_AL_ON"]
["中和池液位高限设置","C.M.LT_ZHC@H_AL_set"]
["中和池液位低报警","C.M.LT_ZHC@L_AL"]
["中和池液位低报警开关","C.M.LT_ZHC@L_AL_ON"]
["中和池液位低限设置","C.M.LT_ZHC@L_AL_set"]
["中和池液位","C.M.LT_ZHC@out"]
["中和池开泵液位设定值","C.M.LT_ZHC_start_sp"]
["中和池关泵液位设定值","C.M.LT_ZHC_stop_sp"]
["CIP-PH报警","C.M.PH_CIP@fault"]
["CIP-PH高报警","C.M.PH_CIP@H_AL"]
["CIP-PH高报警开关","C.M.PH_CIP@H_AL_ON"]
["CIP-PH高限设置","C.M.PH_CIP@H_AL_set"]
["CIP-PH低报警","C.M.PH_CIP@L_AL"]
["CIP-PH低报警开关","C.M.PH_CIP@L_AL_ON"]
["CIP-PH低限设置","C.M.PH_CIP@L_AL_set"]
["CIP-PH","C.M.PH_CIP@out"]
["外供水-PH报警","C.M.PH_WGS@fault"]
["外供水-PH高报警","C.M.PH_WGS@H_AL"]
["外供水-PH高报警开关","C.M.PH_WGS@H_AL_ON"]
["外供水-PH高限设置","C.M.PH_WGS@H_AL_set"]
["外供水-PH低报警","C.M.PH_WGS@L_AL"]
["外供水-PH低报警开关","C.M.PH_WGS@L_AL_ON"]
["外供水-PH低限设置","C.M.PH_WGS@L_AL_set"]
["外供水-PH","C.M.PH_WGS@out"]
["压缩空气压力报警","C.M.PT_KYJ@fault"]
["压缩空气压力高报警","C.M.PT_KYJ@H_AL"]
["压缩空气压力高报警开关","C.M.PT_KYJ@H_AL_ON"]
["压缩空气压力高限设置","C.M.PT_KYJ@H_AL_set"]
["压缩空气压力低报警","C.M.PT_KYJ@L_AL"]
["压缩空气压力低报警开关","C.M.PT_KYJ@L_AL_ON"]
["压缩空气压力低限设置","C.M.PT_KYJ@L_AL_set"]
["压缩空气压力","C.M.PT_KYJ@out"]
["反渗透总产水电导报警","C.M.RO_Cond_ZCS@fault"]
["反渗透总产水电导高报警","C.M.RO_Cond_ZCS@H_AL"]
["反渗透总产水电导高报警开关","C.M.RO_Cond_ZCS@H_AL_ON"]
["反渗透总产水电导高限设置","C.M.RO_Cond_ZCS@H_AL_set"]
["反渗透总产水电导低报警","C.M.RO_Cond_ZCS@L_AL"]
["反渗透总产水电导低报警开关","C.M.RO_Cond_ZCS@L_AL_ON"]
["反渗透总产水电导低限设置","C.M.RO_Cond_ZCS@L_AL_set"]
["反渗透总产水电导","C.M.RO_Cond_ZCS@out"]
["反渗透总进水电导报警","C.M.RO_Cond_ZJS@fault"]
["反渗透总进水电导高报警","C.M.RO_Cond_ZJS@H_AL"]
["反渗透总进水电导高报警开关","C.M.RO_Cond_ZJS@H_AL_ON"]
["反渗透总进水电导高限设置","C.M.RO_Cond_ZJS@H_AL_set"]
["反渗透总进水电导低报警","C.M.RO_Cond_ZJS@L_AL"]
["反渗透总进水电导低报警开关","C.M.RO_Cond_ZJS@L_AL_ON"]
["反渗透总进水电导低限设置","C.M.RO_Cond_ZJS@L_AL_set"]
["反渗透总进水电导","C.M.RO_Cond_ZJS@out"]
["外供水NaClO加药阀手自动","C.M.RO_CS_NaClO@auto_select"]
["外供水NaClO加药阀关操作","C.M.RO_CS_NaClO@close"]
["外供水NaClO加药阀关到位","C.M.RO_CS_NaClO@close_feedback"]
["外供水NaClO加药阀故障","C.M.RO_CS_NaClO@fault_total"]
["外供水NaClO加药阀开操作","C.M.RO_CS_NaClO@open"]
["外供水NaClO加药阀开到位","C.M.RO_CS_NaClO@open_feedback"]
["外供水NaClO加药阀远程","C.M.RO_CS_NaClO@rem"]
["外供水NaClO加药阀复位","C.M.RO_CS_NaClO@reset"]
["外供水NaOH加药阀手自动","C.M.RO_CS_NaOH@auto_select"]
["外供水NaOH加药阀关操作","C.M.RO_CS_NaOH@close"]
["外供水NaOH加药阀关到位","C.M.RO_CS_NaOH@close_feedback"]
["外供水NaOH加药阀故障","C.M.RO_CS_NaOH@fault_total"]
["外供水NaOH加药阀开操作","C.M.RO_CS_NaOH@open"]
["外供水NaOH加药阀开到位","C.M.RO_CS_NaOH@open_feedback"]
["外供水NaOH加药阀远程","C.M.RO_CS_NaOH@rem"]
["外供水NaOH加药阀复位","C.M.RO_CS_NaOH@reset"]
["1#大水量冲洗泵手自动","C.M.RO_CXB1@auto_select"]
["1#大水量冲洗泵故障","C.M.RO_CXB1@fault_total"]
["1#大水量冲洗泵远程","C.M.RO_CXB1@rem"]
["1#大水量冲洗泵复位","C.M.RO_CXB1@reset"]
["1#大水量冲洗泵运行","C.M.RO_CXB1@run"]
["1#大水量冲洗泵运行时间","C.M.RO_CXB1@run_time"]
["1#大水量冲洗泵启动操作","C.M.RO_CXB1@start"]
["1#大水量冲洗泵停止操作","C.M.RO_CXB1@stop"]
["1#大水量冲洗泵电流报警","C.M.RO_CXB1_A@Fault"]
["1#大水量冲洗泵电流高报警","C.M.RO_CXB1_A@H_AL"]
["1#大水量冲洗泵电流高报警开关","C.M.RO_CXB1_A@H_AL_ON"]
["1#大水量冲洗泵电流高限设置","C.M.RO_CXB1_A@H_AL_set"]
["1#大水量冲洗泵电流低报警","C.M.RO_CXB1_A@L_AL"]
["1#大水量冲洗泵电流低报警开关","C.M.RO_CXB1_A@L_AL_ON"]
["1#大水量冲洗泵电流低限设置","C.M.RO_CXB1_A@L_AL_set"]
["1#大水量冲洗泵运行电流","C.M.RO_CXB1_A@out"]
["1#大水量冲洗泵设置频率","C.M.RO_CXB1_AO_FB@spare"]
["1#大水量冲洗泵频率报警","C.M.RO_CXB1_fre@Fault"]
["1#大水量冲洗泵频率高报警","C.M.RO_CXB1_fre@H_AL"]
["1#大水量冲洗泵频率高报警开关","C.M.RO_CXB1_fre@H_AL_ON"]
["1#大水量冲洗泵频率高限设置","C.M.RO_CXB1_fre@H_AL_set"]
["1#大水量冲洗泵频率低报警","C.M.RO_CXB1_fre@L_AL"]
["1#大水量冲洗泵频率低报警开关","C.M.RO_CXB1_fre@L_AL_ON"]
["1#大水量冲洗泵频率低限设置","C.M.RO_CXB1_fre@L_AL_set"]
["1#大水量冲洗泵运行频率","C.M.RO_CXB1_fre@out"]
["2#大水量冲洗泵手自动","C.M.RO_CXB2@auto_select"]
["2#大水量冲洗泵故障","C.M.RO_CXB2@fault_total"]
["2#大水量冲洗泵远程","C.M.RO_CXB2@rem"]
["2#大水量冲洗泵复位","C.M.RO_CXB2@reset"]
["2#大水量冲洗泵运行","C.M.RO_CXB2@run"]
["2#大水量冲洗泵运行时间","C.M.RO_CXB2@run_time"]
["2#大水量冲洗泵启动操作","C.M.RO_CXB2@start"]
["2#大水量冲洗泵停止操作","C.M.RO_CXB2@stop"]
["2#大水量冲洗泵电流报警","C.M.RO_CXB2_A@Fault"]
["2#大水量冲洗泵电流高报警","C.M.RO_CXB2_A@H_AL"]
["2#大水量冲洗泵电流高报警开关","C.M.RO_CXB2_A@H_AL_ON"]
["2#大水量冲洗泵电流高限设置","C.M.RO_CXB2_A@H_AL_set"]
["2#大水量冲洗泵电流低报警","C.M.RO_CXB2_A@L_AL"]
["2#大水量冲洗泵电流低报警开关","C.M.RO_CXB2_A@L_AL_ON"]
["2#大水量冲洗泵电流低限设置","C.M.RO_CXB2_A@L_AL_set"]
["2#大水量冲洗泵运行电流","C.M.RO_CXB2_A@out"]
["2#大水量冲洗泵设置频率","C.M.RO_CXB2_AO_FB@spare"]
["2#大水量冲洗泵频率报警","C.M.RO_CXB2_fre@Fault"]
["2#大水量冲洗泵频率高报警","C.M.RO_CXB2_fre@H_AL"]
["2#大水量冲洗泵频率高报警开关","C.M.RO_CXB2_fre@H_AL_ON"]
["2#大水量冲洗泵频率高限设置","C.M.RO_CXB2_fre@H_AL_set"]
["2#大水量冲洗泵频率低报警","C.M.RO_CXB2_fre@L_AL"]
["2#大水量冲洗泵频率低报警开关","C.M.RO_CXB2_fre@L_AL_ON"]
["2#大水量冲洗泵频率低限设置","C.M.RO_CXB2_fre@L_AL_set"]
["2#大水量冲洗泵运行频率","C.M.RO_CXB2_fre@out"]
["RO还原剂加药流量报警","C.M.RO_FT_HYJ@fault"]
["RO还原剂加药流量高报警","C.M.RO_FT_HYJ@H_AL"]
["RO还原剂加药流量高报警开关","C.M.RO_FT_HYJ@H_AL_ON"]
["RO还原剂加药流量高限设置","C.M.RO_FT_HYJ@H_AL_set"]
["RO还原剂加药流量低报警","C.M.RO_FT_HYJ@L_AL"]
["RO还原剂加药流量低报警开关","C.M.RO_FT_HYJ@L_AL_ON"]
["RO还原剂加药流量低限设置","C.M.RO_FT_HYJ@L_AL_set"]
["RO还原剂加药流量","C.M.RO_FT_HYJ@out"]
["RO还原剂加药阀手自动","C.M.RO_HYJ@auto_select"]
["RO还原剂加药阀关操作","C.M.RO_HYJ@close"]
["RO还原剂加药阀关到位","C.M.RO_HYJ@close_feedback"]
["RO还原剂加药阀故障","C.M.RO_HYJ@fault_total"]
["RO还原剂加药阀开操作","C.M.RO_HYJ@open"]
["RO还原剂加药阀开到位","C.M.RO_HYJ@open_feedback"]
["RO还原剂加药阀远程","C.M.RO_HYJ@rem"]
["RO还原剂加药阀复位","C.M.RO_HYJ@reset"]
["1套反渗透启动还原剂泵频率设置","C.M.RO_HYJ_fre_set[0]"]
["2套反渗透启动还原剂泵频率设置","C.M.RO_HYJ_fre_set[1]"]
["3套反渗透启动还原剂泵频率设置","C.M.RO_HYJ_fre_set[2]"]
["4套反渗透启动还原剂泵频率设置","C.M.RO_HYJ_fre_set[3]"]
["1套反渗透启动还原剂泵台数设置","C.M.RO_HYJ_qua_set[0]"]
["2套反渗透启动还原剂泵台数设置","C.M.RO_HYJ_qua_set[1]"]
["3套反渗透启动还原剂泵台数设置","C.M.RO_HYJ_qua_set[2]"]
["4套反渗透启动还原剂泵台数设置","C.M.RO_HYJ_qua_set[3]"]
["反渗透进水总管开关","C.M.RO_LS_JSZG_L"]
["反渗透总进水ORP报警","C.M.RO_ORP_ZJS@fault"]
["反渗透总进水ORP高报警","C.M.RO_ORP_ZJS@H_AL"]
["反渗透总进水ORP高报警开关","C.M.RO_ORP_ZJS@H_AL_ON"]
["反渗透总进水ORP高限设置","C.M.RO_ORP_ZJS@H_AL_set"]
["反渗透总进水ORP低报警","C.M.RO_ORP_ZJS@L_AL"]
["反渗透总进水ORP低报警开关","C.M.RO_ORP_ZJS@L_AL_ON"]
["反渗透总进水ORP低限设置","C.M.RO_ORP_ZJS@L_AL_set"]
["反渗透总进水ORP","C.M.RO_ORP_ZJS@out"]
["反渗透总进水PH报警","C.M.RO_PH_ZJS@fault"]
["反渗透总进水PH高报警","C.M.RO_PH_ZJS@H_AL"]
["反渗透总进水PH高报警开关","C.M.RO_PH_ZJS@H_AL_ON"]
["反渗透总进水PH高限设置","C.M.RO_PH_ZJS@H_AL_set"]
["反渗透总进水PH低报警","C.M.RO_PH_ZJS@L_AL"]
["反渗透总进水PH低报警开关","C.M.RO_PH_ZJS@L_AL_ON"]
["反渗透总进水PH低限设置","C.M.RO_PH_ZJS@L_AL_set"]
["反渗透总进水PH","C.M.RO_PH_ZJS@out"]
["反渗透总产水压力报警","C.M.RO_PT_ZCS@fault"]
["反渗透总产水压力高报警","C.M.RO_PT_ZCS@H_AL"]
["反渗透总产水压力高报警开关","C.M.RO_PT_ZCS@H_AL_ON"]
["反渗透总产水压力高限设置","C.M.RO_PT_ZCS@H_AL_set"]
["反渗透总产水压力低报警","C.M.RO_PT_ZCS@L_AL"]
["反渗透总产水压力低报警开关","C.M.RO_PT_ZCS@L_AL_ON"]
["反渗透总产水压力低限设置","C.M.RO_PT_ZCS@L_AL_set"]
["反渗透总产水压力","C.M.RO_PT_ZCS@out"]
["反渗透总进水温度报警","C.M.RO_TT_ZJS@fault"]
["反渗透总进水温度高报警","C.M.RO_TT_ZJS@H_AL"]
["反渗透总进水温度高报警开关","C.M.RO_TT_ZJS@H_AL_ON"]
["反渗透总进水温度高限设置","C.M.RO_TT_ZJS@H_AL_set"]
["反渗透总进水温度低报警","C.M.RO_TT_ZJS@L_AL"]
["反渗透总进水温度低报警开关","C.M.RO_TT_ZJS@L_AL_ON"]
["反渗透总进水温度低限设置","C.M.RO_TT_ZJS@L_AL_set"]
["反渗透总进水温度","C.M.RO_TT_ZJS@out"]
["1#清水外供泵手自动","C.M.RO_WGB1@auto_select"]
["1#清水外供泵故障","C.M.RO_WGB1@fault_total"]
["1#清水外供泵远程","C.M.RO_WGB1@rem"]
["1#清水外供泵复位","C.M.RO_WGB1@reset"]
["1#清水外供泵运行","C.M.RO_WGB1@run"]
["1#清水外供泵运行时间","C.M.RO_WGB1@run_time"]
["1#清水外供泵启动操作","C.M.RO_WGB1@start"]
["1#清水外供泵停止操作","C.M.RO_WGB1@stop"]
["1#清水外供泵电流报警","C.M.RO_WGB1_A@Fault"]
["1#清水外供泵电流高报警","C.M.RO_WGB1_A@H_AL"]
["1#清水外供泵电流高报警开关","C.M.RO_WGB1_A@H_AL_ON"]
["1#清水外供泵电流高限设置","C.M.RO_WGB1_A@H_AL_set"]
["1#清水外供泵电流低报警","C.M.RO_WGB1_A@L_AL"]
["1#清水外供泵电流低报警开关","C.M.RO_WGB1_A@L_AL_ON"]
["1#清水外供泵电流低限设置","C.M.RO_WGB1_A@L_AL_set"]
["1#清水外供泵运行电流","C.M.RO_WGB1_A@out"]
["1#清水外供泵设置频率","C.M.RO_WGB1_AO_FB@spare"]
["1#清水外供泵频率报警","C.M.RO_WGB1_fre@Fault"]
["1#清水外供泵频率高报警","C.M.RO_WGB1_fre@H_AL"]
["1#清水外供泵频率高报警开关","C.M.RO_WGB1_fre@H_AL_ON"]
["1#清水外供泵频率高限设置","C.M.RO_WGB1_fre@H_AL_set"]
["1#清水外供泵频率低报警","C.M.RO_WGB1_fre@L_AL"]
["1#清水外供泵频率低报警开关","C.M.RO_WGB1_fre@L_AL_ON"]
["1#清水外供泵频率低限设置","C.M.RO_WGB1_fre@L_AL_set"]
["1#清水外供泵运行频率","C.M.RO_WGB1_fre@out"]
["2#清水外供泵手自动","C.M.RO_WGB2@auto_select"]
["2#清水外供泵故障","C.M.RO_WGB2@fault_total"]
["2#清水外供泵远程","C.M.RO_WGB2@rem"]
["2#清水外供泵复位","C.M.RO_WGB2@reset"]
["2#清水外供泵运行","C.M.RO_WGB2@run"]
["2#清水外供泵运行时间","C.M.RO_WGB2@run_time"]
["2#清水外供泵启动操作","C.M.RO_WGB2@start"]
["2#清水外供泵停止操作","C.M.RO_WGB2@stop"]
["2#清水外供泵电流报警","C.M.RO_WGB2_A@Fault"]
["2#清水外供泵电流高报警","C.M.RO_WGB2_A@H_AL"]
["2#清水外供泵电流高报警开关","C.M.RO_WGB2_A@H_AL_ON"]
["2#清水外供泵电流高限设置","C.M.RO_WGB2_A@H_AL_set"]
["2#清水外供泵电流低报警","C.M.RO_WGB2_A@L_AL"]
["2#清水外供泵电流低报警开关","C.M.RO_WGB2_A@L_AL_ON"]
["2#清水外供泵电流低限设置","C.M.RO_WGB2_A@L_AL_set"]
["2#清水外供泵运行电流","C.M.RO_WGB2_A@out"]
["2#清水外供泵设置频率","C.M.RO_WGB2_AO_FB@spare"]
["2#清水外供泵频率报警","C.M.RO_WGB2_fre@Fault"]
["2#清水外供泵频率高报警","C.M.RO_WGB2_fre@H_AL"]
["2#清水外供泵频率高报警开关","C.M.RO_WGB2_fre@H_AL_ON"]
["2#清水外供泵频率高限设置","C.M.RO_WGB2_fre@H_AL_set"]
["2#清水外供泵频率低报警","C.M.RO_WGB2_fre@L_AL"]
["2#清水外供泵频率低报警开关","C.M.RO_WGB2_fre@L_AL_ON"]
["2#清水外供泵频率低限设置","C.M.RO_WGB2_fre@L_AL_set"]
["2#清水外供泵运行频率","C.M.RO_WGB2_fre@out"]
["3#清水外供泵手自动","C.M.RO_WGB3@auto_select"]
["3#清水外供泵故障","C.M.RO_WGB3@fault_total"]
["3#清水外供泵远程","C.M.RO_WGB3@rem"]
["3#清水外供泵复位","C.M.RO_WGB3@reset"]
["3#清水外供泵运行","C.M.RO_WGB3@run"]
["3#清水外供泵运行时间","C.M.RO_WGB3@run_time"]
["3#清水外供泵启动操作","C.M.RO_WGB3@start"]
["3#清水外供泵停止操作","C.M.RO_WGB3@stop"]
["3#清水外供泵电流报警","C.M.RO_WGB3_A@Fault"]
["3#清水外供泵电流高报警","C.M.RO_WGB3_A@H_AL"]
["3#清水外供泵电流高报警开关","C.M.RO_WGB3_A@H_AL_ON"]
["3#清水外供泵电流高限设置","C.M.RO_WGB3_A@H_AL_set"]
["3#清水外供泵电流低报警","C.M.RO_WGB3_A@L_AL"]
["3#清水外供泵电流低报警开关","C.M.RO_WGB3_A@L_AL_ON"]
["3#清水外供泵电流低限设置","C.M.RO_WGB3_A@L_AL_set"]
["3#清水外供泵运行电流","C.M.RO_WGB3_A@out"]
["3#清水外供泵设置频率","C.M.RO_WGB3_AO_FB@spare"]
["3#清水外供泵频率报警","C.M.RO_WGB3_fre@Fault"]
["3#清水外供泵频率高报警","C.M.RO_WGB3_fre@H_AL"]
["3#清水外供泵频率高报警开关","C.M.RO_WGB3_fre@H_AL_ON"]
["3#清水外供泵频率高限设置","C.M.RO_WGB3_fre@H_AL_set"]
["3#清水外供泵频率低报警","C.M.RO_WGB3_fre@L_AL"]
["3#清水外供泵频率低报警开关","C.M.RO_WGB3_fre@L_AL_ON"]
["3#清水外供泵频率低限设置","C.M.RO_WGB3_fre@L_AL_set"]
["3#清水外供泵运行频率","C.M.RO_WGB3_fre@out"]
["RO1不合格水阀手自动","C.M.RO1_BHGF@auto_select"]
["RO1不合格水阀关操作","C.M.RO1_BHGF@close"]
["RO1不合格水阀关到位","C.M.RO1_BHGF@close_feedback"]
["RO1不合格水阀故障","C.M.RO1_BHGF@fault_total"]
["RO1不合格水阀开操作","C.M.RO1_BHGF@open"]
["RO1不合格水阀开到位","C.M.RO1_BHGF@open_feedback"]
["RO1不合格水阀远程","C.M.RO1_BHGF@rem"]
["RO1不合格水阀复位","C.M.RO1_BHGF@reset"]
["RO1产水CIP回水阀手自动","C.M.RO1_CIP_CSHSF@auto_select"]
["RO1产水CIP回水阀关操作","C.M.RO1_CIP_CSHSF@close"]
["RO1产水CIP回水阀关到位","C.M.RO1_CIP_CSHSF@close_feedback"]
["RO1产水CIP回水阀故障","C.M.RO1_CIP_CSHSF@fault_total"]
["RO1产水CIP回水阀开操作","C.M.RO1_CIP_CSHSF@open"]
["RO1产水CIP回水阀开到位","C.M.RO1_CIP_CSHSF@open_feedback"]
["RO1产水CIP回水阀远程","C.M.RO1_CIP_CSHSF@rem"]
["RO1产水CIP回水阀复位","C.M.RO1_CIP_CSHSF@reset"]
["RO1一段CIP回水阀手自动","C.M.RO1_CIP_HSF1@auto_select"]
["RO1一段CIP回水阀关操作","C.M.RO1_CIP_HSF1@close"]
["RO1一段CIP回水阀关到位","C.M.RO1_CIP_HSF1@close_feedback"]
["RO1一段CIP回水阀故障","C.M.RO1_CIP_HSF1@fault_total"]
["RO1一段CIP回水阀开操作","C.M.RO1_CIP_HSF1@open"]
["RO1一段CIP回水阀开到位","C.M.RO1_CIP_HSF1@open_feedback"]
["RO1一段CIP回水阀远程","C.M.RO1_CIP_HSF1@rem"]
["RO1一段CIP回水阀复位","C.M.RO1_CIP_HSF1@reset"]
["RO1二段CIP回水阀手自动","C.M.RO1_CIP_HSF2@auto_select"]
["RO1二段CIP回水阀关操作","C.M.RO1_CIP_HSF2@close"]
["RO1二段CIP回水阀关到位","C.M.RO1_CIP_HSF2@close_feedback"]
["RO1二段CIP回水阀故障","C.M.RO1_CIP_HSF2@fault_total"]
["RO1二段CIP回水阀开操作","C.M.RO1_CIP_HSF2@open"]
["RO1二段CIP回水阀开到位","C.M.RO1_CIP_HSF2@open_feedback"]
["RO1二段CIP回水阀远程","C.M.RO1_CIP_HSF2@rem"]
["RO1二段CIP回水阀复位","C.M.RO1_CIP_HSF2@reset"]
["RO1一段CIP进水阀手自动","C.M.RO1_CIP_JSF1@auto_select"]
["RO1一段CIP进水阀关操作","C.M.RO1_CIP_JSF1@close"]
["RO1一段CIP进水阀关到位","C.M.RO1_CIP_JSF1@close_feedback"]
["RO1一段CIP进水阀故障","C.M.RO1_CIP_JSF1@fault_total"]
["RO1一段CIP进水阀开操作","C.M.RO1_CIP_JSF1@open"]
["RO1一段CIP进水阀开到位","C.M.RO1_CIP_JSF1@open_feedback"]
["RO1一段CIP进水阀远程","C.M.RO1_CIP_JSF1@rem"]
["RO1一段CIP进水阀复位","C.M.RO1_CIP_JSF1@reset"]
["RO1二段CIP进水阀手自动","C.M.RO1_CIP_JSF2@auto_select"]
["RO1二段CIP进水阀关操作","C.M.RO1_CIP_JSF2@close"]
["RO1二段CIP进水阀关到位","C.M.RO1_CIP_JSF2@close_feedback"]
["RO1二段CIP进水阀故障","C.M.RO1_CIP_JSF2@fault_total"]
["RO1二段CIP进水阀开操作","C.M.RO1_CIP_JSF2@open"]
["RO1二段CIP进水阀开到位","C.M.RO1_CIP_JSF2@open_feedback"]
["RO1二段CIP进水阀远程","C.M.RO1_CIP_JSF2@rem"]
["RO1二段CIP进水阀复位","C.M.RO1_CIP_JSF2@reset"]
["RO1产水电导报警","C.M.RO1_Cond_CS@fault"]
["RO1产水电导高报警","C.M.RO1_Cond_CS@H_AL"]
["RO1产水电导高报警开关","C.M.RO1_Cond_CS@H_AL_ON"]
["RO1产水电导高限设置","C.M.RO1_Cond_CS@H_AL_set"]
["RO1产水电导低报警","C.M.RO1_Cond_CS@L_AL"]
["RO1产水电导低报警开关","C.M.RO1_Cond_CS@L_AL_ON"]
["RO1产水电导低限设置","C.M.RO1_Cond_CS@L_AL_set"]
["RO1产水电导","C.M.RO1_Cond_CS@out"]
["RO1产水阀手自动","C.M.RO1_CSF@auto_select"]
["RO1产水阀关操作","C.M.RO1_CSF@close"]
["RO1产水阀关到位","C.M.RO1_CSF@close_feedback"]
["RO1产水阀故障","C.M.RO1_CSF@fault_total"]
["RO1产水阀开操作","C.M.RO1_CSF@open"]
["RO1产水阀开到位","C.M.RO1_CSF@open_feedback"]
["RO1产水阀远程","C.M.RO1_CSF@rem"]
["RO1产水阀复位","C.M.RO1_CSF@reset"]
["RO1一段冲洗进水阀手自动","C.M.RO1_CXJF1@auto_select"]
["RO1一段冲洗进水阀关操作","C.M.RO1_CXJF1@close"]
["RO1一段冲洗进水阀关到位","C.M.RO1_CXJF1@close_feedback"]
["RO1一段冲洗进水阀故障","C.M.RO1_CXJF1@fault_total"]
["RO1一段冲洗进水阀开操作","C.M.RO1_CXJF1@open"]
["RO1一段冲洗进水阀开到位","C.M.RO1_CXJF1@open_feedback"]
["RO1一段冲洗进水阀远程","C.M.RO1_CXJF1@rem"]
["RO1一段冲洗进水阀复位","C.M.RO1_CXJF1@reset"]
["RO1二段冲洗进水阀手自动","C.M.RO1_CXJF2@auto_select"]
["RO1二段冲洗进水阀关操作","C.M.RO1_CXJF2@close"]
["RO1二段冲洗进水阀关到位","C.M.RO1_CXJF2@close_feedback"]
["RO1二段冲洗进水阀故障","C.M.RO1_CXJF2@fault_total"]
["RO1二段冲洗进水阀开操作","C.M.RO1_CXJF2@open"]
["RO1二段冲洗进水阀开到位","C.M.RO1_CXJF2@open_feedback"]
["RO1二段冲洗进水阀远程","C.M.RO1_CXJF2@rem"]
["RO1二段冲洗进水阀复位","C.M.RO1_CXJF2@reset"]
["RO1一段冲洗排水阀手自动","C.M.RO1_CXPF1@auto_select"]
["RO1一段冲洗排水阀关操作","C.M.RO1_CXPF1@close"]
["RO1一段冲洗排水阀关到位","C.M.RO1_CXPF1@close_feedback"]
["RO1一段冲洗排水阀故障","C.M.RO1_CXPF1@fault_total"]
["RO1一段冲洗排水阀开操作","C.M.RO1_CXPF1@open"]
["RO1一段冲洗排水阀开到位","C.M.RO1_CXPF1@open_feedback"]
["RO1一段冲洗排水阀远程","C.M.RO1_CXPF1@rem"]
["RO1一段冲洗排水阀复位","C.M.RO1_CXPF1@reset"]
["RO1二段冲洗排水阀手自动","C.M.RO1_CXPF2@auto_select"]
["RO1二段冲洗排水阀关操作","C.M.RO1_CXPF2@close"]
["RO1二段冲洗排水阀关到位","C.M.RO1_CXPF2@close_feedback"]
["RO1二段冲洗排水阀故障","C.M.RO1_CXPF2@fault_total"]
["RO1二段冲洗排水阀开操作","C.M.RO1_CXPF2@open"]
["RO1二段冲洗排水阀开到位","C.M.RO1_CXPF2@open_feedback"]
["RO1二段冲洗排水阀远程","C.M.RO1_CXPF2@rem"]
["RO1二段冲洗排水阀复位","C.M.RO1_CXPF2@reset"]
["RO1紧急停车","C.M.RO1_DB@button[00]"]
["RO1自动开机","C.M.RO1_DB@button[01]"]
["RO1自动停止","C.M.RO1_DB@button[02]"]
["RO1自动正常冲洗","C.M.RO1_DB@button[03]"]
["RO1自动反向冲洗","C.M.RO1_DB@button[04]"]
["RO1自动杀菌冲洗","C.M.RO1_DB@button[05]"]
["RO1未知1（不确定）","C.M.RO1_DB@button[06]"]
["RO1未知2（不确定）","C.M.RO1_DB@button[07]"]
["RO1全自动开机","C.M.RO1_DB@button[08]"]
["RO1CIP启停","C.M.RO1_DB@button[09]"]
["RO1信息清除","C.M.RO1_DB@button[10]"]
["RO1自动杀菌投入/切除","C.M.RO1_DB@button[11]"]
["RO1高压泵PID/定频控制","C.M.RO1_DB@button[12]"]
["RO1段间泵PID/定频控制","C.M.RO1_DB@button[13]"]
["RO1一段CIP（保持）","C.M.RO1_DB@button[14]"]
["RO1二段CIP（保持）","C.M.RO1_DB@button[15]"]
["RO1一段酸洗（选中保持）","C.M.RO1_DB@button[16]"]
["RO1二段酸洗（选中保持）","C.M.RO1_DB@button[17]"]
["RO1一段碱洗（选中保持）","C.M.RO1_DB@button[18]"]
["RO1二段碱洗（选中保持）","C.M.RO1_DB@button[19]"]
["RO1一段非氧洗（选中保持）","C.M.RO1_DB@button[20]"]
["RO1二段非氧洗（选中保持）","C.M.RO1_DB@button[21]"]
["RO1一段酸洗（手动保持）","C.M.RO1_DB@button[22]"]
["RO1二段酸洗（手动保持）","C.M.RO1_DB@button[23]"]
["RO1一段碱洗（手动保持）","C.M.RO1_DB@button[24]"]
["RO1二段碱洗（手动保持）","C.M.RO1_DB@button[25]"]
["RO1一段非氧洗（手动保持）","C.M.RO1_DB@button[26]"]
["RO1二段非氧洗（手动保持）","C.M.RO1_DB@button[27]"]
["RO1HOLDHB1","C.M.RO1_DB@button[28]"]
["RO1HOLDHB2","C.M.RO1_DB@button[29]"]
["RO1HOLDHB3","C.M.RO1_DB@button[30]"]
["RO1HOLDHB4","C.M.RO1_DB@button[31]"]
["RO1 ZBOOL HOLD1","C.M.RO1_DB@Zbool[0]"]
["RO1 ZBOOL HOLD2","C.M.RO1_DB@Zbool[1]"]
["RO1 ZBOOL HOLD3","C.M.RO1_DB@Zbool[2]"]
["RO1 ZDint HOLD1","C.M.RO1_DB@ZDint[0]"]
["RO1 ZDint HOLD2","C.M.RO1_DB@ZDint[1]"]
["RO1 ZDint HOLD3","C.M.RO1_DB@ZDint[2]"]
["RO1一段需要酸洗标志","C.M.RO1_DB@ZFlag[0]"]
["RO1二段需要酸洗标志","C.M.RO1_DB@ZFlag[1]"]
["RO1一段需要J洗标志","C.M.RO1_DB@ZFlag[2]"]
["RO1二段需要J洗标志","C.M.RO1_DB@ZFlag[3]"]
["RO1一段需要FY洗标志","C.M.RO1_DB@ZFlag[4]"]
["RO1二段需要FY洗标志","C.M.RO1_DB@ZFlag[5]"]
["RO1跳转一段酸洗","C.M.RO1_DB@ZFlag[6]"]
["RO1跳转二段酸洗","C.M.RO1_DB@ZFlag[7]"]
["RO1跳转一段J洗","C.M.RO1_DB@ZFlag[8]"]
["RO1跳转二段J洗","C.M.RO1_DB@ZFlag[9]"]
["RO1跳转一段非氧洗","C.M.RO1_DB@ZFlag[10]"]
["RO1跳转二段非氧洗","C.M.RO1_DB@ZFlag[11]"]
["RO1HOLD ZFLAG1","C.M.RO1_DB@ZFlag[12]"]
["RO1HOLD ZFLAG2","C.M.RO1_DB@ZFlag[13]"]
["RO1HOLD ZFLAG3","C.M.RO1_DB@ZFlag[14]"]
["RO1HOLD ZFLAG4","C.M.RO1_DB@ZFlag[15]"]
["RO1当前步序时间","C.M.RO1_DB@ZZZreal[0]"]
["RO1当前步序设定时间","C.M.RO1_DB@ZZZreal[1]"]
["RO1 1段酸洗记次数","C.M.RO1_DB@ZZZreal[2]"]
["RO1 2段酸洗记次数","C.M.RO1_DB@ZZZreal[3]"]
["RO1 1段J洗记次数","C.M.RO1_DB@ZZZreal[4]"]
["RO1 2段J洗记次数","C.M.RO1_DB@ZZZreal[5]"]
["RO1 1段FY洗记次数","C.M.RO1_DB@ZZZreal[6]"]
["RO1 2段FY洗记次数","C.M.RO1_DB@ZZZreal[7]"]
["RO1 1段酸洗设定次数","C.M.RO1_DB@ZZZreal[8]"]
["RO1 2段酸洗设定次数","C.M.RO1_DB@ZZZreal[9]"]
["RO1 1段J洗设定次数","C.M.RO1_DB@ZZZreal[10]"]
["RO1 2段J洗设定次数","C.M.RO1_DB@ZZZreal[11]"]
["RO1 1段FY洗设定次数","C.M.RO1_DB@ZZZreal[12]"]
["RO1 2段FY洗设定次数","C.M.RO1_DB@ZZZreal[13]"]
["RO1HOLD1","C.M.RO1_DB@ZZZreal[14]"]
["RO1HOLD2","C.M.RO1_DB@ZZZreal[15]"]
["RO1一段加药前冲时间设定","C.M.RO1_DB@ZZZreal[16]"]
["RO1一段加药浸泡时间设定","C.M.RO1_DB@ZZZreal[17]"]
["RO1一段加药后冲时间设定","C.M.RO1_DB@ZZZreal[18]"]
["RO1二段加药前冲时间设定","C.M.RO1_DB@ZZZreal[19]"]
["RO1二段加药浸泡时间设定","C.M.RO1_DB@ZZZreal[20]"]
["RO1二段加药后冲时间设定","C.M.RO1_DB@ZZZreal[21]"]
["RO1HOLD3","C.M.RO1_DB@ZZZreal[22]"]
["RO1HOLD4","C.M.RO1_DB@ZZZreal[23]"]
["RO1HOLD5","C.M.RO1_DB@ZZZreal[24]"]
["RO1HOLD6","C.M.RO1_DB@ZZZreal[25]"]
["RO1一段CIP循环","C.M.RO1_DB@ZZZreal[26]"]
["RO1一段CIP浸泡","C.M.RO1_DB@ZZZreal[27]"]
["RO1二段CIP循环","C.M.RO1_DB@ZZZreal[28]"]
["RO1二段CIP浸泡","C.M.RO1_DB@ZZZreal[29]"]
["RO1产水杀菌时间设定","C.M.RO1_DB@ZZZreal[30]"]
["RO1产水杀菌等待时间设定","C.M.RO1_DB@ZZZreal[31]"]
["RO1产水杀菌时间READ","C.M.RO1_DB@ZZZreal[32]"]
["RO1产水杀菌等待时间READ","C.M.RO1_DB@ZZZreal[33]"]
["RO1HOLD7","C.M.RO1_DB@ZZZreal[34]"]
["RO1HOLD8","C.M.RO1_DB@ZZZreal[35]"]
["RO1HOLD9","C.M.RO1_DB@ZZZreal[36]"]
["RO1HOLD10","C.M.RO1_DB@ZZZreal[37]"]
["RO1HOLD11","C.M.RO1_DB@ZZZreal[38]"]
["RO1HOLD12","C.M.RO1_DB@ZZZreal[39]"]
["RO1——碱冲洗设备ready","C.M.RO1_DB@ready[08]"]
["RO1——杀菌冲洗设备ready","C.M.RO1_DB@ready[09]"]
["RO1——备用1","C.M.RO1_DB@ready[10]"]
["RO1——备用2","C.M.RO1_DB@ready[11]"]
["RO1控制字","C.M.RO1_DB@control_word"]
["RO1反渗透段间泵频率设定","C.M.RO1_DB@DJB_fre_sp"]
["RO1一段压差","C.M.RO1_DB@DPT_1"]
["RO1一段差压高设定","C.M.RO1_DB@DPT_1_stop_sp"]
["RO1二段压差","C.M.RO1_DB@DPT_2"]
["RO1二段差压高设定","C.M.RO1_DB@DPT_2_stop_sp"]
["RO1电导正常可产水设定","C.M.RO1_DB@EC_ZCS_sp"]
["RO1产水电导高设定","C.M.RO1_DB@EC_ZCS_stop_sp"]
["RO1故障字","C.M.RO1_DB@fault_word"]
["RO1二段产水流量设定","C.M.RO1_DB@FT_CS2_sp"]
["RO1进水流量设定","C.M.RO1_DB@FT_JS_sp"]
["RO1反渗透高压泵频率设定","C.M.RO1_DB@GYB_fre_sp"]
["RO1控制模式","C.M.RO1_DB@model_word"]
["RO1未知3（不确定）","C.M.RO1_DB@PS[00]"]
["RO1未知4（不确定）","C.M.RO1_DB@PS[01]"]
["RO1未知5（不确定）","C.M.RO1_DB@PS[02]"]
["RO1未知6（不确定）","C.M.RO1_DB@PS[03]"]
["RO1产水压力高设定","C.M.RO1_DB@PT_CS_stop_sp"]
["RO1段间泵出水压力高设定","C.M.RO1_DB@PT_DJB_CS_stop_sp"]
["RO1段间泵进水压力低设定","C.M.RO1_DB@PT_DJB_JS_stop_sp"]
["RO1高压泵出水压力高设定","C.M.RO1_DB@PT_JS_stop_sp"]
["RO1未知7（不确定）","C.M.RO1_DB@ready[00]"]
["RO1未知8（不确定）","C.M.RO1_DB@ready[01]"]
["RO1未知9（不确定）","C.M.RO1_DB@ready[02]"]
["RO1产水准备好","C.M.RO1_DB@ready[03]"]
["RO1冲洗准备好","C.M.RO1_DB@ready[04]"]
["RO1杀菌准备好","C.M.RO1_DB@ready[05]"]
["RO1CIP准备好","C.M.RO1_DB@ready[06]"]
["RO1未知10（不确定）","C.M.RO1_DB@ready[07]"]
["RO1提醒字","C.M.RO1_DB@reminder_word"]
["RO1运行时间","C.M.RO1_DB@run_time"]
["RO1停止时间","C.M.RO1_DB@stop_time"]
["RO1不合格排水","C.M.RO1_DB@time_bhgs_display"]
["RO1不合格排水设定","C.M.RO1_DB@time_bhgs_sp"]
["RO1产水可延迟时间设定","C.M.RO1_DB@time_CS_delay_sp"]
["RO1产水时间","C.M.RO1_DB@time_CS_display"]
["RO1产水时间设定","C.M.RO1_DB@time_CS_sp"]
["RO1一段反冲","C.M.RO1_DB@time_FX1_display"]
["RO1一段反冲设定","C.M.RO1_DB@time_FX1_sp"]
["RO1开机等待","C.M.RO1_DB@time_kj_wait"]
["RO1排气时间","C.M.RO1_DB@time_kjcx_display1"]
["RO1开机冲洗","C.M.RO1_DB@time_kjcx_display2"]
["RO1排气时间设定","C.M.RO1_DB@time_kjcx_sp1"]
["RO1开机冲洗设定","C.M.RO1_DB@time_kjcx_sp2"]
["RO1杀菌间隔","C.M.RO1_DB@time_shajun_display"]
["RO1杀菌间隔设定","C.M.RO1_DB@time_shajun_sp"]
["RO1杀菌等待","C.M.RO1_DB@time_sj_wait"]
["RO1一段反冲","C.M.RO1_DB@time_sjcx1_display"]
["RO1一段反冲设定","C.M.RO1_DB@time_sjcx1_sp"]
["RO1二段反冲","C.M.RO1_DB@time_sjcx2_display"]
["RO1二段反冲设定","C.M.RO1_DB@time_sjcx2_sp"]
["RO1浸泡时间","C.M.RO1_DB@time_sjjp_display"]
["RO1浸泡时间设定","C.M.RO1_DB@time_sjjp_sp"]
["RO1加药时间","C.M.RO1_DB@time_sjjy_display"]
["RO1加药时间设定","C.M.RO1_DB@time_sjjy_sp"]
["RO1冲洗等待","C.M.RO1_DB@time_tj_wait"]
["RO1二段正冲","C.M.RO1_DB@time_ZX2_display"]
["RO1二段反冲设定","C.M.RO1_DB@time_ZX2_sp"]
["RO1正常冲洗","C.M.RO1_DB@time_ZX12_display"]
["RO1正常冲洗设定","C.M.RO1_DB@time_ZX12_sp"]
["RO1反渗透段间泵手自动","C.M.RO1_DJB@auto_select"]
["RO1反渗透段间泵故障","C.M.RO1_DJB@fault_total"]
["RO1反渗透段间泵远程","C.M.RO1_DJB@rem"]
["RO1反渗透段间泵复位","C.M.RO1_DJB@reset"]
["RO1反渗透段间泵运行","C.M.RO1_DJB@run"]
["RO1反渗透段间泵运行时间","C.M.RO1_DJB@run_time"]
["RO1反渗透段间泵启动操作","C.M.RO1_DJB@start"]
["RO1反渗透段间泵停止操作","C.M.RO1_DJB@stop"]
["RO1反渗透段间泵电流报警","C.M.RO1_DJB_A@Fault"]
["RO1反渗透段间泵电流高报警","C.M.RO1_DJB_A@H_AL"]
["RO1反渗透段间泵电流高报警开关","C.M.RO1_DJB_A@H_AL_ON"]
["RO1反渗透段间泵电流高限设置","C.M.RO1_DJB_A@H_AL_set"]
["RO1反渗透段间泵电流低报警","C.M.RO1_DJB_A@L_AL"]
["RO1反渗透段间泵电流低报警开关","C.M.RO1_DJB_A@L_AL_ON"]
["RO1反渗透段间泵电流低限设置","C.M.RO1_DJB_A@L_AL_set"]
["RO1反渗透段间泵运行电流","C.M.RO1_DJB_A@out"]
["RO1反渗透段间泵设置频率","C.M.RO1_DJB_AO_FB@spare"]
["RO1反渗透段间泵频率报警","C.M.RO1_DJB_fre@Fault"]
["RO1反渗透段间泵频率高报警","C.M.RO1_DJB_fre@H_AL"]
["RO1反渗透段间泵频率高报警开关","C.M.RO1_DJB_fre@H_AL_ON"]
["RO1反渗透段间泵频率高限设置","C.M.RO1_DJB_fre@H_AL_set"]
["RO1反渗透段间泵频率低报警","C.M.RO1_DJB_fre@L_AL"]
["RO1反渗透段间泵频率低报警开关","C.M.RO1_DJB_fre@L_AL_ON"]
["RO1反渗透段间泵频率低限设置","C.M.RO1_DJB_fre@L_AL_set"]
["RO1反渗透段间泵运行频率","C.M.RO1_DJB_fre@out"]
["RO1反渗透二段产水流量报警","C.M.RO1_FT_CS2@fault"]
["RO1反渗透二段产水流量高报警","C.M.RO1_FT_CS2@H_AL"]
["RO1反渗透二段产水流量高报警开关","C.M.RO1_FT_CS2@H_AL_ON"]
["RO1反渗透二段产水流量高限设置","C.M.RO1_FT_CS2@H_AL_set"]
["RO1反渗透二段产水流量低报警","C.M.RO1_FT_CS2@L_AL"]
["RO1反渗透二段产水流量低报警开关","C.M.RO1_FT_CS2@L_AL_ON"]
["RO1反渗透二段产水流量低限设置","C.M.RO1_FT_CS2@L_AL_set"]
["RO1反渗透二段产水流量","C.M.RO1_FT_CS2@out"]
["RO1反渗透进水流量报警","C.M.RO1_FT_JS@fault"]
["RO1反渗透进水流量高报警","C.M.RO1_FT_JS@H_AL"]
["RO1反渗透进水流量高报警开关","C.M.RO1_FT_JS@H_AL_ON"]
["RO1反渗透进水流量高限设置","C.M.RO1_FT_JS@H_AL_set"]
["RO1反渗透进水流量低报警","C.M.RO1_FT_JS@L_AL"]
["RO1反渗透进水流量低报警开关","C.M.RO1_FT_JS@L_AL_ON"]
["RO1反渗透进水流量低限设置","C.M.RO1_FT_JS@L_AL_set"]
["RO1反渗透进水流量","C.M.RO1_FT_JS@out"]
["RO1反渗透浓水流量报警","C.M.RO1_FT_NS@fault"]
["RO1反渗透浓水流量高报警","C.M.RO1_FT_NS@H_AL"]
["RO1反渗透浓水流量高报警开关","C.M.RO1_FT_NS@H_AL_ON"]
["RO1反渗透浓水流量高限设置","C.M.RO1_FT_NS@H_AL_set"]
["RO1反渗透浓水流量低报警","C.M.RO1_FT_NS@L_AL"]
["RO1反渗透浓水流量低报警开关","C.M.RO1_FT_NS@L_AL_ON"]
["RO1反渗透浓水流量低限设置","C.M.RO1_FT_NS@L_AL_set"]
["RO1反渗透浓水流量","C.M.RO1_FT_NS@out"]
["RO1反渗透高压泵手自动","C.M.RO1_GYB@auto_select"]
["RO1反渗透高压泵故障","C.M.RO1_GYB@fault_total"]
["RO1反渗透高压泵远程","C.M.RO1_GYB@rem"]
["RO1反渗透高压泵复位","C.M.RO1_GYB@reset"]
["RO1反渗透高压泵运行","C.M.RO1_GYB@run"]
["RO1反渗透高压泵运行时间","C.M.RO1_GYB@run_time"]
["RO1反渗透高压泵启动操作","C.M.RO1_GYB@start"]
["RO1反渗透高压泵停止操作","C.M.RO1_GYB@stop"]
["RO1反渗透高压泵电流报警","C.M.RO1_GYB_A@Fault"]
["RO1反渗透高压泵电流高报警","C.M.RO1_GYB_A@H_AL"]
["RO1反渗透高压泵电流高报警开关","C.M.RO1_GYB_A@H_AL_ON"]
["RO1反渗透高压泵电流高限设置","C.M.RO1_GYB_A@H_AL_set"]
["RO1反渗透高压泵电流低报警","C.M.RO1_GYB_A@L_AL"]
["RO1反渗透高压泵电流低报警开关","C.M.RO1_GYB_A@L_AL_ON"]
["RO1反渗透高压泵电流低限设置","C.M.RO1_GYB_A@L_AL_set"]
["RO1反渗透高压泵运行电流","C.M.RO1_GYB_A@out"]
["RO1反渗透高压泵设置频率","C.M.RO1_GYB_AO_FB@spare"]
["RO1反渗透高压泵频率报警","C.M.RO1_GYB_fre@Fault"]
["RO1反渗透高压泵频率高报警","C.M.RO1_GYB_fre@H_AL"]
["RO1反渗透高压泵频率高报警开关","C.M.RO1_GYB_fre@H_AL_ON"]
["RO1反渗透高压泵频率高限设置","C.M.RO1_GYB_fre@H_AL_set"]
["RO1反渗透高压泵频率低报警","C.M.RO1_GYB_fre@L_AL"]
["RO1反渗透高压泵频率低报警开关","C.M.RO1_GYB_fre@L_AL_ON"]
["RO1反渗透高压泵频率低限设置","C.M.RO1_GYB_fre@L_AL_set"]
["RO1反渗透高压泵运行频率","C.M.RO1_GYB_fre@out"]
["RO1进水调节阀开度设定值","C.M.RO1_GYBF_AO_FB@spare"]
["RO1进水调节阀开度报警","C.M.RO1_GYBF_kd@fault"]
["RO1进水调节阀开度高报警","C.M.RO1_GYBF_kd@H_AL"]
["RO1进水调节阀开度高报警开关","C.M.RO1_GYBF_kd@H_AL_ON"]
["RO1进水调节阀开度高限设置","C.M.RO1_GYBF_kd@H_AL_set"]
["RO1进水调节阀开度低报警","C.M.RO1_GYBF_kd@L_AL"]
["RO1进水调节阀开度低报警开关","C.M.RO1_GYBF_kd@L_AL_ON"]
["RO1进水调节阀开度低限设置","C.M.RO1_GYBF_kd@L_AL_set"]
["RO1进水调节阀开度","C.M.RO1_GYBF_kd@out"]
["RO1反渗透段间泵高压开关","C.M.RO1_LS_DJB_H"]
["RO1反渗透段间泵低压开关","C.M.RO1_LS_DJB_L"]
["RO1反渗透高压泵高压开关","C.M.RO1_LS_GYB_H"]
["RO1反渗透高压泵低压开关","C.M.RO1_LS_GYB_L"]
["RO1排气阀1手自动","C.M.RO1_PQF1@auto_select"]
["RO1排气阀1关操作","C.M.RO1_PQF1@close"]
["RO1排气阀1关到位","C.M.RO1_PQF1@close_feedback"]
["RO1排气阀1故障","C.M.RO1_PQF1@fault_total"]
["RO1排气阀1开操作","C.M.RO1_PQF1@open"]
["RO1排气阀1开到位","C.M.RO1_PQF1@open_feedback"]
["RO1排气阀1远程","C.M.RO1_PQF1@rem"]
["RO1排气阀1复位","C.M.RO1_PQF1@reset"]
["RO1排气阀2手自动","C.M.RO1_PQF2@auto_select"]
["RO1排气阀2关操作","C.M.RO1_PQF2@close"]
["RO1排气阀2关到位","C.M.RO1_PQF2@close_feedback"]
["RO1排气阀2故障","C.M.RO1_PQF2@fault_total"]
["RO1排气阀2开操作","C.M.RO1_PQF2@open"]
["RO1排气阀2开到位","C.M.RO1_PQF2@open_feedback"]
["RO1排气阀2远程","C.M.RO1_PQF2@rem"]
["RO1排气阀2复位","C.M.RO1_PQF2@reset"]
["RO1排气阀3手自动","C.M.RO1_PQF3@auto_select"]
["RO1排气阀3关操作","C.M.RO1_PQF3@close"]
["RO1排气阀3关到位","C.M.RO1_PQF3@close_feedback"]
["RO1排气阀3故障","C.M.RO1_PQF3@fault_total"]
["RO1排气阀3开操作","C.M.RO1_PQF3@open"]
["RO1排气阀3开到位","C.M.RO1_PQF3@open_feedback"]
["RO1排气阀3远程","C.M.RO1_PQF3@rem"]
["RO1排气阀3复位","C.M.RO1_PQF3@reset"]
["RO1排气阀4手自动","C.M.RO1_PQF4@auto_select"]
["RO1排气阀4关操作","C.M.RO1_PQF4@close"]
["RO1排气阀4关到位","C.M.RO1_PQF4@close_feedback"]
["RO1排气阀4故障","C.M.RO1_PQF4@fault_total"]
["RO1排气阀4开操作","C.M.RO1_PQF4@open"]
["RO1排气阀4开到位","C.M.RO1_PQF4@open_feedback"]
["RO1排气阀4远程","C.M.RO1_PQF4@rem"]
["RO1排气阀4复位","C.M.RO1_PQF4@reset"]
["RO1排气阀5手自动","C.M.RO1_PQF5@auto_select"]
["RO1排气阀5关操作","C.M.RO1_PQF5@close"]
["RO1排气阀5关到位","C.M.RO1_PQF5@close_feedback"]
["RO1排气阀5故障","C.M.RO1_PQF5@fault_total"]
["RO1排气阀5开操作","C.M.RO1_PQF5@open"]
["RO1排气阀5开到位","C.M.RO1_PQF5@open_feedback"]
["RO1排气阀5远程","C.M.RO1_PQF5@rem"]
["RO1排气阀5复位","C.M.RO1_PQF5@reset"]
["RO1排气阀6手自动","C.M.RO1_PQF6@auto_select"]
["RO1排气阀6关操作","C.M.RO1_PQF6@close"]
["RO1排气阀6关到位","C.M.RO1_PQF6@close_feedback"]
["RO1排气阀6故障","C.M.RO1_PQF6@fault_total"]
["RO1排气阀6开操作","C.M.RO1_PQF6@open"]
["RO1排气阀6开到位","C.M.RO1_PQF6@open_feedback"]
["RO1排气阀6远程","C.M.RO1_PQF6@rem"]
["RO1排气阀6复位","C.M.RO1_PQF6@reset"]
["RO1排气阀7手自动","C.M.RO1_PQF7@auto_select"]
["RO1排气阀7关操作","C.M.RO1_PQF7@close"]
["RO1排气阀7关到位","C.M.RO1_PQF7@close_feedback"]
["RO1排气阀7故障","C.M.RO1_PQF7@fault_total"]
["RO1排气阀7开操作","C.M.RO1_PQF7@open"]
["RO1排气阀7开到位","C.M.RO1_PQF7@open_feedback"]
["RO1排气阀7远程","C.M.RO1_PQF7@rem"]
["RO1排气阀7复位","C.M.RO1_PQF7@reset"]
["RO1产水压力报警","C.M.RO1_PT_CS@fault"]
["RO1产水压力高报警","C.M.RO1_PT_CS@H_AL"]
["RO1产水压力高报警开关","C.M.RO1_PT_CS@H_AL_ON"]
["RO1产水压力高限设置","C.M.RO1_PT_CS@H_AL_set"]
["RO1产水压力低报警","C.M.RO1_PT_CS@L_AL"]
["RO1产水压力低报警开关","C.M.RO1_PT_CS@L_AL_ON"]
["RO1产水压力低限设置","C.M.RO1_PT_CS@L_AL_set"]
["RO1产水压力","C.M.RO1_PT_CS@out"]
["RO1一段浓水压力报警","C.M.RO1_PT_DJ1@fault"]
["RO1一段浓水压力高报警","C.M.RO1_PT_DJ1@H_AL"]
["RO1一段浓水压力高报警开关","C.M.RO1_PT_DJ1@H_AL_ON"]
["RO1一段浓水压力高限设置","C.M.RO1_PT_DJ1@H_AL_set"]
["RO1一段浓水压力低报警","C.M.RO1_PT_DJ1@L_AL"]
["RO1一段浓水压力低报警开关","C.M.RO1_PT_DJ1@L_AL_ON"]
["RO1一段浓水压力低限设置","C.M.RO1_PT_DJ1@L_AL_set"]
["RO1一段浓水压力","C.M.RO1_PT_DJ1@out"]
["RO1二段进水压力报警","C.M.RO1_PT_DJ2@fault"]
["RO1二段进水压力高报警","C.M.RO1_PT_DJ2@H_AL"]
["RO1二段进水压力高报警开关","C.M.RO1_PT_DJ2@H_AL_ON"]
["RO1二段进水压力高限设置","C.M.RO1_PT_DJ2@H_AL_set"]
["RO1二段进水压力低报警","C.M.RO1_PT_DJ2@L_AL"]
["RO1二段进水压力低报警开关","C.M.RO1_PT_DJ2@L_AL_ON"]
["RO1二段进水压力低限设置","C.M.RO1_PT_DJ2@L_AL_set"]
["RO1二段进水压力","C.M.RO1_PT_DJ2@out"]
["RO1一段进水压力报警","C.M.RO1_PT_JS@fault"]
["RO1一段进水压力高报警","C.M.RO1_PT_JS@H_AL"]
["RO1一段进水压力高报警开关","C.M.RO1_PT_JS@H_AL_ON"]
["RO1一段进水压力高限设置","C.M.RO1_PT_JS@H_AL_set"]
["RO1一段进水压力低报警","C.M.RO1_PT_JS@L_AL"]
["RO1一段进水压力低报警开关","C.M.RO1_PT_JS@L_AL_ON"]
["RO1一段进水压力低限设置","C.M.RO1_PT_JS@L_AL_set"]
["RO1一段进水压力","C.M.RO1_PT_JS@out"]
["RO1二段浓水压力报警","C.M.RO1_PT_NS@fault"]
["RO1二段浓水压力高报警","C.M.RO1_PT_NS@H_AL"]
["RO1二段浓水压力高报警开关","C.M.RO1_PT_NS@H_AL_ON"]
["RO1二段浓水压力高限设置","C.M.RO1_PT_NS@H_AL_set"]
["RO1二段浓水压力低报警","C.M.RO1_PT_NS@L_AL"]
["RO1二段浓水压力低报警开关","C.M.RO1_PT_NS@L_AL_ON"]
["RO1二段浓水压力低限设置","C.M.RO1_PT_NS@L_AL_set"]
["RO1二段浓水压力","C.M.RO1_PT_NS@out"]
["RO1未知阀手自动","C.M.RO1_SJJF@auto_select"]
["RO1未知阀关操作","C.M.RO1_SJJF@close"]
["RO1未知阀关到位","C.M.RO1_SJJF@close_feedback"]
["RO1未知阀故障","C.M.RO1_SJJF@fault_total"]
["RO1未知阀开操作","C.M.RO1_SJJF@open"]
["RO1未知阀开到位","C.M.RO1_SJJF@open_feedback"]
["RO1未知阀远程","C.M.RO1_SJJF@rem"]
["RO1未知阀复位","C.M.RO1_SJJF@reset"]
["1#阻垢剂加药阀手自动","C.M.RO1_ZGJF@auto_select"]
["1#阻垢剂加药阀关操作","C.M.RO1_ZGJF@close"]
["1#阻垢剂加药阀关到位","C.M.RO1_ZGJF@close_feedback"]
["1#阻垢剂加药阀故障","C.M.RO1_ZGJF@fault_total"]
["1#阻垢剂加药阀开操作","C.M.RO1_ZGJF@open"]
["1#阻垢剂加药阀开到位","C.M.RO1_ZGJF@open_feedback"]
["1#阻垢剂加药阀远程","C.M.RO1_ZGJF@rem"]
["1#阻垢剂加药阀复位","C.M.RO1_ZGJF@reset"]
["RO2不合格水阀手自动","C.M.RO2_BHGF@auto_select"]
["RO2不合格水阀关操作","C.M.RO2_BHGF@close"]
["RO2不合格水阀关到位","C.M.RO2_BHGF@close_feedback"]
["RO2不合格水阀故障","C.M.RO2_BHGF@fault_total"]
["RO2不合格水阀开操作","C.M.RO2_BHGF@open"]
["RO2不合格水阀开到位","C.M.RO2_BHGF@open_feedback"]
["RO2不合格水阀远程","C.M.RO2_BHGF@rem"]
["RO2不合格水阀复位","C.M.RO2_BHGF@reset"]
["RO2产水CIP回水阀手自动","C.M.RO2_CIP_CSHSF@auto_select"]
["RO2产水CIP回水阀关操作","C.M.RO2_CIP_CSHSF@close"]
["RO2产水CIP回水阀关到位","C.M.RO2_CIP_CSHSF@close_feedback"]
["RO2产水CIP回水阀故障","C.M.RO2_CIP_CSHSF@fault_total"]
["RO2产水CIP回水阀开操作","C.M.RO2_CIP_CSHSF@open"]
["RO2产水CIP回水阀开到位","C.M.RO2_CIP_CSHSF@open_feedback"]
["RO2产水CIP回水阀远程","C.M.RO2_CIP_CSHSF@rem"]
["RO2产水CIP回水阀复位","C.M.RO2_CIP_CSHSF@reset"]
["RO2一段CIP回水阀手自动","C.M.RO2_CIP_HSF1@auto_select"]
["RO2一段CIP回水阀关操作","C.M.RO2_CIP_HSF1@close"]
["RO2一段CIP回水阀关到位","C.M.RO2_CIP_HSF1@close_feedback"]
["RO2一段CIP回水阀故障","C.M.RO2_CIP_HSF1@fault_total"]
["RO2一段CIP回水阀开操作","C.M.RO2_CIP_HSF1@open"]
["RO2一段CIP回水阀开到位","C.M.RO2_CIP_HSF1@open_feedback"]
["RO2一段CIP回水阀远程","C.M.RO2_CIP_HSF1@rem"]
["RO2一段CIP回水阀复位","C.M.RO2_CIP_HSF1@reset"]
["RO2二段CIP回水阀手自动","C.M.RO2_CIP_HSF2@auto_select"]
["RO2二段CIP回水阀关操作","C.M.RO2_CIP_HSF2@close"]
["RO2二段CIP回水阀关到位","C.M.RO2_CIP_HSF2@close_feedback"]
["RO2二段CIP回水阀故障","C.M.RO2_CIP_HSF2@fault_total"]
["RO2二段CIP回水阀开操作","C.M.RO2_CIP_HSF2@open"]
["RO2二段CIP回水阀开到位","C.M.RO2_CIP_HSF2@open_feedback"]
["RO2二段CIP回水阀远程","C.M.RO2_CIP_HSF2@rem"]
["RO2二段CIP回水阀复位","C.M.RO2_CIP_HSF2@reset"]
["RO2一段CIP进水阀手自动","C.M.RO2_CIP_JSF1@auto_select"]
["RO2一段CIP进水阀关操作","C.M.RO2_CIP_JSF1@close"]
["RO2一段CIP进水阀关到位","C.M.RO2_CIP_JSF1@close_feedback"]
["RO2一段CIP进水阀故障","C.M.RO2_CIP_JSF1@fault_total"]
["RO2一段CIP进水阀开操作","C.M.RO2_CIP_JSF1@open"]
["RO2一段CIP进水阀开到位","C.M.RO2_CIP_JSF1@open_feedback"]
["RO2一段CIP进水阀远程","C.M.RO2_CIP_JSF1@rem"]
["RO2一段CIP进水阀复位","C.M.RO2_CIP_JSF1@reset"]
["RO2二段CIP进水阀手自动","C.M.RO2_CIP_JSF2@auto_select"]
["RO2二段CIP进水阀关操作","C.M.RO2_CIP_JSF2@close"]
["RO2二段CIP进水阀关到位","C.M.RO2_CIP_JSF2@close_feedback"]
["RO2二段CIP进水阀故障","C.M.RO2_CIP_JSF2@fault_total"]
["RO2二段CIP进水阀开操作","C.M.RO2_CIP_JSF2@open"]
["RO2二段CIP进水阀开到位","C.M.RO2_CIP_JSF2@open_feedback"]
["RO2二段CIP进水阀远程","C.M.RO2_CIP_JSF2@rem"]
["RO2二段CIP进水阀复位","C.M.RO2_CIP_JSF2@reset"]
["RO2产水电导报警","C.M.RO2_Cond_CS@fault"]
["RO2产水电导高报警","C.M.RO2_Cond_CS@H_AL"]
["RO2产水电导高报警开关","C.M.RO2_Cond_CS@H_AL_ON"]
["RO2产水电导高限设置","C.M.RO2_Cond_CS@H_AL_set"]
["RO2产水电导低报警","C.M.RO2_Cond_CS@L_AL"]
["RO2产水电导低报警开关","C.M.RO2_Cond_CS@L_AL_ON"]
["RO2产水电导低限设置","C.M.RO2_Cond_CS@L_AL_set"]
["RO2产水电导","C.M.RO2_Cond_CS@out"]
["RO2产水阀手自动","C.M.RO2_CSF@auto_select"]
["RO2产水阀关操作","C.M.RO2_CSF@close"]
["RO2产水阀关到位","C.M.RO2_CSF@close_feedback"]
["RO2产水阀故障","C.M.RO2_CSF@fault_total"]
["RO2产水阀开操作","C.M.RO2_CSF@open"]
["RO2产水阀开到位","C.M.RO2_CSF@open_feedback"]
["RO2产水阀远程","C.M.RO2_CSF@rem"]
["RO2产水阀复位","C.M.RO2_CSF@reset"]
["RO2一段冲洗进水阀手自动","C.M.RO2_CXJF1@auto_select"]
["RO2一段冲洗进水阀关操作","C.M.RO2_CXJF1@close"]
["RO2一段冲洗进水阀关到位","C.M.RO2_CXJF1@close_feedback"]
["RO2一段冲洗进水阀故障","C.M.RO2_CXJF1@fault_total"]
["RO2一段冲洗进水阀开操作","C.M.RO2_CXJF1@open"]
["RO2一段冲洗进水阀开到位","C.M.RO2_CXJF1@open_feedback"]
["RO2一段冲洗进水阀远程","C.M.RO2_CXJF1@rem"]
["RO2一段冲洗进水阀复位","C.M.RO2_CXJF1@reset"]
["RO2二段冲洗进水阀手自动","C.M.RO2_CXJF2@auto_select"]
["RO2二段冲洗进水阀关操作","C.M.RO2_CXJF2@close"]
["RO2二段冲洗进水阀关到位","C.M.RO2_CXJF2@close_feedback"]
["RO2二段冲洗进水阀故障","C.M.RO2_CXJF2@fault_total"]
["RO2二段冲洗进水阀开操作","C.M.RO2_CXJF2@open"]
["RO2二段冲洗进水阀开到位","C.M.RO2_CXJF2@open_feedback"]
["RO2二段冲洗进水阀远程","C.M.RO2_CXJF2@rem"]
["RO2二段冲洗进水阀复位","C.M.RO2_CXJF2@reset"]
["RO2一段冲洗排水阀手自动","C.M.RO2_CXPF1@auto_select"]
["RO2一段冲洗排水阀关操作","C.M.RO2_CXPF1@close"]
["RO2一段冲洗排水阀关到位","C.M.RO2_CXPF1@close_feedback"]
["RO2一段冲洗排水阀故障","C.M.RO2_CXPF1@fault_total"]
["RO2一段冲洗排水阀开操作","C.M.RO2_CXPF1@open"]
["RO2一段冲洗排水阀开到位","C.M.RO2_CXPF1@open_feedback"]
["RO2一段冲洗排水阀远程","C.M.RO2_CXPF1@rem"]
["RO2一段冲洗排水阀复位","C.M.RO2_CXPF1@reset"]
["RO2二段冲洗排水阀手自动","C.M.RO2_CXPF2@auto_select"]
["RO2二段冲洗排水阀关操作","C.M.RO2_CXPF2@close"]
["RO2二段冲洗排水阀关到位","C.M.RO2_CXPF2@close_feedback"]
["RO2二段冲洗排水阀故障","C.M.RO2_CXPF2@fault_total"]
["RO2二段冲洗排水阀开操作","C.M.RO2_CXPF2@open"]
["RO2二段冲洗排水阀开到位","C.M.RO2_CXPF2@open_feedback"]
["RO2二段冲洗排水阀远程","C.M.RO2_CXPF2@rem"]
["RO2二段冲洗排水阀复位","C.M.RO2_CXPF2@reset"]
["RO2紧急停车","C.M.RO2_DB@button[00]"]
["RO2自动开机","C.M.RO2_DB@button[01]"]
["RO2自动停止","C.M.RO2_DB@button[02]"]
["RO2自动正常冲洗","C.M.RO2_DB@button[03]"]
["RO2自动反向冲洗","C.M.RO2_DB@button[04]"]
["RO2自动杀菌冲洗","C.M.RO2_DB@button[05]"]
["RO2未知1（不确定）","C.M.RO2_DB@button[06]"]
["RO2未知2（不确定）","C.M.RO2_DB@button[07]"]
["RO2全自动开机","C.M.RO2_DB@button[08]"]
["RO2CIP启停","C.M.RO2_DB@button[09]"]
["RO2信息清除","C.M.RO2_DB@button[10]"]
["RO2自动杀菌投入/切除","C.M.RO2_DB@button[11]"]
["RO2高压泵PID/定频控制","C.M.RO2_DB@button[12]"]
["RO2段间泵PID/定频控制","C.M.RO2_DB@button[13]"]
["RO2一段CIP（保持）","C.M.RO2_DB@button[14]"]
["RO2二段CIP（保持）","C.M.RO2_DB@button[15]"]
["RO2一段酸洗（选中保持）","C.M.RO2_DB@button[16]"]
["RO2二段酸洗（选中保持）","C.M.RO2_DB@button[17]"]
["RO2一段碱洗（选中保持）","C.M.RO2_DB@button[18]"]
["RO2二段碱洗（选中保持）","C.M.RO2_DB@button[19]"]
["RO2一段非氧洗（选中保持）","C.M.RO2_DB@button[20]"]
["RO2二段非氧洗（选中保持）","C.M.RO2_DB@button[21]"]
["RO2一段酸洗（手动保持）","C.M.RO2_DB@button[22]"]
["RO2二段酸洗（手动保持）","C.M.RO2_DB@button[23]"]
["RO2一段碱洗（手动保持）","C.M.RO2_DB@button[24]"]
["RO2二段碱洗（手动保持）","C.M.RO2_DB@button[25]"]
["RO2一段非氧洗（手动保持）","C.M.RO2_DB@button[26]"]
["RO2二段非氧洗（手动保持）","C.M.RO2_DB@button[27]"]
["RO2HOLD HB1","C.M.RO2_DB@button[28]"]
["RO2HOLD HB2","C.M.RO2_DB@button[29]"]
["RO2HOLD HB3","C.M.RO2_DB@button[30]"]
["RO2HOLD HB4","C.M.RO2_DB@button[31]"]
["RO2 ZBOOL HOLD1","C.M.RO2_DB@Zbool[0]"]
["RO2 ZBOOL HOLD2","C.M.RO2_DB@Zbool[1]"]
["RO2 ZBOOL HOLD3","C.M.RO2_DB@Zbool[2]"]
["RO2 ZDint HOLD1","C.M.RO2_DB@ZDint[0]"]
["RO2 ZDint HOLD2","C.M.RO2_DB@ZDint[1]"]
["RO2 ZDint HOLD3","C.M.RO2_DB@ZDint[2]"]
["RO2一段需要酸洗标志","C.M.RO2_DB@ZFlag[0]"]
["RO2二段需要酸洗标志","C.M.RO2_DB@ZFlag[1]"]
["RO2一段需要J洗标志","C.M.RO2_DB@ZFlag[2]"]
["RO2二段需要J洗标志","C.M.RO2_DB@ZFlag[3]"]
["RO2一段需要FY洗标志","C.M.RO2_DB@ZFlag[4]"]
["RO2二段需要FY洗标志","C.M.RO2_DB@ZFlag[5]"]
["RO2跳转一段酸洗","C.M.RO2_DB@ZFlag[6]"]
["RO2跳转二段酸洗","C.M.RO2_DB@ZFlag[7]"]
["RO2跳转一段J洗","C.M.RO2_DB@ZFlag[8]"]
["RO2跳转二段J洗","C.M.RO2_DB@ZFlag[9]"]
["RO2跳转一段非氧洗","C.M.RO2_DB@ZFlag[10]"]
["RO2跳转二段非氧洗","C.M.RO2_DB@ZFlag[11]"]
["RO2HOLD ZFLAG1","C.M.RO2_DB@ZFlag[12]"]
["RO2HOLD ZFLAG2","C.M.RO2_DB@ZFlag[13]"]
["RO2HOLD ZFLAG3","C.M.RO2_DB@ZFlag[14]"]
["RO2HOLD ZFLAG4","C.M.RO2_DB@ZFlag[15]"]
["RO2当前步序时间","C.M.RO2_DB@ZZZreal[0]"]
["RO2当前步序设定时间","C.M.RO2_DB@ZZZreal[1]"]
["RO2 1段酸洗记次数","C.M.RO2_DB@ZZZreal[2]"]
["RO2 2段酸洗记次数","C.M.RO2_DB@ZZZreal[3]"]
["RO2 1段J洗记次数","C.M.RO2_DB@ZZZreal[4]"]
["RO2 2段J洗记次数","C.M.RO2_DB@ZZZreal[5]"]
["RO2 1段FY洗记次数","C.M.RO2_DB@ZZZreal[6]"]
["RO2 2段FY洗记次数","C.M.RO2_DB@ZZZreal[7]"]
["RO2 1段酸洗设定次数","C.M.RO2_DB@ZZZreal[8]"]
["RO2 2段酸洗设定次数","C.M.RO2_DB@ZZZreal[9]"]
["RO2 1段J洗设定次数","C.M.RO2_DB@ZZZreal[10]"]
["RO2 2段J洗设定次数","C.M.RO2_DB@ZZZreal[11]"]
["RO2 1段FY洗设定次数","C.M.RO2_DB@ZZZreal[12]"]
["RO2 2段FY洗设定次数","C.M.RO2_DB@ZZZreal[13]"]
["RO2HOLD1","C.M.RO2_DB@ZZZreal[14]"]
["RO2HOLD2","C.M.RO2_DB@ZZZreal[15]"]
["RO2 一段加药前冲时间设定","C.M.RO2_DB@ZZZreal[16]"]
["RO2 一段加药浸泡时间设定","C.M.RO2_DB@ZZZreal[17]"]
["RO2 一段加药后冲时间设定","C.M.RO2_DB@ZZZreal[18]"]
["RO2 二段加药前冲时间设定","C.M.RO2_DB@ZZZreal[19]"]
["RO2 二段加药浸泡时间设定","C.M.RO2_DB@ZZZreal[20]"]
["RO2 二段加药后冲时间设定","C.M.RO2_DB@ZZZreal[21]"]
["RO2HOLD3","C.M.RO2_DB@ZZZreal[22]"]
["RO2HOLD4","C.M.RO2_DB@ZZZreal[23]"]
["RO2HOLD5","C.M.RO2_DB@ZZZreal[24]"]
["RO2HOLD6","C.M.RO2_DB@ZZZreal[25]"]
["RO2 一段CIP循环","C.M.RO2_DB@ZZZreal[26]"]
["RO2 一段CIP浸泡","C.M.RO2_DB@ZZZreal[27]"]
["RO2 二段CIP循环","C.M.RO2_DB@ZZZreal[28]"]
["RO2 二段CIP浸泡","C.M.RO2_DB@ZZZreal[29]"]
["RO2 产水杀菌时间设定","C.M.RO2_DB@ZZZreal[30]"]
["RO2 产水杀菌等待时间设定","C.M.RO2_DB@ZZZreal[31]"]
["RO2 产水杀菌时间READ","C.M.RO2_DB@ZZZreal[32]"]
["RO2 产水杀菌等待时间READ","C.M.RO2_DB@ZZZreal[33]"]
["RO2HOLD7","C.M.RO2_DB@ZZZreal[34]"]
["RO2HOLD8","C.M.RO2_DB@ZZZreal[35]"]
["RO2HOLD9","C.M.RO2_DB@ZZZreal[36]"]
["RO2HOLD10","C.M.RO2_DB@ZZZreal[37]"]
["RO2HOLD11","C.M.RO2_DB@ZZZreal[38]"]
["RO2HOLD12","C.M.RO2_DB@ZZZreal[39]"]
["RO2——碱冲洗设备ready","C.M.RO2_DB@ready[08]"]
["RO2——杀菌冲洗设备ready","C.M.RO2_DB@ready[09]"]
["RO2——备用1","C.M.RO2_DB@ready[10]"]
["RO2——备用2","C.M.RO2_DB@ready[11]"]
["RO2控制字","C.M.RO2_DB@control_word"]
["RO2反渗透段间泵频率设定","C.M.RO2_DB@DJB_fre_sp"]
["RO2一段压差","C.M.RO2_DB@DPT_1"]
["RO2一段差压高设定","C.M.RO2_DB@DPT_1_stop_sp"]
["RO2二段压差","C.M.RO2_DB@DPT_2"]
["RO2二段差压高设定","C.M.RO2_DB@DPT_2_stop_sp"]
["RO2电导正常可产水设定","C.M.RO2_DB@EC_ZCS_sp"]
["RO2产水电导高设定","C.M.RO2_DB@EC_ZCS_stop_sp"]
["RO2故障字","C.M.RO2_DB@fault_word"]
["RO2二段产水流量设定","C.M.RO2_DB@FT_CS2_sp"]
["RO2进水流量设定","C.M.RO2_DB@FT_JS_sp"]
["RO2反渗透高压泵频率设定","C.M.RO2_DB@GYB_fre_sp"]
["RO2控制模式","C.M.RO2_DB@model_word"]
["RO2未知3（不确定）","C.M.RO2_DB@PS[00]"]
["RO2未知4（不确定）","C.M.RO2_DB@PS[01]"]
["RO2未知5（不确定）","C.M.RO2_DB@PS[02]"]
["RO2未知6（不确定）","C.M.RO2_DB@PS[03]"]
["RO2产水压力高设定","C.M.RO2_DB@PT_CS_stop_sp"]
["RO2段间泵出水压力高设定","C.M.RO2_DB@PT_DJB_CS_stop_sp"]
["RO2段间泵进水压力低设定","C.M.RO2_DB@PT_DJB_JS_stop_sp"]
["RO2高压泵出水压力高设定","C.M.RO2_DB@PT_JS_stop_sp"]
["RO2未知7（不确定）","C.M.RO2_DB@ready[00]"]
["RO2未知8（不确定）","C.M.RO2_DB@ready[01]"]
["RO2未知9（不确定）","C.M.RO2_DB@ready[02]"]
["RO2产水准备好","C.M.RO2_DB@ready[03]"]
["RO2冲洗准备好","C.M.RO2_DB@ready[04]"]
["RO2杀菌准备好","C.M.RO2_DB@ready[05]"]
["RO2CIP准备好","C.M.RO2_DB@ready[06]"]
["RO2未知10（不确定）","C.M.RO2_DB@ready[07]"]
["RO2提醒字","C.M.RO2_DB@reminder_word"]
["RO2运行时间","C.M.RO2_DB@run_time"]
["RO2停止时间","C.M.RO2_DB@stop_time"]
["RO2不合格排水","C.M.RO2_DB@time_bhgs_display"]
["RO2不合格排水设定","C.M.RO2_DB@time_bhgs_sp"]
["RO2产水可延迟时间设定","C.M.RO2_DB@time_CS_delay_sp"]
["RO2产水时间","C.M.RO2_DB@time_CS_display"]
["RO2产水时间设定","C.M.RO2_DB@time_CS_sp"]
["RO2一段反冲","C.M.RO2_DB@time_FX1_display"]
["RO2一段反冲设定","C.M.RO2_DB@time_FX1_sp"]
["RO2开机等待","C.M.RO2_DB@time_kj_wait"]
["RO2排气时间","C.M.RO2_DB@time_kjcx_display1"]
["RO2开机冲洗","C.M.RO2_DB@time_kjcx_display2"]
["RO2排气时间设定","C.M.RO2_DB@time_kjcx_sp1"]
["RO2开机冲洗设定","C.M.RO2_DB@time_kjcx_sp2"]
["RO2杀菌间隔","C.M.RO2_DB@time_shajun_display"]
["RO2杀菌间隔设定","C.M.RO2_DB@time_shajun_sp"]
["RO2杀菌等待","C.M.RO2_DB@time_sj_wait"]
["RO2一段反冲","C.M.RO2_DB@time_sjcx1_display"]
["RO2一段反冲设定","C.M.RO2_DB@time_sjcx1_sp"]
["RO2二段反冲","C.M.RO2_DB@time_sjcx2_display"]
["RO2二段反冲设定","C.M.RO2_DB@time_sjcx2_sp"]
["RO2浸泡时间","C.M.RO2_DB@time_sjjp_display"]
["RO2浸泡时间设定","C.M.RO2_DB@time_sjjp_sp"]
["RO2加药时间","C.M.RO2_DB@time_sjjy_display"]
["RO2加药时间设定","C.M.RO2_DB@time_sjjy_sp"]
["RO2冲洗等待","C.M.RO2_DB@time_tj_wait"]
["RO2二段正冲","C.M.RO2_DB@time_ZX2_display"]
["RO2二段反冲设定","C.M.RO2_DB@time_ZX2_sp"]
["RO2正常冲洗","C.M.RO2_DB@time_ZX12_display"]
["RO2正常冲洗设定","C.M.RO2_DB@time_ZX12_sp"]
["RO2反渗透段间泵手自动","C.M.RO2_DJB@auto_select"]
["RO2反渗透段间泵故障","C.M.RO2_DJB@fault_total"]
["RO2反渗透段间泵远程","C.M.RO2_DJB@rem"]
["RO2反渗透段间泵复位","C.M.RO2_DJB@reset"]
["RO2反渗透段间泵运行","C.M.RO2_DJB@run"]
["RO2反渗透段间泵运行时间","C.M.RO2_DJB@run_time"]
["RO2反渗透段间泵启动操作","C.M.RO2_DJB@start"]
["RO2反渗透段间泵停止操作","C.M.RO2_DJB@stop"]
["RO2反渗透段间泵电流报警","C.M.RO2_DJB_A@Fault"]
["RO2反渗透段间泵电流高报警","C.M.RO2_DJB_A@H_AL"]
["RO2反渗透段间泵电流高报警开关","C.M.RO2_DJB_A@H_AL_ON"]
["RO2反渗透段间泵电流高限设置","C.M.RO2_DJB_A@H_AL_set"]
["RO2反渗透段间泵电流低报警","C.M.RO2_DJB_A@L_AL"]
["RO2反渗透段间泵电流低报警开关","C.M.RO2_DJB_A@L_AL_ON"]
["RO2反渗透段间泵电流低限设置","C.M.RO2_DJB_A@L_AL_set"]
["RO2反渗透段间泵运行电流","C.M.RO2_DJB_A@out"]
["RO2反渗透段间泵设置频率","C.M.RO2_DJB_AO_FB@spare"]
["RO2反渗透段间泵频率报警","C.M.RO2_DJB_fre@Fault"]
["RO2反渗透段间泵频率高报警","C.M.RO2_DJB_fre@H_AL"]
["RO2反渗透段间泵频率高报警开关","C.M.RO2_DJB_fre@H_AL_ON"]
["RO2反渗透段间泵频率高限设置","C.M.RO2_DJB_fre@H_AL_set"]
["RO2反渗透段间泵频率低报警","C.M.RO2_DJB_fre@L_AL"]
["RO2反渗透段间泵频率低报警开关","C.M.RO2_DJB_fre@L_AL_ON"]
["RO2反渗透段间泵频率低限设置","C.M.RO2_DJB_fre@L_AL_set"]
["RO2反渗透段间泵运行频率","C.M.RO2_DJB_fre@out"]
["RO2反渗透二段产水流量报警","C.M.RO2_FT_CS2@fault"]
["RO2反渗透二段产水流量高报警","C.M.RO2_FT_CS2@H_AL"]
["RO2反渗透二段产水流量高报警开关","C.M.RO2_FT_CS2@H_AL_ON"]
["RO2反渗透二段产水流量高限设置","C.M.RO2_FT_CS2@H_AL_set"]
["RO2反渗透二段产水流量低报警","C.M.RO2_FT_CS2@L_AL"]
["RO2反渗透二段产水流量低报警开关","C.M.RO2_FT_CS2@L_AL_ON"]
["RO2反渗透二段产水流量低限设置","C.M.RO2_FT_CS2@L_AL_set"]
["RO2反渗透二段产水流量","C.M.RO2_FT_CS2@out"]
["RO2反渗透进水流量报警","C.M.RO2_FT_JS@fault"]
["RO2反渗透进水流量高报警","C.M.RO2_FT_JS@H_AL"]
["RO2反渗透进水流量高报警开关","C.M.RO2_FT_JS@H_AL_ON"]
["RO2反渗透进水流量高限设置","C.M.RO2_FT_JS@H_AL_set"]
["RO2反渗透进水流量低报警","C.M.RO2_FT_JS@L_AL"]
["RO2反渗透进水流量低报警开关","C.M.RO2_FT_JS@L_AL_ON"]
["RO2反渗透进水流量低限设置","C.M.RO2_FT_JS@L_AL_set"]
["RO2反渗透进水流量","C.M.RO2_FT_JS@out"]
["RO2反渗透浓水流量报警","C.M.RO2_FT_NS@fault"]
["RO2反渗透浓水流量高报警","C.M.RO2_FT_NS@H_AL"]
["RO2反渗透浓水流量高报警开关","C.M.RO2_FT_NS@H_AL_ON"]
["RO2反渗透浓水流量高限设置","C.M.RO2_FT_NS@H_AL_set"]
["RO2反渗透浓水流量低报警","C.M.RO2_FT_NS@L_AL"]
["RO2反渗透浓水流量低报警开关","C.M.RO2_FT_NS@L_AL_ON"]
["RO2反渗透浓水流量低限设置","C.M.RO2_FT_NS@L_AL_set"]
["RO2反渗透浓水流量","C.M.RO2_FT_NS@out"]
["RO2反渗透高压泵手自动","C.M.RO2_GYB@auto_select"]
["RO2反渗透高压泵故障","C.M.RO2_GYB@fault_total"]
["RO2反渗透高压泵远程","C.M.RO2_GYB@rem"]
["RO2反渗透高压泵复位","C.M.RO2_GYB@reset"]
["RO2反渗透高压泵运行","C.M.RO2_GYB@run"]
["RO2反渗透高压泵运行时间","C.M.RO2_GYB@run_time"]
["RO2反渗透高压泵启动操作","C.M.RO2_GYB@start"]
["RO2反渗透高压泵停止操作","C.M.RO2_GYB@stop"]
["RO2反渗透高压泵电流报警","C.M.RO2_GYB_A@Fault"]
["RO2反渗透高压泵电流高报警","C.M.RO2_GYB_A@H_AL"]
["RO2反渗透高压泵电流高报警开关","C.M.RO2_GYB_A@H_AL_ON"]
["RO2反渗透高压泵电流高限设置","C.M.RO2_GYB_A@H_AL_set"]
["RO2反渗透高压泵电流低报警","C.M.RO2_GYB_A@L_AL"]
["RO2反渗透高压泵电流低报警开关","C.M.RO2_GYB_A@L_AL_ON"]
["RO2反渗透高压泵电流低限设置","C.M.RO2_GYB_A@L_AL_set"]
["RO2反渗透高压泵运行电流","C.M.RO2_GYB_A@out"]
["RO2反渗透高压泵设置频率","C.M.RO2_GYB_AO_FB@spare"]
["RO2反渗透高压泵频率报警","C.M.RO2_GYB_fre@Fault"]
["RO2反渗透高压泵频率高报警","C.M.RO2_GYB_fre@H_AL"]
["RO2反渗透高压泵频率高报警开关","C.M.RO2_GYB_fre@H_AL_ON"]
["RO2反渗透高压泵频率高限设置","C.M.RO2_GYB_fre@H_AL_set"]
["RO2反渗透高压泵频率低报警","C.M.RO2_GYB_fre@L_AL"]
["RO2反渗透高压泵频率低报警开关","C.M.RO2_GYB_fre@L_AL_ON"]
["RO2反渗透高压泵频率低限设置","C.M.RO2_GYB_fre@L_AL_set"]
["RO2反渗透高压泵运行频率","C.M.RO2_GYB_fre@out"]
["RO2进水调节阀开度设定值","C.M.RO2_GYBF_AO_FB@spare"]
["RO2进水调节阀开度报警","C.M.RO2_GYBF_kd@fault"]
["RO2进水调节阀开度高报警","C.M.RO2_GYBF_kd@H_AL"]
["RO2进水调节阀开度高报警开关","C.M.RO2_GYBF_kd@H_AL_ON"]
["RO2进水调节阀开度高限设置","C.M.RO2_GYBF_kd@H_AL_set"]
["RO2进水调节阀开度低报警","C.M.RO2_GYBF_kd@L_AL"]
["RO2进水调节阀开度低报警开关","C.M.RO2_GYBF_kd@L_AL_ON"]
["RO2进水调节阀开度低限设置","C.M.RO2_GYBF_kd@L_AL_set"]
["RO2进水调节阀开度","C.M.RO2_GYBF_kd@out"]
["RO2反渗透段间泵高压开关","C.M.RO2_LS_DJB_H"]
["RO2反渗透段间泵低压开关","C.M.RO2_LS_DJB_L"]
["RO2反渗透高压泵高压开关","C.M.RO2_LS_GYB_H"]
["RO2反渗透高压泵低压开关","C.M.RO2_LS_GYB_L"]
["RO2排气阀1手自动","C.M.RO2_PQF1@auto_select"]
["RO2排气阀1关操作","C.M.RO2_PQF1@close"]
["RO2排气阀1关到位","C.M.RO2_PQF1@close_feedback"]
["RO2排气阀1故障","C.M.RO2_PQF1@fault_total"]
["RO2排气阀1开操作","C.M.RO2_PQF1@open"]
["RO2排气阀1开到位","C.M.RO2_PQF1@open_feedback"]
["RO2排气阀1远程","C.M.RO2_PQF1@rem"]
["RO2排气阀1复位","C.M.RO2_PQF1@reset"]
["RO2排气阀2手自动","C.M.RO2_PQF2@auto_select"]
["RO2排气阀2关操作","C.M.RO2_PQF2@close"]
["RO2排气阀2关到位","C.M.RO2_PQF2@close_feedback"]
["RO2排气阀2故障","C.M.RO2_PQF2@fault_total"]
["RO2排气阀2开操作","C.M.RO2_PQF2@open"]
["RO2排气阀2开到位","C.M.RO2_PQF2@open_feedback"]
["RO2排气阀2远程","C.M.RO2_PQF2@rem"]
["RO2排气阀2复位","C.M.RO2_PQF2@reset"]
["RO2排气阀3手自动","C.M.RO2_PQF3@auto_select"]
["RO2排气阀3关操作","C.M.RO2_PQF3@close"]
["RO2排气阀3关到位","C.M.RO2_PQF3@close_feedback"]
["RO2排气阀3故障","C.M.RO2_PQF3@fault_total"]
["RO2排气阀3开操作","C.M.RO2_PQF3@open"]
["RO2排气阀3开到位","C.M.RO2_PQF3@open_feedback"]
["RO2排气阀3远程","C.M.RO2_PQF3@rem"]
["RO2排气阀3复位","C.M.RO2_PQF3@reset"]
["RO2排气阀4手自动","C.M.RO2_PQF4@auto_select"]
["RO2排气阀4关操作","C.M.RO2_PQF4@close"]
["RO2排气阀4关到位","C.M.RO2_PQF4@close_feedback"]
["RO2排气阀4故障","C.M.RO2_PQF4@fault_total"]
["RO2排气阀4开操作","C.M.RO2_PQF4@open"]
["RO2排气阀4开到位","C.M.RO2_PQF4@open_feedback"]
["RO2排气阀4远程","C.M.RO2_PQF4@rem"]
["RO2排气阀4复位","C.M.RO2_PQF4@reset"]
["RO2排气阀5手自动","C.M.RO2_PQF5@auto_select"]
["RO2排气阀5关操作","C.M.RO2_PQF5@close"]
["RO2排气阀5关到位","C.M.RO2_PQF5@close_feedback"]
["RO2排气阀5故障","C.M.RO2_PQF5@fault_total"]
["RO2排气阀5开操作","C.M.RO2_PQF5@open"]
["RO2排气阀5开到位","C.M.RO2_PQF5@open_feedback"]
["RO2排气阀5远程","C.M.RO2_PQF5@rem"]
["RO2排气阀5复位","C.M.RO2_PQF5@reset"]
["RO2排气阀6手自动","C.M.RO2_PQF6@auto_select"]
["RO2排气阀6关操作","C.M.RO2_PQF6@close"]
["RO2排气阀6关到位","C.M.RO2_PQF6@close_feedback"]
["RO2排气阀6故障","C.M.RO2_PQF6@fault_total"]
["RO2排气阀6开操作","C.M.RO2_PQF6@open"]
["RO2排气阀6开到位","C.M.RO2_PQF6@open_feedback"]
["RO2排气阀6远程","C.M.RO2_PQF6@rem"]
["RO2排气阀6复位","C.M.RO2_PQF6@reset"]
["RO2排气阀7手自动","C.M.RO2_PQF7@auto_select"]
["RO2排气阀7关操作","C.M.RO2_PQF7@close"]
["RO2排气阀7关到位","C.M.RO2_PQF7@close_feedback"]
["RO2排气阀7故障","C.M.RO2_PQF7@fault_total"]
["RO2排气阀7开操作","C.M.RO2_PQF7@open"]
["RO2排气阀7开到位","C.M.RO2_PQF7@open_feedback"]
["RO2排气阀7远程","C.M.RO2_PQF7@rem"]
["RO2排气阀7复位","C.M.RO2_PQF7@reset"]
["RO2产水压力报警","C.M.RO2_PT_CS@fault"]
["RO2产水压力高报警","C.M.RO2_PT_CS@H_AL"]
["RO2产水压力高报警开关","C.M.RO2_PT_CS@H_AL_ON"]
["RO2产水压力高限设置","C.M.RO2_PT_CS@H_AL_set"]
["RO2产水压力低报警","C.M.RO2_PT_CS@L_AL"]
["RO2产水压力低报警开关","C.M.RO2_PT_CS@L_AL_ON"]
["RO2产水压力低限设置","C.M.RO2_PT_CS@L_AL_set"]
["RO2产水压力","C.M.RO2_PT_CS@out"]
["RO2一段浓水压力报警","C.M.RO2_PT_DJ1@fault"]
["RO2一段浓水压力高报警","C.M.RO2_PT_DJ1@H_AL"]
["RO2一段浓水压力高报警开关","C.M.RO2_PT_DJ1@H_AL_ON"]
["RO2一段浓水压力高限设置","C.M.RO2_PT_DJ1@H_AL_set"]
["RO2一段浓水压力低报警","C.M.RO2_PT_DJ1@L_AL"]
["RO2一段浓水压力低报警开关","C.M.RO2_PT_DJ1@L_AL_ON"]
["RO2一段浓水压力低限设置","C.M.RO2_PT_DJ1@L_AL_set"]
["RO2一段浓水压力","C.M.RO2_PT_DJ1@out"]
["RO2二段进水压力报警","C.M.RO2_PT_DJ2@fault"]
["RO2二段进水压力高报警","C.M.RO2_PT_DJ2@H_AL"]
["RO2二段进水压力高报警开关","C.M.RO2_PT_DJ2@H_AL_ON"]
["RO2二段进水压力高限设置","C.M.RO2_PT_DJ2@H_AL_set"]
["RO2二段进水压力低报警","C.M.RO2_PT_DJ2@L_AL"]
["RO2二段进水压力低报警开关","C.M.RO2_PT_DJ2@L_AL_ON"]
["RO2二段进水压力低限设置","C.M.RO2_PT_DJ2@L_AL_set"]
["RO2二段进水压力","C.M.RO2_PT_DJ2@out"]
["RO2一段进水压力报警","C.M.RO2_PT_JS@fault"]
["RO2一段进水压力高报警","C.M.RO2_PT_JS@H_AL"]
["RO2一段进水压力高报警开关","C.M.RO2_PT_JS@H_AL_ON"]
["RO2一段进水压力高限设置","C.M.RO2_PT_JS@H_AL_set"]
["RO2一段进水压力低报警","C.M.RO2_PT_JS@L_AL"]
["RO2一段进水压力低报警开关","C.M.RO2_PT_JS@L_AL_ON"]
["RO2一段进水压力低限设置","C.M.RO2_PT_JS@L_AL_set"]
["RO2一段进水压力","C.M.RO2_PT_JS@out"]
["RO2二段浓水压力报警","C.M.RO2_PT_NS@fault"]
["RO2二段浓水压力高报警","C.M.RO2_PT_NS@H_AL"]
["RO2二段浓水压力高报警开关","C.M.RO2_PT_NS@H_AL_ON"]
["RO2二段浓水压力高限设置","C.M.RO2_PT_NS@H_AL_set"]
["RO2二段浓水压力低报警","C.M.RO2_PT_NS@L_AL"]
["RO2二段浓水压力低报警开关","C.M.RO2_PT_NS@L_AL_ON"]
["RO2二段浓水压力低限设置","C.M.RO2_PT_NS@L_AL_set"]
["RO2二段浓水压力","C.M.RO2_PT_NS@out"]
["RO2未知阀手自动","C.M.RO2_SJJF@auto_select"]
["RO2未知阀关操作","C.M.RO2_SJJF@close"]
["RO2未知阀关到位","C.M.RO2_SJJF@close_feedback"]
["RO2未知阀故障","C.M.RO2_SJJF@fault_total"]
["RO2未知阀开操作","C.M.RO2_SJJF@open"]
["RO2未知阀开到位","C.M.RO2_SJJF@open_feedback"]
["RO2未知阀远程","C.M.RO2_SJJF@rem"]
["RO2未知阀复位","C.M.RO2_SJJF@reset"]
["2#阻垢剂加药阀手自动","C.M.RO2_ZGJF@auto_select"]
["2#阻垢剂加药阀关操作","C.M.RO2_ZGJF@close"]
["2#阻垢剂加药阀关到位","C.M.RO2_ZGJF@close_feedback"]
["2#阻垢剂加药阀故障","C.M.RO2_ZGJF@fault_total"]
["2#阻垢剂加药阀开操作","C.M.RO2_ZGJF@open"]
["2#阻垢剂加药阀开到位","C.M.RO2_ZGJF@open_feedback"]
["2#阻垢剂加药阀远程","C.M.RO2_ZGJF@rem"]
["2#阻垢剂加药阀复位","C.M.RO2_ZGJF@reset"]
["RO3不合格水阀手自动","C.M.RO3_BHGF@auto_select"]
["RO3不合格水阀关操作","C.M.RO3_BHGF@close"]
["RO3不合格水阀关到位","C.M.RO3_BHGF@close_feedback"]
["RO3不合格水阀故障","C.M.RO3_BHGF@fault_total"]
["RO3不合格水阀开操作","C.M.RO3_BHGF@open"]
["RO3不合格水阀开到位","C.M.RO3_BHGF@open_feedback"]
["RO3不合格水阀远程","C.M.RO3_BHGF@rem"]
["RO3不合格水阀复位","C.M.RO3_BHGF@reset"]
["RO3产水CIP回水阀手自动","C.M.RO3_CIP_CSHSF@auto_select"]
["RO3产水CIP回水阀关操作","C.M.RO3_CIP_CSHSF@close"]
["RO3产水CIP回水阀关到位","C.M.RO3_CIP_CSHSF@close_feedback"]
["RO3产水CIP回水阀故障","C.M.RO3_CIP_CSHSF@fault_total"]
["RO3产水CIP回水阀开操作","C.M.RO3_CIP_CSHSF@open"]
["RO3产水CIP回水阀开到位","C.M.RO3_CIP_CSHSF@open_feedback"]
["RO3产水CIP回水阀远程","C.M.RO3_CIP_CSHSF@rem"]
["RO3产水CIP回水阀复位","C.M.RO3_CIP_CSHSF@reset"]
["RO3一段CIP回水阀手自动","C.M.RO3_CIP_HSF1@auto_select"]
["RO3一段CIP回水阀关操作","C.M.RO3_CIP_HSF1@close"]
["RO3一段CIP回水阀关到位","C.M.RO3_CIP_HSF1@close_feedback"]
["RO3一段CIP回水阀故障","C.M.RO3_CIP_HSF1@fault_total"]
["RO3一段CIP回水阀开操作","C.M.RO3_CIP_HSF1@open"]
["RO3一段CIP回水阀开到位","C.M.RO3_CIP_HSF1@open_feedback"]
["RO3一段CIP回水阀远程","C.M.RO3_CIP_HSF1@rem"]
["RO3一段CIP回水阀复位","C.M.RO3_CIP_HSF1@reset"]
["RO3二段CIP回水阀手自动","C.M.RO3_CIP_HSF2@auto_select"]
["RO3二段CIP回水阀关操作","C.M.RO3_CIP_HSF2@close"]
["RO3二段CIP回水阀关到位","C.M.RO3_CIP_HSF2@close_feedback"]
["RO3二段CIP回水阀故障","C.M.RO3_CIP_HSF2@fault_total"]
["RO3二段CIP回水阀开操作","C.M.RO3_CIP_HSF2@open"]
["RO3二段CIP回水阀开到位","C.M.RO3_CIP_HSF2@open_feedback"]
["RO3二段CIP回水阀远程","C.M.RO3_CIP_HSF2@rem"]
["RO3二段CIP回水阀复位","C.M.RO3_CIP_HSF2@reset"]
["RO3一段CIP进水阀手自动","C.M.RO3_CIP_JSF1@auto_select"]
["RO3一段CIP进水阀关操作","C.M.RO3_CIP_JSF1@close"]
["RO3一段CIP进水阀关到位","C.M.RO3_CIP_JSF1@close_feedback"]
["RO3一段CIP进水阀故障","C.M.RO3_CIP_JSF1@fault_total"]
["RO3一段CIP进水阀开操作","C.M.RO3_CIP_JSF1@open"]
["RO3一段CIP进水阀开到位","C.M.RO3_CIP_JSF1@open_feedback"]
["RO3一段CIP进水阀远程","C.M.RO3_CIP_JSF1@rem"]
["RO3一段CIP进水阀复位","C.M.RO3_CIP_JSF1@reset"]
["RO3二段CIP进水阀手自动","C.M.RO3_CIP_JSF2@auto_select"]
["RO3二段CIP进水阀关操作","C.M.RO3_CIP_JSF2@close"]
["RO3二段CIP进水阀关到位","C.M.RO3_CIP_JSF2@close_feedback"]
["RO3二段CIP进水阀故障","C.M.RO3_CIP_JSF2@fault_total"]
["RO3二段CIP进水阀开操作","C.M.RO3_CIP_JSF2@open"]
["RO3二段CIP进水阀开到位","C.M.RO3_CIP_JSF2@open_feedback"]
["RO3二段CIP进水阀远程","C.M.RO3_CIP_JSF2@rem"]
["RO3二段CIP进水阀复位","C.M.RO3_CIP_JSF2@reset"]
["产水排空阀手自动","C.M.RO3_CIP_PKF1@auto_select"]
["产水排空阀关操作","C.M.RO3_CIP_PKF1@close"]
["产水排空阀关到位","C.M.RO3_CIP_PKF1@close_feedback"]
["产水排空阀故障","C.M.RO3_CIP_PKF1@fault_total"]
["产水排空阀开操作","C.M.RO3_CIP_PKF1@open"]
["产水排空阀开到位","C.M.RO3_CIP_PKF1@open_feedback"]
["产水排空阀远程","C.M.RO3_CIP_PKF1@rem"]
["产水排空阀复位","C.M.RO3_CIP_PKF1@reset"]
["RO3产水电导报警","C.M.RO3_Cond_CS@fault"]
["RO3产水电导高报警","C.M.RO3_Cond_CS@H_AL"]
["RO3产水电导高报警开关","C.M.RO3_Cond_CS@H_AL_ON"]
["RO3产水电导高限设置","C.M.RO3_Cond_CS@H_AL_set"]
["RO3产水电导低报警","C.M.RO3_Cond_CS@L_AL"]
["RO3产水电导低报警开关","C.M.RO3_Cond_CS@L_AL_ON"]
["RO3产水电导低限设置","C.M.RO3_Cond_CS@L_AL_set"]
["RO3产水电导","C.M.RO3_Cond_CS@out"]
["RO3产水阀手自动","C.M.RO3_CSF@auto_select"]
["RO3产水阀关操作","C.M.RO3_CSF@close"]
["RO3产水阀关到位","C.M.RO3_CSF@close_feedback"]
["RO3产水阀故障","C.M.RO3_CSF@fault_total"]
["RO3产水阀开操作","C.M.RO3_CSF@open"]
["RO3产水阀开到位","C.M.RO3_CSF@open_feedback"]
["RO3产水阀远程","C.M.RO3_CSF@rem"]
["RO3产水阀复位","C.M.RO3_CSF@reset"]
["RO3一段冲洗进水阀手自动","C.M.RO3_CXJF1@auto_select"]
["RO3一段冲洗进水阀关操作","C.M.RO3_CXJF1@close"]
["RO3一段冲洗进水阀关到位","C.M.RO3_CXJF1@close_feedback"]
["RO3一段冲洗进水阀故障","C.M.RO3_CXJF1@fault_total"]
["RO3一段冲洗进水阀开操作","C.M.RO3_CXJF1@open"]
["RO3一段冲洗进水阀开到位","C.M.RO3_CXJF1@open_feedback"]
["RO3一段冲洗进水阀远程","C.M.RO3_CXJF1@rem"]
["RO3一段冲洗进水阀复位","C.M.RO3_CXJF1@reset"]
["RO3二段冲洗进水阀手自动","C.M.RO3_CXJF2@auto_select"]
["RO3二段冲洗进水阀关操作","C.M.RO3_CXJF2@close"]
["RO3二段冲洗进水阀关到位","C.M.RO3_CXJF2@close_feedback"]
["RO3二段冲洗进水阀故障","C.M.RO3_CXJF2@fault_total"]
["RO3二段冲洗进水阀开操作","C.M.RO3_CXJF2@open"]
["RO3二段冲洗进水阀开到位","C.M.RO3_CXJF2@open_feedback"]
["RO3二段冲洗进水阀远程","C.M.RO3_CXJF2@rem"]
["RO3二段冲洗进水阀复位","C.M.RO3_CXJF2@reset"]
["RO3一段冲洗排水阀手自动","C.M.RO3_CXPF1@auto_select"]
["RO3一段冲洗排水阀关操作","C.M.RO3_CXPF1@close"]
["RO3一段冲洗排水阀关到位","C.M.RO3_CXPF1@close_feedback"]
["RO3一段冲洗排水阀故障","C.M.RO3_CXPF1@fault_total"]
["RO3一段冲洗排水阀开操作","C.M.RO3_CXPF1@open"]
["RO3一段冲洗排水阀开到位","C.M.RO3_CXPF1@open_feedback"]
["RO3一段冲洗排水阀远程","C.M.RO3_CXPF1@rem"]
["RO3一段冲洗排水阀复位","C.M.RO3_CXPF1@reset"]
["RO3二段冲洗排水阀手自动","C.M.RO3_CXPF2@auto_select"]
["RO3二段冲洗排水阀关操作","C.M.RO3_CXPF2@close"]
["RO3二段冲洗排水阀关到位","C.M.RO3_CXPF2@close_feedback"]
["RO3二段冲洗排水阀故障","C.M.RO3_CXPF2@fault_total"]
["RO3二段冲洗排水阀开操作","C.M.RO3_CXPF2@open"]
["RO3二段冲洗排水阀开到位","C.M.RO3_CXPF2@open_feedback"]
["RO3二段冲洗排水阀远程","C.M.RO3_CXPF2@rem"]
["RO3二段冲洗排水阀复位","C.M.RO3_CXPF2@reset"]
["RO3紧急停车","C.M.RO3_DB@button[00]"]
["RO3自动开机","C.M.RO3_DB@button[01]"]
["RO3自动停止","C.M.RO3_DB@button[02]"]
["RO3自动正常冲洗","C.M.RO3_DB@button[03]"]
["RO3自动反向冲洗","C.M.RO3_DB@button[04]"]
["RO3自动杀菌冲洗","C.M.RO3_DB@button[05]"]
["RO3未知1（不确定）","C.M.RO3_DB@button[06]"]
["RO3未知2（不确定）","C.M.RO3_DB@button[07]"]
["RO3全自动开机","C.M.RO3_DB@button[08]"]
["RO3CIP启停","C.M.RO3_DB@button[09]"]
["RO3信息清除","C.M.RO3_DB@button[10]"]
["RO3自动杀菌投入/切除","C.M.RO3_DB@button[11]"]
["RO3高压泵PID/定频控制","C.M.RO3_DB@button[12]"]
["RO3段间泵PID/定频控制","C.M.RO3_DB@button[13]"]
["RO3一段CIP（保持）","C.M.RO3_DB@button[14]"]
["RO3二段CIP（保持）","C.M.RO3_DB@button[15]"]
["RO3一段酸洗（选中保持）","C.M.RO3_DB@button[16]"]
["RO3二段酸洗（选中保持）","C.M.RO3_DB@button[17]"]
["RO3一段碱洗（选中保持）","C.M.RO3_DB@button[18]"]
["RO3二段碱洗（选中保持）","C.M.RO3_DB@button[19]"]
["RO3一段非氧洗（选中保持）","C.M.RO3_DB@button[20]"]
["RO3二段非氧洗（选中保持）","C.M.RO3_DB@button[21]"]
["RO3一段酸洗（手动保持）","C.M.RO3_DB@button[22]"]
["RO3二段酸洗（手动保持）","C.M.RO3_DB@button[23]"]
["RO3一段碱洗（手动保持）","C.M.RO3_DB@button[24]"]
["RO3二段碱洗（手动保持）","C.M.RO3_DB@button[25]"]
["RO3一段非氧洗（手动保持）","C.M.RO3_DB@button[26]"]
["RO3二段非氧洗（手动保持）","C.M.RO3_DB@button[27]"]
["RO3HOLDHB1","C.M.RO3_DB@button[28]"]
["RO3HOLDHB2","C.M.RO3_DB@button[29]"]
["RO3HOLDHB3","C.M.RO3_DB@button[30]"]
["RO3HOLDHB4","C.M.RO3_DB@button[31]"]
["RO3 ZBOOL HOLD1","C.M.RO3_DB@Zbool[0]"]
["RO3 ZBOOL HOLD2","C.M.RO3_DB@Zbool[1]"]
["RO3 ZBOOL HOLD3","C.M.RO3_DB@Zbool[2]"]
["RO3 ZDint HOLD1","C.M.RO3_DB@ZDint[0]"]
["RO3 ZDint HOLD2","C.M.RO3_DB@ZDint[1]"]
["RO3 ZDint HOLD3","C.M.RO3_DB@ZDint[2]"]
["RO3一段需要酸洗标志","C.M.RO3_DB@ZFlag[0]"]
["RO3二段需要酸洗标志","C.M.RO3_DB@ZFlag[1]"]
["RO3一段需要J洗标志","C.M.RO3_DB@ZFlag[2]"]
["RO3二段需要J洗标志","C.M.RO3_DB@ZFlag[3]"]
["RO3一段需要FY洗标志","C.M.RO3_DB@ZFlag[4]"]
["RO3二段需要FY洗标志","C.M.RO3_DB@ZFlag[5]"]
["RO3跳转一段酸洗","C.M.RO3_DB@ZFlag[6]"]
["RO3跳转二段酸洗","C.M.RO3_DB@ZFlag[7]"]
["RO3跳转一段J洗","C.M.RO3_DB@ZFlag[8]"]
["RO3跳转二段J洗","C.M.RO3_DB@ZFlag[9]"]
["RO3跳转一段非氧洗","C.M.RO3_DB@ZFlag[10]"]
["RO3跳转二段非氧洗","C.M.RO3_DB@ZFlag[11]"]
["RO3HOLD ZFLAG1","C.M.RO3_DB@ZFlag[12]"]
["RO3HOLD ZFLAG2","C.M.RO3_DB@ZFlag[13]"]
["RO3HOLD ZFLAG3","C.M.RO3_DB@ZFlag[14]"]
["RO3HOLD ZFLAG4","C.M.RO3_DB@ZFlag[15]"]
["RO3 当前步序时间","C.M.RO3_DB@ZZZreal[0]"]
["RO3 当前步序设定时间","C.M.RO3_DB@ZZZreal[1]"]
["RO3 1段酸洗记次数","C.M.RO3_DB@ZZZreal[2]"]
["RO3 2段酸洗记次数","C.M.RO3_DB@ZZZreal[3]"]
["RO3 1段J洗记次数","C.M.RO3_DB@ZZZreal[4]"]
["RO3 2段J洗记次数","C.M.RO3_DB@ZZZreal[5]"]
["RO3 1段FY洗记次数","C.M.RO3_DB@ZZZreal[6]"]
["RO3 2段FY洗记次数","C.M.RO3_DB@ZZZreal[7]"]
["RO3 1段酸洗设定次数","C.M.RO3_DB@ZZZreal[8]"]
["RO3 2段酸洗设定次数","C.M.RO3_DB@ZZZreal[9]"]
["RO3 1段J洗设定次数","C.M.RO3_DB@ZZZreal[10]"]
["RO3 2段J洗设定次数","C.M.RO3_DB@ZZZreal[11]"]
["RO3 1段FY洗设定次数","C.M.RO3_DB@ZZZreal[12]"]
["RO3 2段FY洗设定次数","C.M.RO3_DB@ZZZreal[13]"]
["RO3HOLD1","C.M.RO3_DB@ZZZreal[14]"]
["RO3HOLD2","C.M.RO3_DB@ZZZreal[15]"]
["RO3 一段加药前冲时间设定","C.M.RO3_DB@ZZZreal[16]"]
["RO3 一段加药浸泡时间设定","C.M.RO3_DB@ZZZreal[17]"]
["RO3 一段加药后冲时间设定","C.M.RO3_DB@ZZZreal[18]"]
["RO3 二段加药前冲时间设定","C.M.RO3_DB@ZZZreal[19]"]
["RO3 二段加药浸泡时间设定","C.M.RO3_DB@ZZZreal[20]"]
["RO3 二段加药后冲时间设定","C.M.RO3_DB@ZZZreal[21]"]
["RO3HOLD3","C.M.RO3_DB@ZZZreal[22]"]
["RO3HOLD4","C.M.RO3_DB@ZZZreal[23]"]
["RO3HOLD5","C.M.RO3_DB@ZZZreal[24]"]
["RO3HOLD6","C.M.RO3_DB@ZZZreal[25]"]
["RO3 一段CIP循环","C.M.RO3_DB@ZZZreal[26]"]
["RO3 一段CIP浸泡","C.M.RO3_DB@ZZZreal[27]"]
["RO3 二段CIP循环","C.M.RO3_DB@ZZZreal[28]"]
["RO3 二段CIP浸泡","C.M.RO3_DB@ZZZreal[29]"]
["RO3 产水杀菌时间设定","C.M.RO3_DB@ZZZreal[30]"]
["RO3 产水杀菌等待时间设定","C.M.RO3_DB@ZZZreal[31]"]
["RO3 产水杀菌时间READ","C.M.RO3_DB@ZZZreal[32]"]
["RO3 产水杀菌等待时间READ","C.M.RO3_DB@ZZZreal[33]"]
["RO3HOLD7","C.M.RO3_DB@ZZZreal[34]"]
["RO3HOLD8","C.M.RO3_DB@ZZZreal[35]"]
["RO3HOLD9","C.M.RO3_DB@ZZZreal[36]"]
["RO3HOLD10","C.M.RO3_DB@ZZZreal[37]"]
["RO3HOLD11","C.M.RO3_DB@ZZZreal[38]"]
["RO3HOLD12","C.M.RO3_DB@ZZZreal[39]"]
["RO3——碱冲洗设备ready","C.M.RO3_DB@ready[08]"]
["RO3——杀菌冲洗设备ready","C.M.RO3_DB@ready[09]"]
["RO3——备用1","C.M.RO3_DB@ready[10]"]
["RO3——备用2","C.M.RO3_DB@ready[11]"]
["RO3控制字","C.M.RO3_DB@control_word"]
["RO3反渗透段间泵频率设定","C.M.RO3_DB@DJB_fre_sp"]
["RO3一段压差","C.M.RO3_DB@DPT_1"]
["RO3一段差压高设定","C.M.RO3_DB@DPT_1_stop_sp"]
["RO3二段压差","C.M.RO3_DB@DPT_2"]
["RO3二段差压高设定","C.M.RO3_DB@DPT_2_stop_sp"]
["RO3电导正常可产水设定","C.M.RO3_DB@EC_ZCS_sp"]
["RO3产水电导高设定","C.M.RO3_DB@EC_ZCS_stop_sp"]
["RO3故障字","C.M.RO3_DB@fault_word"]
["RO3二段产水流量设定","C.M.RO3_DB@FT_CS2_sp"]
["RO3进水流量设定","C.M.RO3_DB@FT_JS_sp"]
["RO3反渗透高压泵频率设定","C.M.RO3_DB@GYB_fre_sp"]
["RO3控制模式","C.M.RO3_DB@model_word"]
["RO3未知3（不确定）","C.M.RO3_DB@PS[00]"]
["RO3未知4（不确定）","C.M.RO3_DB@PS[01]"]
["RO3未知5（不确定）","C.M.RO3_DB@PS[02]"]
["RO3未知6（不确定）","C.M.RO3_DB@PS[03]"]
["RO3产水压力高设定","C.M.RO3_DB@PT_CS_stop_sp"]
["RO3段间泵出水压力高设定","C.M.RO3_DB@PT_DJB_CS_stop_sp"]
["RO3段间泵进水压力低设定","C.M.RO3_DB@PT_DJB_JS_stop_sp"]
["RO3高压泵出水压力高设定","C.M.RO3_DB@PT_JS_stop_sp"]
["RO3未知7（不确定）","C.M.RO3_DB@ready[00]"]
["RO3未知8（不确定）","C.M.RO3_DB@ready[01]"]
["RO3未知9（不确定）","C.M.RO3_DB@ready[02]"]
["RO3产水准备好","C.M.RO3_DB@ready[03]"]
["RO3冲洗准备好","C.M.RO3_DB@ready[04]"]
["RO3杀菌准备好","C.M.RO3_DB@ready[05]"]
["RO3CIP准备好","C.M.RO3_DB@ready[06]"]
["RO3未知10（不确定）","C.M.RO3_DB@ready[07]"]
["RO3提醒字","C.M.RO3_DB@reminder_word"]
["RO3运行时间","C.M.RO3_DB@run_time"]
["RO3停止时间","C.M.RO3_DB@stop_time"]
["RO3不合格排水","C.M.RO3_DB@time_bhgs_display"]
["RO3不合格排水设定","C.M.RO3_DB@time_bhgs_sp"]
["RO3产水可延迟时间设定","C.M.RO3_DB@time_CS_delay_sp"]
["RO3产水时间","C.M.RO3_DB@time_CS_display"]
["RO3产水时间设定","C.M.RO3_DB@time_CS_sp"]
["RO3一段反冲","C.M.RO3_DB@time_FX1_display"]
["RO3一段反冲设定","C.M.RO3_DB@time_FX1_sp"]
["RO3开机等待","C.M.RO3_DB@time_kj_wait"]
["RO3排气时间","C.M.RO3_DB@time_kjcx_display1"]
["RO3开机冲洗","C.M.RO3_DB@time_kjcx_display2"]
["RO3排气时间设定","C.M.RO3_DB@time_kjcx_sp1"]
["RO3开机冲洗设定","C.M.RO3_DB@time_kjcx_sp2"]
["RO3杀菌间隔","C.M.RO3_DB@time_shajun_display"]
["RO3杀菌间隔设定","C.M.RO3_DB@time_shajun_sp"]
["RO3杀菌等待","C.M.RO3_DB@time_sj_wait"]
["RO3一段反冲","C.M.RO3_DB@time_sjcx1_display"]
["RO3一段反冲设定","C.M.RO3_DB@time_sjcx1_sp"]
["RO3二段反冲","C.M.RO3_DB@time_sjcx2_display"]
["RO3二段反冲设定","C.M.RO3_DB@time_sjcx2_sp"]
["RO3浸泡时间","C.M.RO3_DB@time_sjjp_display"]
["RO3浸泡时间设定","C.M.RO3_DB@time_sjjp_sp"]
["RO3加药时间","C.M.RO3_DB@time_sjjy_display"]
["RO3加药时间设定","C.M.RO3_DB@time_sjjy_sp"]
["RO3冲洗等待","C.M.RO3_DB@time_tj_wait"]
["RO3二段正冲","C.M.RO3_DB@time_ZX2_display"]
["RO3二段反冲设定","C.M.RO3_DB@time_ZX2_sp"]
["RO3正常冲洗","C.M.RO3_DB@time_ZX12_display"]
["RO3正常冲洗设定","C.M.RO3_DB@time_ZX12_sp"]
["RO3反渗透段间泵手自动","C.M.RO3_DJB@auto_select"]
["RO3反渗透段间泵故障","C.M.RO3_DJB@fault_total"]
["RO3反渗透段间泵远程","C.M.RO3_DJB@rem"]
["RO3反渗透段间泵复位","C.M.RO3_DJB@reset"]
["RO3反渗透段间泵运行","C.M.RO3_DJB@run"]
["RO3反渗透段间泵运行时间","C.M.RO3_DJB@run_time"]
["RO3反渗透段间泵启动操作","C.M.RO3_DJB@start"]
["RO3反渗透段间泵停止操作","C.M.RO3_DJB@stop"]
["RO3反渗透段间泵电流报警","C.M.RO3_DJB_A@Fault"]
["RO3反渗透段间泵电流高报警","C.M.RO3_DJB_A@H_AL"]
["RO3反渗透段间泵电流高报警开关","C.M.RO3_DJB_A@H_AL_ON"]
["RO3反渗透段间泵电流高限设置","C.M.RO3_DJB_A@H_AL_set"]
["RO3反渗透段间泵电流低报警","C.M.RO3_DJB_A@L_AL"]
["RO3反渗透段间泵电流低报警开关","C.M.RO3_DJB_A@L_AL_ON"]
["RO3反渗透段间泵电流低限设置","C.M.RO3_DJB_A@L_AL_set"]
["RO3反渗透段间泵运行电流","C.M.RO3_DJB_A@out"]
["RO3反渗透段间泵设置频率","C.M.RO3_DJB_AO_FB@spare"]
["RO3反渗透段间泵频率报警","C.M.RO3_DJB_fre@Fault"]
["RO3反渗透段间泵频率高报警","C.M.RO3_DJB_fre@H_AL"]
["RO3反渗透段间泵频率高报警开关","C.M.RO3_DJB_fre@H_AL_ON"]
["RO3反渗透段间泵频率高限设置","C.M.RO3_DJB_fre@H_AL_set"]
["RO3反渗透段间泵频率低报警","C.M.RO3_DJB_fre@L_AL"]
["RO3反渗透段间泵频率低报警开关","C.M.RO3_DJB_fre@L_AL_ON"]
["RO3反渗透段间泵频率低限设置","C.M.RO3_DJB_fre@L_AL_set"]
["RO3反渗透段间泵运行频率","C.M.RO3_DJB_fre@out"]
["RO3反渗透二段产水流量报警","C.M.RO3_FT_CS2@fault"]
["RO3反渗透二段产水流量高报警","C.M.RO3_FT_CS2@H_AL"]
["RO3反渗透二段产水流量高报警开关","C.M.RO3_FT_CS2@H_AL_ON"]
["RO3反渗透二段产水流量高限设置","C.M.RO3_FT_CS2@H_AL_set"]
["RO3反渗透二段产水流量低报警","C.M.RO3_FT_CS2@L_AL"]
["RO3反渗透二段产水流量低报警开关","C.M.RO3_FT_CS2@L_AL_ON"]
["RO3反渗透二段产水流量低限设置","C.M.RO3_FT_CS2@L_AL_set"]
["RO3反渗透二段产水流量","C.M.RO3_FT_CS2@out"]
["RO3反渗透进水流量报警","C.M.RO3_FT_JS@fault"]
["RO3反渗透进水流量高报警","C.M.RO3_FT_JS@H_AL"]
["RO3反渗透进水流量高报警开关","C.M.RO3_FT_JS@H_AL_ON"]
["RO3反渗透进水流量高限设置","C.M.RO3_FT_JS@H_AL_set"]
["RO3反渗透进水流量低报警","C.M.RO3_FT_JS@L_AL"]
["RO3反渗透进水流量低报警开关","C.M.RO3_FT_JS@L_AL_ON"]
["RO3反渗透进水流量低限设置","C.M.RO3_FT_JS@L_AL_set"]
["RO3反渗透进水流量","C.M.RO3_FT_JS@out"]
["RO3反渗透浓水流量报警","C.M.RO3_FT_NS@fault"]
["RO3反渗透浓水流量高报警","C.M.RO3_FT_NS@H_AL"]
["RO3反渗透浓水流量高报警开关","C.M.RO3_FT_NS@H_AL_ON"]
["RO3反渗透浓水流量高限设置","C.M.RO3_FT_NS@H_AL_set"]
["RO3反渗透浓水流量低报警","C.M.RO3_FT_NS@L_AL"]
["RO3反渗透浓水流量低报警开关","C.M.RO3_FT_NS@L_AL_ON"]
["RO3反渗透浓水流量低限设置","C.M.RO3_FT_NS@L_AL_set"]
["RO3反渗透浓水流量","C.M.RO3_FT_NS@out"]
["RO3反渗透高压泵手自动","C.M.RO3_GYB@auto_select"]
["RO3反渗透高压泵故障","C.M.RO3_GYB@fault_total"]
["RO3反渗透高压泵远程","C.M.RO3_GYB@rem"]
["RO3反渗透高压泵复位","C.M.RO3_GYB@reset"]
["RO3反渗透高压泵运行","C.M.RO3_GYB@run"]
["RO3反渗透高压泵运行时间","C.M.RO3_GYB@run_time"]
["RO3反渗透高压泵启动操作","C.M.RO3_GYB@start"]
["RO3反渗透高压泵停止操作","C.M.RO3_GYB@stop"]
["RO3反渗透高压泵电流报警","C.M.RO3_GYB_A@Fault"]
["RO3反渗透高压泵电流高报警","C.M.RO3_GYB_A@H_AL"]
["RO3反渗透高压泵电流高报警开关","C.M.RO3_GYB_A@H_AL_ON"]
["RO3反渗透高压泵电流高限设置","C.M.RO3_GYB_A@H_AL_set"]
["RO3反渗透高压泵电流低报警","C.M.RO3_GYB_A@L_AL"]
["RO3反渗透高压泵电流低报警开关","C.M.RO3_GYB_A@L_AL_ON"]
["RO3反渗透高压泵电流低限设置","C.M.RO3_GYB_A@L_AL_set"]
["RO3反渗透高压泵运行电流","C.M.RO3_GYB_A@out"]
["RO3反渗透高压泵设置频率","C.M.RO3_GYB_AO_FB@spare"]
["RO3反渗透高压泵频率报警","C.M.RO3_GYB_fre@Fault"]
["RO3反渗透高压泵频率高报警","C.M.RO3_GYB_fre@H_AL"]
["RO3反渗透高压泵频率高报警开关","C.M.RO3_GYB_fre@H_AL_ON"]
["RO3反渗透高压泵频率高限设置","C.M.RO3_GYB_fre@H_AL_set"]
["RO3反渗透高压泵频率低报警","C.M.RO3_GYB_fre@L_AL"]
["RO3反渗透高压泵频率低报警开关","C.M.RO3_GYB_fre@L_AL_ON"]
["RO3反渗透高压泵频率低限设置","C.M.RO3_GYB_fre@L_AL_set"]
["RO3反渗透高压泵运行频率","C.M.RO3_GYB_fre@out"]
["RO3进水调节阀开度设定值","C.M.RO3_GYBF_AO_FB@spare"]
["RO3进水调节阀开度报警","C.M.RO3_GYBF_kd@fault"]
["RO3进水调节阀开度高报警","C.M.RO3_GYBF_kd@H_AL"]
["RO3进水调节阀开度高报警开关","C.M.RO3_GYBF_kd@H_AL_ON"]
["RO3进水调节阀开度高限设置","C.M.RO3_GYBF_kd@H_AL_set"]
["RO3进水调节阀开度低报警","C.M.RO3_GYBF_kd@L_AL"]
["RO3进水调节阀开度低报警开关","C.M.RO3_GYBF_kd@L_AL_ON"]
["RO3进水调节阀开度低限设置","C.M.RO3_GYBF_kd@L_AL_set"]
["RO3进水调节阀开度","C.M.RO3_GYBF_kd@out"]
["RO3反渗透段间泵高压开关","C.M.RO3_LS_DJB_H"]
["RO3反渗透段间泵低压开关","C.M.RO3_LS_DJB_L"]
["RO3反渗透高压泵高压开关","C.M.RO3_LS_GYB_H"]
["RO3反渗透高压泵低压开关","C.M.RO3_LS_GYB_L"]
["RO3排气阀1手自动","C.M.RO3_PQF1@auto_select"]
["RO3排气阀1关操作","C.M.RO3_PQF1@close"]
["RO3排气阀1关到位","C.M.RO3_PQF1@close_feedback"]
["RO3排气阀1故障","C.M.RO3_PQF1@fault_total"]
["RO3排气阀1开操作","C.M.RO3_PQF1@open"]
["RO3排气阀1开到位","C.M.RO3_PQF1@open_feedback"]
["RO3排气阀1远程","C.M.RO3_PQF1@rem"]
["RO3排气阀1复位","C.M.RO3_PQF1@reset"]
["RO3排气阀2手自动","C.M.RO3_PQF2@auto_select"]
["RO3排气阀2关操作","C.M.RO3_PQF2@close"]
["RO3排气阀2关到位","C.M.RO3_PQF2@close_feedback"]
["RO3排气阀2故障","C.M.RO3_PQF2@fault_total"]
["RO3排气阀2开操作","C.M.RO3_PQF2@open"]
["RO3排气阀2开到位","C.M.RO3_PQF2@open_feedback"]
["RO3排气阀2远程","C.M.RO3_PQF2@rem"]
["RO3排气阀2复位","C.M.RO3_PQF2@reset"]
["RO3排气阀3手自动","C.M.RO3_PQF3@auto_select"]
["RO3排气阀3关操作","C.M.RO3_PQF3@close"]
["RO3排气阀3关到位","C.M.RO3_PQF3@close_feedback"]
["RO3排气阀3故障","C.M.RO3_PQF3@fault_total"]
["RO3排气阀3开操作","C.M.RO3_PQF3@open"]
["RO3排气阀3开到位","C.M.RO3_PQF3@open_feedback"]
["RO3排气阀3远程","C.M.RO3_PQF3@rem"]
["RO3排气阀3复位","C.M.RO3_PQF3@reset"]
["RO3排气阀4手自动","C.M.RO3_PQF4@auto_select"]
["RO3排气阀4关操作","C.M.RO3_PQF4@close"]
["RO3排气阀4关到位","C.M.RO3_PQF4@close_feedback"]
["RO3排气阀4故障","C.M.RO3_PQF4@fault_total"]
["RO3排气阀4开操作","C.M.RO3_PQF4@open"]
["RO3排气阀4开到位","C.M.RO3_PQF4@open_feedback"]
["RO3排气阀4远程","C.M.RO3_PQF4@rem"]
["RO3排气阀4复位","C.M.RO3_PQF4@reset"]
["RO3排气阀5手自动","C.M.RO3_PQF5@auto_select"]
["RO3排气阀5关操作","C.M.RO3_PQF5@close"]
["RO3排气阀5关到位","C.M.RO3_PQF5@close_feedback"]
["RO3排气阀5故障","C.M.RO3_PQF5@fault_total"]
["RO3排气阀5开操作","C.M.RO3_PQF5@open"]
["RO3排气阀5开到位","C.M.RO3_PQF5@open_feedback"]
["RO3排气阀5远程","C.M.RO3_PQF5@rem"]
["RO3排气阀5复位","C.M.RO3_PQF5@reset"]
["RO3排气阀6手自动","C.M.RO3_PQF6@auto_select"]
["RO3排气阀6关操作","C.M.RO3_PQF6@close"]
["RO3排气阀6关到位","C.M.RO3_PQF6@close_feedback"]
["RO3排气阀6故障","C.M.RO3_PQF6@fault_total"]
["RO3排气阀6开操作","C.M.RO3_PQF6@open"]
["RO3排气阀6开到位","C.M.RO3_PQF6@open_feedback"]
["RO3排气阀6远程","C.M.RO3_PQF6@rem"]
["RO3排气阀6复位","C.M.RO3_PQF6@reset"]
["RO3排气阀7手自动","C.M.RO3_PQF7@auto_select"]
["RO3排气阀7关操作","C.M.RO3_PQF7@close"]
["RO3排气阀7关到位","C.M.RO3_PQF7@close_feedback"]
["RO3排气阀7故障","C.M.RO3_PQF7@fault_total"]
["RO3排气阀7开操作","C.M.RO3_PQF7@open"]
["RO3排气阀7开到位","C.M.RO3_PQF7@open_feedback"]
["RO3排气阀7远程","C.M.RO3_PQF7@rem"]
["RO3排气阀7复位","C.M.RO3_PQF7@reset"]
["RO3产水压力报警","C.M.RO3_PT_CS@fault"]
["RO3产水压力高报警","C.M.RO3_PT_CS@H_AL"]
["RO3产水压力高报警开关","C.M.RO3_PT_CS@H_AL_ON"]
["RO3产水压力高限设置","C.M.RO3_PT_CS@H_AL_set"]
["RO3产水压力低报警","C.M.RO3_PT_CS@L_AL"]
["RO3产水压力低报警开关","C.M.RO3_PT_CS@L_AL_ON"]
["RO3产水压力低限设置","C.M.RO3_PT_CS@L_AL_set"]
["RO3产水压力","C.M.RO3_PT_CS@out"]
["RO3一段浓水压力报警","C.M.RO3_PT_DJ1@fault"]
["RO3一段浓水压力高报警","C.M.RO3_PT_DJ1@H_AL"]
["RO3一段浓水压力高报警开关","C.M.RO3_PT_DJ1@H_AL_ON"]
["RO3一段浓水压力高限设置","C.M.RO3_PT_DJ1@H_AL_set"]
["RO3一段浓水压力低报警","C.M.RO3_PT_DJ1@L_AL"]
["RO3一段浓水压力低报警开关","C.M.RO3_PT_DJ1@L_AL_ON"]
["RO3一段浓水压力低限设置","C.M.RO3_PT_DJ1@L_AL_set"]
["RO3一段浓水压力","C.M.RO3_PT_DJ1@out"]
["RO3二段进水压力报警","C.M.RO3_PT_DJ2@fault"]
["RO3二段进水压力高报警","C.M.RO3_PT_DJ2@H_AL"]
["RO3二段进水压力高报警开关","C.M.RO3_PT_DJ2@H_AL_ON"]
["RO3二段进水压力高限设置","C.M.RO3_PT_DJ2@H_AL_set"]
["RO3二段进水压力低报警","C.M.RO3_PT_DJ2@L_AL"]
["RO3二段进水压力低报警开关","C.M.RO3_PT_DJ2@L_AL_ON"]
["RO3二段进水压力低限设置","C.M.RO3_PT_DJ2@L_AL_set"]
["RO3二段进水压力","C.M.RO3_PT_DJ2@out"]
["RO3一段进水压力报警","C.M.RO3_PT_JS@fault"]
["RO3一段进水压力高报警","C.M.RO3_PT_JS@H_AL"]
["RO3一段进水压力高报警开关","C.M.RO3_PT_JS@H_AL_ON"]
["RO3一段进水压力高限设置","C.M.RO3_PT_JS@H_AL_set"]
["RO3一段进水压力低报警","C.M.RO3_PT_JS@L_AL"]
["RO3一段进水压力低报警开关","C.M.RO3_PT_JS@L_AL_ON"]
["RO3一段进水压力低限设置","C.M.RO3_PT_JS@L_AL_set"]
["RO3一段进水压力","C.M.RO3_PT_JS@out"]
["RO3二段浓水压力报警","C.M.RO3_PT_NS@fault"]
["RO3二段浓水压力高报警","C.M.RO3_PT_NS@H_AL"]
["RO3二段浓水压力高报警开关","C.M.RO3_PT_NS@H_AL_ON"]
["RO3二段浓水压力高限设置","C.M.RO3_PT_NS@H_AL_set"]
["RO3二段浓水压力低报警","C.M.RO3_PT_NS@L_AL"]
["RO3二段浓水压力低报警开关","C.M.RO3_PT_NS@L_AL_ON"]
["RO3二段浓水压力低限设置","C.M.RO3_PT_NS@L_AL_set"]
["RO3二段浓水压力","C.M.RO3_PT_NS@out"]
["RO3未知阀手自动","C.M.RO3_SJJF@auto_select"]
["RO3未知阀关操作","C.M.RO3_SJJF@close"]
["RO3未知阀关到位","C.M.RO3_SJJF@close_feedback"]
["RO3未知阀故障","C.M.RO3_SJJF@fault_total"]
["RO3未知阀开操作","C.M.RO3_SJJF@open"]
["RO3未知阀开到位","C.M.RO3_SJJF@open_feedback"]
["RO3未知阀远程","C.M.RO3_SJJF@rem"]
["RO3未知阀复位","C.M.RO3_SJJF@reset"]
["3#阻垢剂加药阀手自动","C.M.RO3_ZGJF@auto_select"]
["3#阻垢剂加药阀关操作","C.M.RO3_ZGJF@close"]
["3#阻垢剂加药阀关到位","C.M.RO3_ZGJF@close_feedback"]
["3#阻垢剂加药阀故障","C.M.RO3_ZGJF@fault_total"]
["3#阻垢剂加药阀开操作","C.M.RO3_ZGJF@open"]
["3#阻垢剂加药阀开到位","C.M.RO3_ZGJF@open_feedback"]
["3#阻垢剂加药阀远程","C.M.RO3_ZGJF@rem"]
["3#阻垢剂加药阀复位","C.M.RO3_ZGJF@reset"]
["RO4不合格水阀手自动","C.M.RO4_BHGF@auto_select"]
["RO4不合格水阀关操作","C.M.RO4_BHGF@close"]
["RO4不合格水阀关到位","C.M.RO4_BHGF@close_feedback"]
["RO4不合格水阀故障","C.M.RO4_BHGF@fault_total"]
["RO4不合格水阀开操作","C.M.RO4_BHGF@open"]
["RO4不合格水阀开到位","C.M.RO4_BHGF@open_feedback"]
["RO4不合格水阀远程","C.M.RO4_BHGF@rem"]
["RO4不合格水阀复位","C.M.RO4_BHGF@reset"]
["RO4产水CIP回水阀手自动","C.M.RO4_CIP_CSHSF@auto_select"]
["RO4产水CIP回水阀关操作","C.M.RO4_CIP_CSHSF@close"]
["RO4产水CIP回水阀关到位","C.M.RO4_CIP_CSHSF@close_feedback"]
["RO4产水CIP回水阀故障","C.M.RO4_CIP_CSHSF@fault_total"]
["RO4产水CIP回水阀开操作","C.M.RO4_CIP_CSHSF@open"]
["RO4产水CIP回水阀开到位","C.M.RO4_CIP_CSHSF@open_feedback"]
["RO4产水CIP回水阀远程","C.M.RO4_CIP_CSHSF@rem"]
["RO4产水CIP回水阀复位","C.M.RO4_CIP_CSHSF@reset"]
["RO4一段CIP回水阀手自动","C.M.RO4_CIP_HSF1@auto_select"]
["RO4一段CIP回水阀关操作","C.M.RO4_CIP_HSF1@close"]
["RO4一段CIP回水阀关到位","C.M.RO4_CIP_HSF1@close_feedback"]
["RO4一段CIP回水阀故障","C.M.RO4_CIP_HSF1@fault_total"]
["RO4一段CIP回水阀开操作","C.M.RO4_CIP_HSF1@open"]
["RO4一段CIP回水阀开到位","C.M.RO4_CIP_HSF1@open_feedback"]
["RO4一段CIP回水阀远程","C.M.RO4_CIP_HSF1@rem"]
["RO4一段CIP回水阀复位","C.M.RO4_CIP_HSF1@reset"]
["RO4二段CIP回水阀手自动","C.M.RO4_CIP_HSF2@auto_select"]
["RO4二段CIP回水阀关操作","C.M.RO4_CIP_HSF2@close"]
["RO4二段CIP回水阀关到位","C.M.RO4_CIP_HSF2@close_feedback"]
["RO4二段CIP回水阀故障","C.M.RO4_CIP_HSF2@fault_total"]
["RO4二段CIP回水阀开操作","C.M.RO4_CIP_HSF2@open"]
["RO4二段CIP回水阀开到位","C.M.RO4_CIP_HSF2@open_feedback"]
["RO4二段CIP回水阀远程","C.M.RO4_CIP_HSF2@rem"]
["RO4二段CIP回水阀复位","C.M.RO4_CIP_HSF2@reset"]
["RO4一段CIP进水阀手自动","C.M.RO4_CIP_JSF1@auto_select"]
["RO4一段CIP进水阀关操作","C.M.RO4_CIP_JSF1@close"]
["RO4一段CIP进水阀关到位","C.M.RO4_CIP_JSF1@close_feedback"]
["RO4一段CIP进水阀故障","C.M.RO4_CIP_JSF1@fault_total"]
["RO4一段CIP进水阀开操作","C.M.RO4_CIP_JSF1@open"]
["RO4一段CIP进水阀开到位","C.M.RO4_CIP_JSF1@open_feedback"]
["RO4一段CIP进水阀远程","C.M.RO4_CIP_JSF1@rem"]
["RO4一段CIP进水阀复位","C.M.RO4_CIP_JSF1@reset"]
["RO4二段CIP进水阀手自动","C.M.RO4_CIP_JSF2@auto_select"]
["RO4二段CIP进水阀关操作","C.M.RO4_CIP_JSF2@close"]
["RO4二段CIP进水阀关到位","C.M.RO4_CIP_JSF2@close_feedback"]
["RO4二段CIP进水阀故障","C.M.RO4_CIP_JSF2@fault_total"]
["RO4二段CIP进水阀开操作","C.M.RO4_CIP_JSF2@open"]
["RO4二段CIP进水阀开到位","C.M.RO4_CIP_JSF2@open_feedback"]
["RO4二段CIP进水阀远程","C.M.RO4_CIP_JSF2@rem"]
["RO4二段CIP进水阀复位","C.M.RO4_CIP_JSF2@reset"]
["进水排空阀手自动","C.M.RO4_CIP_PKF1@auto_select"]
["进水排空阀关操作","C.M.RO4_CIP_PKF1@close"]
["进水排空阀关到位","C.M.RO4_CIP_PKF1@close_feedback"]
["进水排空阀故障","C.M.RO4_CIP_PKF1@fault_total"]
["进水排空阀开操作","C.M.RO4_CIP_PKF1@open"]
["进水排空阀开到位","C.M.RO4_CIP_PKF1@open_feedback"]
["进水排空阀远程","C.M.RO4_CIP_PKF1@rem"]
["进水排空阀复位","C.M.RO4_CIP_PKF1@reset"]
["回水排空阀手自动","C.M.RO4_CIP_PKF2@auto_select"]
["回水排空阀关操作","C.M.RO4_CIP_PKF2@close"]
["回水排空阀关到位","C.M.RO4_CIP_PKF2@close_feedback"]
["回水排空阀故障","C.M.RO4_CIP_PKF2@fault_total"]
["回水排空阀开操作","C.M.RO4_CIP_PKF2@open"]
["回水排空阀开到位","C.M.RO4_CIP_PKF2@open_feedback"]
["回水排空阀远程","C.M.RO4_CIP_PKF2@rem"]
["回水排空阀复位","C.M.RO4_CIP_PKF2@reset"]
["RO4产水电导报警","C.M.RO4_Cond_CS@fault"]
["RO4产水电导高报警","C.M.RO4_Cond_CS@H_AL"]
["RO4产水电导高报警开关","C.M.RO4_Cond_CS@H_AL_ON"]
["RO4产水电导高限设置","C.M.RO4_Cond_CS@H_AL_set"]
["RO4产水电导低报警","C.M.RO4_Cond_CS@L_AL"]
["RO4产水电导低报警开关","C.M.RO4_Cond_CS@L_AL_ON"]
["RO4产水电导低限设置","C.M.RO4_Cond_CS@L_AL_set"]
["RO4产水电导","C.M.RO4_Cond_CS@out"]
["RO4产水阀手自动","C.M.RO4_CSF@auto_select"]
["RO4产水阀关操作","C.M.RO4_CSF@close"]
["RO4产水阀关到位","C.M.RO4_CSF@close_feedback"]
["RO4产水阀故障","C.M.RO4_CSF@fault_total"]
["RO4产水阀开操作","C.M.RO4_CSF@open"]
["RO4产水阀开到位","C.M.RO4_CSF@open_feedback"]
["RO4产水阀远程","C.M.RO4_CSF@rem"]
["RO4产水阀复位","C.M.RO4_CSF@reset"]
["RO4一段冲洗进水阀手自动","C.M.RO4_CXJF1@auto_select"]
["RO4一段冲洗进水阀关操作","C.M.RO4_CXJF1@close"]
["RO4一段冲洗进水阀关到位","C.M.RO4_CXJF1@close_feedback"]
["RO4一段冲洗进水阀故障","C.M.RO4_CXJF1@fault_total"]
["RO4一段冲洗进水阀开操作","C.M.RO4_CXJF1@open"]
["RO4一段冲洗进水阀开到位","C.M.RO4_CXJF1@open_feedback"]
["RO4一段冲洗进水阀远程","C.M.RO4_CXJF1@rem"]
["RO4一段冲洗进水阀复位","C.M.RO4_CXJF1@reset"]
["RO4二段冲洗进水阀手自动","C.M.RO4_CXJF2@auto_select"]
["RO4二段冲洗进水阀关操作","C.M.RO4_CXJF2@close"]
["RO4二段冲洗进水阀关到位","C.M.RO4_CXJF2@close_feedback"]
["RO4二段冲洗进水阀故障","C.M.RO4_CXJF2@fault_total"]
["RO4二段冲洗进水阀开操作","C.M.RO4_CXJF2@open"]
["RO4二段冲洗进水阀开到位","C.M.RO4_CXJF2@open_feedback"]
["RO4二段冲洗进水阀远程","C.M.RO4_CXJF2@rem"]
["RO4二段冲洗进水阀复位","C.M.RO4_CXJF2@reset"]
["RO4一段冲洗排水阀手自动","C.M.RO4_CXPF1@auto_select"]
["RO4一段冲洗排水阀关操作","C.M.RO4_CXPF1@close"]
["RO4一段冲洗排水阀关到位","C.M.RO4_CXPF1@close_feedback"]
["RO4一段冲洗排水阀故障","C.M.RO4_CXPF1@fault_total"]
["RO4一段冲洗排水阀开操作","C.M.RO4_CXPF1@open"]
["RO4一段冲洗排水阀开到位","C.M.RO4_CXPF1@open_feedback"]
["RO4一段冲洗排水阀远程","C.M.RO4_CXPF1@rem"]
["RO4一段冲洗排水阀复位","C.M.RO4_CXPF1@reset"]
["RO4二段冲洗排水阀手自动","C.M.RO4_CXPF2@auto_select"]
["RO4二段冲洗排水阀关操作","C.M.RO4_CXPF2@close"]
["RO4二段冲洗排水阀关到位","C.M.RO4_CXPF2@close_feedback"]
["RO4二段冲洗排水阀故障","C.M.RO4_CXPF2@fault_total"]
["RO4二段冲洗排水阀开操作","C.M.RO4_CXPF2@open"]
["RO4二段冲洗排水阀开到位","C.M.RO4_CXPF2@open_feedback"]
["RO4二段冲洗排水阀远程","C.M.RO4_CXPF2@rem"]
["RO4二段冲洗排水阀复位","C.M.RO4_CXPF2@reset"]
["RO4紧急停车","C.M.RO4_DB@button[00]"]
["RO4自动开机","C.M.RO4_DB@button[01]"]
["RO4自动停止","C.M.RO4_DB@button[02]"]
["RO4自动正常冲洗","C.M.RO4_DB@button[03]"]
["RO4自动反向冲洗","C.M.RO4_DB@button[04]"]
["RO4自动杀菌冲洗","C.M.RO4_DB@button[05]"]
["RO4未知1（不确定）","C.M.RO4_DB@button[06]"]
["RO4未知2（不确定）","C.M.RO4_DB@button[07]"]
["RO4全自动开机","C.M.RO4_DB@button[08]"]
["RO4CIP启停","C.M.RO4_DB@button[09]"]
["RO4信息清除","C.M.RO4_DB@button[10]"]
["RO4自动杀菌投入/切除","C.M.RO4_DB@button[11]"]
["RO4高压泵PID/定频控制","C.M.RO4_DB@button[12]"]
["RO4段间泵PID/定频控制","C.M.RO4_DB@button[13]"]
["RO4一段CIP（保持）","C.M.RO4_DB@button[14]"]
["RO4二段CIP（保持）","C.M.RO4_DB@button[15]"]
["RO4一段酸洗（选中保持）","C.M.RO4_DB@button[16]"]
["RO4二段酸洗（选中保持）","C.M.RO4_DB@button[17]"]
["RO4一段碱洗（选中保持）","C.M.RO4_DB@button[18]"]
["RO4二段碱洗（选中保持）","C.M.RO4_DB@button[19]"]
["RO4一段非氧洗（选中保持）","C.M.RO4_DB@button[20]"]
["RO4二段非氧洗（选中保持）","C.M.RO4_DB@button[21]"]
["RO4一段酸洗（手动保持）","C.M.RO4_DB@button[22]"]
["RO4二段酸洗（手动保持）","C.M.RO4_DB@button[23]"]
["RO4一段碱洗（手动保持）","C.M.RO4_DB@button[24]"]
["RO4二段碱洗（手动保持）","C.M.RO4_DB@button[25]"]
["RO4一段非氧洗（手动保持）","C.M.RO4_DB@button[26]"]
["RO4二段非氧洗（手动保持）","C.M.RO4_DB@button[27]"]
["RO4HOLDHB1","C.M.RO4_DB@button[28]"]
["RO4HOLDHB2","C.M.RO4_DB@button[29]"]
["RO4HOLDHB3","C.M.RO4_DB@button[30]"]
["RO4HOLDHB4","C.M.RO4_DB@button[31]"]
["RO4 ZBOOL HOLD1","C.M.RO4_DB@Zbool[0]"]
["RO4 ZBOOL HOLD2","C.M.RO4_DB@Zbool[1]"]
["RO4 ZBOOL HOLD3","C.M.RO4_DB@Zbool[2]"]
["RO4 ZDint HOLD1","C.M.RO4_DB@ZDint[0]"]
["RO4 ZDint HOLD2","C.M.RO4_DB@ZDint[1]"]
["RO4 ZDint HOLD3","C.M.RO4_DB@ZDint[2]"]
["RO4一段需要酸洗标志","C.M.RO4_DB@ZFlag[0]"]
["RO4二段需要酸洗标志","C.M.RO4_DB@ZFlag[1]"]
["RO4一段需要J洗标志","C.M.RO4_DB@ZFlag[2]"]
["RO4二段需要J洗标志","C.M.RO4_DB@ZFlag[3]"]
["RO4一段需要FY洗标志","C.M.RO4_DB@ZFlag[4]"]
["RO4二段需要FY洗标志","C.M.RO4_DB@ZFlag[5]"]
["RO4跳转一段酸洗","C.M.RO4_DB@ZFlag[6]"]
["RO4跳转二段酸洗","C.M.RO4_DB@ZFlag[7]"]
["RO4跳转一段J洗","C.M.RO4_DB@ZFlag[8]"]
["RO4跳转二段J洗","C.M.RO4_DB@ZFlag[9]"]
["RO4跳转一段非氧洗","C.M.RO4_DB@ZFlag[10]"]
["RO4跳转二段非氧洗","C.M.RO4_DB@ZFlag[11]"]
["RO4HOLD ZFLAG 1","C.M.RO4_DB@ZFlag[12]"]
["RO4HOLD ZFLAG 2","C.M.RO4_DB@ZFlag[13]"]
["RO4HOLD ZFLAG 3","C.M.RO4_DB@ZFlag[14]"]
["RO4HOLD ZFLAG 4","C.M.RO4_DB@ZFlag[15]"]
["RO4当前步序时间","C.M.RO4_DB@ZZZreal[0]"]
["RO4当前步序设定时间","C.M.RO4_DB@ZZZreal[1]"]
["RO41段酸洗记次数","C.M.RO4_DB@ZZZreal[2]"]
["RO4 2段酸洗记次数","C.M.RO4_DB@ZZZreal[3]"]
["RO4 1段J洗记次数","C.M.RO4_DB@ZZZreal[4]"]
["RO4 2段J洗记次数","C.M.RO4_DB@ZZZreal[5]"]
["RO4 1段FY洗记次数","C.M.RO4_DB@ZZZreal[6]"]
["RO4 2段FY洗记次数","C.M.RO4_DB@ZZZreal[7]"]
["RO4 1段酸洗设定次数","C.M.RO4_DB@ZZZreal[8]"]
["RO4 2段酸洗设定次数","C.M.RO4_DB@ZZZreal[9]"]
["RO4 1段J洗设定次数","C.M.RO4_DB@ZZZreal[10]"]
["RO4 2段J洗设定次数","C.M.RO4_DB@ZZZreal[11]"]
["RO4 1段FY洗设定次数","C.M.RO4_DB@ZZZreal[12]"]
["RO4 2段FY洗设定次数","C.M.RO4_DB@ZZZreal[13]"]
["RO4HOLD1","C.M.RO4_DB@ZZZreal[14]"]
["RO4HOLD2","C.M.RO4_DB@ZZZreal[15]"]
["RO4 一段加药前冲时间设定","C.M.RO4_DB@ZZZreal[16]"]
["RO4 一段加药浸泡时间设定","C.M.RO4_DB@ZZZreal[17]"]
["RO4一段加药后冲时间设定","C.M.RO4_DB@ZZZreal[18]"]
["RO4二段加药前冲时间设定","C.M.RO4_DB@ZZZreal[19]"]
["RO4二段加药浸泡时间设定","C.M.RO4_DB@ZZZreal[20]"]
["RO4二段加药后冲时间设定","C.M.RO4_DB@ZZZreal[21]"]
["RO4HOLD3","C.M.RO4_DB@ZZZreal[22]"]
["RO4HOLD4","C.M.RO4_DB@ZZZreal[23]"]
["RO4HOLD5","C.M.RO4_DB@ZZZreal[24]"]
["RO4HOLD6","C.M.RO4_DB@ZZZreal[25]"]
["RO4一段CIP循环","C.M.RO4_DB@ZZZreal[26]"]
["RO4一段CIP浸泡","C.M.RO4_DB@ZZZreal[27]"]
["RO4二段CIP循环","C.M.RO4_DB@ZZZreal[28]"]
["RO4二段CIP浸泡","C.M.RO4_DB@ZZZreal[29]"]
["RO4产水杀菌时间设定","C.M.RO4_DB@ZZZreal[30]"]
["RO4产水杀菌等待时间设定","C.M.RO4_DB@ZZZreal[31]"]
["RO4产水杀菌时间READ","C.M.RO4_DB@ZZZreal[32]"]
["RO4产水杀菌等待时间READ","C.M.RO4_DB@ZZZreal[33]"]
["RO4HOLD7","C.M.RO4_DB@ZZZreal[34]"]
["RO4HOLD8","C.M.RO4_DB@ZZZreal[35]"]
["RO4HOLD9","C.M.RO4_DB@ZZZreal[36]"]
["RO4HOLD10","C.M.RO4_DB@ZZZreal[37]"]
["RO4HOLD11","C.M.RO4_DB@ZZZreal[38]"]
["RO4HOLD12","C.M.RO4_DB@ZZZreal[39]"]
["RO4——碱冲洗设备ready","C.M.RO4_DB@ready[08]"]
["RO4——杀菌冲洗设备ready","C.M.RO4_DB@ready[09]"]
["RO4——备用1","C.M.RO4_DB@ready[10]"]
["RO4——备用2","C.M.RO4_DB@ready[11]"]
["RO4控制字","C.M.RO4_DB@control_word"]
["RO4反渗透段间泵频率设定","C.M.RO4_DB@DJB_fre_sp"]
["RO4一段压差","C.M.RO4_DB@DPT_1"]
["RO4一段差压高设定","C.M.RO4_DB@DPT_1_stop_sp"]
["RO4二段压差","C.M.RO4_DB@DPT_2"]
["RO4二段差压高设定","C.M.RO4_DB@DPT_2_stop_sp"]
["RO4电导正常可产水设定","C.M.RO4_DB@EC_ZCS_sp"]
["RO4产水电导高设定","C.M.RO4_DB@EC_ZCS_stop_sp"]
["RO4故障字","C.M.RO4_DB@fault_word"]
["RO4二段产水流量设定","C.M.RO4_DB@FT_CS2_sp"]
["RO4进水流量设定","C.M.RO4_DB@FT_JS_sp"]
["RO4反渗透高压泵频率设定","C.M.RO4_DB@GYB_fre_sp"]
["RO4控制模式","C.M.RO4_DB@model_word"]
["RO4未知3（不确定）","C.M.RO4_DB@PS[00]"]
["RO4未知4（不确定）","C.M.RO4_DB@PS[01]"]
["RO4未知5（不确定）","C.M.RO4_DB@PS[02]"]
["RO4未知6（不确定）","C.M.RO4_DB@PS[03]"]
["RO4产水压力高设定","C.M.RO4_DB@PT_CS_stop_sp"]
["RO4段间泵出水压力高设定","C.M.RO4_DB@PT_DJB_CS_stop_sp"]
["RO4段间泵进水压力低设定","C.M.RO4_DB@PT_DJB_JS_stop_sp"]
["RO4高压泵出水压力高设定","C.M.RO4_DB@PT_JS_stop_sp"]
["RO4未知7（不确定）","C.M.RO4_DB@ready[00]"]
["RO4未知8（不确定）","C.M.RO4_DB@ready[01]"]
["RO4未知9（不确定）","C.M.RO4_DB@ready[02]"]
["RO4产水准备好","C.M.RO4_DB@ready[03]"]
["RO4冲洗准备好","C.M.RO4_DB@ready[04]"]
["RO4杀菌准备好","C.M.RO4_DB@ready[05]"]
["RO4CIP准备好","C.M.RO4_DB@ready[06]"]
["RO4未知10（不确定）","C.M.RO4_DB@ready[07]"]
["RO4提醒字","C.M.RO4_DB@reminder_word"]
["RO4运行时间","C.M.RO4_DB@run_time"]
["RO4停止时间","C.M.RO4_DB@stop_time"]
["RO4不合格排水","C.M.RO4_DB@time_bhgs_display"]
["RO4不合格排水设定","C.M.RO4_DB@time_bhgs_sp"]
["RO4产水可延迟时间设定","C.M.RO4_DB@time_CS_delay_sp"]
["RO4产水时间","C.M.RO4_DB@time_CS_display"]
["RO4产水时间设定","C.M.RO4_DB@time_CS_sp"]
["RO4一段反冲","C.M.RO4_DB@time_FX1_display"]
["RO4一段反冲设定","C.M.RO4_DB@time_FX1_sp"]
["RO4开机等待","C.M.RO4_DB@time_kj_wait"]
["RO4排气时间","C.M.RO4_DB@time_kjcx_display1"]
["RO4开机冲洗","C.M.RO4_DB@time_kjcx_display2"]
["RO4排气时间设定","C.M.RO4_DB@time_kjcx_sp1"]
["RO4开机冲洗设定","C.M.RO4_DB@time_kjcx_sp2"]
["RO4杀菌间隔","C.M.RO4_DB@time_shajun_display"]
["RO4杀菌间隔设定","C.M.RO4_DB@time_shajun_sp"]
["RO4杀菌等待","C.M.RO4_DB@time_sj_wait"]
["RO4一段反冲","C.M.RO4_DB@time_sjcx1_display"]
["RO4一段反冲设定","C.M.RO4_DB@time_sjcx1_sp"]
["RO4二段反冲","C.M.RO4_DB@time_sjcx2_display"]
["RO4二段反冲设定","C.M.RO4_DB@time_sjcx2_sp"]
["RO4浸泡时间","C.M.RO4_DB@time_sjjp_display"]
["RO4浸泡时间设定","C.M.RO4_DB@time_sjjp_sp"]
["RO4加药时间","C.M.RO4_DB@time_sjjy_display"]
["RO4加药时间设定","C.M.RO4_DB@time_sjjy_sp"]
["RO4冲洗等待","C.M.RO4_DB@time_tj_wait"]
["RO4二段正冲","C.M.RO4_DB@time_ZX2_display"]
["RO4二段反冲设定","C.M.RO4_DB@time_ZX2_sp"]
["RO4正常冲洗","C.M.RO4_DB@time_ZX12_display"]
["RO4正常冲洗设定","C.M.RO4_DB@time_ZX12_sp"]
["RO4反渗透段间泵手自动","C.M.RO4_DJB@auto_select"]
["RO4反渗透段间泵故障","C.M.RO4_DJB@fault_total"]
["RO4反渗透段间泵远程","C.M.RO4_DJB@rem"]
["RO4反渗透段间泵复位","C.M.RO4_DJB@reset"]
["RO4反渗透段间泵运行","C.M.RO4_DJB@run"]
["RO4反渗透段间泵运行时间","C.M.RO4_DJB@run_time"]
["RO4反渗透段间泵启动操作","C.M.RO4_DJB@start"]
["RO4反渗透段间泵停止操作","C.M.RO4_DJB@stop"]
["RO4反渗透段间泵电流报警","C.M.RO4_DJB_A@Fault"]
["RO4反渗透段间泵电流高报警","C.M.RO4_DJB_A@H_AL"]
["RO4反渗透段间泵电流高报警开关","C.M.RO4_DJB_A@H_AL_ON"]
["RO4反渗透段间泵电流高限设置","C.M.RO4_DJB_A@H_AL_set"]
["RO4反渗透段间泵电流低报警","C.M.RO4_DJB_A@L_AL"]
["RO4反渗透段间泵电流低报警开关","C.M.RO4_DJB_A@L_AL_ON"]
["RO4反渗透段间泵电流低限设置","C.M.RO4_DJB_A@L_AL_set"]
["RO4反渗透段间泵运行电流","C.M.RO4_DJB_A@out"]
["RO4反渗透段间泵设置频率","C.M.RO4_DJB_AO_FB@spare"]
["RO4反渗透段间泵频率报警","C.M.RO4_DJB_fre@Fault"]
["RO4反渗透段间泵频率高报警","C.M.RO4_DJB_fre@H_AL"]
["RO4反渗透段间泵频率高报警开关","C.M.RO4_DJB_fre@H_AL_ON"]
["RO4反渗透段间泵频率高限设置","C.M.RO4_DJB_fre@H_AL_set"]
["RO4反渗透段间泵频率低报警","C.M.RO4_DJB_fre@L_AL"]
["RO4反渗透段间泵频率低报警开关","C.M.RO4_DJB_fre@L_AL_ON"]
["RO4反渗透段间泵频率低限设置","C.M.RO4_DJB_fre@L_AL_set"]
["RO4反渗透段间泵运行频率","C.M.RO4_DJB_fre@out"]
["RO4反渗透二段产水流量报警","C.M.RO4_FT_CS2@fault"]
["RO4反渗透二段产水流量高报警","C.M.RO4_FT_CS2@H_AL"]
["RO4反渗透二段产水流量高报警开关","C.M.RO4_FT_CS2@H_AL_ON"]
["RO4反渗透二段产水流量高限设置","C.M.RO4_FT_CS2@H_AL_set"]
["RO4反渗透二段产水流量低报警","C.M.RO4_FT_CS2@L_AL"]
["RO4反渗透二段产水流量低报警开关","C.M.RO4_FT_CS2@L_AL_ON"]
["RO4反渗透二段产水流量低限设置","C.M.RO4_FT_CS2@L_AL_set"]
["RO4反渗透二段产水流量","C.M.RO4_FT_CS2@out"]
["RO4反渗透进水流量报警","C.M.RO4_FT_JS@fault"]
["RO4反渗透进水流量高报警","C.M.RO4_FT_JS@H_AL"]
["RO4反渗透进水流量高报警开关","C.M.RO4_FT_JS@H_AL_ON"]
["RO4反渗透进水流量高限设置","C.M.RO4_FT_JS@H_AL_set"]
["RO4反渗透进水流量低报警","C.M.RO4_FT_JS@L_AL"]
["RO4反渗透进水流量低报警开关","C.M.RO4_FT_JS@L_AL_ON"]
["RO4反渗透进水流量低限设置","C.M.RO4_FT_JS@L_AL_set"]
["RO4反渗透进水流量","C.M.RO4_FT_JS@out"]
["RO4反渗透浓水流量报警","C.M.RO4_FT_NS@fault"]
["RO4反渗透浓水流量高报警","C.M.RO4_FT_NS@H_AL"]
["RO4反渗透浓水流量高报警开关","C.M.RO4_FT_NS@H_AL_ON"]
["RO4反渗透浓水流量高限设置","C.M.RO4_FT_NS@H_AL_set"]
["RO4反渗透浓水流量低报警","C.M.RO4_FT_NS@L_AL"]
["RO4反渗透浓水流量低报警开关","C.M.RO4_FT_NS@L_AL_ON"]
["RO4反渗透浓水流量低限设置","C.M.RO4_FT_NS@L_AL_set"]
["RO4反渗透浓水流量","C.M.RO4_FT_NS@out"]
["RO4反渗透高压泵手自动","C.M.RO4_GYB@auto_select"]
["RO4反渗透高压泵故障","C.M.RO4_GYB@fault_total"]
["RO4反渗透高压泵远程","C.M.RO4_GYB@rem"]
["RO4反渗透高压泵复位","C.M.RO4_GYB@reset"]
["RO4反渗透高压泵运行","C.M.RO4_GYB@run"]
["RO4反渗透高压泵运行时间","C.M.RO4_GYB@run_time"]
["RO4反渗透高压泵启动操作","C.M.RO4_GYB@start"]
["RO4反渗透高压泵停止操作","C.M.RO4_GYB@stop"]
["RO4反渗透高压泵电流报警","C.M.RO4_GYB_A@Fault"]
["RO4反渗透高压泵电流高报警","C.M.RO4_GYB_A@H_AL"]
["RO4反渗透高压泵电流高报警开关","C.M.RO4_GYB_A@H_AL_ON"]
["RO4反渗透高压泵电流高限设置","C.M.RO4_GYB_A@H_AL_set"]
["RO4反渗透高压泵电流低报警","C.M.RO4_GYB_A@L_AL"]
["RO4反渗透高压泵电流低报警开关","C.M.RO4_GYB_A@L_AL_ON"]
["RO4反渗透高压泵电流低限设置","C.M.RO4_GYB_A@L_AL_set"]
["RO4反渗透高压泵运行电流","C.M.RO4_GYB_A@out"]
["RO4反渗透高压泵设置频率","C.M.RO4_GYB_AO_FB@spare"]
["RO4反渗透高压泵频率报警","C.M.RO4_GYB_fre@Fault"]
["RO4反渗透高压泵频率高报警","C.M.RO4_GYB_fre@H_AL"]
["RO4反渗透高压泵频率高报警开关","C.M.RO4_GYB_fre@H_AL_ON"]
["RO4反渗透高压泵频率高限设置","C.M.RO4_GYB_fre@H_AL_set"]
["RO4反渗透高压泵频率低报警","C.M.RO4_GYB_fre@L_AL"]
["RO4反渗透高压泵频率低报警开关","C.M.RO4_GYB_fre@L_AL_ON"]
["RO4反渗透高压泵频率低限设置","C.M.RO4_GYB_fre@L_AL_set"]
["RO4反渗透高压泵运行频率","C.M.RO4_GYB_fre@out"]
["RO4进水调节阀开度设定值","C.M.RO4_GYBF_AO_FB@spare"]
["RO4进水调节阀开度报警","C.M.RO4_GYBF_kd@fault"]
["RO4进水调节阀开度高报警","C.M.RO4_GYBF_kd@H_AL"]
["RO4进水调节阀开度高报警开关","C.M.RO4_GYBF_kd@H_AL_ON"]
["RO4进水调节阀开度高限设置","C.M.RO4_GYBF_kd@H_AL_set"]
["RO4进水调节阀开度低报警","C.M.RO4_GYBF_kd@L_AL"]
["RO4进水调节阀开度低报警开关","C.M.RO4_GYBF_kd@L_AL_ON"]
["RO4进水调节阀开度低限设置","C.M.RO4_GYBF_kd@L_AL_set"]
["RO4进水调节阀开度","C.M.RO4_GYBF_kd@out"]
["RO4反渗透段间泵高压开关","C.M.RO4_LS_DJB_H"]
["RO4反渗透段间泵低压开关","C.M.RO4_LS_DJB_L"]
["RO4反渗透高压泵高压开关","C.M.RO4_LS_GYB_H"]
["RO4反渗透高压泵低压开关","C.M.RO4_LS_GYB_L"]
["RO4排气阀1手自动","C.M.RO4_PQF1@auto_select"]
["RO4排气阀1关操作","C.M.RO4_PQF1@close"]
["RO4排气阀1关到位","C.M.RO4_PQF1@close_feedback"]
["RO4排气阀1故障","C.M.RO4_PQF1@fault_total"]
["RO4排气阀1开操作","C.M.RO4_PQF1@open"]
["RO4排气阀1开到位","C.M.RO4_PQF1@open_feedback"]
["RO4排气阀1远程","C.M.RO4_PQF1@rem"]
["RO4排气阀1复位","C.M.RO4_PQF1@reset"]
["RO4排气阀2手自动","C.M.RO4_PQF2@auto_select"]
["RO4排气阀2关操作","C.M.RO4_PQF2@close"]
["RO4排气阀2关到位","C.M.RO4_PQF2@close_feedback"]
["RO4排气阀2故障","C.M.RO4_PQF2@fault_total"]
["RO4排气阀2开操作","C.M.RO4_PQF2@open"]
["RO4排气阀2开到位","C.M.RO4_PQF2@open_feedback"]
["RO4排气阀2远程","C.M.RO4_PQF2@rem"]
["RO4排气阀2复位","C.M.RO4_PQF2@reset"]
["RO4排气阀3手自动","C.M.RO4_PQF3@auto_select"]
["RO4排气阀3关操作","C.M.RO4_PQF3@close"]
["RO4排气阀3关到位","C.M.RO4_PQF3@close_feedback"]
["RO4排气阀3故障","C.M.RO4_PQF3@fault_total"]
["RO4排气阀3开操作","C.M.RO4_PQF3@open"]
["RO4排气阀3开到位","C.M.RO4_PQF3@open_feedback"]
["RO4排气阀3远程","C.M.RO4_PQF3@rem"]
["RO4排气阀3复位","C.M.RO4_PQF3@reset"]
["RO4排气阀4手自动","C.M.RO4_PQF4@auto_select"]
["RO4排气阀4关操作","C.M.RO4_PQF4@close"]
["RO4排气阀4关到位","C.M.RO4_PQF4@close_feedback"]
["RO4排气阀4故障","C.M.RO4_PQF4@fault_total"]
["RO4排气阀4开操作","C.M.RO4_PQF4@open"]
["RO4排气阀4开到位","C.M.RO4_PQF4@open_feedback"]
["RO4排气阀4远程","C.M.RO4_PQF4@rem"]
["RO4排气阀4复位","C.M.RO4_PQF4@reset"]
["RO4排气阀5手自动","C.M.RO4_PQF5@auto_select"]
["RO4排气阀5关操作","C.M.RO4_PQF5@close"]
["RO4排气阀5关到位","C.M.RO4_PQF5@close_feedback"]
["RO4排气阀5故障","C.M.RO4_PQF5@fault_total"]
["RO4排气阀5开操作","C.M.RO4_PQF5@open"]
["RO4排气阀5开到位","C.M.RO4_PQF5@open_feedback"]
["RO4排气阀5远程","C.M.RO4_PQF5@rem"]
["RO4排气阀5复位","C.M.RO4_PQF5@reset"]
["RO4排气阀6手自动","C.M.RO4_PQF6@auto_select"]
["RO4排气阀6关操作","C.M.RO4_PQF6@close"]
["RO4排气阀6关到位","C.M.RO4_PQF6@close_feedback"]
["RO4排气阀6故障","C.M.RO4_PQF6@fault_total"]
["RO4排气阀6开操作","C.M.RO4_PQF6@open"]
["RO4排气阀6开到位","C.M.RO4_PQF6@open_feedback"]
["RO4排气阀6远程","C.M.RO4_PQF6@rem"]
["RO4排气阀6复位","C.M.RO4_PQF6@reset"]
["RO4排气阀7手自动","C.M.RO4_PQF7@auto_select"]
["RO4排气阀7关操作","C.M.RO4_PQF7@close"]
["RO4排气阀7关到位","C.M.RO4_PQF7@close_feedback"]
["RO4排气阀7故障","C.M.RO4_PQF7@fault_total"]
["RO4排气阀7开操作","C.M.RO4_PQF7@open"]
["RO4排气阀7开到位","C.M.RO4_PQF7@open_feedback"]
["RO4排气阀7远程","C.M.RO4_PQF7@rem"]
["RO4排气阀7复位","C.M.RO4_PQF7@reset"]
["RO4产水压力报警","C.M.RO4_PT_CS@fault"]
["RO4产水压力高报警","C.M.RO4_PT_CS@H_AL"]
["RO4产水压力高报警开关","C.M.RO4_PT_CS@H_AL_ON"]
["RO4产水压力高限设置","C.M.RO4_PT_CS@H_AL_set"]
["RO4产水压力低报警","C.M.RO4_PT_CS@L_AL"]
["RO4产水压力低报警开关","C.M.RO4_PT_CS@L_AL_ON"]
["RO4产水压力低限设置","C.M.RO4_PT_CS@L_AL_set"]
["RO4产水压力","C.M.RO4_PT_CS@out"]
["RO4一段浓水压力报警","C.M.RO4_PT_DJ1@fault"]
["RO4一段浓水压力高报警","C.M.RO4_PT_DJ1@H_AL"]
["RO4一段浓水压力高报警开关","C.M.RO4_PT_DJ1@H_AL_ON"]
["RO4一段浓水压力高限设置","C.M.RO4_PT_DJ1@H_AL_set"]
["RO4一段浓水压力低报警","C.M.RO4_PT_DJ1@L_AL"]
["RO4一段浓水压力低报警开关","C.M.RO4_PT_DJ1@L_AL_ON"]
["RO4一段浓水压力低限设置","C.M.RO4_PT_DJ1@L_AL_set"]
["RO4一段浓水压力","C.M.RO4_PT_DJ1@out"]
["RO4二段进水压力报警","C.M.RO4_PT_DJ2@fault"]
["RO4二段进水压力高报警","C.M.RO4_PT_DJ2@H_AL"]
["RO4二段进水压力高报警开关","C.M.RO4_PT_DJ2@H_AL_ON"]
["RO4二段进水压力高限设置","C.M.RO4_PT_DJ2@H_AL_set"]
["RO4二段进水压力低报警","C.M.RO4_PT_DJ2@L_AL"]
["RO4二段进水压力低报警开关","C.M.RO4_PT_DJ2@L_AL_ON"]
["RO4二段进水压力低限设置","C.M.RO4_PT_DJ2@L_AL_set"]
["RO4二段进水压力","C.M.RO4_PT_DJ2@out"]
["RO4一段进水压力报警","C.M.RO4_PT_JS@fault"]
["RO4一段进水压力高报警","C.M.RO4_PT_JS@H_AL"]
["RO4一段进水压力高报警开关","C.M.RO4_PT_JS@H_AL_ON"]
["RO4一段进水压力高限设置","C.M.RO4_PT_JS@H_AL_set"]
["RO4一段进水压力低报警","C.M.RO4_PT_JS@L_AL"]
["RO4一段进水压力低报警开关","C.M.RO4_PT_JS@L_AL_ON"]
["RO4一段进水压力低限设置","C.M.RO4_PT_JS@L_AL_set"]
["RO4一段进水压力","C.M.RO4_PT_JS@out"]
["RO4二段浓水压力报警","C.M.RO4_PT_NS@fault"]
["RO4二段浓水压力高报警","C.M.RO4_PT_NS@H_AL"]
["RO4二段浓水压力高报警开关","C.M.RO4_PT_NS@H_AL_ON"]
["RO4二段浓水压力高限设置","C.M.RO4_PT_NS@H_AL_set"]
["RO4二段浓水压力低报警","C.M.RO4_PT_NS@L_AL"]
["RO4二段浓水压力低报警开关","C.M.RO4_PT_NS@L_AL_ON"]
["RO4二段浓水压力低限设置","C.M.RO4_PT_NS@L_AL_set"]
["RO4二段浓水压力","C.M.RO4_PT_NS@out"]
["RO4未知阀手自动","C.M.RO4_SJJF@auto_select"]
["RO4未知阀关操作","C.M.RO4_SJJF@close"]
["RO4未知阀关到位","C.M.RO4_SJJF@close_feedback"]
["RO4未知阀故障","C.M.RO4_SJJF@fault_total"]
["RO4未知阀开操作","C.M.RO4_SJJF@open"]
["RO4未知阀开到位","C.M.RO4_SJJF@open_feedback"]
["RO4未知阀远程","C.M.RO4_SJJF@rem"]
["RO4未知阀复位","C.M.RO4_SJJF@reset"]
["4#阻垢剂加药阀手自动","C.M.RO4_ZGJF@auto_select"]
["4#阻垢剂加药阀关操作","C.M.RO4_ZGJF@close"]
["4#阻垢剂加药阀关到位","C.M.RO4_ZGJF@close_feedback"]
["4#阻垢剂加药阀故障","C.M.RO4_ZGJF@fault_total"]
["4#阻垢剂加药阀开操作","C.M.RO4_ZGJF@open"]
["4#阻垢剂加药阀开到位","C.M.RO4_ZGJF@open_feedback"]
["4#阻垢剂加药阀远程","C.M.RO4_ZGJF@rem"]
["4#阻垢剂加药阀复位","C.M.RO4_ZGJF@reset"]
["1#杀菌剂加药泵手自动","C.M.SJJB1@auto_select"]
["1#杀菌剂加药泵故障","C.M.SJJB1@fault_total"]
["1#杀菌剂加药泵远程","C.M.SJJB1@rem"]
["1#杀菌剂加药泵复位","C.M.SJJB1@reset"]
["1#杀菌剂加药泵运行","C.M.SJJB1@run"]
["1#杀菌剂加药泵运行时间","C.M.SJJB1@run_time"]
["1#杀菌剂加药泵启动操作","C.M.SJJB1@start"]
["1#杀菌剂加药泵停止操作","C.M.SJJB1@stop"]
["2#杀菌剂加药泵手自动","C.M.SJJB2@auto_select"]
["2#杀菌剂加药泵故障","C.M.SJJB2@fault_total"]
["2#杀菌剂加药泵远程","C.M.SJJB2@rem"]
["2#杀菌剂加药泵复位","C.M.SJJB2@reset"]
["2#杀菌剂加药泵运行","C.M.SJJB2@run"]
["2#杀菌剂加药泵运行时间","C.M.SJJB2@run_time"]
["2#杀菌剂加药泵启动操作","C.M.SJJB2@start"]
["2#杀菌剂加药泵停止操作","C.M.SJJB2@stop"]
["CIP-温度报警","C.M.TT_CIP@fault"]
["CIP-温度高报警","C.M.TT_CIP@H_AL"]
["CIP-温度高报警开关","C.M.TT_CIP@H_AL_ON"]
["CIP-温度高限设置","C.M.TT_CIP@H_AL_set"]
["CIP-温度低报警","C.M.TT_CIP@L_AL"]
["CIP-温度低报警开关","C.M.TT_CIP@L_AL_ON"]
["CIP-温度低限设置","C.M.TT_CIP@L_AL_set"]
["CIP-温度","C.M.TT_CIP@out"]
["1#脱碳风机手自动","C.M.TTFJ1@auto_select"]
["1#脱碳风机故障","C.M.TTFJ1@fault_total"]
["1#脱碳风机远程","C.M.TTFJ1@rem"]
["1#脱碳风机复位","C.M.TTFJ1@reset"]
["1#脱碳风机运行","C.M.TTFJ1@run"]
["1#脱碳风机运行时间","C.M.TTFJ1@run_time"]
["1#脱碳风机启动操作","C.M.TTFJ1@start"]
["1#脱碳风机停止操作","C.M.TTFJ1@stop"]
["2#脱碳风机手自动","C.M.TTFJ2@auto_select"]
["2#脱碳风机故障","C.M.TTFJ2@fault_total"]
["2#脱碳风机远程","C.M.TTFJ2@rem"]
["2#脱碳风机复位","C.M.TTFJ2@reset"]
["2#脱碳风机运行","C.M.TTFJ2@run"]
["2#脱碳风机运行时间","C.M.TTFJ2@run_time"]
["2#脱碳风机启动操作","C.M.TTFJ2@start"]
["2#脱碳风机停止操作","C.M.TTFJ2@stop"]
["UFCEB排放阀手自动","C.M.UF_CEBPF@auto_select"]
["UFCEB排放阀关操作","C.M.UF_CEBPF@close"]
["UFCEB排放阀关到位","C.M.UF_CEBPF@close_feedback"]
["UFCEB排放阀故障","C.M.UF_CEBPF@fault_total"]
["UFCEB排放阀开操作","C.M.UF_CEBPF@open"]
["UFCEB排放阀开到位","C.M.UF_CEBPF@open_feedback"]
["UFCEB排放阀远程","C.M.UF_CEBPF@rem"]
["UFCEB排放阀复位","C.M.UF_CEBPF@reset"]
["超滤总产水余氯报警","C.M.UF_Cl_ZCS@fault"]
["超滤总产水余氯高报警","C.M.UF_Cl_ZCS@H_AL"]
["超滤总产水余氯高报警开关","C.M.UF_Cl_ZCS@H_AL_ON"]
["超滤总产水余氯高限设置","C.M.UF_Cl_ZCS@H_AL_set"]
["超滤总产水余氯低报警","C.M.UF_Cl_ZCS@L_AL"]
["超滤总产水余氯低报警开关","C.M.UF_Cl_ZCS@L_AL_ON"]
["超滤总产水余氯低限设置","C.M.UF_Cl_ZCS@L_AL_set"]
["超滤总产水余氯","C.M.UF_Cl_ZCS@out"]
["UF排气阀手自动","C.M.UF_CSPQF@auto_select"]
["UF排气阀关操作","C.M.UF_CSPQF@close"]
["UF排气阀关到位","C.M.UF_CSPQF@close_feedback"]
["UF排气阀故障","C.M.UF_CSPQF@fault_total"]
["UF排气阀开操作","C.M.UF_CSPQF@open"]
["UF排气阀开到位","C.M.UF_CSPQF@open_feedback"]
["UF排气阀远程","C.M.UF_CSPQF@rem"]
["UF排气阀复位","C.M.UF_CSPQF@reset"]
["超滤反洗流量报警","C.M.UF_FT_FX@fault"]
["超滤反洗流量高报警","C.M.UF_FT_FX@H_AL"]
["超滤反洗流量高报警开关","C.M.UF_FT_FX@H_AL_ON"]
["超滤反洗流量高限设置","C.M.UF_FT_FX@H_AL_set"]
["超滤反洗流量低报警","C.M.UF_FT_FX@L_AL"]
["超滤反洗流量低报警开关","C.M.UF_FT_FX@L_AL_ON"]
["超滤反洗流量低限设置","C.M.UF_FT_FX@L_AL_set"]
["超滤反洗流量","C.M.UF_FT_FX@out"]
["超滤总产水流量报警","C.M.UF_FT_ZCS@fault"]
["超滤总产水流量高报警","C.M.UF_FT_ZCS@H_AL"]
["超滤总产水流量高报警开关","C.M.UF_FT_ZCS@H_AL_ON"]
["超滤总产水流量高限设置","C.M.UF_FT_ZCS@H_AL_set"]
["超滤总产水流量低报警","C.M.UF_FT_ZCS@L_AL"]
["超滤总产水流量低报警开关","C.M.UF_FT_ZCS@L_AL_ON"]
["超滤总产水流量低限设置","C.M.UF_FT_ZCS@L_AL_set"]
["超滤总产水流量","C.M.UF_FT_ZCS@out"]
["超滤反洗排队1","C.M.UF_FXB_line_DB@queue[1]"]
["超滤反洗排队2","C.M.UF_FXB_line_DB@queue[2]"]
["超滤反洗排队3","C.M.UF_FXB_line_DB@queue[3]"]
["超滤反洗排队4","C.M.UF_FXB_line_DB@queue[4]"]
["超滤反洗泵定频率-反洗","C.M.UF_FXB_pid_man1"]
["超滤反洗泵定频率-加药","C.M.UF_FXB_pid_man2"]
["超滤反洗泵流量PID/定频率按钮","C.M.UF_FXB_pid_on"]
["1#超滤反洗水泵手自动","C.M.UF_FXB1@auto_select"]
["1#超滤反洗水泵故障","C.M.UF_FXB1@fault_total"]
["1#超滤反洗水泵远程","C.M.UF_FXB1@rem"]
["1#超滤反洗水泵复位","C.M.UF_FXB1@reset"]
["1#超滤反洗水泵运行","C.M.UF_FXB1@run"]
["1#超滤反洗水泵运行时间","C.M.UF_FXB1@run_time"]
["1#超滤反洗水泵启动操作","C.M.UF_FXB1@start"]
["1#超滤反洗水泵停止操作","C.M.UF_FXB1@stop"]
["1#超滤反洗水泵电流报警","C.M.UF_FXB1_A@Fault"]
["1#超滤反洗水泵电流高报警","C.M.UF_FXB1_A@H_AL"]
["1#超滤反洗水泵电流高报警开关","C.M.UF_FXB1_A@H_AL_ON"]
["1#超滤反洗水泵电流高限设置","C.M.UF_FXB1_A@H_AL_set"]
["1#超滤反洗水泵电流低报警","C.M.UF_FXB1_A@L_AL"]
["1#超滤反洗水泵电流低报警开关","C.M.UF_FXB1_A@L_AL_ON"]
["1#超滤反洗水泵电流低限设置","C.M.UF_FXB1_A@L_AL_set"]
["1#超滤反洗水泵运行电流","C.M.UF_FXB1_A@out"]
["1#超滤反洗水泵设置频率","C.M.UF_FXB1_AO_FB@spare"]
["1#超滤反洗水泵频率报警","C.M.UF_FXB1_fre@Fault"]
["1#超滤反洗水泵频率高报警","C.M.UF_FXB1_fre@H_AL"]
["1#超滤反洗水泵频率高报警开关","C.M.UF_FXB1_fre@H_AL_ON"]
["1#超滤反洗水泵频率高限设置","C.M.UF_FXB1_fre@H_AL_set"]
["1#超滤反洗水泵频率低报警","C.M.UF_FXB1_fre@L_AL"]
["1#超滤反洗水泵频率低报警开关","C.M.UF_FXB1_fre@L_AL_ON"]
["1#超滤反洗水泵频率低限设置","C.M.UF_FXB1_fre@L_AL_set"]
["1#超滤反洗水泵运行频率","C.M.UF_FXB1_fre@out"]
["2#超滤反洗水泵手自动","C.M.UF_FXB2@auto_select"]
["2#超滤反洗水泵故障","C.M.UF_FXB2@fault_total"]
["2#超滤反洗水泵远程","C.M.UF_FXB2@rem"]
["2#超滤反洗水泵复位","C.M.UF_FXB2@reset"]
["2#超滤反洗水泵运行","C.M.UF_FXB2@run"]
["2#超滤反洗水泵运行时间","C.M.UF_FXB2@run_time"]
["2#超滤反洗水泵启动操作","C.M.UF_FXB2@start"]
["2#超滤反洗水泵停止操作","C.M.UF_FXB2@stop"]
["2#超滤反洗水泵电流报警","C.M.UF_FXB2_A@Fault"]
["2#超滤反洗水泵电流高报警","C.M.UF_FXB2_A@H_AL"]
["2#超滤反洗水泵电流高报警开关","C.M.UF_FXB2_A@H_AL_ON"]
["2#超滤反洗水泵电流高限设置","C.M.UF_FXB2_A@H_AL_set"]
["2#超滤反洗水泵电流低报警","C.M.UF_FXB2_A@L_AL"]
["2#超滤反洗水泵电流低报警开关","C.M.UF_FXB2_A@L_AL_ON"]
["2#超滤反洗水泵电流低限设置","C.M.UF_FXB2_A@L_AL_set"]
["2#超滤反洗水泵运行电流","C.M.UF_FXB2_A@out"]
["2#超滤反洗水泵设置频率","C.M.UF_FXB2_AO_FB@spare"]
["2#超滤反洗水泵频率报警","C.M.UF_FXB2_fre@Fault"]
["2#超滤反洗水泵频率高报警","C.M.UF_FXB2_fre@H_AL"]
["2#超滤反洗水泵频率高报警开关","C.M.UF_FXB2_fre@H_AL_ON"]
["2#超滤反洗水泵频率高限设置","C.M.UF_FXB2_fre@H_AL_set"]
["2#超滤反洗水泵频率低报警","C.M.UF_FXB2_fre@L_AL"]
["2#超滤反洗水泵频率低报警开关","C.M.UF_FXB2_fre@L_AL_ON"]
["2#超滤反洗水泵频率低限设置","C.M.UF_FXB2_fre@L_AL_set"]
["2#超滤反洗水泵运行频率","C.M.UF_FXB2_fre@out"]
["3#超滤反洗水泵手自动","C.M.UF_FXB3@auto_select"]
["3#超滤反洗水泵故障","C.M.UF_FXB3@fault_total"]
["3#超滤反洗水泵远程","C.M.UF_FXB3@rem"]
["3#超滤反洗水泵复位","C.M.UF_FXB3@reset"]
["3#超滤反洗水泵运行","C.M.UF_FXB3@run"]
["3#超滤反洗水泵运行时间","C.M.UF_FXB3@run_time"]
["3#超滤反洗水泵启动操作","C.M.UF_FXB3@start"]
["3#超滤反洗水泵停止操作","C.M.UF_FXB3@stop"]
["3#超滤反洗水泵电流报警","C.M.UF_FXB3_A@Fault"]
["3#超滤反洗水泵电流高报警","C.M.UF_FXB3_A@H_AL"]
["3#超滤反洗水泵电流高报警开关","C.M.UF_FXB3_A@H_AL_ON"]
["3#超滤反洗水泵电流高限设置","C.M.UF_FXB3_A@H_AL_set"]
["3#超滤反洗水泵电流低报警","C.M.UF_FXB3_A@L_AL"]
["3#超滤反洗水泵电流低报警开关","C.M.UF_FXB3_A@L_AL_ON"]
["3#超滤反洗水泵电流低限设置","C.M.UF_FXB3_A@L_AL_set"]
["3#超滤反洗水泵运行电流","C.M.UF_FXB3_A@out"]
["3#超滤反洗水泵设置频率","C.M.UF_FXB3_AO_FB@spare"]
["3#超滤反洗水泵频率报警","C.M.UF_FXB3_fre@Fault"]
["3#超滤反洗水泵频率高报警","C.M.UF_FXB3_fre@H_AL"]
["3#超滤反洗水泵频率高报警开关","C.M.UF_FXB3_fre@H_AL_ON"]
["3#超滤反洗水泵频率高限设置","C.M.UF_FXB3_fre@H_AL_set"]
["3#超滤反洗水泵频率低报警","C.M.UF_FXB3_fre@L_AL"]
["3#超滤反洗水泵频率低报警开关","C.M.UF_FXB3_fre@L_AL_ON"]
["3#超滤反洗水泵频率低限设置","C.M.UF_FXB3_fre@L_AL_set"]
["3#超滤反洗水泵运行频率","C.M.UF_FXB3_fre@out"]
["UF反洗排水阀手自动","C.M.UF_FXPF@auto_select"]
["UF反洗排水阀关操作","C.M.UF_FXPF@close"]
["UF反洗排水阀关到位","C.M.UF_FXPF@close_feedback"]
["UF反洗排水阀故障","C.M.UF_FXPF@fault_total"]
["UF反洗排水阀开操作","C.M.UF_FXPF@open"]
["UF反洗排水阀开到位","C.M.UF_FXPF@open_feedback"]
["UF反洗排水阀远程","C.M.UF_FXPF@rem"]
["UF反洗排水阀复位","C.M.UF_FXPF@reset"]
["反洗水池补水阀开度设定值","C.M.UF_FXSCBSF_AO_FB@spare"]
["反洗水池补水阀手自动","C.M.UF_FXSCBSF_auto_set"]
["反洗水池补水阀开度报警","C.M.UF_FXSCBSF_kd@fault"]
["反洗水池补水阀开度高报警","C.M.UF_FXSCBSF_kd@H_AL"]
["反洗水池补水阀开度高报警开关","C.M.UF_FXSCBSF_kd@H_AL_ON"]
["反洗水池补水阀开度高限设置","C.M.UF_FXSCBSF_kd@H_AL_set"]
["反洗水池补水阀开度低报警","C.M.UF_FXSCBSF_kd@L_AL"]
["反洗水池补水阀开度低报警开关","C.M.UF_FXSCBSF_kd@L_AL_ON"]
["反洗水池补水阀开度低限设置","C.M.UF_FXSCBSF_kd@L_AL_set"]
["反洗水池补水阀开度","C.M.UF_FXSCBSF_kd@out"]
["1套超滤1-3#供水泵设置频率","C.M.UF_GSB_fre_set[0]"]
["2套超滤1-3#供水泵设置频率","C.M.UF_GSB_fre_set[1]"]
["3套超滤1-3#供水泵设置频率","C.M.UF_GSB_fre_set[2]"]
["4套超滤1-3#供水泵设置频率","C.M.UF_GSB_fre_set[3]"]
["供水泵PID/定频控制","C.M.UF_GSB_pid_on"]
["1套超滤供水泵启动台数设置","C.M.UF_GSB_qua_set[0]"]
["2套超滤供水泵启动台数设置","C.M.UF_GSB_qua_set[1]"]
["3套超滤供水泵启动台数设置","C.M.UF_GSB_qua_set[2]"]
["4套超滤供水泵启动台数设置","C.M.UF_GSB_qua_set[3]"]
["1#超滤供水泵手自动","C.M.UF_GSB1@auto_select"]
["1#超滤供水泵故障","C.M.UF_GSB1@fault_total"]
["1#超滤供水泵远程","C.M.UF_GSB1@rem"]
["1#超滤供水泵复位","C.M.UF_GSB1@reset"]
["1#超滤供水泵运行","C.M.UF_GSB1@run"]
["1#超滤供水泵运行时间","C.M.UF_GSB1@run_time"]
["1#超滤供水泵启动操作","C.M.UF_GSB1@start"]
["1#超滤供水泵停止操作","C.M.UF_GSB1@stop"]
["1#超滤供水泵电流报警","C.M.UF_GSB1_A@Fault"]
["1#超滤供水泵电流高报警","C.M.UF_GSB1_A@H_AL"]
["1#超滤供水泵电流高报警开关","C.M.UF_GSB1_A@H_AL_ON"]
["1#超滤供水泵电流高限设置","C.M.UF_GSB1_A@H_AL_set"]
["1#超滤供水泵电流低报警","C.M.UF_GSB1_A@L_AL"]
["1#超滤供水泵电流低报警开关","C.M.UF_GSB1_A@L_AL_ON"]
["1#超滤供水泵电流低限设置","C.M.UF_GSB1_A@L_AL_set"]
["1#超滤供水泵运行电流","C.M.UF_GSB1_A@out"]
["1#超滤供水泵设置频率","C.M.UF_GSB1_AO_FB@spare"]
["1#超滤供水泵频率报警","C.M.UF_GSB1_fre@Fault"]
["1#超滤供水泵频率高报警","C.M.UF_GSB1_fre@H_AL"]
["1#超滤供水泵频率高报警开关","C.M.UF_GSB1_fre@H_AL_ON"]
["1#超滤供水泵频率高限设置","C.M.UF_GSB1_fre@H_AL_set"]
["1#超滤供水泵频率低报警","C.M.UF_GSB1_fre@L_AL"]
["1#超滤供水泵频率低报警开关","C.M.UF_GSB1_fre@L_AL_ON"]
["1#超滤供水泵频率低限设置","C.M.UF_GSB1_fre@L_AL_set"]
["1#超滤供水泵运行频率","C.M.UF_GSB1_fre@out"]
["2#超滤供水泵手自动","C.M.UF_GSB2@auto_select"]
["2#超滤供水泵故障","C.M.UF_GSB2@fault_total"]
["2#超滤供水泵远程","C.M.UF_GSB2@rem"]
["2#超滤供水泵复位","C.M.UF_GSB2@reset"]
["2#超滤供水泵运行","C.M.UF_GSB2@run"]
["2#超滤供水泵运行时间","C.M.UF_GSB2@run_time"]
["2#超滤供水泵启动操作","C.M.UF_GSB2@start"]
["2#超滤供水泵停止操作","C.M.UF_GSB2@stop"]
["2#超滤供水泵电流报警","C.M.UF_GSB2_A@Fault"]
["2#超滤供水泵电流高报警","C.M.UF_GSB2_A@H_AL"]
["2#超滤供水泵电流高报警开关","C.M.UF_GSB2_A@H_AL_ON"]
["2#超滤供水泵电流高限设置","C.M.UF_GSB2_A@H_AL_set"]
["2#超滤供水泵电流低报警","C.M.UF_GSB2_A@L_AL"]
["2#超滤供水泵电流低报警开关","C.M.UF_GSB2_A@L_AL_ON"]
["2#超滤供水泵电流低限设置","C.M.UF_GSB2_A@L_AL_set"]
["2#超滤供水泵运行电流","C.M.UF_GSB2_A@out"]
["2#超滤供水泵设置频率","C.M.UF_GSB2_AO_FB@spare"]
["2#超滤供水泵频率报警","C.M.UF_GSB2_fre@Fault"]
["2#超滤供水泵频率高报警","C.M.UF_GSB2_fre@H_AL"]
["2#超滤供水泵频率高报警开关","C.M.UF_GSB2_fre@H_AL_ON"]
["2#超滤供水泵频率高限设置","C.M.UF_GSB2_fre@H_AL_set"]
["2#超滤供水泵频率低报警","C.M.UF_GSB2_fre@L_AL"]
["2#超滤供水泵频率低报警开关","C.M.UF_GSB2_fre@L_AL_ON"]
["2#超滤供水泵频率低限设置","C.M.UF_GSB2_fre@L_AL_set"]
["2#超滤供水泵运行频率","C.M.UF_GSB2_fre@out"]
["3#超滤供水泵手自动","C.M.UF_GSB3@auto_select"]
["3#超滤供水泵故障","C.M.UF_GSB3@fault_total"]
["3#超滤供水泵远程","C.M.UF_GSB3@rem"]
["3#超滤供水泵复位","C.M.UF_GSB3@reset"]
["3#超滤供水泵运行","C.M.UF_GSB3@run"]
["3#超滤供水泵运行时间","C.M.UF_GSB3@run_time"]
["3#超滤供水泵启动操作","C.M.UF_GSB3@start"]
["3#超滤供水泵停止操作","C.M.UF_GSB3@stop"]
["3#超滤供水泵电流报警","C.M.UF_GSB3_A@Fault"]
["3#超滤供水泵电流高报警","C.M.UF_GSB3_A@H_AL"]
["3#超滤供水泵电流高报警开关","C.M.UF_GSB3_A@H_AL_ON"]
["3#超滤供水泵电流高限设置","C.M.UF_GSB3_A@H_AL_set"]
["3#超滤供水泵电流低报警","C.M.UF_GSB3_A@L_AL"]
["3#超滤供水泵电流低报警开关","C.M.UF_GSB3_A@L_AL_ON"]
["3#超滤供水泵电流低限设置","C.M.UF_GSB3_A@L_AL_set"]
["3#超滤供水泵运行电流","C.M.UF_GSB3_A@out"]
["3#超滤供水泵设置频率","C.M.UF_GSB3_AO_FB@spare"]
["3#超滤供水泵频率报警","C.M.UF_GSB3_fre@Fault"]
["3#超滤供水泵频率高报警","C.M.UF_GSB3_fre@H_AL"]
["3#超滤供水泵频率高报警开关","C.M.UF_GSB3_fre@H_AL_ON"]
["3#超滤供水泵频率高限设置","C.M.UF_GSB3_fre@H_AL_set"]
["3#超滤供水泵频率低报警","C.M.UF_GSB3_fre@L_AL"]
["3#超滤供水泵频率低报警开关","C.M.UF_GSB3_fre@L_AL_ON"]
["3#超滤供水泵频率低限设置","C.M.UF_GSB3_fre@L_AL_set"]
["3#超滤供水泵运行频率","C.M.UF_GSB3_fre@out"]
["4#超滤供水泵手自动","C.M.UF_GSB4@auto_select"]
["4#超滤供水泵故障","C.M.UF_GSB4@fault_total"]
["4#超滤供水泵远程","C.M.UF_GSB4@rem"]
["4#超滤供水泵复位","C.M.UF_GSB4@reset"]
["4#超滤供水泵运行","C.M.UF_GSB4@run"]
["4#超滤供水泵运行时间","C.M.UF_GSB4@run_time"]
["4#超滤供水泵启动操作","C.M.UF_GSB4@start"]
["4#超滤供水泵停止操作","C.M.UF_GSB4@stop"]
["4#超滤供水泵电流报警","C.M.UF_GSB4_A@Fault"]
["4#超滤供水泵电流高报警","C.M.UF_GSB4_A@H_AL"]
["4#超滤供水泵电流高报警开关","C.M.UF_GSB4_A@H_AL_ON"]
["4#超滤供水泵电流高限设置","C.M.UF_GSB4_A@H_AL_set"]
["4#超滤供水泵电流低报警","C.M.UF_GSB4_A@L_AL"]
["4#超滤供水泵电流低报警开关","C.M.UF_GSB4_A@L_AL_ON"]
["4#超滤供水泵电流低限设置","C.M.UF_GSB4_A@L_AL_set"]
["4#超滤供水泵运行电流","C.M.UF_GSB4_A@out"]
["4#超滤供水泵设置频率","C.M.UF_GSB4_AO_FB@spare"]
["4#超滤供水泵频率报警","C.M.UF_GSB4_fre@Fault"]
["4#超滤供水泵频率高报警","C.M.UF_GSB4_fre@H_AL"]
["4#超滤供水泵频率高报警开关","C.M.UF_GSB4_fre@H_AL_ON"]
["4#超滤供水泵频率高限设置","C.M.UF_GSB4_fre@H_AL_set"]
["4#超滤供水泵频率低报警","C.M.UF_GSB4_fre@L_AL"]
["4#超滤供水泵频率低报警开关","C.M.UF_GSB4_fre@L_AL_ON"]
["4#超滤供水泵频率低限设置","C.M.UF_GSB4_fre@L_AL_set"]
["4#超滤供水泵运行频率","C.M.UF_GSB4_fre@out"]
["3套超滤4#供水泵设置频率","C.M.UF_GSB4_fre_set1"]
["4套超滤4#供水泵设置频率","C.M.UF_GSB4_fre_set2"]
["进水池NaClO加药阀手自动","C.M.UF_JS_NaClO@auto_select"]
["进水池NaClO加药阀关操作","C.M.UF_JS_NaClO@close"]
["进水池NaClO加药阀关到位","C.M.UF_JS_NaClO@close_feedback"]
["进水池NaClO加药阀故障","C.M.UF_JS_NaClO@fault_total"]
["进水池NaClO加药阀开操作","C.M.UF_JS_NaClO@open"]
["进水池NaClO加药阀开到位","C.M.UF_JS_NaClO@open_feedback"]
["进水池NaClO加药阀远程","C.M.UF_JS_NaClO@rem"]
["进水池NaClO加药阀复位","C.M.UF_JS_NaClO@reset"]
["超滤总产水ORP报警","C.M.UF_ORP_ZCS@fault"]
["超滤总产水ORP高报警","C.M.UF_ORP_ZCS@H_AL"]
["超滤总产水ORP高报警开关","C.M.UF_ORP_ZCS@H_AL_ON"]
["超滤总产水ORP高限设置","C.M.UF_ORP_ZCS@H_AL_set"]
["超滤总产水ORP低报警","C.M.UF_ORP_ZCS@L_AL"]
["超滤总产水ORP低报警开关","C.M.UF_ORP_ZCS@L_AL_ON"]
["超滤总产水ORP低限设置","C.M.UF_ORP_ZCS@L_AL_set"]
["超滤总产水ORP","C.M.UF_ORP_ZCS@out"]
["絮凝剂加药阀手自动","C.M.UF_PAC@auto_select"]
["絮凝剂加药阀关操作","C.M.UF_PAC@close"]
["絮凝剂加药阀关到位","C.M.UF_PAC@close_feedback"]
["絮凝剂加药阀故障","C.M.UF_PAC@fault_total"]
["絮凝剂加药阀开操作","C.M.UF_PAC@open"]
["絮凝剂加药阀开到位","C.M.UF_PAC@open_feedback"]
["絮凝剂加药阀远程","C.M.UF_PAC@rem"]
["絮凝剂加药阀复位","C.M.UF_PAC@reset"]
["超滤总产水PH报警","C.M.UF_PH_ZCS@fault"]
["超滤总产水PH高报警","C.M.UF_PH_ZCS@H_AL"]
["超滤总产水PH高报警开关","C.M.UF_PH_ZCS@H_AL_ON"]
["超滤总产水PH高限设置","C.M.UF_PH_ZCS@H_AL_set"]
["超滤总产水PH低报警","C.M.UF_PH_ZCS@L_AL"]
["超滤总产水PH低报警开关","C.M.UF_PH_ZCS@L_AL_ON"]
["超滤总产水PH低限设置","C.M.UF_PH_ZCS@L_AL_set"]
["超滤总产水PH","C.M.UF_PH_ZCS@out"]
["超滤反洗压力报警","C.M.UF_PT_FX@fault"]
["超滤反洗压力高报警","C.M.UF_PT_FX@H_AL"]
["超滤反洗压力高报警开关","C.M.UF_PT_FX@H_AL_ON"]
["超滤反洗压力高限设置","C.M.UF_PT_FX@H_AL_set"]
["超滤反洗压力低报警","C.M.UF_PT_FX@L_AL"]
["超滤反洗压力低报警开关","C.M.UF_PT_FX@L_AL_ON"]
["超滤反洗压力低限设置","C.M.UF_PT_FX@L_AL_set"]
["超滤反洗压力","C.M.UF_PT_FX@out"]
["超滤总产水压力报警","C.M.UF_PT_ZCS@fault"]
["超滤总产水压力高报警","C.M.UF_PT_ZCS@H_AL"]
["超滤总产水压力高报警开关","C.M.UF_PT_ZCS@H_AL_ON"]
["超滤总产水压力高限设置","C.M.UF_PT_ZCS@H_AL_set"]
["超滤总产水压力低报警","C.M.UF_PT_ZCS@L_AL"]
["超滤总产水压力低报警开关","C.M.UF_PT_ZCS@L_AL_ON"]
["超滤总产水压力低限设置","C.M.UF_PT_ZCS@L_AL_set"]
["超滤总产水压力","C.M.UF_PT_ZCS@out"]
["超滤总进水压力报警","C.M.UF_PT_ZJS@fault"]
["超滤总进水压力高报警","C.M.UF_PT_ZJS@H_AL"]
["超滤总进水压力高报警开关","C.M.UF_PT_ZJS@H_AL_ON"]
["超滤总进水压力高限设置","C.M.UF_PT_ZJS@H_AL_set"]
["超滤总进水压力低报警","C.M.UF_PT_ZJS@L_AL"]
["超滤总进水压力低报警开关","C.M.UF_PT_ZJS@L_AL_ON"]
["超滤总进水压力低限设置","C.M.UF_PT_ZJS@L_AL_set"]
["超滤总进水压力","C.M.UF_PT_ZJS@out"]
["超滤总产水浊度报警","C.M.UF_Tur_ZCS@fault"]
["超滤总产水浊度高报警","C.M.UF_Tur_ZCS@H_AL"]
["超滤总产水浊度高报警开关","C.M.UF_Tur_ZCS@H_AL_ON"]
["超滤总产水浊度高限设置","C.M.UF_Tur_ZCS@H_AL_set"]
["超滤总产水浊度低报警","C.M.UF_Tur_ZCS@L_AL"]
["超滤总产水浊度低报警开关","C.M.UF_Tur_ZCS@L_AL_ON"]
["超滤总产水浊度低限设置","C.M.UF_Tur_ZCS@L_AL_set"]
["超滤总产水浊度","C.M.UF_Tur_ZCS@out"]
["超滤总进水浊度报警","C.M.UF_Tur_ZJS@fault"]
["超滤总进水浊度高报警","C.M.UF_Tur_ZJS@H_AL"]
["超滤总进水浊度高报警开关","C.M.UF_Tur_ZJS@H_AL_ON"]
["超滤总进水浊度高限设置","C.M.UF_Tur_ZJS@H_AL_set"]
["超滤总进水浊度低报警","C.M.UF_Tur_ZJS@L_AL"]
["超滤总进水浊度低报警开关","C.M.UF_Tur_ZJS@L_AL_ON"]
["超滤总进水浊度低限设置","C.M.UF_Tur_ZJS@L_AL_set"]
["超滤总进水浊度","C.M.UF_Tur_ZJS@out"]
["UF1不合格水阀手自动","C.M.UF1_BHGF@auto_select"]
["UF1不合格水阀关操作","C.M.UF1_BHGF@close"]
["UF1不合格水阀关到位","C.M.UF1_BHGF@close_feedback"]
["UF1不合格水阀故障","C.M.UF1_BHGF@fault_total"]
["UF1不合格水阀开操作","C.M.UF1_BHGF@open"]
["UF1不合格水阀开到位","C.M.UF1_BHGF@open_feedback"]
["UF1不合格水阀远程","C.M.UF1_BHGF@rem"]
["UF1不合格水阀复位","C.M.UF1_BHGF@reset"]
["UF1产水阀手自动","C.M.UF1_CSF@auto_select"]
["UF1产水阀关操作","C.M.UF1_CSF@close"]
["UF1产水阀关到位","C.M.UF1_CSF@close_feedback"]
["UF1产水阀故障","C.M.UF1_CSF@fault_total"]
["UF1产水阀开操作","C.M.UF1_CSF@open"]
["UF1产水阀开到位","C.M.UF1_CSF@open_feedback"]
["UF1产水阀远程","C.M.UF1_CSF@rem"]
["UF1产水阀复位","C.M.UF1_CSF@reset"]
["UF1右侧排空阀手自动","C.M.UF1_CSPKF@auto_select"]
["UF1右侧排空阀关操作","C.M.UF1_CSPKF@close"]
["UF1右侧排空阀关到位","C.M.UF1_CSPKF@close_feedback"]
["UF1右侧排空阀故障","C.M.UF1_CSPKF@fault_total"]
["UF1右侧排空阀开操作","C.M.UF1_CSPKF@open"]
["UF1右侧排空阀开到位","C.M.UF1_CSPKF@open_feedback"]
["UF1右侧排空阀远程","C.M.UF1_CSPKF@rem"]
["UF1右侧排空阀复位","C.M.UF1_CSPKF@reset"]
["UF1不合格冲洗","C.M.UF1_DB@BHG_residue"]
["UF1紧急停车","C.M.UF1_DB@button[00]"]
["UF1半自动开机","C.M.UF1_DB@button[01]"]
["UF1半自动停止","C.M.UF1_DB@button[02]"]
["UF1半自动反洗","C.M.UF1_DB@button[03]"]
["UF1半自动CEB","C.M.UF1_DB@button[04]"]
["UF1全自动开机/停止","C.M.UF1_DB@button[08]"]
["UF1CIP启动/停止","C.M.UF1_DB@button[09]"]
["UF1反洗请求（不确定）","C.M.UF1_DB@BW_request"]
["UF1CEB运行中（不确定）","C.M.UF1_DB@CEB_running"]
["UF1药剂残留","C.M.UF1_DB@chemical_residue"]
["UF1CIP完成（不确定）","C.M.UF1_DB@CIP_finish"]
["UF1CIP1选择","C.M.UF1_DB@CIP1_select"]
["UF1CIP2选择","C.M.UF1_DB@CIP2_select"]
["UF1余氯合格设定","C.M.UF1_DB@Cl_low_set"]
["UF1故障信息清除","C.M.UF1_DB@clean_fault"]
["UF1CIP1周期次数显示","C.M.UF1_DB@cycle_CIP1_display"]
["UF1CIP1周期设定","C.M.UF1_DB@cycle_CIP1_SP"]
["UF1CIP2周期次数显示","C.M.UF1_DB@cycle_CIP2_display"]
["UF1CIP2周期设定","C.M.UF1_DB@cycle_CIP2_SP"]
["UF1次数显示（CEB周期）","C.M.UF1_DB@cycle_out"]
["UF1CEB次数设定","C.M.UF1_DB@cycle_sp"]
["UF1故障字","C.M.UF1_DB@Fault_word"]
["UF1反洗流量设定","C.M.UF1_DB@flow_BW_SP"]
["UF1CEB流量设定","C.M.UF1_DB@flow_CEB_wash_SP"]
["UF1过滤流量设定","C.M.UF1_DB@flow_production_SP"]
["UF1液位开关连锁解锁","C.M.UF1_DB@LS_OFF"]
["UF1手动CEB选择（不确定）","C.M.UF1_DB@man_CEB_check"]
["UF1控制模式","C.M.UF1_DB@model_word"]
["UF1跨膜压差高设定","C.M.UF1_DB@press_CEB_SP"]
["UF1跨膜压差超高设定值（不确定）","C.M.UF1_DB@press_hh_SP"]
["UF1跨膜压差","C.M.UF1_DB@press_PV"]
["UF1反洗准备好","C.M.UF1_DB@ready_BW"]
["UF1碱洗准备好","C.M.UF1_DB@ready_CEB1"]
["UF1酸洗准备好","C.M.UF1_DB@ready_CEB2"]
["UF1水洗准备好","C.M.UF1_DB@ready_CEB3"]
["UF1CIP准备好（不确定）","C.M.UF1_DB@ready_CIP"]
["UF1CIP配药装备好","C.M.UF1_DB@ready_CIP_chemical"]
["UF1过滤准备好","C.M.UF1_DB@ready_production"]
["UF1阀门准备好（不确定）","C.M.UF1_DB@ready_valve"]
["UF1提醒字","C.M.UF1_DB@reminder_word"]
["UF1产水累计时间","C.M.UF1_DB@run_time"]
["UF1停机时间","C.M.UF1_DB@stop_time"]
["UF1反洗时间设定","C.M.UF1_DB@time_BW_SP"]
["UF1CEB1加药前冲洗时间设定","C.M.UF1_DB@time_CEB_wash_A"]
["UF1CEB2加药前冲洗时间设定","C.M.UF1_DB@time_CEB_wash_B"]
["UF1正冲时间设定","C.M.UF1_DB@time_CEB_wash_C"]
["UF1CIP时间显示","C.M.UF1_DB@time_CIP_display"]
["UF1CIP1循环时间设定","C.M.UF1_DB@time_CIP_SP1"]
["UF1CIP1浸泡时间设定）","C.M.UF1_DB@time_CIP_SP2"]
["UF1CIP2循环时间设定","C.M.UF1_DB@time_CIP_SP3"]
["UF1CIP2浸泡时间设定","C.M.UF1_DB@time_CIP_SP4"]
["UF1时间显示","C.M.UF1_DB@time_display"]
["UF1CEB1加药时间设定","C.M.UF1_DB@time_Dosing_A"]
["UF1CEB2加药时间设定","C.M.UF1_DB@time_Dosing_B"]
["UF1CEB1冲管时间设定","C.M.UF1_DB@time_Dosing_delay"]
["UF1产水时间设定","C.M.UF1_DB@time_production"]
["UF1产水时间显示","C.M.UF1_DB@time_production_display"]
["UF1CEB1浸泡时间设定","C.M.UF1_DB@time_steep_A"]
["UF1CEB2浸泡时间设定","C.M.UF1_DB@time_steep_B"]
["UF1冲洗A时间（不确定）","C.M.UF1_DB@time_wash_A"]
["UF1正冲进水阀开度设定","C.M.UF1_DB@V_JS_wash_sp"]
["UF1控制字","C.M.UF1_DB@word_control"]
["UF1进水流量报警","C.M.UF1_FT_JS@fault"]
["UF1进水流量高报警","C.M.UF1_FT_JS@H_AL"]
["UF1进水流量高报警开关","C.M.UF1_FT_JS@H_AL_ON"]
["UF1进水流量高限设置","C.M.UF1_FT_JS@H_AL_set"]
["UF1进水流量低报警","C.M.UF1_FT_JS@L_AL"]
["UF1进水流量低报警开关","C.M.UF1_FT_JS@L_AL_ON"]
["UF1进水流量低限设置","C.M.UF1_FT_JS@L_AL_set"]
["UF1进水流量","C.M.UF1_FT_JS@out"]
["UF1反洗进水阀手自动","C.M.UF1_FXJSF@auto_select"]
["UF1反洗进水阀关操作","C.M.UF1_FXJSF@close"]
["UF1反洗进水阀关到位","C.M.UF1_FXJSF@close_feedback"]
["UF1反洗进水阀故障","C.M.UF1_FXJSF@fault_total"]
["UF1反洗进水阀开操作","C.M.UF1_FXJSF@open"]
["UF1反洗进水阀开到位","C.M.UF1_FXJSF@open_feedback"]
["UF1反洗进水阀远程","C.M.UF1_FXJSF@rem"]
["UF1反洗进水阀复位","C.M.UF1_FXJSF@reset"]
["UF1反洗排水阀手自动","C.M.UF1_FXPSF@auto_select"]
["UF1反洗排水阀关操作","C.M.UF1_FXPSF@close"]
["UF1反洗排水阀关到位","C.M.UF1_FXPSF@close_feedback"]
["UF1反洗排水阀故障","C.M.UF1_FXPSF@fault_total"]
["UF1反洗排水阀开操作","C.M.UF1_FXPSF@open"]
["UF1反洗排水阀开到位","C.M.UF1_FXPSF@open_feedback"]
["UF1反洗排水阀远程","C.M.UF1_FXPSF@rem"]
["UF1反洗排水阀复位","C.M.UF1_FXPSF@reset"]
["UF1隔断阀手自动","C.M.UF1_GDF@auto_select"]
["UF1隔断阀关操作","C.M.UF1_GDF@close"]
["UF1隔断阀关到位","C.M.UF1_GDF@close_feedback"]
["UF1隔断阀故障","C.M.UF1_GDF@fault_total"]
["UF1隔断阀开操作","C.M.UF1_GDF@open"]
["UF1隔断阀开到位","C.M.UF1_GDF@open_feedback"]
["UF1隔断阀远程","C.M.UF1_GDF@rem"]
["UF1隔断阀复位","C.M.UF1_GDF@reset"]
["UF1进水调节阀开度设定值","C.M.UF1_JSF_AO_FB@spare"]
["UF1进水调节阀开度报警","C.M.UF1_JSF_kd@fault"]
["UF1进水调节阀开度高报警","C.M.UF1_JSF_kd@H_AL"]
["UF1进水调节阀开度高报警开关","C.M.UF1_JSF_kd@H_AL_ON"]
["UF1进水调节阀开度高限设置","C.M.UF1_JSF_kd@H_AL_set"]
["UF1进水调节阀开度低报警","C.M.UF1_JSF_kd@L_AL"]
["UF1进水调节阀开度低报警开关","C.M.UF1_JSF_kd@L_AL_ON"]
["UF1进水调节阀开度低限设置","C.M.UF1_JSF_kd@L_AL_set"]
["UF1进水调节阀开度","C.M.UF1_JSF_kd@out"]
["UF1左侧排空阀手自动","C.M.UF1_JSPKF@auto_select"]
["UF1左侧排空阀关操作","C.M.UF1_JSPKF@close"]
["UF1左侧排空阀关到位","C.M.UF1_JSPKF@close_feedback"]
["UF1左侧排空阀故障","C.M.UF1_JSPKF@fault_total"]
["UF1左侧排空阀开操作","C.M.UF1_JSPKF@open"]
["UF1左侧排空阀开到位","C.M.UF1_JSPKF@open_feedback"]
["UF1左侧排空阀远程","C.M.UF1_JSPKF@rem"]
["UF1左侧排空阀复位","C.M.UF1_JSPKF@reset"]
["UF1左产排气液位开关","C.M.UF1_LS1"]
["UF1左进排气液位开关","C.M.UF1_LS2"]
["UF1右进排气液位开关","C.M.UF1_LS3"]
["UF1右产排气液位开关","C.M.UF1_LS4"]
["UF1左产排气阀手自动","C.M.UF1_PQF1@auto_select"]
["UF1左产排气阀关操作","C.M.UF1_PQF1@close"]
["UF1左产排气阀关到位","C.M.UF1_PQF1@close_feedback"]
["UF1左产排气阀故障","C.M.UF1_PQF1@fault_total"]
["UF1左产排气阀开操作","C.M.UF1_PQF1@open"]
["UF1左产排气阀开到位","C.M.UF1_PQF1@open_feedback"]
["UF1左产排气阀远程","C.M.UF1_PQF1@rem"]
["UF1左产排气阀复位","C.M.UF1_PQF1@reset"]
["UF1左进排气阀手自动","C.M.UF1_PQF2@auto_select"]
["UF1左进排气阀关操作","C.M.UF1_PQF2@close"]
["UF1左进排气阀关到位","C.M.UF1_PQF2@close_feedback"]
["UF1左进排气阀故障","C.M.UF1_PQF2@fault_total"]
["UF1左进排气阀开操作","C.M.UF1_PQF2@open"]
["UF1左进排气阀开到位","C.M.UF1_PQF2@open_feedback"]
["UF1左进排气阀远程","C.M.UF1_PQF2@rem"]
["UF1左进排气阀复位","C.M.UF1_PQF2@reset"]
["UF1右进排气阀手自动","C.M.UF1_PQF3@auto_select"]
["UF1右进排气阀关操作","C.M.UF1_PQF3@close"]
["UF1右进排气阀关到位","C.M.UF1_PQF3@close_feedback"]
["UF1右进排气阀故障","C.M.UF1_PQF3@fault_total"]
["UF1右进排气阀开操作","C.M.UF1_PQF3@open"]
["UF1右进排气阀开到位","C.M.UF1_PQF3@open_feedback"]
["UF1右进排气阀远程","C.M.UF1_PQF3@rem"]
["UF1右进排气阀复位","C.M.UF1_PQF3@reset"]
["UF1右产排气阀手自动","C.M.UF1_PQF4@auto_select"]
["UF1右产排气阀关操作","C.M.UF1_PQF4@close"]
["UF1右产排气阀关到位","C.M.UF1_PQF4@close_feedback"]
["UF1右产排气阀故障","C.M.UF1_PQF4@fault_total"]
["UF1右产排气阀开操作","C.M.UF1_PQF4@open"]
["UF1右产排气阀开到位","C.M.UF1_PQF4@open_feedback"]
["UF1右产排气阀远程","C.M.UF1_PQF4@rem"]
["UF1右产排气阀复位","C.M.UF1_PQF4@reset"]
["UF1产水压力报警","C.M.UF1_PT_CS@fault"]
["UF1产水压力高报警","C.M.UF1_PT_CS@H_AL"]
["UF1产水压力高报警开关","C.M.UF1_PT_CS@H_AL_ON"]
["UF1产水压力高限设置","C.M.UF1_PT_CS@H_AL_set"]
["UF1产水压力低报警","C.M.UF1_PT_CS@L_AL"]
["UF1产水压力低报警开关","C.M.UF1_PT_CS@L_AL_ON"]
["UF1产水压力低限设置","C.M.UF1_PT_CS@L_AL_set"]
["UF1产水压力","C.M.UF1_PT_CS@out"]
["UF1进水压力报警","C.M.UF1_PT_JS@fault"]
["UF1进水压力高报警","C.M.UF1_PT_JS@H_AL"]
["UF1进水压力高报警开关","C.M.UF1_PT_JS@H_AL_ON"]
["UF1进水压力高限设置","C.M.UF1_PT_JS@H_AL_set"]
["UF1进水压力低报警","C.M.UF1_PT_JS@L_AL"]
["UF1进水压力低报警开关","C.M.UF1_PT_JS@L_AL_ON"]
["UF1进水压力低限设置","C.M.UF1_PT_JS@L_AL_set"]
["UF1进水压力","C.M.UF1_PT_JS@out"]
["UF2不合格水阀手自动","C.M.UF2_BHGF@auto_select"]
["UF2不合格水阀关操作","C.M.UF2_BHGF@close"]
["UF2不合格水阀关到位","C.M.UF2_BHGF@close_feedback"]
["UF2不合格水阀故障","C.M.UF2_BHGF@fault_total"]
["UF2不合格水阀开操作","C.M.UF2_BHGF@open"]
["UF2不合格水阀开到位","C.M.UF2_BHGF@open_feedback"]
["UF2不合格水阀远程","C.M.UF2_BHGF@rem"]
["UF2不合格水阀复位","C.M.UF2_BHGF@reset"]
["UF2产水阀手自动","C.M.UF2_CSF@auto_select"]
["UF2产水阀关操作","C.M.UF2_CSF@close"]
["UF2产水阀关到位","C.M.UF2_CSF@close_feedback"]
["UF2产水阀故障","C.M.UF2_CSF@fault_total"]
["UF2产水阀开操作","C.M.UF2_CSF@open"]
["UF2产水阀开到位","C.M.UF2_CSF@open_feedback"]
["UF2产水阀远程","C.M.UF2_CSF@rem"]
["UF2产水阀复位","C.M.UF2_CSF@reset"]
["UF2右侧排空阀手自动","C.M.UF2_CSPKF@auto_select"]
["UF2右侧排空阀关操作","C.M.UF2_CSPKF@close"]
["UF2右侧排空阀关到位","C.M.UF2_CSPKF@close_feedback"]
["UF2右侧排空阀故障","C.M.UF2_CSPKF@fault_total"]
["UF2右侧排空阀开操作","C.M.UF2_CSPKF@open"]
["UF2右侧排空阀开到位","C.M.UF2_CSPKF@open_feedback"]
["UF2右侧排空阀远程","C.M.UF2_CSPKF@rem"]
["UF2右侧排空阀复位","C.M.UF2_CSPKF@reset"]
["UF2不合格冲洗","C.M.UF2_DB@BHG_residue"]
["UF2紧急停车","C.M.UF2_DB@button[00]"]
["UF2半自动开机","C.M.UF2_DB@button[01]"]
["UF2半自动停止","C.M.UF2_DB@button[02]"]
["UF2半自动反洗","C.M.UF2_DB@button[03]"]
["UF2半自动CEB","C.M.UF2_DB@button[04]"]
["UF2全自动开机/停止","C.M.UF2_DB@button[08]"]
["UF2CIP启动/停止","C.M.UF2_DB@button[09]"]
["UF2反洗请求（不确定）","C.M.UF2_DB@BW_request"]
["UF2CEB运行中（不确定）","C.M.UF2_DB@CEB_running"]
["UF2药剂残留","C.M.UF2_DB@chemical_residue"]
["UF2CIP完成（不确定）","C.M.UF2_DB@CIP_finish"]
["UF2CIP1选择","C.M.UF2_DB@CIP1_select"]
["UF2CIP2选择","C.M.UF2_DB@CIP2_select"]
["UF2余氯合格设定","C.M.UF2_DB@Cl_low_set"]
["UF2故障信息清除","C.M.UF2_DB@clean_fault"]
["UF2CIP1周期次数显示","C.M.UF2_DB@cycle_CIP1_display"]
["UF2CIP1周期设定","C.M.UF2_DB@cycle_CIP1_SP"]
["UF2CIP2周期次数显示","C.M.UF2_DB@cycle_CIP2_display"]
["UF2CIP2周期设定","C.M.UF2_DB@cycle_CIP2_SP"]
["UF2次数显示（CEB周期）","C.M.UF2_DB@cycle_out"]
["UF2CEB次数设定","C.M.UF2_DB@cycle_sp"]
["UF2故障字","C.M.UF2_DB@Fault_word"]
["UF2反洗流量设定","C.M.UF2_DB@flow_BW_SP"]
["UF2CEB流量设定","C.M.UF2_DB@flow_CEB_wash_SP"]
["UF2过滤流量设定","C.M.UF2_DB@flow_production_SP"]
["UF2液位开关连锁解锁","C.M.UF2_DB@LS_OFF"]
["UF2手动CEB选择（不确定）","C.M.UF2_DB@man_CEB_check"]
["UF2控制模式","C.M.UF2_DB@model_word"]
["UF2跨膜压差高设定","C.M.UF2_DB@press_CEB_SP"]
["UF2跨膜压差超高设定值（不确定）","C.M.UF2_DB@press_hh_SP"]
["UF2跨膜压差","C.M.UF2_DB@press_PV"]
["UF2反洗准备好","C.M.UF2_DB@ready_BW"]
["UF2碱洗准备好","C.M.UF2_DB@ready_CEB1"]
["UF2酸洗准备好","C.M.UF2_DB@ready_CEB2"]
["UF2水洗准备好","C.M.UF2_DB@ready_CEB3"]
["UF2CIP准备好（不确定）","C.M.UF2_DB@ready_CIP"]
["UF2CIP配药装备好","C.M.UF2_DB@ready_CIP_chemical"]
["UF2过滤准备好","C.M.UF2_DB@ready_production"]
["UF2阀门准备好（不确定）","C.M.UF2_DB@ready_valve"]
["UF2提醒字","C.M.UF2_DB@reminder_word"]
["UF2产水累计时间","C.M.UF2_DB@run_time"]
["UF2停机时间","C.M.UF2_DB@stop_time"]
["UF2反洗时间设定","C.M.UF2_DB@time_BW_SP"]
["UF2CEB1加药前冲洗时间设定","C.M.UF2_DB@time_CEB_wash_A"]
["UF2CEB2加药前冲洗时间设定","C.M.UF2_DB@time_CEB_wash_B"]
["UF2正冲时间设定","C.M.UF2_DB@time_CEB_wash_C"]
["UF2CIP时间显示","C.M.UF2_DB@time_CIP_display"]
["UF2CIP1循环时间设定","C.M.UF2_DB@time_CIP_SP1"]
["UF2CIP1浸泡时间设定）","C.M.UF2_DB@time_CIP_SP2"]
["UF2CIP2循环时间设定","C.M.UF2_DB@time_CIP_SP3"]
["UF2CIP2浸泡时间设定","C.M.UF2_DB@time_CIP_SP4"]
["UF2时间显示","C.M.UF2_DB@time_display"]
["UF2CEB1加药时间设定","C.M.UF2_DB@time_Dosing_A"]
["UF2CEB2加药时间设定","C.M.UF2_DB@time_Dosing_B"]
["UF2CEB1冲管时间设定","C.M.UF2_DB@time_Dosing_delay"]
["UF2产水时间设定","C.M.UF2_DB@time_production"]
["UF2产水时间显示","C.M.UF2_DB@time_production_display"]
["UF2CEB1浸泡时间设定","C.M.UF2_DB@time_steep_A"]
["UF2CEB2浸泡时间设定","C.M.UF2_DB@time_steep_B"]
["UF2冲洗A时间（不确定）","C.M.UF2_DB@time_wash_A"]
["UF2正冲进水阀开度设定","C.M.UF2_DB@V_JS_wash_sp"]
["UF2控制字","C.M.UF2_DB@word_control"]
["UF2进水流量报警","C.M.UF2_FT_JS@fault"]
["UF2进水流量高报警","C.M.UF2_FT_JS@H_AL"]
["UF2进水流量高报警开关","C.M.UF2_FT_JS@H_AL_ON"]
["UF2进水流量高限设置","C.M.UF2_FT_JS@H_AL_set"]
["UF2进水流量低报警","C.M.UF2_FT_JS@L_AL"]
["UF2进水流量低报警开关","C.M.UF2_FT_JS@L_AL_ON"]
["UF2进水流量低限设置","C.M.UF2_FT_JS@L_AL_set"]
["UF2进水流量","C.M.UF2_FT_JS@out"]
["UF2反洗进水阀手自动","C.M.UF2_FXJSF@auto_select"]
["UF2反洗进水阀关操作","C.M.UF2_FXJSF@close"]
["UF2反洗进水阀关到位","C.M.UF2_FXJSF@close_feedback"]
["UF2反洗进水阀故障","C.M.UF2_FXJSF@fault_total"]
["UF2反洗进水阀开操作","C.M.UF2_FXJSF@open"]
["UF2反洗进水阀开到位","C.M.UF2_FXJSF@open_feedback"]
["UF2反洗进水阀远程","C.M.UF2_FXJSF@rem"]
["UF2反洗进水阀复位","C.M.UF2_FXJSF@reset"]
["UF2反洗排水阀手自动","C.M.UF2_FXPSF@auto_select"]
["UF2反洗排水阀关操作","C.M.UF2_FXPSF@close"]
["UF2反洗排水阀关到位","C.M.UF2_FXPSF@close_feedback"]
["UF2反洗排水阀故障","C.M.UF2_FXPSF@fault_total"]
["UF2反洗排水阀开操作","C.M.UF2_FXPSF@open"]
["UF2反洗排水阀开到位","C.M.UF2_FXPSF@open_feedback"]
["UF2反洗排水阀远程","C.M.UF2_FXPSF@rem"]
["UF2反洗排水阀复位","C.M.UF2_FXPSF@reset"]
["UF2隔断阀手自动","C.M.UF2_GDF@auto_select"]
["UF2隔断阀关操作","C.M.UF2_GDF@close"]
["UF2隔断阀关到位","C.M.UF2_GDF@close_feedback"]
["UF2隔断阀故障","C.M.UF2_GDF@fault_total"]
["UF2隔断阀开操作","C.M.UF2_GDF@open"]
["UF2隔断阀开到位","C.M.UF2_GDF@open_feedback"]
["UF2隔断阀远程","C.M.UF2_GDF@rem"]
["UF2隔断阀复位","C.M.UF2_GDF@reset"]
["UF2进水调节阀开度设定值","C.M.UF2_JSF_AO_FB@spare"]
["UF2进水调节阀开度报警","C.M.UF2_JSF_kd@fault"]
["UF2进水调节阀开度高报警","C.M.UF2_JSF_kd@H_AL"]
["UF2进水调节阀开度高报警开关","C.M.UF2_JSF_kd@H_AL_ON"]
["UF2进水调节阀开度高限设置","C.M.UF2_JSF_kd@H_AL_set"]
["UF2进水调节阀开度低报警","C.M.UF2_JSF_kd@L_AL"]
["UF2进水调节阀开度低报警开关","C.M.UF2_JSF_kd@L_AL_ON"]
["UF2进水调节阀开度低限设置","C.M.UF2_JSF_kd@L_AL_set"]
["UF2进水调节阀开度","C.M.UF2_JSF_kd@out"]
["UF2左侧排空阀手自动","C.M.UF2_JSPKF@auto_select"]
["UF2左侧排空阀关操作","C.M.UF2_JSPKF@close"]
["UF2左侧排空阀关到位","C.M.UF2_JSPKF@close_feedback"]
["UF2左侧排空阀故障","C.M.UF2_JSPKF@fault_total"]
["UF2左侧排空阀开操作","C.M.UF2_JSPKF@open"]
["UF2左侧排空阀开到位","C.M.UF2_JSPKF@open_feedback"]
["UF2左侧排空阀远程","C.M.UF2_JSPKF@rem"]
["UF2左侧排空阀复位","C.M.UF2_JSPKF@reset"]
["UF2左产排气液位开关","C.M.UF2_LS1"]
["UF2左进排气液位开关","C.M.UF2_LS2"]
["UF2右进排气液位开关","C.M.UF2_LS3"]
["UF2右产排气液位开关","C.M.UF2_LS4"]
["UF2左产排气阀手自动","C.M.UF2_PQF1@auto_select"]
["UF2左产排气阀关操作","C.M.UF2_PQF1@close"]
["UF2左产排气阀关到位","C.M.UF2_PQF1@close_feedback"]
["UF2左产排气阀故障","C.M.UF2_PQF1@fault_total"]
["UF2左产排气阀开操作","C.M.UF2_PQF1@open"]
["UF2左产排气阀开到位","C.M.UF2_PQF1@open_feedback"]
["UF2左产排气阀远程","C.M.UF2_PQF1@rem"]
["UF2左产排气阀复位","C.M.UF2_PQF1@reset"]
["UF2左进排气阀手自动","C.M.UF2_PQF2@auto_select"]
["UF2左进排气阀关操作","C.M.UF2_PQF2@close"]
["UF2左进排气阀关到位","C.M.UF2_PQF2@close_feedback"]
["UF2左进排气阀故障","C.M.UF2_PQF2@fault_total"]
["UF2左进排气阀开操作","C.M.UF2_PQF2@open"]
["UF2左进排气阀开到位","C.M.UF2_PQF2@open_feedback"]
["UF2左进排气阀远程","C.M.UF2_PQF2@rem"]
["UF2左进排气阀复位","C.M.UF2_PQF2@reset"]
["UF2右进排气阀手自动","C.M.UF2_PQF3@auto_select"]
["UF2右进排气阀关操作","C.M.UF2_PQF3@close"]
["UF2右进排气阀关到位","C.M.UF2_PQF3@close_feedback"]
["UF2右进排气阀故障","C.M.UF2_PQF3@fault_total"]
["UF2右进排气阀开操作","C.M.UF2_PQF3@open"]
["UF2右进排气阀开到位","C.M.UF2_PQF3@open_feedback"]
["UF2右进排气阀远程","C.M.UF2_PQF3@rem"]
["UF2右进排气阀复位","C.M.UF2_PQF3@reset"]
["UF2右产排气阀手自动","C.M.UF2_PQF4@auto_select"]
["UF2右产排气阀关操作","C.M.UF2_PQF4@close"]
["UF2右产排气阀关到位","C.M.UF2_PQF4@close_feedback"]
["UF2右产排气阀故障","C.M.UF2_PQF4@fault_total"]
["UF2右产排气阀开操作","C.M.UF2_PQF4@open"]
["UF2右产排气阀开到位","C.M.UF2_PQF4@open_feedback"]
["UF2右产排气阀远程","C.M.UF2_PQF4@rem"]
["UF2右产排气阀复位","C.M.UF2_PQF4@reset"]
["UF2产水压力报警","C.M.UF2_PT_CS@fault"]
["UF2产水压力高报警","C.M.UF2_PT_CS@H_AL"]
["UF2产水压力高报警开关","C.M.UF2_PT_CS@H_AL_ON"]
["UF2产水压力高限设置","C.M.UF2_PT_CS@H_AL_set"]
["UF2产水压力低报警","C.M.UF2_PT_CS@L_AL"]
["UF2产水压力低报警开关","C.M.UF2_PT_CS@L_AL_ON"]
["UF2产水压力低限设置","C.M.UF2_PT_CS@L_AL_set"]
["UF2产水压力","C.M.UF2_PT_CS@out"]
["UF2进水压力报警","C.M.UF2_PT_JS@fault"]
["UF2进水压力高报警","C.M.UF2_PT_JS@H_AL"]
["UF2进水压力高报警开关","C.M.UF2_PT_JS@H_AL_ON"]
["UF2进水压力高限设置","C.M.UF2_PT_JS@H_AL_set"]
["UF2进水压力低报警","C.M.UF2_PT_JS@L_AL"]
["UF2进水压力低报警开关","C.M.UF2_PT_JS@L_AL_ON"]
["UF2进水压力低限设置","C.M.UF2_PT_JS@L_AL_set"]
["UF2进水压力","C.M.UF2_PT_JS@out"]
["UF3不合格水阀手自动","C.M.UF3_BHGF@auto_select"]
["UF3不合格水阀关操作","C.M.UF3_BHGF@close"]
["UF3不合格水阀关到位","C.M.UF3_BHGF@close_feedback"]
["UF3不合格水阀故障","C.M.UF3_BHGF@fault_total"]
["UF3不合格水阀开操作","C.M.UF3_BHGF@open"]
["UF3不合格水阀开到位","C.M.UF3_BHGF@open_feedback"]
["UF3不合格水阀远程","C.M.UF3_BHGF@rem"]
["UF3不合格水阀复位","C.M.UF3_BHGF@reset"]
["UF3产水阀手自动","C.M.UF3_CSF@auto_select"]
["UF3产水阀关操作","C.M.UF3_CSF@close"]
["UF3产水阀关到位","C.M.UF3_CSF@close_feedback"]
["UF3产水阀故障","C.M.UF3_CSF@fault_total"]
["UF3产水阀开操作","C.M.UF3_CSF@open"]
["UF3产水阀开到位","C.M.UF3_CSF@open_feedback"]
["UF3产水阀远程","C.M.UF3_CSF@rem"]
["UF3产水阀复位","C.M.UF3_CSF@reset"]
["UF3右侧排空阀手自动","C.M.UF3_CSPKF@auto_select"]
["UF3右侧排空阀关操作","C.M.UF3_CSPKF@close"]
["UF3右侧排空阀关到位","C.M.UF3_CSPKF@close_feedback"]
["UF3右侧排空阀故障","C.M.UF3_CSPKF@fault_total"]
["UF3右侧排空阀开操作","C.M.UF3_CSPKF@open"]
["UF3右侧排空阀开到位","C.M.UF3_CSPKF@open_feedback"]
["UF3右侧排空阀远程","C.M.UF3_CSPKF@rem"]
["UF3右侧排空阀复位","C.M.UF3_CSPKF@reset"]
["UF3不合格冲洗","C.M.UF3_DB@BHG_residue"]
["UF3紧急停车","C.M.UF3_DB@button[00]"]
["UF3半自动开机","C.M.UF3_DB@button[01]"]
["UF3半自动停止","C.M.UF3_DB@button[02]"]
["UF3半自动反洗","C.M.UF3_DB@button[03]"]
["UF3半自动CEB","C.M.UF3_DB@button[04]"]
["UF3全自动开机/停止","C.M.UF3_DB@button[08]"]
["UF3CIP启动/停止","C.M.UF3_DB@button[09]"]
["UF3反洗请求（不确定）","C.M.UF3_DB@BW_request"]
["UF3CEB运行中（不确定）","C.M.UF3_DB@CEB_running"]
["UF3药剂残留","C.M.UF3_DB@chemical_residue"]
["UF3CIP完成（不确定）","C.M.UF3_DB@CIP_finish"]
["UF3CIP1选择","C.M.UF3_DB@CIP1_select"]
["UF3CIP2选择","C.M.UF3_DB@CIP2_select"]
["UF3余氯合格设定","C.M.UF3_DB@Cl_low_set"]
["UF3故障信息清除","C.M.UF3_DB@clean_fault"]
["UF3CIP1周期次数显示","C.M.UF3_DB@cycle_CIP1_display"]
["UF3CIP1周期设定","C.M.UF3_DB@cycle_CIP1_SP"]
["UF3CIP2周期次数显示","C.M.UF3_DB@cycle_CIP2_display"]
["UF3CIP2周期设定","C.M.UF3_DB@cycle_CIP2_SP"]
["UF3次数显示（CEB周期）","C.M.UF3_DB@cycle_out"]
["UF3CEB次数设定","C.M.UF3_DB@cycle_sp"]
["UF3故障字","C.M.UF3_DB@Fault_word"]
["UF3反洗流量设定","C.M.UF3_DB@flow_BW_SP"]
["UF3CEB流量设定","C.M.UF3_DB@flow_CEB_wash_SP"]
["UF3过滤流量设定","C.M.UF3_DB@flow_production_SP"]
["UF3液位开关连锁解锁","C.M.UF3_DB@LS_OFF"]
["UF3手动CEB选择（不确定）","C.M.UF3_DB@man_CEB_check"]
["UF3控制模式","C.M.UF3_DB@model_word"]
["UF3跨膜压差高设定","C.M.UF3_DB@press_CEB_SP"]
["UF3跨膜压差超高设定值（不确定）","C.M.UF3_DB@press_hh_SP"]
["UF3跨膜压差","C.M.UF3_DB@press_PV"]
["UF3反洗准备好","C.M.UF3_DB@ready_BW"]
["UF3碱洗准备好","C.M.UF3_DB@ready_CEB1"]
["UF3酸洗准备好","C.M.UF3_DB@ready_CEB2"]
["UF3水洗准备好","C.M.UF3_DB@ready_CEB3"]
["UF3CIP准备好（不确定）","C.M.UF3_DB@ready_CIP"]
["UF3CIP配药装备好","C.M.UF3_DB@ready_CIP_chemical"]
["UF3过滤准备好","C.M.UF3_DB@ready_production"]
["UF3阀门准备好（不确定）","C.M.UF3_DB@ready_valve"]
["UF3提醒字","C.M.UF3_DB@reminder_word"]
["UF3产水累计时间","C.M.UF3_DB@run_time"]
["UF3停机时间","C.M.UF3_DB@stop_time"]
["UF3反洗时间设定","C.M.UF3_DB@time_BW_SP"]
["UF3CEB1加药前冲洗时间设定","C.M.UF3_DB@time_CEB_wash_A"]
["UF3CEB2加药前冲洗时间设定","C.M.UF3_DB@time_CEB_wash_B"]
["UF3正冲时间设定","C.M.UF3_DB@time_CEB_wash_C"]
["UF3CIP时间显示","C.M.UF3_DB@time_CIP_display"]
["UF3CIP1循环时间设定","C.M.UF3_DB@time_CIP_SP1"]
["UF3CIP1浸泡时间设定）","C.M.UF3_DB@time_CIP_SP2"]
["UF3CIP2循环时间设定","C.M.UF3_DB@time_CIP_SP3"]
["UF3CIP2浸泡时间设定","C.M.UF3_DB@time_CIP_SP4"]
["UF3时间显示","C.M.UF3_DB@time_display"]
["UF3CEB1加药时间设定","C.M.UF3_DB@time_Dosing_A"]
["UF3CEB2加药时间设定","C.M.UF3_DB@time_Dosing_B"]
["UF3CEB1冲管时间设定","C.M.UF3_DB@time_Dosing_delay"]
["UF3产水时间设定","C.M.UF3_DB@time_production"]
["UF3产水时间显示","C.M.UF3_DB@time_production_display"]
["UF3CEB1浸泡时间设定","C.M.UF3_DB@time_steep_A"]
["UF3CEB2浸泡时间设定","C.M.UF3_DB@time_steep_B"]
["UF3冲洗A时间（不确定）","C.M.UF3_DB@time_wash_A"]
["UF3正冲进水阀开度设定","C.M.UF3_DB@V_JS_wash_sp"]
["UF3控制字","C.M.UF3_DB@word_control"]
["UF3进水流量报警","C.M.UF3_FT_JS@fault"]
["UF3进水流量高报警","C.M.UF3_FT_JS@H_AL"]
["UF3进水流量高报警开关","C.M.UF3_FT_JS@H_AL_ON"]
["UF3进水流量高限设置","C.M.UF3_FT_JS@H_AL_set"]
["UF3进水流量低报警","C.M.UF3_FT_JS@L_AL"]
["UF3进水流量低报警开关","C.M.UF3_FT_JS@L_AL_ON"]
["UF3进水流量低限设置","C.M.UF3_FT_JS@L_AL_set"]
["UF3进水流量","C.M.UF3_FT_JS@out"]
["UF3反洗进水阀手自动","C.M.UF3_FXJSF@auto_select"]
["UF3反洗进水阀关操作","C.M.UF3_FXJSF@close"]
["UF3反洗进水阀关到位","C.M.UF3_FXJSF@close_feedback"]
["UF3反洗进水阀故障","C.M.UF3_FXJSF@fault_total"]
["UF3反洗进水阀开操作","C.M.UF3_FXJSF@open"]
["UF3反洗进水阀开到位","C.M.UF3_FXJSF@open_feedback"]
["UF3反洗进水阀远程","C.M.UF3_FXJSF@rem"]
["UF3反洗进水阀复位","C.M.UF3_FXJSF@reset"]
["UF3反洗排水阀手自动","C.M.UF3_FXPSF@auto_select"]
["UF3反洗排水阀关操作","C.M.UF3_FXPSF@close"]
["UF3反洗排水阀关到位","C.M.UF3_FXPSF@close_feedback"]
["UF3反洗排水阀故障","C.M.UF3_FXPSF@fault_total"]
["UF3反洗排水阀开操作","C.M.UF3_FXPSF@open"]
["UF3反洗排水阀开到位","C.M.UF3_FXPSF@open_feedback"]
["UF3反洗排水阀远程","C.M.UF3_FXPSF@rem"]
["UF3反洗排水阀复位","C.M.UF3_FXPSF@reset"]
["UF3隔断阀手自动","C.M.UF3_GDF@auto_select"]
["UF3隔断阀关操作","C.M.UF3_GDF@close"]
["UF3隔断阀关到位","C.M.UF3_GDF@close_feedback"]
["UF3隔断阀故障","C.M.UF3_GDF@fault_total"]
["UF3隔断阀开操作","C.M.UF3_GDF@open"]
["UF3隔断阀开到位","C.M.UF3_GDF@open_feedback"]
["UF3隔断阀远程","C.M.UF3_GDF@rem"]
["UF3隔断阀复位","C.M.UF3_GDF@reset"]
["UF3进水调节阀开度设定值","C.M.UF3_JSF_AO_FB@spare"]
["UF3进水调节阀开度报警","C.M.UF3_JSF_kd@fault"]
["UF3进水调节阀开度高报警","C.M.UF3_JSF_kd@H_AL"]
["UF3进水调节阀开度高报警开关","C.M.UF3_JSF_kd@H_AL_ON"]
["UF3进水调节阀开度高限设置","C.M.UF3_JSF_kd@H_AL_set"]
["UF3进水调节阀开度低报警","C.M.UF3_JSF_kd@L_AL"]
["UF3进水调节阀开度低报警开关","C.M.UF3_JSF_kd@L_AL_ON"]
["UF3进水调节阀开度低限设置","C.M.UF3_JSF_kd@L_AL_set"]
["UF3进水调节阀开度","C.M.UF3_JSF_kd@out"]
["UF3左侧排空阀手自动","C.M.UF3_JSPKF@auto_select"]
["UF3左侧排空阀关操作","C.M.UF3_JSPKF@close"]
["UF3左侧排空阀关到位","C.M.UF3_JSPKF@close_feedback"]
["UF3左侧排空阀故障","C.M.UF3_JSPKF@fault_total"]
["UF3左侧排空阀开操作","C.M.UF3_JSPKF@open"]
["UF3左侧排空阀开到位","C.M.UF3_JSPKF@open_feedback"]
["UF3左侧排空阀远程","C.M.UF3_JSPKF@rem"]
["UF3左侧排空阀复位","C.M.UF3_JSPKF@reset"]
["UF3左产排气液位开关","C.M.UF3_LS1"]
["UF3左进排气液位开关","C.M.UF3_LS2"]
["UF3右进排气液位开关","C.M.UF3_LS3"]
["UF3右产排气液位开关","C.M.UF3_LS4"]
["UF3左产排气阀手自动","C.M.UF3_PQF1@auto_select"]
["UF3左产排气阀关操作","C.M.UF3_PQF1@close"]
["UF3左产排气阀关到位","C.M.UF3_PQF1@close_feedback"]
["UF3左产排气阀故障","C.M.UF3_PQF1@fault_total"]
["UF3左产排气阀开操作","C.M.UF3_PQF1@open"]
["UF3左产排气阀开到位","C.M.UF3_PQF1@open_feedback"]
["UF3左产排气阀远程","C.M.UF3_PQF1@rem"]
["UF3左产排气阀复位","C.M.UF3_PQF1@reset"]
["UF3左进排气阀手自动","C.M.UF3_PQF2@auto_select"]
["UF3左进排气阀关操作","C.M.UF3_PQF2@close"]
["UF3左进排气阀关到位","C.M.UF3_PQF2@close_feedback"]
["UF3左进排气阀故障","C.M.UF3_PQF2@fault_total"]
["UF3左进排气阀开操作","C.M.UF3_PQF2@open"]
["UF3左进排气阀开到位","C.M.UF3_PQF2@open_feedback"]
["UF3左进排气阀远程","C.M.UF3_PQF2@rem"]
["UF3左进排气阀复位","C.M.UF3_PQF2@reset"]
["UF3右进排气阀手自动","C.M.UF3_PQF3@auto_select"]
["UF3右进排气阀关操作","C.M.UF3_PQF3@close"]
["UF3右进排气阀关到位","C.M.UF3_PQF3@close_feedback"]
["UF3右进排气阀故障","C.M.UF3_PQF3@fault_total"]
["UF3右进排气阀开操作","C.M.UF3_PQF3@open"]
["UF3右进排气阀开到位","C.M.UF3_PQF3@open_feedback"]
["UF3右进排气阀远程","C.M.UF3_PQF3@rem"]
["UF3右进排气阀复位","C.M.UF3_PQF3@reset"]
["UF3右产排气阀手自动","C.M.UF3_PQF4@auto_select"]
["UF3右产排气阀关操作","C.M.UF3_PQF4@close"]
["UF3右产排气阀关到位","C.M.UF3_PQF4@close_feedback"]
["UF3右产排气阀故障","C.M.UF3_PQF4@fault_total"]
["UF3右产排气阀开操作","C.M.UF3_PQF4@open"]
["UF3右产排气阀开到位","C.M.UF3_PQF4@open_feedback"]
["UF3右产排气阀远程","C.M.UF3_PQF4@rem"]
["UF3右产排气阀复位","C.M.UF3_PQF4@reset"]
["UF3产水压力报警","C.M.UF3_PT_CS@fault"]
["UF3产水压力高报警","C.M.UF3_PT_CS@H_AL"]
["UF3产水压力高报警开关","C.M.UF3_PT_CS@H_AL_ON"]
["UF3产水压力高限设置","C.M.UF3_PT_CS@H_AL_set"]
["UF3产水压力低报警","C.M.UF3_PT_CS@L_AL"]
["UF3产水压力低报警开关","C.M.UF3_PT_CS@L_AL_ON"]
["UF3产水压力低限设置","C.M.UF3_PT_CS@L_AL_set"]
["UF3产水压力","C.M.UF3_PT_CS@out"]
["UF3进水压力报警","C.M.UF3_PT_JS@fault"]
["UF3进水压力高报警","C.M.UF3_PT_JS@H_AL"]
["UF3进水压力高报警开关","C.M.UF3_PT_JS@H_AL_ON"]
["UF3进水压力高限设置","C.M.UF3_PT_JS@H_AL_set"]
["UF3进水压力低报警","C.M.UF3_PT_JS@L_AL"]
["UF3进水压力低报警开关","C.M.UF3_PT_JS@L_AL_ON"]
["UF3进水压力低限设置","C.M.UF3_PT_JS@L_AL_set"]
["UF3进水压力","C.M.UF3_PT_JS@out"]
["UF4不合格水阀手自动","C.M.UF4_BHGF@auto_select"]
["UF4不合格水阀关操作","C.M.UF4_BHGF@close"]
["UF4不合格水阀关到位","C.M.UF4_BHGF@close_feedback"]
["UF4不合格水阀故障","C.M.UF4_BHGF@fault_total"]
["UF4不合格水阀开操作","C.M.UF4_BHGF@open"]
["UF4不合格水阀开到位","C.M.UF4_BHGF@open_feedback"]
["UF4不合格水阀远程","C.M.UF4_BHGF@rem"]
["UF4不合格水阀复位","C.M.UF4_BHGF@reset"]
["UF4产水阀手自动","C.M.UF4_CSF@auto_select"]
["UF4产水阀关操作","C.M.UF4_CSF@close"]
["UF4产水阀关到位","C.M.UF4_CSF@close_feedback"]
["UF4产水阀故障","C.M.UF4_CSF@fault_total"]
["UF4产水阀开操作","C.M.UF4_CSF@open"]
["UF4产水阀开到位","C.M.UF4_CSF@open_feedback"]
["UF4产水阀远程","C.M.UF4_CSF@rem"]
["UF4产水阀复位","C.M.UF4_CSF@reset"]
["UF4右侧排空阀手自动","C.M.UF4_CSPKF@auto_select"]
["UF4右侧排空阀关操作","C.M.UF4_CSPKF@close"]
["UF4右侧排空阀关到位","C.M.UF4_CSPKF@close_feedback"]
["UF4右侧排空阀故障","C.M.UF4_CSPKF@fault_total"]
["UF4右侧排空阀开操作","C.M.UF4_CSPKF@open"]
["UF4右侧排空阀开到位","C.M.UF4_CSPKF@open_feedback"]
["UF4右侧排空阀远程","C.M.UF4_CSPKF@rem"]
["UF4右侧排空阀复位","C.M.UF4_CSPKF@reset"]
["UF4不合格冲洗","C.M.UF4_DB@BHG_residue"]
["UF4紧急停车","C.M.UF4_DB@button[00]"]
["UF4半自动开机","C.M.UF4_DB@button[01]"]
["UF4半自动停止","C.M.UF4_DB@button[02]"]
["UF4半自动反洗","C.M.UF4_DB@button[03]"]
["UF4半自动CEB","C.M.UF4_DB@button[04]"]
["UF4全自动开机/停止","C.M.UF4_DB@button[08]"]
["UF4CIP启动/停止","C.M.UF4_DB@button[09]"]
["UF4反洗请求（不确定）","C.M.UF4_DB@BW_request"]
["UF4CEB运行中（不确定）","C.M.UF4_DB@CEB_running"]
["UF4药剂残留","C.M.UF4_DB@chemical_residue"]
["UF4CIP完成（不确定）","C.M.UF4_DB@CIP_finish"]
["UF4CIP1选择","C.M.UF4_DB@CIP1_select"]
["UF4CIP2选择","C.M.UF4_DB@CIP2_select"]
["UF4余氯合格设定","C.M.UF4_DB@Cl_low_set"]
["UF4故障信息清除","C.M.UF4_DB@clean_fault"]
["UF4CIP1周期次数显示","C.M.UF4_DB@cycle_CIP1_display"]
["UF4CIP1周期设定","C.M.UF4_DB@cycle_CIP1_SP"]
["UF4CIP2周期次数显示","C.M.UF4_DB@cycle_CIP2_display"]
["UF4CIP2周期设定","C.M.UF4_DB@cycle_CIP2_SP"]
["UF4次数显示（CEB周期）","C.M.UF4_DB@cycle_out"]
["UF4CEB次数设定","C.M.UF4_DB@cycle_sp"]
["UF4故障字","C.M.UF4_DB@Fault_word"]
["UF4反洗流量设定","C.M.UF4_DB@flow_BW_SP"]
["UF4CEB流量设定","C.M.UF4_DB@flow_CEB_wash_SP"]
["UF4过滤流量设定","C.M.UF4_DB@flow_production_SP"]
["UF4液位开关连锁解锁","C.M.UF4_DB@LS_OFF"]
["UF4手动CEB选择（不确定）","C.M.UF4_DB@man_CEB_check"]
["UF4控制模式","C.M.UF4_DB@model_word"]
["UF4跨膜压差高设定","C.M.UF4_DB@press_CEB_SP"]
["UF4跨膜压差超高设定值（不确定）","C.M.UF4_DB@press_hh_SP"]
["UF4跨膜压差","C.M.UF4_DB@press_PV"]
["UF4反洗准备好","C.M.UF4_DB@ready_BW"]
["UF4碱洗准备好","C.M.UF4_DB@ready_CEB1"]
["UF4酸洗准备好","C.M.UF4_DB@ready_CEB2"]
["UF4水洗准备好","C.M.UF4_DB@ready_CEB3"]
["UF4CIP准备好（不确定）","C.M.UF4_DB@ready_CIP"]
["UF4CIP配药装备好","C.M.UF4_DB@ready_CIP_chemical"]
["UF4过滤准备好","C.M.UF4_DB@ready_production"]
["UF4阀门准备好（不确定）","C.M.UF4_DB@ready_valve"]
["UF4提醒字","C.M.UF4_DB@reminder_word"]
["UF4产水累计时间","C.M.UF4_DB@run_time"]
["UF4停机时间","C.M.UF4_DB@stop_time"]
["UF4反洗时间设定","C.M.UF4_DB@time_BW_SP"]
["UF4CEB1加药前冲洗时间设定","C.M.UF4_DB@time_CEB_wash_A"]
["UF4CEB2加药前冲洗时间设定","C.M.UF4_DB@time_CEB_wash_B"]
["UF4正冲时间设定","C.M.UF4_DB@time_CEB_wash_C"]
["UF4CIP时间显示","C.M.UF4_DB@time_CIP_display"]
["UF4CIP1循环时间设定","C.M.UF4_DB@time_CIP_SP1"]
["UF4CIP1浸泡时间设定）","C.M.UF4_DB@time_CIP_SP2"]
["UF4CIP2循环时间设定","C.M.UF4_DB@time_CIP_SP3"]
["UF4CIP2浸泡时间设定","C.M.UF4_DB@time_CIP_SP4"]
["UF4时间显示","C.M.UF4_DB@time_display"]
["UF4CEB1加药时间设定","C.M.UF4_DB@time_Dosing_A"]
["UF4CEB2加药时间设定","C.M.UF4_DB@time_Dosing_B"]
["UF4CEB1冲管时间设定","C.M.UF4_DB@time_Dosing_delay"]
["UF4产水时间设定","C.M.UF4_DB@time_production"]
["UF4产水时间显示","C.M.UF4_DB@time_production_display"]
["UF4CEB1浸泡时间设定","C.M.UF4_DB@time_steep_A"]
["UF4CEB2浸泡时间设定","C.M.UF4_DB@time_steep_B"]
["UF4冲洗A时间（不确定）","C.M.UF4_DB@time_wash_A"]
["UF4正冲进水阀开度设定","C.M.UF4_DB@V_JS_wash_sp"]
["UF4控制字","C.M.UF4_DB@word_control"]
["UF4进水流量报警","C.M.UF4_FT_JS@fault"]
["UF4进水流量高报警","C.M.UF4_FT_JS@H_AL"]
["UF4进水流量高报警开关","C.M.UF4_FT_JS@H_AL_ON"]
["UF4进水流量高限设置","C.M.UF4_FT_JS@H_AL_set"]
["UF4进水流量低报警","C.M.UF4_FT_JS@L_AL"]
["UF4进水流量低报警开关","C.M.UF4_FT_JS@L_AL_ON"]
["UF4进水流量低限设置","C.M.UF4_FT_JS@L_AL_set"]
["UF4进水流量","C.M.UF4_FT_JS@out"]
["UF4反洗进水阀手自动","C.M.UF4_FXJSF@auto_select"]
["UF4反洗进水阀关操作","C.M.UF4_FXJSF@close"]
["UF4反洗进水阀关到位","C.M.UF4_FXJSF@close_feedback"]
["UF4反洗进水阀故障","C.M.UF4_FXJSF@fault_total"]
["UF4反洗进水阀开操作","C.M.UF4_FXJSF@open"]
["UF4反洗进水阀开到位","C.M.UF4_FXJSF@open_feedback"]
["UF4反洗进水阀远程","C.M.UF4_FXJSF@rem"]
["UF4反洗进水阀复位","C.M.UF4_FXJSF@reset"]
["UF4反洗排水阀手自动","C.M.UF4_FXPSF@auto_select"]
["UF4反洗排水阀关操作","C.M.UF4_FXPSF@close"]
["UF4反洗排水阀关到位","C.M.UF4_FXPSF@close_feedback"]
["UF4反洗排水阀故障","C.M.UF4_FXPSF@fault_total"]
["UF4反洗排水阀开操作","C.M.UF4_FXPSF@open"]
["UF4反洗排水阀开到位","C.M.UF4_FXPSF@open_feedback"]
["UF4反洗排水阀远程","C.M.UF4_FXPSF@rem"]
["UF4反洗排水阀复位","C.M.UF4_FXPSF@reset"]
["UF4隔断阀手自动","C.M.UF4_GDF@auto_select"]
["UF4隔断阀关操作","C.M.UF4_GDF@close"]
["UF4隔断阀关到位","C.M.UF4_GDF@close_feedback"]
["UF4隔断阀故障","C.M.UF4_GDF@fault_total"]
["UF4隔断阀开操作","C.M.UF4_GDF@open"]
["UF4隔断阀开到位","C.M.UF4_GDF@open_feedback"]
["UF4隔断阀远程","C.M.UF4_GDF@rem"]
["UF4隔断阀复位","C.M.UF4_GDF@reset"]
["UF4进水调节阀开度设定值","C.M.UF4_JSF_AO_FB@spare"]
["UF4进水调节阀开度报警","C.M.UF4_JSF_kd@fault"]
["UF4进水调节阀开度高报警","C.M.UF4_JSF_kd@H_AL"]
["UF4进水调节阀开度高报警开关","C.M.UF4_JSF_kd@H_AL_ON"]
["UF4进水调节阀开度高限设置","C.M.UF4_JSF_kd@H_AL_set"]
["UF4进水调节阀开度低报警","C.M.UF4_JSF_kd@L_AL"]
["UF4进水调节阀开度低报警开关","C.M.UF4_JSF_kd@L_AL_ON"]
["UF4进水调节阀开度低限设置","C.M.UF4_JSF_kd@L_AL_set"]
["UF4进水调节阀开度","C.M.UF4_JSF_kd@out"]
["UF4左侧排空阀手自动","C.M.UF4_JSPKF@auto_select"]
["UF4左侧排空阀关操作","C.M.UF4_JSPKF@close"]
["UF4左侧排空阀关到位","C.M.UF4_JSPKF@close_feedback"]
["UF4左侧排空阀故障","C.M.UF4_JSPKF@fault_total"]
["UF4左侧排空阀开操作","C.M.UF4_JSPKF@open"]
["UF4左侧排空阀开到位","C.M.UF4_JSPKF@open_feedback"]
["UF4左侧排空阀远程","C.M.UF4_JSPKF@rem"]
["UF4左侧排空阀复位","C.M.UF4_JSPKF@reset"]
["UF4左产排气液位开关","C.M.UF4_LS1"]
["UF4左进排气液位开关","C.M.UF4_LS2"]
["UF4右进排气液位开关","C.M.UF4_LS3"]
["UF4右产排气液位开关","C.M.UF4_LS4"]
["UF4左产排气阀手自动","C.M.UF4_PQF1@auto_select"]
["UF4左产排气阀关操作","C.M.UF4_PQF1@close"]
["UF4左产排气阀关到位","C.M.UF4_PQF1@close_feedback"]
["UF4左产排气阀故障","C.M.UF4_PQF1@fault_total"]
["UF4左产排气阀开操作","C.M.UF4_PQF1@open"]
["UF4左产排气阀开到位","C.M.UF4_PQF1@open_feedback"]
["UF4左产排气阀远程","C.M.UF4_PQF1@rem"]
["UF4左产排气阀复位","C.M.UF4_PQF1@reset"]
["UF4左进排气阀手自动","C.M.UF4_PQF2@auto_select"]
["UF4左进排气阀关操作","C.M.UF4_PQF2@close"]
["UF4左进排气阀关到位","C.M.UF4_PQF2@close_feedback"]
["UF4左进排气阀故障","C.M.UF4_PQF2@fault_total"]
["UF4左进排气阀开操作","C.M.UF4_PQF2@open"]
["UF4左进排气阀开到位","C.M.UF4_PQF2@open_feedback"]
["UF4左进排气阀远程","C.M.UF4_PQF2@rem"]
["UF4左进排气阀复位","C.M.UF4_PQF2@reset"]
["UF4右进排气阀手自动","C.M.UF4_PQF3@auto_select"]
["UF4右进排气阀关操作","C.M.UF4_PQF3@close"]
["UF4右进排气阀关到位","C.M.UF4_PQF3@close_feedback"]
["UF4右进排气阀故障","C.M.UF4_PQF3@fault_total"]
["UF4右进排气阀开操作","C.M.UF4_PQF3@open"]
["UF4右进排气阀开到位","C.M.UF4_PQF3@open_feedback"]
["UF4右进排气阀远程","C.M.UF4_PQF3@rem"]
["UF4右进排气阀复位","C.M.UF4_PQF3@reset"]
["UF4右产排气阀手自动","C.M.UF4_PQF4@auto_select"]
["UF4右产排气阀关操作","C.M.UF4_PQF4@close"]
["UF4右产排气阀关到位","C.M.UF4_PQF4@close_feedback"]
["UF4右产排气阀故障","C.M.UF4_PQF4@fault_total"]
["UF4右产排气阀开操作","C.M.UF4_PQF4@open"]
["UF4右产排气阀开到位","C.M.UF4_PQF4@open_feedback"]
["UF4右产排气阀远程","C.M.UF4_PQF4@rem"]
["UF4右产排气阀复位","C.M.UF4_PQF4@reset"]
["UF4产水压力报警","C.M.UF4_PT_CS@fault"]
["UF4产水压力高报警","C.M.UF4_PT_CS@H_AL"]
["UF4产水压力高报警开关","C.M.UF4_PT_CS@H_AL_ON"]
["UF4产水压力高限设置","C.M.UF4_PT_CS@H_AL_set"]
["UF4产水压力低报警","C.M.UF4_PT_CS@L_AL"]
["UF4产水压力低报警开关","C.M.UF4_PT_CS@L_AL_ON"]
["UF4产水压力低限设置","C.M.UF4_PT_CS@L_AL_set"]
["UF4产水压力","C.M.UF4_PT_CS@out"]
["UF4进水压力报警","C.M.UF4_PT_JS@fault"]
["UF4进水压力高报警","C.M.UF4_PT_JS@H_AL"]
["UF4进水压力高报警开关","C.M.UF4_PT_JS@H_AL_ON"]
["UF4进水压力高限设置","C.M.UF4_PT_JS@H_AL_set"]
["UF4进水压力低报警","C.M.UF4_PT_JS@L_AL"]
["UF4进水压力低报警开关","C.M.UF4_PT_JS@L_AL_ON"]
["UF4进水压力低限设置","C.M.UF4_PT_JS@L_AL_set"]
["UF4进水压力","C.M.UF4_PT_JS@out"]
["外供水压力设定","C.M.WGS_pid_sp"]
["卸料泵手自动","C.M.XLB@auto_select"]
["卸料泵故障","C.M.XLB@fault_total"]
["卸料泵远程","C.M.XLB@rem"]
["卸料泵复位","C.M.XLB@reset"]
["卸料泵运行","C.M.XLB@run"]
["卸料泵运行时间","C.M.XLB@run_time"]
["卸料泵启动操作","C.M.XLB@start"]
["卸料泵停止操作","C.M.XLB@stop"]
["1#中和废水泵手自动","C.M.ZH_FSB1@auto_select"]
["1#中和废水泵故障","C.M.ZH_FSB1@fault_total"]
["1#中和废水泵远程","C.M.ZH_FSB1@rem"]
["1#中和废水泵复位","C.M.ZH_FSB1@reset"]
["1#中和废水泵运行","C.M.ZH_FSB1@run"]
["1#中和废水泵运行时间","C.M.ZH_FSB1@run_time"]
["1#中和废水泵启动操作","C.M.ZH_FSB1@start"]
["1#中和废水泵停止操作","C.M.ZH_FSB1@stop"]
["2#中和废水泵手自动","C.M.ZH_FSB2@auto_select"]
["2#中和废水泵故障","C.M.ZH_FSB2@fault_total"]
["2#中和废水泵远程","C.M.ZH_FSB2@rem"]
["2#中和废水泵复位","C.M.ZH_FSB2@reset"]
["2#中和废水泵运行","C.M.ZH_FSB2@run"]
["2#中和废水泵运行时间","C.M.ZH_FSB2@run_time"]
["2#中和废水泵启动操作","C.M.ZH_FSB2@start"]
["2#中和废水泵停止操作","C.M.ZH_FSB2@stop"]
["盐酸加药阀(中和)手自动","C.M.ZH_HCl@auto_select"]
["盐酸加药阀(中和)关操作","C.M.ZH_HCl@close"]
["盐酸加药阀(中和)关到位","C.M.ZH_HCl@close_feedback"]
["盐酸加药阀(中和)故障","C.M.ZH_HCl@fault_total"]
["盐酸加药阀(中和)开操作","C.M.ZH_HCl@open"]
["盐酸加药阀(中和)开到位","C.M.ZH_HCl@open_feedback"]
["盐酸加药阀(中和)远程","C.M.ZH_HCl@rem"]
["盐酸加药阀(中和)复位","C.M.ZH_HCl@reset"]
["还原剂加药阀(中和)手自动","C.M.ZH_HYJ@auto_select"]
["还原剂加药阀(中和)关操作","C.M.ZH_HYJ@close"]
["还原剂加药阀(中和)关到位","C.M.ZH_HYJ@close_feedback"]
["还原剂加药阀(中和)故障","C.M.ZH_HYJ@fault_total"]
["还原剂加药阀(中和)开操作","C.M.ZH_HYJ@open"]
["还原剂加药阀(中和)开到位","C.M.ZH_HYJ@open_feedback"]
["还原剂加药阀(中和)远程","C.M.ZH_HYJ@rem"]
["还原剂加药阀(中和)复位","C.M.ZH_HYJ@reset"]
["NaOH加药阀(中和)手自动","C.M.ZH_NaOH@auto_select"]
["NaOH加药阀(中和)关操作","C.M.ZH_NaOH@close"]
["NaOH加药阀(中和)关到位","C.M.ZH_NaOH@close_feedback"]
["NaOH加药阀(中和)故障","C.M.ZH_NaOH@fault_total"]
["NaOH加药阀(中和)开操作","C.M.ZH_NaOH@open"]
["NaOH加药阀(中和)开到位","C.M.ZH_NaOH@open_feedback"]
["NaOH加药阀(中和)远程","C.M.ZH_NaOH@rem"]
["NaOH加药阀(中和)复位","C.M.ZH_NaOH@reset"]
["中和ORP报警","C.M.ZH_ORP@fault"]
["中和ORP高报警","C.M.ZH_ORP@H_AL"]
["中和ORP高报警开关","C.M.ZH_ORP@H_AL_ON"]
["中和ORP高限设置","C.M.ZH_ORP@H_AL_set"]
["中和ORP低报警","C.M.ZH_ORP@L_AL"]
["中和ORP低报警开关","C.M.ZH_ORP@L_AL_ON"]
["中和ORP低限设置","C.M.ZH_ORP@L_AL_set"]
["中和ORP","C.M.ZH_ORP@out"]
["中和水池PH报警","C.M.ZH_PH@fault"]
["中和水池PH高报警","C.M.ZH_PH@H_AL"]
["中和水池PH高报警开关","C.M.ZH_PH@H_AL_ON"]
["中和水池PH高限设置","C.M.ZH_PH@H_AL_set"]
["中和水池PH低报警","C.M.ZH_PH@L_AL"]
["中和水池PH低报警开关","C.M.ZH_PH@L_AL_ON"]
["中和水池PH低限设置","C.M.ZH_PH@L_AL_set"]
["中和水池PH","C.M.ZH_PH@out"]
["中和外排阀手自动","C.M.ZH_WPF@auto_select"]
["中和外排阀关操作","C.M.ZH_WPF@close"]
["中和外排阀关到位","C.M.ZH_WPF@close_feedback"]
["中和外排阀故障","C.M.ZH_WPF@fault_total"]
["中和外排阀开操作","C.M.ZH_WPF@open"]
["中和外排阀开到位","C.M.ZH_WPF@open_feedback"]
["中和外排阀远程","C.M.ZH_WPF@rem"]
["中和外排阀复位","C.M.ZH_WPF@reset"]
["中和循环阀手自动","C.M.ZH_XHF@auto_select"]
["中和循环阀关操作","C.M.ZH_XHF@close"]
["中和循环阀关到位","C.M.ZH_XHF@close_feedback"]
["中和循环阀故障","C.M.ZH_XHF@fault_total"]
["中和循环阀开操作","C.M.ZH_XHF@open"]
["中和循环阀开到位","C.M.ZH_XHF@open_feedback"]
["中和循环阀远程","C.M.ZH_XHF@rem"]
["中和循环阀复位","C.M.ZH_XHF@reset"]
["RO1杀菌剂阀开到位","C5.M5.RO1_SJJF_op"]
["RO1杀菌剂阀关到位","C5.M5.RO1_SJJF_cs"]
["RO2杀菌剂阀开到位","C5.M5.RO2_SJJF_op"]
["RO2杀菌剂阀关到位","C5.M5.RO2_SJJF_cs"]
["RO3杀菌剂阀开到位","C5.M5.RO3_SJJF_op"]
["RO3杀菌剂阀关到位","C5.M5.RO3_SJJF_cs"]
["RO4杀菌剂阀开到位","C5.M5.RO4_SJJF_op"]
["RO4杀菌剂阀关到位","C5.M5.RO4_SJJF_cs"]
["RO1杀菌剂阀手动打开/关闭","C5.M5.RO1_SJJF_Mstart"]
["RO1杀菌剂阀手动/自动","C5.M5.RO1_SJJF_AM"]
["RO1杀菌剂阀自动打开/关闭","C5.M5.RO1_SJJF_Astart"]
["RO1杀菌剂阀故障","C5.M5.RO1_SJJF_GZ"]
["RO2杀菌剂阀手动打开/关闭","C5.M5.RO2_SJJF_Mstart"]
["RO2杀菌剂阀手动/自动","C5.M5.RO2_SJJF_AM"]
["RO2杀菌剂阀自动打开/关闭","C5.M5.RO2_SJJF_Astart"]
["RO2杀菌剂阀故障","C5.M5.RO2_SJJF_GZ"]
["RO3杀菌剂阀手动打开/关闭","C5.M5.RO3_SJJF_Mstart"]
["RO3杀菌剂阀手动/自动","C5.M5.RO3_SJJF_AM"]
["RO3杀菌剂阀自动打开/关闭","C5.M5.RO3_SJJF_Astart"]
["RO3杀菌剂阀故障","C5.M5.RO3_SJJF_GZ"]
["RO4杀菌剂阀手动打开/关闭","C5.M5.RO4_SJJF_Mstart"]
["RO4杀菌剂阀手动/自动","C5.M5.RO4_SJJF_AM"]
["RO4杀菌剂阀自动打开/关闭","C5.M5.RO4_SJJF_Astart"]
["RO4杀菌剂阀故障","C5.M5.RO4_SJJF_GZ"]
["RO1杀菌剂阀故障复位","C5.M5.RO1_SJJF_FW"]
["RO2杀菌剂阀故障复位","C5.M5.RO2_SJJF_FW"]
["RO3杀菌剂阀故障复位","C5.M5.RO3_SJJF_FW"]
["RO4杀菌剂阀故障复位","C5.M5.RO4_SJJF_FW"]
["杀菌剂阀远控","C5.M5.RO_YK"]
["RO1杀菌启动","C5.M5.RO1_SJQD"]
["RO1杀菌时长设定 ","C5.M5.RO1_SJSCSD"]
["RO1杀菌时长显示","C5.M5.RO1_SJSCXS"]
["RO1杀菌计时开关","C5.M5.RO1_SJJSKG"]
["RO1杀菌步序","C5.M5.RO1_SJBX"]
["RO2杀菌启动","C5.M5.RO2_SJQD"]
["RO2杀菌时长设定 ","C5.M5.RO2_SJSCSD"]
["RO2杀菌时长显示","C5.M5.RO2_SJSCXS"]
["RO2杀菌计时开关","C5.M5.RO2_SJJSKG"]
["RO2杀菌步序","C5.M5.RO2_SJBX"]
["RO3杀菌启动","C5.M5.RO3_SJQD"]
["RO3杀菌时长设定 ","C5.M5.RO3_SJSCSD"]
["RO3杀菌时长显示","C5.M5.RO3_SJSCXS"]
["RO3杀菌计时开关","C5.M5.RO3_SJJSKG"]
["RO3杀菌步序","C5.M5.RO3_SJBX"]
["RO4杀菌启动","C5.M5.RO4_SJQD"]
["RO4杀菌时长设定 ","C5.M5.RO4_SJSCSD"]
["RO4杀菌时长显示","C5.M5.RO4_SJSCXS"]
["RO4杀菌计时开关","C5.M5.RO4_SJJSKG"]
["RO4杀菌步序","C5.M5.RO4_SJBX"]
["RO1一段故障复位","C5.M5.RO1_YDGZFW"]
["RO1一段反冲加药选择","C5.M5.RO1_YDFCJYXZ"]
["RO1一段是否关联此次反冲","C5.M5.RO1_YDGLFC"]
["RO1一段加药时长设定","C5.M5.RO1_YDJYSCSD"]
["RO1一段加药时长（显示）计时","C5.M5.RO1_YDJYSCXS"]
["RO1一段加药计时开关","C5.M5.RO1_YDJYJSKG"]
["RO1一段加药状态","C5.M5.RO1_YDJYZT"]
["RO1二段故障复位","C5.M5.RO1_EDGZFW"]
["RO1二段反冲加药选择","C5.M5.RO1_EDFCJYXZ"]
["RO1二段是否关联此次反冲","C5.M5.RO1_EDGLFC"]
["RO1二段加药时长设定","C5.M5.RO1_EDJYSCSD"]
["RO1二段加药时长（显示）计时","C5.M5.RO1_EDJYSCXS"]
["RO1二段加药计时开关","C5.M5.RO1_EDJYJSKG"]
["RO1二段加药状态","C5.M5.RO1_EDJYZT"]
["RO2一段故障复位","C5.M5.RO2_YDGZFW"]
["RO2一段反冲加药选择","C5.M5.RO2_YDFCJYXZ"]
["RO2一段是否关联此次反冲","C5.M5.RO2_YDGLFC"]
["RO2一段加药时长设定","C5.M5.RO2_YDJYSCSD"]
["RO2一段加药时长（显示）计时","C5.M5.RO2_YDJYSCXS"]
["RO2一段加药计时开关","C5.M5.RO2_YDJYJSKG"]
["RO2一段加药状态","C5.M5.RO2_YDJYZT"]
["RO2二段故障复位","C5.M5.RO2_EDGZFW"]
["RO2二段反冲加药选择","C5.M5.RO2_EDFCJYXZ"]
["RO2二段是否关联此次反冲","C5.M5.RO2_EDGLFC"]
["RO2二段加药时长设定","C5.M5.RO2_EDJYSCSD"]
["RO2二段加药时长（显示）计时","C5.M5.RO2_EDJYSCXS"]
["RO2二段加药计时开关","C5.M5.RO2_EDJYJSKG"]
["RO2二段加药状态","C5.M5.RO2_EDJYZT"]
["RO3一段故障复位","C5.M5.RO3_YDGZFW"]
["RO3一段反冲加药选择","C5.M5.RO3_YDFCJYXZ"]
["RO3一段是否关联此次反冲","C5.M5.RO3_YDGLFC"]
["RO3一段加药时长设定","C5.M5.RO3_YDJYSCSD"]
["RO3一段加药时长（显示）计时","C5.M5.RO3_YDJYSCXS"]
["RO3一段加药计时开关","C5.M5.RO3_YDJYJSKG"]
["RO3一段加药状态","C5.M5.RO3_YDJYZT"]
["RO3二段故障复位","C5.M5.RO3_EDGZFW"]
["RO3二段反冲加药选择","C5.M5.RO3_EDFCJYXZ"]
["RO3二段是否关联此次反冲","C5.M5.RO3_EDGLFC"]
["RO3二段加药时长设定","C5.M5.RO3_EDJYSCSD"]
["RO3二段加药时长（显示）计时","C5.M5.RO3_EDJYSCXS"]
["RO3二段加药计时开关","C5.M5.RO3_EDJYJSKG"]
["RO3二段加药状态","C5.M5.RO3_EDJYZT"]
["RO4一段故障复位","C5.M5.RO4_YDGZFW"]
["RO4一段反冲加药选择","C5.M5.RO4_YDFCJYXZ"]
["RO4一段是否关联此次反冲","C5.M5.RO4_YDGLFC"]
["RO4一段加药时长设定","C5.M5.RO4_YDJYSCSD"]
["RO4一段加药时长（显示）计时","C5.M5.RO4_YDJYSCXS"]
["RO4一段加药计时开关","C5.M5.RO4_YDJYJSKG"]
["RO4一段加药状态","C5.M5.RO4_YDJYZT"]
["RO4二段故障复位","C5.M5.RO4_EDGZFW"]
["RO4二段反冲加药选择","C5.M5.RO4_EDFCJYXZ"]
["RO4二段是否关联此次反冲","C5.M5.RO4_EDGLFC"]
["RO4二段加药时长设定","C5.M5.RO4_EDJYSCSD"]
["RO4二段加药时长（显示）计时","C5.M5.RO4_EDJYSCXS"]
["RO4二段加药计时开关","C5.M5.RO4_EDJYJSKG"]
["RO4二段加药状态","C5.M5.RO4_EDJYZT"]
["报警红灯","C.M.faultLampRed"]
["报警绿灯","C.M.faultLampGreen"]
["报警蓝灯","C.M.faultLampBlue"]
["报警器","C.M.faultAlarm"]
["报警灯备用1","C.M.faultLampZBY1"]
["报警灯备用2","C.M.faultLampZBY2"]
["高德PH","OPC.GD.P11.PH"]
["高德PH低报警","OPC.GD.P11.PH_L_BJ"]
["高德PH低设定","OPC.GD.P11.PH_L_SD"]
["高德PH高报警","OPC.GD.P11.PH_H_BJ"]
["高德PH高设定","OPC.GD.P11.PH_H_SD"]
["高德电导率","OPC.GD.P11.DDL"]
["高德电导率_A","OPC.GD.P11.DDL_A"]
["高德电导率低报警","OPC.GD.P11.DDL_L_BJ"]
["高德电导率低设定","OPC.GD.P11.DDL_L_SD"]
["高德电导率高报警","OPC.GD.P11.DDL_H_BJ"]
["高德电导率高设定","OPC.GD.P11.DDL_H_SD"]
["高德累计流量","OPC.GD.P11.LJLL"]
["高德瞬时流量","OPC.GD.P11.SSLL"]
["健鼎PH","OPC.JD.P21.PH"]
["健鼎PH低报警","OPC.JD.P21.PH_L_BJ"]
["健鼎PH低设定","OPC.JD.P21.PH_L_SD"]
["健鼎PH高报警","OPC.JD.P21.PH_H_BJ"]
["健鼎PH高设定","OPC.JD.P21.PH_H_SD"]
["健鼎电导率","OPC.JD.P21.DDL"]
["健鼎电导率_A","OPC.JD.P21.DDL_A"]
["健鼎电导率低报警","OPC.JD.P21.DDL_L_BJ"]
["健鼎电导率低设定","OPC.JD.P21.DDL_L_SD"]
["健鼎电导率高报警","OPC.JD.P21.DDL_H_BJ"]
["健鼎电导率高设定","OPC.JD.P21.DDL_H_SD"]
["健鼎累计流量","OPC.JD.P21.LJLL"]
["健鼎瞬时流量","OPC.JD.P21.SSLL"]
["健鼎调节阀反馈","OPC.JD.P22.TJF_FK"]
["健鼎调节阀设定","OPC.JD.P22.TJF_SD"]
["能达PH","OPC.ND.P31.PH"]
["能达PH低报警","OPC.ND.P31.PH_L_BJ"]
["能达PH低设定","OPC.ND.P31.PH_L_SD"]
["能达PH高报警","OPC.ND.P31.PH_H_BJ"]
["能达PH高设定","OPC.ND.P31.PH_H_SD"]
["能达电导率","OPC.ND.P31.DDL"]
["能达电导率_A","OPC.ND.P31.DDL_A"]
["能达电导率低报警","OPC.ND.P31.DDL_L_BJ"]
["能达电导率低设定","OPC.ND.P31.DDL_L_SD"]
["能达电导率高报警","OPC.ND.P31.DDL_H_BJ"]
["能达电导率高设定","OPC.ND.P31.DDL_H_SD"]
["能达累计流量","OPC.ND.P32.LJLL"]
["能达瞬时流量","OPC.ND.P32.SSLL"]
["统盟2厂PH","OPC.TM.P41.PH"]
["统盟2厂PH低报警","OPC.TM.P41.PH_L_BJ"]
["统盟2厂PH低设定","OPC.TM.P41.PH_L_SD"]
["统盟2厂PH高报警","OPC.TM.P41.PH_H_BJ"]
["统盟2厂PH高设定","OPC.TM.P41.PH_H_SD"]
["统盟2厂电导率","OPC.TM.P41.DDL"]
["统盟2厂电导率_A","OPC.TM.P41.DDL_A"]
["统盟2厂电导率低报警","OPC.TM.P41.DDL_L_BJ"]
["统盟2厂电导率低设定","OPC.TM.P41.DDL_L_SD"]
["统盟2厂电导率高报警","OPC.TM.P41.DDL_H_BJ"]
["统盟2厂电导率高设定","OPC.TM.P41.DDL_H_SD"]
["统盟2厂累计流量","OPC.TM.P41.LJLL"]
["统盟2厂瞬时流量","OPC.TM.P41.SSLL"]
["反渗透回收率","ROHSL"]
["高压配电室温度","C2.M21.WD1"]
["管廊间温度1","C2.M22.WD2"]
["管廊间温度2","C2.M23.WD3"]
["低压配电室温度","C2.M24.WD4"]
["膜车间温度1","C2.M25.WD5"]
["膜车间温度2","C2.M26.WD6"]
["加药间温度1","C3.M31.WD7"]
["泵房温度1","C3.M32.WD8"]
["泵房温度2","C3.M33.WD9"]
["加药间温度2","C3.M34.WD10"]
["超滤供水泵A 相电压A","WG_A.1AA1-1.A1"]
["超滤供水泵A 相电压B","WG_A.1AA1-1.A2"]
["超滤供水泵A 相电压C","WG_A.1AA1-1.A3"]
["超滤供水泵A 相电流A","WG_A.1AA1-1.A7"]
["超滤供水泵A 相电流B","WG_A.1AA1-1.A8"]
["超滤供水泵A 相电流C","WG_A.1AA1-1.A9"]
["超滤供水泵A 功率","WG_A.1AA1-1.A13"]
["超滤供水泵A 功率因数","WG_A.1AA1-1.A58"]
["超滤供水泵A 累计电量","_AdvancedTags.1AA1_1_LJ"]
["超滤供水泵B 相电压A","WG_A.1AA1-2.A1"]
["超滤供水泵B 相电压B","WG_A.1AA1-2.A2"]
["超滤供水泵B 相电压C","WG_A.1AA1-2.A3"]
["超滤供水泵B 相电流A","WG_A.1AA1-2.A7"]
["超滤供水泵B 相电流B","WG_A.1AA1-2.A8"]
["超滤供水泵B 相电流C","WG_A.1AA1-2.A9"]
["超滤供水泵B 功率","WG_A.1AA1-2.A13"]
["超滤供水泵B 功率因数","WG_A.1AA1-2.A58"]
["超滤供水泵B 累计电量","_AdvancedTags.1AA1_2_LJ"]
["超滤反洗泵A 相电压A","WG_A.1AA2-1.A1"]
["超滤反洗泵A 相电压B","WG_A.1AA2-1.A2"]
["超滤反洗泵A 相电压C","WG_A.1AA2-1.A3"]
["超滤反洗泵A 相电流A","WG_A.1AA2-1.A7"]
["超滤反洗泵A 相电流B","WG_A.1AA2-1.A8"]
["超滤反洗泵A 相电流C","WG_A.1AA2-1.A9"]
["超滤反洗泵A 功率","WG_A.1AA2-1.A13"]
["超滤反洗泵A 功率因数","WG_A.1AA2-1.A58"]
["超滤反洗泵A 累计电量","_AdvancedTags.1AA2_1_LJ"]
["超滤反洗泵B 相电压A","WG_A.1AA2-2.A1"]
["超滤反洗泵B 相电压B","WG_A.1AA2-2.A2"]
["超滤反洗泵B 相电压C","WG_A.1AA2-2.A3"]
["超滤反洗泵B 相电流A","WG_A.1AA2-2.A7"]
["超滤反洗泵B 相电流B","WG_A.1AA2-2.A8"]
["超滤反洗泵B 相电流C","WG_A.1AA2-2.A9"]
["超滤反洗泵B 功率","WG_A.1AA2-2.A13"]
["超滤反洗泵B 功率因数","WG_A.1AA2-2.A58"]
["超滤反洗泵B 累计电量","_AdvancedTags.1AA2_2_LJ"]
["RO高压泵A 相电压A","WG_A.1AA3.A1"]
["RO高压泵A 相电压B","WG_A.1AA3.A2"]
["RO高压泵A 相电压C","WG_A.1AA3.A3"]
["RO高压泵A 相电流A","WG_A.1AA3.A7"]
["RO高压泵A 相电流B","WG_A.1AA3.A8"]
["RO高压泵A 相电流C","WG_A.1AA3.A9"]
["RO高压泵A 功率","WG_A.1AA3.A13"]
["RO高压泵A 功率因数","WG_A.1AA3.A58"]
["RO高压泵A 累计电量","_AdvancedTags.1AA3_LJ"]
["RO高压泵B 相电压A","WG_A.1AA4.A1"]
["RO高压泵B 相电压B","WG_A.1AA4.A2"]
["RO高压泵B 相电压C","WG_A.1AA4.A3"]
["RO高压泵B 相电流A","WG_A.1AA4.A7"]
["RO高压泵B 相电流B","WG_A.1AA4.A8"]
["RO高压泵B 相电流C","WG_A.1AA4.A9"]
["RO高压泵B 功率","WG_A.1AA4.A13"]
["RO高压泵B 功率因数","WG_A.1AA4.A58"]
["RO高压泵B 累计电量","_AdvancedTags.1AA4_LJ"]
["RO段间泵A 相电压A","WG_A.1AA5-1.A1"]
["RO段间泵A 相电压B","WG_A.1AA5-1.A2"]
["RO段间泵A 相电压C","WG_A.1AA5-1.A3"]
["RO段间泵A 相电流A","WG_A.1AA5-1.A7"]
["RO段间泵A 相电流B","WG_A.1AA5-1.A8"]
["RO段间泵A 相电流C","WG_A.1AA5-1.A9"]
["RO段间泵A 功率","WG_A.1AA5-1.A13"]
["RO段间泵A 功率因数","WG_A.1AA5-1.A58"]
["RO段间泵A 累计电量","_AdvancedTags.1AA5_1_LJ"]
["RO段间泵B 相电压A","WG_A.1AA5-2.A1"]
["RO段间泵B 相电压B","WG_A.1AA5-2.A2"]
["RO段间泵B 相电压C","WG_A.1AA5-2.A3"]
["RO段间泵B 相电流A","WG_A.1AA5-2.A7"]
["RO段间泵B 相电流B","WG_A.1AA5-2.A8"]
["RO段间泵B 相电流C","WG_A.1AA5-2.A9"]
["RO段间泵B 功率","WG_A.1AA5-2.A13"]
["RO段间泵B 功率因数","WG_A.1AA5-2.A58"]
["RO段间泵B 累计电量","_AdvancedTags.1AA5_2_LJ"]
["RO外供水泵A 相电压A","WG_A.1AA6.A1"]
["RO外供水泵A 相电压B","WG_A.1AA6.A2"]
["RO外供水泵A 相电压C","WG_A.1AA6.A3"]
["RO外供水泵A 相电流A","WG_A.1AA6.A7"]
["RO外供水泵A 相电流B","WG_A.1AA6.A8"]
["RO外供水泵A 相电流C","WG_A.1AA6.A9"]
["RO外供水泵A 功率","WG_A.1AA6.A13"]
["RO外供水泵A 功率因数","WG_A.1AA6.A58"]
["RO外供水泵A 累计电量","_AdvancedTags.1AA6_LJ"]
["大水量冲洗泵A 相电压A","WG_A.1AA7-1.A1"]
["大水量冲洗泵A 相电压B","WG_A.1AA7-1.A2"]
["大水量冲洗泵A 相电压C","WG_A.1AA7-1.A3"]
["大水量冲洗泵A 相电流A","WG_A.1AA7-1.A7"]
["大水量冲洗泵A 相电流B","WG_A.1AA7-1.A8"]
["大水量冲洗泵A 相电流C","WG_A.1AA7-1.A9"]
["大水量冲洗泵A 功率","WG_A.1AA7-1.A13"]
["大水量冲洗泵A 功率因数","WG_A.1AA7-1.A58"]
["大水量冲洗泵A 累计电量","_AdvancedTags.1AA7_1_LJ"]
["化学清洗水泵A 相电压A","WG_A.1AA7-2.A1"]
["化学清洗水泵A 相电压B","WG_A.1AA7-2.A2"]
["化学清洗水泵A 相电压C","WG_A.1AA7-2.A3"]
["化学清洗水泵A 相电流A","WG_A.1AA7-2.A7"]
["化学清洗水泵A 相电流B","WG_A.1AA7-2.A8"]
["化学清洗水泵A 相电流C","WG_A.1AA7-2.A9"]
["化学清洗水泵A 功率","WG_A.1AA7-2.A13"]
["化学清洗水泵A 功率因数","WG_A.1AA7-2.A58"]
["化学清洗水泵A 累计电量","_AdvancedTags.1AA7_2_LJ"]
["脱碳风机A 相电压A","WG_B.1AA8-1.A1"]
["脱碳风机A 相电压B","WG_B.1AA8-1.A2"]
["脱碳风机A 相电压C","WG_B.1AA8-1.A3"]
["脱碳风机A 相电流A","WG_B.1AA8-1.A7"]
["脱碳风机A 相电流B","WG_B.1AA8-1.A8"]
["脱碳风机A 相电流C","WG_B.1AA8-1.A9"]
["脱碳风机A 功率","WG_B.1AA8-1.A13"]
["脱碳风机A 功率因数","WG_B.1AA8-1.A58"]
["脱碳风机A 累计电量","_AdvancedTags.1AA8_1_LJ"]
["脱碳风机B 相电压A","WG_B.1AA8-2.A1"]
["脱碳风机B 相电压B","WG_B.1AA8-2.A2"]
["脱碳风机B 相电压C","WG_B.1AA8-2.A3"]
["脱碳风机B 相电流A","WG_B.1AA8-2.A7"]
["脱碳风机B 相电流B","WG_B.1AA8-2.A8"]
["脱碳风机B 相电流C","WG_B.1AA8-2.A9"]
["脱碳风机B 功率","WG_B.1AA8-2.A13"]
["脱碳风机B 功率因数","WG_B.1AA8-2.A58"]
["脱碳风机B 累计电量","_AdvancedTags.1AA8_2_LJ"]
["中和废水泵A 相电压A","WG_B.1AA8-3.A1"]
["中和废水泵A 相电压B","WG_B.1AA8-3.A2"]
["中和废水泵A 相电压C","WG_B.1AA8-3.A3"]
["中和废水泵A 相电流A","WG_B.1AA8-3.A7"]
["中和废水泵A 相电流B","WG_B.1AA8-3.A8"]
["中和废水泵A 相电流C","WG_B.1AA8-3.A9"]
["中和废水泵A 功率","WG_B.1AA8-3.A13"]
["中和废水泵A 功率因数","WG_B.1AA8-3.A58"]
["中和废水泵A 累计电量","_AdvancedTags.1AA8_3_LJ"]
["中和废水泵B 相电压A","WG_B.1AA8-4.A1"]
["中和废水泵B 相电压B","WG_B.1AA8-4.A2"]
["中和废水泵B 相电压C","WG_B.1AA8-4.A3"]
["中和废水泵B 相电流A","WG_B.1AA8-4.A7"]
["中和废水泵B 相电流B","WG_B.1AA8-4.A8"]
["中和废水泵B 相电流C","WG_B.1AA8-4.A9"]
["中和废水泵B 功率","WG_B.1AA8-4.A13"]
["中和废水泵B 功率因数","WG_B.1AA8-4.A58"]
["中和废水泵B 累计电量","_AdvancedTags.1AA8_4_LJ"]
["清洗水箱电加热器A 相电压A","WG_B.1AA8-5.A1"]
["清洗水箱电加热器A 相电压B","WG_B.1AA8-5.A2"]
["清洗水箱电加热器A 相电压C","WG_B.1AA8-5.A3"]
["清洗水箱电加热器A 相电流A","WG_B.1AA8-5.A7"]
["清洗水箱电加热器A 相电流B","WG_B.1AA8-5.A8"]
["清洗水箱电加热器A 相电流C","WG_B.1AA8-5.A9"]
["清洗水箱电加热器A 功率","WG_B.1AA8-5.A13"]
["清洗水箱电加热器A 功率因数","WG_B.1AA8-5.A58"]
["清洗水箱电加热器A 累计电量","_AdvancedTags.1AA8_5_LJ"]
["清洗水箱电加热器B 相电压A","WG_B.1AA8-6.A1"]
["清洗水箱电加热器B 相电压B","WG_B.1AA8-6.A2"]
["清洗水箱电加热器B 相电压C","WG_B.1AA8-6.A3"]
["清洗水箱电加热器B 相电流A","WG_B.1AA8-6.A7"]
["清洗水箱电加热器B 相电流B","WG_B.1AA8-6.A8"]
["清洗水箱电加热器B 相电流C","WG_B.1AA8-6.A9"]
["清洗水箱电加热器B 功率","WG_B.1AA8-6.A13"]
["清洗水箱电加热器B 功率因数","WG_B.1AA8-6.A58"]
["清洗水箱电加热器B 累计电量","_AdvancedTags.1AA8_6_LJ"]
["泵房潜污泵A 相电压A","WG_B.1AA9-1.A1"]
["泵房潜污泵A 相电压B","WG_B.1AA9-1.A2"]
["泵房潜污泵A 相电压C","WG_B.1AA9-1.A3"]
["泵房潜污泵A 相电流A","WG_B.1AA9-1.A7"]
["泵房潜污泵A 相电流B","WG_B.1AA9-1.A8"]
["泵房潜污泵A 相电流C","WG_B.1AA9-1.A9"]
["泵房潜污泵A 功率","WG_B.1AA9-1.A13"]
["泵房潜污泵A 功率因数","WG_B.1AA9-1.A58"]
["泵房潜污泵A 累计电量","_AdvancedTags.1AA9_1_LJ"]
["泵房潜污泵B 相电压A","WG_B.1AA9-2.A1"]
["泵房潜污泵B 相电压B","WG_B.1AA9-2.A2"]
["泵房潜污泵B 相电压C","WG_B.1AA9-2.A3"]
["泵房潜污泵B 相电流A","WG_B.1AA9-2.A7"]
["泵房潜污泵B 相电流B","WG_B.1AA9-2.A8"]
["泵房潜污泵B 相电流C","WG_B.1AA9-2.A9"]
["泵房潜污泵B 功率","WG_B.1AA9-2.A13"]
["泵房潜污泵B 功率因数","WG_B.1AA9-2.A58"]
["泵房潜污泵B 累计电量","_AdvancedTags.1AA9_2_LJ"]
["泵房潜污泵C 相电压A","WG_B.1AA9-3.A1"]
["泵房潜污泵C 相电压B","WG_B.1AA9-3.A2"]
["泵房潜污泵C 相电压C","WG_B.1AA9-3.A3"]
["泵房潜污泵C 相电流A","WG_B.1AA9-3.A7"]
["泵房潜污泵C 相电流B","WG_B.1AA9-3.A8"]
["泵房潜污泵C 相电流C","WG_B.1AA9-3.A9"]
["泵房潜污泵C 功率","WG_B.1AA9-3.A13"]
["泵房潜污泵C 功率因数","WG_B.1AA9-3.A58"]
["泵房潜污泵C 累计电量","_AdvancedTags.1AA9_3_LJ"]
["泵房潜污泵D 相电压A","WG_B.1AA9-4.A1"]
["泵房潜污泵D 相电压B","WG_B.1AA9-4.A2"]
["泵房潜污泵D 相电压C","WG_B.1AA9-4.A3"]
["泵房潜污泵D 相电流A","WG_B.1AA9-4.A7"]
["泵房潜污泵D 相电流B","WG_B.1AA9-4.A8"]
["泵房潜污泵D 相电流C","WG_B.1AA9-4.A9"]
["泵房潜污泵D 功率","WG_B.1AA9-4.A13"]
["泵房潜污泵D 功率因数","WG_B.1AA9-4.A58"]
["泵房潜污泵D 累计电量","_AdvancedTags.1AA9_4_LJ"]
["空压机A 相电压A","WG_B.1AA9-5.A1"]
["空压机A 相电压B","WG_B.1AA9-5.A2"]
["空压机A 相电压C","WG_B.1AA9-5.A3"]
["空压机A 相电流A","WG_B.1AA9-5.A7"]
["空压机A 相电流B","WG_B.1AA9-5.A8"]
["空压机A 相电流C","WG_B.1AA9-5.A9"]
["空压机A 功率","WG_B.1AA9-5.A13"]
["空压机A 功率因数","WG_B.1AA9-5.A58"]
["空压机A 累计电量","_AdvancedTags.1AA9_5_LJ"]
["空压机B 相电压A","WG_B.1AA9-6.A1"]
["空压机B 相电压B","WG_B.1AA9-6.A2"]
["空压机B 相电压C","WG_B.1AA9-6.A3"]
["空压机B 相电流A","WG_B.1AA9-6.A7"]
["空压机B 相电流B","WG_B.1AA9-6.A8"]
["空压机B 相电流C","WG_B.1AA9-6.A9"]
["空压机B 功率","WG_B.1AA9-6.A13"]
["空压机B 功率因数","WG_B.1AA9-6.A58"]
["空压机B 累计电量","_AdvancedTags.1AA9_6_LJ"]
["供水泵房间电动葫芦 相电压A","WG_B.1AA9-7.A1"]
["供水泵房间电动葫芦 相电压B","WG_B.1AA9-7.A2"]
["供水泵房间电动葫芦 相电压C","WG_B.1AA9-7.A3"]
["供水泵房间电动葫芦 相电流A","WG_B.1AA9-7.A7"]
["供水泵房间电动葫芦 相电流B","WG_B.1AA9-7.A8"]
["供水泵房间电动葫芦 相电流C","WG_B.1AA9-7.A9"]
["供水泵房间电动葫芦 功率","WG_B.1AA9-7.A13"]
["供水泵房间电动葫芦 功率因数","WG_B.1AA9-7.A58"]
["供水泵房间电动葫芦 累计电量","_AdvancedTags.1AA9_7_LJ"]
["UPS柜 相电压A","WG_B.1AA9-8.A1"]
["UPS柜 相电压B","WG_B.1AA9-8.A2"]
["UPS柜 相电压C","WG_B.1AA9-8.A3"]
["UPS柜 相电流A","WG_B.1AA9-8.A7"]
["UPS柜 相电流B","WG_B.1AA9-8.A8"]
["UPS柜 相电流C","WG_B.1AA9-8.A9"]
["UPS柜 功率","WG_B.1AA9-8.A13"]
["UPS柜 功率因数","WG_B.1AA9-8.A58"]
["UPS柜 累计电量","_AdvancedTags.1AA9_8_LJ"]
["轴流风机柜 相电压A","WG_B.1AA9-9.A1"]
["轴流风机柜 相电压B","WG_B.1AA9-9.A2"]
["轴流风机柜 相电压C","WG_B.1AA9-9.A3"]
["轴流风机柜 相电流A","WG_B.1AA9-9.A7"]
["轴流风机柜 相电流B","WG_B.1AA9-9.A8"]
["轴流风机柜 相电流C","WG_B.1AA9-9.A9"]
["轴流风机柜 功率","WG_B.1AA9-9.A13"]
["轴流风机柜 功率因数","WG_B.1AA9-9.A58"]
["轴流风机柜 累计电量","_AdvancedTags.1AA9_9_LJ"]
["辅助用房 相电压A","WG_B.1AA10-1.A1"]
["辅助用房 相电压B","WG_B.1AA10-1.A2"]
["辅助用房 相电压C","WG_B.1AA10-1.A3"]
["辅助用房 相电流A","WG_B.1AA10-1.A7"]
["辅助用房 相电流B","WG_B.1AA10-1.A8"]
["辅助用房 相电流C","WG_B.1AA10-1.A9"]
["辅助用房 功率","WG_B.1AA10-1.A13"]
["辅助用房 功率因数","WG_B.1AA10-1.A58"]
["辅助用房 累计电量","_AdvancedTags.1AA10_1_LJ"]
["门卫 相电压A","WG_B.1AA10-2.A1"]
["门卫 相电压B","WG_B.1AA10-2.A2"]
["门卫 相电压C","WG_B.1AA10-2.A3"]
["门卫 相电流A","WG_B.1AA10-2.A7"]
["门卫 相电流B","WG_B.1AA10-2.A8"]
["门卫 相电流C","WG_B.1AA10-2.A9"]
["门卫 功率","WG_B.1AA10-2.A13"]
["门卫 功率因数","WG_B.1AA10-2.A58"]
["门卫 累计电量","_AdvancedTags.1AA10_2_LJ"]
["夹层中控室空调 相电压A","WG_B.1AA10-3.A1"]
["夹层中控室空调 相电压B","WG_B.1AA10-3.A2"]
["夹层中控室空调 相电压C","WG_B.1AA10-3.A3"]
["夹层中控室空调 相电流A","WG_B.1AA10-3.A7"]
["夹层中控室空调 相电流B","WG_B.1AA10-3.A8"]
["夹层中控室空调 相电流C","WG_B.1AA10-3.A9"]
["夹层中控室空调 功率","WG_B.1AA10-3.A13"]
["夹层中控室空调 功率因数","WG_B.1AA10-3.A58"]
["夹层中控室空调 累计电量","_AdvancedTags.1AA10_3_LJ"]
["夹层低压配电间空调 相电压A","WG_B.1AA10-4.A1"]
["夹层低压配电间空调 相电压B","WG_B.1AA10-4.A2"]
["夹层低压配电间空调 相电压C","WG_B.1AA10-4.A3"]
["夹层低压配电间空调 相电流A","WG_B.1AA10-4.A7"]
["夹层低压配电间空调 相电流B","WG_B.1AA10-4.A8"]
["夹层低压配电间空调 相电流C","WG_B.1AA10-4.A9"]
["夹层低压配电间空调 功率","WG_B.1AA10-4.A13"]
["夹层低压配电间空调 功率因数","WG_B.1AA10-4.A58"]
["夹层低压配电间空调 累计电量","_AdvancedTags.1AA10_4_LJ"]
["一层高压配电间空调 相电压A","WG_B.1AA10-5.A1"]
["一层高压配电间空调 相电压B","WG_B.1AA10-5.A2"]
["一层高压配电间空调 相电压C","WG_B.1AA10-5.A3"]
["一层高压配电间空调 相电流A","WG_B.1AA10-5.A7"]
["一层高压配电间空调 相电流B","WG_B.1AA10-5.A8"]
["一层高压配电间空调 相电流C","WG_B.1AA10-5.A9"]
["一层高压配电间空调 功率","WG_B.1AA10-5.A13"]
["一层高压配电间空调 功率因数","WG_B.1AA10-5.A58"]
["一层高压配电间空调 累计电量","_AdvancedTags.1AA10_5_LJ"]
["照明箱 相电压A","WG_B.1AA10-6.A1"]
["照明箱 相电压B","WG_B.1AA10-6.A2"]
["照明箱 相电压C","WG_B.1AA10-6.A3"]
["照明箱 相电流A","WG_B.1AA10-6.A7"]
["照明箱 相电流B","WG_B.1AA10-6.A8"]
["照明箱 相电流C","WG_B.1AA10-6.A9"]
["照明箱 功率","WG_B.1AA10-6.A13"]
["照明箱 功率因数","WG_B.1AA10-6.A58"]
["照明箱 累计电量","_AdvancedTags.1AA10_6_LJ"]
["超滤供水泵D 相电压A","WG_B.1AA11.A1"]
["超滤供水泵D 相电压B","WG_B.1AA11.A2"]
["超滤供水泵D 相电压C","WG_B.1AA11.A3"]
["超滤供水泵D 相电流A","WG_B.1AA11.A7"]
["超滤供水泵D 相电流B","WG_B.1AA11.A8"]
["超滤供水泵D 相电流C","WG_B.1AA11.A9"]
["超滤供水泵D 功率","WG_B.1AA11.A13"]
["超滤供水泵D 功率因数","WG_B.1AA11.A58"]
["超滤供水泵D 累计电量","_AdvancedTags.1AA11_LJ"]
["超滤供水泵C 相电压A","WG_C.2AA1-1.A1"]
["超滤供水泵C 相电压B","WG_C.2AA1-1.A2"]
["超滤供水泵C 相电压C","WG_C.2AA1-1.A3"]
["超滤供水泵C 相电流A","WG_C.2AA1-1.A7"]
["超滤供水泵C 相电流B","WG_C.2AA1-1.A8"]
["超滤供水泵C 相电流C","WG_C.2AA1-1.A9"]
["超滤供水泵C 功率","WG_C.2AA1-1.A13"]
["超滤供水泵C 功率因数","WG_C.2AA1-1.A58"]
["超滤供水泵C 累计电量","_AdvancedTags.2AA1_1_LJ"]
["超滤反洗泵C 相电压A","WG_C.2AA1-2.A1"]
["超滤反洗泵C 相电压B","WG_C.2AA1-2.A2"]
["超滤反洗泵C 相电压C","WG_C.2AA1-2.A3"]
["超滤反洗泵C 相电流A","WG_C.2AA1-2.A7"]
["超滤反洗泵C 相电流B","WG_C.2AA1-2.A8"]
["超滤反洗泵C 相电流C","WG_C.2AA1-2.A9"]
["超滤反洗泵C 功率","WG_C.2AA1-2.A13"]
["超滤反洗泵C 功率因数","WG_C.2AA1-2.A58"]
["超滤反洗泵C 累计电量","_AdvancedTags.2AA1_2_LJ"]
["RO高压泵C 相电压A","WG_C.2AA2.A1"]
["RO高压泵C 相电压B","WG_C.2AA2.A2"]
["RO高压泵C 相电压C","WG_C.2AA2.A3"]
["RO高压泵C 相电流A","WG_C.2AA2.A7"]
["RO高压泵C 相电流B","WG_C.2AA2.A8"]
["RO高压泵C 相电流C","WG_C.2AA2.A9"]
["RO高压泵C 功率","WG_C.2AA2.A13"]
["RO高压泵C 功率因数","WG_C.2AA2.A58"]
["RO高压泵C 累计电量","_AdvancedTags.2AA2_LJ"]
["RO高压泵D 相电压A","WG_C.2AA3.A1"]
["RO高压泵D 相电压B","WG_C.2AA3.A2"]
["RO高压泵D 相电压C","WG_C.2AA3.A3"]
["RO高压泵D 相电流A","WG_C.2AA3.A7"]
["RO高压泵D 相电流B","WG_C.2AA3.A8"]
["RO高压泵D 相电流C","WG_C.2AA3.A9"]
["RO高压泵D 功率","WG_C.2AA3.A13"]
["RO高压泵D 功率因数","WG_C.2AA3.A58"]
["RO高压泵D 累计电量","_AdvancedTags.2AA3_LJ"]
["RO段间泵C 相电压A","WG_C.2AA4-1.A1"]
["RO段间泵C 相电压B","WG_C.2AA4-1.A2"]
["RO段间泵C 相电压C","WG_C.2AA4-1.A3"]
["RO段间泵C 相电流A","WG_C.2AA4-1.A7"]
["RO段间泵C 相电流B","WG_C.2AA4-1.A8"]
["RO段间泵C 相电流C","WG_C.2AA4-1.A9"]
["RO段间泵C 功率","WG_C.2AA4-1.A13"]
["RO段间泵C 功率因数","WG_C.2AA4-1.A58"]
["RO段间泵C 累计电量","_AdvancedTags.2AA4_1_LJ"]
["RO段间泵D 相电压A","WG_C.2AA4-2.A1"]
["RO段间泵D 相电压B","WG_C.2AA4-2.A2"]
["RO段间泵D 相电压C","WG_C.2AA4-2.A3"]
["RO段间泵D 相电流A","WG_C.2AA4-2.A7"]
["RO段间泵D 相电流B","WG_C.2AA4-2.A8"]
["RO段间泵D 相电流C","WG_C.2AA4-2.A9"]
["RO段间泵D 功率","WG_C.2AA4-2.A13"]
["RO段间泵D 功率因数","WG_C.2AA4-2.A58"]
["RO段间泵D 累计电量","_AdvancedTags.2AA4_2_LJ"]
["RO外供水泵B 相电压A","WG_C.2AA5.A1"]
["RO外供水泵B 相电压B","WG_C.2AA5.A2"]
["RO外供水泵B 相电压C","WG_C.2AA5.A3"]
["RO外供水泵B 相电流A","WG_C.2AA5.A7"]
["RO外供水泵B 相电流B","WG_C.2AA5.A8"]
["RO外供水泵B 相电流C","WG_C.2AA5.A9"]
["RO外供水泵B 功率","WG_C.2AA5.A13"]
["RO外供水泵B 功率因数","WG_C.2AA5.A58"]
["RO外供水泵B 累计电量","_AdvancedTags.2AA5_LJ"]
["RO外供水泵C 相电压A","WG_C.2AA6.A1"]
["RO外供水泵C 相电压B","WG_C.2AA6.A2"]
["RO外供水泵C 相电压C","WG_C.2AA6.A3"]
["RO外供水泵C 相电流A","WG_C.2AA6.A7"]
["RO外供水泵C 相电流B","WG_C.2AA6.A8"]
["RO外供水泵C 相电流C","WG_C.2AA6.A9"]
["RO外供水泵C 功率","WG_C.2AA6.A13"]
["RO外供水泵C 功率因数","WG_C.2AA6.A58"]
["RO外供水泵C 累计电量","_AdvancedTags.2AA6_LJ"]
["大水量冲洗泵B 相电压A","WG_C.2AA7-1.A1"]
["大水量冲洗泵B 相电压B","WG_C.2AA7-1.A2"]
["大水量冲洗泵B 相电压C","WG_C.2AA7-1.A3"]
["大水量冲洗泵B 相电流A","WG_C.2AA7-1.A7"]
["大水量冲洗泵B 相电流B","WG_C.2AA7-1.A8"]
["大水量冲洗泵B 相电流C","WG_C.2AA7-1.A9"]
["大水量冲洗泵B 功率","WG_C.2AA7-1.A13"]
["大水量冲洗泵B 功率因数","WG_C.2AA7-1.A58"]
["大水量冲洗泵B 累计电量","_AdvancedTags.2AA7_1_LJ"]
["化学清洗水泵B 相电压A","WG_C.2AA7-2.A1"]
["化学清洗水泵B 相电压B","WG_C.2AA7-2.A2"]
["化学清洗水泵B 相电压C","WG_C.2AA7-2.A3"]
["化学清洗水泵B 相电流A","WG_C.2AA7-2.A7"]
["化学清洗水泵B 相电流B","WG_C.2AA7-2.A8"]
["化学清洗水泵B 相电流C","WG_C.2AA7-2.A9"]
["化学清洗水泵B 功率","WG_C.2AA7-2.A13"]
["化学清洗水泵B 功率因数","WG_C.2AA7-2.A58"]
["化学清洗水泵B 累计电量","_AdvancedTags.2AA7_2_LJ"]
["反渗透冲洗水泵A温度","C4.M4.RO_CXB1_WD"]
["超滤供水泵A温度","C4.M4.UF_GSB1_WD"]
["反渗透高压泵A温度","C4.M4.RO1_GYB_WD"]
["反渗透外供水泵A温度","C4.M4.RO_WGB1_WD"]
["超滤反洗水泵A温度","C4.M4.UF_FXB1_WD"]
["段间泵A温度","C4.M4.RO1_DJB_WD"]
["反渗透冲洗水泵AX轴速度","C4.M4.RO_CXB1_XSD"]
["反渗透冲洗水泵AY轴速度","C4.M4.RO_CXB1_YSD"]
["反渗透冲洗水泵AZ轴速度","C4.M4.RO_CXB1_ZSD"]
["反渗透冲洗水泵AX轴位移","C4.M4.RO_CXB1_XWY"]
["反渗透冲洗水泵AY轴位移","C4.M4.RO_CXB1_YWY"]
["反渗透冲洗水泵AZ轴位移","C4.M4.RO_CXB1_ZWY"]
["超滤供水泵AX轴速度","C4.M4.UF_GSB1_XSD"]
["超滤供水泵AY轴速度","C4.M4.UF_GSB1_YSD"]
["超滤供水泵AZ轴速度","C4.M4.UF_GSB1_ZSD"]
["超滤供水泵AX轴位移","C4.M4.UF_GSB1_XWY"]
["超滤供水泵AY轴位移","C4.M4.UF_GSB1_YWY"]
["超滤供水泵AZ轴位移","C4.M4.UF_GSB1_ZWY"]
["反渗透高压泵AX轴速度","C4.M4.RO1_GYB_XSD"]
["反渗透高压泵AY轴速度","C4.M4.RO1_GYB_YSD"]
["反渗透高压泵AZ轴速度","C4.M4.RO1_GYB_ZSD"]
["反渗透高压泵AX轴位移","C4.M4.RO1_GYB_XWY"]
["反渗透高压泵AY轴位移","C4.M4.RO1_GYB_YWY"]
["反渗透高压泵AZ轴位移","C4.M4.RO1_GYB_ZWY"]
["反渗透外供水泵AX轴速度","C4.M4.RO_WGB1_XSD"]
["反渗透外供水泵AY轴速度","C4.M4.RO_WGB1_YSD"]
["反渗透外供水泵AZ轴速度","C4.M4.RO_WGB1_ZSD"]
["反渗透外供水泵AX轴位移","C4.M4.RO_WGB1_XWY"]
["反渗透外供水泵AY轴位移","C4.M4.RO_WGB1_YWY"]
["反渗透外供水泵AZ轴位移","C4.M4.RO_WGB1_ZWY"]
["超滤反洗水泵AX轴速度","C4.M4.UF_FXB1_XSD"]
["超滤反洗水泵AY轴速度","C4.M4.UF_FXB1_YSD"]
["超滤反洗水泵AZ轴速度","C4.M4.UF_FXB1_ZSD"]
["超滤反洗水泵AX轴位移","C4.M4.UF_FXB1_XWY"]
["超滤反洗水泵AY轴位移","C4.M4.UF_FXB1_YWY"]
["超滤反洗水泵AZ轴位移","C4.M4.UF_FXB1_ZWY"]
["段间泵AX轴速度","C4.M4.RO1_DJB_XSD"]
["段间泵AY轴速度","C4.M4.RO1_DJB_YSD"]
["段间泵AZ轴速度","C4.M4.RO1_DJB_ZSD"]
["段间泵AX轴位移","C4.M4.RO1_DJB_XWY"]
["段间泵AY轴位移","C4.M4.RO1_DJB_YWY"]
["段间泵AZ轴位移","C4.M4.RO1_DJB_ZWY"]
["原水池低液位校准开关","C4.M4.LS_JSC_JZL"]
["原水池高液位校准开关","C4.M4.LS_JSC_JZH"]
["阻垢剂药箱低液位校准开关","C4.M4.LS_ZGJ_JZL"]
["阻垢剂药箱高液位校准开关","C4.M4.LS_ZGJ_JZH"]
["阻垢剂加药泵噪音","C4.M4.ZY_ZGJB"]
["阻垢剂加药泵50Hz噪音","C4.M4.ZY_ZGJB_F1"]
["阻垢剂加药泵100Hz噪音","C4.M4.ZY_ZGJB_F2"]
["阻垢剂加药泵150Hz噪音","C4.M4.ZY_ZGJB_F3"]
["阻垢剂加药泵200Hz噪音","C4.M4.ZY_ZGJB_F4"]
["阻垢剂加药泵250Hz噪音","C4.M4.ZY_ZGJB_F5"]
["阻垢剂加药泵300Hz噪音","C4.M4.ZY_ZGJB_F6"]
["阻垢剂加药泵350Hz噪音","C4.M4.ZY_ZGJB_F7"]
["阻垢剂加药泵400Hz噪音","C4.M4.ZY_ZGJB_F8"]
["阻垢剂加药泵450Hz噪音","C4.M4.ZY_ZGJB_F9"]
["阻垢剂加药泵500Hz噪音","C4.M4.ZY_ZGJB_F10"]
["阻垢剂加药泵550Hz噪音","C4.M4.ZY_ZGJB_F11"]
["阻垢剂加药泵600Hz噪音","C4.M4.ZY_ZGJB_F12"]
["阻垢剂加药泵650Hz噪音","C4.M4.ZY_ZGJB_F13"]
["阻垢剂加药泵700Hz噪音","C4.M4.ZY_ZGJB_F14"]
["阻垢剂加药泵750Hz噪音","C4.M4.ZY_ZGJB_F15"]
["阻垢剂加药泵800Hz噪音","C4.M4.ZY_ZGJB_F16"]
["阻垢剂加药泵850Hz噪音","C4.M4.ZY_ZGJB_F17"]
["阻垢剂加药泵900Hz噪音","C4.M4.ZY_ZGJB_F18"]
["阻垢剂加药泵950Hz噪音","C4.M4.ZY_ZGJB_F19"]
["阻垢剂加药泵1000Hz噪音","C4.M4.ZY_ZGJB_F20"]
["阻垢剂加药泵1050Hz噪音","C4.M4.ZY_ZGJB_F21"]
["阻垢剂加药泵1100Hz噪音","C4.M4.ZY_ZGJB_F22"]
["阻垢剂加药泵1150Hz噪音","C4.M4.ZY_ZGJB_F23"]
["阻垢剂加药泵1200Hz噪音","C4.M4.ZY_ZGJB_F24"]
["阻垢剂加药泵1250Hz噪音","C4.M4.ZY_ZGJB_F25"]
["阻垢剂加药泵1300Hz噪音","C4.M4.ZY_ZGJB_F26"]
["阻垢剂加药泵1350Hz噪音","C4.M4.ZY_ZGJB_F27"]
["阻垢剂加药泵1400Hz噪音","C4.M4.ZY_ZGJB_F28"]
["阻垢剂加药泵1450Hz噪音","C4.M4.ZY_ZGJB_F29"]
["阻垢剂加药泵1500Hz噪音","C4.M4.ZY_ZGJB_F30"]
["阻垢剂加药泵1550Hz噪音","C4.M4.ZY_ZGJB_F31"]
["阻垢剂加药泵1600Hz噪音","C4.M4.ZY_ZGJB_F32"]
["阻垢剂加药泵1650Hz噪音","C4.M4.ZY_ZGJB_F33"]
["阻垢剂加药泵1700Hz噪音","C4.M4.ZY_ZGJB_F34"]
["阻垢剂加药泵1750Hz噪音","C4.M4.ZY_ZGJB_F35"]
["阻垢剂加药泵1800Hz噪音","C4.M4.ZY_ZGJB_F36"]
["阻垢剂加药泵1850Hz噪音","C4.M4.ZY_ZGJB_F37"]
["阻垢剂加药泵1900Hz噪音","C4.M4.ZY_ZGJB_F38"]
["阻垢剂加药泵1950Hz噪音","C4.M4.ZY_ZGJB_F39"]
["阻垢剂加药泵2000Hz噪音","C4.M4.ZY_ZGJB_F40"]
["阻垢剂加药泵2050Hz噪音","C4.M4.ZY_ZGJB_F41"]
["阻垢剂加药泵2100Hz噪音","C4.M4.ZY_ZGJB_F42"]
["阻垢剂加药泵2150Hz噪音","C4.M4.ZY_ZGJB_F43"]
["阻垢剂加药泵2200Hz噪音","C4.M4.ZY_ZGJB_F44"]
["阻垢剂加药泵2250Hz噪音","C4.M4.ZY_ZGJB_F45"]
["阻垢剂加药泵2300Hz噪音","C4.M4.ZY_ZGJB_F46"]
["阻垢剂加药泵2350Hz噪音","C4.M4.ZY_ZGJB_F47"]
["阻垢剂加药泵2400Hz噪音","C4.M4.ZY_ZGJB_F48"]
["阻垢剂加药泵2450Hz噪音","C4.M4.ZY_ZGJB_F49"]
["阻垢剂加药泵2500Hz噪音","C4.M4.ZY_ZGJB_F50"]
["阻垢剂加药泵2550Hz噪音","C4.M4.ZY_ZGJB_F51"]
["阻垢剂加药泵2600Hz噪音","C4.M4.ZY_ZGJB_F52"]
["阻垢剂加药泵2650Hz噪音","C4.M4.ZY_ZGJB_F53"]
["阻垢剂加药泵2700Hz噪音","C4.M4.ZY_ZGJB_F54"]
["阻垢剂加药泵2750Hz噪音","C4.M4.ZY_ZGJB_F55"]
["阻垢剂加药泵2800Hz噪音","C4.M4.ZY_ZGJB_F56"]
["阻垢剂加药泵2850Hz噪音","C4.M4.ZY_ZGJB_F57"]
["阻垢剂加药泵2900Hz噪音","C4.M4.ZY_ZGJB_F58"]
["阻垢剂加药泵2950Hz噪音","C4.M4.ZY_ZGJB_F59"]
["阻垢剂加药泵3000Hz噪音","C4.M4.ZY_ZGJB_F60"]
["阻垢剂加药泵3050Hz噪音","C4.M4.ZY_ZGJB_F61"]
["阻垢剂加药泵3100Hz噪音","C4.M4.ZY_ZGJB_F62"]
["阻垢剂加药泵3150Hz噪音","C4.M4.ZY_ZGJB_F63"]
["阻垢剂加药泵3200Hz噪音","C4.M4.ZY_ZGJB_F64"]
["阻垢剂加药泵3250Hz噪音","C4.M4.ZY_ZGJB_F65"]
["阻垢剂加药泵3300Hz噪音","C4.M4.ZY_ZGJB_F66"]
["阻垢剂加药泵3350Hz噪音","C4.M4.ZY_ZGJB_F67"]
["阻垢剂加药泵3400Hz噪音","C4.M4.ZY_ZGJB_F68"]
["阻垢剂加药泵3450Hz噪音","C4.M4.ZY_ZGJB_F69"]
["阻垢剂加药泵3500Hz噪音","C4.M4.ZY_ZGJB_F70"]
["阻垢剂加药泵3550Hz噪音","C4.M4.ZY_ZGJB_F71"]
["阻垢剂加药泵3600Hz噪音","C4.M4.ZY_ZGJB_F72"]
["阻垢剂加药泵3650Hz噪音","C4.M4.ZY_ZGJB_F73"]
["阻垢剂加药泵3700Hz噪音","C4.M4.ZY_ZGJB_F74"]
["阻垢剂加药泵3750Hz噪音","C4.M4.ZY_ZGJB_F75"]
["阻垢剂加药泵3800Hz噪音","C4.M4.ZY_ZGJB_F76"]
["阻垢剂加药泵3850Hz噪音","C4.M4.ZY_ZGJB_F77"]
["阻垢剂加药泵3900Hz噪音","C4.M4.ZY_ZGJB_F78"]
["阻垢剂加药泵3950Hz噪音","C4.M4.ZY_ZGJB_F79"]
["阻垢剂加药泵4000Hz噪音","C4.M4.ZY_ZGJB_F80"]
["阻垢剂加药泵4050Hz噪音","C4.M4.ZY_ZGJB_F81"]
["阻垢剂加药泵4100Hz噪音","C4.M4.ZY_ZGJB_F82"]
["阻垢剂加药泵4150Hz噪音","C4.M4.ZY_ZGJB_F83"]
["阻垢剂加药泵4200Hz噪音","C4.M4.ZY_ZGJB_F84"]
["阻垢剂加药泵4250Hz噪音","C4.M4.ZY_ZGJB_F85"]
["阻垢剂加药泵4300Hz噪音","C4.M4.ZY_ZGJB_F86"]
["阻垢剂加药泵4350Hz噪音","C4.M4.ZY_ZGJB_F87"]
["阻垢剂加药泵4400Hz噪音","C4.M4.ZY_ZGJB_F88"]
["阻垢剂加药泵4450Hz噪音","C4.M4.ZY_ZGJB_F89"]
["阻垢剂加药泵4500Hz噪音","C4.M4.ZY_ZGJB_F90"]
["阻垢剂加药泵4550Hz噪音","C4.M4.ZY_ZGJB_F91"]
["阻垢剂加药泵4600Hz噪音","C4.M4.ZY_ZGJB_F92"]
["阻垢剂加药泵4650Hz噪音","C4.M4.ZY_ZGJB_F93"]
["阻垢剂加药泵4700Hz噪音","C4.M4.ZY_ZGJB_F94"]
["阻垢剂加药泵4750Hz噪音","C4.M4.ZY_ZGJB_F95"]
["阻垢剂加药泵4800Hz噪音","C4.M4.ZY_ZGJB_F96"]
["阻垢剂加药泵4850Hz噪音","C4.M4.ZY_ZGJB_F97"]
["阻垢剂加药泵4900Hz噪音","C4.M4.ZY_ZGJB_F98"]
["阻垢剂加药泵4950Hz噪音","C4.M4.ZY_ZGJB_F99"]
["阻垢剂加药泵5000Hz噪音","C4.M4.ZY_ZGJB_F100"]
["阻垢剂加药泵5050Hz噪音","C4.M4.ZY_ZGJB_F101"]
["阻垢剂加药泵5100Hz噪音","C4.M4.ZY_ZGJB_F102"]
["阻垢剂加药泵5150Hz噪音","C4.M4.ZY_ZGJB_F103"]
["阻垢剂加药泵5200Hz噪音","C4.M4.ZY_ZGJB_F104"]
["阻垢剂加药泵5250Hz噪音","C4.M4.ZY_ZGJB_F105"]
["阻垢剂加药泵5300Hz噪音","C4.M4.ZY_ZGJB_F106"]
["阻垢剂加药泵5350Hz噪音","C4.M4.ZY_ZGJB_F107"]
["阻垢剂加药泵5400Hz噪音","C4.M4.ZY_ZGJB_F108"]
["阻垢剂加药泵5450Hz噪音","C4.M4.ZY_ZGJB_F109"]
["阻垢剂加药泵5500Hz噪音","C4.M4.ZY_ZGJB_F110"]
["阻垢剂加药泵5550Hz噪音","C4.M4.ZY_ZGJB_F111"]
["阻垢剂加药泵5600Hz噪音","C4.M4.ZY_ZGJB_F112"]
["阻垢剂加药泵5650Hz噪音","C4.M4.ZY_ZGJB_F113"]
["阻垢剂加药泵5700Hz噪音","C4.M4.ZY_ZGJB_F114"]
["阻垢剂加药泵5750Hz噪音","C4.M4.ZY_ZGJB_F115"]
["阻垢剂加药泵5800Hz噪音","C4.M4.ZY_ZGJB_F116"]
["阻垢剂加药泵5850Hz噪音","C4.M4.ZY_ZGJB_F117"]
["阻垢剂加药泵5900Hz噪音","C4.M4.ZY_ZGJB_F118"]
["阻垢剂加药泵5950Hz噪音","C4.M4.ZY_ZGJB_F119"]
["阻垢剂加药泵6000Hz噪音","C4.M4.ZY_ZGJB_F120"]
["阻垢剂加药泵6050Hz噪音","C4.M4.ZY_ZGJB_F121"]
["阻垢剂加药泵6100Hz噪音","C4.M4.ZY_ZGJB_F122"]
["阻垢剂加药泵6150Hz噪音","C4.M4.ZY_ZGJB_F123"]
["阻垢剂加药泵6200Hz噪音","C4.M4.ZY_ZGJB_F124"]
["阻垢剂加药泵6250Hz噪音","C4.M4.ZY_ZGJB_F125"]
["阻垢剂加药泵6300Hz噪音","C4.M4.ZY_ZGJB_F126"]
["阻垢剂加药泵6350Hz噪音","C4.M4.ZY_ZGJB_F127"]