{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":1416,"n_cols":2,"rows_kept":1416,"cut":false,"hidden":false,"merged":[]}
["item_alias","item_name"]
["超滤总进水量","water_in"]
["1#RO回收率","RO1HSL"]
["2#RO回收率","RO2HSL"]
["UF供水泵运行数量","UFGSB_shuliang"]
["超滤泵出水流量","UF_bump_avg"]
["超滤反洗泵运行数量","UFFXB_shuliang"]
["反洗泵出水流量","UFFXB_runFlow"]
["CIP清洗水泵运行数量","CIP_QXB_runnumber"]
["清洗水泵流量","CIP_QXB_runFlow"]
["1#超滤供水泵效率","UF_bump1_n"]
["2#超滤供水泵效率","UF_bump2_n"]
["3#超滤供水泵效率","UF_bump3_n"]
["4#超滤供水泵效率","UF_bump4_n"]
["UF1膜运行通量","UF1_FluxF"]
["UF2膜运行通量  ","UF2_FluxF"]
["UF3膜运行通量  ","UF3_FluxF"]
["UF4膜运行通量 ","UF4_FluxF"]
["自清洗过滤器压差","PFTMP"]
["UF1膜渗透率","UF1Per"]
["UF2膜渗透率","UF2Per"]
["UF3膜渗透率","UF3Per"]
["UF4膜渗透率","UF4Per"]
["反洗膜通量","UFFX_Flux"]
["RO总进水流量","RO_TotalFlow"]
["RO总产水流量","RO_TCHFlow"]
["3#RO回收率","RO3HSL"]
["4#RO回收率","RO4HSL"]
["3#清水外供泵效率","QSWGB3_n"]
["2#清水外供泵效率","QSWGB2_n"]
["1#清水外供泵效率","QSWGB1_n"]
["清水外供泵出水流量 ","QSWGB_Flow"]
["RO4脱盐率","RO4_TYL"]
["RO3脱盐率","RO3_TYL"]
["RO2脱盐率","RO2_TYL"]
["RO1脱盐率","RO1_TYL"]
["RO4膜运行通量","RO4_FluxF"]
["RO3膜运行通量","RO3_FluxF"]
["RO2膜运行通量","RO2_FluxF"]
["RO1膜运行通量","RO1_FluxF"]
["RO4一二段产水流量比值","RO4_SPK"]
["RO3一二段产水流量比值","RO3_SPK"]
["RO2一二段产水流量比值","RO2_SPK"]
["RO1一二段产水流量比值","RO1_SPK"]
["RO4段间泵效率","RO4_DJB_n"]
["RO3段间泵效率","RO3_DJB_n"]
["RO2段间泵效率","RO2_DJB_n"]
["RO1段间泵效率","RO1_DJB_n"]
["RO4高压泵效率","RO4_GYB_n"]
["RO3高压泵效率","RO3_GYB_n"]
["RO2高压泵效率","RO2_GYB_n"]
["RO1高压泵效率","RO1_GYB_n"]
["反渗透RO2步序和产水时长","C.M.RO2_DB@control_word_time"]
["反渗透RO1步序和产水时长","C.M.RO1_DB@control_word_time"]
["反渗透RO3步序和产水时长","C.M.RO3_DB@control_word_time"]
["反渗透RO4步序和产水时长","C.M.RO4_DB@control_word_time"]
["UF反洗时间显示","UF_DB@time_display"]
["清洗膜通量","UFQX_Flux"]
["UF反洗步序","UF_FXBX"]
["UF酸洗步序","UF_SXBX"]
["UF碱洗步序","UF_JXBX"]
["UF1步序和产水时长","C.M.UF1_DB@word_control_time"]
["UF2步序和产水时长","C.M.UF2_DB@word_control_time"]
["UF3步序和产水时长","C.M.UF3_DB@word_control_time"]
["UF4步序和产水时长","C.M.UF4_DB@word_control_time"]
["膜车间进出水流量校验","Flow_check"]
["RO1产水流量","RO1_CSFlow"]
["RO2产水流量","RO2_CSFlow"]
["RO3产水流量","RO3_CSFlow"]
["RO4产水流量","RO4_CSFlow"]
["UF1反洗压差","C.M.UF1_DW@press_PV"]
["UF2反洗压差","C.M.UF2_DW@press_PV"]
["UF3反洗压差","C.M.UF3_DW@press_PV"]
["UF4反洗压差","C.M.UF4_DW@press_PV"]
["UF1运行过滤压差","UF1_FF_TMP"]
["UF2运行过滤压差","UF2_FF_TMP"]
["UF3运行过滤压差","UF3_FF_TMP"]
["UF4运行过滤压差","UF4_FF_TMP"]
["UF1反洗前压差","UF1_BW_Before_TMP"]
["UF1反洗后压差","UF1_BW_After_TMP"]
["UF2反洗前压差","UF2_BW_Before_TMP"]
["UF3反洗前压差","UF3_BW_Before_TMP"]
["UF4反洗前压差","UF4_BW_Before_TMP"]
["UF2反洗后压差","UF2_BW_After_TMP"]
["UF3反洗后压差","UF3_BW_After_TMP"]
["UF4反洗后压差","UF4_BW_After_TMP"]
["UF1反洗前渗透率","UF1_BW_Before_Per"]
["UF1反洗后渗透率","UF1_BW_After_Per"]
["UF2反洗前渗透率","UF2_BW_Before_Per"]
["UF3反洗前渗透率","UF3_BW_Before_Per"]
["UF4反洗前渗透率","UF4_BW_Before_Per"]
["UF2反洗后渗透率","UF2_BW_After_Per"]
["UF3反洗后渗透率","UF3_BW_After_Per"]
["UF4反洗后渗透率","UF4_BW_After_Per"]
["水温校正因子","SW_ jzyz"]
["UF1膜渗透率（标准25℃）","UF1_BZ_Per"]
["UF2膜渗透率（标准25℃）","UF2_BZ_Per"]
["UF3膜渗透率（标准25℃）","UF3_BZ_Per"]
["UF4膜渗透率（标准25℃）","UF4_BZ_Per"]
["1#RO运行回收率","RO1_YX_HSL"]
["2#RO运行回收率","RO2_YX_HSL"]
["3#RO运行回收率","RO3_YX_HSL"]
["4#RO运行回收率","RO4_YX_HSL"]
["az_feed_in_flow","az_feed_in_flow"]
["az_feed_out_flow","az_feed_out_flow"]
["RO1过滤一段压差","RO1_FF_TMP1"]
["RO1过滤二段压差","RO1_FF_TMP2"]
["RO2过滤一段压差","RO2_FF_TMP1"]
["RO2过滤二段压差","RO2_FF_TMP2"]
["RO3过滤二段压差","RO3_FF_TMP2"]
["RO4过滤二段压差","RO4_FF_TMP2"]
["RO3过滤一段压差","RO3_FF_TMP1"]
["RO4过滤一段压差","RO4_FF_TMP1"]
["RO3冲洗后一段压差","RO3_CX_After_TMP1"]
["RO1冲洗前一段压差","RO1_CX_Before_TMP1"]
["RO3冲洗后时间节点","RO3_CX_After_TIme"]
["RO1冲洗后一段压差","RO1_CX_After_TMP1"]
["RO2冲洗后一段压差","RO2_CX_After_TMP1"]
["RO4冲洗后一段压差","RO4_CX_After_TMP1"]
["RO1冲洗后二段压差","RO1_CX_After_TMP2"]
["RO2冲洗后二段压差","RO2_CX_After_TMP2"]
["RO3冲洗后二段压差","RO3_CX_After_TMP2"]
["RO4冲洗后二段压差","RO4_CX_After_TMP2"]
["RO1冲洗前二段压差","RO1_CX_Before_TMP2"]
["RO2冲洗前一段压差","RO2_CX_Before_TMP1"]
["RO2冲洗前二段压差","RO2_CX_Before_TMP2"]
["RO3冲洗前一段压差","RO3_CX_Before_TMP1"]
["RO3冲洗前二段压差","RO3_CX_Before_TMP2"]
["RO4冲洗前一段压差","RO4_CX_Before_TMP1"]
["RO4冲洗前二段压差","RO4_CX_Before_TMP2"]
["反渗透进水ORP超高（组态弹窗用）","ORP_CX"]
["反渗透D产水电导率新","C.M.RO4_Cond_CS_filter@out"]
["反渗透C产水电导率新","C.M.RO3_Cond_CS_filter@out"]
["反渗透B产水电导率新","C.M.RO2_Cond_CS_filter@out"]
["反渗透A产水电导率新","C.M.RO1_Cond_CS_filter@out"]
["1#反渗透CIP状态","RO1_CIP_STATE"]
["2#反渗透CIP状态","RO2_CIP_STATE"]
["3#反渗透CIP状态","RO3_CIP_STATE"]
["4#反渗透CIP状态","RO4_CIP_STATE"]
["超滤回收率","UFHSL"]
["非氧加药泵1——自动/手动","C.M.PRO_cxsx_FY1@auto_select"]
["非氧加药泵1——故障","C.M.PRO_cxsx_FY1@fault_total"]
["非氧加药泵1——运行反馈","C.M.PRO_cxsx_FY1@run"]
["非氧加药泵1——运行时间","C.M.PRO_cxsx_FY1@run_time"]
["非氧加药泵1——手动频率","C.M.PRO_cxsx_FY1_AO_FB@spare"]
["非氧加药泵1——故障","C.M.PRO_cxsx_FY1_fre@Fault"]
["非氧加药泵1——频率反馈","C.M.PRO_cxsx_FY1_fre@out"]
["非氧加药泵2——自动/手动","C.M.PRO_cxsx_FY2@auto_select"]
["非氧加药泵2——故障","C.M.PRO_cxsx_FY2@fault_total"]
["非氧加药泵2——运行反馈","C.M.PRO_cxsx_FY2@run"]
["非氧加药泵2——运行时间","C.M.PRO_cxsx_FY2@run_time"]
["非氧加药泵2——手动频率","C.M.PRO_cxsx_FY2_AO_FB@spare"]
["非氧加药泵2——故障","C.M.PRO_cxsx_FY2_fre@Fault"]
["非氧加药泵2——频率反馈","C.M.PRO_cxsx_FY2_fre@out"]
["冲洗碱加药泵1——自动/手动","C.M.PRO_cxsx_J1@auto_select"]
["冲洗碱加药泵1——故障","C.M.PRO_cxsx_J1@fault_total"]
["冲洗碱加药泵1——运行反馈","C.M.PRO_cxsx_J1@run"]
["冲洗碱加药泵1——运行时间","C.M.PRO_cxsx_J1@run_time"]
["冲洗碱加药泵1——手动频率","C.M.PRO_cxsx_J1_AO_FB@spare"]
["冲洗碱加药泵1——故障","C.M.PRO_cxsx_J1_fre@Fault"]
["冲洗碱加药泵1——频率反馈","C.M.PRO_cxsx_J1_fre@out"]
["冲洗碱加药泵2——自动/手动","C.M.PRO_cxsx_J2@auto_select"]
["冲洗碱加药泵2——故障","C.M.PRO_cxsx_J2@fault_total"]
["冲洗碱加药泵2——运行反馈","C.M.PRO_cxsx_J2@run"]
["冲洗碱加药泵2——运行时间","C.M.PRO_cxsx_J2@run_time"]
["冲洗碱加药泵2——手动频率","C.M.PRO_cxsx_J2_AO_FB@spare"]
["冲洗碱加药泵2——故障","C.M.PRO_cxsx_J2_fre@Fault"]
["冲洗碱加药泵2——频率反馈","C.M.PRO_cxsx_J2_fre@out"]
["冲洗酸加药泵1——自动/手动","C.M.PRO_cxsx_S1@auto_select"]
["冲洗酸加药泵1——故障","C.M.PRO_cxsx_S1@fault_total"]
["冲洗酸加药泵1——运行反馈","C.M.PRO_cxsx_S1@run"]
["冲洗酸加药泵1——运行时间","C.M.PRO_cxsx_S1@run_time"]
["冲洗酸加药泵1——手动频率","C.M.PRO_cxsx_S1_AO_FB@spare"]
["冲洗酸加药泵1——故障","C.M.PRO_cxsx_S1_fre@Fault"]
["冲洗酸加药泵1——频率反馈","C.M.PRO_cxsx_S1_fre@out"]
["冲洗酸加药泵2——自动/手动","C.M.PRO_cxsx_S2@auto_select"]
["冲洗酸加药泵2——故障","C.M.PRO_cxsx_S2@fault_total"]
["冲洗酸加药泵2——运行反馈","C.M.PRO_cxsx_S2@run"]
["冲洗酸加药泵2——运行时间","C.M.PRO_cxsx_S2@run_time"]
["冲洗酸加药泵2——手动频率","C.M.PRO_cxsx_S2_AO_FB@spare"]
["冲洗酸加药泵2——故障","C.M.PRO_cxsx_S2_fre@Fault"]
["冲洗酸加药泵2——频率反馈","C.M.PRO_cxsx_S2_fre@out"]
["非氧产水加药——水量","C.M.RO_FYcsJY[0]"]
["非氧产水加药——系数","C.M.RO_FYcsJY[3]"]
["非氧产水加药——频率输出","C.M.RO_FYcsJY[4]"]
["BW优先 UF1","C.M.BW_First_Order[0]"]
["BW优先 UF2","C.M.BW_First_Order[1]"]
["BW优先 UF3","C.M.BW_First_Order[2]"]
["BW优先 UF4","C.M.BW_First_Order[3]"]
["外供流量 当天","C.M.FL_WG_day[0]"]
["外供流量 前1天","C.M.FL_WG_day[1]"]
["外供流量 前2天","C.M.FL_WG_day[2]"]
["外供流量 前3天","C.M.FL_WG_day[3]"]
["外供流量 前4天","C.M.FL_WG_day[4]"]
["还原剂频率输出","C.M.HYJ_out_Final"]
["还原剂PID 目标值 ","C.M.HYJ_PID_SP"]
["PAC频率输出","C.M.PACFreSetRead[0]"]
["PAC数量输出","C.M.PACNumSetRead[0]"]
["RO产水数量","C.M.RO_CStotalNum"]
["单套产水基准值","C.M.RO_FlowLDBasicF"]
["RO运行数量","C.M.RO_RunNum"]
["RO自动运行数量输出","C.M.RO_RunNumFinalSet"]
["RO联动UF数量","C.M.RO_UF_NeedNum"]
["RO自动可用数量","C.M.ROAutoReadyNumSSD"]
["RO自动运行数量输出","C.M.ROAutoRunNumSSD"]
["RO产水池联动数量","C.M.ROcscLDnum"]
["RO进水池联动数量","C.M.ROjscLDnum"]
["RO手动联动数量","C.M.ROManLDnum"]
["RO液位联动数量","C.M.ROYWLDnum"]
["UF产水结束信号","C.M.UF_CSendingApply"]
["UF产水中数量","C.M.UF_CSingNum"]
["UF1 渗透率","C.M.UF1_Count[0]"]
["UF1 产水进度","C.M.UF1_Count[4]"]
["RO1 产水进度","C.M.UF1_Count[5]"]
["UF1 CEB 进度","C.M.UF1_Count[6]"]
["总进水流量","C.M.UF1_Count[7]"]
["UF2 渗透率","C.M.UF2_Count[0]"]
["UF2 产水进度","C.M.UF2_Count[4]"]
["RO2 产水进度","C.M.UF2_Count[5]"]
["UF2 CEB 进度","C.M.UF2_Count[6]"]
["总进水流量","C.M.UF2_Count[7]"]
["UF3 渗透率","C.M.UF3_Count[0]"]
["UF3 产水进度","C.M.UF3_Count[4]"]
["RO3 产水进度","C.M.UF3_Count[5]"]
["UF3 CEB 进度","C.M.UF3_Count[6]"]
["总进水流量","C.M.UF3_Count[7]"]
["UF4 渗透率","C.M.UF4_Count[0]"]
["UF4 产水进度","C.M.UF4_Count[4]"]
["RO4 产水进度","C.M.UF4_Count[5]"]
["UF4 CEB 进度","C.M.UF4_Count[6]"]
["总进水流量","C.M.UF4_Count[7]"]
["1#CIP清洗水泵故障","C.M.CIP_QXB1@fault_total"]
["1#CIP清洗水泵运行","C.M.CIP_QXB1@run"]
["1#CIP清洗水泵运行时间","C.M.CIP_QXB1@run_time"]
["1#CIP清洗水泵运行频率","C.M.CIP_QXB1_fre@out"]
["2#CIP清洗水泵故障","C.M.CIP_QXB2@fault_total"]
["2#CIP清洗水泵运行","C.M.CIP_QXB2@run"]
["2#CIP清洗水泵运行时间","C.M.CIP_QXB2@run_time"]
["2#CIP清洗水泵运行频率","C.M.CIP_QXB2_fre@out"]
["CIP出水阀故障","C.M.CIP_QXCSF@fault_total"]
["外排水余氯","C.M.Cl_WPS@out"]
["1#NaClO加药泵(出水)故障","C.M.CS_NaClO1@fault_total"]
["1#NaClO加药泵(出水)运行","C.M.CS_NaClO1@run"]
["1#NaClO加药泵(出水)运行时间","C.M.CS_NaClO1@run_time"]
["1#NaClO加药泵(出水)运行频率","C.M.CS_NaClO1_fre@out"]
["2#NaClO加药泵(出水)故障","C.M.CS_NaClO2@fault_total"]
["2#NaClO加药泵(出水)运行","C.M.CS_NaClO2@run"]
["2#NaClO加药泵(出水)运行时间","C.M.CS_NaClO2@run_time"]
["2#NaClO加药泵(出水)运行频率","C.M.CS_NaClO2_fre@out"]
["膜车间1#排风扇故障","C.M.Fan1@fault_total"]
["膜车间1#排风扇运行","C.M.Fan1@run"]
["膜车间1#排风扇运行时间","C.M.Fan1@run_time"]
["膜车间2#排风扇故障","C.M.Fan2@fault_total"]
["膜车间2#排风扇运行","C.M.Fan2@run"]
["膜车间2#排风扇运行时间","C.M.Fan2@run_time"]
["膜车间3#排风扇故障","C.M.Fan3@fault_total"]
["膜车间3#排风扇运行","C.M.Fan3@run"]
["膜车间3#排风扇运行时间","C.M.Fan3@run_time"]
["膜车间4#排风扇故障","C.M.Fan4@fault_total"]
["膜车间4#排风扇运行","C.M.Fan4@run"]
["膜车间4#排风扇运行时间","C.M.Fan4@run_time"]
["膜车间5#排风扇故障","C.M.Fan5@fault_total"]
["膜车间5#排风扇运行","C.M.Fan5@run"]
["膜车间5#排风扇运行时间","C.M.Fan5@run_time"]
["膜车间6#排风扇故障","C.M.Fan6@fault_total"]
["膜车间6#排风扇运行","C.M.Fan6@run"]
["膜车间6#排风扇运行时间","C.M.Fan6@run_time"]
["水泵间1#排风扇故障","C.M.Fan7@fault_total"]
["水泵间1#排风扇运行","C.M.Fan7@run"]
["水泵间1#排风扇运行时间","C.M.Fan7@run_time"]
["水泵间2#排风扇故障","C.M.Fan8@fault_total"]
["水泵间2#排风扇运行","C.M.Fan8@run"]
["水泵间2#排风扇运行时间","C.M.Fan8@run_time"]
["水泵间3#排风扇故障","C.M.Fan9@fault_total"]
["水泵间3#排风扇运行","C.M.Fan9@run"]
["水泵间3#排风扇运行时间","C.M.Fan9@run_time"]
["水泵间4#排风扇故障","C.M.Fan10@fault_total"]
["水泵间4#排风扇运行","C.M.Fan10@run"]
["水泵间4#排风扇运行时间","C.M.Fan10@run_time"]
["水泵间5#排风扇故障","C.M.Fan11@fault_total"]
["水泵间5#排风扇运行","C.M.Fan11@run"]
["水泵间5#排风扇运行时间","C.M.Fan11@run_time"]
["水泵间6#排风扇故障","C.M.Fan12@fault_total"]
["水泵间6#排风扇运行","C.M.Fan12@run"]
["水泵间6#排风扇运行时间","C.M.Fan12@run_time"]
["水泵间7#排风扇故障","C.M.Fan13@fault_total"]
["水泵间7#排风扇运行","C.M.Fan13@run"]
["水泵间7#排风扇运行时间","C.M.Fan13@run_time"]
["水泵间8#排风扇故障","C.M.Fan14@fault_total"]
["水泵间8#排风扇运行","C.M.Fan14@run"]
["水泵间8#排风扇运行时间","C.M.Fan14@run_time"]
["中控室排风扇故障","C.M.Fan15@fault_total"]
["中控室排风扇运行","C.M.Fan15@run"]
["中控室排风扇运行时间","C.M.Fan15@run_time"]
["楼梯间1#排风扇故障","C.M.Fan16@fault_total"]
["楼梯间1#排风扇运行","C.M.Fan16@run"]
["楼梯间1#排风扇运行时间","C.M.Fan16@run_time"]
["楼梯间2#排风扇故障","C.M.Fan17@fault_total"]
["楼梯间2#排风扇运行","C.M.Fan17@run"]
["楼梯间2#排风扇运行时间","C.M.Fan17@run_time"]
["高配室排风扇故障","C.M.Fan18@fault_total"]
["高配室排风扇运行","C.M.Fan18@run"]
["高配室排风扇运行时间","C.M.Fan18@run_time"]
["低配室1#排风扇故障","C.M.Fan19@fault_total"]
["低配室1#排风扇运行","C.M.Fan19@run"]
["低配室1#排风扇运行时间","C.M.Fan19@run_time"]
["低配室2#排风扇故障","C.M.Fan20@fault_total"]
["低配室2#排风扇运行","C.M.Fan20@run"]
["低配室2#排风扇运行时间","C.M.Fan20@run_time"]
["加药间1#排风扇故障","C.M.Fan21@fault_total"]
["加药间1#排风扇运行","C.M.Fan21@run"]
["加药间1#排风扇运行时间","C.M.Fan21@run_time"]
["加药间2#排风扇故障","C.M.Fan22@fault_total"]
["加药间2#排风扇运行","C.M.Fan22@run"]
["加药间2#排风扇运行时间","C.M.Fan22@run_time"]
["小加药间1#排风扇故障","C.M.Fan23@fault_total"]
["小加药间1#排风扇运行","C.M.Fan23@run"]
["小加药间1#排风扇运行时间","C.M.Fan23@run_time"]
["小加药间2#排风扇故障","C.M.Fan24@fault_total"]
["小加药间2#排风扇运行","C.M.Fan24@run"]
["小加药间2#排风扇运行时间","C.M.Fan24@run_time"]
["外供累计流量","C.M.flow_ZCS_acc"]
["外供累计流量清零","C.M.flow_ZCS_acc_reset"]
["CIP流量","C.M.FT_CIP@out"]
["补水流量","C.M.FT_FXSC@out"]
["还原剂流量","C.M.FT_HYJJY1@out"]
["总浓水排水流量","C.M.FT_NSPS@out"]
["清水池流量","C.M.FT_QSC@out"]
["1#反渗透阻垢剂流量","C.M.FT_ZGJJY1@out"]
["2#反渗透阻垢剂流量","C.M.FT_ZGJJY2@out"]
["3#反渗透阻垢剂流量","C.M.FT_ZGJJY3@out"]
["4#反渗透阻垢剂流量","C.M.FT_ZGJJY4@out"]
["总进水流量","C.M.FT_ZJS@out"]
["1#自清洗过滤器反洗","C.M.GLQ1_FX"]
["1#自清洗过滤器过滤","C.M.GLQ1_GL"]
["1#自清洗过滤器故障","C.M.GLQ1_GZ"]
["2#自清洗过滤器反洗","C.M.GLQ2_FX"]
["2#自清洗过滤器过滤","C.M.GLQ2_GL"]
["2#自清洗过滤器故障","C.M.GLQ2_GZ"]
["3#自清洗过滤器反洗","C.M.GLQ3_FX"]
["3#自清洗过滤器过滤","C.M.GLQ3_GL"]
["3#自清洗过滤器故障","C.M.GLQ3_GZ"]
["1#NaClO加药泵(进水)故障","C.M.JS_NaClO1@fault_total"]
["1#NaClO加药泵(进水)运行","C.M.JS_NaClO1@run"]
["1#NaClO加药泵(进水)运行时间","C.M.JS_NaClO1@run_time"]
["1#NaClO加药泵(进水)运行频率","C.M.JS_NaClO1_fre@out"]
["2#NaClO加药泵(进水)故障","C.M.JS_NaClO2@fault_total"]
["2#NaClO加药泵(进水)运行","C.M.JS_NaClO2@run"]
["2#NaClO加药泵(进水)运行时间","C.M.JS_NaClO2@run_time"]
["2#NaClO加药泵(进水)运行频率","C.M.JS_NaClO2_fre@out"]
["1#盐酸加药泵故障","C.M.JYB1_HCl1@fault_total"]
["1#盐酸加药泵运行","C.M.JYB1_HCl1@run"]
["1#盐酸加药泵运行时间","C.M.JYB1_HCl1@run_time"]
["2#盐酸加药泵故障","C.M.JYB1_HCl2@fault_total"]
["2#盐酸加药泵运行","C.M.JYB1_HCl2@run"]
["2#盐酸加药泵运行时间","C.M.JYB1_HCl2@run_time"]
["1#还原剂加药泵(中和)故障","C.M.JYB1_HYJ1@fault_total"]
["1#还原剂加药泵(中和)运行","C.M.JYB1_HYJ1@run"]
["1#还原剂加药泵(中和)运行时间","C.M.JYB1_HYJ1@run_time"]
["2#还原剂加药泵(中和)故障","C.M.JYB1_HYJ2@fault_total"]
["2#还原剂加药泵(中和)运行","C.M.JYB1_HYJ2@run"]
["2#还原剂加药泵(中和)运行时间","C.M.JYB1_HYJ2@run_time"]
["1#NaClO加药泵故障","C.M.JYB1_NaClO1@fault_total"]
["1#NaClO加药泵运行","C.M.JYB1_NaClO1@run"]
["1#NaClO加药泵运行时间","C.M.JYB1_NaClO1@run_time"]
["2#NaClO加药泵故障","C.M.JYB1_NaClO2@fault_total"]
["2#NaClO加药泵运行","C.M.JYB1_NaClO2@run"]
["2#NaClO加药泵运行时间","C.M.JYB1_NaClO2@run_time"]
["1#NaOH加药泵(中和)故障","C.M.JYB1_NaOH1@fault_total"]
["1#NaOH加药泵(中和)运行","C.M.JYB1_NaOH1@run"]
["1#NaOH加药泵(中和)运行时间","C.M.JYB1_NaOH1@run_time"]
["2#NaOH加药泵(CEB)故障","C.M.JYB1_NaOH2@fault_total"]
["2#NaOH加药泵(CEB)运行","C.M.JYB1_NaOH2@run"]
["2#NaOH加药泵(CEB)运行时间","C.M.JYB1_NaOH2@run_time"]
["1#还原剂加药泵(RO)故障","C.M.JYB2_HYJ1@fault_total"]
["1#还原剂加药泵(RO)运行","C.M.JYB2_HYJ1@run"]
["1#还原剂加药泵(RO)运行时间","C.M.JYB2_HYJ1@run_time"]
["1#还原剂加药泵(RO)运行频率","C.M.JYB2_HYJ1_fre@out"]
["2#还原剂加药泵(RO)故障","C.M.JYB2_HYJ2@fault_total"]
["2#还原剂加药泵(RO)运行","C.M.JYB2_HYJ2@run"]
["2#还原剂加药泵(RO)运行时间","C.M.JYB2_HYJ2@run_time"]
["2#还原剂加药泵(RO)运行频率","C.M.JYB2_HYJ2_fre@out"]
["3#还原剂加药泵(RO)故障","C.M.JYB2_HYJ3@fault_total"]
["3#还原剂加药泵(RO)运行","C.M.JYB2_HYJ3@run"]
["3#还原剂加药泵(RO)运行时间","C.M.JYB2_HYJ3@run_time"]
["3#还原剂加药泵(RO)运行频率","C.M.JYB2_HYJ3_fre@out"]
["1#NaOH加药泵(出水)故障","C.M.JYB2_NaOH1@fault_total"]
["1#NaOH加药泵(出水)运行","C.M.JYB2_NaOH1@run"]
["1#NaOH加药泵(出水)运行时间","C.M.JYB2_NaOH1@run_time"]
["1#NaOH加药泵(出水)运行频率","C.M.JYB2_NaOH1_fre@out"]
["2#NaOH加药泵(出水)故障","C.M.JYB2_NaOH2@fault_total"]
["2#NaOH加药泵(出水)运行","C.M.JYB2_NaOH2@run"]
["2#NaOH加药泵(出水)运行时间","C.M.JYB2_NaOH2@run_time"]
["2#NaOH加药泵(出水)运行频率","C.M.JYB2_NaOH2_fre@out"]
["1#絮凝剂加药泵(UF)故障","C.M.JYB2_XNJ1@fault_total"]
["1#絮凝剂加药泵(UF)运行","C.M.JYB2_XNJ1@run"]
["1#絮凝剂加药泵(UF)运行时间","C.M.JYB2_XNJ1@run_time"]
["1#絮凝剂加药泵(UF)运行频率","C.M.JYB2_XNJ1_fre@out"]
["2#絮凝剂加药泵(UF)故障","C.M.JYB2_XNJ2@fault_total"]
["2#絮凝剂加药泵(UF)运行","C.M.JYB2_XNJ2@run"]
["2#絮凝剂加药泵(UF)运行时间","C.M.JYB2_XNJ2@run_time"]
["2#絮凝剂加药泵(UF)运行频率","C.M.JYB2_XNJ2_fre@out"]
["1#阻垢剂加药泵(RO)故障","C.M.JYB2_ZGJ1@fault_total"]
["1#阻垢剂加药泵(RO)运行","C.M.JYB2_ZGJ1@run"]
["1#阻垢剂加药泵(RO)运行时间","C.M.JYB2_ZGJ1@run_time"]
["1#阻垢剂加药泵(RO)运行频率","C.M.JYB2_ZGJ1_fre@out"]
["2#阻垢剂加药泵(RO)故障","C.M.JYB2_ZGJ2@fault_total"]
["2#阻垢剂加药泵(RO)运行","C.M.JYB2_ZGJ2@run"]
["2#阻垢剂加药泵(RO)运行时间","C.M.JYB2_ZGJ2@run_time"]
["2#阻垢剂加药泵(RO)运行频率","C.M.JYB2_ZGJ2_fre@out"]
["3#阻垢剂加药泵(RO)故障","C.M.JYB2_ZGJ3@fault_total"]
["3#阻垢剂加药泵(RO)运行","C.M.JYB2_ZGJ3@run"]
["3#阻垢剂加药泵(RO)运行时间","C.M.JYB2_ZGJ3@run_time"]
["3#阻垢剂加药泵(RO)运行频率","C.M.JYB2_ZGJ3_fre@out"]
["4#阻垢剂加药泵(RO)故障","C.M.JYB2_ZGJ4@fault_total"]
["4#阻垢剂加药泵(RO)运行","C.M.JYB2_ZGJ4@run"]
["4#阻垢剂加药泵(RO)运行时间","C.M.JYB2_ZGJ4@run_time"]
["4#阻垢剂加药泵(RO)运行频率","C.M.JYB2_ZGJ4_fre@out"]
["5#阻垢剂加药泵(RO)故障","C.M.JYB2_ZGJ5@fault_total"]
["5#阻垢剂加药泵(RO)运行","C.M.JYB2_ZGJ5@run"]
["5#阻垢剂加药泵(RO)运行时间","C.M.JYB2_ZGJ5@run_time"]
["5#阻垢剂加药泵(RO)运行频率","C.M.JYB2_ZGJ5_fre@out"]
["CIP水箱液位","C.M.LT_CIP@out"]
["超滤反洗水池液位","C.M.LT_FXSC@out"]
["盐酸药箱液位","C.M.LT_HCl@out"]
["还原剂药箱2液位","C.M.LT_HYJ1@out"]
["还原剂药箱1液位","C.M.LT_HYJ2@out"]
["超滤原水池液位","C.M.LT_JSC@out"]
["次氯酸钠药箱液位","C.M.LT_NaClO@out"]
["氢氧化钠药箱液位","C.M.LT_NaOH@out"]
["絮凝剂药箱液位","C.M.LT_PAC@out"]
["清水池液位","C.M.LT_QSC@out"]
["杀菌剂药箱液位","C.M.LT_SJJ@out"]
["阻垢剂药箱液位","C.M.LT_ZGJ@out"]
["中和池液位","C.M.LT_ZHC@out"]
["CIP-PH","C.M.PH_CIP@out"]
["外供水-PH","C.M.PH_WGS@out"]
["压缩空气压力","C.M.PT_KYJ@out"]
["反渗透总产水电导","C.M.RO_Cond_ZCS@out"]
["反渗透总进水电导","C.M.RO_Cond_ZJS@out"]
["1#大水量冲洗泵故障","C.M.RO_CXB1@fault_total"]
["1#大水量冲洗泵运行","C.M.RO_CXB1@run"]
["1#大水量冲洗泵运行时间","C.M.RO_CXB1@run_time"]
["1#大水量冲洗泵运行频率","C.M.RO_CXB1_fre@out"]
["2#大水量冲洗泵故障","C.M.RO_CXB2@fault_total"]
["2#大水量冲洗泵运行","C.M.RO_CXB2@run"]
["2#大水量冲洗泵运行时间","C.M.RO_CXB2@run_time"]
["2#大水量冲洗泵运行频率","C.M.RO_CXB2_fre@out"]
["RO还原剂加药流量","C.M.RO_FT_HYJ@out"]
["反渗透总进水ORP","C.M.RO_ORP_ZJS@out"]
["反渗透总进水PH","C.M.RO_PH_ZJS@out"]
["反渗透总产水压力","C.M.RO_PT_ZCS@out"]
["反渗透总进水温度","C.M.RO_TT_ZJS@out"]
["1#清水外供泵故障","C.M.RO_WGB1@fault_total"]
["1#清水外供泵运行","C.M.RO_WGB1@run"]
["1#清水外供泵运行时间","C.M.RO_WGB1@run_time"]
["1#清水外供泵运行频率","C.M.RO_WGB1_fre@out"]
["2#清水外供泵故障","C.M.RO_WGB2@fault_total"]
["2#清水外供泵运行","C.M.RO_WGB2@run"]
["2#清水外供泵运行时间","C.M.RO_WGB2@run_time"]
["2#清水外供泵运行频率","C.M.RO_WGB2_fre@out"]
["3#清水外供泵故障","C.M.RO_WGB3@fault_total"]
["3#清水外供泵运行","C.M.RO_WGB3@run"]
["3#清水外供泵运行时间","C.M.RO_WGB3@run_time"]
["3#清水外供泵运行频率","C.M.RO_WGB3_fre@out"]
["RO1不合格水阀故障","C.M.RO1_BHGF@fault_total"]
["RO1产水CIP回水阀故障","C.M.RO1_CIP_CSHSF@fault_total"]
["RO1一段CIP回水阀故障","C.M.RO1_CIP_HSF1@fault_total"]
["RO1二段CIP回水阀故障","C.M.RO1_CIP_HSF2@fault_total"]
["RO1一段CIP进水阀故障","C.M.RO1_CIP_JSF1@fault_total"]
["RO1二段CIP进水阀故障","C.M.RO1_CIP_JSF2@fault_total"]
["RO1产水电导","C.M.RO1_Cond_CS@out"]
["RO1产水阀故障","C.M.RO1_CSF@fault_total"]
["RO1一段冲洗进水阀故障","C.M.RO1_CXJF1@fault_total"]
["RO1二段冲洗进水阀故障","C.M.RO1_CXJF2@fault_total"]
["RO1一段冲洗排水阀故障","C.M.RO1_CXPF1@fault_total"]
["RO1二段冲洗排水阀故障","C.M.RO1_CXPF2@fault_total"]
["RO1自动开机","C.M.RO1_DB@button[01]"]
["RO1自动停止","C.M.RO1_DB@button[02]"]
["RO1自动正常冲洗","C.M.RO1_DB@button[03]"]
["RO1自动反向冲洗","C.M.RO1_DB@button[04]"]
["RO1自动杀菌冲洗","C.M.RO1_DB@button[05]"]
["RO1全自动开机","C.M.RO1_DB@button[08]"]
["RO1一段CIP（保持）","C.M.RO1_DB@button[14]"]
["RO1二段CIP（保持）","C.M.RO1_DB@button[15]"]
["RO1一段酸洗（选中保持）","C.M.RO1_DB@button[16]"]
["RO1二段酸洗（选中保持）","C.M.RO1_DB@button[17]"]
["RO1一段碱洗（选中保持）","C.M.RO1_DB@button[18]"]
["RO1二段碱洗（选中保持）","C.M.RO1_DB@button[19]"]
["RO1一段非氧洗（选中保持）","C.M.RO1_DB@button[20]"]
["RO1二段非氧洗（选中保持）","C.M.RO1_DB@button[21]"]
["RO1一段酸洗（手动保持）","C.M.RO1_DB@button[22]"]
["RO1二段酸洗（手动保持）","C.M.RO1_DB@button[23]"]
["RO1一段碱洗（手动保持）","C.M.RO1_DB@button[24]"]
["RO1二段碱洗（手动保持）","C.M.RO1_DB@button[25]"]
["RO1一段非氧洗（手动保持）","C.M.RO1_DB@button[26]"]
["RO1二段非氧洗（手动保持）","C.M.RO1_DB@button[27]"]
["RO1HOLDHB1","C.M.RO1_DB@button[28]"]
["RO1HOLDHB2","C.M.RO1_DB@button[29]"]
["RO1HOLDHB3","C.M.RO1_DB@button[30]"]
["RO1HOLDHB4","C.M.RO1_DB@button[31]"]
["RO1 ZBOOL HOLD1","C.M.RO1_DB@Zbool[0]"]
["RO1 ZBOOL HOLD2","C.M.RO1_DB@Zbool[1]"]
["RO1 ZBOOL HOLD3","C.M.RO1_DB@Zbool[2]"]
["RO1 ZDint HOLD1","C.M.RO1_DB@ZDint[0]"]
["RO1 ZDint HOLD2","C.M.RO1_DB@ZDint[1]"]
["RO1 ZDint HOLD3","C.M.RO1_DB@ZDint[2]"]
["RO1当前步序时间","C.M.RO1_DB@ZZZreal[0]"]
["RO1 1段酸洗记次数","C.M.RO1_DB@ZZZreal[2]"]
["RO1 2段酸洗记次数","C.M.RO1_DB@ZZZreal[3]"]
["RO1 1段J洗记次数","C.M.RO1_DB@ZZZreal[4]"]
["RO1 2段J洗记次数","C.M.RO1_DB@ZZZreal[5]"]
["RO1 1段FY洗记次数","C.M.RO1_DB@ZZZreal[6]"]
["RO1 2段FY洗记次数","C.M.RO1_DB@ZZZreal[7]"]
["RO1HOLD1","C.M.RO1_DB@ZZZreal[14]"]
["RO1HOLD2","C.M.RO1_DB@ZZZreal[15]"]
["RO1HOLD3","C.M.RO1_DB@ZZZreal[22]"]
["RO1HOLD4","C.M.RO1_DB@ZZZreal[23]"]
["RO1HOLD5","C.M.RO1_DB@ZZZreal[24]"]
["RO1HOLD6","C.M.RO1_DB@ZZZreal[25]"]
["RO1一段CIP浸泡","C.M.RO1_DB@ZZZreal[27]"]
["RO1二段CIP浸泡","C.M.RO1_DB@ZZZreal[29]"]
["RO1产水杀菌时间READ","C.M.RO1_DB@ZZZreal[32]"]
["RO1产水杀菌等待时间READ","C.M.RO1_DB@ZZZreal[33]"]
["RO1HOLD7","C.M.RO1_DB@ZZZreal[34]"]
["RO1HOLD8","C.M.RO1_DB@ZZZreal[35]"]
["RO1HOLD9","C.M.RO1_DB@ZZZreal[36]"]
["RO1HOLD10","C.M.RO1_DB@ZZZreal[37]"]
["RO1HOLD11","C.M.RO1_DB@ZZZreal[38]"]
["RO1HOLD12","C.M.RO1_DB@ZZZreal[39]"]
["RO1——碱冲洗设备ready","C.M.RO1_DB@ready[08]"]
["RO1——杀菌冲洗设备ready","C.M.RO1_DB@ready[09]"]
["RO1一段压差","C.M.RO1_DB@DPT_1"]
["RO1二段压差","C.M.RO1_DB@DPT_2"]
["RO1运行时间","C.M.RO1_DB@run_time"]
["RO1停止时间","C.M.RO1_DB@stop_time"]
["RO1不合格排水","C.M.RO1_DB@time_bhgs_display"]
["RO1产水时间","C.M.RO1_DB@time_CS_display"]
["RO1一段反冲","C.M.RO1_DB@time_FX1_display"]
["RO1开机等待","C.M.RO1_DB@time_kj_wait"]
["RO1排气时间","C.M.RO1_DB@time_kjcx_display1"]
["RO1开机冲洗","C.M.RO1_DB@time_kjcx_display2"]
["RO1杀菌间隔","C.M.RO1_DB@time_shajun_display"]
["RO1杀菌等待","C.M.RO1_DB@time_sj_wait"]
["RO1一段反冲","C.M.RO1_DB@time_sjcx1_display"]
["RO1二段反冲","C.M.RO1_DB@time_sjcx2_display"]
["RO1浸泡时间","C.M.RO1_DB@time_sjjp_display"]
["RO1加药时间","C.M.RO1_DB@time_sjjy_display"]
["RO1冲洗等待","C.M.RO1_DB@time_tj_wait"]
["RO1二段正冲","C.M.RO1_DB@time_ZX2_display"]
["RO1正常冲洗","C.M.RO1_DB@time_ZX12_display"]
["RO1反渗透段间泵故障","C.M.RO1_DJB@fault_total"]
["RO1反渗透段间泵运行","C.M.RO1_DJB@run"]
["RO1反渗透段间泵运行时间","C.M.RO1_DJB@run_time"]
["RO1反渗透段间泵运行频率","C.M.RO1_DJB_fre@out"]
["RO1反渗透二段产水流量","C.M.RO1_FT_CS2@out"]
["RO1反渗透进水流量","C.M.RO1_FT_JS@out"]
["RO1反渗透浓水流量","C.M.RO1_FT_NS@out"]
["RO1反渗透高压泵故障","C.M.RO1_GYB@fault_total"]
["RO1反渗透高压泵运行","C.M.RO1_GYB@run"]
["RO1反渗透高压泵运行时间","C.M.RO1_GYB@run_time"]
["RO1反渗透高压泵运行频率","C.M.RO1_GYB_fre@out"]
["RO1进水调节阀开度","C.M.RO1_GYBF_kd@out"]
["RO1排气阀1故障","C.M.RO1_PQF1@fault_total"]
["RO1排气阀2故障","C.M.RO1_PQF2@fault_total"]
["RO1排气阀3故障","C.M.RO1_PQF3@fault_total"]
["RO1排气阀4故障","C.M.RO1_PQF4@fault_total"]
["RO1排气阀5故障","C.M.RO1_PQF5@fault_total"]
["RO1排气阀6故障","C.M.RO1_PQF6@fault_total"]
["RO1排气阀7故障","C.M.RO1_PQF7@fault_total"]
["RO1产水压力","C.M.RO1_PT_CS@out"]
["RO1一段浓水压力","C.M.RO1_PT_DJ1@out"]
["RO1二段进水压力","C.M.RO1_PT_DJ2@out"]
["RO1一段进水压力","C.M.RO1_PT_JS@out"]
["RO1二段浓水压力","C.M.RO1_PT_NS@out"]
["RO2不合格水阀故障","C.M.RO2_BHGF@fault_total"]
["RO2产水CIP回水阀故障","C.M.RO2_CIP_CSHSF@fault_total"]
["RO2一段CIP回水阀故障","C.M.RO2_CIP_HSF1@fault_total"]
["RO2二段CIP回水阀故障","C.M.RO2_CIP_HSF2@fault_total"]
["RO2一段CIP进水阀故障","C.M.RO2_CIP_JSF1@fault_total"]
["RO2二段CIP进水阀故障","C.M.RO2_CIP_JSF2@fault_total"]
["RO2产水电导","C.M.RO2_Cond_CS@out"]
["RO2产水阀故障","C.M.RO2_CSF@fault_total"]
["RO2一段冲洗进水阀故障","C.M.RO2_CXJF1@fault_total"]
["RO2二段冲洗进水阀故障","C.M.RO2_CXJF2@fault_total"]
["RO2一段冲洗排水阀故障","C.M.RO2_CXPF1@fault_total"]
["RO2二段冲洗排水阀故障","C.M.RO2_CXPF2@fault_total"]
["RO2自动开机","C.M.RO2_DB@button[01]"]
["RO2自动停止","C.M.RO2_DB@button[02]"]
["RO2自动正常冲洗","C.M.RO2_DB@button[03]"]
["RO2自动反向冲洗","C.M.RO2_DB@button[04]"]
["RO2自动杀菌冲洗","C.M.RO2_DB@button[05]"]
["RO2全自动开机","C.M.RO2_DB@button[08]"]
["RO2一段CIP（保持）","C.M.RO2_DB@button[14]"]
["RO2二段CIP（保持）","C.M.RO2_DB@button[15]"]
["RO2一段酸洗（选中保持）","C.M.RO2_DB@button[16]"]
["RO2二段酸洗（选中保持）","C.M.RO2_DB@button[17]"]
["RO2一段碱洗（选中保持）","C.M.RO2_DB@button[18]"]
["RO2二段碱洗（选中保持）","C.M.RO2_DB@button[19]"]
["RO2一段非氧洗（选中保持）","C.M.RO2_DB@button[20]"]
["RO2二段非氧洗（选中保持）","C.M.RO2_DB@button[21]"]
["RO2一段酸洗（手动保持）","C.M.RO2_DB@button[22]"]
["RO2二段酸洗（手动保持）","C.M.RO2_DB@button[23]"]
["RO2一段碱洗（手动保持）","C.M.RO2_DB@button[24]"]
["RO2二段碱洗（手动保持）","C.M.RO2_DB@button[25]"]
["RO2一段非氧洗（手动保持）","C.M.RO2_DB@button[26]"]
["RO2二段非氧洗（手动保持）","C.M.RO2_DB@button[27]"]
["RO2HOLD HB1","C.M.RO2_DB@button[28]"]
["RO2HOLD HB2","C.M.RO2_DB@button[29]"]
["RO2HOLD HB3","C.M.RO2_DB@button[30]"]
["RO2HOLD HB4","C.M.RO2_DB@button[31]"]
["RO2 ZBOOL HOLD1","C.M.RO2_DB@Zbool[0]"]
["RO2 ZBOOL HOLD2","C.M.RO2_DB@Zbool[1]"]
["RO2 ZBOOL HOLD3","C.M.RO2_DB@Zbool[2]"]
["RO2 ZDint HOLD1","C.M.RO2_DB@ZDint[0]"]
["RO2 ZDint HOLD2","C.M.RO2_DB@ZDint[1]"]
["RO2 ZDint HOLD3","C.M.RO2_DB@ZDint[2]"]
["RO2当前步序时间","C.M.RO2_DB@ZZZreal[0]"]
["RO2 1段酸洗记次数","C.M.RO2_DB@ZZZreal[2]"]
["RO2 2段酸洗记次数","C.M.RO2_DB@ZZZreal[3]"]
["RO2 1段J洗记次数","C.M.RO2_DB@ZZZreal[4]"]
["RO2 2段J洗记次数","C.M.RO2_DB@ZZZreal[5]"]
["RO2 1段FY洗记次数","C.M.RO2_DB@ZZZreal[6]"]
["RO2 2段FY洗记次数","C.M.RO2_DB@ZZZreal[7]"]
["RO2HOLD1","C.M.RO2_DB@ZZZreal[14]"]
["RO2HOLD2","C.M.RO2_DB@ZZZreal[15]"]
["RO2HOLD3","C.M.RO2_DB@ZZZreal[22]"]
["RO2HOLD4","C.M.RO2_DB@ZZZreal[23]"]
["RO2HOLD5","C.M.RO2_DB@ZZZreal[24]"]
["RO2HOLD6","C.M.RO2_DB@ZZZreal[25]"]
["RO2 一段CIP浸泡","C.M.RO2_DB@ZZZreal[27]"]
["RO2 二段CIP浸泡","C.M.RO2_DB@ZZZreal[29]"]
["RO2 产水杀菌时间READ","C.M.RO2_DB@ZZZreal[32]"]
["RO2 产水杀菌等待时间READ","C.M.RO2_DB@ZZZreal[33]"]
["RO2HOLD7","C.M.RO2_DB@ZZZreal[34]"]
["RO2HOLD8","C.M.RO2_DB@ZZZreal[35]"]
["RO2HOLD9","C.M.RO2_DB@ZZZreal[36]"]
["RO2HOLD10","C.M.RO2_DB@ZZZreal[37]"]
["RO2HOLD11","C.M.RO2_DB@ZZZreal[38]"]
["RO2HOLD12","C.M.RO2_DB@ZZZreal[39]"]
["RO2——碱冲洗设备ready","C.M.RO2_DB@ready[08]"]
["RO2——杀菌冲洗设备ready","C.M.RO2_DB@ready[09]"]
["RO2一段压差","C.M.RO2_DB@DPT_1"]
["RO2二段压差","C.M.RO2_DB@DPT_2"]
["RO2运行时间","C.M.RO2_DB@run_time"]
["RO2停止时间","C.M.RO2_DB@stop_time"]
["RO2不合格排水","C.M.RO2_DB@time_bhgs_display"]
["RO2产水时间","C.M.RO2_DB@time_CS_display"]
["RO2一段反冲","C.M.RO2_DB@time_FX1_display"]
["RO2开机等待","C.M.RO2_DB@time_kj_wait"]
["RO2排气时间","C.M.RO2_DB@time_kjcx_display1"]
["RO2开机冲洗","C.M.RO2_DB@time_kjcx_display2"]
["RO2杀菌间隔","C.M.RO2_DB@time_shajun_display"]
["RO2杀菌等待","C.M.RO2_DB@time_sj_wait"]
["RO2一段反冲","C.M.RO2_DB@time_sjcx1_display"]
["RO2二段反冲","C.M.RO2_DB@time_sjcx2_display"]
["RO2浸泡时间","C.M.RO2_DB@time_sjjp_display"]
["RO2加药时间","C.M.RO2_DB@time_sjjy_display"]
["RO2冲洗等待","C.M.RO2_DB@time_tj_wait"]
["RO2二段正冲","C.M.RO2_DB@time_ZX2_display"]
["RO2正常冲洗","C.M.RO2_DB@time_ZX12_display"]
["RO2反渗透段间泵故障","C.M.RO2_DJB@fault_total"]
["RO2反渗透段间泵运行","C.M.RO2_DJB@run"]
["RO2反渗透段间泵运行时间","C.M.RO2_DJB@run_time"]
["RO2反渗透段间泵运行频率","C.M.RO2_DJB_fre@out"]
["RO2反渗透二段产水流量","C.M.RO2_FT_CS2@out"]
["RO2反渗透进水流量","C.M.RO2_FT_JS@out"]
["RO2反渗透浓水流量","C.M.RO2_FT_NS@out"]
["RO2反渗透高压泵故障","C.M.RO2_GYB@fault_total"]
["RO2反渗透高压泵运行","C.M.RO2_GYB@run"]
["RO2反渗透高压泵运行时间","C.M.RO2_GYB@run_time"]
["RO2反渗透高压泵运行频率","C.M.RO2_GYB_fre@out"]
["RO2进水调节阀开度","C.M.RO2_GYBF_kd@out"]
["RO2排气阀1故障","C.M.RO2_PQF1@fault_total"]
["RO2排气阀2故障","C.M.RO2_PQF2@fault_total"]
["RO2排气阀3故障","C.M.RO2_PQF3@fault_total"]
["RO2排气阀4故障","C.M.RO2_PQF4@fault_total"]
["RO2排气阀5故障","C.M.RO2_PQF5@fault_total"]
["RO2排气阀6故障","C.M.RO2_PQF6@fault_total"]
["RO2排气阀7故障","C.M.RO2_PQF7@fault_total"]
["RO2产水压力","C.M.RO2_PT_CS@out"]
["RO2一段浓水压力","C.M.RO2_PT_DJ1@out"]
["RO2二段进水压力","C.M.RO2_PT_DJ2@out"]
["RO2一段进水压力","C.M.RO2_PT_JS@out"]
["RO2二段浓水压力","C.M.RO2_PT_NS@out"]
["RO3不合格水阀故障","C.M.RO3_BHGF@fault_total"]
["RO3产水CIP回水阀故障","C.M.RO3_CIP_CSHSF@fault_total"]
["RO3一段CIP回水阀故障","C.M.RO3_CIP_HSF1@fault_total"]
["RO3二段CIP回水阀故障","C.M.RO3_CIP_HSF2@fault_total"]
["RO3一段CIP进水阀故障","C.M.RO3_CIP_JSF1@fault_total"]
["RO3二段CIP进水阀故障","C.M.RO3_CIP_JSF2@fault_total"]
["产水排空阀故障","C.M.RO3_CIP_PKF1@fault_total"]
["RO3产水电导","C.M.RO3_Cond_CS@out"]
["RO3产水阀故障","C.M.RO3_CSF@fault_total"]
["RO3一段冲洗进水阀故障","C.M.RO3_CXJF1@fault_total"]
["RO3二段冲洗进水阀故障","C.M.RO3_CXJF2@fault_total"]
["RO3一段冲洗排水阀故障","C.M.RO3_CXPF1@fault_total"]
["RO3二段冲洗排水阀故障","C.M.RO3_CXPF2@fault_total"]
["RO3自动开机","C.M.RO3_DB@button[01]"]
["RO3自动停止","C.M.RO3_DB@button[02]"]
["RO3自动正常冲洗","C.M.RO3_DB@button[03]"]
["RO3自动反向冲洗","C.M.RO3_DB@button[04]"]
["RO3自动杀菌冲洗","C.M.RO3_DB@button[05]"]
["RO3全自动开机","C.M.RO3_DB@button[08]"]
["RO3一段CIP（保持）","C.M.RO3_DB@button[14]"]
["RO3二段CIP（保持）","C.M.RO3_DB@button[15]"]
["RO3一段酸洗（选中保持）","C.M.RO3_DB@button[16]"]
["RO3二段酸洗（选中保持）","C.M.RO3_DB@button[17]"]
["RO3一段碱洗（选中保持）","C.M.RO3_DB@button[18]"]
["RO3二段碱洗（选中保持）","C.M.RO3_DB@button[19]"]
["RO3一段非氧洗（选中保持）","C.M.RO3_DB@button[20]"]
["RO3二段非氧洗（选中保持）","C.M.RO3_DB@button[21]"]
["RO3一段酸洗（手动保持）","C.M.RO3_DB@button[22]"]
["RO3二段酸洗（手动保持）","C.M.RO3_DB@button[23]"]
["RO3一段碱洗（手动保持）","C.M.RO3_DB@button[24]"]
["RO3二段碱洗（手动保持）","C.M.RO3_DB@button[25]"]
["RO3一段非氧洗（手动保持）","C.M.RO3_DB@button[26]"]
["RO3二段非氧洗（手动保持）","C.M.RO3_DB@button[27]"]
["RO3HOLDHB1","C.M.RO3_DB@button[28]"]
["RO3HOLDHB2","C.M.RO3_DB@button[29]"]
["RO3HOLDHB3","C.M.RO3_DB@button[30]"]
["RO3HOLDHB4","C.M.RO3_DB@button[31]"]
["RO3 ZBOOL HOLD1","C.M.RO3_DB@Zbool[0]"]
["RO3 ZBOOL HOLD2","C.M.RO3_DB@Zbool[1]"]
["RO3 ZBOOL HOLD3","C.M.RO3_DB@Zbool[2]"]
["RO3 ZDint HOLD1","C.M.RO3_DB@ZDint[0]"]
["RO3 ZDint HOLD2","C.M.RO3_DB@ZDint[1]"]
["RO3 ZDint HOLD3","C.M.RO3_DB@ZDint[2]"]
["RO3 当前步序时间","C.M.RO3_DB@ZZZreal[0]"]
["RO3 1段酸洗记次数","C.M.RO3_DB@ZZZreal[2]"]
["RO3 2段酸洗记次数","C.M.RO3_DB@ZZZreal[3]"]
["RO3 1段J洗记次数","C.M.RO3_DB@ZZZreal[4]"]
["RO3 2段J洗记次数","C.M.RO3_DB@ZZZreal[5]"]
["RO3 1段FY洗记次数","C.M.RO3_DB@ZZZreal[6]"]
["RO3 2段FY洗记次数","C.M.RO3_DB@ZZZreal[7]"]
["RO3HOLD1","C.M.RO3_DB@ZZZreal[14]"]
["RO3HOLD2","C.M.RO3_DB@ZZZreal[15]"]
["RO3HOLD3","C.M.RO3_DB@ZZZreal[22]"]
["RO3HOLD4","C.M.RO3_DB@ZZZreal[23]"]
["RO3HOLD5","C.M.RO3_DB@ZZZreal[24]"]
["RO3HOLD6","C.M.RO3_DB@ZZZreal[25]"]
["RO3 一段CIP浸泡","C.M.RO3_DB@ZZZreal[27]"]
["RO3 二段CIP浸泡","C.M.RO3_DB@ZZZreal[29]"]
["RO3 产水杀菌时间READ","C.M.RO3_DB@ZZZreal[32]"]
["RO3 产水杀菌等待时间READ","C.M.RO3_DB@ZZZreal[33]"]
["RO3HOLD7","C.M.RO3_DB@ZZZreal[34]"]
["RO3HOLD8","C.M.RO3_DB@ZZZreal[35]"]
["RO3HOLD9","C.M.RO3_DB@ZZZreal[36]"]
["RO3HOLD10","C.M.RO3_DB@ZZZreal[37]"]
["RO3HOLD11","C.M.RO3_DB@ZZZreal[38]"]
["RO3HOLD12","C.M.RO3_DB@ZZZreal[39]"]
["RO3——碱冲洗设备ready","C.M.RO3_DB@ready[08]"]
["RO3——杀菌冲洗设备ready","C.M.RO3_DB@ready[09]"]
["RO3一段压差","C.M.RO3_DB@DPT_1"]
["RO3二段压差","C.M.RO3_DB@DPT_2"]
["RO3运行时间","C.M.RO3_DB@run_time"]
["RO3停止时间","C.M.RO3_DB@stop_time"]
["RO3不合格排水","C.M.RO3_DB@time_bhgs_display"]
["RO3产水时间","C.M.RO3_DB@time_CS_display"]
["RO3一段反冲","C.M.RO3_DB@time_FX1_display"]
["RO3开机等待","C.M.RO3_DB@time_kj_wait"]
["RO3排气时间","C.M.RO3_DB@time_kjcx_display1"]
["RO3开机冲洗","C.M.RO3_DB@time_kjcx_display2"]
["RO3杀菌间隔","C.M.RO3_DB@time_shajun_display"]
["RO3杀菌等待","C.M.RO3_DB@time_sj_wait"]
["RO3一段反冲","C.M.RO3_DB@time_sjcx1_display"]
["RO3二段反冲","C.M.RO3_DB@time_sjcx2_display"]
["RO3浸泡时间","C.M.RO3_DB@time_sjjp_display"]
["RO3加药时间","C.M.RO3_DB@time_sjjy_display"]
["RO3冲洗等待","C.M.RO3_DB@time_tj_wait"]
["RO3二段正冲","C.M.RO3_DB@time_ZX2_display"]
["RO3正常冲洗","C.M.RO3_DB@time_ZX12_display"]
["RO3反渗透段间泵故障","C.M.RO3_DJB@fault_total"]
["RO3反渗透段间泵运行","C.M.RO3_DJB@run"]
["RO3反渗透段间泵运行时间","C.M.RO3_DJB@run_time"]
["RO3反渗透段间泵运行频率","C.M.RO3_DJB_fre@out"]
["RO3反渗透二段产水流量","C.M.RO3_FT_CS2@out"]
["RO3反渗透进水流量","C.M.RO3_FT_JS@out"]
["RO3反渗透浓水流量","C.M.RO3_FT_NS@out"]
["RO3反渗透高压泵故障","C.M.RO3_GYB@fault_total"]
["RO3反渗透高压泵运行","C.M.RO3_GYB@run"]
["RO3反渗透高压泵运行时间","C.M.RO3_GYB@run_time"]
["RO3反渗透高压泵运行频率","C.M.RO3_GYB_fre@out"]
["RO3进水调节阀开度","C.M.RO3_GYBF_kd@out"]
["RO3排气阀1故障","C.M.RO3_PQF1@fault_total"]
["RO3排气阀2故障","C.M.RO3_PQF2@fault_total"]
["RO3排气阀3故障","C.M.RO3_PQF3@fault_total"]
["RO3排气阀4故障","C.M.RO3_PQF4@fault_total"]
["RO3排气阀5故障","C.M.RO3_PQF5@fault_total"]
["RO3排气阀6故障","C.M.RO3_PQF6@fault_total"]
["RO3排气阀7故障","C.M.RO3_PQF7@fault_total"]
["RO3产水压力","C.M.RO3_PT_CS@out"]
["RO3一段浓水压力","C.M.RO3_PT_DJ1@out"]
["RO3二段进水压力","C.M.RO3_PT_DJ2@out"]
["RO3一段进水压力","C.M.RO3_PT_JS@out"]
["RO3二段浓水压力","C.M.RO3_PT_NS@out"]
["RO4不合格水阀故障","C.M.RO4_BHGF@fault_total"]
["RO4产水CIP回水阀故障","C.M.RO4_CIP_CSHSF@fault_total"]
["RO4一段CIP回水阀故障","C.M.RO4_CIP_HSF1@fault_total"]
["RO4二段CIP回水阀故障","C.M.RO4_CIP_HSF2@fault_total"]
["RO4一段CIP进水阀故障","C.M.RO4_CIP_JSF1@fault_total"]
["RO4二段CIP进水阀故障","C.M.RO4_CIP_JSF2@fault_total"]
["进水排空阀故障","C.M.RO4_CIP_PKF1@fault_total"]
["回水排空阀故障","C.M.RO4_CIP_PKF2@fault_total"]
["RO4产水电导","C.M.RO4_Cond_CS@out"]
["RO4产水阀故障","C.M.RO4_CSF@fault_total"]
["RO4一段冲洗进水阀故障","C.M.RO4_CXJF1@fault_total"]
["RO4二段冲洗进水阀故障","C.M.RO4_CXJF2@fault_total"]
["RO4一段冲洗排水阀故障","C.M.RO4_CXPF1@fault_total"]
["RO4二段冲洗排水阀故障","C.M.RO4_CXPF2@fault_total"]
["RO4自动开机","C.M.RO4_DB@button[01]"]
["RO4自动停止","C.M.RO4_DB@button[02]"]
["RO4自动正常冲洗","C.M.RO4_DB@button[03]"]
["RO4自动反向冲洗","C.M.RO4_DB@button[04]"]
["RO4自动杀菌冲洗","C.M.RO4_DB@button[05]"]
["RO4全自动开机","C.M.RO4_DB@button[08]"]
["RO4一段CIP（保持）","C.M.RO4_DB@button[14]"]
["RO4二段CIP（保持）","C.M.RO4_DB@button[15]"]
["RO4一段酸洗（选中保持）","C.M.RO4_DB@button[16]"]
["RO4二段酸洗（选中保持）","C.M.RO4_DB@button[17]"]
["RO4一段碱洗（选中保持）","C.M.RO4_DB@button[18]"]
["RO4二段碱洗（选中保持）","C.M.RO4_DB@button[19]"]
["RO4一段非氧洗（选中保持）","C.M.RO4_DB@button[20]"]
["RO4二段非氧洗（选中保持）","C.M.RO4_DB@button[21]"]
["RO4一段酸洗（手动保持）","C.M.RO4_DB@button[22]"]
["RO4二段酸洗（手动保持）","C.M.RO4_DB@button[23]"]
["RO4一段碱洗（手动保持）","C.M.RO4_DB@button[24]"]
["RO4二段碱洗（手动保持）","C.M.RO4_DB@button[25]"]
["RO4一段非氧洗（手动保持）","C.M.RO4_DB@button[26]"]
["RO4二段非氧洗（手动保持）","C.M.RO4_DB@button[27]"]
["RO4HOLDHB1","C.M.RO4_DB@button[28]"]
["RO4HOLDHB2","C.M.RO4_DB@button[29]"]
["RO4HOLDHB3","C.M.RO4_DB@button[30]"]
["RO4HOLDHB4","C.M.RO4_DB@button[31]"]
["RO4 ZBOOL HOLD1","C.M.RO4_DB@Zbool[0]"]
["RO4 ZBOOL HOLD2","C.M.RO4_DB@Zbool[1]"]
["RO4 ZBOOL HOLD3","C.M.RO4_DB@Zbool[2]"]
["RO4 ZDint HOLD1","C.M.RO4_DB@ZDint[0]"]
["RO4 ZDint HOLD2","C.M.RO4_DB@ZDint[1]"]
["RO4 ZDint HOLD3","C.M.RO4_DB@ZDint[2]"]
["RO4当前步序时间","C.M.RO4_DB@ZZZreal[0]"]
["RO41段酸洗记次数","C.M.RO4_DB@ZZZreal[2]"]
["RO4 2段酸洗记次数","C.M.RO4_DB@ZZZreal[3]"]
["RO4 1段J洗记次数","C.M.RO4_DB@ZZZreal[4]"]
["RO4 2段J洗记次数","C.M.RO4_DB@ZZZreal[5]"]
["RO4 1段FY洗记次数","C.M.RO4_DB@ZZZreal[6]"]
["RO4 2段FY洗记次数","C.M.RO4_DB@ZZZreal[7]"]
["RO4HOLD1","C.M.RO4_DB@ZZZreal[14]"]
["RO4HOLD2","C.M.RO4_DB@ZZZreal[15]"]
["RO4HOLD3","C.M.RO4_DB@ZZZreal[22]"]
["RO4HOLD4","C.M.RO4_DB@ZZZreal[23]"]
["RO4HOLD5","C.M.RO4_DB@ZZZreal[24]"]
["RO4HOLD6","C.M.RO4_DB@ZZZreal[25]"]
["RO4一段CIP浸泡","C.M.RO4_DB@ZZZreal[27]"]
["RO4二段CIP浸泡","C.M.RO4_DB@ZZZreal[29]"]
["RO4产水杀菌时间READ","C.M.RO4_DB@ZZZreal[32]"]
["RO4产水杀菌等待时间READ","C.M.RO4_DB@ZZZreal[33]"]
["RO4HOLD7","C.M.RO4_DB@ZZZreal[34]"]
["RO4HOLD8","C.M.RO4_DB@ZZZreal[35]"]
["RO4HOLD9","C.M.RO4_DB@ZZZreal[36]"]
["RO4HOLD10","C.M.RO4_DB@ZZZreal[37]"]
["RO4HOLD11","C.M.RO4_DB@ZZZreal[38]"]
["RO4HOLD12","C.M.RO4_DB@ZZZreal[39]"]
["RO4——碱冲洗设备ready","C.M.RO4_DB@ready[08]"]
["RO4——杀菌冲洗设备ready","C.M.RO4_DB@ready[09]"]
["RO4一段压差","C.M.RO4_DB@DPT_1"]
["RO4二段压差","C.M.RO4_DB@DPT_2"]
["RO4运行时间","C.M.RO4_DB@run_time"]
["RO4停止时间","C.M.RO4_DB@stop_time"]
["RO4不合格排水","C.M.RO4_DB@time_bhgs_display"]
["RO4产水时间","C.M.RO4_DB@time_CS_display"]
["RO4一段反冲","C.M.RO4_DB@time_FX1_display"]
["RO4开机等待","C.M.RO4_DB@time_kj_wait"]
["RO4排气时间","C.M.RO4_DB@time_kjcx_display1"]
["RO4开机冲洗","C.M.RO4_DB@time_kjcx_display2"]
["RO4杀菌间隔","C.M.RO4_DB@time_shajun_display"]
["RO4杀菌等待","C.M.RO4_DB@time_sj_wait"]
["RO4一段反冲","C.M.RO4_DB@time_sjcx1_display"]
["RO4二段反冲","C.M.RO4_DB@time_sjcx2_display"]
["RO4浸泡时间","C.M.RO4_DB@time_sjjp_display"]
["RO4加药时间","C.M.RO4_DB@time_sjjy_display"]
["RO4冲洗等待","C.M.RO4_DB@time_tj_wait"]
["RO4二段正冲","C.M.RO4_DB@time_ZX2_display"]
["RO4正常冲洗","C.M.RO4_DB@time_ZX12_display"]
["RO4反渗透段间泵故障","C.M.RO4_DJB@fault_total"]
["RO4反渗透段间泵运行","C.M.RO4_DJB@run"]
["RO4反渗透段间泵运行时间","C.M.RO4_DJB@run_time"]
["RO4反渗透段间泵运行频率","C.M.RO4_DJB_fre@out"]
["RO4反渗透二段产水流量","C.M.RO4_FT_CS2@out"]
["RO4反渗透进水流量","C.M.RO4_FT_JS@out"]
["RO4反渗透浓水流量","C.M.RO4_FT_NS@out"]
["RO4反渗透高压泵故障","C.M.RO4_GYB@fault_total"]
["RO4反渗透高压泵运行","C.M.RO4_GYB@run"]
["RO4反渗透高压泵运行时间","C.M.RO4_GYB@run_time"]
["RO4反渗透高压泵运行频率","C.M.RO4_GYB_fre@out"]
["RO4进水调节阀开度","C.M.RO4_GYBF_kd@out"]
["RO4排气阀1故障","C.M.RO4_PQF1@fault_total"]
["RO4排气阀2故障","C.M.RO4_PQF2@fault_total"]
["RO4排气阀3故障","C.M.RO4_PQF3@fault_total"]
["RO4排气阀4故障","C.M.RO4_PQF4@fault_total"]
["RO4排气阀5故障","C.M.RO4_PQF5@fault_total"]
["RO4排气阀6故障","C.M.RO4_PQF6@fault_total"]
["RO4排气阀7故障","C.M.RO4_PQF7@fault_total"]
["RO4产水压力","C.M.RO4_PT_CS@out"]
["RO4一段浓水压力","C.M.RO4_PT_DJ1@out"]
["RO4二段进水压力","C.M.RO4_PT_DJ2@out"]
["RO4一段进水压力","C.M.RO4_PT_JS@out"]
["RO4二段浓水压力","C.M.RO4_PT_NS@out"]
["1#杀菌剂加药泵故障","C.M.SJJB1@fault_total"]
["1#杀菌剂加药泵运行","C.M.SJJB1@run"]
["1#杀菌剂加药泵运行时间","C.M.SJJB1@run_time"]
["2#杀菌剂加药泵故障","C.M.SJJB2@fault_total"]
["2#杀菌剂加药泵运行","C.M.SJJB2@run"]
["2#杀菌剂加药泵运行时间","C.M.SJJB2@run_time"]
["CIP-温度","C.M.TT_CIP@out"]
["1#脱碳风机故障","C.M.TTFJ1@fault_total"]
["1#脱碳风机运行","C.M.TTFJ1@run"]
["1#脱碳风机运行时间","C.M.TTFJ1@run_time"]
["2#脱碳风机故障","C.M.TTFJ2@fault_total"]
["2#脱碳风机运行","C.M.TTFJ2@run"]
["2#脱碳风机运行时间","C.M.TTFJ2@run_time"]
["UFCEB排放阀故障","C.M.UF_CEBPF@fault_total"]
["超滤总产水余氯","C.M.UF_Cl_ZCS@out"]
["UF排气阀故障","C.M.UF_CSPQF@fault_total"]
["超滤反洗流量","C.M.UF_FT_FX@out"]
["超滤总产水流量","C.M.UF_FT_ZCS@out"]
["1#超滤反洗水泵故障","C.M.UF_FXB1@fault_total"]
["1#超滤反洗水泵运行","C.M.UF_FXB1@run"]
["1#超滤反洗水泵运行时间","C.M.UF_FXB1@run_time"]
["1#超滤反洗水泵运行频率","C.M.UF_FXB1_fre@out"]
["2#超滤反洗水泵故障","C.M.UF_FXB2@fault_total"]
["2#超滤反洗水泵运行","C.M.UF_FXB2@run"]
["2#超滤反洗水泵运行时间","C.M.UF_FXB2@run_time"]
["2#超滤反洗水泵运行频率","C.M.UF_FXB2_fre@out"]
["3#超滤反洗水泵故障","C.M.UF_FXB3@fault_total"]
["3#超滤反洗水泵运行","C.M.UF_FXB3@run"]
["3#超滤反洗水泵运行时间","C.M.UF_FXB3@run_time"]
["3#超滤反洗水泵运行频率","C.M.UF_FXB3_fre@out"]
["UF反洗排水阀故障","C.M.UF_FXPF@fault_total"]
["反洗水池补水阀开度","C.M.UF_FXSCBSF_kd@out"]
["1#超滤供水泵故障","C.M.UF_GSB1@fault_total"]
["1#超滤供水泵运行","C.M.UF_GSB1@run"]
["1#超滤供水泵运行时间","C.M.UF_GSB1@run_time"]
["1#超滤供水泵运行频率","C.M.UF_GSB1_fre@out"]
["2#超滤供水泵故障","C.M.UF_GSB2@fault_total"]
["2#超滤供水泵运行","C.M.UF_GSB2@run"]
["2#超滤供水泵运行时间","C.M.UF_GSB2@run_time"]
["2#超滤供水泵运行频率","C.M.UF_GSB2_fre@out"]
["3#超滤供水泵故障","C.M.UF_GSB3@fault_total"]
["3#超滤供水泵运行","C.M.UF_GSB3@run"]
["3#超滤供水泵运行时间","C.M.UF_GSB3@run_time"]
["3#超滤供水泵运行频率","C.M.UF_GSB3_fre@out"]
["4#超滤供水泵故障","C.M.UF_GSB4@fault_total"]
["4#超滤供水泵运行","C.M.UF_GSB4@run"]
["4#超滤供水泵运行时间","C.M.UF_GSB4@run_time"]
["4#超滤供水泵运行频率","C.M.UF_GSB4_fre@out"]
["超滤总产水ORP","C.M.UF_ORP_ZCS@out"]
["超滤总产水PH","C.M.UF_PH_ZCS@out"]
["超滤反洗压力","C.M.UF_PT_FX@out"]
["超滤总产水压力","C.M.UF_PT_ZCS@out"]
["超滤总进水压力","C.M.UF_PT_ZJS@out"]
["超滤总产水浊度","C.M.UF_Tur_ZCS@out"]
["超滤总进水浊度","C.M.UF_Tur_ZJS@out"]
["UF1不合格水阀故障","C.M.UF1_BHGF@fault_total"]
["UF1产水阀故障","C.M.UF1_CSF@fault_total"]
["UF1右侧排空阀故障","C.M.UF1_CSPKF@fault_total"]
["UF1不合格冲洗","C.M.UF1_DB@BHG_residue"]
["UF1半自动开机","C.M.UF1_DB@button[01]"]
["UF1半自动停止","C.M.UF1_DB@button[02]"]
["UF1半自动反洗","C.M.UF1_DB@button[03]"]
["UF1半自动CEB","C.M.UF1_DB@button[04]"]
["UF1药剂残留","C.M.UF1_DB@chemical_residue"]
["UF1CIP1周期次数显示","C.M.UF1_DB@cycle_CIP1_display"]
["UF1CIP2周期次数显示","C.M.UF1_DB@cycle_CIP2_display"]
["UF1次数显示（CEB周期）","C.M.UF1_DB@cycle_out"]
["UF1跨膜压差","C.M.UF1_DB@press_PV"]
["UF1CIP配药装备好","C.M.UF1_DB@ready_CIP_chemical"]
["UF1产水累计时间","C.M.UF1_DB@run_time"]
["UF1停机时间","C.M.UF1_DB@stop_time"]
["UF1CIP时间显示","C.M.UF1_DB@time_CIP_display"]
["UF1时间显示","C.M.UF1_DB@time_display"]
["UF1产水时间显示","C.M.UF1_DB@time_production_display"]
["UF1进水流量","C.M.UF1_FT_JS@out"]
["UF1反洗进水阀故障","C.M.UF1_FXJSF@fault_total"]
["UF1反洗排水阀故障","C.M.UF1_FXPSF@fault_total"]
["UF1隔断阀故障","C.M.UF1_GDF@fault_total"]
["UF1进水调节阀开度","C.M.UF1_JSF_kd@out"]
["UF1左侧排空阀故障","C.M.UF1_JSPKF@fault_total"]
["UF1左产排气阀故障","C.M.UF1_PQF1@fault_total"]
["UF1左进排气阀故障","C.M.UF1_PQF2@fault_total"]
["UF1右进排气阀故障","C.M.UF1_PQF3@fault_total"]
["UF1右产排气阀故障","C.M.UF1_PQF4@fault_total"]
["UF1产水压力","C.M.UF1_PT_CS@out"]
["UF1进水压力","C.M.UF1_PT_JS@out"]
["UF2不合格水阀故障","C.M.UF2_BHGF@fault_total"]
["UF2产水阀故障","C.M.UF2_CSF@fault_total"]
["UF2右侧排空阀故障","C.M.UF2_CSPKF@fault_total"]
["UF2不合格冲洗","C.M.UF2_DB@BHG_residue"]
["UF2半自动开机","C.M.UF2_DB@button[01]"]
["UF2半自动停止","C.M.UF2_DB@button[02]"]
["UF2半自动反洗","C.M.UF2_DB@button[03]"]
["UF2半自动CEB","C.M.UF2_DB@button[04]"]
["UF2药剂残留","C.M.UF2_DB@chemical_residue"]
["UF2CIP1周期次数显示","C.M.UF2_DB@cycle_CIP1_display"]
["UF2CIP2周期次数显示","C.M.UF2_DB@cycle_CIP2_display"]
["UF2次数显示（CEB周期）","C.M.UF2_DB@cycle_out"]
["UF2跨膜压差","C.M.UF2_DB@press_PV"]
["UF2CIP配药装备好","C.M.UF2_DB@ready_CIP_chemical"]
["UF2产水累计时间","C.M.UF2_DB@run_time"]
["UF2停机时间","C.M.UF2_DB@stop_time"]
["UF2CIP时间显示","C.M.UF2_DB@time_CIP_display"]
["UF2时间显示","C.M.UF2_DB@time_display"]
["UF2产水时间显示","C.M.UF2_DB@time_production_display"]
["UF2进水流量","C.M.UF2_FT_JS@out"]
["UF2反洗进水阀故障","C.M.UF2_FXJSF@fault_total"]
["UF2反洗排水阀故障","C.M.UF2_FXPSF@fault_total"]
["UF2隔断阀故障","C.M.UF2_GDF@fault_total"]
["UF2进水调节阀开度","C.M.UF2_JSF_kd@out"]
["UF2左侧排空阀故障","C.M.UF2_JSPKF@fault_total"]
["UF2左产排气阀故障","C.M.UF2_PQF1@fault_total"]
["UF2左进排气阀故障","C.M.UF2_PQF2@fault_total"]
["UF2右进排气阀故障","C.M.UF2_PQF3@fault_total"]
["UF2右产排气阀故障","C.M.UF2_PQF4@fault_total"]
["UF2产水压力","C.M.UF2_PT_CS@out"]
["UF2进水压力","C.M.UF2_PT_JS@out"]
["UF3不合格水阀故障","C.M.UF3_BHGF@fault_total"]
["UF3产水阀故障","C.M.UF3_CSF@fault_total"]
["UF3右侧排空阀故障","C.M.UF3_CSPKF@fault_total"]
["UF3不合格冲洗","C.M.UF3_DB@BHG_residue"]
["UF3半自动开机","C.M.UF3_DB@button[01]"]
["UF3半自动停止","C.M.UF3_DB@button[02]"]
["UF3半自动反洗","C.M.UF3_DB@button[03]"]
["UF3半自动CEB","C.M.UF3_DB@button[04]"]
["UF3药剂残留","C.M.UF3_DB@chemical_residue"]
["UF3CIP1周期次数显示","C.M.UF3_DB@cycle_CIP1_display"]
["UF3CIP2周期次数显示","C.M.UF3_DB@cycle_CIP2_display"]
["UF3次数显示（CEB周期）","C.M.UF3_DB@cycle_out"]
["UF3跨膜压差","C.M.UF3_DB@press_PV"]
["UF3CIP配药装备好","C.M.UF3_DB@ready_CIP_chemical"]
["UF3产水累计时间","C.M.UF3_DB@run_time"]
["UF3停机时间","C.M.UF3_DB@stop_time"]
["UF3CIP时间显示","C.M.UF3_DB@time_CIP_display"]
["UF3时间显示","C.M.UF3_DB@time_display"]
["UF3产水时间显示","C.M.UF3_DB@time_production_display"]
["UF3进水流量","C.M.UF3_FT_JS@out"]
["UF3反洗进水阀故障","C.M.UF3_FXJSF@fault_total"]
["UF3反洗排水阀故障","C.M.UF3_FXPSF@fault_total"]
["UF3隔断阀故障","C.M.UF3_GDF@fault_total"]
["UF3进水调节阀开度","C.M.UF3_JSF_kd@out"]
["UF3左侧排空阀故障","C.M.UF3_JSPKF@fault_total"]
["UF3左产排气阀故障","C.M.UF3_PQF1@fault_total"]
["UF3左进排气阀故障","C.M.UF3_PQF2@fault_total"]
["UF3右进排气阀故障","C.M.UF3_PQF3@fault_total"]
["UF3右产排气阀故障","C.M.UF3_PQF4@fault_total"]
["UF3产水压力","C.M.UF3_PT_CS@out"]
["UF3进水压力","C.M.UF3_PT_JS@out"]
["UF4不合格水阀故障","C.M.UF4_BHGF@fault_total"]
["UF4产水阀故障","C.M.UF4_CSF@fault_total"]
["UF4右侧排空阀故障","C.M.UF4_CSPKF@fault_total"]
["UF4不合格冲洗","C.M.UF4_DB@BHG_residue"]
["UF4半自动开机","C.M.UF4_DB@button[01]"]
["UF4半自动停止","C.M.UF4_DB@button[02]"]
["UF4半自动反洗","C.M.UF4_DB@button[03]"]
["UF4半自动CEB","C.M.UF4_DB@button[04]"]
["UF4药剂残留","C.M.UF4_DB@chemical_residue"]
["UF4CIP1周期次数显示","C.M.UF4_DB@cycle_CIP1_display"]
["UF4CIP2周期次数显示","C.M.UF4_DB@cycle_CIP2_display"]
["UF4次数显示（CEB周期）","C.M.UF4_DB@cycle_out"]
["UF4跨膜压差","C.M.UF4_DB@press_PV"]
["UF4CIP配药装备好","C.M.UF4_DB@ready_CIP_chemical"]
["UF4产水累计时间","C.M.UF4_DB@run_time"]
["UF4停机时间","C.M.UF4_DB@stop_time"]
["UF4CIP时间显示","C.M.UF4_DB@time_CIP_display"]
["UF4时间显示","C.M.UF4_DB@time_display"]
["UF4产水时间显示","C.M.UF4_DB@time_production_display"]
["UF4进水流量","C.M.UF4_FT_JS@out"]
["UF4反洗进水阀故障","C.M.UF4_FXJSF@fault_total"]
["UF4反洗排水阀故障","C.M.UF4_FXPSF@fault_total"]
["UF4隔断阀故障","C.M.UF4_GDF@fault_total"]
["UF4进水调节阀开度","C.M.UF4_JSF_kd@out"]
["UF4左侧排空阀故障","C.M.UF4_JSPKF@fault_total"]
["UF4左产排气阀故障","C.M.UF4_PQF1@fault_total"]
["UF4左进排气阀故障","C.M.UF4_PQF2@fault_total"]
["UF4右进排气阀故障","C.M.UF4_PQF3@fault_total"]
["UF4右产排气阀故障","C.M.UF4_PQF4@fault_total"]
["UF4产水压力","C.M.UF4_PT_CS@out"]
["UF4进水压力","C.M.UF4_PT_JS@out"]
["卸料泵故障","C.M.XLB@fault_total"]
["卸料泵运行","C.M.XLB@run"]
["卸料泵运行时间","C.M.XLB@run_time"]
["1#中和废水泵故障","C.M.ZH_FSB1@fault_total"]
["1#中和废水泵运行","C.M.ZH_FSB1@run"]
["1#中和废水泵运行时间","C.M.ZH_FSB1@run_time"]
["2#中和废水泵故障","C.M.ZH_FSB2@fault_total"]
["2#中和废水泵运行","C.M.ZH_FSB2@run"]
["2#中和废水泵运行时间","C.M.ZH_FSB2@run_time"]
["中和ORP","C.M.ZH_ORP@out"]
["中和水池PH","C.M.ZH_PH@out"]
["中和外排阀故障","C.M.ZH_WPF@fault_total"]
["RO1杀菌剂阀故障","C5.M5.RO1_SJJF_GZ"]
["RO2杀菌剂阀故障","C5.M5.RO2_SJJF_GZ"]
["RO3杀菌剂阀故障","C5.M5.RO3_SJJF_GZ"]
["RO4杀菌剂阀故障","C5.M5.RO4_SJJF_GZ"]
["杀菌剂阀远控","C5.M5.RO_YK"]
["RO1杀菌启动","C5.M5.RO1_SJQD"]
["RO1杀菌时长显示","C5.M5.RO1_SJSCXS"]
["RO2杀菌启动","C5.M5.RO2_SJQD"]
["RO2杀菌时长显示","C5.M5.RO2_SJSCXS"]
["RO3杀菌启动","C5.M5.RO3_SJQD"]
["RO3杀菌时长显示","C5.M5.RO3_SJSCXS"]
["RO4杀菌启动","C5.M5.RO4_SJQD"]
["RO4杀菌时长显示","C5.M5.RO4_SJSCXS"]
["RO1一段加药时长（显示）计时","C5.M5.RO1_YDJYSCXS"]
["RO1一段加药状态","C5.M5.RO1_YDJYZT"]
["RO1二段加药时长（显示）计时","C5.M5.RO1_EDJYSCXS"]
["RO1二段加药状态","C5.M5.RO1_EDJYZT"]
["RO2一段加药时长（显示）计时","C5.M5.RO2_YDJYSCXS"]
["RO2一段加药状态","C5.M5.RO2_YDJYZT"]
["RO2二段加药时长（显示）计时","C5.M5.RO2_EDJYSCXS"]
["RO2二段加药状态","C5.M5.RO2_EDJYZT"]
["RO3一段加药时长（显示）计时","C5.M5.RO3_YDJYSCXS"]
["RO3一段加药状态","C5.M5.RO3_YDJYZT"]
["RO3二段加药时长（显示）计时","C5.M5.RO3_EDJYSCXS"]
["RO3二段加药状态","C5.M5.RO3_EDJYZT"]
["RO4一段加药时长（显示）计时","C5.M5.RO4_YDJYSCXS"]
["RO4一段加药状态","C5.M5.RO4_YDJYZT"]
["RO4二段加药时长（显示）计时","C5.M5.RO4_EDJYSCXS"]
["RO4二段加药状态","C5.M5.RO4_EDJYZT"]
["高德PH","OPC.GD.P11.PH"]
["高德电导率","OPC.GD.P11.DDL"]
["高德电导率_A","OPC.GD.P11.DDL_A"]
["高德累计流量","OPC.GD.P11.LJLL"]
["高德瞬时流量","OPC.GD.P11.SSLL"]
["健鼎PH","OPC.JD.P21.PH"]
["健鼎电导率","OPC.JD.P21.DDL"]
["健鼎电导率_A","OPC.JD.P21.DDL_A"]
["健鼎累计流量","OPC.JD.P21.LJLL"]
["健鼎瞬时流量","OPC.JD.P21.SSLL"]
["健鼎调节阀反馈","OPC.JD.P22.TJF_FK"]
["能达PH","OPC.ND.P31.PH"]
["能达电导率","OPC.ND.P31.DDL"]
["能达电导率_A","OPC.ND.P31.DDL_A"]
["能达累计流量","OPC.ND.P32.LJLL"]
["能达瞬时流量","OPC.ND.P32.SSLL"]
["统盟2厂PH","OPC.TM.P41.PH"]
["统盟2厂电导率","OPC.TM.P41.DDL"]
["统盟2厂电导率_A","OPC.TM.P41.DDL_A"]
["统盟2厂累计流量","OPC.TM.P41.LJLL"]
["统盟2厂瞬时流量","OPC.TM.P41.SSLL"]
["反渗透回收率","ROHSL"]
["高压配电室温度","C2.M21.WD1"]
["管廊间温度1","C2.M22.WD2"]
["管廊间温度2","C2.M23.WD3"]
["低压配电室温度","C2.M24.WD4"]
["膜车间温度1","C2.M25.WD5"]
["膜车间温度2","C2.M26.WD6"]
["加药间温度1","C3.M31.WD7"]
["泵房温度1","C3.M32.WD8"]
["泵房温度2","C3.M33.WD9"]
["加药间温度2","C3.M34.WD10"]
["超滤供水泵A 功率","WG_A.1AA1-1.A13"]
["超滤供水泵A 累计电量","_AdvancedTags.1AA1_1_LJ"]
["超滤供水泵B 功率","WG_A.1AA1-2.A13"]
["超滤供水泵B 累计电量","_AdvancedTags.1AA1_2_LJ"]
["超滤反洗泵A 功率","WG_A.1AA2-1.A13"]
["超滤反洗泵A 累计电量","_AdvancedTags.1AA2_1_LJ"]
["超滤反洗泵B 功率","WG_A.1AA2-2.A13"]
["超滤反洗泵B 累计电量","_AdvancedTags.1AA2_2_LJ"]
["RO高压泵A 功率","WG_A.1AA3.A13"]
["RO高压泵A 累计电量","_AdvancedTags.1AA3_LJ"]
["RO高压泵B 功率","WG_A.1AA4.A13"]
["RO高压泵B 累计电量","_AdvancedTags.1AA4_LJ"]
["RO段间泵A 功率","WG_A.1AA5-1.A13"]
["RO段间泵A 累计电量","_AdvancedTags.1AA5_1_LJ"]
["RO段间泵B 功率","WG_A.1AA5-2.A13"]
["RO段间泵B 累计电量","_AdvancedTags.1AA5_2_LJ"]
["RO外供水泵A 功率","WG_A.1AA6.A13"]
["RO外供水泵A 累计电量","_AdvancedTags.1AA6_LJ"]
["大水量冲洗泵A 功率","WG_A.1AA7-1.A13"]
["大水量冲洗泵A 累计电量","_AdvancedTags.1AA7_1_LJ"]
["化学清洗水泵A 功率","WG_A.1AA7-2.A13"]
["化学清洗水泵A 累计电量","_AdvancedTags.1AA7_2_LJ"]
["脱碳风机A 功率","WG_B.1AA8-1.A13"]
["脱碳风机A 累计电量","_AdvancedTags.1AA8_1_LJ"]
["脱碳风机B 功率","WG_B.1AA8-2.A13"]
["脱碳风机B 累计电量","_AdvancedTags.1AA8_2_LJ"]
["中和废水泵A 功率","WG_B.1AA8-3.A13"]
["中和废水泵A 累计电量","_AdvancedTags.1AA8_3_LJ"]
["中和废水泵B 功率","WG_B.1AA8-4.A13"]
["中和废水泵B 累计电量","_AdvancedTags.1AA8_4_LJ"]
["清洗水箱电加热器A 功率","WG_B.1AA8-5.A13"]
["清洗水箱电加热器A 累计电量","_AdvancedTags.1AA8_5_LJ"]
["清洗水箱电加热器B 功率","WG_B.1AA8-6.A13"]
["清洗水箱电加热器B 累计电量","_AdvancedTags.1AA8_6_LJ"]
["泵房潜污泵A 功率","WG_B.1AA9-1.A13"]
["泵房潜污泵A 累计电量","_AdvancedTags.1AA9_1_LJ"]
["泵房潜污泵B 功率","WG_B.1AA9-2.A13"]
["泵房潜污泵B 累计电量","_AdvancedTags.1AA9_2_LJ"]
["泵房潜污泵C 功率","WG_B.1AA9-3.A13"]
["泵房潜污泵C 累计电量","_AdvancedTags.1AA9_3_LJ"]
["泵房潜污泵D 功率","WG_B.1AA9-4.A13"]
["泵房潜污泵D 累计电量","_AdvancedTags.1AA9_4_LJ"]
["空压机A 功率","WG_B.1AA9-5.A13"]
["空压机A 累计电量","_AdvancedTags.1AA9_5_LJ"]
["空压机B 功率","WG_B.1AA9-6.A13"]
["空压机B 累计电量","_AdvancedTags.1AA9_6_LJ"]
["供水泵房间电动葫芦 功率","WG_B.1AA9-7.A13"]
["供水泵房间电动葫芦 累计电量","_AdvancedTags.1AA9_7_LJ"]
["UPS柜 功率","WG_B.1AA9-8.A13"]
["UPS柜 累计电量","_AdvancedTags.1AA9_8_LJ"]
["轴流风机柜 功率","WG_B.1AA9-9.A13"]
["轴流风机柜 累计电量","_AdvancedTags.1AA9_9_LJ"]
["辅助用房 功率","WG_B.1AA10-1.A13"]
["辅助用房 累计电量","_AdvancedTags.1AA10_1_LJ"]
["门卫 功率","WG_B.1AA10-2.A13"]
["门卫 累计电量","_AdvancedTags.1AA10_2_LJ"]
["夹层中控室空调 功率","WG_B.1AA10-3.A13"]
["夹层中控室空调 累计电量","_AdvancedTags.1AA10_3_LJ"]
["夹层低压配电间空调 功率","WG_B.1AA10-4.A13"]
["夹层低压配电间空调 累计电量","_AdvancedTags.1AA10_4_LJ"]
["一层高压配电间空调 功率","WG_B.1AA10-5.A13"]
["一层高压配电间空调 累计电量","_AdvancedTags.1AA10_5_LJ"]
["照明箱 功率","WG_B.1AA10-6.A13"]
["照明箱 累计电量","_AdvancedTags.1AA10_6_LJ"]
["超滤供水泵D 功率","WG_B.1AA11.A13"]
["超滤供水泵D 累计电量","_AdvancedTags.1AA11_LJ"]
["超滤供水泵C 功率","WG_C.2AA1-1.A13"]
["超滤供水泵C 累计电量","_AdvancedTags.2AA1_1_LJ"]
["超滤反洗泵C 功率","WG_C.2AA1-2.A13"]
["超滤反洗泵C 累计电量","_AdvancedTags.2AA1_2_LJ"]
["RO高压泵C 功率","WG_C.2AA2.A13"]
["RO高压泵C 累计电量","_AdvancedTags.2AA2_LJ"]
["RO高压泵D 功率","WG_C.2AA3.A13"]
["RO高压泵D 累计电量","_AdvancedTags.2AA3_LJ"]
["RO段间泵C 功率","WG_C.2AA4-1.A13"]
["RO段间泵C 累计电量","_AdvancedTags.2AA4_1_LJ"]
["RO段间泵D 功率","WG_C.2AA4-2.A13"]
["RO段间泵D 累计电量","_AdvancedTags.2AA4_2_LJ"]
["RO外供水泵B 功率","WG_C.2AA5.A13"]
["RO外供水泵B 累计电量","_AdvancedTags.2AA5_LJ"]
["RO外供水泵C 功率","WG_C.2AA6.A13"]
["RO外供水泵C 累计电量","_AdvancedTags.2AA6_LJ"]
["大水量冲洗泵B 功率","WG_C.2AA7-1.A13"]
["大水量冲洗泵B 累计电量","_AdvancedTags.2AA7_1_LJ"]
["化学清洗水泵B 功率","WG_C.2AA7-2.A13"]
["化学清洗水泵B 累计电量","_AdvancedTags.2AA7_2_LJ"]
["反渗透冲洗水泵A温度","C4.M4.RO_CXB1_WD"]
["超滤供水泵A温度","C4.M4.UF_GSB1_WD"]
["反渗透高压泵A温度","C4.M4.RO1_GYB_WD"]
["反渗透外供水泵A温度","C4.M4.RO_WGB1_WD"]
["超滤反洗水泵A温度","C4.M4.UF_FXB1_WD"]
["段间泵A温度","C4.M4.RO1_DJB_WD"]
["反渗透冲洗水泵AX轴速度","C4.M4.RO_CXB1_XSD"]
["反渗透冲洗水泵AY轴速度","C4.M4.RO_CXB1_YSD"]
["反渗透冲洗水泵AZ轴速度","C4.M4.RO_CXB1_ZSD"]
["反渗透冲洗水泵AX轴位移","C4.M4.RO_CXB1_XWY"]
["反渗透冲洗水泵AY轴位移","C4.M4.RO_CXB1_YWY"]
["反渗透冲洗水泵AZ轴位移","C4.M4.RO_CXB1_ZWY"]
["超滤供水泵AX轴速度","C4.M4.UF_GSB1_XSD"]
["超滤供水泵AY轴速度","C4.M4.UF_GSB1_YSD"]
["超滤供水泵AZ轴速度","C4.M4.UF_GSB1_ZSD"]
["超滤供水泵AX轴位移","C4.M4.UF_GSB1_XWY"]
["超滤供水泵AY轴位移","C4.M4.UF_GSB1_YWY"]
["超滤供水泵AZ轴位移","C4.M4.UF_GSB1_ZWY"]
["反渗透高压泵AX轴速度","C4.M4.RO1_GYB_XSD"]
["反渗透高压泵AY轴速度","C4.M4.RO1_GYB_YSD"]
["反渗透高压泵AZ轴速度","C4.M4.RO1_GYB_ZSD"]
["反渗透高压泵AX轴位移","C4.M4.RO1_GYB_XWY"]
["反渗透高压泵AY轴位移","C4.M4.RO1_GYB_YWY"]
["反渗透高压泵AZ轴位移","C4.M4.RO1_GYB_ZWY"]
["反渗透外供水泵AX轴速度","C4.M4.RO_WGB1_XSD"]
["反渗透外供水泵AY轴速度","C4.M4.RO_WGB1_YSD"]
["反渗透外供水泵AZ轴速度","C4.M4.RO_WGB1_ZSD"]
["反渗透外供水泵AX轴位移","C4.M4.RO_WGB1_XWY"]
["反渗透外供水泵AY轴位移","C4.M4.RO_WGB1_YWY"]
["反渗透外供水泵AZ轴位移","C4.M4.RO_WGB1_ZWY"]
["超滤反洗水泵AX轴速度","C4.M4.UF_FXB1_XSD"]
["超滤反洗水泵AY轴速度","C4.M4.UF_FXB1_YSD"]
["超滤反洗水泵AZ轴速度","C4.M4.UF_FXB1_ZSD"]
["超滤反洗水泵AX轴位移","C4.M4.UF_FXB1_XWY"]
["超滤反洗水泵AY轴位移","C4.M4.UF_FXB1_YWY"]
["超滤反洗水泵AZ轴位移","C4.M4.UF_FXB1_ZWY"]
["段间泵AX轴速度","C4.M4.RO1_DJB_XSD"]
["段间泵AY轴速度","C4.M4.RO1_DJB_YSD"]
["段间泵AZ轴速度","C4.M4.RO1_DJB_ZSD"]
["段间泵AX轴位移","C4.M4.RO1_DJB_XWY"]
["段间泵AY轴位移","C4.M4.RO1_DJB_YWY"]
["段间泵AZ轴位移","C4.M4.RO1_DJB_ZWY"]
["阻垢剂加药泵噪音","C4.M4.ZY_ZGJB"]
["阻垢剂加药泵50Hz噪音","C4.M4.ZY_ZGJB_F1"]
["阻垢剂加药泵100Hz噪音","C4.M4.ZY_ZGJB_F2"]
["阻垢剂加药泵150Hz噪音","C4.M4.ZY_ZGJB_F3"]
["阻垢剂加药泵200Hz噪音","C4.M4.ZY_ZGJB_F4"]
["阻垢剂加药泵250Hz噪音","C4.M4.ZY_ZGJB_F5"]
["阻垢剂加药泵300Hz噪音","C4.M4.ZY_ZGJB_F6"]
["阻垢剂加药泵350Hz噪音","C4.M4.ZY_ZGJB_F7"]
["阻垢剂加药泵400Hz噪音","C4.M4.ZY_ZGJB_F8"]
["阻垢剂加药泵450Hz噪音","C4.M4.ZY_ZGJB_F9"]
["阻垢剂加药泵500Hz噪音","C4.M4.ZY_ZGJB_F10"]
["阻垢剂加药泵550Hz噪音","C4.M4.ZY_ZGJB_F11"]
["阻垢剂加药泵600Hz噪音","C4.M4.ZY_ZGJB_F12"]
["阻垢剂加药泵650Hz噪音","C4.M4.ZY_ZGJB_F13"]
["阻垢剂加药泵700Hz噪音","C4.M4.ZY_ZGJB_F14"]
["阻垢剂加药泵750Hz噪音","C4.M4.ZY_ZGJB_F15"]
["阻垢剂加药泵800Hz噪音","C4.M4.ZY_ZGJB_F16"]
["阻垢剂加药泵850Hz噪音","C4.M4.ZY_ZGJB_F17"]
["阻垢剂加药泵900Hz噪音","C4.M4.ZY_ZGJB_F18"]
["阻垢剂加药泵950Hz噪音","C4.M4.ZY_ZGJB_F19"]
["阻垢剂加药泵1000Hz噪音","C4.M4.ZY_ZGJB_F20"]
["阻垢剂加药泵1050Hz噪音","C4.M4.ZY_ZGJB_F21"]
["阻垢剂加药泵1100Hz噪音","C4.M4.ZY_ZGJB_F22"]
["阻垢剂加药泵1150Hz噪音","C4.M4.ZY_ZGJB_F23"]
["阻垢剂加药泵1200Hz噪音","C4.M4.ZY_ZGJB_F24"]
["阻垢剂加药泵1250Hz噪音","C4.M4.ZY_ZGJB_F25"]
["阻垢剂加药泵1300Hz噪音","C4.M4.ZY_ZGJB_F26"]
["阻垢剂加药泵1350Hz噪音","C4.M4.ZY_ZGJB_F27"]
["阻垢剂加药泵1400Hz噪音","C4.M4.ZY_ZGJB_F28"]
["阻垢剂加药泵1450Hz噪音","C4.M4.ZY_ZGJB_F29"]
["阻垢剂加药泵1500Hz噪音","C4.M4.ZY_ZGJB_F30"]
["阻垢剂加药泵1550Hz噪音","C4.M4.ZY_ZGJB_F31"]
["阻垢剂加药泵1600Hz噪音","C4.M4.ZY_ZGJB_F32"]
["阻垢剂加药泵1650Hz噪音","C4.M4.ZY_ZGJB_F33"]
["阻垢剂加药泵1700Hz噪音","C4.M4.ZY_ZGJB_F34"]
["阻垢剂加药泵1750Hz噪音","C4.M4.ZY_ZGJB_F35"]
["阻垢剂加药泵1800Hz噪音","C4.M4.ZY_ZGJB_F36"]
["阻垢剂加药泵1850Hz噪音","C4.M4.ZY_ZGJB_F37"]
["阻垢剂加药泵1900Hz噪音","C4.M4.ZY_ZGJB_F38"]
["阻垢剂加药泵1950Hz噪音","C4.M4.ZY_ZGJB_F39"]
["阻垢剂加药泵2000Hz噪音","C4.M4.ZY_ZGJB_F40"]
["阻垢剂加药泵2050Hz噪音","C4.M4.ZY_ZGJB_F41"]
["阻垢剂加药泵2100Hz噪音","C4.M4.ZY_ZGJB_F42"]
["阻垢剂加药泵2150Hz噪音","C4.M4.ZY_ZGJB_F43"]
["阻垢剂加药泵2200Hz噪音","C4.M4.ZY_ZGJB_F44"]
["阻垢剂加药泵2250Hz噪音","C4.M4.ZY_ZGJB_F45"]
["阻垢剂加药泵2300Hz噪音","C4.M4.ZY_ZGJB_F46"]
["阻垢剂加药泵2350Hz噪音","C4.M4.ZY_ZGJB_F47"]
["阻垢剂加药泵2400Hz噪音","C4.M4.ZY_ZGJB_F48"]
["阻垢剂加药泵2450Hz噪音","C4.M4.ZY_ZGJB_F49"]
["阻垢剂加药泵2500Hz噪音","C4.M4.ZY_ZGJB_F50"]
["阻垢剂加药泵2550Hz噪音","C4.M4.ZY_ZGJB_F51"]
["阻垢剂加药泵2600Hz噪音","C4.M4.ZY_ZGJB_F52"]
["阻垢剂加药泵2650Hz噪音","C4.M4.ZY_ZGJB_F53"]
["阻垢剂加药泵2700Hz噪音","C4.M4.ZY_ZGJB_F54"]
["阻垢剂加药泵2750Hz噪音","C4.M4.ZY_ZGJB_F55"]
["阻垢剂加药泵2800Hz噪音","C4.M4.ZY_ZGJB_F56"]
["阻垢剂加药泵2850Hz噪音","C4.M4.ZY_ZGJB_F57"]
["阻垢剂加药泵2900Hz噪音","C4.M4.ZY_ZGJB_F58"]
["阻垢剂加药泵2950Hz噪音","C4.M4.ZY_ZGJB_F59"]
["阻垢剂加药泵3000Hz噪音","C4.M4.ZY_ZGJB_F60"]
["阻垢剂加药泵3050Hz噪音","C4.M4.ZY_ZGJB_F61"]
["阻垢剂加药泵3100Hz噪音","C4.M4.ZY_ZGJB_F62"]
["阻垢剂加药泵3150Hz噪音","C4.M4.ZY_ZGJB_F63"]
["阻垢剂加药泵3200Hz噪音","C4.M4.ZY_ZGJB_F64"]
["阻垢剂加药泵3250Hz噪音","C4.M4.ZY_ZGJB_F65"]
["阻垢剂加药泵3300Hz噪音","C4.M4.ZY_ZGJB_F66"]
["阻垢剂加药泵3350Hz噪音","C4.M4.ZY_ZGJB_F67"]
["阻垢剂加药泵3400Hz噪音","C4.M4.ZY_ZGJB_F68"]
["阻垢剂加药泵3450Hz噪音","C4.M4.ZY_ZGJB_F69"]
["阻垢剂加药泵3500Hz噪音","C4.M4.ZY_ZGJB_F70"]
["阻垢剂加药泵3550Hz噪音","C4.M4.ZY_ZGJB_F71"]
["阻垢剂加药泵3600Hz噪音","C4.M4.ZY_ZGJB_F72"]
["阻垢剂加药泵3650Hz噪音","C4.M4.ZY_ZGJB_F73"]
["阻垢剂加药泵3700Hz噪音","C4.M4.ZY_ZGJB_F74"]
["阻垢剂加药泵3750Hz噪音","C4.M4.ZY_ZGJB_F75"]
["阻垢剂加药泵3800Hz噪音","C4.M4.ZY_ZGJB_F76"]
["阻垢剂加药泵3850Hz噪音","C4.M4.ZY_ZGJB_F77"]
["阻垢剂加药泵3900Hz噪音","C4.M4.ZY_ZGJB_F78"]
["阻垢剂加药泵3950Hz噪音","C4.M4.ZY_ZGJB_F79"]
["阻垢剂加药泵4000Hz噪音","C4.M4.ZY_ZGJB_F80"]
["阻垢剂加药泵4050Hz噪音","C4.M4.ZY_ZGJB_F81"]
["阻垢剂加药泵4100Hz噪音","C4.M4.ZY_ZGJB_F82"]
["阻垢剂加药泵4150Hz噪音","C4.M4.ZY_ZGJB_F83"]
["阻垢剂加药泵4200Hz噪音","C4.M4.ZY_ZGJB_F84"]
["阻垢剂加药泵4250Hz噪音","C4.M4.ZY_ZGJB_F85"]
["阻垢剂加药泵4300Hz噪音","C4.M4.ZY_ZGJB_F86"]
["阻垢剂加药泵4350Hz噪音","C4.M4.ZY_ZGJB_F87"]
["阻垢剂加药泵4400Hz噪音","C4.M4.ZY_ZGJB_F88"]
["阻垢剂加药泵4450Hz噪音","C4.M4.ZY_ZGJB_F89"]
["阻垢剂加药泵4500Hz噪音","C4.M4.ZY_ZGJB_F90"]
["阻垢剂加药泵4550Hz噪音","C4.M4.ZY_ZGJB_F91"]
["阻垢剂加药泵4600Hz噪音","C4.M4.ZY_ZGJB_F92"]
["阻垢剂加药泵4650Hz噪音","C4.M4.ZY_ZGJB_F93"]
["阻垢剂加药泵4700Hz噪音","C4.M4.ZY_ZGJB_F94"]
["阻垢剂加药泵4750Hz噪音","C4.M4.ZY_ZGJB_F95"]
["阻垢剂加药泵4800Hz噪音","C4.M4.ZY_ZGJB_F96"]
["阻垢剂加药泵4850Hz噪音","C4.M4.ZY_ZGJB_F97"]
["阻垢剂加药泵4900Hz噪音","C4.M4.ZY_ZGJB_F98"]
["阻垢剂加药泵4950Hz噪音","C4.M4.ZY_ZGJB_F99"]
["阻垢剂加药泵5000Hz噪音","C4.M4.ZY_ZGJB_F100"]
["阻垢剂加药泵5050Hz噪音","C4.M4.ZY_ZGJB_F101"]
["阻垢剂加药泵5100Hz噪音","C4.M4.ZY_ZGJB_F102"]
["阻垢剂加药泵5150Hz噪音","C4.M4.ZY_ZGJB_F103"]
["阻垢剂加药泵5200Hz噪音","C4.M4.ZY_ZGJB_F104"]
["阻垢剂加药泵5250Hz噪音","C4.M4.ZY_ZGJB_F105"]
["阻垢剂加药泵5300Hz噪音","C4.M4.ZY_ZGJB_F106"]
["阻垢剂加药泵5350Hz噪音","C4.M4.ZY_ZGJB_F107"]
["阻垢剂加药泵5400Hz噪音","C4.M4.ZY_ZGJB_F108"]
["阻垢剂加药泵5450Hz噪音","C4.M4.ZY_ZGJB_F109"]
["阻垢剂加药泵5500Hz噪音","C4.M4.ZY_ZGJB_F110"]
["阻垢剂加药泵5550Hz噪音","C4.M4.ZY_ZGJB_F111"]
["阻垢剂加药泵5600Hz噪音","C4.M4.ZY_ZGJB_F112"]
["阻垢剂加药泵5650Hz噪音","C4.M4.ZY_ZGJB_F113"]
["阻垢剂加药泵5700Hz噪音","C4.M4.ZY_ZGJB_F114"]
["阻垢剂加药泵5750Hz噪音","C4.M4.ZY_ZGJB_F115"]
["阻垢剂加药泵5800Hz噪音","C4.M4.ZY_ZGJB_F116"]
["阻垢剂加药泵5850Hz噪音","C4.M4.ZY_ZGJB_F117"]
["阻垢剂加药泵5900Hz噪音","C4.M4.ZY_ZGJB_F118"]
["阻垢剂加药泵5950Hz噪音","C4.M4.ZY_ZGJB_F119"]
["阻垢剂加药泵6000Hz噪音","C4.M4.ZY_ZGJB_F120"]
["阻垢剂加药泵6050Hz噪音","C4.M4.ZY_ZGJB_F121"]
["阻垢剂加药泵6100Hz噪音","C4.M4.ZY_ZGJB_F122"]
["阻垢剂加药泵6150Hz噪音","C4.M4.ZY_ZGJB_F123"]
["阻垢剂加药泵6200Hz噪音","C4.M4.ZY_ZGJB_F124"]
["阻垢剂加药泵6250Hz噪音","C4.M4.ZY_ZGJB_F125"]
["阻垢剂加药泵6300Hz噪音","C4.M4.ZY_ZGJB_F126"]
["阻垢剂加药泵6350Hz噪音","C4.M4.ZY_ZGJB_F127"]